{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Cennik","Zenergy-OE","Oferta","Zgrupuj","Zestawienie","Zbaza"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cennik","index":0,"n_rows":8599,"n_cols":17,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
[]
[null,"Cennik 03-2025"]
["Symbol","Nazwa","Cena","Grupa rabat","QTY-%","FREQ-%M","Rodzina","Grafika","Unit","Intrastat","PKWiU","Activity","EAN-13","FR","EN","ES","HG"]
["00006","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H400 6M - H300MM",39.6,"1-ZE-03",0.2,1,"ON_SUPPORT","00006","SZT","85389099","27.12.40.0",null,"5901988000066","ON/PT - Deux supports de rail DIN H400 6M - H300mm","ON/PT - Two DIN rail supports of the housing H400 6M - H300mm","ON/EMP- CHASIS CARRIL DIN (2UDS) H400 6M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H400 6M - H300MM HÁZHOZ"]
["00009","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H550 9M - H450mm",42.3,"1-ZE-03",0.8,4,"ON_SUPPORT","00009","SZT","85389099","27.12.40.0",null,"5901988000097","ON/PT - Deux supports de rail DIN H550 9M - H450mm","ON/PT - Two DIN rail brackets of the H550 9M - H450mm housing","ON/EMP- CHASIS CARRIL DIN (2UDS) H550 9M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H550 9M - H450mm HÁZHOZ"]
["00012","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H700 12M - H600MM",43.6,"1-ZE-03",2.75,11,"ON_SUPPORT","00012","SZT","85389099","27.12.40.0",null,"5901988000127","ON/PT - Deux supports de rail DIN H700 12M - H600mm","ON/PT - Two DIN rail supports of the H700 12M - H600mm housing","ON/EMP- CHASIS CARRIL DIN (2UDS) H700 12M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H700 HÁZHOZ 12M - H600MM"]
["00015","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H850 15M - H750MM",52.8,"1-ZE-03",2.65,7,"ON_SUPPORT","00015","SZT","85389099","27.12.40.0",null,"5901988000158","ON/PT - Deux supports de rail DIN H850 15M - H750mm","ON/PT - Two DIN rail brackets of the H850 15M - H750mm housing","ON/EMP- CHASIS CARRIL DIN (2UDS) H850 15M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H850 15M - H750MM HÁZHOZ"]
["00018","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H1000 18M - H900MM",62.1,"1-ZE-03",0.8833333333333333,6,"ON_SUPPORT","00018","SZT","85389099","27.12.40.0",null,"5901988000189","ON/PT - Deux supports de rail DIN H1000 18M - H900mm","ON/PT - Two DIN rail brackets of the H1000 18M - H900mm housing","ON/EMP- CHASIS CARRIL DIN (2UDS) H1000 18M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H1000 HÁZHOZ 18M - H900MM"]
["00021","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H1150 21M - H1050MM",71.3,"1-ZE-03",0.96666666666666667,6,"ON_SUPPORT","00021","SZT","85389099","27.12.40.0",null,"5901988000219","ON/PT - Deux supports de rail DIN H1150 21M - H1050mm","ON/PT - Two DIN rail brackets of the housing H1150 21M - H1050mm","ON/EMP- CHASIS CARRIL DIN (2UDS) H1150 21M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H1150 21M - H1050MM HÁZHOZ"]
["00024","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H1300 24M - H1200MM",79.3,"1-ZE-03",0.28333333333333333,2,"ON_SUPPORT","00024","SZT","85389099","27.12.40.0",null,"5901988000240","ON/PT - Deux supports de rail DIN H1300 24M - H1200mm","ON/PT - Two DIN rail brackets of the housing H1300 24M - H1200mm","ON/EMP- CHASIS CARRIL DIN (2UDS) H1300 24M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H1300 24M - H1200MM HÁZHOZ"]
["00027","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H1450 27M - H1350MM",85.9,"1-ZE-03",8.3333333333333329E-2,2,"ON_SUPPORT","00027","SZT","85389099","27.12.40.0",null,"5901988000271","ON/PT - Deux supports de rail DIN H1450 27M - H1350mm","ON/PT - Two DIN rail brackets of the housing H1450 27M - H1350mm","ON/EMP- CHASIS CARRIL DIN (2UDS) H1450 27M ","ZENERGY ON/PT - KÉT DIN SÍN TARTÓK HÁZHOZ H1450 27M - H1350MM"]
["00030","ZENERGY ON/PT - DWA WSPORNIKI SZYN DIN OBUDOWY H1600 30M - H1500MM",129.30000000000001,"1-ZE-03",0.24166666666666667,5,"ON_SUPPORT","00030","SZT","85389099","27.12.40.0",null,"5901988000301","ON/PT - Deux supports de rail DIN H1600 30M - H1500mm","ON/PT - Two DIN rail supports for the H1600 30M - H1500mm housing","ON/EMP- CHASIS CARRIL DIN (2UDS) H1600 30M","ZENERGY ON/PT - KÉT DIN SÍN TARTÁS H1600 HÁZHOZ 30M - H1500MM"]
["00100","ZENERGY ON/PT - SZYNA DIN / TS-35D APARATURY MODUŁOWEJ 24MOD, W600",22,"1-ZE-03",39.858333333333334,6,"ON_RAIL_DIN","00100","SZT","85389099","27.12.40.0",null,"5901988001001","ON/PT - Appareil modulaire sur rail DIN / TS-35D 24MOD, L600","ON/PT - DIN / TS-35D rail for 24MOD, W600 modular equipment","ON/EMP- CARRIL DIN /TS-35D FIJO 24MOD, W600","ZENERGY ON/PT - DIN SÍN / TS-35D MODULÁRUS KÉSZÜLÉK 24MOD, W600"]
["00101","ZENERGY ON/PT - POKRYWA TYLNA W600, 3M, OCYNK",15.9,"1-ZE-03",22.7,11,"PT_BACK_PLATE","00101","SZT","85389099","27.12.40.0",null,"5901988001018","ON/PT - Couvercle arrière L600, 3M, galvanisé","ON/PT - Back Cover W600, 3M, galv","ON/EMP- PANEL TRASERO W600 3M GALV.","ZENERGY ON/PT - HÁTSÓ BURKOLAT W600, 3M, HORGANYOZÁS"]
["00102","ZENERGY ON/PT - SZYNA DIN / TS-35D APARATURY MODUŁOWEJ 35MOD, W800",25.9,"1-ZE-03",0.15833333333333333,1,"ON_RAIL_DIN",null,null,"85389099",null,null,"5901988001025"]
["00103","ZENERGY ON/PT - POKRYWA TYLNA W800, 3M, OCYNK",19,"1-ZE-03",1.5,4,"PT_BACK_PLATE","00103","SZT","85389099","27.12.40.0",null,"5901988001032","ON/PT - Couvercle arrière L800, 3M, galvanisé","ON/PT - Back Cover W800, 3M, Galvanized","ON/EMP- PANEL TRASERO W800, 3M, GALV.","ZENERGY ON/PT - HÁTSÓ BURKOLAT W800, 3M, HORGANYOZÁS"]
["00106","ZENERGY ON - DWIE POKRYWY PIONOWE H400 6M IP-30",106,"1-ZE-03",0.23333333333333334,2,"ON_VERTICAL_COVER","00106","SZT","85389099","27.12.40.0",null,"5901988001063","ON - Deux couvercles verticaux H400 6M IP-30","ON - Two Vertical Lids H400 6M IP-30","ON- PANEL LATERAL (2UDS) H400 6M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H400 6M IP-30"]
["00107","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H400 6M IP-30)",51.5,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001070","produit invalidé ON - Deux profils arrière H400 6M IP-30","product cancelled ON - Two Rear Profiles H400 6M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H400 6M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H400 6M IP-30)"]
["00108","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H400 6M IP-30",116.6,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00108","SZT","85389099","27.12.40.0",null,"5901988001087","ON - Couvercle d'extension verticale - ravine H400 6M IP-30","ON - Vertical Extension Cover - H400 6M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H400 6M IP30","ZENERGY ON - FÜGGŐLEGES BŐVÍTŐ BURKOLAT - BULLET H400 6M IP-30"]
["00109","ZENERGY ON - DWIE POKRYWY PIONOWE H550 9M IP-30",108.1,"1-ZE-03",0.68333333333333335,5,"ON_VERTICAL_COVER","00109","SZT","85389099","27.12.40.0",null,"5901988001094","ON - Deux couvercles verticaux H550 9M IP-30","ON - Two Vertical Lids H550 9M IP-30","ON- PANEL LATERAL (2UDS) H550 9M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H550 9M IP-30"]
["00110","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H550 9M IP-30)",54.3,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001100","produit invalidé ON - Deux profils arrière H550 9M IP-30","product cancelled ON - Two Rear Profiles H550 9M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H550 9M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H550 9M IP-30)"]
["00111","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H550 9M IP-30",121.9,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00111","SZT","85389099","27.12.40.0",null,"5901988001117","ON - Cache d'extension verticale - H550 9M IP-30","ON - Vertical Extension Cover - H550 9M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H550 9M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H550 9M IP-30"]
["00112","ZENERGY ON - DWIE POKRYWY PIONOWE H700 12M IP-30",111.3,"1-ZE-03",1.2333333333333334,6,"ON_VERTICAL_COVER","00112","SZT","85389099","27.12.40.0",null,"5901988001124","ON - Deux couvercles verticaux H700 12M IP-30","ON - Two Vertical Lids H700 12M IP-30","ON- PANEL LATERAL (2UDS) H700 12M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H700 12M IP-30"]
["00113","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H700 12M IP-30)",55.5,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001131","produit invalidé ON - Deux profils arrière H700 12M IP-30","product cancelled ON - Two Rear Profiles H700 12M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H700 12M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H700 12M IP-30)"]
["00114","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H700 12M IP-30",128.30000000000001,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00114","SZT","85389099","27.12.40.0",null,"5901988001148","ON - Couvercle d'extension verticale - Gully H700 12M IP-30","ON - Vertical Extension Cover - H700 12M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H700 12M IP30","ZENERGY ON - FÜGGŐLEGES BŐVÍTŐ BURKOLAT - BULLET H700 12M IP-30"]
["00115","ZENERGY ON - DWIE POKRYWY PIONOWE H850 15M IP-30",134.6,"1-ZE-03",0.7,5,"ON_VERTICAL_COVER","00115","SZT","85389099","27.12.40.0",null,"5901988001155","ON - Deux couvercles verticaux H850 15M IP-30","ON - Two Vertical Lids H850 15M IP-30","ON- PANEL LATERAL (2UDS) H850 15M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H850 15M IP-30"]
["00116","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H850 15M IP-30)",67.400000000000006,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001162","produit invalidé ON - Deux profils arrière H850 15M IP-30","product cancelled ON - Two Rear Profiles H850 15M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H850 15M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H850 15M IP-30)"]
["00117","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H850 15M IP-30",155.80000000000001,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00117","SZT","85389099","27.12.40.0",null,"5901988001179","ON - Couvercle d'extension verticale - bague H850 15M IP-30","ON - Vertical Extension Cover - H850 15M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H850 15M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H850 15M IP-30"]
["00118","ZENERGY ON - DWIE POKRYWY PIONOWE H1000 18M IP-30",155.80000000000001,"1-ZE-03",0.70833333333333337,6,"ON_VERTICAL_COVER","00118","SZT","85389099","27.12.40.0",null,"5901988001186","ON - Deux couvercles verticaux H1000 18M IP-30","ON - Two Vertical Lids H1000 18M IP-30","ON- PANEL LATERAL (2UDS) H1000 18M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H1000 18M IP-30"]
["00119","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H1000 18M IP-30)",77.900000000000006,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001193","produit invalidé ON - Deux profils arrière H1000 18M IP-30","product cancelled ON - Two Rear Profiles H1000 18M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H1000 18M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H1000 18M IP-30)"]
["00120","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H1000 18M IP-30",182.3,"1-ZE-03",1.6666666666666666E-2,1,"ON_VERTICAL_COVER","00120","SZT","85389099","27.12.40.0",null,"5901988001209","ON - Couvercle de rallonge vertical - bague H1000 18M IP-30","ON - Vertical Extension Cover - H1000 18M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H1000 18M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H1000 18M IP-30"]
["00121","ZENERGY ON - DWIE POKRYWY PIONOWE H1150 21M IP-30",180.2,"1-ZE-03",0.60833333333333328,4,"ON_VERTICAL_COVER","00121","SZT","85389099","27.12.40.0",null,"5901988001216","ON - Deux couvercles verticaux H1150 21M IP-30","ON - Two Vertical Lids H1150 21M IP-30","ON- PANEL LATERAL (2UDS) H1150 21M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H1150 21M IP-30"]
["00122","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H1150 21M IP-30)",89.8,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001223","produit invalidé ON - Deux profils arrière H1150 21M IP-30","product cancelled ON - Two Rear Profiles H1150 21M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H1150 21M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H1150 21M IP-30)"]
["00123","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H1150 21M IP-30",208.8,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00123","SZT","85389099","27.12.40.0",null,"5901988001230","ON - Couvercle d'extension verticale - Câbles H1150 21M IP-30","ON - Vertical Extension Cover - H1150 21M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H1150 21M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H1150 21M IP-30"]
["00124","ZENERGY ON - DWIE POKRYWY PIONOWE H1300 24M IP-30",198.2,"1-ZE-03",0.01,1,"ON_VERTICAL_COVER","00124","SZT","85389099","27.12.40.0",null,"5901988001247","ON - Deux couvercles verticaux H1300 24M IP-30","ON - Two Vertical Lids H1300 24M IP-30","ON- PANEL LATERAL (2UDS) H1300 24M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H1300 24M IP-30"]
["00125","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H1300 24M IP-30)",99.1,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001254","produit invalidé ON - Deux profils arrière H1300 24M IP-30","product cancelled ON - Two Rear Profiles H1300 24M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H1300 24M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H1300 24M IP-30)"]
["00126","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H1300 24M IP-30",230,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00126","SZT","85389099","27.12.40.0",null,"5901988001261","ON - Couvercle d'extension verticale - bague H1300 24M IP-30","ON - Vertical Extension Cover - H1300 24M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H1300 24M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H1300 24M IP-30"]
["00127","ZENERGY ON - DWIE POKRYWY PIONOWE H1450 27M IP-30",214.1,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00127","SZT","85389099","27.12.40.0",null,"5901988001278","ON - Deux couvercles verticaux H1450 27M IP-30","ON - Two Vertical Lids H1450 27M IP-30","ON- PANEL LATERAL (2UDS) H1450 27M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H1450 27M IP-30"]
["00128","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H1450 27M IP-30)",107.1,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001285","produit invalidé ON - Deux profils arrière H1450 27M IP-30","product cancelled ON - Two Rear Profiles H1450 27M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H1450 27M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H1450 27M IP-30)"]
["00129","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H1450 27M IP-30",252.3,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00129","SZT","85389099","27.12.40.0",null,"5901988001292","ON - Couvercle d'extension verticale - bague H1450 27M IP-30","ON - Vertical Extension Cover - H1450 27M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H1450 27M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H1450 27M IP-30"]
["00130","ZENERGY ON - DWIE POKRYWY PIONOWE H1600 30M IP-30",322.2,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00130","SZT","85389099","27.12.40.0",null,"5901988001308","ON - Deux couvercles verticaux H1600 30M IP-30","ON - Two Vertical Lids H1600 30M IP-30","ON- PANEL LATERAL (2UDS) H1600 30M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT H1600 30M IP-30"]
["00131","produkt wycofany (ZENERGY ON - DWA PROFILE TYLNE H1600 30M IP-30)",161.1,"1-ZE-03",null,null,"ON_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988001315","produit invalidé ON - Deux profils arrière H1600 30M IP-30","product cancelled ON - Two Rear Profiles H1600 30M IP-30","producto suspendido ON- PERFIL TRASERO (2UDS) H1600 30M IP30","kivont termék (ZENERGY ON - KÉT HÁTSÓ PROFIL H1600 30M IP-30)"]
["00132","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST H1600 30M IP-30",323.3,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00132","SZT","85389099","27.12.40.0",null,"5901988001322","ON - Couvercle d'extension verticale - Goulotte H1600 30M IP-30","ON - Vertical Extension Cover - H1600 30M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. H1600 30M IP30","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET H1600 30M IP-30"]
["00160","ZENERGY ON - DWIE POKRYWY POZIOME W600 IP-30",110.2,"1-ZE-03",1.6083333333333334,7,"ON_HORIZONTAL_COVER","00160","SZT","85389099","27.12.40.0",null,"5901988001605","ON - Deux couvercles horizontaux L600 IP-30","ON - Two Horizontal Lids W600 IP-30","ON- TECHO/SUELO (2UUDS) W600 IP30","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W600 IP-30"]
["00161","ZENERGY ON - COKÓŁ W600 IP-30",251.2,"1-ZE-03",null,null,"ON_PLINTHS","00161","SZT","85389099","27.12.40.0",null,"5901988001612","ON - Socle L600 IP-30","ON - W600 IP-30 plinth","ON- ZOCALO  W600 IP30","ZENERGY ON - LÁZAT W600 IP-30"]
["00163","ZENERGY ON - DWIE POKRYWY POZIOME W600 IP-30, GÓRNA Z OTWOREM 81X222 POD PRZEPUST IP-55",110.2,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00163","SZT","85389099","27.12.40.0",null,"5901988001636","ON - Deux couvercles horizontaux L600 IP-30, supérieur avec ouverture 81x222 sous passage IP-55","ON - Two Horizontal W600 IP-30 Lids, the top with an opening 81x222 for the IP-55 bushing","ON- TECHO/SUELO (2UUDS) W600 IP30","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W600 IP-30, FELSŐ 81X222 LYUKAL, IP-55 GOLYÓHOZ"]
["00164","ZENERGY ON - DWIE POKRYWY POZIOME W600 IP-30, Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",110.2,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00164","SZT","85389099","27.12.40.0",null,"5901988001643","ON - Deux capots horizontaux L600 IP-30, supérieur avec DEUX trous 81x222 sous passage IP-55","ON - Two Horizontal W600 IP-30 Lids, the top with TWO holes 81x222 for the IP-55 bushing","ON- TECHO/SUELO (2UUDS) W600 IP30","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W600 IP-30, KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["00165","ZENERGY ON - DWIE POKRYWY POZIOME W600 IP-30, Z OTWOREM 81X222 POD PRZEPUST IP-55",110.2,"1-ZE-03",2.7416666666666667,6,"ON_HORIZONTAL_COVER","00165","SZT","85389099","27.12.40.0",null,"5901988001650","ON - Deux couvercles horizontaux L600 IP-30, haut et bas, avec ouverture 81x222 sous IP-55 Pass","ON - Two Horizontal W600 IP-30 covers, top and bottom with a 81x222 opening for the IP-55 bushing","ON- TECHO/SUELO CON ENTRADA CABLES (2UUDS) W600 IP30","ZENERGY ON – KÉT VÍZSZINTES BURKOLAT W600 IP-30, 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["00166","ZENERGY ON - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W600 IP-30",103,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00166","SZT","85389099","27.12.40.0",null,"5901988001667","ON - Extension de poignée horizontale - Passe-câble L600 IP-30","ON - Horizontal Extension Cover - W600 IP-30 Grommet","ON- TECHO PARA UNION ARMARIOS - W600 IP30","ZENERGY ON - BŐVÍTÉSI SZINT FEDÉL - BULLET W600 IP-30"]
["00170","ZENERGY ON - DWIE POKRYWY POZIOME W600 D205 IP-30",121.9,"1-ZE-03",1.6666666666666666E-2,1,"ON_HORIZONTAL_COVER","00170","SZT","85389099",null,null,"5901988001704","ON - Deux couvercles horizontaux L600 D205 IP-30","ON - Two Horizontal Covers W600 D205 IP-30","ON- TECHO/SUELO (2UDS) W600 D205 IP30","ZENERGY ON – KÉT VÍZSZINTES BORÍTÓ W600 D205 IP-30"]
["00171","ZENERGY ON - COKÓŁ W600 D205 IP-30",276.7,"1-ZE-03",null,null,"ON_PLINTHS","00171","SZT","85389099","27.12.40.0",null,"5901988001711","ON - Socle L600 D205 IP-30","ON - Plinth W600 D205 IP-30","ON- ZOCALO W600 D205 IP30","ZENERGY ON - LÁZAT W600 D205 IP-30"]
["00173","ZENERGY ON - DWIE POKRYWY POZIOME W600 D205 IP-30, GÓRNA Z OTWOREM 81X222 POD PRZEPUST IP-55",121.9,"1-ZE-03",1.6666666666666666E-2,1,"ON_HORIZONTAL_COVER","00173","SZT","85389099",null,null,"5901988001735","ON - Deux couvercles horizontaux L600 D205 IP-30, supérieur avec ouverture 81x222 sous passage IP-55","ON - Two Horizontal W600 D205 IP-30 covers, the upper one with an opening 81x222 for the IP-55 bushing","ON- TECHO/SUELO (2UDS) W600 D205 IP30, CON 81X222 PARA MEMBRANA IP55","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W600 D205 IP-30, FELSŐ 81X222 LYUKAL IP-55 LÖVEDEKHEZ"]
["00174","ZENERGY ON - DWIE POKRYWY POZIOME W600 D205 IP-30, GÓRNA Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",121.9,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00174","SZT","85389099",null,null,"5901988001742","ON - Deux capots horizontaux L600 D205 IP-30, supérieur avec DEUX trous 81x222 sous passage IP-55","ON - Two Horizontal Covers W600 D205 IP-30, top and bottom with two holes 81x222 for the IP-55 bushing","ON- TECHO/SUELO (2UDS) W600 D205 IP30, CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W600 D205 IP-30, FELSŐ KÉT LYUKAL 81X222 IP-55 LÖVEDEKHEZ"]
["00175","ZENERGY ON - DWIE POKRYWY POZIOME W600 D205 IP-30, GÓRNA I DOLNA Z OTWOREM 81X222 POD PRZEPUST IP-55",121.9,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00175","SZT","85389099",null,null,"5901988001759","ON - Deux couvercles horizontaux L600 D205 IP-30, haut et bas, avec ouverture 81x222 sous IP-55 Pass","ON - Two Horizontal Covers W600 D205 IP-30, top and bottom with an opening 81x222 for the IP-55 gland","ON- TECHO/SUELO (2UDS) W600 P205 IP30, CON 81X222 PARA  MEMBRANA IP55","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W600 D205 IP-30, FELSŐ ÉS ALSÓ 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["00176","ZENERGY ON - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W600 D205 IP-30",113.4,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00176","SZT","85389099",null,null,"5901988001766","ON - Extension de poignée horizontale - Passe-câble L600 D205 IP-30","ON - Horizontal Extension Cover - W600 D205 IP-30 Grommet","ON- TECHO DE MODULO AUX. HORIZ.  W600 D205 IP30","ZENERGY ON – BŐVÍTÉSI SZINT FEDÉL – BULLET W600 D205 IP-30"]
["00180","ZENERGY ON - DWIE POKRYWY POZIOME W800 D205 IP-30",132.5,"1-ZE-03",0.11666666666666667,7,"ON_HORIZONTAL_COVER","00180","SZT","85389099",null,null,"5901988001803","ON - Deux couvercles horizontaux L800 D205 IP-30","ON - Two Horizontal Lids W800 D205 IP-30","ON- TECHO/SUELO (2UDS) W800 D205 IP30","ZENERGY ON – KÉT VÍZSZINTES BORÍTÓ W800 D205 IP-30"]
["00181","ZENERGY ON - COKÓŁ W800 D205 IP-30",302.10000000000002,"1-ZE-03",1.6666666666666666E-2,1,"ON_PLINTHS","00181","SZT","85389099",null,null,"5901988001810","ON - Socle L800 D205 IP-30","ON - W800 D205 IP-30 plinth","ON- ZOCALO W800 D205 IP30","ZENERGY ON - LÁZAT W800 D205 IP-30"]
["00183","ZENERGY ON - DWIE POKRYWY POZIOME W800 D205 IP-30, GÓRNA Z OTWOREM 81X222 POD PRZEPUST IP-55",132.5,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00183","SZT","85389099",null,null,"5901988001834","ON - Deux couvercles horizontaux L800 D205 IP-30, supérieur avec ouverture 81x222 sous passage IP-55","ON - Two Horizontal Covers W800 D205 IP-30, the top with an opening 81x222 for the IP-55 gland","ON- TECHO/SUELO (2UDS) W800 D205 IP30, CON 81X222 PARA MEMBRANA IP55","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W800 D205 IP-30, FELSŐ 81X222 LYUKAL, IP-55 GOLYÓHOZ"]
["00184","ZENERGY ON - DWIE POKRYWY POZIOME W800 D205 IP-30, Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",132.5,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00184","SZT","85389099",null,null,"5901988001841","ON - Deux capots horizontaux L800 D205 IP-30, supérieur avec DEUX trous 81x222 sous passage IP-55","ON - Two Horizontal W800 D205 IP-30 covers, top and bottom with two holes 81x222 for the IP-55 bushing","ON- TECHO/SUELO (2UDS) W800 D205 IP30, CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W800 D205 IP-30, KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["00185","ZENERGY ON - DWIE POKRYWY POZIOME W800 D205 IP-30, Z OTWOREM 81X222 POD PRZEPUST IP-55",132.5,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00185","SZT","85389099",null,null,"5901988001858","ON - Deux couvercles horizontaux L800 D205 IP-30, haut et bas, avec ouverture 81x222 sous IP-55 Pass","ON - Two Horizontal Covers W800 D205 IP-30, top and bottom with an opening 81x222 for the IP-55 gland","ON- TECHO/SUELO (2UDS) W800 D205 IP30, CON 81X222 PARA MEMBRANA IP55","ZENERGY ON - KÉT VÍZSZINTES BURKOLAT W800 D205 IP-30, 81X222 LYUKAL, IP-55 GOLYÓHOZ"]
["00186","ZENERGY ON - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W800 D205 IP-30",124,"1-ZE-03",null,null,"ON_HORIZONTAL_COVER","00186","SZT","85389099",null,null,"5901988001865","ON - Extension de poignée horizontale - Passe-câble L800 D205 IP-30","ON - Horizontal Extension Cover - W800 D205 IP-30 Grommet","ON- TECHO DE MODULO AUX. HORIZ.  W800 D205 IP30","ZENERGY ON – BŐVÍTÉSI SZINT BURKOLAT – BULLET W800 D205 IP-30"]
["00190","IT - Prowadnice do montażu akumulatorów RACK 19 ( 2 szt. ) obudowa D=775",92,null,1.3083333333333333,4,"IT_SUPPORT",null,null,null,null,"240202PW",null,"IT - Guides pour le montage des batteries RACK 19 (2 pcs.) boîtier D=775","IT - Guides for mounting RACK 19 batteries (2 pcs.) housing D=775","IT - Guías para montaje de carcasa de baterías RACK 19 (2 uds.) D=775","IT - Útmutatók RACK 19 akkumulátor (2 db) felszereléséhez D=775 ház"]
["00191","IT - Podstawka pod panel operatorski",121.9,null,null,null,"IT_SUPPORT",null,null,null,null,"240202PW",null,"IT - Support pour le panneau opérateur","IT - Stand for the operator panel","IT - Soporte para el panel del operador","IT - Állvány a kezelőpanelhez"]
["00192","IT - WYGRODZENIE SZYN POZIOMYCH RACK 19, 3U - W600 2 FORMA",142.19999999999999,null,null,null,"OE_SEPARATION_BUSBAR",null,null,null,null,"240201PW",null,"IT - CLÔTURE DE RAILS HORIZONTAUX RACK 19, 3U - W600 2 FORM","IT - FENCE OF HORIZONTAL RAILS RACK 19, 3U - W600 2 FORM","IT - VALLA DE RAILES HORIZONTALES RACK 19, 3U - W600 2 FORM","IT - VÍZSZINTES SÍNEK KERÍTÉSE RACK 19, 3U - W600 2 FORM"]
["00193","IT - WYGRODZENIE SZYN POZIOMYCH RACK 19, 5U - W600 2 FORMA",268.8,null,0.24166666666666667,4,"OE_SEPARATION_BUSBAR",null,null,null,null,"240206PW",null,"IT - CLÔTURE DE RAILS HORIZONTAUX RACK 19, 5U - W600 2 FORM","IT - FENCE OF HORIZONTAL RAILS RACK 19, 5U - W600 2 FORM","IT - VALLA DE RAILES HORIZONTALES RACK 19, 5U - W600 2 FORM","IT - VÍZSZINTES RÚDAK KERÍTÉSE RACK 19, 5U - W600 2 FORMA"]
["00194","IT - PŁYTA MONTAŻOWA NOARK400A RACK 19, W600, 6U, PIONOWO, DŹWIGNIA",212.8,null,6.6666666666666666E-2,1,"IT_MCCB_PLATES",null,null,null,null,"240202PW",null,"IT - PLAQUE DE MONTAGE NOARK400A RACK 19, W600, 6U, VERTICAL, LEVIER","​IT - MOUNTING PLATE NOARK400A RACK 19, W600, 6U, VERTICAL, LEVER","IT - PLACA DE MONTAJE NOARK400A RACK 19, W600, 6U, VERTICAL, PALANCA","IT - SZERELŐLEMEZ NOARK400A RACK 19, W600, 6U, FÜGGŐLEGES, KAR"]
["00196","IT - OSŁONA CZOŁOWA NOARK400A 3P, RACK 19 W600, 9U, PIONOWO, DŹWIGNIA",146.69999999999999,null,6.6666666666666666E-2,1,"03_SWITCHES_COVERS",null,null,null,null,"240202PW",null,"IT - COUVERCLE AVANT NOARK400A 3P, RACK 19 W600, 9U, VERTICAL, LEVIER","​​​IT - FRONT COVER NOARK400A 3P, RACK 19 W600, 9U, VERTICAL, LEVER","IT - TAPA FRONTAL NOARK400A 3P, RACK 19 W600, 9U, VERTICAL, PALANCA","IT - ELSŐ BURKOLAT NOARK400A 3P, RACK 19 W600, 9U, FÜGGŐLEGES, KAR"]
["00197","ZENERGY IT - OSŁONA CZOŁOWA NOARK400A 4P, RACK 19 W600, 9U, PIONOWO, DŹWIGNIA",141.5,"1-ZE-01",null,null,null,null,null,"85389099",null,null,"5901988011970"]
["00209","ZENERGY OM - DWIE POKRYWY PIONOWE H550 D230 9M IP-30",104.8,"1-ZE-09",0.34166666666666667,2,"OM_VERTICAL_COVER","00209","SZT","85389099","27.12.40.0",null,"5901988002091","OM - Couvercle vertical H550 9M IP-30","OM - Two Vertical Lids H550 9M IP-30","OM- PANEL LATERAL (2UDS)  H550 9M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H550 D230 9M IP-30"]
["00210","ZENERGY OM - DWIE POKRYWY PIONOWE H550 D300 9M IP-30",122,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00210","SZT","85389099","27.12.40.0",null,"5901988002107","OM - Couvercle vertical H550 P300 9M IP-30","OM - Two Vertical Lids H550 D300 9M IP-30","OM- PANEL LATERAL (2UDS) H550 D300 9M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H550 D300 9M IP-30"]
["00212","ZENERGY OM - DWIE POKRYWY PIONOWE H700 D230 12M IP-30",116.6,"1-ZE-09",0.55000000000000004,5,"OM_VERTICAL_COVER","00212","SZT","85389099","27.12.40.0",null,"5901988002121","OM - Couvercle vertical H700 12M IP-30","OM - Two Vertical Lids H700 12M IP-30","OM- PANEL LATERAL (2UDS)  H700 12M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H700 D230 12M IP-30"]
["00213","ZENERGY OM - DWIE POKRYWY PIONOWE H700 D300 12M IP-30",135,"1-ZE-09",0.25,4,"OM_VERTICAL_COVER","00213","SZT","85389099","27.12.40.0",null,"5901988002138","OM - Couvercle vertical H700 P300 12M IP-30","OM - Two Vertical Lids H700 D300 12M IP-30","OM- PANEL LATERAL (2UDS) H700 D300 12M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H700 D300 12M IP-30"]
["00215","ZENERGY OM - DWIE POKRYWY PIONOWE H850 D230 15M IP-30",140.4,"1-ZE-09",0.53333333333333333,6,"OM_VERTICAL_COVER","00215","SZT","85389099","27.12.40.0",null,"5901988002152","OM - Couvercle vertical H850 15M IP-30","OM - Two Vertical Lids H850 15M IP-30","OM- PANEL LATERAL (2UDS)  H850 15M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H850 D230 15M IP-30"]
["00216","ZENERGY OM - DWIE POKRYWY PIONOWE H850 D300 15M IP-30",163.1,"1-ZE-09",0.29166666666666669,2,"OM_VERTICAL_COVER","00216","SZT","85389099","27.12.40.0",null,"5901988002169","OM - Couvercle vertical H850 P300 15M IP-30","OM - Two Vertical Lids H850 D300 15M IP-30","OM- PANEL LATERAL (2UDS) H850 D300 15M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H850 D300 15M IP-30"]
["00218","ZENERGY OM - DWIE POKRYWY PIONOWE H1000 D230 18M IP-30",164.2,"1-ZE-09",0.43333333333333335,4,"OM_VERTICAL_COVER","00218","SZT","85389099","27.12.40.0",null,"5901988002183","OM - Couvercle vertical H1000 18M IP-30","OM - Two Vertical Lids H1000 18M IP-30","OM- PANEL LATERAL (2UDS)  H1000 18M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1000 D230 18M IP-30"]
["00219","ZENERGY OM - DWIE POKRYWY PIONOWE H1000 D300 18M IP-30",191.2,"1-ZE-09",5.8333333333333334E-2,4,"OM_VERTICAL_COVER","00219","SZT","85389099","27.12.40.0",null,"5901988002190","OM - Couvercle vertical H1000 P300 18M IP-30","OM - Two Vertical Lids H1000 D300 18M IP-30","OM- PANEL LATERAL (2UDS) H1000 D300 18M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1000 D300 18M IP-30"]
["00221","ZENERGY OM - DWIE POKRYWY PIONOWE H1150 D230 21M IP-30",187.9,"1-ZE-09",0.53333333333333333,5,"OM_VERTICAL_COVER","00221","SZT","85389099","27.12.40.0",null,"5901988002213","OM - Couvercle vertical H1150 21M IP-30","OM - Two Vertical Lids H1150 21M IP-30","OM- PANEL LATERAL (2UDS)  H1150 21M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1150 D230 21M IP-30"]
["00222","ZENERGY OM - DWIE POKRYWY PIONOWE H1150 D300 21M IP-30",218.2,"1-ZE-09",0.05,2,"OM_VERTICAL_COVER","00222","SZT","85389099","27.12.40.0",null,"5901988002220","OM - Couvercle vertical H1150 P300 21M IP-30","OM - Two Vertical Lids H1150 D300 21M IP-30","OM- PANEL LATERAL (2UDS) H1150 D300 21M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1150 D300 21M IP-30"]
["00223","ZENERGY OM - DWIE POKRYWY PIONOWE H1300 D300 24M IP-30",239.8,"1-ZE-09",0.13333333333333333,5,"OM_VERTICAL_COVER","00223","SZT","85389099","27.12.40.0",null,"5901988002237","OM - Couvercle vertical H1300 P300 24M IP-30","OM - Two Vertical Lids H1300 D300 24M IP-30","OM- PANEL LATERAL (2UDS) H1300 D300 24M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1300 D300 24M IP-30"]
["00224","ZENERGY OM - DWIE POKRYWY PIONOWE H1300 D230 24M IP-30",206.3,"1-ZE-09",0.33333333333333331,6,"OM_VERTICAL_COVER","00224","SZT","85389099","27.12.40.0",null,"5901988002244","OM - Couvercle vertical H1300 24M IP-30","OM - Two Vertical Lids H1300 24M IP-30","OM- PANEL LATERAL (2UDS)  H1300 24M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1300 D230 24M IP-30"]
["00225","ZENERGY OM - DWIE POKRYWY PIONOWE H1450 D300 27M IP-30",261.39999999999998,"1-ZE-09",8.3333333333333329E-2,4,"OM_VERTICAL_COVER","00225","SZT","85389099","27.12.40.0",null,"5901988002251","OM - Couvercle vertical H1450 P300 27M IP-30","OM - Two Vertical Lids H1450 D300 27M IP-30","OM- PANEL LATERAL (2UDS) H1450 D300 27M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1450 D300 27M IP-30"]
["00226","ZENERGY OM - DWIE POKRYWY PIONOWE H1600 D300 28M IP-30",290.5,"1-ZE-09",3.3333333333333333E-2,2,"OM_VERTICAL_COVER","00226","SZT","85389099","27.12.40.0",null,"5901988002268","OM - Couvercle vertical H1600 P300 28M IP-30","OM - Two Vertical Lids H1600 D300 28M IP-30","OM- PANEL LATERAL (2UDS) H1600 D300 28M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1600 D300 28M IP-30"]
["00227","ZENERGY OM - DWIE POKRYWY PIONOWE H1450 D230 27M IP-30",225.7,"1-ZE-09",0.16666666666666666,2,"OM_VERTICAL_COVER","00227","SZT","85389099","27.12.40.0",null,"5901988002275","OM - Couvercle vertical H1450 27M IP-30","OM - Two Vertical Lids H1450 27M IP-30","OM- PANEL LATERAL (2UDS)  H1450 27M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1450 D230 27M IP-30"]
["00228","ZENERGY OM - DWIE POKRYWY PIONOWE H1600 D230 28M IP-30",249.5,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00228","SZT","85389099","27.12.40.0",null,"5901988002282","OM - Couvercle vertical H1600 28M IP-30","OM - Two Vertical Lids H1600 28M IP-30","OM- PANEL LATERAL (2UDS) H1600 28M IP30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1600 D230 28M IP-30"]
["00229","ZENERGY OM - DWIE POKRYWY PIONOWE H1550 D230 29M IP-30",276.5,"1-ZE-09",0.05,1,"OM_VERTICAL_COVER","00229","SZT","85389099","27.12.40.0",null,"5901988002299","OM - Couvercle vertical H1550 29M IP-30","OM - Two Vertical Lids H1550 29M IP-30","OM- PANEL LATERAL (2UDS) H1550 29M IP30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1550 D230 29M IP-30"]
["00230","ZENERGY OM - DWIE POKRYWY PIONOWE H1700 D230 30M IP-30",338,"1-ZE-09",0.53333333333333333,5,"OM_VERTICAL_COVER","00230","SZT","85389099","27.12.40.0",null,"5901988002305","OM - Couvercle vertical H1700 30M IP-30","OM - Two Vertical Lids H1700 30M IP-30","OM- PANEL LATERAL (2UDS)  H1700 30M IP30 ","ZENERGY OM – KÉT FÜGGŐLEGES BORÍTÓ H1700 D230 30M IP-30"]
["00231","ZENERGY OM - DWIE POKRYWY PIONOWE H1550 D300 29M IP-30",319.7,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00231","SZT","85389099","27.12.40.0",null,"5901988002312","OM - Couvercle vertical H1550 P300 29M IP-30","OM - Two Vertical Lids H1550 D300 29M IP-30","OM- PANEL LATERAL (2UDS) H1550 D300 29M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1550 D300 29M IP-30"]
["00232","ZENERGY OM - DWIE POKRYWY PIONOWE H1700 D300 30M IP-30",392,"1-ZE-09",6.6666666666666666E-2,5,"OM_VERTICAL_COVER","00232","SZT","85389099","27.12.40.0",null,"5901988002329","OM - Couvercle vertical H1700 P300 30M IP-30","OM - Two Vertical Lids H1700 D300 30M IP-30","OM- PANEL LATERAL (2UDS) H1700 D300 30M IP-30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1700 D300 30M IP-30"]
["00233","ZENERGY OM - DWIE POKRYWY PIONOWE H1850 D230 33M IP-30",427.7,"1-ZE-09",0.80833333333333335,6,"OM_VERTICAL_COVER","00233","SZT","85389099","27.12.40.0",null,"5901988002336","OM - Couvercle vertical H1850 33M IP-30","OM - Two Vertical Lids H1850 33M IP-30","OM- PANEL LATERAL (2UDS)  H1850 33M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1850 D230 33M IP-30"]
["00234","ZENERGY OM - DWIE POKRYWY PIONOWE H1850 D300 33M IP-30",495.7,"1-ZE-09",0.18333333333333332,2,"OM_VERTICAL_COVER","00234","SZT","85389099","27.12.40.0",null,"5901988002343","OM - Deux couvercles verticaux H1850 P300 33M IP-30","OM - Two Vertical Lids H1850 D300 33M IP-30","OM- PANEL LATERAL (2UDS) H1850 D300 33M IP30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1850 D300 33M IP-30"]
["00236","ZENERGY OM - DWIE POKRYWY PIONOWE H2000 D230 36M IP-30",479.5,"1-ZE-09",0.30833333333333335,4,"OM_VERTICAL_COVER","00236","SZT","85389099","27.12.40.0",null,"5901988002367","OM - Couvercle vertical H2000 36M IP-30","OM - Two Vertical Lids H2000 36M IP-30","OM- PANEL LATERAL (2UDS)  H2000 36M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2000 D230 36M IP-30"]
["00237","ZENERGY OM - DWIE POKRYWY PIONOWE H2000 D300 36M IP-30",556.20000000000005,"1-ZE-09",0.10833333333333334,2,"OM_VERTICAL_COVER","00237","SZT","85389099","27.12.40.0",null,"5901988002374","OM - Deux couvercles verticaux H2000 P300 36M IP-30","OM - Two Vertical Lids H2000 D300 36M IP-30","OM- PANEL LATERAL (2UDS) H2000 D300 36M IP30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2000 D300 36M IP-30"]
["00239","ZENERGY OM - DWIE POKRYWY PIONOWE H2150 D230 39M IP-30",585.4,"1-ZE-09",0.36666666666666664,4,"OM_VERTICAL_COVER","00239","SZT","85389099","27.12.40.0",null,"5901988002398","OM - Couvercle vertical H2150 39M IP-30","OM - Two Vertical Lids H2150 39M IP-30","OM- PANEL LATERAL (2UDS)  H2150 39M IP30 ","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2150 D230 39M IP-30"]
["00240","ZENERGY OM - DWIE POKRYWY PIONOWE H2150 D300 39M IP-30",678.2,"1-ZE-09",0.25,5,"OM_VERTICAL_COVER","00240","SZT","85389099","27.12.40.0",null,"5901988002404","OM - Deux couvercles verticaux H2150 P300 39M IP-30","OM - Two Vertical Lids H2150 D300 39M IP-30","OM- PANEL LATERAL (2UDS) H2150 D300 39M IP30","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2150 D300 39M IP-30"]
["00309","ZENERGY OM - DWIE POKRYWY PIONOWE H550 D230 9M IP-55",131.80000000000001,"1-ZE-09",1.6666666666666666E-2,1,"OM_VERTICAL_COVER","00209","SZT","85389099","27.12.40.0",null,"5901988003098","OM - Couvercle vertical H550 9M IP-55","OM - Two Vertical Lids H550 9M IP-55","OM- PANEL LATERAL (2UDS)  H550 9M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H550 D230 9M IP-55"]
["00310","ZENERGY OM - DWIE POKRYWY PIONOWE H550 D300 9M IP-55",152.30000000000001,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00210","SZT","85389099","27.12.40.0",null,"5901988003104","OM - Couvercle vertical H550 P300 9M IP-55","OM - Two Vertical Lids H550 D300 9M IP-55","OM- PANEL LATERAL (2UDS) H550 D300 9M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H550 D300 9M IP-55"]
["00312","ZENERGY OM - DWIE POKRYWY PIONOWE H700 D230 12M IP-55",139.30000000000001,"1-ZE-09",4.1666666666666664E-2,2,"OM_VERTICAL_COVER","00212","SZT","85389099","27.12.40.0",null,"5901988003128","OM - Couvercle vertical H700 12M IP-55","OM - Two Vertical Lids H700 12M IP-55","OM- PANEL LATERAL (2UDS)  H700 12M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H700 D230 12M IP-55"]
["00313","ZENERGY OM - DWIE POKRYWY PIONOWE H700 D300 12M IP-55",162,"1-ZE-09",3.3333333333333333E-2,1,"OM_VERTICAL_COVER","00213","SZT","85389099","27.12.40.0",null,"5901988003135","OM - Couvercle vertical H700 P300 12M IP-55","OM - Two Vertical Lids H700 D300 12M IP-55","OM- PANEL LATERAL (2UDS) H700 D300 12M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H700 D300 12M IP-55"]
["00315","ZENERGY OM - DWIE POKRYWY PIONOWE H850 D230 15M IP-55",166.3,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00215","SZT","85389099","27.12.40.0",null,"5901988003159","OM - Couvercle vertical H850 15M IP-55","OM - Two Vertical Lids H850 15M IP-55","OM- PANEL LATERAL (2UDS)  H850 15M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H850 D230 15M IP-55"]
["00316","ZENERGY OM - DWIE POKRYWY PIONOWE H850 D300 15M IP-55",192.2,"1-ZE-09",4.1666666666666664E-2,1,"OM_VERTICAL_COVER","00216","SZT","85389099","27.12.40.0",null,"5901988003166","OM - Couvercle vertical H850 P300 15M IP-55","OM - Two Vertical Lids H850 D300 15M IP-55","OM- PANEL LATERAL (2UDS) H850 D300 15M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H850 D300 15M IP-55"]
["00318","ZENERGY OM - DWIE POKRYWY PIONOWE H1000 D230 18M IP-55",186.8,"1-ZE-09",3.3333333333333333E-2,1,"OM_VERTICAL_COVER","00218","SZT","85389099","27.12.40.0",null,"5901988003180","OM - Couvercle vertical H1000 18M IP-55","OM - Two Vertical Lids H1000 18M IP-55","OM- PANEL LATERAL (2UDS)  H1000 18M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1000 D230 18M IP-55"]
["00319","ZENERGY OM - DWIE POKRYWY PIONOWE H1000 D300 18M IP-55",217.1,"1-ZE-09",1.6666666666666666E-2,2,"OM_VERTICAL_COVER","00219","SZT","85389099","27.12.40.0",null,"5901988003197","OM - Couvercle vertical H1000 P300 18M IP-55","OM - Two Vertical Lids H1000 D300 18M IP-55","OM- PANEL LATERAL (2UDS) H1000 D300 18M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1000 D300 18M IP-55"]
["00321","ZENERGY OM - DWIE POKRYWY PIONOWE H1150 D230 21M IP-55",213.8,"1-ZE-09",3.3333333333333333E-2,2,"OM_VERTICAL_COVER","00221","SZT","85389099","27.12.40.0",null,"5901988003210","OM - Couvercle vertical H1150 21M IP-55","OM - Two Vertical Lids H1150 21M IP-55","OM- PANEL LATERAL (2UDS)  H1150 21M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1150 D230 21M IP-55"]
["00322","ZENERGY OM - DWIE POKRYWY PIONOWE H1150 D300 21M IP-55",248.4,"1-ZE-09",3.3333333333333333E-2,2,"OM_VERTICAL_COVER","00222","SZT","85389099","27.12.40.0",null,"5901988003227","OM - Couvercle vertical H1150 P300 21M IP-55","OM - Two Vertical Lids H1150 D300 21M IP-55","OM- PANEL LATERAL (2UDS) H1150 D300 21M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1150 D300 21M IP-55"]
["00323","ZENERGY OM - DWIE POKRYWY PIONOWE H1300 D300 24M IP-55",274.3,"1-ZE-09",6.6666666666666666E-2,4,"OM_VERTICAL_COVER","00223","SZT","85389099","27.12.40.0",null,"5901988003234","OM - Couvercle vertical H1300 P300 24M IP-55","OM - Two Vertical Lids H1300 D300 24M IP-55","OM- PANEL LATERAL (2UDS) H1300 D300 24M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1300 D300 24M IP-55"]
["00324","ZENERGY OM - DWIE POKRYWY PIONOWE H1300 D230 24M IP-55",236.5,"1-ZE-09",4.1666666666666664E-2,2,"OM_VERTICAL_COVER","00224","SZT","85389099","27.12.40.0",null,"5901988003241","OM - Couvercle vertical H1300 24M IP-55","OM - Two Vertical Lids H1300 24M IP-55","OM- PANEL LATERAL (2UDS)  H1300 24M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1300 D230 24M IP-55"]
["00325","ZENERGY OM - DWIE POKRYWY PIONOWE H1450 D300 27M IP-55",301.3,"1-ZE-09",1.6666666666666666E-2,2,"OM_VERTICAL_COVER","00225","SZT","85389099","27.12.40.0",null,"5901988003258","OM - Couvercle vertical H1450 P300 27M IP-55","OM - Two Vertical Lids H1450 D300 27M IP-55","OM- PANEL LATERAL (2UDS) H1450 D300 27M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1450 D300 27M IP-55"]
["00326","ZENERGY OM - DWIE POKRYWY PIONOWE H1600 D300 28M IP-55",333.7,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00226","SZT","85389099","27.12.40.0",null,"5901988003265","OM - Couvercle vertical H1600 P300 28M IP-55","OM - Two Vertical Lids H1600 D300 28M IP-55","OM- PANEL LATERAL (2UDS) H1600 D300 28M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1600 D300 28M IP-55"]
["00327","ZENERGY OM - DWIE POKRYWY PIONOWE H1450 D230 27M IP-55",259.2,"1-ZE-09",3.3333333333333333E-2,1,"OM_VERTICAL_COVER","00227","SZT","85389099","27.12.40.0",null,"5901988003272","OM - Couvercle vertical H1450 27M IP-55","OM - Two Vertical Lids H1450 27M IP-55","OM- PANEL LATERAL (2UDS)  H1450 27M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1450 D230 27M IP-55"]
["00328","ZENERGY OM - DWIE POKRYWY PIONOWE H1600 D230 28M IP-55",287.3,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00227","SZT","85389099","27.12.40.0",null,"5901988003289","OM - Couvercle vertical H1600 28M IP-55","OM - Two Vertical Lids H1600 28M IP-55","OM- PANEL LATERAL (2UDS) H1600 28M IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1600 D230 28M IP-55"]
["00329","ZENERGY OM - DWIE POKRYWY PIONOWE H1550 D230 29M IP-55",311,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00229","SZT","85389099","27.12.40.0",null,"5901988003296","OM - Couvercle vertical H1550 29M IP-55","OM - Two Vertical Lids H1550 29M IP-55","OM- PANEL LATERAL (2UDS) H1550 29M IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1550 D230 29M IP-55"]
["00330","ZENERGY OM - DWIE POKRYWY PIONOWE H1700 D230 30M IP-55",372.6,"1-ZE-09",6.6666666666666666E-2,2,"OM_VERTICAL_COVER","00230","SZT","85389099","27.12.40.0",null,"5901988003302","OM - Couvercle vertical H1700 30M IP-55","OM - Two Vertical Lids H1700 30M IP-55","OM- PANEL LATERAL (2UDS)  H1700 30M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1700 D230 30M IP-55"]
["00331","ZENERGY OM - DWIE POKRYWY PIONOWE H1550 D300 29M IP-55",360.7,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00231","SZT","85389099","27.12.40.0",null,"5901988003319","OM - Couvercle vertical H1550 P300 29M IP-55","OM - Two Vertical Lids H1550 D300 29M IP-55","OM- PANEL LATERAL (2UDS) H1550 D300 29M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1550 D300 29M IP-55"]
["00332","ZENERGY OM - DWIE POKRYWY PIONOWE H1700 D300 30M IP-55",432,"1-ZE-09",1.6666666666666666E-2,2,"OM_VERTICAL_COVER","00232","SZT","85389099","27.12.40.0",null,"5901988003326","OM - Couvercle vertical H1700 P300 30M IP-55","OM - Two Vertical Lids H1700 D300 30M IP-55","OM- PANEL LATERAL (2UDS) H1700 D300 30M IP-55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1700 D300 30M IP-55"]
["00333","ZENERGY OM - DWIE POKRYWY PIONOWE H1850 D230 33M IP-55",461.2,"1-ZE-09",3.3333333333333333E-2,4,"OM_VERTICAL_COVER","00233","SZT","85389099","27.12.40.0",null,"5901988003333","OM - Couvercle vertical H1850 33M IP-55","OM - Two Vertical Lids H1850 33M IP-55","OM- PANEL LATERAL (2UDS)  H1850 33M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1850 D230 33M IP-55"]
["00334","ZENERGY OM - DWIE POKRYWY PIONOWE H1850 D300 33M IP-55",534.6,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00234","SZT","85389099","27.12.40.0",null,"5901988003340","OM - Deux couvercles verticaux H1850 P300 33M IP-55","OM - Two Vertical Lids H1850 D300 33M IP-55","OM- PANEL LATERAL (2UDS) H1850 D300 33M IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H1850 D300 33M IP-55"]
["00336","ZENERGY OM - DWIE POKRYWY PIONOWE H2000 D230 36M IP-55",516.20000000000005,"1-ZE-09",3.3333333333333333E-2,1,"OM_VERTICAL_COVER","00236","SZT","85389099","27.12.40.0",null,"5901988003364","OM - Couvercle vertical H2000 36M IP-55","OM - Two Vertical Lids H2000 36M IP-55","OM- PANEL LATERAL (2UDS)  H2000 36M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2000 D230 36M IP-55"]
["00337","ZENERGY OM - DWIE POKRYWY PIONOWE H2000 D300 36M IP-55",598.29999999999995,"1-ZE-09",0.01,1,"OM_VERTICAL_COVER","00237","SZT","85389099","27.12.40.0",null,"5901988003371","OM - Deux couvercles verticaux H2000 P300 P300 P300 36M IP-55","OM - Two Vertical Lids H2000 D300 36M IP-55","OM- PANEL LATERAL (2UDS) H2000 D300 36M IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2000 D300 36M IP-55"]
["00339","ZENERGY OM - DWIE POKRYWY PIONOWE H2150 D230 39M IP-55",619.9,"1-ZE-09",0.15833333333333333,2,"OM_VERTICAL_COVER","00239","SZT","85389099","27.12.40.0",null,"5901988003395","OM - Couvercle vertical H2150 39M IP-55","OM - Two Vertical Lids H2150 39M IP-55","OM- PANEL LATERAL (2UDS)  H2150 39M  IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2150 D230 39M IP-55"]
["00340","ZENERGY OM - DWIE POKRYWY PIONOWE H2150 D300 39M IP-55",719.3,"1-ZE-09",null,null,"OM_VERTICAL_COVER","00240","SZT","85389099","27.12.40.0",null,"5901988003401","OM - Deux couvercles verticaux H2150 P300 39M IP-55","OM - Two Vertical Lids H2150 D300 39M IP-55","OM- PANEL LATERAL (2UDS) H2150 D300 39M IP55","ZENERGY OM - KÉT FÜGGŐLEGES BURKOLAT H2150 D300 39M IP-55"]
["00409","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H550 D230 9M IP-30",127.4,"1-ZE-09",null,null,"OM_EXTENSION","00409","SZT","85389099","27.12.40.0",null,"5901988004095","OM - Extensions de couverture - H550 9M IP-30","OM - Extension Cover - H550 9M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H550 9M IP30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H550 D230 9M IP-30"]
["00410","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H550 D300 9M IP-30",148,"1-ZE-09",null,null,"OM_EXTENSION","00410","SZT","85389099","27.12.40.0",null,"5901988004101","OM - Extensions de couverture - H550 P300 9M IP-30","OM - Extension Cover - H550 D300 9M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H550 D300 9M IP-30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H550 D300 9M IP-30"]
["00412","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H700 D230 12M IP-30",135,"1-ZE-09",1.6666666666666666E-2,1,"OM_EXTENSION","00412","SZT","85389099","27.12.40.0",null,"5901988004125","OM - Couvercle de boîtier - Passe-câble H700 12M IP-30","OM - Extension Cover - H700 12M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H700 12M IP30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H700 D230 12M IP-30"]
["00413","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H700 D300 12M IP-30",156.6,"1-ZE-09",null,null,"OM_EXTENSION","00413","SZT","85389099","27.12.40.0",null,"5901988004132","OM - Extensions de couverture - H700 P300 12M IP-30","OM - Extension Cover - H700 D300 12M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H700 D300 12M IP-30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H700 D300 12M IP-30"]
["00415","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H850 D230 15M IP-30",163.1,"1-ZE-09",1.6666666666666666E-2,2,"OM_EXTENSION","00415","SZT","85389099","27.12.40.0",null,"5901988004156","OM - Extensions de couverture - Bague H850 15M IP-30","OM - Extension Cover - H850 15M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H850 15M IP30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H850 D230 15M IP-30"]
["00416","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H850 D300 15M IP-30",189,"1-ZE-09",null,null,"OM_EXTENSION","00416","SZT","85389099","27.12.40.0",null,"5901988004163","OM - Extensions de couverture - H850 P300 15M IP-30","OM - Extension Cover - H850 D300 15M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H850 D300 15M IP-30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H850 D300 15M IP-30"]
["00418","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1000 D230 18M IP-30",192.2,"1-ZE-09",0.05,2,"OM_EXTENSION","00418","SZT","85389099","27.12.40.0",null,"5901988004187","OM - Extensions de couverture - Douille H1000 18M IP-30","OM - Extension Cover - H1000 18M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1000 18M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1000 D230 18M IP-30"]
["00419","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1000 D300 18M IP-30",222.5,"1-ZE-09",0.01,1,"OM_EXTENSION","00419","SZT","85389099","27.12.40.0",null,"5901988004194","OM - Extensions de couverture - H1000 P300 18M IP-30","OM - Extension Cover - H1000 D300 18M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1000 D300 18M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1000 D300 18M IP-30"]
["00421","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1150 D230 21M IP-30",219.2,"1-ZE-09",6.6666666666666666E-2,2,"OM_EXTENSION","00421","SZT","85389099","27.12.40.0",null,"5901988004217","OM - Extensions de couverture - H1150 21M IP-30","OM - Extension Cover - H1150 21M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1150 21M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1150 D230 21M IP-30"]
["00422","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1150 D300 21M IP-30",254.9,"1-ZE-09",null,null,"OM_EXTENSION","00422","SZT","85389099","27.12.40.0",null,"5901988004224","OM - Extensions de couverture - H1150 P300 21M IP-30","OM - Extension Cover - H1150 D300 21M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1150 D300 21M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1150 D300 21M IP-30"]
["00423","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1300 D300 24M IP-30",280.8,"1-ZE-09",null,null,"OM_EXTENSION","00423","SZT","85389099","27.12.40.0",null,"5901988004231","OM - Extensions de couverture - H1300 P300 24M IP-30","OM - Extension Cover - H1300 D300 24M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1300 D300 24M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1300 D300 24M IP-30"]
["00424","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1300 D230 24M IP-30",241.9,"1-ZE-09",0.20833333333333334,5,"OM_EXTENSION","00424","SZT","85389099","27.12.40.0",null,"5901988004248","OM - Extensions de couverture - Bague H1300 24M IP-30","OM - Extension Cover - H1300 24M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1300 24M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1300 D230 24M IP-30"]
["00425","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1450 D300 27M IP-30",307.8,"1-ZE-09",null,null,"OM_EXTENSION","00425","SZT","85389099","27.12.40.0",null,"5901988004255","OM - Extensions de couverture - H1450 P300 27M IP-30","OM - Extension Cover - H1450 D300 27M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1450 D300 27M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1450 D300 27M IP-30"]
["00426","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1600 D300 28M IP-30",312.10000000000002,"1-ZE-09",null,null,"OM_EXTENSION","00426","SZT","85389099","27.12.40.0",null,"5901988004262","OM - Extensions de couverture - H1600 P300 28M IP-30","OM - Extension Cover - H1600 D300 28M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1600 D300 28M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1600 D300 28M IP-30"]
["00427","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1450 D230 27M IP-30",265.7,"1-ZE-09",5.8333333333333334E-2,1,"OM_EXTENSION","00427","SZT","85389099","27.12.40.0",null,"5901988004279","OM - Extensions de couverture - Bague H1450 27M IP-30","OM - Extension Cover - H1450 27M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1450 27M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1450 D230 27M IP-30"]
["00428","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1600 D230 28M IP-30",268.89999999999998,"1-ZE-09",0.01,1,"OM_EXTENSION","00428","SZT","85389099","27.12.40.0",null,"5901988004286","OM - Couvercle d'extension - Câbles H1600 28M IP-30","OM - Extension Cover - H1600 28M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1600 28M IP30 ","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1600 D230 28M IP-30"]
["00429","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1550 D230 29M IP-30",303.5,"1-ZE-09",null,null,"OM_EXTENSION","00429","SZT","85389099","27.12.40.0",null,"5901988004293","OM - Extensions de couverture - H1550 29M IP-30","OM - Extension Cover - H1550 29M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1550 29M IP30 ","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1550 D230 29M IP-30"]
["00430","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1700 D230 30M IP-30",340.2,"1-ZE-09",4.1666666666666664E-2,1,"OM_EXTENSION","00430","SZT","85389099","27.12.40.0",null,"5901988004309","OM - Extensions de couverture - H1700 30M IP-30","OM - Extension Cover - H1700 30M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1700 30M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1700 D230 30M IP-30"]
["00431","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1550 D300 29M IP-30",352.1,"1-ZE-09",null,null,"OM_EXTENSION","00431","SZT","85389099","27.12.40.0",null,"5901988004316","OM - Extensions de couverture - H1550 P300 29M IP-30","OM - Extension Cover - H1550 D300 29M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1550 D300 29M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1550 D300 29M IP-30"]
["00432","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1700 D300 30M IP-30",394.2,"1-ZE-09",0.01,1,"OM_EXTENSION","00432","SZT","85389099","27.12.40.0",null,"5901988004323","OM - Extensions de couverture - H1700 P300 30M IP-30","OM - Extension Cover - H1700 D300 30M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1700 D300 30M IP-30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1700 D300 30M IP-30"]
["00433","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1850 D230 33M IP-30",403.9,"1-ZE-09",0.24166666666666667,4,"OM_EXTENSION","00433","SZT","85389099","27.12.40.0",null,"5901988004330","OM - Extensions de couverture - H1850 33M IP-30","OM - Extension Cover - H1850 33M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1850 33M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1850 D230 33M IP-30"]
["00434","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1850 D300 33M IP-30",468.7,"1-ZE-09",1.6666666666666666E-2,1,"OM_EXTENSION","00434","SZT","85389099","27.12.40.0",null,"5901988004347","OM - Couvercle de rallonge - H1850 P300 33M IP-30 ponceau","OM - Extension Cover - H1850 D300 33M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H1850 D300 33M IP30 ","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1850 D300 33M IP-30"]
["00436","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2000 D230 36M IP-30",459,"1-ZE-09",0.18333333333333332,1,"OM_EXTENSION","00436","SZT","85389099","27.12.40.0",null,"5901988004361","OM - Extension de couverture - Covert H2000 36M IP-30","OM - Extension Cover - H2000 36M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H2000 36M IP30","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H2000 D230 36M IP-30"]
["00437","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2000 D300 36M IP-30",533.5,"1-ZE-09",0.01,1,"OM_EXTENSION","00437","SZT","85389099","27.12.40.0",null,"5901988004378","OM - Couvercle de rallonge - H2000 P300 36M IP-30 ponceau","OM - Extension Cover - H2000 D300 36M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H2000 D300 36M IP30 ","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H2000 D300 36M IP-30"]
["00439","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2150 D230 39M IP-30",594,"1-ZE-09",null,null,"OM_EXTENSION","00439","SZT","85389099","27.12.40.0",null,"5901988004392","OM - Extensions de couverture - Bague H2150 39M IP-30","OM - Extension Cover - H2150 39M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H2150 39M IP30","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H2150 D230 39M IP-30"]
["00440","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2150 D300 39M IP-30",689,"1-ZE-09",8.3333333333333329E-2,2,"OM_EXTENSION","00440","SZT","85389099","27.12.40.0",null,"5901988004408","OM - Couvercle de rallonge - H2150 P300 39M IP-30 ponceau","OM - Extension Cover - H2150 D300 39M IP-30 Grommet","OM- PIEZA UNION MOD. AUX. H2150 D300 39M IP30 ","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H2150 D300 39M IP-30"]
["00509","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H550 D230 9M IP-55",145.80000000000001,"1-ZE-09",null,null,"OM_EXTENSION","00409","SZT","85389099","27.12.40.0",null,"5901988005092","OM - Extensions de couverture - H550 9M IP-55","OM - Extension Cover - H550 9M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H550 9M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H550 D230 9M IP-55"]
["00510","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H550 D300 9M IP-55",168.5,"1-ZE-09",null,null,"OM_EXTENSION","00410","SZT","85389099","27.12.40.0",null,"5901988005108","OM - Extensions de couverture - H550 P300 9M IP-55","OM - Extension Cover - H550 D300 9M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H550 D300 9M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H550 D300 9M IP-55"]
["00512","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H700 D230 12M IP-55",157.69999999999999,"1-ZE-09",null,null,"OM_EXTENSION","00412","SZT","85389099","27.12.40.0",null,"5901988005122","OM - Couvercle de boîtier - Passe-câble H700 12M IP-55","OM - Extension Cover - H700 12M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H700 12M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H700 D230 12M IP-55"]
["00513","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H700 D300 12M IP-55",182.5,"1-ZE-09",null,null,"OM_EXTENSION","00413","SZT","85389099","27.12.40.0",null,"5901988005139","OM - Extensions de couverture - H700 P300 12M IP-55","OM - Extension Cover - H700 D300 12M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H700 D300 12M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H700 D300 12M IP-55"]
["00515","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H850 D230 15M IP-55",187.9,"1-ZE-09",null,null,"OM_EXTENSION","00415","SZT","85389099","27.12.40.0",null,"5901988005153","OM - Extensions de couverture - H850 15M IP-55","OM - Extension Cover - H850 15M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H850 15M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H850 D230 15M IP-55"]
["00516","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H850 D300 15M IP-55",218.2,"1-ZE-09",null,null,"OM_EXTENSION","00416","SZT","85389099","27.12.40.0",null,"5901988005160","OM - Extensions de couverture - H850 P300 15M IP-55","OM - Extension Cover - H850 D300 15M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H850 D300 15M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H850 D300 15M IP-55"]
["00518","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1000 D230 18M IP-55",212.8,"1-ZE-09",null,null,"OM_EXTENSION","00418","SZT","85389099","27.12.40.0",null,"5901988005184","OM - Couvercle de boîtier - Drainage H1000 18M IP-55","OM - Extension Cover - H1000 18M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1000 18M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1000 D230 18M IP-55"]
["00519","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1000 D300 18M IP-55",247.3,"1-ZE-09",null,null,"OM_EXTENSION","00419","SZT","85389099","27.12.40.0",null,"5901988005191","OM - Extensions de couverture - H1000 P300 18M IP-55","OM - Extension Cover - H1000 D300 18M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1000 D300 18M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1000 D300 18M IP-55"]
["00521","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1150 D230 21M IP-55",244.1,"1-ZE-09",null,null,"OM_EXTENSION","00421","SZT","85389099","27.12.40.0",null,"5901988005214","OM - Extensions de couverture - H1150 21M IP-55","OM - Extension Cover - H1150 21M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1150 21M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1150 D230 21M IP-55"]
["00522","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1150 D300 21M IP-55",283,"1-ZE-09",null,null,"OM_EXTENSION","00422","SZT","85389099","27.12.40.0",null,"5901988005221","OM - Extensions de couverture - H1150 P300 21M IP-55","OM - Extension Cover - H1150 D300 21M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1150 D300 21M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1150 D300 21M IP-55"]
["00523","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1300 D300 24M IP-55",313.2,"1-ZE-09",null,null,"OM_EXTENSION","00423","SZT","85389099","27.12.40.0",null,"5901988005238","OM - Extensions de couverture - H1300 P300 24M IP-55","OM - Extension Cover - H1300 D300 24M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1300 D300 24M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1300 D300 24M IP-55"]
["00524","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1300 D230 24M IP-55",270,"1-ZE-09",1.6666666666666666E-2,1,"OM_EXTENSION","00424","SZT","85389099","27.12.40.0",null,"5901988005245","OM - Couvercle d'extension - Drainage H1300 24M IP-55","OM - Extension Cover - H1300 24M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1300 24M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1300 D230 24M IP-55"]
["00525","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1450 D300 27M IP-55",344.5,"1-ZE-09",null,null,"OM_EXTENSION","00425","SZT","85389099","27.12.40.0",null,"5901988005252","OM - Extensions de couverture - H1450 P300 27M IP-55","OM - Extension Cover - H1450 D300 27M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1450 D300 27M IP-55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1450 D300 27M IP-55"]
["00526","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1600 D300 28M IP-55",346.7,"1-ZE-09",null,null,"OM_EXTENSION","00426","SZT","85389099","27.12.40.0",null,"5901988005269","OM - Extensions de couverture - H1600 P300 28M IP-55","OM - Extension Cover - H1600 D300 28M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1600 D300 28M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1600 D300 28M IP-55"]
["00527","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1450 D230 27M IP-55",297,"1-ZE-09",0.01,1,"OM_EXTENSION","00427","SZT","85389099","27.12.40.0",null,"5901988005276","OM - Extensions de couverture - H1450 27M IP-55","OM - Extension Cover - H1450 27M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1450 27M IP55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1450 D230 27M IP-55"]
["00528","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1600 D230 28M IP-55",298.10000000000002,"1-ZE-09",null,null,"OM_EXTENSION","00428","SZT","85389099","27.12.40.0",null,"5901988005283","OM - Couvercle d'extension - Drainage H1600 28M IP-55","OM - Extension Cover - H1600 28M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1600 28M IP55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1600 D230 28M IP-55"]
["00529","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1550 D230 29M IP-55",338,"1-ZE-09",null,null,"OM_EXTENSION","00429","SZT","85389099","27.12.40.0",null,"5901988005290","OM - Extensions de couverture - H1550 29M IP-55","OM - Extension Cover - H1550 29M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1550 29M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1550 D230 29M IP-55"]
["00530","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1700 D230 30M IP-55",378,"1-ZE-09",null,null,"OM_EXTENSION","00430","SZT","85389099","27.12.40.0",null,"5901988005306","OM - Extensions de couverture - H1700 30M IP-55","OM - Extension Cover - H1700 30M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1700 30M IP55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1700 D230 30M IP-55"]
["00531","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1550 D300 29M IP-55",392,"1-ZE-09",null,null,"OM_EXTENSION","00431","SZT","85389099","27.12.40.0",null,"5901988005313","OM - Extensions de couverture - H1550 P300 29M IP-55","OM - Extension Cover - H1550 D300 29M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1550 D300 29M IP-55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H1550 D300 29M IP-55"]
["00532","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1700 D300 30M IP-55",438.5,"1-ZE-09",0.01,1,"OM_EXTENSION","00432","SZT","85389099","27.12.40.0",null,"5901988005320","OM - Extensions de couverture - H1700 P300 30M IP-55","OM - Extension Cover - H1700 D300 30M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1700 D300 30M IP-55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1700 D300 30M IP-55"]
["00533","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1850 D230 33M IP-55",449.3,"1-ZE-09",null,null,"OM_EXTENSION","00433","SZT","85389099","27.12.40.0",null,"5901988005337","OM - Extensions de couverture - H1850 33M IP-55","OM - Extension Cover - H1850 33M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1850 33M IP55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H1850 D230 33M IP-55"]
["00534","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H1850 D300 33M IP-55",520.6,"1-ZE-09",null,null,"OM_EXTENSION","00434","SZT","85389099","27.12.40.0",null,"5901988005344","OM - Couvercle de rallonge - H1850 P300 33M IP-55 ponceau","OM - Extension Cover - H1850 D300 33M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H1850 D300 33M IP55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLATA - BULLET H1850 D300 33M IP-55"]
["00536","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2000 D230 36M IP-55",509.8,"1-ZE-09",3.3333333333333333E-2,1,"OM_EXTENSION","00436","SZT","85389099","27.12.40.0",null,"5901988005368","OM - Extension de couverture - Covert H2000 36M IP-55","OM - Extension Cover - H2000 36M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H2000 36M IP55","ZENERGY OM - KIEGÉSZÍTŐ BURKOLAT - BULLET H2000 D230 36M IP-55"]
["00537","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2000 D300 36M IP-55",591.79999999999995,"1-ZE-09",0.01,1,"OM_EXTENSION","00437","SZT","85389099","27.12.40.0",null,"5901988005375","OM - Couvercle de rallonge - H2000 P300 36M IP-55 ponceau","OM - Extension Cover - H2000 D300 36M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H2000 D300 36M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H2000 D300 36M IP-55"]
["00539","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2150 D230 39M IP-55",659.9,"1-ZE-09",null,null,"OM_EXTENSION","00439","SZT","85389099","27.12.40.0",null,"5901988005399","OM - Extensions de couverture - H2150 39M IP-55","OM - Extension Cover - H2150 39M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H2150 39M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H2150 D230 39M IP-55"]
["00540","ZENERGY OM - POKRYWA ROZSZERZENIA - PRZEPUST H2150 D300 39M IP-55",765.7,"1-ZE-09",null,null,"OM_EXTENSION","00440","SZT","85389099","27.12.40.0",null,"5901988005405","OM - Couvercle de rallonge - H2150 P300 39M ponceau IP-55","OM - Extension Cover - H2150 D300 39M IP-55 Grommet","OM- PIEZA UNION MOD. AUX. H2150 D300 39M IP55","ZENERGY OM - HOSSZABBÍTÓ BURKOLAT - BULLET H2150 D300 39M IP-55"]
["00609","ZENERGY OM - SŁUPEK ŚRODKOWY H550 9M IP-30",28.3,"1-ZE-09",null,null,"OM_EXTENSION","00609","SZT","85389099","27.12.40.0",null,"5901988006099","OM - Poteau central H550 9M IP-30","OM - Middle post H550 9M IP-30","OM- POSTE MEDIO H550 9M IP30","ZENERGY OM - CENTER POST H550 9M IP-30"]
["00612","ZENERGY OM - SŁUPEK ŚRODKOWY H700 12M IP-30",29.3,"1-ZE-09",null,null,"OM_EXTENSION","00612","SZT","85389099","27.12.40.0",null,"5901988006129","OM - Poteau central H700 12M IP-30","OM - Central post H700 12M IP-30","OM- POSTE MEDIO H700 12M IP30","ZENERGY OM - CENTER POST H700 12M IP-30"]
["00615","ZENERGY OM - SŁUPEK ŚRODKOWY H850 15M IP-30",35.299999999999997,"1-ZE-09",null,null,"OM_EXTENSION","00615","SZT","85389099","27.12.40.0",null,"5901988006150","OM - Poteau central H850 15M IP-30","OM - Central post H850 15M IP-30","OM- POSTE CENTRAL H850 15M IP30","ZENERGY OM - CENTER POST H850 15M IP-30"]
["00618","ZENERGY OM - SŁUPEK ŚRODKOWY H1000 18M IP-30",41.1,"1-ZE-09",0.01,1,"OM_EXTENSION","00618","SZT","85389099","27.12.40.0",null,"5901988006181","OM - Pilier moyen H1000 18M IP-30","OM - Middle post H1000 18M IP-30","OM- POSTE CENTRAL H1000 18M IP30","ZENERGY OM - CENTER POST H1000 18M IP-30"]
["00621","ZENERGY OM - SŁUPEK ŚRODKOWY H1150 21M IP-30",47.1,"1-ZE-09",1.6666666666666666E-2,1,"OM_EXTENSION","00621","SZT","85389099","27.12.40.0",null,"5901988006211","OM - Poteau central H1150 21M IP-30","OM - Central post H1150 21M IP-30","OM- POSTE CENTRAL H1150 21M IP30","ZENERGY OM - CENTER POST H1150 21M IP-30"]
["00624","ZENERGY OM - SŁUPEK ŚRODKOWY H1300 24M IP-30",51.5,"1-ZE-09",0.01,1,"OM_EXTENSION","00624","SZT","85389099","27.12.40.0",null,"5901988006242","OM - Poteau central H1300 24M IP-30","OM - Central post H1300 24M IP-30","OM- POSTE CENTRAL H1300 24M IP30","ZENERGY OM - CENTER POST H1300 24M IP-30"]
["00627","ZENERGY OM - SŁUPEK ŚRODKOWY H1450 27M IP-30",56.3,"1-ZE-09",null,null,"OM_EXTENSION","00627","SZT","85389099","27.12.40.0",null,"5901988006273","OM - Poteau central H1450 27M IP-30","OM - Central post H1450 27M IP-30","OM- POSTE CENTRAL H1450 27M IP30","ZENERGY OM - CENTER POST H1450 27M IP-30"]
["00628","ZENERGY OM - SŁUPEK ŚRODKOWY H1600 28M IP-30",62.6,"1-ZE-09",null,null,"OM_EXTENSION","00628","SZT","85389099","27.12.40.0",null,"5901988006280","OM - Poteau central H1600 28M IP-30","OM - Middle post H1600 28M IP-30","OM- POSTE CENTRAL H1600 28M IP30","ZENERGY OM - CENTER POST H1600 28M IP-30"]
["00629","ZENERGY OM - SŁUPEK ŚRODKOWY H1550 29M IP-30",66,"1-ZE-09",null,null,"OM_EXTENSION","00629","SZT","85389099","27.12.40.0",null,"5901988006297","OM - Poteau central H1550 29M IP-30","OM - Central post H1550 29M IP-30","OM- POSTE CENTRAL H1550 29M IP30","ZENERGY OM - CENTER POST H1550 29M IP-30"]
["00630","ZENERGY OM - SŁUPEK ŚRODKOWY H1700 30M IP-30",84.3,"1-ZE-09",0.01,1,"OM_EXTENSION","00630","SZT","85389099","27.12.40.0",null,"5901988006303","OM - Poteau central H1700 30M IP-30","OM - Middle post H1700 30M IP-30","OM- POSTE CENTRAL H1700 30M IP30","ZENERGY OM - CENTER POST H1700 30M IP-30"]
["00633","ZENERGY OM - SŁUPEK ŚRODKOWY H1850 33M IP-30",108.9,"1-ZE-09",0.28333333333333333,4,"OM_EXTENSION","00633","SZT","85389099","27.12.40.0",null,"5901988006334","OM - Poteau central H1850 33M IP-30","OM - Central post H1850 33M IP-30","OM- POSTE CENTRAL H1850 33M IP30","ZENERGY OM - CENTER POST H1850 33M IP-30"]
["00636","ZENERGY OM - SŁUPEK ŚRODKOWY H2000 36M IP-30",119.9,"1-ZE-09",8.3333333333333329E-2,2,"OM_EXTENSION","00636","SZT","85389099","27.12.40.0",null,"5901988006365","OM - Pilier moyen H2000 36M IP-30","OM - Central post H2000 36M IP-30","OM- POSTE CENTRAL H2000 36M IP30","ZENERGY OM - CENTER POST H2000 36M IP-30"]
["00639","ZENERGY OM - SŁUPEK ŚRODKOWY H2150 39M IP-30",146.9,"1-ZE-09",0.18333333333333332,2,"OM_EXTENSION","00639","SZT","85389099","27.12.40.0",null,"5901988006396","OM - Poteau central H2150 39M IP-30","OM - Central post H2150 39M IP-30","OM- POSTE CENTRAL H2150 39M IP30","ZENERGY OM - CENTER POST H2150 39M IP-30"]
["00709","ZENERGY OM - SŁUPEK ŚRODKOWY H550 9M IP-55",46.7,"1-ZE-09",null,null,"OM_EXTENSION","00609","SZT","85389099","27.12.40.0",null,"5901988007096","OM - Pilier moyen H550 9M IP-55","OM - Middle post H550 9M IP-55","OM- POSTE CENTRAL H550 9M IP55","ZENERGY OM - CENTER POST H550 9M IP-55"]
["00712","ZENERGY OM - SŁUPEK ŚRODKOWY H700 12M IP-55",49.7,"1-ZE-09",null,null,"OM_EXTENSION","00612","SZT","85389099","27.12.40.0",null,"5901988007126","OM - Poteau central H700 12M IP-55","OM - Central post H700 12M IP-55","OM- POSTE CENTRAL H700 12M IP55","ZENERGY OM - CENTER POST H700 12M IP-55"]
["00715","ZENERGY OM - SŁUPEK ŚRODKOWY H850 15M IP-55",59.1,"1-ZE-09",null,null,"OM_EXTENSION","00615","SZT","85389099","27.12.40.0",null,"5901988007157","OM - Poteau central H850 15M IP-55","OM - Middle post H850 15M IP-55","OM- POSTE CENTRAL H850 15M IP55","ZENERGY OM - CENTER POST H850 15M IP-55"]
["00718","ZENERGY OM - SŁUPEK ŚRODKOWY H1000 18M IP-55",66.7,"1-ZE-09",null,null,"OM_EXTENSION","00618","SZT","85389099","27.12.40.0",null,"5901988007188","OM - Poteau central H1000 18M IP-55","OM - Central post H1000 18M IP-55","OM- POSTE CENTRAL H1000 18M IP55","ZENERGY OM - CENTER POST H1000 18M IP-55"]
["00721","ZENERGY OM - SŁUPEK ŚRODKOWY H1150 21M IP-55",76.5,"1-ZE-09",null,null,"OM_EXTENSION","00621","SZT","85389099","27.12.40.0",null,"5901988007218","OM - Poteau central H1150 21M IP-55","OM - Central post H1150 21M IP-55","OM- POSTE CENTRAL H1150 21M IP55","ZENERGY OM - CENTER POST H1150 21M IP-55"]
["00724","ZENERGY OM - SŁUPEK ŚRODKOWY H1300 24M IP-55",84.2,"1-ZE-09",0.01,1,"OM_EXTENSION","00624","SZT","85389099","27.12.40.0",null,"5901988007249","OM - Poteau central H1300 24M IP-55","OM - Central post H1300 24M IP-55","OM- POSTE CENTRAL H1300 24M IP55","ZENERGY OM - CENTER POST H1300 24M IP-55"]
["00727","ZENERGY OM - SŁUPEK ŚRODKOWY H1450 27M IP-55",92.6,"1-ZE-09",null,null,"OM_EXTENSION","00627","SZT","85389099","27.12.40.0",null,"5901988007270","OM - Poteau central H1450 27M IP-55","OM - Central post H1450 27M IP-55","OM- POSTE CENTRAL H1450 27M IP55","ZENERGY OM - CENTER POST H1450 27M IP-55"]
["00728","ZENERGY OM - SŁUPEK ŚRODKOWY H1600 28M IP-55",102.5,"1-ZE-09",null,null,"OM_EXTENSION","00628","SZT","85389099","27.12.40.0",null,"5901988007287","OM - Poteau central H1600 28M IP-55","OM - Central post H1600 28M IP-55","OM- POSTE CENTRAL H1600 28M IP55","ZENERGY OM - CENTER POST H1600 28M IP-55"]
["00729","ZENERGY OM - SŁUPEK ŚRODKOWY H1550 29M IP-55",106.9,"1-ZE-09",null,null,"OM_EXTENSION","00629","SZT","85389099","27.12.40.0",null,"5901988007294","OM - Poteau central H1550 29M IP-55","OM - Central post H1550 29M IP-55","OM- POSTE CENTRAL H1550 29M IP55","ZENERGY OM - CENTER POST H1550 29M IP-55"]
["00730","ZENERGY OM - SŁUPEK ŚRODKOWY H1700 30M IP-55",132.80000000000001,"1-ZE-09",0.01,1,"OM_EXTENSION","00630","SZT","85389099","27.12.40.0",null,"5901988007300","OM - Poteau central H1700 30M IP-55","OM - Central post H1700 30M IP-55","OM- POSTE CENTRAL H1700 30M IP55","ZENERGY OM - CENTER POST H1700 30M IP-55"]
["00733","ZENERGY OM - SŁUPEK ŚRODKOWY H1850 33M IP-55",164.2,"1-ZE-09",null,null,"OM_EXTENSION","00633","SZT","85389099","27.12.40.0",null,"5901988007331","OM - Poteau central H1850 33M IP-55","OM - Central post H1850 33M IP-55","OM- POSTE CENTRAL H1850 33M IP55","ZENERGY OM - CENTER POST H1850 33M IP-55"]
["00736","ZENERGY OM - SŁUPEK ŚRODKOWY H2000 36M IP-55",184.7,"1-ZE-09",0.01,1,"OM_EXTENSION","00636","SZT","85389099","27.12.40.0",null,"5901988007362","OM - Pilier moyen H2000 36M IP-55","OM - Central post H2000 36M IP-55","OM- POSTE CENTRAL H2000 36M IP55","ZENERGY OM - CENTER POST H2000 36M IP-55"]
["00739","ZENERGY OM - SŁUPEK ŚRODKOWY H2150 39M IP-55",221.4,"1-ZE-09",0.11666666666666667,1,"OM_EXTENSION","00639","SZT","85389099","27.12.40.0",null,"5901988007393","OM - Poteau central H2150 39M IP-55","OM - Central post H2150 39M IP-55","OM- POSTE CENTRAL H2150 39M IP55","ZENERGY OM - CENTER POST H2150 39M IP-55"]
["00806","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H400 6M IP-30",120.8,"1-ZE-03",3.3333333333333333E-2,4,"ON_VERTICAL_COVER","00806","SZT","85389099",null,null,"5901988008062","ON - Deux couvercles verticaux D205 H400 6M IP-30","ON - Two Vertical Lids D205 H400 6M IP-30","ON- PANEL LATERAL (2UDS) D205 H400 6M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H400 6M IP-30"]
["00808","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H400 6M IP-30",139.9,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00808","SZT","85389099",null,null,"5901988008086","ON - Couvercle d'extension verticale - ravine D205 H400 6M IP-30","ON - Vertical Extension Cover - D205 H400 6M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. VERTIC.- D205 H400 6M IP30 PASACABLES","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET D205 H400 6M IP-30"]
["00809","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H550 9M IP-30",127.2,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00809","SZT","85389099",null,null,"5901988008093","ON - Deux couvercles verticaux D205 H550 9M IP-30","ON - Two Vertical Lids D205 H550 9M IP-30","ON- PANEL LATERAL (2UDS) D205 H550 9M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H550 9M IP-30"]
["00811","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H550 9M IP-30",146.30000000000001,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00811","SZT","85389099",null,null,"5901988008116","ON - Cache d'extension verticale - D205 H550 9M IP-30","ON - Vertical Extension Cover - D205 H550 9M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. VERTIC.- D205 H550 9M IP30 PASACABLES","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET D205 H550 9M IP-30"]
["00812","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H700 12M IP-30",131.4,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00812","SZT","85389099",null,null,"5901988008123","ON - Deux couvercles verticaux D205 H700 12M IP-30","ON - Two Vertical Lids D205 H700 12M IP-30","ON- PANEL LATERAL (2UDS) D205 H700 12M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H700 12M IP-30"]
["00814","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H700 12M IP-30",153.69999999999999,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00814","SZT","85389099",null,null,"5901988008147","ON - Couvercle d'extension verticale - Gully D205 H700 12M IP-30","ON - Vertical Extension Cover - D205 H700 12M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. VERTIC.- D205 H700 12M IP30 PASACABLES","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET D205 H700 12M IP-30"]
["00815","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H850 15M IP-30",139.9,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00815","SZT","85389099",null,null,"5901988008154","ON - Deux couvercles verticaux D205 H850 15M IP-30","ON - Two Vertical Lids D205 H850 15M IP-30","ON- PANEL LATERAL (2UDS) D205 H850 15M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H850 15M IP-30"]
["00817","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H850 15M IP-30",186.6,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00817","SZT","85389099",null,null,"5901988008178","ON - Couvercle d'extension verticale - bague D205 H850 15M IP-30","ON - Vertical Extension Cover - D205 H850 15M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. VERTIC.- D205 H850 15M IP30 PASACABLES","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET D205 H850 15M IP-30"]
["00818","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H1000 18M IP-30",143.1,"1-ZE-03",1.6666666666666666E-2,2,"ON_VERTICAL_COVER","00818","SZT","85389099",null,null,"5901988008185","ON - Deux couvercles verticaux D205 H1000 18M IP-30","ON - Two Vertical Lids D205 H1000 18M IP-30","ON- PANEL LATERAL (2UDS) D205 H1000 18M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H1000 18M IP-30"]
["00820","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H1000 18M IP-30",219.4,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00820","SZT","85389099",null,null,"5901988008208","ON - Couvercle de rallonge vertical - bague D205 H1000 18M IP-30","ON - Vertical Extension Cover - D205 H1000 18M IP-30 Grommet","ON- PIEZA UNION MOD. AUX. VERTIC.- D205 H1000 18M IP30 PASACABLES","ZENERGY ON – FÜGGŐLEGES KIBOCSÁTÓ BURKOLAT – BULLET D205 H1000 18M IP-30"]
["00821","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H1150 21M IP-30",147.30000000000001,"1-ZE-03",0.01,1,"ON_VERTICAL_COVER","00821","SZT","85389099",null,null,"5901988008215","ON - Deux couvercles verticaux D205 H1150 21M IP-30","ON - Two Vertical Lids D205 H1150 21M IP-30","ON- PANEL LATERAL (2UDS) D205 H1150 21M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H1150 21M IP-30"]
["00823","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H1150 21M IP-30",251.2,"1-ZE-03",0.01,1,"ON_VERTICAL_COVER","00823","SZT","85389099",null,null,"5901988008239","ON - Couvercle d'extension verticale - Câbles D205 H1150 21M IP-30","ON - Vertical Extension Cover - D205 H1150 21M IP-30 Grommet","ON- TECHO DE MODULO AUX. VERTIC.- D205 H1150 21M IP30 ","ZENERGY ON – FÜGGŐLEGES KIBOCSÁTÓ BURKOLAT – BULLET D205 H1150 21M IP-30"]
["00824","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H1300 24M IP-30",216.2,"1-ZE-03",0.01,1,"ON_VERTICAL_COVER","00824","SZT","85389099",null,null,"5901988008246","ON - Deux couvercles verticaux D205 H1300 24M IP-30","ON - Two Vertical Lids D205 H1300 24M IP-30","ON- PANEL LATERAL (2UDS) D205 H1300 24M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H1300 24M IP-30"]
["00826","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H1300 24M IP-30",276.7,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00826","SZT","85389099",null,null,"5901988008260","ON - Couvercle d'extension verticale - bague D205 H1300 24M IP-30","ON - Vertical Extension Cover - D205 H1300 24M IP-30 Grommet","ON- TECHO DE MODULO AUX. VERTIC.- D205 H1300 24M IP30 PASACABLES","ZENERGY ON - FÜGGŐLEGES BŐVÍTŐ BURKOLAT - BULLET D205 H1300 24M IP-30"]
["00827","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H1450 27M IP-30",221.5,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00827","SZT","85389099",null,null,"5901988008277","ON - Deux couvercles verticaux D205 H1450 27M IP-30","ON - Two Vertical Lids D205 H1450 27M IP-30","OM- PANEL LATERAL (2UDS)  H1450 27M IP30 ","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H1450 27M IP-30"]
["00829","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H1450 27M IP-30",303.2,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00829","SZT","85389099",null,null,"5901988008291","ON - Couvercle d'extension verticale - bague D205 H1450 27M IP-30","ON - Vertical Extension Cover - D205 H1450 27M IP-30 Grommet","ON- TECHO DE MODULO AUX. VERTIC.- D205 H1450 27M IP30 PASACABLES","ZENERGY ON - FÜGGŐLEGES BŐVÍTŐ BURKOLAT - BULLET D205 H1450 27M IP-30"]
["00830","ZENERGY ON - DWIE POKRYWY PIONOWE D205 H1600 30M IP-30",368.9,"1-ZE-03",6.6666666666666666E-2,2,"ON_VERTICAL_COVER","00830","SZT","85389099",null,null,"5901988008307","ON - Deux couvercles verticaux D205 H1600 30M IP-30","ON - Two Vertical Lids D205 H1600 30M IP-30","ON- PANEL LATERAL (2UDS) D205 H1600 30M IP30","ZENERGY ON - KÉT FÜGGŐLEGES BURKOLAT D205 H1600 30M IP-30"]
["00832","ZENERGY ON - POKRYWA PIONOWA ROZSZERZENIA - PRZEPUST D205 H1600 30M IP-30",389,"1-ZE-03",null,null,"ON_VERTICAL_COVER","00832","SZT","85389099",null,null,"5901988008321","ON - Couvercle d'extension verticale - Goulotte D205 H1600 30M IP-30","ON - Vertical Extension Cover - D205 H1600 30M IP-30 Grommet","ON- TECHO DE MODULO AUX. VERTIC.- D205 H1600 30M IP30 PASACABLES","ZENERGY ON – FÜGGŐLEGES BŐVÍTŐ BURKOLAT – BULLET D205 H1600 30M IP-30"]
["01000","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, W650 - PODSTAWA",83.3,"1-ZE-10",2.0333333333333332,8,"POWER_QUALITY",null,"SZT","85389099",null,"171019LK","5901988010003","OE - Batterie plug-in, panneau de droite, P600, L650 - support","OE - Plug-in battery, right panel, D600, W650 - base","*OE- Batería enchufable, panel derecho, D600, W650 - base","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, W650 - ALAP"]
["01001","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600,W650, PRZEGRODA DŁUGA PRAWA",21.8,"1-ZE-10",2.1,11,"POWER_QUALITY",null,"SZT","85389099",null,"171019LK","5901988010010","OE - Batterie plug-in, panneau de droite, P600, L650, long mur, droite","OE - Plug-in battery, right panel, D600, W650, long right drawer","*OE- Batería enchufable, panel derecho, D600, W650, partición derecha larga","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, JOBB PANEL, D600,W650, HOSSZÚ REKESZ JOBB"]
["01002","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, MOCOWANIE UCHWYTU ZŁĄCZEK - PUSZKA",80.900000000000006,"1-ZE-10",2.3416666666666668,11,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010027","OE - Batterie plug-in, panneau de droite, P600, fixation du support de connecteur - possible","OE - Plug-in battery, right panel, D600, fastening of the connector holder - box","*OE- Batería enchufable, panel derecho, D600, fijación del soporte del conector - puede","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, CSATLAKOZÓKANULCS RÖGZÍTÉS - DOBOZ"]
["01003","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, PROWADNICA PRAWA WYSOKA",31,"1-ZE-10",2.0083333333333333,10,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010034","OE - Batterie plug-in, panneau de droite, P600, rail supérieur droit","OE - Plug-in battery, right panel, D600, high right guide","*OE- Batería enchufable, panel derecho, D600, guía superior derecha","ZENERGY – DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, JOBB MAGAS ÚTMUTATÓ"]
["01004","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, PROWADNICA LEWA NISKA",18.399999999999999,"1-ZE-10",2,8,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010041","OE - Batterie enfichable, panneau de droite, P600, guide de gauche","OE - Plug-in battery, right panel, D600, low guide rail","*OE- Batería enchufable, panel derecho, D600, guía baja izquierda","ZENERGY – DUGATTHATÓ AKKUMULÁTOR, JOBB PANEL, D600, BAL ALSÓ ÚTMUTATÓ"]
["01005","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600,W650 - PODSTAWA",83.3,"1-ZE-10",2.0166666666666666,10,"POWER_QUALITY","01005","SZT","85389099",null,"171019LK","5901988010058","OE - Batterie plug-in, panneau gauche, P600, L650 - support","OE - Plug-in battery, left panel, D600, W650 - base","OE- BATERÍA ENCHUFABLE, PANEL IZQUIERDO, D600, W650- BASE","ZENERGY - DUGATOZÓ AKKUMULÁTOR, BAL PANEL, D600,W650 - ALAP"]
["01006","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600,W650, PRZEGRODA DŁUGA LEWA",21.8,"1-ZE-10",1.5583333333333333,8,"POWER_QUALITY",null,"SZT","85389099",null,"171019LK","5901988010065","OE - Batterie plug-in, panneau gauche, P600, L650, long mur gauche","OE - Plug-in battery, left panel, D600, W650, long left divider","*OE- Batería enchufable, panel izquierdo, D600, W650, partición izquierda larga","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600,W650, HOSSZÚ REKESZ BAL"]
["01007","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, MOCOWANIE UCHWYTU ZŁĄCZEK - PUSZKA",80.900000000000006,"1-ZE-10",1.9083333333333334,10,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010072","OE - Batterie plug-in, panneau gauche, P600, fixation du support de connecteur - possible","OE - Plug-in battery, left panel, D600, fastening of the connector holder - box","*OE- Batería enchufable, panel izquierdo, D600, fijación del soporte del conector - can","ZENERGY - DUGATOZÓ AKKUMULÁTOR, BAL PANEL, D600, CSATLAKOZÓKANULCS RÖGZÍTÉS - DOBOZ"]
["01008","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, PROWADNICA LEWA WYSOKA",31,"1-ZE-10",1.75,10,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010089","OE - Batterie plug-in, panneau gauche, P600, rail supérieur gauche","OE - Plug-in battery, left panel, D600, high left guide","*OE- Batería enchufable, panel izquierdo, D600, guía alta izquierda","ZENERGY – DUGATTHATÓ AKKUMULÁTOR, BAL PANEL, D600, MAGAS BAL ÚTMUTATÓ"]
["01009","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, PROWADNICA PRAWA NISKA",18.399999999999999,"1-ZE-10",1.75,10,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010096","OE - Batterie plug-in, panneau gauche, P600, rail inférieur droit","OE - Plug-in battery, left panel, D600, right guide, low","*OE- Batería enchufable, panel izquierdo, D600, guía baja derecha","ZENERGY – DUGATTHATÓ AKKUMULÁTOR, BAL PANEL, D600, JOBB ALSÓ ÚTMUTATÓ"]
["01010","ZENERGY - BATERIA WTYKOWA, WSPORNIK DO SZYNY ALU TS-35 (170MM), PRAWY",3.6,"1-ZE-10",1.1916666666666667,7,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010102","OE - Batterie rechargeable, support de rail TS-35 (170mm), droite","OE - Plug-in battery, bracket for alu TS-35 rail (170mm), Right","*OE- Batería enchufable, soporte para riel de aluminio TS-35 (170 mm), derecha","ZENERGY - DUGATOZÓ AKKUMULÁTOR, TÁMOGATÁS AZ ALU TS-35 SÍNHOZ (170MM), JOBB"]
["01011","ZENERGY - BATERIA WTYKOWA,OSŁONA WENTYLATORA",9.1,"1-ZE-10",4.0166666666666666,12,"POWER_QUALITY",null,"SZT","85389099",null,"171023LK","5901988010119","OE - Batterie rechargeable, Couvercle de ventilateur","OE - Plug-in battery, Fan cover","*OE- Batería enchufable, tapa del ventilador","ZENERGY - DUGATÓ AKKUMULÁTOR, VENTILÁTORBURKOLAT"]
["01013","ZENERGY - BATERIA WTYKOWA,WSPORNIK DO SZYNY ALU TS-35 (170MM), LEWY",3.6,"1-ZE-10",1.2083333333333333,7,"POWER_QUALITY",null,"SZT","85389099",null,"180123PK","5901988010133","OE - Batterie plug-in, support de rail TS-35 (170mm), gauche","OE - Plug-in battery, bracket for alu TS-35 rail (170mm), Left","*OE- Batería enchufable, soporte para riel de aluminio TS-35 (170 mm), izquierda","ZENERGY - DUGATOZÓ AKKUMULÁTOR, TÁMOGATÁS AZ ALU TS-35 SÍNHOZ (170MM), BAL"]
["01014","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, PŁYTA EFEN 160 + WSPORNIK",11.9,"1-ZE-10",0.66666666666666663,6,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010140","OE - Batterie plug-in, panneau de droite, P600, carte mère EFEN 160 + support","OE - Plug-in battery, right panel, D600, EFEN 160 board + bracket","*OE- Batería enchufable, panel derecho, D600, placa EFEN 160 + soporte","ZENERGY - DUGATÓ AKKUMULÁTOR, JOBB PANEL, D600, EFEN 160 LEMEZ + KONZER"]
["01015","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, OSŁONA CZOŁOWA FUPACT 00, 5M / 500",67,"1-ZE-10",0.95833333333333337,6,"00_OTHERS","01015","SZT","85389099",null,null,"5901988010157","OE - Batterie plug-in, panneau droit, P600, capot avant Fupact 00, 5M / 500","OE - Plug-in Battery, Right Panel, D600, Fupact 00 Front cover, 5M / 500","OE- BATERÍA ENCHUFABLE, PANEL DERECHO, D600, TAPA TROQ.  ","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, FUPACT 00 ELSŐ BURKOLAT, 5M / 500"]
["01019","ZENERGY - BATERIA WTYKOWA, UCHWYT ZŁĄCZEK 25-50A - GRZEBIEŃ MAŁY -  OBUDOWA",3.6,"1-ZE-10",0.83333333333333337,7,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010195","OE - Batterie embrochable, support de connecteur 25-50A - petit peigne - boîtier","OE - Plug-in battery, connector holder 25-50A - small comb - housing","*OE- Batería enchufable, soporte de conector 25-50A - peine pequeño - carcasa","ZENERGY - DUGATÓ ELEM, CSATLAKOZÓ TARTÓ 25-50A - KIS FÉSŰ - HÁZ"]
["01020","ZENERGY - BATERIA WTYKOWA, UCHWYT ZŁĄCZEK 3X82A - GRZEBIEŃ DUŻY - OBUDOWA",4.3,"1-ZE-10",3.6916666666666669,10,"OE_MCC","01020","SZT","85389099",null,"171020LK","5901988010201","OE - Batterie rechargeable, support de connecteur 3x82A - Grand peigne - Boîtier","OE - Plug-in battery, connector holder 3x82A - large comb - housing","OE- BATERÍA ENCHUFABLE, SOPORTE CONECTOR 3X82A","ZENERGY - DUGATÓ ELEM, CSATLAKOZÓTARTÓ 3X82A - NAGY FÉSŰ - HÁZ"]
["01021","ZENERGY - BATERIA WTYKOWA, UCHWYT ZŁĄCZEK 3X82A - GRZEBIEŃ DUŻY - PANEL",4.3,"1-ZE-10",3.7166666666666668,10,"OE_MCC","01021","SZT","85389099",null,"171020LK","5901988010218","OE - Batterie rechargeable, support de connecteur 3x82A - grand peigne - panneau","OE - Plug-in battery, connector holder 3x82A - large comb - panel","OE- BATERÍA ENCHUFABLE, SOPORTE CONECTOR 3X82A","ZENERGY - DUGATÓ ELEM, CSATLAKOZÓTARTÓ 3X82A - NAGY FÉSŰ - PANEL"]
["01022","ZENERGY - BATERIA WTYKOWA, UCHWYT ZŁĄCZEK 25-50A - GRZEBIEŃ MAŁY - PANEL",3.6,"1-ZE-10",1.1333333333333333,8,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010225","OE - Batterie embrochable, support de connecteur 25-50A - petit peigne - panneau","OE - Plug-in battery, connector holder 25-50A - small comb - panel","*OE- Batería enchufable, soporte de conector 25-50A - peine pequeño - panel","ZENERGY - DUGATOZÓ AKKUMULÁTOR, CSATLAKOZÓTARTÓ 25-50A - KIS FÉSŰ - PANEL"]
["01024","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, PŁYTA EFEN 160 + WSPORNIK",11.9,"1-ZE-10",0.70833333333333337,6,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988010249","OE - Batterie plug-in, panneau gauche, P600, carte mère EFEN 160 + support","OE - Plug-in battery, left panel, D600, EFEN 160 board + bracket","*OE- Batería enchufable, panel izquierdo, D600, placa EFEN 160 + soporte","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600, EFEN 160 LEMEZ + KONZER"]
["01025","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, OSŁONA CZOŁOWA FUPACT 00, 5M / 500",64.099999999999994,"1-ZE-10",0.8833333333333333,5,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010256","OE - Batterie plug-in, panneau gauche, P600, capot avant Fupact 00, 5M / 500","OE - Plug-in Battery, Left Panel, D600, Fupact 00 Front cover, 5M / 500","*OE- Batería enchufable, panel izquierdo, D600, cubierta frontal Fupact 00, 5M / 500","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600, FUPACT 00 ELSŐ BURKOLAT, 5M / 500"]
["01030","ZENERGY - BATERIA WTYKOWA, PUSZKA MOCOWANIA ZŁĄCZEK - OBUDOWA",16.2,"1-ZE-10",3.7833333333333332,12,"POWER_QUALITY",null,"SZT","85389099",null,"180117PK","5901988010300","OE - Batterie rechargeable, Boîte de fixation pour connecteurs - Boîtier","OE - Plug-in battery, Connector mounting box - Housing","*OE- Batería enchufable, Caja de acoplamiento - Carcasa","ZENERGY - DUGATÓ AKKUMULÁTOR, CSATLAKOZÓ RÖGZÍTŐ DOBOZ - HÁZ"]
["01031","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, OSŁONA CZOŁOWA FH125, 5M / 500",64.099999999999994,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010317","OE - Batterie plug-in, panneau droit, P600, capot avant FH125, 5M / 500","OE - Plug-in Battery, Right Panel, D600, FH125 Front cover, 5M / 500","*OE- Batería enchufable, panel derecho, D600, cubierta frontal FH125, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, ELSŐ BURKOLAT FH125, 5M / 500"]
["01032","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, OSŁONA CZOŁOWA FH63, 5M / 500",64.099999999999994,"1-ZE-10",0.3,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010324","OE - Batterie plug-in, panneau droit, P600, capot avant FH63, 5M / 500","OE - Plug-in Battery, Right Panel, D600, FH63 Front cover, 5M / 500","*OE- Batería enchufable, panel derecho, D600, cubierta frontal FH63, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, ELSŐ BURKOLAT FH63, 5M / 500"]
["01033","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, OSŁONA CZOŁOWA 2XFH63, 5M / 500",64.099999999999994,"1-ZE-10",0.15833333333333333,2,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010331","OE - Batterie plug-in, panneau droit, P600, capot avant 2xFH63, 5M / 500","OE - Plug-in battery, right panel, D600, 2xFH63 Front cover, 5M / 500","*OE- Batería enchufable, panel derecho, D600, cubierta frontal 2xFH63, 5M / 500","ZENERGY - DUGATÓ AKKUMULÁTOR, JOBB PANEL, D600, ELSŐ BURKOLAT 2XFH63, 5M / 500"]
["01034","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, OSŁONA CZOŁOWA FH32, 5M / 500",64.099999999999994,"1-ZE-10",0.2,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010348","OE - Batterie plug-in, panneau droit, P600, capot avant FH32, 5M / 500","OE - Plug-in Battery, Right Panel, D600, FH32 Front cover, 5M / 500","*OE- Batería enchufable, panel derecho, D600, cubierta frontal FH32, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, ELSŐ BURKOLAT FH32, 5M / 500"]
["01035","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, OSŁONA CZOŁOWA 2XFH32, 5M / 500",64.099999999999994,"1-ZE-10",0.43333333333333335,4,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010355","OE - Batterie plug-in, panneau droit, P600, capot avant 2xFH32, 5M / 500","OE - Plug-in battery, right panel, D600, 2xFH32 Front cover, 5M / 500","*OE- Batería enchufable, panel derecho, D600, cubierta frontal 2xFH32, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, D600, ELSŐ BURKOLAT 2XFH32, 5M / 500"]
["01041","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, OSŁONA CZOŁOWA FH125, 5M / 500",64.099999999999994,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010416","OE - Batterie plug-in, panneau gauche, P600, capot avant FH125, 5M / 500","OE - Plug-in battery, left panel, D600, Front cover FH125, 5M / 500","*OE- Batería enchufable, panel izquierdo, D600, cubierta frontal FH125, 5M / 500","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, BAL PANEL, D600, ELSŐ BURKOLAT FH125, 5M / 500"]
["01042","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, OSŁONA CZOŁOWA FH63, 5M / 500",64.099999999999994,"1-ZE-10",1.5,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010423","OE - Batterie plug-in, panneau gauche, P600, capot avant FH63, 5M / 500","OE - Plug-in battery, left panel, D600, FH63 Front cover, 5M / 500","*OE- Batería enchufable, panel izquierdo, D600, cubierta frontal FH63, 5M / 500","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600, ELSŐ BURKOLAT FH63, 5M / 500"]
["01043","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, OSŁONA CZOŁOWA 2XFH63, 5M / 500",64.099999999999994,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010430","OE - Batterie plug-in, panneau gauche, P600, capot avant 2xFH63, 5M / 500","OE - Plug-in battery, left panel, D600, 2xFH63 Front cover, 5M / 500","*OE- Batería enchufable, panel izquierdo, D600, cubierta frontal 2xFH63, 5M / 500","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600, ELSŐ BURKOLAT 2XFH63, 5M / 500"]
["01044","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, OSŁONA CZOŁOWA FH32, 5M / 500",64.099999999999994,"1-ZE-10",0.40833333333333333,2,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010447","OE - Batterie plug-in, panneau gauche, P600, capot avant FH32, 5M / 500","OE - Plug-in battery, left panel, D600, FH32 Front cover, 5M / 500","*OE- Batería enchufable, panel izquierdo, D600, cubierta frontal FH32, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, BAL PANEL, D600, ELSŐ BURKOLAT FH32, 5M / 500"]
["01045","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, OSŁONA CZOŁOWA 2XFH32, 5M / 500",64.099999999999994,"1-ZE-10",0.26666666666666666,4,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010454","OE - Batterie plug-in, panneau gauche, P600, capot avant 2xFH32, 5M / 500","OE - Plug-in battery, left panel, D600, 2xFH32 Front cover, 5M / 500","*OE- Batería enchufable, panel izquierdo, D600, cubierta frontal 2xFH32, 5M / 500","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600, ELSŐ BURKOLAT 2XFH32, 5M / 500"]
["01051","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA 2XFH32, 4M / 500",58.7,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010515","OE - Batterie externe, couvercle avant 2xFH32, 4M / 500","OE - Plug-in battery, 2xFH32, 4M / 500 front control panel","*OE- Batería enchufable, 2xFH32, cubierta de control frontal 4M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT 2XFH32, 4M / 500"]
["01052","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA 2XFH32, 5M / 500",64.099999999999994,"1-ZE-10",0.1,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010522","OE - Batterie externe, couvercle avant 2xFH32, 5M / 500","OE - Plug-in battery, 2xFH32, 5M / 500 front control cover","*OE- Batería enchufable, 2xFH32, cubierta de control frontal 5M / 500","ZENERGY - BDUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT 2XFH32, 5M / 500"]
["01053","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA 2XFH32, 6M / 500",67.8,"1-ZE-10",0.69166666666666665,2,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010539","OE - Batterie externe, couvercle avant 2xFH32, 6M / 500","OE - Plug-in battery, 2xFH32, 6M / 500 front control panel","*OE- Batería enchufable, 2xFH32, tapa de control frontal 6M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT 2XFH32, 6M / 500"]
["01054","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA REGULATORA, 5M / 500",64.099999999999994,"1-ZE-10",0.05,5,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010546","OE - Batterie rechargeable, couvercle avant du régulateur, 5M / 500","OE - Plug-in battery, regulator Front cover, 5M / 500","*OE- Batería enchufable, tapa frontal del regulador, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, SZABÁLYOZÓ ELSŐ BURKOLAT, 5M / 500"]
["01055","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA PERFOROWANA, W650, 4M / 500",67.400000000000006,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010553","OE - Batterie rechargeable, couvercle avant perforé, 4M / 500","OE - Plug-in battery, Perforated Front cover, 4M / 500","*OE- Batería enchufable, cubierta frontal perforada, 4M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PERFORÁLT ELSŐ BURKOLAT, W650, 4M / 500"]
["01056","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA PERFOROWANA, W650, 5M / 500",73.2,"1-ZE-10",1.6666666666666666E-2,2,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010560","OE - Batterie rechargeable, couvercle avant perforé, 5M / 500","OE - Plug-in battery, Perforated Front cover, 5M / 500","*OE- Batería enchufable, cubierta frontal perforada, 5M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PERFORÁLT ELSŐ BURKOLAT, W650, 5M / 500"]
["01057","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA PERFOROWANA, W650, 6M / 500",76.900000000000006,"1-ZE-10",0.13333333333333333,5,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010577","OE - Batterie rechargeable, couvercle avant perforé, 6M / 500","OE - Plug-in battery, Perforated Front cover, 6M / 500","*OE- Batería enchufable, tapa frontal perforada, 6M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PERFORÁLT ELSŐ BURKOLAT, W650, 6M / 500"]
["01059","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA, PEŁNA 2XFH32, 6M / 500",67.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010591","OE - Batterie rechargeable, cache de protection avant, 2xFH32 complet, 6M / 500","OE - Plug-in battery, control Front cover, Plain 2xFH32, 6M / 500","*OE- Batería enchufable, cubierta de control frontal, completa 2xFH32, 6M / 500","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ FEDÉL, TELJES 2XFH32, 6M / 500"]
["01060","ZENERGY - BATERIA WTYKOWA, UCHWYT GÓRNY KORYTKA",2.5,"1-ZE-10",null,null,"POWER_QUALITY","01060","SZT","85389099",null,"231113LK","5901988010607","OE - Batterie enfichable, support de plateau supérieur","OE - Plug-in faucet, upper tray handle","*OE- Batería enchufable, asa de la bandeja superior","ZENERGY - DUGATOZÓ AKKUMULÁTOR, TÁLCA FELSŐ FONTOS"]
["01061","ZENERGY - BATERIA WTYKOWA, PŁYTA STEROWANIA W650, 4M 2XFH32",79,"1-ZE-10",0.7,4,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010614","OE - Batterie rechargeable, Carte de contrôle 4M, 2xFH32","OE - Plugin capacitor bank, W650 control board, 4M 2xFH32","*OE- Batería enchufable, tablero de control W650, 4M 2xFH32","ZENERGY - DUGATOZÓ AKKUMULÁTOR, W650 VEZÉRLŐPÁR, 4M 2XFH32"]
["01064","ZENERGY - BATERIA WTYKOWA, PŁYTA STEROWANIA W650, 5M 2XFH32",90.2,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010645","OE - Batterie enfichable, tableau de commande 5M, UCB630 / 800 + 2xFH32","OE - Plugin capacitor bank, W650 control board, 5M 2xFH32","*OE- Batería enchufable, tablero de control W650, 5M 2xFH32","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, W650 VEZÉRLŐPÁR, 5M 2XFH32"]
["01068","ZENERGY - BATERIA WTYKOWA, PŁYTA STEROWANIA SVG-APF D800, 2M TS-35",60.5,"1-ZE-10",0.1,5,"POWER_QUALITY","01068","SZT","85389099",null,"231113LK","5901988010683","OE - Batterie enfichable, tableau de commande SVG-APF D800, 2M TS-35","OE - Plugin capacitor bank, W650 control board, SVG-APF D800, 2M TS-35","*OE- Batería enchufable, tablero de control SVG-APF D800, 2M TS-35","ZENERGY – DUGATTHATÓ AKKUMULÁTOR, VEZÉRLŐPAP SVG-APF D800, 2M TS-35"]
["01070","ZENERGY - BATERIA WTYKOWA,WSPORNIK UNIWERSALNY, KORYTKO, PE",7.5,"1-ZE-10",0.89166666666666672,5,"POWER_QUALITY",null,"SZT","85389099",null,"171023LK","5901988010706","OE - Batterie rechargeable, support universel, plateau, PE","OE - Plug-in faucet, universal bracket, tray, PE","*OE- Batería enchufable, soporte universal, bandeja, PE","ZENERGY - DUGATOZÓ AKKUMULÁTOR, UNIVERZÁLIS KERET, TÁLCA, PE"]
["01071","ZENERGY - BATERIA WTYKOWA,D600, W650, PRZEGRODA KRÓTKA PRAWA",12.8,"1-ZE-10",0.1,4,"POWER_QUALITY",null,"SZT","85389099",null,"171023LK","5901988010713","OE - Batterie enfichable, P600, L650, chicane courte à droite","OE - Plug-in battery, D600, W650, short right drawer","*OE- Batería enchufable, D600, W650, partición derecha corta","ZENERGY - DUGATOZÓ AKKUMULÁTOR, D600, W650, RÖVID REKESZ JOBB"]
["01072","ZENERGY - BATERIA WTYKOWA,D600, W650, PRZEGRODA KRÓTKA LEWA",12.8,"1-ZE-10",0.15,6,"POWER_QUALITY",null,"SZT","85389099",null,"171023LK","5901988010720","OE - Batterie enfichable, P600, L650, petit mur, gauche","OE - Plug-in battery, D600, W650, short left divider","*OE- Batería enchufable, D600, W650, partición corta izquierda","ZENERGY - DUGATÓ AKKUMULÁTOR, D600, W650, RÖVID REKESZ BAL"]
["01073","ZENERGY - BATERIA WTYKOWA,D600, 2XWSPORNIK POD DŁAWIKI",20.399999999999999,"1-ZE-10",0.25,8,"POWER_QUALITY",null,"SZT","85389099",null,"180206PK","5901988010737","OE - Batterie enfichable, P600, 2x avec selfs","OE - Plug-in battery, D600, 2xbracket for chokes","*OE- Batería enchufable, D600, 2x soporte para estranguladores","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, D600, 2X SZÍVATÓ KERET"]
["01075","ZENERGY - BATERIA WTYKOWA, WSPORNIK KORYTKA DŁUGI",7.4,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,"180123PK","5901988010751","OE - Batterie enfichable, support de plateau long","OE - Plug-in battery, long tray support","*OE- batería enchufable, soporte de bandeja larga","ZENERGY - DUGATOZÓ AKKUMULÁTOR, HOSSZÚ TÁLCS TÁMOGATÁS"]
["01077","ZENERGY - BATERIA WTYKOWA, IZOLATOR 630A 3P, W650, MOST PIONOWY NA PLECACH WGŁĘBIONY",137.5,"1-ZE-10",1.4583333333333333,10,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010775","OE - BATTERIE PRISE, ISOLANT 630A 3P, L650, PONT ARRIERE VERTICAL RECENT","OE - Plugin capacitor bank, insulator 630A 3P, W650, Vertical busbars back support","*OE - ENCHUFE BATERIA, AISLADOR 630A 3P, W650, PUENTE TRASERO VERTICAL RECIENTE","ZENERGY - DUGATOZÓ AKKUMULÁTOR, ISOLATOR 630A 3P, W650, FÜGGŐLEGES HÍD A HÁTSON FOGADVA"]
["01078","ZENERGY - BATERIA WTYKOWA, IZOLATOR 630A 3P, W800, MOST PIONOWY NA PLECACH WGŁĘBIONY",141.9,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010782","OE - BATTERIE PRISE, ISOLANT 630A 3P, L800, PONT ARRIERE VERTICAL RECENT","OE - Plugin capacitor bank, insulator 630A 3P, W800, Vertical busbars back support","*OE - ENCHUFE BATERIA, AISLADOR 630A 3P, W800, PUENTE TRASERO VERTICAL RECIENTE","ZENERGY - DUGATOZÓ AKKUMULÁTOR, ISOLATOR 630A 3P, W800, FÜGGŐLEGES HÍD A HÁTSON FOGADVA"]
["01084","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY,  ZAPADKA - BLOKADA NA SPRĘŻYNIE",2.4,"1-ZE-10",1.6166666666666667,12,"POWER_QUALITY",null,"SZT","85389099",null,"180123PK","5901988010843","OE - Batterie plug-in, panneau droit, Loquet - Verrou à ressort","OE - Plug-in battery, right panel, Latch - lock on a spring","*OE- Batería enchufable, panel derecho, Trinquete - bloqueo de resorte","ZENERGY – DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, RÁCS – RUGÓZÁR"]
["01085","ZENERGY - BATERIA WTYKOWA PANEL LEWY,  ZAPADKA - BLOKADA NA SPRĘŻYNIE",2.4,"1-ZE-10",1.6666666666666667,8,"POWER_QUALITY",null,"SZT","85389099",null,"171110PK","5901988010850","OE - Batterie rechargeable, panneau gauche, Loquet - Verrou à ressort","OE - Plug-in battery, left panel, Latch - lock on a spring","*OE- Panel izquierdo de la batería enchufable, Trinquete - bloqueo de resorte","ZENERGY - DUGATÓ AKKUMULÁTOR BAL PANEL, RÁCS - RUGÓZÁR"]
["01086","ZENERGY - BATERIA WTYKOWA, BLOKADA MECHANICZNA PANELI",2.8,"1-ZE-10",3.3833333333333333,11,"POWER_QUALITY",null,"SZT","85389099",null,"171023LK","5901988010867","OE - PLUG BATTERIE, VERROUILLAGE MÉCANIQUE DES PANNEAUX","OE - Plugin capacitor bank, Panels mechanical lock","*OE - ENCHUFE BATERÍA, PANELES BLOQUEO MECÁNICO","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PANEL MECHANIKUS ZÁRÁSA"]
["01087","ZENERGY - BATERIA WTYKOWA, IZOLATOR 630A 4P, W650, MOST PIONOWY NA PLECACH WGŁĘBIONY",177.1,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010874","OE - BATTERIE PRISE, ISOLANT 630A 4P, L650, PONT ARRIERE VERTICAL RECENT","OE - Plugin capacitor bank, insulator 630A 4P, W650, Vertical busbars back support","*OE - ENCHUFE BATERIA, AISLADOR 630A 4P, W650, PUENTE TRASERO VERTICAL RECIENTE","ZENERGY - DUGATOZÓ AKKUMULÁTOR, ISOLATOR 630A 4P, W650, FÜGGŐLEGES HÍD A HÁTSON FOGADVA"]
["01088","ZENERGY - BATERIA WTYKOWA, IZOLATOR 630A 4P, W800, MOST PIONOWY NA PLECACH WGŁĘBIONY",183.7,"1-ZE-10",0.33333333333333331,4,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988010881","OE - BATTERIE PRISE, ISOLANT 630A 4P, L800, PONT ARRIERE VERTICAL RECENT","OE - Plugin capacitor bank, insulator 630A 4P, W800, Vertical busbars back support","*OE - ENCHUFE BATERIA, AISLADOR 630A 4P, W800, PUENTE TRASERO VERTICAL RECIENTE","ZENERGY - DUGATOZÓ AKKUMULÁTOR, ISOLATOR 630A 4P, W800, FÜGGŐLEGES HÍD A HÁTSON FOGADVA"]
["01090","ZENERGY - METALOWA KRATKA WENTYLACYJNA NA DRZWI FRONT IP54:230x270mm; głebokość:50mm",117.6,"1-ZE-10",null,null,"OE_VENTILATION",null,"SZT","85389099",null,null,"5901988010904","OE - Grille de ventilation métallique POUR PORTE AVANT IP54 : 230 x 270 mm ; profondeur : 50 mm","OE - Metal ventilation grille for front door IP54:230x270mm; depth:50mm","*OE - Rejilla ventilación metálica PARA PUERTA FRONTAL IP54:230x270mm; profundidad: 50 mm","ZENERGY - FÉM SZELLŐZŐRÁCS BELSŐ AJTÓHOZ IP54: 230x270mm; mélység: 50mm"]
["01091","ZENERGY - METALOWA KRATKA WENTYLACYJNA NA DRZWI FRONT IP54:230x430mm; głębokość:50mm",150.1,"1-ZE-10",0.11666666666666667,2,"OE_VENTILATION",null,"SZT","85389099",null,null,"5901988010911","OE - Grille de ventilation métallique POUR PORTE AVANT IP54 : 230x430 mm ; profondeur : 50 mm","OE - Metal ventilation grille for front door IP54:230x430mm; depth:50mm","*OE - Rejilla ventilación metálica PARA PUERTA FRONTAL IP54:230x430mm; profundidad: 50 mm","ZENERGY - FÉM SZELLŐZŐRÁCS BELSŐ AJTÓHOZ IP54: 230x430mm; mélység: 50mm"]
["01094","ZENERGY - Zamknięcie osłony czołowej 10 sztuk",49.7,"1-ZE-01",36,11,"OE_SUPPORT","01094","SZT","85389099","27.12.40.0",null,"5901988010942","Zenergy - Fermetures de plastron 1/4 de tour - pièce rechange (x10)","ZENERGY - Closing for the Front cover - 10 pieces","ZEN- CIERRE TAPA FRONTAL ZENERGY (10UDS)","ZENERGY - Előlap záró 10 db"]
["01095","ZENERGY - Blokada otwarcia osłony czołowej - 10szt.",52.2,"1-ZE-01",null,null,"OE_SUPPORT","01095","SZT","85389099",null,null,"5901988010959","OE - Blocage de l'ouverture du capot avant - 10 pcs.","OE - Front cover opening blockade - 10 pcs.","*OE - Bloqueo apertura tapa frontal - 10 uds.","ZENERGY - Előlap nyitózár - 10 db."]
["01100","ZENERGY PT - ŁĄCZNIK OBUDÓW PODTYNKOWYCH - 1 SZT.",6.7,"1-ZE-03",null,null,"PT_VERTICAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988011000","PT - Connecteur pour boîtiers encastrés","PT - Coupler for flush-mounted enclosures - 1 pc.","EMP- PIEZA UNION ARMARIOS DE EMPOTRAR","ZENERGY PT - SÜLTETETT HÁZOK CSATLAKOZÓJA - 1 DB."]
["01102","ZENERGY PT - DWIE POKRYWY POZIOME W600",92.4,"1-ZE-03",3.9666666666666668,8,"PT_HORIZONTAL_COVER","01102","SZT","85389099","27.12.40.0",null,"5901988011024","PT - Deux couvercles horizontaux L600","PT - Two Horizontal Lids W600","EMP- TECHO/SUELO (2UUDS) W600","ZENERGY PT - KÉT VÍZSZINTES BORÍTÓ W600"]
["01103","ZENERGY PT - DWIE POKRYWY POZIOME W600 D180",101.7,"1-ZE-03",8.3333333333333329E-2,6,"PT_HORIZONTAL_COVER","01103","SZT","85389099","27.12.40.0",null,"5901988011031","PT - Deux couvercles horizontaux L600 D180","PT - Two Horizontal Lids W600 D180","EMP- TECHO/SUELO (2UDS) W600 D180","ZENERGY PT - KÉT VÍZSZINTES BURKOLAT W600 D180"]
["01106","ZENERGY PT - RAMKA DO DRZWI 6H MOD, H400 X W600",59.7,"1-ZE-03",0.10833333333333334,2,"PT_DOOR_FRAME","01106","SZT","85389099","27.12.40.0",null,"5901988011062","PT - Portes pleine IP40, MOD 6H, H400 x L600","PT - 6H MOD door frame, H400 x W600","EMP- MARCO PUERTA 6H MOD, H400 x W600","ZENERGY PT - AJTÓKERET 6H MOD, H400 X W600"]
["01107","ZENERGY ON - POKRYWA TYLNA W600 H400 6M IP-30",91.2,"1-ZE-03",0.25,2,"ON_BACK_PLATE","01107","SZT","85389099","27.12.40.0",null,"5901988011079","ON - Capot arrière H400 6M IP-30","ON - Rear cover H400 6M IP-30","ON- PANEL TRASERO H400 6M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H400 6M IP-30"]
["01109","ZENERGY PT - RAMKA DO DRZWI 9H MOD, H550 X W600",66.599999999999994,"1-ZE-03",0.40833333333333333,5,"PT_DOOR_FRAME","01109","SZT","85389099","27.12.40.0",null,"5901988011093","PT - Portes complètes IP40, MOD 9H, H550 x L600","PT - Door frame 9H MOD, H550 x W600","EMP- MARCO PUERTA 9H MOD, H550 x W600","ZENERGY PT - AJTÓKERET 9H MOD, H550 X W600"]
["01110","ZENERGY ON - POKRYWA TYLNA W600 H550 9M IP-30",108.1,"1-ZE-03",0.81666666666666665,6,"ON_BACK_PLATE","01110","SZT","85389099","27.12.40.0",null,"5901988011109","ON - Capot arrière H550 9M IP-30","ON - Rear cover H550 9M IP-30","ON- PANEL TRASERO H550 9M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H550 9M IP-30"]
["01112","ZENERGY PT - RAMKA DO DRZWI 12H MOD, H700 X W600",71.099999999999994,"1-ZE-03",1.7,8,"PT_DOOR_FRAME","01112","SZT","85389099","27.12.40.0",null,"5901988011123","PT - Portes pleine IP40, MOD 12H, H700 x L600","PT - Door frame 12H MOD, H700 x W600","EMP- MARCO PUERTA 12H MOD, H700 x W600","ZENERGY PT - AJTÓKERET 12H MOD, H700 X W600"]
["01113","ZENERGY ON - POKRYWA TYLNA W600 H700 12M IP-30",125.1,"1-ZE-03",1.5416666666666667,8,"ON_BACK_PLATE","01113","SZT","85389099","27.12.40.0",null,"5901988011130","ON - Capot arrière H700 12M IP-30","ON - Rear cover H700 12M IP-30","ON- PANEL TRASERO H700 12M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H700 12M IP-30"]
["01115","ZENERGY PT - RAMKA DO DRZWI 15H MOD, H850 X W600",76.400000000000006,"1-ZE-03",1.3416666666666666,11,"PT_DOOR_FRAME","01115","SZT","85389099","27.12.40.0",null,"5901988011154","PT - Portes pleine IP40, MOD 15H, H850 x L600","PT - Door frame 15H MOD, H850 x W600","EMP- MARCO PUERTA 15H MOD, H850 x W600","ZENERGY PT - AJTÓKERET 15H MOD, H850 X W600"]
["01116","ZENERGY ON - POKRYWA TYLNA W600 H850 15M IP-30",145.19999999999999,"1-ZE-03",1.2416666666666667,7,"ON_BACK_PLATE","01116","SZT","85389099","27.12.40.0",null,"5901988011161","ON - Capot arrière H850 15M IP-30","ON - Rear cover H850 15M IP-30","ON- PANEL TRASERO H850 15M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H850 15M IP-30"]
["01118","ZENERGY PT - RAMKA DO DRZWI 18H MOD, H1000 X W600",83.5,"1-ZE-03",0.2,2,"PT_DOOR_FRAME","01118","SZT","85389099","27.12.40.0",null,"5901988011185","PT - Portes pleines IP40, MOD 18H, H1000 x L600","PT - Door frame 18H MOD, H1000 x W600","EMP- MARCO PUERTA 18H MOD, H1000 x W600","ZENERGY PT - AJTÓKERET 18H MOD, H1000 X W600"]
["01119","ZENERGY ON - POKRYWA TYLNA W600 H1000 18M IP-30",172.8,"1-ZE-03",0.8666666666666667,5,"ON_BACK_PLATE","01119","SZT","85389099","27.12.40.0",null,"5901988011192","ON - Capot arrière H1000 18M IP-30","ON - Rear cover H1000 18M IP-30","ON- PANEL TRASERO H1000 18M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H1000 18M IP-30"]
["01121","ZENERGY PT - RAMKA DO DRZWI 21H MOD, H1150 X W600",92.9,"1-ZE-03",0.34166666666666667,4,"PT_DOOR_FRAME","01121","SZT","85389099","27.12.40.0",null,"5901988011215","PT - Portes pleines IP40, MOD 21H, H1150 x L600","PT - 21H MOD door frame, H1150 x W600","EMP- MARCO PUERTA 21H MOD, H1150 x W600","ZENERGY PT - AJTÓKERET 21H MOD, H1150 X W600"]
["01122","ZENERGY ON - POKRYWA TYLNA W600 H1150 21M IP-30",200.3,"1-ZE-03",0.66666666666666663,5,"ON_BACK_PLATE","01122","SZT","85389099","27.12.40.0",null,"5901988011222","ON - Capot arrière H1150 21M IP-30","ON - Rear cover H1150 21M IP-30","ON- PANEL TRASERO H1150 21M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H1150 21M IP-30"]
["01124","ZENERGY PT - RAMKA DO DRZWI 24H MOD, H1300 X W600",101.4,"1-ZE-03",9.166666666666666E-2,6,"PT_DOOR_FRAME","01124","SZT","85389099","27.12.40.0",null,"5901988011246","PT - Portes pleine IP40, MOD 24H, H1300 x L600","PT - 24H MOD door frame, H1300 x W600","EMP- MARCO PUERTA 24H MOD, H1300XW600","ZENERGY PT - AJTÓKERET 24H MOD, H1300 X W600"]
["01125","ZENERGY ON - POKRYWA TYLNA W600 H1300 24M IP-30",239.6,"1-ZE-03",1.6666666666666666E-2,2,"ON_BACK_PLATE","01125","SZT","85389099","27.12.40.0",null,"5901988011253","ON - Capot arrière H1300 24M IP-30","ON - Rear cover H1300 24M IP-30","ON- PANEL TRASERO H1300 24M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H1300 24M IP-30"]
["01127","ZENERGY PT - RAMKA DO DRZWI 27H MOD, H1450 X W600",108.1,"1-ZE-03",3.3333333333333333E-2,2,"PT_DOOR_FRAME","01127","SZT","85389099","27.12.40.0",null,"5901988011277","PT - Portes pleines IP40, MOD 27H, H1450 x L600","PT - 27H MOD door frame, H1450 x W600","EMP- MARCO PUERTA 27H MOD, H1450XW600","ZENERGY PT - AJTÓKERET 27H MOD, H1450 X W600"]
["01128","ZENERGY ON - POKRYWA TYLNA W600 H1450 27M IP-30",262.89999999999998,"1-ZE-03",0.01,1,"ON_BACK_PLATE","01128","SZT","85389099","27.12.40.0",null,"5901988011284","ON - Capot arrière H1450 27M IP-30","ON - Rear cover H1450 27M IP-30","ON- PANEL TRASERO H1450 27M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H1450 27M IP-30"]
["01130","ZENERGY PT - RAMKA DO DRZWI 30H MOD, H1600 X W600",139.9,"1-ZE-03",0.05,5,"PT_DOOR_FRAME","01130","SZT","85389099","27.12.40.0",null,"5901988011307","PT - Portes pleine IP40, MOD 30H, H1600 x L600","PT - 30H MOD door frame, H1600 x W600","EMP- MARCO PUERTA 30H MOD, H1600XW600","ZENERGY PT - AJTÓKERET 30H MOD, H1600 X W600"]
["01131","ZENERGY ON - POKRYWA TYLNA W600 H1600 30M IP-30",286.2,"1-ZE-03",null,null,"ON_BACK_PLATE","01131","SZT","85389099","27.12.40.0",null,"5901988011314","ON - Capot arrière H1600 30M IP-30","ON - Rear cover H1600 30M IP-30","ON- PANEL TRASERO H1600 30M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W600 H1600 30M IP-30"]
["01206","ZENERGY PT - DWIE POKRYWY PIONOWE H400 6M",91.2,"1-ZE-03",null,null,"PT_VERTICAL_COVER","01206","SZT","85389099","27.12.40.0",null,"5901988012069","PT - Couvercles à deux couvercles H400 6M","PT - Two Vertical Lids H400 6M","EMP- PANEL LATERAL (2UDS) H400 6M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H400 6M"]
["01207","ZENERGY PT - POKRYWA TYLNA H400 W600, 6M IP30",26.5,"1-ZE-03",null,null,"PT_BACK_PLATE","01207","SZT","85389099","27.12.40.0",null,"5901988012076","PT - Capot arrière H400 L600, 6M IP30","PT - Rear cover H400 W600, 6M IP30","EMP- PANEL TRASERO H400 W600, 6M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H400 W600, 6M IP30"]
["01209","ZENERGY PT - DWIE POKRYWY PIONOWE H550 9M",93.5,"1-ZE-03",null,null,"PT_VERTICAL_COVER","01209","SZT","85389099","27.12.40.0",null,"5901988012090","PT - Deux couvercles verticaux H550 9M","PT - Two Vertical Lids H550 9M","EMP- PANEL LATERAL (2UDS) H550 9M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H550 9M"]
["01210","ZENERGY PT - POKRYWA TYLNA H550 W600, 9M IP30",39.6,"1-ZE-03",null,null,"PT_BACK_PLATE","01210","SZT","85389099","27.12.40.0",null,"5901988012106","PT - Capot arrière H550 L600, 9M IP30","PT - Rear cover H550 W600, 9M IP30","EMP- PANEL TRASERO H550 W600, 9M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H550 W600, 9M IP30"]
["01212","ZENERGY PT - DWIE POKRYWY PIONOWE H700 12M",95.9,"1-ZE-03",1.6416666666666666,6,"PT_VERTICAL_COVER","01212","SZT","85389099","27.12.40.0",null,"5901988012120","PT - Deux couvercles verticaux H700 12M","PT - Two Vertical Lids H700 12M","EMP- PANEL LATERAL (2UDS) H700 12M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H700 12M"]
["01213","ZENERGY PT - POKRYWA TYLNA H700 W600, 12M IP30",52.8,"1-ZE-03",1.6666666666666666E-2,1,"PT_BACK_PLATE","01213","SZT","85389099","27.12.40.0",null,"5901988012137","PT - Capot arrière H700 L600, 12M IP30","PT - Rear cover H700 W600, 12M IP30","EMP- PANEL TRASERO H700 W600, 12M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H700 W600, 12M IP30"]
["01215","ZENERGY PT - DWIE POKRYWY PIONOWE H850 15M",116.6,"1-ZE-03",0.4,2,"PT_VERTICAL_COVER","01215","SZT","85389099","27.12.40.0",null,"5901988012151","PT - Deux couvercles verticaux H850 15M","PT - Two Vertical Lids H850 15M","EMP- PANEL LATERAL (2UDS) H850 15M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H850 15M"]
["01216","ZENERGY PT - POKRYWA TYLNA H850 W600, 15M IP30",66.099999999999994,"1-ZE-03",null,null,"PT_BACK_PLATE","01216","SZT","85389099","27.12.40.0",null,"5901988012168","PT - Capot arrière H850 L600, 15M IP30","PT - Rear cover H850 W600, 15M IP30","EMP- PANEL TRASERO H850 W600, 15M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H850 W600, 15M IP30"]
["01218","ZENERGY PT - DWIE POKRYWY PIONOWE H1000 18M",134.6,"1-ZE-03",0.25,1,"PT_VERTICAL_COVER","01218","SZT","85389099","27.12.40.0",null,"5901988012182","PT - Deux couvercles verticaux H1000 18M","PT - Two Vertical Lids H1000 18M","EMP- PANEL LATERAL (2UDS) H1000 18M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H1000 18M"]
["01219","ZENERGY PT - POKRYWA TYLNA H1000 W600, 18M IP30",79.3,"1-ZE-03",null,null,"PT_BACK_PLATE","01219","SZT","85389099","27.12.40.0",null,"5901988012199","PT - Capot arrière H1000 L600, 18M IP30","PT - Rear cover H1000 W600, 18M IP30","EMP- PANEL TRASERO H1000 W600, 18M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1000 W600, 18M IP30"]
["01221","ZENERGY PT - DWIE POKRYWY PIONOWE H1150 21M",155.80000000000001,"1-ZE-03",0.35,4,"PT_VERTICAL_COVER","01221","SZT","85389099","27.12.40.0",null,"5901988012212","PT - Deux couvercles verticaux H1150 21M","PT - Two Vertical Lids H1150 21M","EMP- PANEL LATERAL (2UDS) H1150 21M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H1150 21M"]
["01222","ZENERGY PT - POKRYWA TYLNA H1150 W600, 21M IP30",92.4,"1-ZE-03",null,null,"PT_BACK_PLATE","01222","SZT","85389099","27.12.40.0",null,"5901988012229","PT - Capot arrière H1150 L600, 21M IP30","PT - Rear cover H1150 W600, 21M IP30","EMP- PANEL TRASERO H1150 W600, 21M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1150 W600, 21M IP30"]
["01224","ZENERGY PT - DWIE POKRYWY PIONOWE H1300 24M",171.7,"1-ZE-03",4.1666666666666664E-2,1,"PT_VERTICAL_COVER","01224","SZT","85389099","27.12.40.0",null,"5901988012243","PT - Deux couvercles verticaux H1300 24M","PT - Two Vertical Lids H1300 24M","EMP- PANEL LATERAL (2UDS) H1300 24M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H1300 24M"]
["01225","ZENERGY PT - POKRYWA TYLNA H1300 W600, 24M IP30",106,"1-ZE-03",null,null,"PT_BACK_PLATE","01225","SZT","85389099","27.12.40.0",null,"5901988012250","PT - Capot arrière H1300 L600, 24M IP30","PT - Rear cover H1300 W600, 24M IP30","EMP- PANEL TRASERO H1300 W600, 24M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1300 W600, 24M IP30"]
["01227","ZENERGY PT - DWIE POKRYWY PIONOWE H1450 27M",184.4,"1-ZE-03",null,null,"PT_VERTICAL_COVER","01227","SZT","85389099","27.12.40.0",null,"5901988012274","PT - Deux couvercles verticaux H1450 27M","PT - Two Vertical Lids H1450 27M","EMP- PANEL LATERAL (2UDS) H1450 27M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H1450 27M"]
["01228","ZENERGY PT - POKRYWA TYLNA H1450 W600, 27M IP30",118.7,"1-ZE-03",null,null,"PT_BACK_PLATE","01228","SZT","85389099","27.12.40.0",null,"5901988012281","PT - Capot arrière H1450 L600, 27M IP30","PT - Rear cover H1450 W600, 27M IP30","EMP- PANEL TRASERO H1450 W600, 27M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1450 W600, 27M IP30"]
["01230","ZENERGY PT - DWIE POKRYWY PIONOWE H1600 30M",278.8,"1-ZE-03",0.05,5,"PT_VERTICAL_COVER","01230","SZT","85389099","27.12.40.0",null,"5901988012304","PT - Deux couvercles verticaux H1600 30M","PT - Two Vertical Lids H1600 30M","EMP- PANEL LATERAL (2UDS) H1600 30M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT H1600 30M"]
["01231","ZENERGY PT - POKRYWA TYLNA H1600 W600, 30M IP30",132.5,"1-ZE-03",null,null,"PT_BACK_PLATE","01231","SZT","85389099","27.12.40.0",null,"5901988012311","PT - Capot arrière H1600 L600, 30M IP30","PT - Back cover H1600 W600, 30M IP30","EMP- PANEL TRASERO H1600 W600, 30M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1600 W600, 30M IP30"]
["01306","ZENERGY ON/PT - DRZWI PEŁNE IP40, 6 MOD, H400 X W600",108.1,"1-ZE-03",0.16666666666666666,5,"ON-PT_DOORS","01306","SZT","85389099","27.12.40.0",null,"5901988013066","PT - Portes transparentes IP40, MOD 6H, H400 x L600","ON/PT - Plain door IP40, 6 mod, H400 x W600","ON/EMP- PUERTA OPACA IP40, 6 MOD, H400 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 6 MOD, H400 X W600"]
["01307","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 6H MOD, H400 X W600",178.1,"1-ZE-03",null,null,"ON-PT_DOORS","01307","SZT","85389099","27.12.40.0",null,"5901988013073","ON/PT - Portes transparentes IP40, MOD 6H, H400 x L600","ON/PT - Transparent door IP40, 6H MOD, H400 x W600","ON/EMP- PUERTA TRANSP. IP40, 6H MOD, H400 x W600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 6H MOD, H400 X W600"]
["01309","ZENERGY ON/PT - DRZWI PEŁNE IP40, 9 MOD, H550 X W600",119.8,"1-ZE-03",1.2333333333333334,10,"ON-PT_DOORS","01309","SZT","85389099","27.12.40.0",null,"5901988013097","PT - Portes transparentes IP40, MOD 9H, H550 x L600","ON/PT - Plain door IP40, 9 mod, H550 x W600","ON/EMP- PUERTA OPACA IP40, 9 MOD, H550 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 9 MOD, H550 X W600"]
["01310","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 9H MOD, H550 X W600",198.2,"1-ZE-03",4.1666666666666664E-2,1,"ON-PT_DOORS","01310","SZT","85389099","27.12.40.0",null,"5901988013103","ON/PT - Portes transparentes IP40, MOD 9H, H550 x L600","ON/PT - Transparent door IP40, 9H MOD, H550 x W600","ON/EMP- PUERTA TRANSP. IP40, 9H MOD, H550 x W600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 9H MOD, H550 X W600"]
["01312","ZENERGY ON/PT - DRZWI PEŁNE IP40, 12 MOD, H700 X W600",128.30000000000001,"1-ZE-03",2.5833333333333335,12,"ON-PT_DOORS","01312","SZT","85389099","27.12.40.0",null,"5901988013127","PT - Portes transparentes IP40, MOD 12H, H700 x L600","ON/PT - Plain door IP40, 12 mod, H700 x W600","ON/EMP- PUERTA OPACA IP40, 12 MOD, H700 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 12 MOD, H700 X W600"]
["01313","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 12H MOD, H700 X W600",210.9,"1-ZE-03",0.10833333333333334,1,"ON-PT_DOORS","01313","SZT","85389099","27.12.40.0",null,"5901988013134","ON/PT - Portes transparentes IP40, MOD 12H, H700 x L600","ON/PT - Transparent door IP40, 12H MOD, H700 x W600","ON/EMP- PUERTA TRANSP. IP40, 12H MOD, H700 x W600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 12H MOD, H700 X W600"]
["01315","ZENERGY ON/PT - DRZWI PEŁNE IP40, 15 MOD, H850 X W600",159,"1-ZE-03",2.3166666666666669,11,"ON-PT_DOORS","01315","SZT","85389099","27.12.40.0",null,"5901988013158","PT - Portes transparentes IP40, MOD 15H, H850 x L600","ON/PT - Plain door IP40, 15 mod, H850 x W600","ON/EMP- PUERTA OPACA IP40, 15 MOD, H850 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 15 MOD, H850 X W600"]
["01316","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 15H MOD, H850 X W600",253.3,"1-ZE-03",1.6666666666666666E-2,1,"ON-PT_DOORS","01316","SZT","85389099","27.12.40.0",null,"5901988013165","ON/PT - Portes transparentes IP40, MOD 15H, H850 x L600","ON/PT - Transparent door IP40, 15H MOD, H850 x W600","ON/EMP- PUERTA TRANSP. IP40, 15H MOD, H850 x W600","ZENERGY ON/PT - ÁTLÁTSZÓ AJTÓK IP40, 15H MOD, H850 X W600"]
["01318","ZENERGY ON/PT - DRZWI PEŁNE IP40, 18 MOD, H1000 X W600",198.2,"1-ZE-03",1.1333333333333333,10,"ON-PT_DOORS","01318","SZT","85389099","27.12.40.0",null,"5901988013189","PT - Portes transparentes IP40, MOD 18H, H1000 x L600","ON/PT - Plain door IP40, 18 mod, H1000 x W600","ON/EMP- PUERTA OPACA IP40, 18 MOD, H1000 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 18 MOD, H1000 X W600"]
["01319","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 18H MOD, H1000 X W600",300,"1-ZE-03",0.01,1,"ON-PT_DOORS","01319","SZT","85389099","27.12.40.0",null,"5901988013196","ON/PT - Portes transparentes IP40, MOD 18H, H1000 x L600","ON/PT - Transparent door IP40, 18H MOD, H1000 x W600","ON/EMP- PUERTA TRANSP. IP40, 18H MOD, H1000 x W600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 18H MOD, H1000 X W600"]
["01321","ZENERGY ON/PT - DRZWI PEŁNE IP40, 21 MOD, H1150 X W600",237.4,"1-ZE-03",0.95833333333333337,12,"ON-PT_DOORS","01321","SZT","85389099","27.12.40.0",null,"5901988013219","PT - Portes transparentes IP40, MOD 21H, H1150 x L600","ON/PT - Plain door IP40, 21 mod, H1150 x W600","ON/EMP- PUERTA OPACA IP40, 21 MOD, H1150 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 21 MOD, H1150 X W600"]
["01322","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 21H MOD, H1150 X W600",348.7,"1-ZE-03",null,null,"ON-PT_DOORS","01322","SZT","85389099","27.12.40.0",null,"5901988013226","ON/PT - Portes transparentes IP40, MOD 21H, H1150 x L600","ON/PT - Transparent door IP40, 21H MOD, H1150 x W600","ON/EMP- PUERTA TRANSP. IP40, 21H MOD, H1150 x W600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 21H MOD, H1150 X W600"]
["01324","ZENERGY ON/PT - DRZWI PEŁNE IP40, 24 MOD, H1300 X W600",277.7,"1-ZE-03",0.10833333333333334,7,"ON-PT_DOORS","01324","SZT","85389099","27.12.40.0",null,"5901988013240","PT - Portes transparentes IP40, MOD 24H, H1300 x L600","ON/PT - Plain door IP40, 24 mod, H1300 x W600","ON/EMP- PUERTA OPACA IP40, 24 MOD H1300XW600","ZENERGY ON/PT – TELJES AJTÓ IP40, 24 MOD, H1300 X W600"]
["01325","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 24H MOD, H1300 X W600",384.8,"1-ZE-03",null,null,"ON-PT_DOORS","01325","SZT","85389099","27.12.40.0",null,"5901988013257","ON/PT - Portes transparentes IP40, MOD 24H, H1300 x L600","ON/PT - Transparent door IP40, 24H MOD, H1300 x W600","ON/EMP- PUERTA TRANSP. IP40, 24H MOD, H1300XW600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 24H MOD, H1300 X W600"]
["01327","ZENERGY ON/PT - DRZWI PEŁNE IP40, 27 MOD, H1450 X W600",316.89999999999998,"1-ZE-03",4.1666666666666664E-2,5,"ON-PT_DOORS","01327","SZT","85389099","27.12.40.0",null,"5901988013271","PT - Portes transparentes IP40, MOD 27H, H1450 x L600","ON/PT - Plain door IP40, 27 mod, H1450 x W600","ON/EMP- PUERTA OPACA IP40, 27 MOD, H1450XW600","ZENERGY ON/PT – TELJES AJTÓ IP40, 27 MOD, H1450 X W600"]
["01328","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 27H MOD, H1450 X W600",418.7,"1-ZE-03",null,null,"ON-PT_DOORS","01328","SZT","85389099","27.12.40.0",null,"5901988013288","ON/PT - Portes transparentes IP40, MOD 27H, H1450 x L600","ON/PT - Transparent door IP40, 27H MOD, H1450 x W600","ON/EMP- PUERTA TRANSP. IP40, 27H MOD, H1450XW600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 27H MOD, H1450 X W600"]
["01330","ZENERGY ON/PT - DRZWI PEŁNE IP40, 30 MOD, H1600 X W600",356.2,"1-ZE-03",5.8333333333333334E-2,5,"ON-PT_DOORS","01330","SZT","85389099","27.12.40.0",null,"5901988013301","PT - Portes transparentes IP40, MOD 30H, H1600 x L600","ON/PT - Plain door IP40, 30 mod, H1600 x W600","EMP- PUERTA TRANSPARENTE IP40, 30H MOD, H1600 x W600","ZENERGY ON/PT – TELJES AJTÓ IP40, 30 MOD, H1600 X W600"]
["01331","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 30H MOD, H1600 X W600",543.79999999999995,"1-ZE-03",0.01,1,"ON-PT_DOORS","01331","SZT","85389099","27.12.40.0",null,"5901988013318","ON/PT - Portes transparentes IP40, MOD 30H, H1600 x L600","ON/PT - Transparent door IP40, 30H MOD, H1600 x W600","ON/EMP- PUERTA TRANSP. IP40, 30H MOD, H1600XW600","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 30H MOD, H1600 X W600"]
["01402","ZENERGY PT - DWIE POKRYWY POZIOME W800",106,"1-ZE-03",3.3333333333333333E-2,2,"PT_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988014025","PT - Deux couvercles horizontaux L800","PT - Two Horizontal Lids W800","*PT- Dos tapas horizontales W800","ZENERGY PT - KÉT VÍZSZINTES BORÍTÓ W800"]
["01403","ZENERGY PT - DWIE POKRYWY POZIOME W800 D180",111.3,"1-ZE-03",0.16666666666666666,7,"PT_HORIZONTAL_COVER","01403","SZT","85389099","27.12.40.0",null,"5901988014032","PT - Deux couvercles horizontaux L800 D180","PT - Two Horizontal Lids W800 D180","EMP- TECHO/SUELO (2UDS) W800 D180","ZENERGY PT - KÉT VÍZSZINTES BURKOLAT W800 D180"]
["01406","ZENERGY PT - RAMKA DO DRZWI 6H MOD, H400 X W800",71.8,"1-ZE-03",null,null,"PT_DOOR_FRAME","01406","SZT","85389099","27.12.40.0",null,"5901988014063","PT - Portes pleine IP40, MOD 6H, H400 x L800","PT - 6H MOD door frame, H400 x W800","EMP- MARCO PUERTA 6H MOD, H400XW800","ZENERGY PT - AJTÓKERET 6H MOD, H400 X W800"]
["01407","ZENERGY ON - POKRYWA TYLNA W800 H400 6M IP-30",109.2,"1-ZE-03",3.3333333333333333E-2,4,"ON_BACK_PLATE","01407","SZT","85389099",null,null,"5901988014070","ON - Capot arrière L800 H400 6M IP-30","ON - Back cover W800 H400 6M IP-30","ON- PANEL TRASERO W800 H400 6M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H400 6M IP-30"]
["01409","ZENERGY PT - RAMKA DO DRZWI 9H MOD, H550 X W800",79.900000000000006,"1-ZE-03",0.01,1,"PT_DOOR_FRAME","01409","SZT","85389099","27.12.40.0",null,"5901988014094","PT - Portes pleine IP40, MOD 9H, H550 x L800","PT - Door frame 9H MOD, H550 x W800","EMP- MARCO PUERTA 9H MOD, H550XW800","ZENERGY PT - AJTÓKERET 9H MOD, H550 X W800"]
["01410","ZENERGY ON - POKRYWA TYLNA W800 H550 9M IP-30",130.4,"1-ZE-03",null,null,"ON_BACK_PLATE","01410","SZT","85389099",null,null,"5901988014100","ON - Capot arrière L800 H550 9M IP-30","ON - Back cover W800 H550 9M IP-30","ON- PANEL TRASERO W800 H550 9M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H550 9M IP-30"]
["01412","ZENERGY PT - RAMKA DO DRZWI 12H MOD, H700 X W800",85.2,"1-ZE-03",null,null,"PT_DOOR_FRAME","01412","SZT","85389099","27.12.40.0",null,"5901988014124","PT - Portes pleine IP40, MOD 12H, H700 x L800","PT - Door frame 12H MOD, H700 x W800","EMP- MARCO PUERTA 12H MOD, H700XW800","ZENERGY PT - AJTÓKERET 12H MOD, H700 X W800"]
["01413","ZENERGY ON - POKRYWA TYLNA W800 H700 12M IP-30",150.5,"1-ZE-03",null,null,"ON_BACK_PLATE","01413","SZT","85389099",null,null,"5901988014131","ON - Capot arrière L800 H700 12M IP-30","ON - Back cover W800 H700 12M IP-30","ON- PANEL TRASERO W800 H700 12M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H700 12M IP-30"]
["01415","ZENERGY PT - RAMKA DO DRZWI 15H MOD, H850 X W800",91.7,"1-ZE-03",0.01,1,"PT_DOOR_FRAME","01415","SZT","85389099","27.12.40.0",null,"5901988014155","PT - Portes pleine IP40, MOD 15H, H850 x L800","PT - Door frame 15H MOD, H850 x W800","EMP- MARCO PUERTA 15H MOD, H850XW800","ZENERGY PT - AJTÓKERET 15H MOD, H850 X W800"]
["01416","ZENERGY ON - POKRYWA TYLNA W800 H850 15M IP-30",174.9,"1-ZE-03",null,null,"ON_BACK_PLATE","01416","SZT","85389099",null,null,"5901988014162","ON - Capot arrière L800 H850 15M IP-30","ON - Back cover W800 H850 15M IP-30","ON- PANEL TRASERO W800 H850 15M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H850 15M IP-30"]
["01418","ZENERGY PT - RAMKA DO DRZWI 18H MOD, H1000 X W800",100.2,"1-ZE-03",0.05,4,"PT_DOOR_FRAME","01418","SZT","85389099","27.12.40.0",null,"5901988014186","PT - Portes pleine IP40, MOD 18H, H1000 x L800","PT - Door frame 18H MOD, H1000 x W800","EMP- MARCO PUERTA 18H MOD, H1000XW800","ZENERGY PT - AJTÓKERET 18H MOD, H1000 X W800"]
["01419","ZENERGY ON - POKRYWA TYLNA W800 H1000 18M IP-30",207.8,"1-ZE-03",1.6666666666666666E-2,2,"ON_BACK_PLATE","01419","SZT","85389099",null,null,"5901988014193","ON - Capot arrière L800 H1000 18M IP-30","ON - Back cover W800 H1000 18M IP-30","ON- PANEL TRASERO W800 H1000 18M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H1000 18M IP-30"]
["01421","ZENERGY PT - RAMKA DO DRZWI 21H MOD, H1150 X W800",111.3,"1-ZE-03",1.6666666666666666E-2,1,"PT_DOOR_FRAME","01421","SZT","85389099","27.12.40.0",null,"5901988014216","PT - Portes pleine IP40, MOD 21H, H1150 x L800","PT - 21H MOD door frame, H1150 x W800","EMP- MARCO PUERTA 21H MOD, H1150XW800","ZENERGY PT - AJTÓKERET 21H MOD, H1150 X W800"]
["01422","ZENERGY ON - POKRYWA TYLNA W800 H1150 21M IP-30",240.6,"1-ZE-03",0.01,1,"ON_BACK_PLATE","01422","SZT","85389099",null,null,"5901988014223","ON - Capot arrière L800 H1150 21M IP-30","ON - Back cover W800 H1150 21M IP-30","ON- PANEL TRASERO W800 H1150 21M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H1150 21M IP-30"]
["01424","ZENERGY PT - RAMKA DO DRZWI 24H MOD, H1300 X W800",121.9,"1-ZE-03",null,null,"PT_DOOR_FRAME","01424","SZT","85389099","27.12.40.0",null,"5901988014247","PT - Portes pleine IP40, MOD 24H, H1300 x L800","PT - 24H MOD door frame, H1300 x W800","EMP- MARCO PUERTA 24H MOD, H1300XW800","ZENERGY PT – AJTÓKERET 24H MOD, H1300 X W800"]
["01425","ZENERGY ON - POKRYWA TYLNA W800 H1300 24M IP-30",287.3,"1-ZE-03",0.01,1,"ON_BACK_PLATE","01425","SZT","85389099",null,null,"5901988014254","ON - Capot arrière L800 H1300 24M IP-30","ON - Back cover W800 H1300 24M IP-30","ON- PANEL TRASERO W800 H1300 24M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H1300 24M IP-30"]
["01427","ZENERGY PT - RAMKA DO DRZWI 27H MOD, H1450 X W800",129.30000000000001,"1-ZE-03",0.01,1,"PT_DOOR_FRAME","01427","SZT","85389099","27.12.40.0",null,"5901988014278","PT - Portes pleine IP40, MOD 27H, H1450 x L800","PT - 27H MOD door frame, H1450 x W800","EMP- MARCO PUERTA 27H MOD, H1450XW800","ZENERGY PT – AJTÓKERET 27H MOD, H1450 X W800"]
["01428","ZENERGY ON - POKRYWA TYLNA W800 H1450 27M IP-30",315.89999999999998,"1-ZE-03",null,null,"ON_BACK_PLATE","01428","SZT","85389099",null,null,"5901988014285","ON - Capot arrière L800 H1450 27M IP-30","ON - Back cover W800 H1450 27M IP-30","ON- PANEL TRASERO W800 H1450 27M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H1450 27M IP-30"]
["01430","ZENERGY PT - RAMKA DO DRZWI 30H MOD, H1600 X W800",208.8,"1-ZE-03",9.166666666666666E-2,4,"PT_DOOR_FRAME","01430","SZT","85389099","27.12.40.0",null,"5901988014308","PT - Portes pleine IP40, MOD 30H, H1600 x L800","PT - 30H MOD door frame, H1600 x W800","EMP- MARCO PUERTA 30H MOD, H1600XW800","ZENERGY PT - AJTÓKERET 30H MOD, H1600 X W800"]
["01431","ZENERGY ON - POKRYWA TYLNA W800 H1600 30M IP-30",344.5,"1-ZE-03",5.8333333333333334E-2,4,"ON_BACK_PLATE","01431","SZT","85389099",null,null,"5901988014315","ON - Capot arrière L800 H1600 30M IP-30","ON - Back cover W800 H1600 30M IP-30","ON- PANEL TRASERO W800 H1600 30M IP30","ZENERGY ON - HÁTSÓ BURKOLAT W800 H1600 30M IP-30"]
["01506","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H400 6M",109.2,"1-ZE-03",null,null,"PT_VERTICAL_COVER","01506","SZT","85389099","27.12.40.0",null,"5901988015060","PT - Couvercles à deux couvercles D180 H400 6M","PT - Two Vertical Lids D180 H400 6M","EMP- PANEL LATERAL (2UDS) D180 H400 6M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H400 6M"]
["01507","ZENERGY PT - POKRYWA TYLNA H400 W800, 6M IP30",31.7,"1-ZE-03",null,null,"PT_BACK_PLATE","01507","SZT","85389099","27.12.40.0",null,"5901988015077","PT - Capot arrière H400 L800, 6M IP30","PT - Back cover H400 W800, 6M IP30","EMP- PANEL TRASERO H400 W800, 6M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H400 W800, 6M IP30"]
["01509","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H550 9M",112.4,"1-ZE-03",0.01,1,"PT_VERTICAL_COVER","01509","SZT","85389099","27.12.40.0",null,"5901988015091","PT - Deux couvercles verticaux D180 H550 9M","PT - Two Vertical Lids D180 H550 9M","EMP- PANEL LATERAL (2UDS) D180 H550 9M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H550 9M"]
["01510","ZENERGY PT - POKRYWA TYLNA H550 W800, 9M IP30",47.6,"1-ZE-03",null,null,"PT_BACK_PLATE","01510","SZT","85389099","27.12.40.0",null,"5901988015107","PT - Capot arrière H550 L800, 9M IP30","PT - Rear cover H550 W800, 9M IP30","EMP- PANEL TRASERO H550 W800, 9M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H550 W800, 9M IP30"]
["01512","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H700 12M",115.5,"1-ZE-03",1.6666666666666666E-2,1,"PT_VERTICAL_COVER","01512","SZT","85389099","27.12.40.0",null,"5901988015121","PT - Deux couvercles verticaux D180 H700 12M","PT - Two Vertical Lids D180 H700 12M","EMP- PANEL LATERAL (2UDS) D180 H700 12M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H700 12M"]
["01513","ZENERGY PT - POKRYWA TYLNA H700 W800, 12M IP30",63.4,"1-ZE-03",null,null,"PT_BACK_PLATE","01513","SZT","85389099","27.12.40.0",null,"5901988015138","PT - Capot arrière H700 L800, 12M IP30","PT - Rear cover H700 W800, 12M IP30","EMP- PANEL TRASERO H700 W800, 12M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H700 W800, 12M IP30"]
["01515","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H850 15M",139.9,"1-ZE-03",1.6666666666666666E-2,1,"PT_VERTICAL_COVER","01515","SZT","85389099","27.12.40.0",null,"5901988015152","PT - Deux couvercles verticaux D180 H850 15M","PT - Two Vertical Lids D180 H850 15M","EMP- PANEL LATERAL (2UDS) D180 H850 15M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H850 15M"]
["01516","ZENERGY PT - POKRYWA TYLNA H850 W800, 15M IP30",79.3,"1-ZE-03",null,null,"PT_BACK_PLATE","01516","SZT","85389099","27.12.40.0",null,"5901988015169","PT - Capot arrière H850 L800, 15M IP30","PT - Rear cover H850 W800, 15M IP30","EMP- PANEL TRASERO H850 W800, 15M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H850 W800, 15M IP30"]
["01518","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H1000 18M",161.1,"1-ZE-03",0.05,4,"PT_VERTICAL_COVER","01518","SZT","85389099","27.12.40.0",null,"5901988015183","PT - Deux couvercles verticaux D180 H1000 18M","PT - Two Vertical Lids D180 H1000 18M","EMP- PANEL LATERAL (2UDS) D180 H1000 18M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H1000 18M"]
["01519","ZENERGY PT - POKRYWA TYLNA H1000 W800, 18M IP30",95.2,"1-ZE-03",null,null,"PT_BACK_PLATE","01519","SZT","85389099","27.12.40.0",null,"5901988015190","PT - Capot arrière H1000 L800, 18M IP30","PT - Rear cover H1000 W800, 18M IP30","EMP- PANEL TRASERO H1000 W800, 18M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1000 W800, 18M IP30"]
["01521","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H1150 21M",186.6,"1-ZE-03",1.6666666666666666E-2,1,"PT_VERTICAL_COVER","01521","SZT","85389099","27.12.40.0",null,"5901988015213","PT - Deux couvercles verticaux D180 H1150 21M","PT - Two Vertical Lids D180 H1150 21M","EMP- PANEL LATERAL (2UDS) D180 H1150 21M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H1150 21M"]
["01522","ZENERGY PT - POKRYWA TYLNA H1150 W800, 21M IP30",111.3,"1-ZE-03",null,null,"PT_BACK_PLATE","01522","SZT","85389099","27.12.40.0",null,"5901988015220","PT - Capot arrière H1150 L800, 21M IP30","PT - Rear cover H1150 W800, 21M IP30","EMP- PANEL TRASERO H1150 W800, 21M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1150 W800, 21M IP30"]
["01524","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H1300 24M",205.6,"1-ZE-03",null,null,"PT_VERTICAL_COVER","01524","SZT","85389099","27.12.40.0",null,"5901988015244","PT - Deux couvercles verticaux D180 H1300 24M","PT - Two Vertical Lids D180 H1300 24M","EMP- PANEL LATERAL (2UDS) D180 H1300 24M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H1300 24M"]
["01525","ZENERGY PT - POKRYWA TYLNA H1300 W800, 24M IP30",127.2,"1-ZE-03",null,null,"PT_BACK_PLATE","01525","SZT","85389099","27.12.40.0",null,"5901988015251","PT - Capot arrière H1300 L800, 24M IP30","PT - Rear cover H1300 W800, 24M IP30","EMP- PANEL TRASERO H1300 W800, 24M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1300 W800, 24M IP30"]
["01527","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H1450 27M",221.5,"1-ZE-03",4.1666666666666664E-2,4,"PT_VERTICAL_COVER","01527","SZT","85389099","27.12.40.0",null,"5901988015275","PT - Deux couvercles verticaux D180 H1450 27M","PT - Two Vertical Lids D180 H1450 27M","EMP- PANEL LATERAL (2UDS) D180 H1450 27M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H1450 27M"]
["01528","ZENERGY PT - POKRYWA TYLNA H1450 W800, 27M IP30",143.1,"1-ZE-03",null,null,"PT_BACK_PLATE","01528","SZT","85389099","27.12.40.0",null,"5901988015282","PT - Capot arrière H1450 L800, 27M IP30","PT - Rear cover H1450 W800, 27M IP30","EMP- PANEL TRASERO H1450 W800, 27M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1450 W800, 27M IP30"]
["01530","ZENERGY PT - DWIE POKRYWY PIONOWE D180 H1600 30M",278.8,"1-ZE-03",9.166666666666666E-2,5,"PT_VERTICAL_COVER","01530","SZT","85389099","27.12.40.0",null,"5901988015305","PT - Deux couvercles verticaux D180 H1600 30M","PT - Two Vertical Lids D180 H1600 30M","EMP- PANEL LATERAL (2UDS) D180 H1600 30M","ZENERGY PT - KÉT FÜGGŐLEGES BURKOLAT D180 H1600 30M"]
["01531","ZENERGY PT - POKRYWA TYLNA H1600 W800, 30M IP30",159,"1-ZE-03",null,null,"PT_BACK_PLATE","01531","SZT","85389099","27.12.40.0",null,"5901988015312","PT - Capot arrière H1600 L800, 30M IP30","PT - Back cover H1600 W800, 30M IP30","EMP- PANEL TRASERO H1600 W800, 30M IP30","ZENERGY PT - HÁTSÓ BURKOLAT H1600 W800, 30M IP30"]
["01606","ZENERGY ON/PT - DRZWI PEŁNE IP40, 6 MOD, H400 X W800",129.30000000000001,"1-ZE-03",3.3333333333333333E-2,4,"ON-PT_DOORS","01606","SZT","85389099",null,null,"5901988016067","PT - Portes transparentes IP40, MOD 6H, H400 x L800","ON/PT - Full door IP40, 6 mod, H400 x W800","ON/EMP- PUERTA OPACA IP40, 6 MOD, H400XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 6 MOD, H400 X W800"]
["01607","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 6H MOD, H400 X W800",214.1,"1-ZE-03",null,null,"ON-PT_DOORS","01607","SZT","85389099",null,null,"5901988016074","ON/PT - Portes transparentes IP40, MOD 6H, H400 x L600","ON/PT - Transparent door IP40, 6H MOD, H400 x W800","ON/EMP- PUERTA TRANSP. IP40, 6H MOD, H400XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 6H MOD, H400 X W800"]
["01609","ZENERGY ON/PT - DRZWI PEŁNE IP40, 9 MOD, H550 X W800",144.19999999999999,"1-ZE-03",0.01,1,"ON-PT_DOORS","01609","SZT","85389099",null,null,"5901988016098","PT - Portes transparentes IP40, MOD 9H, H550 x L800","ON/PT - Full door IP40, 9 mod, H550 x W800","ON/EMP- PUERTA OPACA IP40, 9 MOD, H550XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 9 MOD, H550 X W800"]
["01610","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 9H MOD, H550 X W800",237.4,"1-ZE-03",null,null,"ON-PT_DOORS","01610","SZT","85389099",null,null,"5901988016104","ON/PT - Portes transparentes IP40, MOD 9H, H550 x L600","ON/PT - Transparent door IP40, 9H MOD, H550 x W800","ON/EMP- PUERTA TRANSP. IP40, 9H MOD, H550XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 9H MOD, H550 X W800"]
["01612","ZENERGY ON/PT - DRZWI PEŁNE IP40, 12 MOD, H700 X W800",153.69999999999999,"1-ZE-03",null,null,"ON-PT_DOORS","01612","SZT","85389099",null,null,"5901988016128","PT - Portes transparentes IP40, MOD 12H, H700 x L800","ON/PT - Full door IP40, 12 mod, H700 x W800","ON/EMP- PUERTA OPACA IP40, 12 MOD, H700XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 12 MOD, H700 X W800"]
["01613","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 12H MOD, H700 X W800",253.3,"1-ZE-03",null,null,"ON-PT_DOORS","01613","SZT","85389099",null,null,"5901988016135","ON/PT - Portes transparentes IP40, MOD 12H, H700 x L600","ON/PT - Transparent door IP40, 12H MOD, H700 x W800","ON/EMP- PUERTA TRANSP. IP40, 12H MOD, H700XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 12H MOD, H700 X W800"]
["01615","ZENERGY ON/PT - DRZWI PEŁNE IP40, 15 MOD, H850 X W800",190.8,"1-ZE-03",0.01,1,"ON-PT_DOORS","01615","SZT","85389099",null,null,"5901988016159","PT - Portes transparentes IP40, MOD 15H, H850 x L800","ON/PT - Full door IP40, 15 mod, H850 x W800","ON/EMP- PUERTA OPACA IP40, 15 MOD, H850XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 15 MOD, H850 X W800"]
["01616","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 15H MOD, H850 X W800",304.2,"1-ZE-03",null,null,"ON-PT_DOORS","01616","SZT","85389099",null,null,"5901988016166","ON/PT - Portes transparentes IP40, MOD 15H, H850 x L600","ON/PT - Transparent door IP40, 15H MOD, H850 x W800","ON/EMP- PUERTA TRANSP. IP40, 15H MOD, H850XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 15H MOD, H850 X W800"]
["01618","ZENERGY ON/PT - DRZWI PEŁNE IP40, 18 MOD, H1000 X W800",237.4,"1-ZE-03",6.6666666666666666E-2,6,"ON-PT_DOORS","01618","SZT","85389099",null,null,"5901988016180","PT - Portes transparentes IP40, MOD 18H, H1000 x L800","ON/PT - Full door IP40, 18 mod, H1000 x W800","ON/EMP- PUERTA OPACA IP40, 18 MOD, H1000XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 18 MOD, H1000 X W800"]
["01619","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 18H MOD, H1000 X W800",359.3,"1-ZE-03",null,null,"ON-PT_DOORS","01619","SZT","85389099",null,null,"5901988016197","ON/PT - Portes transparentes IP40, MOD 18H, H1000 x L600","ON/PT - Transparent door IP40, 18H MOD, H1000 x W800","ON/EMP- PUERTA TRANSP. IP40, 18H MOD, H1000XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 18H MOD, H1000 X W800"]
["01621","ZENERGY ON/PT - DRZWI PEŁNE IP40, 21 MOD, H1150 X W800",285.10000000000002,"1-ZE-03",3.3333333333333333E-2,2,"ON-PT_DOORS","01621","SZT","85389099",null,null,"5901988016210","PT - Portes transparentes IP40, MOD 21H, H1150 x L800","ON/PT - Full door IP40, 21 mod, H1150 x W800","ON/EMP- PUERTA OPACA IP40, 21 MOD, H1150XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 21 MOD, H1150 X W800"]
["01622","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 21H MOD, H1150 X W800",418.7,"1-ZE-03",null,null,"ON-PT_DOORS","01622","SZT","85389099",null,null,"5901988016227","ON/PT - Portes transparentes IP40, MOD 21H, H1150 x L600","ON/PT - Transparent door IP40, 21H MOD, H1150 x W800","ON/EMP- PUERTA TRANSP. IP40, 21H MOD, H1150XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 21H MOD, H1150 X W800"]
["01624","ZENERGY ON/PT - DRZWI PEŁNE IP40, 24 MOD, H1300 X W800",332.8,"1-ZE-03",null,null,"ON-PT_DOORS","01624","SZT","85389099",null,null,"5901988016241","PT - Portes transparentes IP40, MOD 24H, H1300 x L800","ON/PT - Full door IP40, 24 mod, H1300 x W800","ON/EMP- PUERTA OPACA IP40, 24 MOD, H1300XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 24 MOD, H1300 X W800"]
["01625","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 24H MOD, H1300 X W800",461.1,"1-ZE-03",0.01,1,"ON-PT_DOORS","01625","SZT","85389099",null,null,"5901988016258","ON/PT - Portes transparentes IP40, MOD 24H, H1300 x L600","ON/PT - Transparent door IP40, 24H MOD, H1300 x W800","ON/EMP- PUERTA TRANSP. IP40, 24H MOD, H1300XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 24H MOD, H1300 X W800"]
["01627","ZENERGY ON/PT - DRZWI PEŁNE IP40, 27 MOD, H1450 X W800",380.5,"1-ZE-03",0.01,1,"ON-PT_DOORS","01627","SZT","85389099",null,null,"5901988016272","PT - Portes transparentes IP40, MOD 27H, H1450 x L800","ON/PT - Full door IP40, 27 mod, H1450 x W800","ON/EMP- PUERTA OPACA IP40, 27 MOD, H1450XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 27 MOD, H1450 X W800"]
["01628","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 27H MOD, H1450 X W800",502.4,"1-ZE-03",null,null,"ON-PT_DOORS","01628","SZT","85389099",null,null,"5901988016289","ON/PT - Portes transparentes IP40, MOD 27H, H1450 x L600","ON/PT - Transparent door IP40, 27H MOD, H1450 x W800","ON/EMP- PUERTA TRANSP. IP40, 27H MOD, H1450XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 27H MOD, H1450 X W800"]
["01630","ZENERGY ON/PT - DRZWI PEŁNE IP40, 30 MOD, H1600 X W800",428.2,"1-ZE-03",0.14166666666666666,7,"ON-PT_DOORS","01630","SZT","85389099",null,null,"5901988016302","PT - Portes transparentes IP40, MOD 30H, H1600 x L800","ON/PT - Full door IP40, 30 mod, H1600 x W800","ON/EMP- PUERTA OPACA IP40, 30 MOD, H1600XW800","ZENERGY ON/PT – TELJES AJTÓ IP40, 30 MOD, H1600 X W800"]
["01631","ZENERGY ON/PT - DRZWI TRANSPARENTNE IP40, 30H MOD, H1600 X W800",653,"1-ZE-03",null,null,"ON-PT_DOORS","01631","SZT","85389099",null,null,"5901988016319","ON/PT - Portes transparentes IP40, MOD 30H, H1600 x L600","ON/PT - Transparent door IP40, 30H MOD, H1600 x W800","ON/EMP- PUERTA TRANSP. IP40, 30H MOD, H1600XW800","ZENERGY ON/PT – ÁTLÁTSZÓ AJTÓK IP40, 30H MOD, H1600 X W800"]
["02000","ZENERGY - ZABUDOWA BATERII H2000, ASEL",191.4,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020002","OE - Batterie intégrée H2000, ASEL","OE - Installation of H2000, ASEL batteries","*OE- Carcasa de batería H2000, ASEL","ZENERGY - H2000 AKKUMULÁTORHÁZ, ASEL"]
["02001","ZENERGY - PANEL BATERI DŁAWIKOWEJI, ASEL",136.4,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020019","OE - Panneau de charge, ASEL","OE - Choke battery panel, ASEL","*OE- Panel de baterías de choque, ASEL","ZENERGY - SZÍJTÓ AKKUMULÁTOR PANEL, ASEL"]
["02002","ZENERGY - PÓŁKA BATERI D400, ASEL",69,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020026","OE - Etagère à piles P400, ASEL","OE - D400, ASEL Battery Shelf","*OE- Bandeja de batería D400, ASEL","ZENERGY - D400 AKKUMULÁTORPOLC, ASEL"]
["02003","ZENERGY - PÓŁKA BATERI W600, KAVAR",39.799999999999997,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020033","OE - Tablette batterie L600, KAVAR","OE - W600, KAVAR battery shelf","*OE- Bandeja de batería W600, KAVAR","ZENERGY - W600 AKKUMULÁTORPOLC, KAVAR"]
["02004","ZENERGY - PÓŁKA BATERI W700, KAVAR",47.2,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020040","OE - Tablette batterie W700, KAVAR","OE - W700, KAVAR battery shelf","*OE- Bandeja de batería W700, KAVAR","ZENERGY - W700 AKKUMULÁTORPOLC, KAVAR"]
["02005","ZENERGY - PÓŁKA BATERI W800, KAVAR",54.6,"1-ZE-10",0.15,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020057","OE - Tablette batterie L800, KAVAR","OE - W800, KAVAR battery shelf","*OE- Bandeja de batería W800, KAVAR","ZENERGY - W800 AKKUMULÁTORPOLC, KAVAR"]
["02015","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, OSŁONA CZOŁOWA FUPACT 00, W800, 5M / 650",70.8,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020156","OE - Batterie enfichable, panneau de droite, Fupact 00, L800, face avant 5M / 650","OE - Plug-in battery, right panel, Front cover Fupact 00, W800, 5M / 650","*OE- Batería enchufable, panel derecho, cubierta frontal Fupact 00, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, ELSŐ BURKOLAT FUPACT 00, W800, 5M / 650"]
["02025","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, OSŁONA CZOŁOWA FUPACT 00, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020255","OE - Batterie enfichable, panneau gauche, Fupact 00, L800, 5M / 650 capot avant","OE - Plug-in battery, left panel, Front cover Fupact 00, W800, 5M / 650","*OE- Batería enchufable, panel izquierdo, cubierta frontal Fupact 00, W800, 5M / 650","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, BAL PANEL, ELSŐ BURKOLAT FUPACT 00, W800, 5M / 650"]
["02031","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, OSŁONA CZOŁOWA FH125, W800, 5M / 650",70.8,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020316","OE - Batterie Plug & Play, panneau droit, protecteur avant FH125, L800, 5M / 650","OE - Plug-in battery, right panel, Front cover FH125, W800, 5M / 650","*OE- Batería enchufable, panel derecho, cubierta frontal FH125, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, ELSŐ BURKOLAT FH125, W800, 5M / 650"]
["02032","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, OSŁONA CZOŁOWA FH63, W800, 5M / 650",70.8,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020323","OE - Batterie Plug & Play, panneau droit, protecteur avant FH63, L800, 5M / 650","OE - Plug-in battery, right panel, Front cover FH63, W800, 5M / 650","*OE- Batería enchufable, panel derecho, cubierta frontal FH63, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, ELSŐ BURKOLAT FH63, W800, 5M / 650"]
["02033","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, OSŁONA CZOŁOWA 2XFH63, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020330","OE - Batterie enfichable, panneau droit, face avant 2xFH63, L800, 5M / 650","OE - Plug-in battery, right panel, 2xFH63, W800, 5M / 650 Front cover","*OE- Batería enchufable, panel derecho, cubierta frontal 2xFH63, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, ELSŐ BURKOLAT 2XFH63, W800, 5M / 650"]
["02034","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, OSŁONA CZOŁOWA FH32, W800, 5M / 650",70.8,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020347","OE - Batterie Plug & Play, panneau droit, protecteur avant FH32, L800, 5M / 650","OE - Plug-in battery, right panel, Front cover FH32, W800, 5M / 650","*OE- Batería enchufable, panel derecho, cubierta frontal FH32, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, ELSŐ BURKOLAT FH32, W800, 5M / 650"]
["02035","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, OSŁONA CZOŁOWA 2XFH32, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020354","OE - Batterie enfichable, panneau droit, face avant 2xFH32, L800, 5M / 650","OE - Plug-in battery, right panel, 2xFH32, W800, 5M / 650 Front cover","*OE- Batería enchufable, panel derecho, cubierta frontal 2xFH32, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, JOBB PANEL, ELSŐ BURKOLAT 2XFH32, W800, 5M / 650"]
["02036","ZENERGY - BATERIA WTYKOWA, PANEL PRAWY, D600, W800, PODSTAWA",104.8,"1-ZE-10",5.8333333333333334E-2,1,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988020361","OE - Batterie Plug & Play, panneau latéral droit, P600, L800, base","OE - Plug-in battery, right panel, D600, W800, base","*OE- Batería enchufable, panel derecho, D600, W800, base","ZENERGY - DUGATÓ AKKUMULÁTOR, JOBB PANEL, D600, W800, ALAP"]
["02041","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, OSŁONA CZOŁOWA FH125, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020415","OE - Batterie Plug & Play, panneau gauche, protection frontale FH125, L800, 5M / 650","OE - Plug-in battery, left panel, Front cover FH125, W800, 5M / 650","*OE- Batería enchufable, panel izquierdo, cubierta frontal FH125, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, BAL PANEL, ELSŐ BURKOLAT FH125, W800, 5M / 650"]
["02042","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, OSŁONA CZOŁOWA FH63, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020422","OE - Batterie Plug & Play, panneau gauche, protecteur avant FH63, L800, 5M / 650","OE - Plug-in battery, left panel, Front cover FH63, W800, 5M / 650","*OE- Batería enchufable, panel izquierdo, cubierta frontal FH63, W800, 5M / 650","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, BAL PANEL, ELSŐ BURKOLAT FH63, W800, 5M / 650"]
["02043","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, OSŁONA CZOŁOWA 2XFH63, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020439","OE - Batterie enfichable, panneau gauche, face avant 2xFH63, L800, 5M / 650","OE - Plug-in battery, left panel, 2xFH63, W800, 5M / 650 Front cover","*OE- Batería enchufable, panel izquierdo, cubierta frontal 2xFH63, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, BAL PANEL, ELSŐ BURKOLAT 2XFH63, W800, 5M / 650"]
["02044","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, OSŁONA CZOŁOWA FH32, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020446","OE - Batterie Plug & Play, panneau gauche, protecteur avant FH32, L800, 5M / 650","OE - Plug-in battery, left panel, Front cover FH32, W800, 5M / 650","*OE- Batería enchufable, panel izquierdo, cubierta frontal FH32, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, BAL PANEL, ELSŐ BURKOLAT FH32, W800, 5M / 650"]
["02045","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, OSŁONA CZOŁOWA 2XFH32, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020453","OE - Batterie enfichable, panneau gauche, face avant 2xFH32, L800, 5M / 650","OE - Plug-in battery, left panel, 2xFH32, W800, 5M / 650 Front cover","*OE- Batería enchufable, panel izquierdo, cubierta frontal 2xFH32, W800, 5M / 650","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, ELSŐ BURKOLAT 2XFH32, W800, 5M / 650"]
["02046","ZENERGY - BATERIA WTYKOWA, PANEL LEWY, D600, W800, PODSTAWA",104.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,"171020LK","5901988020460","OE - Batterie Plug & Play, panneau gauche, P600, L800, base","OE - Plug-in battery, left panel, D600, W800, base","*OE- Batería enchufable, panel izquierdo, D600, W800, base","ZENERGY - DUGATÓ AKKUMULÁTOR, BAL PANEL, D600, W800, ALAP"]
["02051","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA 2XFH32, W800, 4M / 650",63.3,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020514","OE - Batterie enfichable, commande par le couvercle avant 2xFH32, L800, 4M / 650","OE - Plug-in battery, 2xFH32, W800, 4M / 650 control Front cover","*OE- Batería enchufable, 2xFH32, W800, cubierta frontal 4M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT 2XFH32, W800, 4M / 650"]
["02052","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA 2XFH32, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020521","OE - Batterie enfichable, commande par le couvercle avant 2xFH32, L800, 5M / 650","OE - Plug-in battery, 2xFH32, W800, 5M / 650 control Front cover","*OE- Batería enchufable, 2xFH32, W800, cubierta frontal 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT 2XFH32, W800, 5M / 650"]
["02053","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA 2XFH32, W800, 6M / 650",75.900000000000006,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020538","OE - Batterie enfichable, commande par le couvercle avant 2xFH32, L800, 6M / 650","OE - Plug-in battery, 2xFH32, W800, 6M / 650 control Front cover","*OE- Batería enchufable, 2xFH32, W800, tapa frontal 6M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT 2XFH32, W800, 6M / 650"]
["02054","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA REGULATORA, W800, 5M / 650",70.8,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020545","OE - Batterie enfichable, régulateur frontal, L800, 5M / 650","OE - Plug-in battery, regulator Front cover, W800, 5M / 650","*OE- Batería enchufable, tapa frontal del regulador, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, SZABÁLYOZÓ ELSŐ BURKOLAT, W800, 5M / 650"]
["02055","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA PERFOROWANA, W800, 4M / 650",70,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020552","OE - Batterie Plug & Play, protection frontale perforée, L800, 4M / 650","OE - Plug-in battery, Perforated Front cover, W800, 4M / 650","*OE- Batería enchufable, cubierta frontal perforada, W800, 4M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PERFORÁLT ELSŐ BURKOLAT, W800, 4M / 650"]
["02056","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA PERFOROWANA, W800, 5M / 650",80.599999999999994,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020569","OE - Batterie Plug & Play, protection frontale perforée, L800, 5M / 650","OE - Plug-in battery, Perforated Front cover, W800, 5M / 650","*OE- Batería enchufable, cubierta frontal perforada, W800, 5M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PERFORÁLT ELSŐ BURKOLAT, W800, 5M / 650"]
["02057","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA PERFOROWANA, W800, 6M / 650",86,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020576","OE - Batterie Plug & Play, protection frontale perforée, L800, 6M / 650","OE - Plug-in battery, Perforated Front cover, W800, 6M / 650","*OE- Batería enchufable, cubierta frontal perforada, W800, 6M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, PERFORÁLT ELSŐ BURKOLAT, W800, 6M / 650"]
["02059","ZENERGY - BATERIA WTYKOWA, OSŁONA CZOŁOWA STEROWANIA, PEŁNA 2XFH32, W800, 6M / 650",75.900000000000006,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020590","OE - Batterie enfichable, face avant, pleine 2xFH32, L800, 6M / 650","OE - Plug-in battery, control Front cover, Plain 2xFH32, W800, 6M / 650","*OE- Batería enchufable, cubierta de control frontal, completa 2xFH32, W800, 6M / 650","ZENERGY - DUGATOZÓ AKKUMULÁTOR, VEZÉRLŐ ELSŐ BURKOLAT, TELJES 2XFH32, W800, 6M / 650"]
["02061","ZENERGY - BATERIA WTYKOWA, PŁYTA STEROWANIA W800, 4M 2XFH32",91.1,"1-ZE-10",0.01,1,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020613","OE - Batterie enfichable, panneau de commande L800, 4M 2xFH32","OE - Plugin capacitor bank, W800 control board, 4M 2xFH32","*OE- Batería enchufable, tablero de control W800, 4M 2xFH32","ZENERGY - DUGATTHATÓ AKKUMULÁTOR, W800 VEZÉRLŐPÁR, 4M 2XFH32"]
["02064","ZENERGY - BATERIA WTYKOWA, PŁYTA STEROWANIA W800, 5M 2XFH32",105.1,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020644","OE - Batterie enfichable, platine de commande L800, 5M 2xFH32","OE - Plugin capacitor bank, W800 control board, 5M 2xFH32","*OE- Batería enchufable, tablero de control W800, 5M 2xFH32","ZENERGY - DUGATOZÓ AKKUMULÁTOR, W800 VEZÉRLŐPÁR, 5M 2XFH32"]
["02073","ZENERGY - BATERIA WTYKOWA, D800, 2XWSPORNIK POD DŁAWIKI",23.7,"1-ZE-10",null,null,"POWER_QUALITY",null,"SZT","85389099",null,null,"5901988020736","OE - Batterie Plug & Play, P800, 2x support d'étrangleur","OE - Plugin capacitor bank, D800, 2xbracket for chokes","*OE- Batería enchufable, D800, 2x soporte para estranguladores","ZENERGY - DUGATÓ AKKUMULÁTOR, D800, 2X SZÍJTÓ KERET"]
["02200","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-30",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022006","OM - Couvercle horizontal L1200 IP-30","OM - Two Horizontal Lids W1200 IP-30","OM- TECHO /SUELO (2UDS) W1200 IP30 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-30"]
["02201","produkt wycofany (ZENERGY OM - COKÓŁ W1200 IP-30)",376.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022013","produit invalidé OM - Socle L1200 IP-30","product cancelled OM - W1200 IP-30 plinth","OM- ZOCALO W1200 IP30","megszűnt termék (ZENERGY OM - PLINTH W1200 IP-30)"]
["02203","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022037","OM - Couvercle horizontal L1200 IP-30 avec ouverture 81x222 sous IP-55","OM - Two Horizontal Covers W1200 IP-30 with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200 IP30  CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["02204","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022044","OM - Couvercle horizontal IP-30 L1200 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal Covers W1200 IP-30 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200 IP30  CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-30 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["02205","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022051","OM - Couvercle horizontal L1200 IP-30 avec trois ouvertures 81x222 sous le passage IP-55","OM - Two Horizontal Covers W1200 IP-30 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200 IP30  CON TRES AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-30 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["02206","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-30 Z CZTEREMA OTWORAMI 81X222 POD PRZEPUST IP-55",203.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022068","OM - Couvercle horizontal L1200 IP-30 avec quatre ouvertures 81x222 sous passage IP-55","OM - Two Horizontal Covers W1200 IP-30 with FOUR holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200 IP30  CON QUATRO AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-30 NÉGY LYUKAL 81X222 AZ IP-55 LÖVEDEKHEZ"]
["02207","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1200 D230 IP-30",218.3,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","02207","SZT","85389099","27.12.40.0",null,"5901988022075","OM - Couvercle horizontal socle L1200 P230 IP-30","OM - Two Horizontal Plinth Covers W1200 D230 IP-30","OM- TECHO/SUELO (2UDS) W1200 D230 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1200 D230 IP-30"]
["02208","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-30 Z CZTEREMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",1.6666666666666666E-2,2,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988022082"]
["02209","ZENERGY OM - POKRYWA TYLNA W1200 H550 9M IP-30",279.7,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022099","OM - Couvercle arrière L1200 H550 9M IP-30","OM - Rear Cover W1200 H550 9M IP-30","OM- PANEL TRASERO W1200 H550 9M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H550 9M IP-30"]
["02212","ZENERGY OM - POKRYWA TYLNA W1200 H700 12M IP-30",281.89999999999998,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022129","OM - Couvercle arrière L1200 H700 12M IP-30","OM - Rear Cover W1200 H700 12M IP-30","OM- PANEL TRASERO W1200 H700 12M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H700 12M IP-30"]
["02215","ZENERGY OM - POKRYWA TYLNA W1200 H850 15M IP-30",317.5,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022150","OM - Couvercle arrière L1200 H850 15M IP-30","OM - Rear Cover W1200 H850 15M IP-30","OM- PANEL TRASERO W1200 H850 15M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H850 15M IP-30"]
["02218","ZENERGY OM - POKRYWA TYLNA W1200 H1000 18M IP-30",353.2,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022181","OM - Couvercle arrière L1200 H1000 18M IP-30","OM - Rear Cover W1200 H1000 18M IP-30","OM- PANEL TRASERO W1200 H1000 18M IP30","HOGYNERGY OM - HÁTSÓ BURKOLAT W1200 H1000 18M IP-30"]
["02221","ZENERGY OM - POKRYWA TYLNA W1200 H1150 21M IP-30",371.5,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022211","OM - Couvercle arrière L1200 H1150 21M IP-30","OM - Rear Cover W1200 H1150 21M IP-30","OM- PANEL TRASERO W1200 H1150 21M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1150 21M IP-30"]
["02224","ZENERGY OM - POKRYWA TYLNA W1200 H1300 24M IP-30",392,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022242","OM - Couvercle arrière L1200 H1300 24M IP-30","OM - Rear Cover W1200 H1300 24M IP-30","OM- PANEL TRASERO W1200 H1300 24M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1300 24M IP-30"]
["02227","ZENERGY OM - POKRYWA TYLNA W1200 H1450 27M IP-30",408.2,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022273","OM - Couvercle arrière L1200 H1450 27M IP-30","OM - Rear Cover W1200 H1450 27M IP-30","OM- PANEL TRASERO W1200 H1450 27M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1450 27M IP-30"]
["02228","ZENERGY OM - POKRYWA TYLNA W1200 H1600 28M IP-30",667.4,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022280","OM - Couvercle arrière L1200 H1600 28M IP-30","OM - Rear Cover W1200 H1600 28M IP-30","OM- PANEL TRASERO W1200 H1600 28M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1600 28M IP-30"]
["02229","ZENERGY OM - POKRYWA TYLNA W1200 H1550 29M IP-30",454.7,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022297","OM - Couvercle arrière L1200 H1550 29M IP-30","OM - Rear Cover W1200 H1550 29M IP-30","OM- PANEL TRASERO W1200 H1550 29M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1550 29M IP-30"]
["02230","ZENERGY OM - POKRYWA TYLNA W1200 H1700 30M IP-30",703.1,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022303","OM - Couvercle arrière L1200 H1700 30M IP-30","OM - Rear Cover W1200 H1700 30M IP-30","OM- PANEL TRASERO W1200 H1700 30M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1700 30M IP-30"]
["02233","ZENERGY OM - POKRYWA TYLNA W1200 H1850 33M IP-30",907.2,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022334","OM - Couvercle arrière L1200 H1850 33M IP-30","OM - Rear Cover W1200 H1850 33M IP-30","OM- PANEL TRASERO W1200 H1850 33M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1850 33M IP-30"]
["02236","ZENERGY OM - POKRYWA TYLNA W1200 H2000 36M IP-30",981.7,"1-ZE-09",3.3333333333333333E-2,4,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022365","OM - Couvercle arrière L1200 H2000 36M IP-30","OM - Rear Cover W1200 H2000 36M IP-30","OM- PANEL TRASERO W1200 H2000 36M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H2000 36M IP-30"]
["02239","ZENERGY OM - POKRYWA TYLNA W1200 H2150 39M IP-30",1084.3,"1-ZE-09",5.8333333333333334E-2,2,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988022396","OM - Couvercle arrière L1200 H2150 39M IP-30","OM - Rear Cover W1200 H2150 39M IP-30","OM- PANEL TRASERO W1200 H2150 39M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H2150 39M IP-30"]
["02240","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-30",253.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022402","OM - Deux couvercles horizontaux L1200 P300 P300 IP-30","OM - Two Horizontal Covers W1200 D300 IP-30","*OM - Dos cubiertas horizontales W1200 D300 IP-30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-30"]
["02241","produkt wycofany (ZENERGY OM - COKÓŁ W1200 D300 IP-30)",436.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022419","produit invalidé OM - Socle L1200 P300 P300 IP-30","product cancelled OM - Plinth W1200 D300 IP-30","*producto anulado OM - Zócalo, W1200 D300 IP-30","kivont termék (ZENERGY OM - PLINTH W1200 D300 IP-30)"]
["02243","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",253.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022433","OM - Deux couvercles horizontaux L1200 P300 IP-30 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1200 D300 IP-30 with an opening 81x222 for the IP-55 bushing","*OM- dos cubiertas horizontales W1200 D300 IP-30 con una abertura de 81x222 para un casquillo IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["02244","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",253.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022440","OM - Deux couvercles horizontaux L1200 P300 P300 IP-30 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1200 D300 IP-30 with TWO holes 81x222 for the IP-55 bushing","*OM - Dos cubiertas horizontales W1200 D300 IP-30 con DOS agujeros 81x222 para la alcantarilla IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-30 KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["02245","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",253.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022457","OM - Deux couvercles horizontaux L1200 P300 IP-30 avec TROIS trous 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1200 D300 IP-30 with THREE holes 81x222 for the IP-55 bushing","*OM - Dos cubiertas horizontales W1200 D300 IP-30 con TRES agujeros 81x222 para el casquillo IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-30 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["02246","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-30 Z CZTEREMA OTWORAMI 81X222 POD PRZEPUST IP-55",253.6,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988022464","OM - Deux couvercles horizontaux L1200 P300 IP-30 avec QUATRE trous 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1200 D300 IP-30 with FOUR holes 81x222 for the IP-55 bushing","*OM - Dos cubiertas horizontales W1200 D300 IP-30 con CUATRO agujeros de 81x222 para alcantarilla IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-30 NÉGY LYUKAL 81X222 AZ IP-55 LÖVEDEKHEZ"]
["02247","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1200 D300 IP-30",253.6,"1-ZE-09",3.3333333333333333E-2,2,"OM_HORIZONTAL_COVER","02247","SZT","85389099","27.12.40.0",null,"5901988022471","OM - Couvercle horizontal socle L1200 P300 IP-30","OM - Two Horizontal Plinth Covers W1200 D300 IP-30","OM- TECHO/SUELO (2UDS) W1200 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1200 D300 IP-30"]
["02300","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-55",263.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023003","OM - Couvercle horizontal L1200 IP-55","OM - Two Horizontal Covers W1200 IP-55","OM- TECHO /SUELO (2UDS) W1200  IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-55"]
["02301","produkt wycofany (ZENERGY OM - COKÓŁ W1200 IP-55)",383.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023010","produit invalidé OM - Spcle L1200 IP-55","product cancelled OM - W1200 IP-55 plinth","OM- ZOCALO W1200 IP55","kivont termék (ZENERGY OM - PLINTH W1200 IP-55)"]
["02303","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",263.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023034","OM - Couvercle horizontal L1200 IP-55 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W1200 IP-55 Covers with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200  IP55 CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["02304","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",263.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023041","OM - Couvercle horizontal IP-55 L1200 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal Covers W1200 IP-55 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200  IP55 CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-55 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["02305","ZENERGY OM - DWIE POKRYWY POZIOME W1200 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",263.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023058","OM - Couvercle horizontal L1200 IP-55 avec trois ouvertures 81x222 sous le passage IP-55","OM - Two Horizontal Covers W1200 IP-55 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1200  IP55 CON TRES AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 IP-55 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["02306","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W1200 IP-55",248.2,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988023065"]
["02307","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1200 D230 IP-55",263.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","02307","SZT","85389099","27.12.40.0",null,"5901988023072","OM - Couvercle horizontal socle L1200 P230 IP-55","OM - Two Horizontal Plinth Covers W1200 D230 IP-55","OM- TECHO/SUELO (2UDS) W1200 D230 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1200 D230 IP-55"]
["02309","ZENERGY OM - POKRYWA TYLNA W1200 H550 9M IP-55",470.9,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023096","OM - Couvercle arrière L1200 H550 9M IP-55","OM - Rear Cover W1200 H550 9M IP-55","OM- PANEL TRASERO W1200 H550 9M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H550 9M IP-55"]
["02312","ZENERGY OM - POKRYWA TYLNA W1200 H700 12M IP-55",480.6,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023126","OM - Couvercle arrière L1200 H700 12M IP-55","OM - Rear Cover W1200 H700 12M IP-55","OM- PANEL TRASERO W1200 H700 12M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H700 12M IP-55"]
["02315","ZENERGY OM - POKRYWA TYLNA W1200 H850 15M IP-55",529.20000000000005,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023157","OM - Couvercle arrière L1200 H850 15M IP-55","OM - Rear Cover W1200 H850 15M IP-55","OM- PANEL TRASERO W1200 H850 15M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H850 15M IP-55"]
["02318","ZENERGY OM - POKRYWA TYLNA W1200 H1000 18M IP-55",557.29999999999995,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023188","OM - Couvercle arrière L1200 H1000 18M IP-55","OM - Rear Cover W1200 H1000 18M IP-55","OM- PANEL TRASERO W1200 H1000 18M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1000 18M IP-55"]
["02321","ZENERGY OM - POKRYWA TYLNA W1200 H1150 21M IP-55",601.6,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023218","OM - Couvercle arrière L1200 H1150 21M IP-55","OM - Rear Cover W1200 H1150 21M IP-55","OM- PANEL TRASERO W1200 H1150 21M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1150 21M IP-55"]
["02324","ZENERGY OM - POKRYWA TYLNA W1200 H1300 24M IP-55",641.5,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023249","OM - Couvercle arrière L1200 H1300 24M IP-55","OM - Rear Cover W1200 H1300 24M IP-55","OM- PANEL TRASERO W1200 H1300 24M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1300 24M IP-55"]
["02327","ZENERGY OM - POKRYWA TYLNA W1200 H1450 27M IP-55",677.2,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023270","OM - Couvercle arrière L1200 H1450 27M IP-55","OM - Rear Cover W1200 H1450 27M IP-55","OM- PANEL TRASERO W1200 H1450 27M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1450 27M IP-55"]
["02328","ZENERGY OM - POKRYWA TYLNA W1200 H1600 28M IP-55",925.6,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023287","OM - Couvercle arrière W1600 H1600 28M IP-55","OM - Rear Cover W1200 H1600 28M IP-55","OM- PANEL TRASERO W1600 H1600 28M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1600 28M IP-55"]
["02329","ZENERGY OM - POKRYWA TYLNA W1200 H1550 29M IP-55",745.2,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023294","OM - Couvercle arrière L1200 H1550 29M IP-55","OM - Rear Cover W1200 H1550 29M IP-55","OM- PANEL TRASERO W1200 H1550 29M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1550 29M IP-55"]
["02330","ZENERGY OM - POKRYWA TYLNA W1200 H1700 30M IP-55",934.2,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023300","OM - Couvercle arrière L1200 H1700 30M IP-55","OM - Rear Cover W1200 H1700 30M IP-55","OM- PANEL TRASERO W1200 H1700 30M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1700 30M IP-55"]
["02333","ZENERGY OM - POKRYWA TYLNA W1200 H1850 33M IP-55",1117.8,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023331","OM - Couvercle arrière L1200 H1850 33M IP-55","OM - Rear Cover W1200 H1850 33M IP-55","OM- PANEL TRASERO W1200 H1850 33M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H1850 33M IP-55"]
["02336","ZENERGY OM - POKRYWA TYLNA W1200 H2000 36M IP-55",1189.0999999999999,"1-ZE-09",0.01,1,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023362","OM - Couvercle arrière L1200 H2000 36M IP-55","OM - Rear Cover W1200 H2000 36M IP-55","OM- PANEL TRASERO W1200 H2000 36M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H2000 36M IP-55"]
["02339","ZENERGY OM - POKRYWA TYLNA W1200 H2150 39M IP-55",1267.9000000000001,"1-ZE-09",null,null,"OM_BACK_COVER",null,"SZT","85389099","27.12.40.0",null,"5901988023393","OM - Couvercle arrière L1200 H2150 39M IP-55","OM - Rear Cover W1200 H2150 39M IP-55","OM- PANEL TRASERO W1200 H2150 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1200 H2150 39M IP-55"]
["02340","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-55",306,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988023409","OM - Deux couvercles horizontaux L1200 P300 P300 IP-55","OM - Two Horizontal Covers W1200 D300 IP-55","*OM - Dos cubiertas horizontales W1200 D300 IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-55"]
["02341","produkt wycofany (ZENERGY OM - COKÓŁ W1200 D300 IP-55)",445.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988023416","produit invalidé OM - Socle L1200 P300 P300 IP-55","product cancelled OM - Plinth W1200 D300 IP-55","*producto anulado OM - Zócalo, W1200 D300 IP-55","kivont termék (ZENERGY OM - PLINTH W1200 D300 IP-55)"]
["02343","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",306,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988023430","OM - Deux couvercles horizontaux L1200 P300 IP-55 avec trou 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1200 D300 IP-55 with a 81x222 opening for the IP-55 bushing","*OM- dos cubiertas horizontales W1200 D300 IP-55 con una abertura de 81x222 para un casquillo IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["02344","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",306,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988023447","OM - Deux couvercles horizontaux L1200 P300 IP-55 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1200 D300 IP-55 with TWO holes 81x222 for the IP-55 bushing","*OM - Dos cubiertas horizontales W1200 D300 IP-55 con DOS agujeros 81x222 para la alcantarilla IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-55 KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["02345","ZENERGY OM - DWIE POKRYWY POZIOME W1200 D300 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",306,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER",null,"SZT","85389099",null,null,"5901988023454","OM - Deux couvercles horizontaux L1200 P300 IP-55 avec TROIS trous 81x222 pour pénétration IP-55","OM - Two Horizontal Covers W1200 D300 IP-55 with THREE holes 81x222 for the IP-55 bushing","*OM - Dos cubiertas horizontales W1200 D300 IP-55 con TRES agujeros 81x222 para el casquillo IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1200 D300 IP-55 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["02347","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1200 D300 IP-55",306,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","02347","SZT","85389099","27.12.40.0",null,"5901988023478","OM - Couvercle horizontal socle L1200 P300 IP-55","OM - Two Horizontal Plinth Covers W1200 D300 IP-55","OM- TECHO/SUELO (2UDS) W1200 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1200 D300 IP-55"]
["02400","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D230 IP-30",256.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124007"]
["02403","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D230 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",256.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124038"]
["02404","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D230 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",256.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124045"]
["02405","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D230 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",256.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124052"]
["02407","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1400 D230 IP-30",256.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124076"]
["02408","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D230 IP-30 Z CZTEREMA OTWORAMI 81X222 POD PRZEPUST IP-55",256.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124083"]
["02440","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D300 IP-30",294.3,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124403"]
["02443","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",294.3,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124434"]
["02444","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D300 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",294.3,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124441"]
["02445","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D300 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",294.3,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124458"]
["02446","ZENERGY OM - DWIE POKRYWY POZIOME W1400 D300 IP-30 Z CZTEREMA OTWORAMI 81X222 POD PRZEPUST IP-55",294.3,null,0.01,1,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124465"]
["02447","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1400 D300 IP-30",294.3,null,0.01,1,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988124472"]
["03030","ZENERGY - POPRZECZKA RAMY W300",58.2,"1-ZE-10",2.5,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030308","OE - barre transversale L300","OE - Crossbar for the W300 frame","OE- TRAVIESA W300","ZENERGY - W300 KERESZTTEREM"]
["03040","ZENERGY - POPRZECZKA RAMY W400",68.400000000000006,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030407","OE - barre transversale L400","OE - Crossbar for the W400 frame","OE- TRAVIESA W400","ZENERGY - W400 KERESZTTEREM"]
["03045","ZENERGY - POPRZECZKA RAMY W450",73.7,"1-ZE-10",1.4583333333333333,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030452","OE - Cadre Crossbar L450","OE - Crossbar for the W450 frame","OE- TRAVIESA W450","ZENERGY - W450 KERESZTTEREM"]
["03050","ZENERGY - POPRZECZKA RAMY W500",88.9,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030506","OE - barre transversale W500","OE - Crossbar for the W500 frame","OE- TRAVIESA W500","ZENERGY - W500 KERET KERESZT"]
["03051","ZENERGY - POPRZECZKI RAMY W500, DLA POLA NAROŻNEGO D400 - KPL. (4SZT.)",354.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988030513","OE - barres transversales de cadre W500, pour boîte de coin P400 - set. 4 pcs.","OE - W500 frame crossbars, for the D400 corner bay - set (4 pcs.)","*OE- Barras transversales del marco W500, para la caja de esquina D400 - set (4 piezas.)","ZENERGY - W500 KERET KERESZTRUDA, D400 SAROK TERÜLETÉRE - SZETT. (4 DB)"]
["03060","ZENERGY - POPRZECZKA RAMY W600",89.2,"1-ZE-10",1.1333333333333333,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030605","OE - Barre transversale L600","OE - Crossbar for the W600 frame","OE- TRAVIESA W600","ZENERGY - W600 KERET KERESZT"]
["03065","ZENERGY - POPRZECZKA RAMY W650",94,"1-ZE-10",11.016666666666667,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030650","OE - Cadre Crossbar L650","OE - Crossbar for the W650 frame","OE- TRAVIESA W650","ZENERGY - W650 KERESZTTEREM"]
["03070","ZENERGY - POPRZECZKA RAMY W700",399.6,"1-ZE-10",0.8,4,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988030704","OE - Crossbar W700, pour boîte de coin P600 - set. 4 pcs.","OE - W700 frame crossbars, for the D600 corner bay - set (4 pcs.)","*OE- Barras transversales del marco W700, para la caja de esquina D600 - conjunto (4 piezas.)","ZENERGY - W700 KERESZTTEREM"]
["03071","ZENERGY - POPRZECZKI RAMY W700, DLA POLA NAROŻNEGO D600 - KPL. (4SZT.)",370.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988030711","OE - TRAVERSE W700, POUR CHAMP D'ANGLE P600 - KPL. (4 PIÈCES)","OE - crossmember W700, FOR corner field D600 - KPL. (4PCS)","*OE - TRAVESAÑO W700, PARA CAMPO DE ESQUINA D600 - KPL. (4 PIEZAS)","ZENERGY - W700 KERET KERESZTRUDA, D600 SAROKTERÜLETRE - SZETT. (4 DB)"]
["03080","ZENERGY - POPRZECZKA RAMY W800",109.1,"1-ZE-10",1.2916666666666667,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030803","OE - barre transversale L800","OE - Crossbar for the W800 frame","OE- TRAVIESA W800","ZENERGY - W800 KERET KERESZT"]
["03085","ZENERGY - POPRZECZKA RAMY W850",114.5,"1-ZE-10",6.7666666666666666,7,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030858","OE - Cadre Crossbar L850","OE - Crossbar for the W850 frame","OE- TRAVIESA W850","ZENERGY - W850 KERESZTTEREM"]
["03090","ZENERGY - POPRZECZKA RAMY W900",124.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030902","OE - Barre transversale W900","OE - Crossbar for the W900 frame","OE- TRAVIESA W900","ZENERGY - W900 KERESZTTEREM"]
["03091","ZENERGY - POPRZECZKI RAMY W900, DLA POLA NAROŻNEGO D800 - KPL. (4SZT.)",507.1,"1-ZE-10",0.01,1,"OE_SKD_PARTS",null,"KPL","85389099",null,null,"5901988030919","OE - TRAVERSE W900, POUR CHAMP D'ANGLE P800 - KPL. (4 PIÈCES)","OE - crossmember W900, FOR corner field D800 - KPL. (4PCS)","*OE - TRAVESAÑO W900, PARA CAMPO DE ESQUINA D800 - KPL. (4 PIEZAS)","ZENERGY - W900 KERET KERESZTRUDA, D800 SAROK TERÜLETÉRE - SZETT. (4 DB)"]
["03101","ZENERGY - POPRZECZKA RAMY W1000",130.69999999999999,"1-ZE-10",1.2,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988031015","OE - Cadre Crossbar L1000","OE - Crossbar for the W1000 frame","OE- TRAVIESA W1000","ZENERGY - W1000 KERESZTTEREM"]
["03106","produkt wycofany (ZENERGY - POPRZECZKA RAMY W1050 200+650+200)",105.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988031060","produit invalidé OE - Bordure de cadre L1050 200 + 650 + 200","product cancelled OE - Crossbar for the frame W1050 200 + 650 + 200","OE- TRAVIESA W1050 200+650+200","kivont termék (ZENERGY - FRAME CROSS-BAR W1050 200+650+200)"]
["03121","ZENERGY - POPRZECZKA RAMY W1200",149,"1-ZE-10",0.8,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988031213","OE - Cadre Crossbar L1200","OE - Crossbar of the W1200 frame","OE- TRAVIESA W1200","ZENERGY - W1200 KERESZTTEREM"]
["03122","produkt wycofany (ZENERGY - POPRZECZKA RAMY W1200 150+450+450+150)",151.19999999999999,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988031220","produit invalidé OE - Barre transversale L1200 150 + 450 + 450 + 150","product cancelled OE - Crossbar of the frame W1200 150 + 450 + 450 + 150","OE- TRAVIESA W1200 150+450+450+150","kivont termék (ZENERGY - FRAME CROSS-BAR W1200 150+450+450+150)"]
["03131","ZENERGY - POPRZECZKA RAMY W1300",162,"1-ZE-10",4.1666666666666664E-2,1,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988031312","OE - Barre transversale L1300 650 + 650","OE - Crossbar for the frame W1300 650 + 650","OE- TRAVIESA W1300 650+650","ZENERGY - W1300 KERESZTTEREM"]
["03200","ZENERGY OM - DWIE POKRYWY POZIOME W300 IP-30",102.4,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03200","SZT","85389099","27.12.40.0",null,"5901988032005","OM - Couvercle horizontal L300 IP-30","OM - Two Horizontal Lids W300 IP-30","OM- TECHO /SUELO (2UDS) W300 IP30 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 IP-30"]
["03201","produkt wycofany (ZENERGY OM - COKÓŁ W300 IP-30)",238.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03201","SZT","85389099","27.12.40.0",null,"5901988032012","produit invalidé OM - Socle L300 IP-30","product cancelled OM - W300 IP-30 plinth","OM- ZOCALO W300 IP30","megszűnt termék (ZENERGY OM - PLINTH W300 IP-30)"]
["03203","ZENERGY OM - DWIE POKRYWY POZIOME W300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",102.4,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03203","SZT","85389099","27.12.40.0",null,"5901988032036","OM - Couvercle horizontal L300 IP-30 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W300 IP-30 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W300 IP30  CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["03206","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W300 IP-30",95.8,"1-ZE-09",null,null,"OM_EXTENSION","03206","SZT","85389099","27.12.40.0",null,"5901988032067","OM - Couvercle d'extension horizontale - Gully L300 IP-30","OM - Horizontal Extension Cover - W300 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W300 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W300 IP-30"]
["03207","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W300 D230 IP-30",102.4,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","03207","SZT","85389099","27.12.40.0",null,"5901988032074","OM - Couvercle horizontal socle L300 P230 IP-30","OM - Two Horizontal Plinth Covers W300 D230 IP-30","OM- TECHO/SUELO (2UDS) W300 D230 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W300 D230 IP-30"]
["03209","ZENERGY OM - POKRYWA TYLNA W300 H550 9M IP-30",118.8,"1-ZE-09",null,null,"OM_BACK_COVER","03209","SZT","85389099","27.12.40.0",null,"5901988032098","OM - Couvercle arrière L300 H550 9M IP-30","OM - Rear Cover W300 H550 9M IP-30","OM-PANEL TRASERO W300 H550 9M IP-30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H550 9M IP-30"]
["03212","ZENERGY OM - POKRYWA TYLNA W300 H700 12M IP-30",122,"1-ZE-09",null,null,"OM_BACK_COVER","03212","SZT","85389099","27.12.40.0",null,"5901988032128","OM - Couvercle arrière L300 H700 12M IP-30","OM - Rear Cover W300 H700 12M IP-30","OM- PANEL TRASERO W300 H700 12M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H700 12M IP-30"]
["03215","ZENERGY OM - POKRYWA TYLNA W300 H850 15M IP-30",145.80000000000001,"1-ZE-09",null,null,"OM_BACK_COVER","03215","SZT","85389099","27.12.40.0",null,"5901988032159","OM - Couvercle arrière L300 H850 15M IP-30","OM - Rear Cover W300 H850 15M IP-30","OM- PANEL TRASERO W300 H850 15M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H850 15M IP-30"]
["03218","ZENERGY OM - POKRYWA TYLNA W300 H1000 18M IP-30",169.6,"1-ZE-09",0.01,1,"OM_BACK_COVER","03218","SZT","85389099","27.12.40.0",null,"5901988032180","OM - Couvercle arrière L300 H1000 18M IP-30","OM - Rear Cover W300 H1000 18M IP-30","OM- PANEL TRASERO W300 H1000 18M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1000 18M IP-30"]
["03221","ZENERGY OM - POKRYWA TYLNA W300 H1150 21M IP-30",193.3,"1-ZE-09",null,null,"OM_BACK_COVER","03221","SZT","85389099","27.12.40.0",null,"5901988032210","OM - Couvercle arrière L300 H1150 21M IP-30","OM - Rear Cover W300 H1150 21M IP-30","OM- PANEL TRASERO W300 H1150 21M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1150 21M IP-30"]
["03224","ZENERGY OM - POKRYWA TYLNA W300 H1300 24M IP-30",211.7,"1-ZE-09",null,null,"OM_BACK_COVER","03224","SZT","85389099","27.12.40.0",null,"5901988032241","OM - Couvercle arrière L300 H1300 24M IP-30","OM - Rear Cover W300 H1300 24M IP-30","OM- PANEL TRASERO W300 H1300 24M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1300 24M IP-30"]
["03227","ZENERGY OM - POKRYWA TYLNA W300 H1450 27M IP-30",231.1,"1-ZE-09",null,null,"OM_BACK_COVER","03227","SZT","85389099","27.12.40.0",null,"5901988032272","OM - Couvercle arrière L300 H1450 27M IP-30","OM - Rear Cover W300 H1450 27M IP-30","OM- PANEL TRASERO W300 H1450 27M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1450 27M IP-30"]
["03228","ZENERGY OM - POKRYWA TYLNA W300 H1600 28M IP-30",271.10000000000002,"1-ZE-09",1.6666666666666666E-2,2,"OM_BACK_COVER","03228","SZT","85389099","27.12.40.0",null,"5901988032289","OM - Couvercle arrière L300 H1600 28M IP-30","OM - Rear Cover W300 H1600 28M IP-30","OM- PANEL TRASERO W300 H1600 28M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1600 28M IP-30"]
["03229","ZENERGY OM - POKRYWA TYLNA W300 H1550 29M IP-30",256,"1-ZE-09",null,null,"OM_BACK_COVER","03229","SZT","85389099","27.12.40.0",null,"5901988032296","OM - Couvercle arrière L300 H1550 29M IP-30","OM - Rear Cover W300 H1550 29M IP-30","OM- PANEL TRASERO W300 H1550 29M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1550 29M IP-30"]
["03230","ZENERGY OM - POKRYWA TYLNA W300 H1700 30M IP-30",271.10000000000002,"1-ZE-09",null,null,"OM_BACK_COVER","03230","SZT","85389099","27.12.40.0",null,"5901988032302","OM - Couvercle arrière L300 H1700 30M IP-30","OM - Rear Cover W300 H1700 30M IP-30","OM- PANEL TRASERO W300 H1700 30M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1700 30M IP-30"]
["03233","ZENERGY OM - POKRYWA TYLNA W300 H1850 33M IP-30",293.8,"1-ZE-09",null,null,"OM_BACK_COVER","03233","SZT","85389099","27.12.40.0",null,"5901988032333","OM - Couvercle arrière L300 H1850 33M IP-30","OM - Rear Cover W300 H1850 33M IP-30","OM- PANEL TRASERO W300 H1850 33M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1850 33M IP-30"]
["03236","ZENERGY OM - POKRYWA TYLNA W300 H2000 36M IP-30",319.7,"1-ZE-09",0.01,1,"OM_BACK_COVER","03236","SZT","85389099","27.12.40.0",null,"5901988032364","OM - Couvercle arrière L300 H2000 36M IP-30","OM - Rear Cover W300 H2000 36M IP-30","OM- PANEL TRASERO W300 H2000 36M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H2000 36M IP-30"]
["03239","ZENERGY OM - POKRYWA TYLNA W300 H2150 39M IP-30",341.3,"1-ZE-09",null,null,"OM_BACK_COVER","03239","SZT","85389099","27.12.40.0",null,"5901988032395","OM - Couvercle arrière L300 H2150 39M IP-30","OM - Rear Cover W300 H2150 39M IP-30","OM- PANEL TRASERO W300 H2150 39M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W300 H2150 39M IP-30"]
["03240","ZENERGY OM - DWIE POKRYWY POZIOME W300 D300 IP-30",118.8,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","03240","SZT","85389099","27.12.40.0",null,"5901988032401","OM - Deux couvercles horizontaux L300 P300 P300 IP-30","OM - Two Horizontal Covers W300 D300 IP-30","OM- TECHO/SUELO HORIZ. W300 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 D300 IP-30"]
["03241","produkt wycofany (ZENERGY OM - COKÓŁ W300 D300 IP-30)",277.10000000000002,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03241","SZT","85389099","27.12.40.0",null,"5901988032418","produit invalidé OM - Socle L300 P300 P300 IP-30","product cancelled OM - Plinth W300 D300 IP-30","OM- ZOCALO W300 D300 IP30 ","kivont termék (ZENERGY OM - PLINTH W300 D300 IP-30)"]
["03243","ZENERGY OM - DWIE POKRYWY POZIOME W300 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",118.8,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","03243","SZT","85389099","27.12.40.0",null,"5901988032432","OM - Deux couvercles horizontaux L300 P300 IP-30 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W300 D300 IP-30 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W300 D300 IP30 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 D300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["03246","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W300 D300  IP-30",111.2,"1-ZE-09",0.01,1,"OM_EXTENSION","03246","SZT","85389099","27.12.40.0",null,"5901988032463","OM - Couvercle d'expansion horizontal - L300 P300 P300 P300 P300 IP-30 ponceau","OM - Horizontal Extension Cover - W300 D300 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W300 D300 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W300 D300 IP-30"]
["03247","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W300 D300 IP-30",118.8,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","03247","SZT","85389099","27.12.40.0",null,"5901988032470","OM - Couvercle horizontal socle L300 P300 IP-30","OM - Two Horizontal Plinth Covers W300 D300 IP-30","OM- TECHO/SUELO (2UDS) W300 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W300 D300 IP-30"]
["03300","ZENERGY OM - DWIE POKRYWY POZIOME W300 IP-55",105.8,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03200","SZT","85389099","27.12.40.0",null,"5901988033002","OM - Couvercle horizontal L300 IP-55","OM - Two Horizontal Lids W300 IP-55","OM- TECHO /SUELO (2UDS) W300  IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 IP-55"]
["03301","produkt wycofany (ZENERGY OM - COKÓŁ W300 IP-55)",244,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03301","SZT","85389099","27.12.40.0",null,"5901988033019","produit invalidé OM - Socle L300 IP-55","product cancelled OM - W300 IP-55 plinth","OM- ZOCALO W300 IP55","kivont termék (ZENERGY OM - PLINTH W300 IP-55)"]
["03303","ZENERGY OM - DWIE POKRYWY POZIOME W300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",105.8,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03203","SZT","85389099","27.12.40.0",null,"5901988033033","OM - Couvercle horizontal L300 IP-55 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W300 IP-55 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W300  IP55 CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES FEDÉL W300 IP-55 81X222-ES LYUKAL IP-55 CSŐHEZ"]
["03306","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W300 IP-55",102.6,"1-ZE-09",null,null,"OM_EXTENSION","03206","SZT","85389099","27.12.40.0",null,"5901988033064","OM - Couvercle d'extension horizontale - Gully L300 IP-55","OM - Horizontal Extension Cover - W300 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W300 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W300 IP-55"]
["03307","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W300 D230 IP-55",105.8,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03307","SZT","85389099","27.12.40.0",null,"5901988033071","OM - Couvercle horizontal socle L300 P230 IP-55","OM - Two Horizontal Plinth Covers W300 D230 IP-55","OM- TECHO/SUELO (2UDS) W300 D230 IP55","ZENERGY OM – KÉT BÍRÓ PVÍZSZINTES LÁZLET W300 D230 IP-55"]
["03309","ZENERGY OM - POKRYWA TYLNA W300 H550 9M IP-55",214.9,"1-ZE-09",null,null,"OM_BACK_COVER","03209","SZT","85389099","27.12.40.0",null,"5901988033095","OM - Couvercle arrière L300 H550 9M IP-55","OM - Rear Cover W300 H550 9M IP-55","OM- PANEL TRASERO W300 H550 9M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H550 9M IP-55"]
["03312","ZENERGY OM - POKRYWA TYLNA W300 H700 12M IP-55",234.4,"1-ZE-09",null,null,"OM_BACK_COVER","03212","SZT","85389099","27.12.40.0",null,"5901988033125","OM - Couvercle arrière L300 H700 12M IP-55","OM - Rear Cover W300 H700 12M IP-55","OM- PANEL TRASERO W300 H700 12M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H700 12M IP-55"]
["03315","ZENERGY OM - POKRYWA TYLNA W300 H850 15M IP-55",273.2,"1-ZE-09",null,null,"OM_BACK_COVER","03215","SZT","85389099","27.12.40.0",null,"5901988033156","OM - Couvercle arrière L300 H850 15M IP-55","OM - Rear Cover W300 H850 15M IP-55","OM- PANEL TRASERO W300 H850 15M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H850 15M IP-55"]
["03318","ZENERGY OM - POKRYWA TYLNA W300 H1000 18M IP-55",400.7,"1-ZE-09",null,null,"OM_BACK_COVER","03218","SZT","85389099","27.12.40.0",null,"5901988033187","OM - Couvercle arrière L300 H1000 18M IP-55","OM - Rear Cover W300 H1000 18M IP-55","OM- PANEL TRASERO W300 H1000 18M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1000 18M IP-55"]
["03321","ZENERGY OM - POKRYWA TYLNA W300 H1150 21M IP-55",346.7,"1-ZE-09",null,null,"OM_BACK_COVER","03221","SZT","85389099","27.12.40.0",null,"5901988033217","OM - Couvercle arrière L300 H1150 21M IP-55","OM - Rear Cover W300 H1150 21M IP-55","OM- PANEL TRASERO W300 H1150 21M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1150 21M IP-55"]
["03324","ZENERGY OM - POKRYWA TYLNA W300 H1300 24M IP-55",380.2,"1-ZE-09",null,null,"OM_BACK_COVER","03224","SZT","85389099","27.12.40.0",null,"5901988033248","OM - Couvercle arrière L300 H1300 24M IP-55","OM - Rear Cover W300 H1300 24M IP-55","OM- PANEL TRASERO W300 H1300 24M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1300 24M IP-55"]
["03327","ZENERGY OM - POKRYWA TYLNA W300 H1450 27M IP-55",415.8,"1-ZE-09",null,null,"OM_BACK_COVER","03227","SZT","85389099","27.12.40.0",null,"5901988033279","OM - Couvercle arrière L300 H1450 27M IP-55","OM - Rear Cover W300 H1450 27M IP-55","OM- PANEL TRASERO W300 H1450 27M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1450 27M IP-55"]
["03328","ZENERGY OM - POKRYWA TYLNA W300 H1600 28M IP-55",423.4,"1-ZE-09",null,null,"OM_BACK_COVER","03228","SZT","85389099","27.12.40.0",null,"5901988033286","OM - Couvercle arrière L300 H1600 28M IP-55","OM - Rear Cover W300 H1600 28M IP-55","OM- PANEL TRASERO W300 H1600 28M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1600 28M IP-55"]
["03329","ZENERGY OM - POKRYWA TYLNA W300 H1550 29M IP-55",451.4,"1-ZE-09",null,null,"OM_BACK_COVER","03229","SZT","85389099","27.12.40.0",null,"5901988033293","OM - Couvercle arrière L300 H1550 29M IP-55","OM - Rear Cover W300 H1550 29M IP-55","OM- PANEL TRASERO W300 H1550 29M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1550 29M IP-55"]
["03330","ZENERGY OM - POKRYWA TYLNA W300 H1700 39M IP-55",470.9,"1-ZE-09",null,null,"OM_BACK_COVER","03230","SZT","85389099","27.12.40.0",null,"5901988033309","OM - Couvercle arrière L300 H1700 39M IP-55","OM - Rear Cover W300 H1700 39M IP-55","OM- PANEL TRASERO W300 H1700 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1700 39M IP-55"]
["03333","ZENERGY OM - POKRYWA TYLNA W300 H1850 33M IP-55",473,"1-ZE-09",null,null,"OM_BACK_COVER","03233","SZT","85389099","27.12.40.0",null,"5901988033330","OM - Couvercle arrière L300 H1850 33M IP-55","OM - Rear Cover W300 H1850 33M IP-55","OM- PANEL TRASERO W300 H1850 33M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H1850 33M IP-55"]
["03336","ZENERGY OM - POKRYWA TYLNA W300 H2000 36M IP-55",489.2,"1-ZE-09",null,null,"OM_BACK_COVER","03236","SZT","85389099","27.12.40.0",null,"5901988033361","OM - Couvercle arrière L300 H2000 36M IP-55","OM - Rear Cover W300 H2000 36M IP-55","OM- PANEL TRASERO W300 H2000 36M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H2000 36M IP-55"]
["03339","ZENERGY OM - POKRYWA TYLNA W300 H2150 39M IP-55",503.3,"1-ZE-09",null,null,"OM_BACK_COVER","03239","SZT","85389099","27.12.40.0",null,"5901988033392","OM - Couvercle arrière L300 H2150 39M IP-55","OM - Rear Cover W300 H2150 39M IP-55","OM- PANEL TRASERO W300 H2150 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W300 H2150 39M IP-55"]
["03340","ZENERGY OM - DWIE POKRYWY POZIOME W300 D300 IP-55",123.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03240","SZT","85389099","27.12.40.0",null,"5901988033408","OM - Deux couvercles horizontaux L300 P300 P300 IP-55","OM - Two Horizontal Covers W300 D300 IP-55","OM- TECHO/SUELO HORIZ. W300 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 D300 IP-55"]
["03341","produkt wycofany (ZENERGY OM - COKÓŁ W300 D300 IP-55)",282.5,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03341","SZT","85389099","27.12.40.0",null,"5901988033415","produit invalidé OM - L300 Socle/socle P300 IP-55","product cancelled OM - Plinth W300 D300 IP-55","OM- ZOCALO W300 D300 IP55 ","kivont termék (ZENERGY OM - PLINTH W300 D300 IP-55)"]
["03343","ZENERGY OM - DWIE POKRYWY POZIOME W300 D300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",123.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03243","SZT","85389099","27.12.40.0",null,"5901988033439","OM - Deux couvercles horizontaux L300 P300 IP-55 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W300 D300 IP-55 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W300 D300 IP30 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W300 D300 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["03346","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W300 D300 IP-55",118.8,"1-ZE-09",null,null,"OM_EXTENSION","03246","SZT","85389099","27.12.40.0",null,"5901988033460","OM - Couvercle d'expansion horizontal - L300 P300 P300 P300 P300 IP-55 ponceau","OM - Horizontal Extension Cover - W300 D300 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W300 D300 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W300 D300 IP-55"]
["03347","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W300 D300 IP-55",123.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","03347","SZT","85389099","27.12.40.0",null,"5901988033477","OM - Couvercle horizontal socle L300 P300 IP-55","OM - Two Horizontal Plinth Covers W300 D300 IP-55","OM- TECHO/SUELO (2UDS) W300 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W300 D300 IP-55"]
["04015","Zenergy",247.2,"1-ZE-09",null,null,null,null,"SZT","85381000","27.12.40.0",null,null,null,null,null,"Zenergy"]
["04020","ZENERGY - RAMKA ZEWNĘTRZNA, D230, H1200",180.4,"1-ZE-10",4.1666666666666664E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040208","OE - Cadre extérieur, P230, H1200","OE - Outer frame, D230, H1200","OE- MARCO LATERAL EXTERIOR, D230, H1200","ZENERGY - KÜLSŐ KERET, D230, H1200"]
["04022","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D230, H1200",185.8,null,null,null,"OE_SKD_PARTS",null,null,"85389099",null,null,"5901988040222"]
["04030","ZENERGY - RAMKA ZEWNĘTRZNA, D300, H1200",189,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040307","OE - Cadre extérieur, P300, H1200","OE - Outer frame, D300, H1200","OE- MARCO LATERAL EXTERIOR, D300, H1200","ZENERGY - KÜLSŐ KERET, D300, H1200"]
["04032","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D300, H1200",198.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040321","OE - Cadre intérieur, double, P300, H1200","OE - Inner frame, double, D300, H1200","OE- MARCO LATERAL INTERIOR DOBLE, D300, H1200","ZENERGY - BELSŐ KERET, DUPLA, D300, H1200"]
["04040","ZENERGY - RAMKA ZEWNĘTRZNA, D400, H1200",208.4,"1-ZE-10",0.1,2,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040406","OE - Cadre extérieur, P400, H1200","OE - Outer frame, D400, H1200","OE- MARCO LATERAL EXTERIOR, D400, H1200","ZENERGY - KÜLSŐ KERET, D400, H1200"]
["04041","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D400, H1200",208.4,null,null,null,"OE_SKD_PARTS",null,null,"85389099",null,null,"5901988040413"]
["04042","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D400, H1200",221.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040420","OE - Cadre intérieur, double, P400, H1200","OE - Inner frame, double, D400, H1200","OE- MARCO LATERAL INTERIOR DOBLE, D400, H1200","ZENERGY - BELSŐ KERET, DUPLA, D400, H1200"]
["04060","ZENERGY - RAMKA ZEWNĘTRZNA, D600, H1200",226.8,"1-ZE-10",1.6666666666666666E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040604","OE - Cadre extérieur, P600, H1200","OE - Outer frame, D600, H1200","OE- MARCO LATERAL EXTERIOR, D600, H1200","ZENERGY - KÜLSŐ KERET, D600, H1200"]
["04062","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D600, H1200",365,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040628","OE - Cadre intérieur, double, P600, H1200","OE - Inner frame, double, D600, H1200","OE- MARCO LATERAL INTERIOR DOBLE, D600, H1200","ZENERGY - BELSŐ KERET, DUPLA, D600, H1200"]
["04080","ZENERGY - RAMKA ZEWNĘTRZNA, D800, H1200",260.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988040802","OE - Cadre extérieur, P800, H1200","OE - Outer frame, D800, H1200","OE- MARCO LATERAL EXTERIOR, D800, H1200","ZENERGY - KÜLSŐ KERET, D800, H1200"]
["04200","ZENERGY OM - DWIE POKRYWY POZIOME W400 IP-30",109.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04200","SZT","85389099","27.12.40.0",null,"5901988042004","OM - Couvercle horizontal L400 IP-30","OM - Two Horizontal Lids W400 IP-30","OM- TECHO /SUELO (2UDS) W400 IP30 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 IP-30"]
["04201","produkt wycofany (ZENERGY OM - COKÓŁ W400 IP-30)",246.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04201","SZT","85389099","27.12.40.0",null,"5901988042011","produit invalidé OM - Socle L400 IP-30","product cancelled OM - W400 IP-30 plinth","OM- ZOCALO W400 IP30","kivont termék (ZENERGY OM - PLINTH W400 IP-30)"]
["04203","ZENERGY OM - DWIE POKRYWY POZIOME W400 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",109.1,"1-ZE-09",0.55000000000000004,2,"OM_HORIZONTAL_COVER","04203","SZT","85389099","27.12.40.0",null,"5901988042035","OM - Couvercle horizontal L400 IP-30 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W400 IP-30 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W400 IP30  CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["04206","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W400 IP-30",102.6,"1-ZE-09",null,null,"OM_EXTENSION","04206","SZT","85389099","27.12.40.0",null,"5901988042066","OM - Extension de niveau horizontal - L400 IP-30","OM - Horizontal Extension Cover - W400 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W400 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W400 IP-30"]
["04207","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W400 D230 IP-30",109.1,"1-ZE-09",0.3,2,"OM_HORIZONTAL_COVER","04207","SZT","85389099","27.12.40.0",null,"5901988042073","OM - Couvercle horizontal socle L400 P230 IP-30","OM - Two Horizontal Plinth Covers W400 D230 IP-30","OM - TAPA HORIZONTAL ZOCALO (2 UN.) W400 D230 IP-30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W400 D230 IP-30"]
["04209","ZENERGY OM - POKRYWA TYLNA W400 H550 9M IP-30",128.5,"1-ZE-09",0.05,4,"OM_BACK_COVER","04209","SZT","85389099","27.12.40.0",null,"5901988042097","OM - Couvercle arrière L400 H550 9M IP-30","OM - Rear Cover W400 H550 9M IP-30","OM- PANEL TRASERO W400 H550 9M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H550 9M IP-30"]
["04212","ZENERGY OM - POKRYWA TYLNA W400 H700 12M IP-30",133,"1-ZE-09",6.6666666666666666E-2,2,"OM_BACK_COVER","04212","SZT","85389099","27.12.40.0",null,"5901988042127","OM - Couvercle arrière L400 H700 12M IP-30","OM - Rear Cover W400 H700 12M IP-30","OM- PANEL TRASERO W400 H700 12M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H700 12M IP-30"]
["04215","ZENERGY OM - POKRYWA TYLNA W400 H850 15M IP-30",157.69999999999999,"1-ZE-09",5.8333333333333334E-2,4,"OM_BACK_COVER","04215","SZT","85389099","27.12.40.0",null,"5901988042158","OM - Couvercle arrière L400 H850 15M IP-30","OM - Rear Cover W400 H850 15M IP-30","OM- PANEL TRASERO W400 H850 15M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H850 15M IP-30"]
["04218","ZENERGY OM - POKRYWA TYLNA W400 H1000 18M IP-30",182.5,"1-ZE-09",5.8333333333333334E-2,4,"OM_BACK_COVER","04218","SZT","85389099","27.12.40.0",null,"5901988042189","OM - Couvercle arrière L400 H1000 18M IP-30","OM - Rear Cover W400 H1000 18M IP-30","OM- PANEL TRASERO W400 H1000 18M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1000 18M IP-30"]
["04221","ZENERGY OM - POKRYWA TYLNA W400 H1150 21M IP-30",211.5,"1-ZE-09",8.3333333333333329E-2,2,"OM_BACK_COVER","04221","SZT","85389099","27.12.40.0",null,"5901988042219","OM - Couvercle arrière L400 H1150 21M IP-30","OM - Rear Cover W400 H1150 21M IP-30","OM- PANEL TRASERO W400 H1150 21M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1150 21M IP-30"]
["04224","ZENERGY OM - POKRYWA TYLNA W400 H1300 24M IP-30",231.1,"1-ZE-09",0.18333333333333332,2,"OM_BACK_COVER","04224","SZT","85389099","27.12.40.0",null,"5901988042240","OM - Couvercle arrière L400 H1300 24M IP-30","OM - Rear Cover W400 H1300 24M IP-30","OM- PANEL TRASERO W400 H1300 24M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1300 24M IP-30"]
["04227","ZENERGY OM - POKRYWA TYLNA W400 H1450 27M IP-30",252.9,"1-ZE-09",0.2,5,"OM_BACK_COVER","04227","SZT","85389099","27.12.40.0",null,"5901988042271","OM - Couvercle arrière L400 H1450 27M IP-30","OM - Rear Cover W400 H1450 27M IP-30","OM- PANEL TRASERO W400 H1450 27M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1450 27M IP-30"]
["04228","ZENERGY OM - POKRYWA TYLNA W400 H1600 28M IP-30",299.2,"1-ZE-09",null,null,"OM_BACK_COVER","04228","SZT","85389099","27.12.40.0",null,"5901988042288","OM - Couvercle arrière L400 H1600 28M IP-30","OM - Rear Cover W400 H1600 28M IP-30","OM- PANEL TRASERO W400 H1600 28M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1600 28M IP-30"]
["04229","ZENERGY OM - POKRYWA TYLNA W400 H1550 29M IP-30",278.60000000000002,"1-ZE-09",null,null,"OM_BACK_COVER","04229","SZT","85389099","27.12.40.0",null,"5901988042295","OM - Couvercle arrière L400 H1550 29M IP-30","OM - Rear Cover W400 H1550 29M IP-30","OM- PANEL TRASERO W400 H1550 29M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1550 29M IP-30"]
["04230","ZENERGY OM - POKRYWA TYLNA W400 H1700 30M IP-30",304.60000000000002,"1-ZE-09",5.8333333333333334E-2,2,"OM_BACK_COVER","04230","SZT","85389099","27.12.40.0",null,"5901988042301","OM - Couvercle arrière L400 H1700 30M IP-30","OM - Rear Cover W400 H1700 30M IP-30","OM- PANEL TRASERO W400 H1700 30M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1700 30M IP-30"]
["04233","ZENERGY OM - POKRYWA TYLNA W400 H1850 33M IP-30",332.6,"1-ZE-09",null,null,"OM_BACK_COVER","04233","SZT","85389099","27.12.40.0",null,"5901988042332","OM - Couvercle arrière L400 H1850 33M IP-30","OM - Rear Cover W400 H1850 33M IP-30","OM- PANEL TRASERO W400 H1850 33M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1850 33M IP-30"]
["04236","ZENERGY OM - POKRYWA TYLNA W400 H2000 36M IP-30",366.2,"1-ZE-09",0.16666666666666666,5,"OM_BACK_COVER","04236","SZT","85389099","27.12.40.0",null,"5901988042363","OM - Couvercle arrière L400 H2000 36M IP-30","OM - Rear Cover W400 H2000 36M IP-30","OM- PANEL TRASERO W400 H2000 36M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H2000 36M IP-30"]
["04239","ZENERGY OM - POKRYWA TYLNA W400 H2150 39M IP-30",397.9,"1-ZE-09",0.13333333333333333,2,"OM_BACK_COVER","04239","SZT","85389099","27.12.40.0",null,"5901988042394","OM - Couvercle arrière L400 H2150 39M IP-30","OM - Rear Cover W400 H2150 39M IP-30","OM- PANEL TRASERO W400 H2150 39M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W400 H2150 39M IP-30"]
["04240","ZENERGY OM - DWIE POKRYWY POZIOME W400 D300 IP-30",126.3,"1-ZE-09",3.3333333333333333E-2,1,"OM_HORIZONTAL_COVER","04240","SZT","85389099","27.12.40.0",null,"5901988042400","OM - Deux couvercles horizontaux L400 P300 P300 IP-30","OM - Two Horizontal Covers W400 D300 IP-30","OM- TECHO/SUELO  W400 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 D300 IP-30"]
["04241","produkt wycofany (ZENERGY OM - COKÓŁ W400 D300 IP-30)",285.7,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04241","SZT","85389099","27.12.40.0",null,"5901988042417","produit invalidé OM - L400 Socle/socle P300 IP-30","product cancelled OM - Plinth W400 D300 IP-30","OM- ZOCALO W400 D300 IP30 ","kivont termék (ZENERGY OM - PLINTH W400 D300 IP-30)"]
["04243","ZENERGY OM - DWIE POKRYWY POZIOME W400 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",126.3,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","04243","SZT","85389099","27.12.40.0",null,"5901988042431","OM - Deux couvercles horizontaux L400 P300 IP-30 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W400 D300 IP-30 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W400 D300 IP30 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 D300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["04246","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W400 D300 IP-30",118.8,"1-ZE-09",null,null,"OM_EXTENSION","04246","SZT","85389099","27.12.40.0",null,"5901988042462","OM - Couvercle d'expansion horizontal - L400 P300 P300 Ponceau IP-30","OM - Horizontal Extension Cover - W400 D300 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W400 D300 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W400 D300 IP-30"]
["04247","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W400 D300 IP-30",126.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04247","SZT","85389099","27.12.40.0",null,"5901988042479","OM - Couvercle horizontal socle L400 P300 IP-30","OM - Two Horizontal Plinth Covers W400 D300 IP-30","OM- TECHO/SUELO (2UDS) W400 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W400 D300 IP-30"]
["04300","ZENERGY OM - DWIE POKRYWY POZIOME W400 IP-55",117.7,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","04200","SZT","85389099","27.12.40.0",null,"5901988043001","OM - Couvercle horizontal L400 IP-55","OM - Two Horizontal Lids W400 IP-55","OM- TECHO /SUELO (2UDS) W400  IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 IP-55"]
["04301","produkt wycofany (ZENERGY OM - COKÓŁ W400 IP-55)",254.7,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04301","SZT","85389099","27.12.40.0",null,"5901988043018","produit invalidé OM - Socle L400 IP-55","product cancelled OM - W400 IP-55 plinth","OM- ZOCALO W400 IP55","kivont termék (ZENERGY OM - PLINTH W400 IP-55)"]
["04303","ZENERGY OM - DWIE POKRYWY POZIOME W400 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",117.7,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04203","SZT","85389099","27.12.40.0",null,"5901988043032","OM - Couvercle horizontal L400 IP-55 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W400 IP-55 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W400  IP55 CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["04306","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W400 IP-55",115.6,"1-ZE-09",null,null,"OM_EXTENSION","04206","SZT","85389099","27.12.40.0",null,"5901988043063","OM - Extension de grille horizontale - L400 IP-55","OM - Horizontal Extension Cover - W400 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W400 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W400 IP-55"]
["04307","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W400 D230 IP-55",117.7,"1-ZE-09",0.10833333333333334,4,"OM_HORIZONTAL_COVER","04307","SZT","85389099","27.12.40.0",null,"5901988043070","OM - Couvercle horizontal socle L400 P230 IP-55","OM - Two Horizontal Plinth Covers W400 D230 IP-55","OM - TAPA HORIZONTAL ZOCALO (2 UN.) W400 D230 IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W400 D230 IP-55"]
["04309","ZENERGY OM - POKRYWA TYLNA W400 H550 9M IP-55",233.3,"1-ZE-09",0.01,1,"OM_BACK_COVER","04209","SZT","85389099","27.12.40.0",null,"5901988043094","OM - Couvercle arrière L400 H550 9M IP-55","OM - Rear Cover W400 H550 9M IP-55","OM- PANEL TRASERO W400 H550 9M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H550 9M IP-55"]
["04312","ZENERGY OM - POKRYWA TYLNA W400 H700 12M IP-55",253.8,"1-ZE-09",3.3333333333333333E-2,2,"OM_BACK_COVER","04212","SZT","85389099","27.12.40.0",null,"5901988043124","OM - Couvercle arrière L400 H700 12M IP-55","OM - Rear Cover W400 H700 12M IP-55","OM- PANEL TRASERO W400 H700 12M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H700 12M IP-55"]
["04315","ZENERGY OM - POKRYWA TYLNA W400 H850 15M IP-55",293.8,"1-ZE-09",1.6666666666666666E-2,1,"OM_BACK_COVER","04215","SZT","85389099","27.12.40.0",null,"5901988043155","OM - Couvercle arrière L400 H850 15M IP-55","OM - Rear Cover W400 H850 12M IP-55","OM- PANEL TRASERO W400 H700 15M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H850 15M IP-55"]
["04318","ZENERGY OM - POKRYWA TYLNA W400 H1000 18M IP-55",421.2,"1-ZE-09",null,null,"OM_BACK_COVER","04218","SZT","85389099","27.12.40.0",null,"5901988043186","OM - Couvercle arrière L400 H1000 18M IP-55","OM - Rear Cover W400 H1000 18M IP-55","OM- PANEL TRASERO W400 H1000 18M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1000 18M IP-55"]
["04321","ZENERGY OM - POKRYWA TYLNA W400 H1150 21M IP-55",369.4,"1-ZE-09",null,null,"OM_BACK_COVER","04221","SZT","85389099","27.12.40.0",null,"5901988043216","OM - Couvercle arrière L400 H1150 21M IP-55","OM - Rear Cover W400 H1150 21M IP-55","OM- PANEL TRASERO W400 H1150 21M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1150 21M IP-55"]
["04324","ZENERGY OM - POKRYWA TYLNA W400 H1300 24M IP-55",406.1,"1-ZE-09",5.8333333333333334E-2,1,"OM_BACK_COVER","04224","SZT","85389099","27.12.40.0",null,"5901988043247","OM - Couvercle arrière L400 H1300 24M IP-55","OM - Rear Cover W400 H1300 24M IP-55","OM- PANEL TRASERO W400 H1300 24M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1300 24M IP-55"]
["04327","ZENERGY OM - POKRYWA TYLNA W400 H1450 27M IP-55",442.8,"1-ZE-09",null,null,"OM_BACK_COVER","04227","SZT","85389099","27.12.40.0",null,"5901988043278","OM - Couvercle arrière L400 H1450 27M IP-55","OM - Rear Cover W400 H1450 27M IP-55","OM- PANEL TRASERO W400 H1450 27M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1450 27M IP-55"]
["04328","ZENERGY OM - POKRYWA TYLNA W400 H1600 28M IP-55",461.2,"1-ZE-09",null,null,"OM_BACK_COVER","04228","SZT","85389099","27.12.40.0",null,"5901988043285","OM - Couvercle arrière L400 H1600 28M IP-55","OM - Rear Cover W400 H1600 28M IP-55","OM- PANEL TRASERO W400 H1600 28M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1600 28M IP-55"]
["04329","ZENERGY OM - POKRYWA TYLNA W400 H1550 29M IP-55",481.7,"1-ZE-09",null,null,"OM_BACK_COVER","04229","SZT","85389099","27.12.40.0",null,"5901988043292","OM - Couvercle arrière L400 H1550 29M IP-55","OM - Rear Cover W400 H1550 29M IP-55","OM- PANEL TRASERO W400 H1550 29M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1550 29M IP-55"]
["04330","ZENERGY OM - POKRYWA TYLNA W400 H1700 30M IP-55",505.4,"1-ZE-09",0.01,1,"OM_BACK_COVER","04230","SZT","85389099","27.12.40.0",null,"5901988043308","OM - Couvercle arrière L400 H1700 39M IP-55","OM - Rear Cover W400 H1700 30M IP-55","OM- PANEL TRASERO W400 H1700 30M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1700 30M IP-55"]
["04333","ZENERGY OM - POKRYWA TYLNA W400 H1850 33M IP-55",516.20000000000005,"1-ZE-09",0.01,1,"OM_BACK_COVER","04233","SZT","85389099","27.12.40.0",null,"5901988043339","OM - Couvercle arrière L400 H1850 33M IP-55","OM - Rear Cover W400 H1850 33M IP-55","OM- PANEL TRASERO W400 H1850 33M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H1850 33M IP-55"]
["04336","ZENERGY OM - POKRYWA TYLNA W400 H2000 36M IP-55",533.5,"1-ZE-09",1.6666666666666666E-2,1,"OM_BACK_COVER","04236","SZT","85389099","27.12.40.0",null,"5901988043360","OM - Couvercle arrière L400 H2000 36M IP-55","OM - Rear Cover W400 H2000 36M IP-55","OM- PANEL TRASERO W400 H2000 36M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H2000 36M IP-55"]
["04339","ZENERGY OM - POKRYWA TYLNA W400 H2150 39M IP-55",549.70000000000005,"1-ZE-09",null,null,"OM_BACK_COVER","04239","SZT","85389099","27.12.40.0",null,"5901988043391","OM - Couvercle arrière L400 H2150 39M IP-55","OM - Rear Cover W400 H2150 39M IP-55","OM- PANEL TRASERO W400 H2150 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W400 H2150 39M IP-55"]
["04340","ZENERGY OM - DWIE POKRYWY POZIOME W400 D300 IP-55",137,"1-ZE-09",3.3333333333333333E-2,1,"OM_HORIZONTAL_COVER","04240","SZT","85389099","27.12.40.0",null,"5901988043407","OM - Deux couvercles horizontaux L400 P300 P300 IP-55","OM - Two Horizontal Covers W400 D300 IP-55","OM- TECHO/SUELO  W400 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 D300 IP-55"]
["04341","produkt wycofany (ZENERGY OM - COKÓŁ W400 D300 IP-55)",295.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","04341","SZT","85389099","27.12.40.0",null,"5901988043414","produit invalidé OM - L400 Socle/socle P300 IP-55","product cancelled OM - Plinth W400 D300 IP-55","OM- ZOCALO W400 D300 IP55 ","kivont termék (ZENERGY OM - PLINTH W400 D300 IP-55)"]
["04343","ZENERGY OM - DWIE POKRYWY POZIOME W400 D300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",137,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","04243","SZT","85389099","27.12.40.0",null,"5901988043438","OM - Deux couvercles horizontaux L400 P300 IP-55 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W400 D300 IP-55 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W400 D300 IP30 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W400 D300 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["04346","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W400 D300 IP-55",133.9,"1-ZE-09",null,null,"OM_EXTENSION","04246","SZT","85389099","27.12.40.0",null,"5901988043469","OM - Couvercle d'expansion horizontal - L400 P300 P300 Ponceau IP-55","OM - Horizontal Extension Cover - W400 D300 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W400 D300 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W400 D300 IP-55"]
["04347","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W400 D300 IP-55",137,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","04347","SZT","85389099","27.12.40.0",null,"5901988043476","OM - Couvercle horizontal socle L400 P300 IP-55","OM - Two Horizontal Plinth Covers W400 D300 IP-55","OM- TECHO/SUELO (2UDS) W400 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W400 D300 IP-55"]
["04974","ZENERGY - PRZEGRODA POZIOMA DO SZYN W400 D400",511.8,"1-ZE-10",0.11666666666666667,2,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988049744","OE - Diviseur horizontal pour rails L400 P400","OE - Horizontal divider for W400 D400 rails","OE- SEPARACION BARRA HORIZ. W400 D400","ZENERGY - VÍZSZINTES ALKATRÉSZ W400 D400 SÍNHEZ"]
["04976","ZENERGY - WYGRODZENIE SZYN POZIOMYCH W650 D400",595.79999999999995,"1-ZE-10",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988049768","OE - Escrime des rails horizontaux L650 P400","OE - Fencing for W650 D400 Horizontal rails","OE- PROTECCION EMBARRADO HORIZ. W650 D400","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE W650 D400"]
["05020","ZENERGY - RAMKA ZEWNĘTRZNA, D230, H1400",191.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050207","OE - Cadre extérieur, P230, H1400","OE - Outer frame, D230, H1400","OE- MARCO LATERAL EXTERIOR, D230, H1400","ZENERGY - KÜLSŐ KERET, D230, H1400"]
["05021","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D230, H1400",191.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050214","OE - Cadre extérieur, double perforation, P230, H1400","OE - Outer frame, double perforation, D230, H1400","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D230, H1400","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D230, H1400"]
["05022","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D230, H1400",208.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050221","OE - Cadre intérieur, double, P230, H1400","OE - Inner frame, double, D230, H1400","OE- MARCO LATERAL INTERIOR DOBLE, D230, H1400","ZENERGY - BELSŐ KERET, DUPLA, D230, H1400"]
["05030","ZENERGY - RAMKA ZEWNĘTRZNA, D300, H1400",210.6,"1-ZE-10",4.1666666666666664E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050306","OE - Cadre extérieur, P300, H1400","OE - Outer frame, D300, H1400","OE- MARCO LATERAL EXTERIOR, D300, H1400","ZENERGY - KÜLSŐ KERET, D300, H1400"]
["05031","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D300, H1400",210.6,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050313","OE - Cadre extérieur, double perforation, P300, H1400","OE - Outer frame, double perforation, D300, H1400","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D300, H1400","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D300, H1400"]
["05032","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D300, H1400",236.5,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050320","OE - Cadre intérieur, double, P300, H1400","OE - Inner frame, double, D300, H1400","OE- MARCO LATERAL INTERIOR DOBLE, D300, H1400","ZENERGY - BELSŐ KERET, DUPLA, D300, H1400"]
["05040","ZENERGY - RAMKA ZEWNĘTRZNA, D400, H1400",231.1,"1-ZE-10",0.44166666666666665,6,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050405","OE - Cadre extérieur, P400, H1400","OE - Outer frame, D400, H1400","OE- MARCO LATERAL EXTERIOR, D400, H1400","ZENERGY - KÜLSŐ KERET, D400, H1400"]
["05041","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D400, H1400",231.1,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050412","OE - Cadre extérieur, double perforation, P400, H1400","OE - Outer frame, double perforation, D400, H1400","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D400, H1400","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D400, H1400"]
["05042","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D400, H1400",241.9,"1-ZE-10",0.2,6,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050429","OE - Cadre intérieur, double, P400, H1400","OE - Inner frame, double, D400, H1400","OE- MARCO LATERAL INTERIOR DOBLE, D400, H1400","ZENERGY - BELSŐ KERET, DUPLA, D400, H1400"]
["05060","ZENERGY - RAMKA ZEWNĘTRZNA, D600, H1400",385.6,"1-ZE-10",0.7,6,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050603","OE - Cadre extérieur, P600, H1400","OE - Outer frame, D600, H1400","OE- MARCO LATERAL EXTERIOR, D600, H1400","ZENERGY - KÜLSŐ KERET, D600, H1400"]
["05061","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D600, H1400",385.6,"1-ZE-10",0.01,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050610","OE - Cadre extérieur, double perforation, P600, H1400","OE - Outer frame, double perforation, D600, H1400","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D600, H1400","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D600, H1400"]
["05062","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D600, H1400",395.3,"1-ZE-10",1.6666666666666666E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050627","OE - Cadre intérieur, double, P600, H1400","OE - Inner frame, double, D600, H1400","OE- MARCO LATERAL INTERIOR DOBLE, D600, H1400","ZENERGY - BELSŐ KERET, DUPLA, D600, H1400"]
["05080","ZENERGY - RAMKA ZEWNĘTRZNA, D800, H1400",432.3,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050801","OE - Cadre extérieur, P800, H1400","OE - Outer frame, D800, H1400","OE- MARCO LATERAL EXTERIOR, D800, H1400","ZENERGY - KÜLSŐ KERET, D800, H1400"]
["05081","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D800, H1400",432.3,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050818","OE - Cadre extérieur, double perforation, P800, H1400","OE - Outer frame, double perforation, D800, H1400","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D800, H1400","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D800, H1400"]
["05082","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D800, H1400",441.1,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988050825","OE - Cadre intérieur, double, P800, H1400","OE - Inner frame, double, D800, H1400","OE- MARCO LATERAL INTERIOR DOBLE, D800, H1400","ZENERGY - BELSŐ KERET, DUPLA, D800, H1400"]
["06020","ZENERGY - RAMKA ZEWNĘTRZNA, D230, H1600",204.1,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060206","OE - Cadre extérieur, P230, H1600","OE - Outer frame, D230, H1600","OE- MARCO LATERAL EXTERIOR, D230, H1600","ZENERGY - KÜLSŐ KERET, D230, H1600"]
["06021","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D230, H1600",204.1,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060213","OE - Cadre extérieur, double perforation, P230, H1600","OE - Outer frame, double perforation, D230, H1600","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D230, H1600","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D230, H1600"]
["06022","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D230, H1600",223.6,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060220","OE - Cadre intérieur, double, P230, H1600","OE - Inner frame, double, D230, H1600","OE- MARCO LATERAL INTERIOR DOBLE, D230, H1600","ZENERGY - BELSŐ KERET, DUPLA, D230, H1600"]
["06030","ZENERGY - RAMKA ZEWNĘTRZNA, D300, H1600",225.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060305","OE - Cadre extérieur, P300, H1600","OE - Outer frame, D300, H1600","OE- MARCO LATERAL EXTERIOR, D300, H1600","ZENERGY - KÜLSŐ KERET, D300, H1600"]
["06031","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D300, H1600",225.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060312","OE - Cadre extérieur, double perforation, P300, H1600","OE - Outer frame, double perforation, D300, H1600","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D300, H1600","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D300, H1600"]
["06032","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D300, H1600",253.8,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060329","OE - Cadre intérieur, double, P300, H1600","OE - Inner frame, double, D300, H1600","OE- MARCO LATERAL INTERIOR DOBLE, D300, H1600","ZENERGY - BELSŐ KERET, DUPLA, D300, H1600"]
["06040","ZENERGY - RAMKA ZEWNĘTRZNA, D400, H1600",247.3,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060404","OE - Cadre extérieur, P400, H1600","OE - Outer frame, D400, H1600","OE- MARCO LATERAL EXTERIOR, D400, H1600","ZENERGY - KÜLSŐ KERET, D400, H1600"]
["06041","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D400, H1600",247.3,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060411","OE - Cadre extérieur, double perforation, P400, H1600","OE - Outer frame, double perforation, D400, H1600","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D400, H1600","ZENERGY - KÜLSŐ KERETRZNA, DUPLÁS PERFORÁCIÓ, D400, H1600"]
["06042","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D400, H1600",259.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060428","OE - Cadre intérieur, double, P400, H1600","OE - Inner frame, double, D400, H1600","OE- MARCO LATERAL INTERIOR DOBLE, D400, H1600","ZENERGY - BELSŐ KERET, DUPLA, D400, H1600"]
["06060","ZENERGY - RAMKA ZEWNĘTRZNA, D600, H1600",413.6,"1-ZE-10",0.2,2,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060602","OE - Cadre extérieur, P600, H1600","OE - Outer frame, D600, H1600","OE- MARCO LATERAL EXTERIOR, D600, H1600","ZENERGY - KÜLSŐ KERET, D600, H1600"]
["06061","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D600, H1600",413.6,"1-ZE-10",1.6666666666666666E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060619","OE - Cadre extérieur, double perforation, P600, H1600","OE - Outer frame, double perforation, D600, H1600","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D600, H1600","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D600, H1600"]
["06062","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D600, H1600",423.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060626","OE - Cadre intérieur, double, P600, H1600","OE - Inner frame, double, D600, H1600","OE- MARCO LATERAL INTERIOR DOBLE, D600, H1600","ZENERGY - BELSŐ KERET, DUPLA, D600, H1600"]
["06080","ZENERGY - RAMKA ZEWNĘTRZNA, D800, H1600",464.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060800","OE - Cadre extérieur, P800, H1600","OE - Outer frame, D800, H1600","OE- MARCO LATERAL EXTERIOR, D800, H1600","ZENERGY - KÜLSŐ KERET, D800, H1600"]
["06081","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D800, H1600",464.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060817","OE - Cadre extérieur, double perforation, P800, H1600","OE - Outer frame, double perforation, D800, H1600","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D800, H1600","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D800, H1600"]
["06082","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D800, H1600",473,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988060824","OE - Cadre intérieur, double, P800, H1600","OE - Inner frame, double, D800, H1600","OE- MARCO LATERAL INTERIOR DOBLE, D800, H1600","ZENERGY - BELSŐ KERET, DUPLA, D800, H1600"]
["06200","ZENERGY OM - DWIE POKRYWY POZIOME W600 IP-30",114.5,"1-ZE-09",0.84166666666666667,2,"OM_HORIZONTAL_COVER","06200","SZT","85389099","27.12.40.0",null,"5901988062002","OM - Couvercle horizontal L600 IP-30","OM - Two Horizontal Lids W600 IP-30","OM- TECHO /SUELO (2UDS) W600 IP30 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 IP-30"]
["06201","produkt wycofany (ZENERGY OM - COKÓŁ W600 IP-30)",262.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","06201","SZT","85389099","27.12.40.0",null,"5901988062019","produit invalidé OM - Socle L600 IP-30","product cancelled OM - W600 IP-30 plinth","OM- ZOCALO W600 IP30","megszűnt termék (ZENERGY OM - PLINTH W600 IP-30)"]
["06203","ZENERGY OM - DWIE POKRYWY POZIOME W600 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",114.5,"1-ZE-09",3.3166666666666669,6,"OM_HORIZONTAL_COVER","06203","SZT","85389099","27.12.40.0",null,"5901988062033","OM - Couvercle horizontal L600 IP-30 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W600 IP-30 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W600 IP30  CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 IP-30 81X222 LYUKAL AZ IP-55 LÖDÖKHEZ"]
["06204","ZENERGY OM - DWIE POKRYWY POZIOME W600 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",114.5,"1-ZE-09",0.18333333333333332,2,"OM_HORIZONTAL_COVER","06204","SZT","85389099","27.12.40.0",null,"5901988062040","OM - Couvercle horizontal L600 IP-30 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal Covers W600 IP-30 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W600 IP30  CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 IP-30 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["06206","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W600 IP-30",108,"1-ZE-09",null,null,"OM_EXTENSION","06206","SZT","85389099","27.12.40.0",null,"5901988062064","OM - Extension de grille horizontale - Passe-câble L600 IP-30","OM - Horizontal Extension Cover - W600 IP-30 Grommet","OM- TECHO DE MODULO AUX. W600 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W600 IP-30"]
["06207","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W600 D230 IP-30",114.5,"1-ZE-09",0.45,2,"OM_HORIZONTAL_COVER","06207","SZT","85389099","27.12.40.0",null,"5901988062071","OM - Couvercle horizontal socle L600 P230 IP-30","OM - Two Horizontal Plinth Covers W600 D230 IP-30","OM - TAPA HORIZONTAL ZOCALO (2 UN.) W600 D230 IP-30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W600 D230 IP-30"]
["06209","ZENERGY OM - POKRYWA TYLNA W600 H550 9M IP-30",137.30000000000001,"1-ZE-09",0.16666666666666666,4,"OM_BACK_COVER","06209","SZT","85389099","27.12.40.0",null,"5901988062095","OM - Couvercle arrière L600 H550 9M IP-30","OM - Rear Cover W600 H550 9M IP-30","OM- PANEL TRASERO W600 H550 9M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H550 9M IP-30"]
["06212","ZENERGY OM - POKRYWA TYLNA W600 H700 12M IP-30",144.5,"1-ZE-09",0.35833333333333334,6,"OM_BACK_COVER","06212","SZT","85389099","27.12.40.0",null,"5901988062125","OM - Couvercle arrière L600 H700 12M IP-30","OM - Rear Cover W600 H700 12M IP-30","OM- PANEL TRASERO W600 H700 12M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H700 12M IP-30"]
["06215","ZENERGY OM - POKRYWA TYLNA W600 H850 15M IP-30",166.9,"1-ZE-09",0.7,6,"OM_BACK_COVER","06215","SZT","85389099","27.12.40.0",null,"5901988062156","OM - Couvercle arrière L600 H850 15M IP-30","OM - Rear Cover W600 H850 15M IP-30","OM- PANEL TRASERO W600 H850 15M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H850 15M IP-30"]
["06218","ZENERGY OM - POKRYWA TYLNA W600 H1000 18M IP-30",180.9,"1-ZE-09",0.40833333333333333,4,"OM_BACK_COVER","06218","SZT","85389099","27.12.40.0",null,"5901988062187","OM - Couvercle arrière L600 H1000 18M IP-30","OM - Rear Cover W600 H1000 18M IP-30","OM- PANEL TRASERO W600 H1000 18M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1000 18M IP-30"]
["06221","ZENERGY OM - POKRYWA TYLNA W600 H1150 21M IP-30",215.8,"1-ZE-09",0.53333333333333333,5,"OM_BACK_COVER","06221","SZT","85389099","27.12.40.0",null,"5901988062217","OM - Couvercle arrière L600 H1150 21M IP-30","OM - Rear Cover W600 H1150 21M IP-30","OM- PANEL TRASERO W600 H1150 21M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1150 21M IP-30"]
["06224","ZENERGY OM - POKRYWA TYLNA W600 H1300 24M IP-30",230,"1-ZE-09",0.3,6,"OM_BACK_COVER","06224","SZT","85389099","27.12.40.0",null,"5901988062248","OM - Couvercle arrière L600 H1300 24M IP-30","OM - Rear Cover W600 H1300 24M IP-30","OM- PANEL TRASERO W600 H1300 24M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1300 24M IP-30"]
["06227","ZENERGY OM - POKRYWA TYLNA W600 H1450 27M IP-30",239.8,"1-ZE-09",0.48333333333333334,4,"OM_BACK_COVER","06227","SZT","85389099","27.12.40.0",null,"5901988062279","OM - Couvercle arrière L600 H1450 27M IP-30","OM - Rear Cover W600 H1450 27M IP-30","OM- PANEL TRASERO W600 H1450 27M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1450 27M IP-30"]
["06228","ZENERGY OM - POKRYWA TYLNA W600 H1600 28M IP-30",358.6,"1-ZE-09",0.01,1,"OM_BACK_COVER","06228","SZT","85389099","27.12.40.0",null,"5901988062286","OM - Couvercle arrière L600 H1600 28M IP-30","OM - Rear Cover W600 H1600 28M IP-30","OM- PANEL TRASERO W600 H1600 28M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1600 28M IP-30"]
["06229","ZENERGY OM - POKRYWA TYLNA W600 H1550 29M IP-30",261.39999999999998,"1-ZE-09",0.05,2,"OM_BACK_COVER","06229","SZT","85389099","27.12.40.0",null,"5901988062293","OM - Couvercle arrière L600 H1550 29M IP-30","OM - Rear Cover W600 H1550 29M IP-30","OM- PANEL TRASERO W600 H1550 29M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1550 29M IP-30"]
["06230","ZENERGY OM - POKRYWA TYLNA W600 H1700 30M IP-30",365.2,"1-ZE-09",0.40833333333333333,7,"OM_BACK_COVER","06230","SZT","85389099","27.12.40.0",null,"5901988062309","OM - Couvercle arrière L600 H1700 30M IP-30","OM - Rear Cover W600 H1700 30M IP-30","OM- PANEL TRASERO W600 H1700 30M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1700 30M IP-30"]
["06233","ZENERGY OM - POKRYWA TYLNA W600 H1850 33M IP-30",393.5,"1-ZE-09",0.46666666666666667,5,"OM_BACK_COVER","06233","SZT","85389099","27.12.40.0",null,"5901988062330","OM - Couvercle arrière L600 H1850 33M IP-30","OM - Rear Cover W600 H1850 33M IP-30","OM- PANEL TRASERO W600 H1850 33M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1850 33M IP-30"]
["06236","ZENERGY OM - POKRYWA TYLNA W600 H2000 36M IP-30",465.4,"1-ZE-09",0.40833333333333333,6,"OM_BACK_COVER","06236","SZT","85389099","27.12.40.0",null,"5901988062361","OM - Couvercle arrière L600 H2000 36M IP-30","OM - Rear Cover W600 H2000 36M IP-30","OM- PANEL TRASERO W600 H2000 36M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H2000 36M IP-30"]
["06239","ZENERGY OM - POKRYWA TYLNA W600 H2150 39M IP-30",548.29999999999995,"1-ZE-09",0.28333333333333333,2,"OM_BACK_COVER","06239","SZT","85389099","27.12.40.0",null,"5901988062392","OM - Couvercle arrière L600 H2150 39M IP-30","OM - Rear Cover W600 H2150 39M IP-30","OM- PANEL TRASERO W600 H2150 39M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W600 H2150 39M IP-30"]
["06240","ZENERGY OM - DWIE POKRYWY POZIOME W600 D300 IP-30",133.80000000000001,"1-ZE-09",0.2,2,"OM_HORIZONTAL_COVER","06240","SZT","85389099","27.12.40.0",null,"5901988062408","OM - Deux couvercles horizontaux L600 P300 P300 IP-30","OM - Two Horizontal Covers W600 D300 IP-30","OM- TECHO/SUELO  W600 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 D300 IP-30"]
["06241","produkt wycofany (ZENERGY OM - COKÓŁ W600 D300 IP-30)",303.89999999999998,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","06241","SZT","85389099","27.12.40.0",null,"5901988062415","produit invalidé OM - Socle L600 P300 P300 IP-30","product cancelled OM - Plinth W600 D300 IP-30","OM- ZOCALO W600 D300 IP30 ","kivont termék (ZENERGY OM - PLINTH W600 D300 IP-30)"]
["06243","ZENERGY OM - DWIE POKRYWY POZIOME W600 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",133.80000000000001,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","06243","SZT","85389099","27.12.40.0",null,"5901988062439","OM - Deux couvercles horizontaux L600 P300 IP-30 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W600 D300 IP-30 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W600 D300 IP55 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 D300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["06244","ZENERGY OM - DWIE POKRYWY POZIOME W600 D300 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",133.80000000000001,"1-ZE-09",0.23333333333333334,4,"OM_HORIZONTAL_COVER","06244","SZT","85389099","27.12.40.0",null,"5901988062446","OM - Deux couvercles horizontaux L600 P300 IP-30 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W600 D300 IP-30 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W600 D300 IP30 CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 D300 IP-30 KÉT LYUKAL 81X222 IP-55 LÖVEDEKHEZ"]
["06246","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W600 D300 IP-30",125.3,"1-ZE-09",null,null,"OM_EXTENSION","06246","SZT","85389099","27.12.40.0",null,"5901988062460","OM - Couvercle d'expansion horizontal - L600 P300 P300 Ponceau IP-30","OM - Horizontal Extension Cover - W600 D300 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W600 D300 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W600 D300 IP-30"]
["06247","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W600 D300 IP-30",133.80000000000001,"1-ZE-09",0.13333333333333333,4,"OM_HORIZONTAL_COVER","06247","SZT","85389099","27.12.40.0",null,"5901988062477","OM - Couvercle horizontal socle L600 P300 IP-30","OM - Two Horizontal Plinth Covers W600 D300 IP-30","OM- TECHO/SUELO (2UDS) W600 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W600 D300 IP-30"]
["06300","ZENERGY OM - DWIE POKRYWY POZIOME W600 IP-55",134.80000000000001,"1-ZE-09",0.14166666666666666,7,"OM_HORIZONTAL_COVER","06200","SZT","85389099","27.12.40.0",null,"5901988063009","OM - Couvercle horizontal L600 IP-55","OM - Two Horizontal Lids W600 IP-55","OM- TECHO /SUELO (2UDS) W600  IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 IP-55"]
["06301","produkt wycofany (ZENERGY OM - COKÓŁ W600 IP-55)",276.10000000000002,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","06301","SZT","85389099","27.12.40.0",null,"5901988063016","produit invalidé OM - Socle L600 IP-55","product cancelled OM - W600 IP-55 plinth","OM- ZOCALO W600 IP55","kivont termék (ZENERGY OM - PLINTH W600 IP-55)"]
["06303","ZENERGY OM - DWIE POKRYWY POZIOME W600 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",134.80000000000001,"1-ZE-09",0.25833333333333336,2,"OM_HORIZONTAL_COVER","06203","SZT","85389099","27.12.40.0",null,"5901988063030","OM - Couvercle horizontal L600 IP-55 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W600 IP-55 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W600  IP55 CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 IP-55 81X222-ES LYUKAL IP-55 CSŐHEZ"]
["06304","ZENERGY OM - DWIE POKRYWY POZIOME W600 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",134.80000000000001,"1-ZE-09",1.6666666666666666E-2,1,"OM_HORIZONTAL_COVER","06204","SZT","85389099","27.12.40.0",null,"5901988063047","OM - Couvercle horizontal L600 IP-55 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal Lids W600 IP-55 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W600  IP55 CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 IP-55 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["06306","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W600 IP-55",131.80000000000001,"1-ZE-09",null,null,"OM_EXTENSION","06206","SZT","85389099","27.12.40.0",null,"5901988063061","OM - Extension de niveau horizontal - L600 IP-55","OM - Horizontal Extension Cover - W600 IP-55 Grommet","OM- TECHO DE MODULO AUX. W600 IP35","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W600 IP-55"]
["06307","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W600 D230 IP-55",134.80000000000001,"1-ZE-09",0.01,2,"OM_HORIZONTAL_COVER","06307","SZT","85389099","27.12.40.0",null,"5901988063078","OM - Couvercle horizontal socle L600 P230 IP-55","OM - Two Horizontal Plinth Covers W600 D230 IP-55","OM - TAPA HORIZONTAL ZOCALO (2 UN.) W600 D230 IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W600 D230 IP-55"]
["06309","ZENERGY OM - POKRYWA TYLNA W600 H550 9M IP-55",259.2,"1-ZE-09",1.6666666666666666E-2,1,"OM_BACK_COVER","06209","SZT","85389099","27.12.40.0",null,"5901988063092","OM - Couvercle arrière L600 H550 9M IP-55","OM - Rear Cover W600 H550 9M IP-55","OM- PANEL TRASERO W600 H550 9M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H550 9M IP-55"]
["06312","ZENERGY OM - POKRYWA TYLNA W600 H700 12M IP-55",283.8,"1-ZE-09",9.166666666666666E-2,7,"OM_BACK_COVER","06212","SZT","85389099","27.12.40.0",null,"5901988063122","OM - Couvercle arrière L600 H700 12M IP-55","OM - Rear Cover W600 H700 12M IP-55","OM- PANEL TRASERO W600 H700 12M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H700 12M IP-55"]
["06315","ZENERGY OM - POKRYWA TYLNA W600 H850 15M IP-55",320.10000000000002,"1-ZE-09",9.166666666666666E-2,7,"OM_BACK_COVER","06215","SZT","85389099","27.12.40.0",null,"5901988063153","OM - Couvercle arrière L600 H850 15M IP-55","OM - Rear Cover W600 H850 15M IP-55","OM- PANEL TRASERO W600 H850 15M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H850 15M IP-55"]
["06318","ZENERGY OM - POKRYWA TYLNA W600 H1000 18M IP-55",439.3,"1-ZE-09",0.11666666666666667,5,"OM_BACK_COVER","06218","SZT","85389099","27.12.40.0",null,"5901988063184","OM - Couvercle arrière L600 H1000 18M IP-55","OM - Rear Cover W600 H1000 18M IP-55","OM- PANEL TRASERO W600 H1000 18M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1000 18M IP-55"]
["06321","ZENERGY OM - POKRYWA TYLNA W600 H1150 21M IP-55",395.7,"1-ZE-09",0.1,7,"OM_BACK_COVER","06221","SZT","85389099","27.12.40.0",null,"5901988063214","OM - Couvercle arrière L600 H1150 21M IP-55","OM - Rear Cover W600 H1150 21M IP-55","OM- PANEL TRASERO W600 H1150 21M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1150 21M IP-55"]
["06324","ZENERGY OM - POKRYWA TYLNA W600 H1300 24M IP-55",425.1,"1-ZE-09",9.166666666666666E-2,5,"OM_BACK_COVER","06224","SZT","85389099","27.12.40.0",null,"5901988063245","OM - Couvercle arrière L600 H1300 24M IP-55","OM - Rear Cover W600 H1300 24M IP-55","OM- PANEL TRASERO W600 H1300 24M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1300 24M IP-55"]
["06327","ZENERGY OM - POKRYWA TYLNA W600 H1450 27M IP-55",449.3,"1-ZE-09",5.8333333333333334E-2,4,"OM_BACK_COVER","06227","SZT","85389099","27.12.40.0",null,"5901988063276","OM - Couvercle arrière L600 H1450 27M IP-55","OM - Rear Cover W600 H1450 27M IP-55","OM- PANEL TRASERO W600 H1450 27M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1450 27M IP-55"]
["06328","ZENERGY OM - POKRYWA TYLNA W600 H1600 28M IP-55",526,"1-ZE-09",1.6666666666666666E-2,1,"OM_BACK_COVER","06228","SZT","85389099","27.12.40.0",null,"5901988063283","OM - Couvercle arrière L600 H1600 28M IP-55","OM - Rear Cover W600 H1600 28M IP-55","OM- PANEL TRASERO W600 H1600 28M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1600 28M IP-55"]
["06329","ZENERGY OM - POKRYWA TYLNA W600 H1550 29M IP-55",482.8,"1-ZE-09",0.01,1,"OM_BACK_COVER","06229","SZT","85389099","27.12.40.0",null,"5901988063290","OM - Couvercle arrière L600 H1550 29M IP-55","OM - Rear Cover W600 H1550 29M IP-55","OM- PANEL TRASERO W600 H1550 29M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1550 29M IP-55"]
["06330","ZENERGY OM - POKRYWA TYLNA W600 H1700 30M IP-55",578.9,"1-ZE-09",3.3333333333333333E-2,1,"OM_BACK_COVER","06230","SZT","85389099","27.12.40.0",null,"5901988063306","OM - Couvercle arrière L600 H1700 30M IP-55","OM - Rear Cover W600 H1700 30M IP-55","OM- PANEL TRASERO W600 H1700 30M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1700 30M IP-55"]
["06333","ZENERGY OM - POKRYWA TYLNA W600 H1850 33M IP-55",582.1,"1-ZE-09",6.6666666666666666E-2,4,"OM_BACK_COVER","06233","SZT","85389099","27.12.40.0",null,"5901988063337","OM - Couvercle arrière L600 H1850 33M IP-55","OM - Rear Cover W600 H1850 33M IP-55","OM- PANEL TRASERO W600 H1850 33M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H1850 33M IP-55"]
["06336","ZENERGY OM - POKRYWA TYLNA W600 H2000 36M IP-55",632.9,"1-ZE-09",3.3333333333333333E-2,4,"OM_BACK_COVER","06236","SZT","85389099","27.12.40.0",null,"5901988063368","OM - Couvercle arrière L600 H2000 36M IP-55","OM - Rear Cover W600 H2000 36M IP-55","OM- PANEL TRASERO W600 H2000 36M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H2000 36M IP-55"]
["06339","ZENERGY OM - POKRYWA TYLNA W600 H2150 39M IP-55",652.29999999999995,"1-ZE-09",0.05,1,"OM_BACK_COVER","06239","SZT","85389099","27.12.40.0",null,"5901988063399","OM - Couvercle arrière L600 H2150 39M IP-55","OM - Rear Cover W600 H2150 39M IP-55","OM- PANEL TRASERO W600 H2150 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W600 H2150 39M IP-55"]
["06340","ZENERGY OM - DWIE POKRYWY POZIOME W600 D300 IP-55",157.30000000000001,"1-ZE-09",9.166666666666666E-2,4,"OM_HORIZONTAL_COVER","06240","SZT","85389099","27.12.40.0",null,"5901988063405","OM - Deux couvercles horizontaux L600 P300 P300 IP-55","OM - Two Horizontal Covers W600 D300 IP-55","OM- TECHO/SUELO  W600 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 D300 IP-55"]
["06341","produkt wycofany (ZENERGY OM - COKÓŁ W600 D300 IP-55)",319.89999999999998,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","06341","SZT","85389099","27.12.40.0",null,"5901988063412","produit invalidé OM - Socle L600 P300 P300 IP-55","product cancelled OM - Plinth W600 D300 IP-55","OM- ZOCALO W600 D300 IP55 ","kivont termék (ZENERGY OM - PLINTH W600 D300 IP-55)"]
["06343","ZENERGY OM - DWIE POKRYWY POZIOME W600 D300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",157.30000000000001,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","06243","SZT","85389099","27.12.40.0",null,"5901988063436","OM - Deux couvercles horizontaux L600 P300 IP-55 avec trou 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W600 D300 IP-55 with a hole 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W600 D300 IP55 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 D300 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["06344","ZENERGY OM - DWIE POKRYWY POZIOME W600 D300 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",157.30000000000001,"1-ZE-09",2.5000000000000001E-2,2,"OM_HORIZONTAL_COVER","06244","SZT","85389099","27.12.40.0",null,"5901988063443","OM - Deux couvercles horizontaux L600 P300 IP-55 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W600 D300 IP-55 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W600 D300 IP55 CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W600 D300 IP-55 KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["06346","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W600 D300 IP-55",153.4,"1-ZE-09",null,null,"OM_EXTENSION","06246","SZT","85389099","27.12.40.0",null,"5901988063467","OM - Couvercle d'expansion horizontal - Ponceau L600 P300 IP-55","OM - Horizontal Extension Cover - W600 D300 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W600 D300 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W600 D300 IP-55"]
["06347","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W600 D300 IP-55",157.30000000000001,"1-ZE-09",1.6666666666666666E-2,4,"OM_HORIZONTAL_COVER","06347","SZT","85389099","27.12.40.0",null,"5901988063474","OM - Couvercle horizontal socle L600 P300 IP-55","OM - Two Horizontal Plinth Covers W600 D300 IP-55","OM- TECHO/SUELO (2UDS) W600 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W600 D300 IP-55"]
["07020","ZENERGY - RAMKA ZEWNĘTRZNA, D230, H1800",213.8,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988070205","OE - Cadre extérieur, P230, H1800","OE - Outer frame, D230, H1800","OE- MARCO LATERAL EXTERIOR, D230, H1800","ZENERGY - KÜLSŐ KERET, D230, H1800"]
["07021","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D230, H1800",213.8,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070212","OE - Cadre extérieur, double perforation, P230, H1800","OE - Outer frame, double perforation, D230, H1800","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D230, H1800","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D230, H1800"]
["07022","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D230, H1800",234.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070229","OE - Cadre intérieur, double, P230, H1800","OE - Inner frame, double, D230, H1800","OE- MARCO LATERAL INTERIOR DOBLE, D230, H1800","ZENERGY - BELSŐ KERET, DUPLA, D230, H1800"]
["07030","ZENERGY - RAMKA ZEWNĘTRZNA, D300, H1800",235.4,"1-ZE-10",0.38333333333333336,5,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070304","OE - Cadre extérieur, P300, H1800","OE - Outer frame, D300, H1800","OE- MARCO LATERAL EXTERIOR, D300, H1800","ZENERGY - KÜLSŐ KERET, D300, H1800"]
["07031","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D300, H1800",235.4,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070311","OE - Cadre extérieur, double perforation, P300, H1800","OE - Outer frame, double perforation, D300, H1800","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D300, H1800","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D300, H1800"]
["07032","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D300, H1800",265.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070328","OE - Cadre intérieur, double, P300, H1800","OE - Inner frame, double, D300, H1800","OE- MARCO LATERAL INTERIOR DOBLE, D300, H1800","ZENERGY - BELSŐ KERET, DUPLA, D300, H1800"]
["07040","ZENERGY - RAMKA ZEWNĘTRZNA, D400, H1800",258.10000000000002,"1-ZE-10",0.6166666666666667,5,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988070403","OE - Cadre extérieur, P400, H1800","OE - Outer frame, D400, H1800","OE- MARCO LATERAL EXTERIOR, D400, H1800","ZENERGY - KÜLSŐ KERET, D400, H1800"]
["07041","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D400, H1800",258.10000000000002,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070410","OE - Cadre extérieur, double perforation, P400, H1800","OE - Outer frame, double perforation, D400, H1800","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D400, H1800","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D400, H1800"]
["07042","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D400, H1800",271.10000000000002,"1-ZE-10",6.6666666666666666E-2,2,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070427","OE - Cadre intérieur, double, P400, H1800","OE - Inner frame, double, D400, H1800","OE- MARCO LATERAL INTERIOR DOBLE, D400, H1800","ZENERGY - BELSŐ KERET, DUPLA, D400, H1800"]
["07060","ZENERGY - RAMKA ZEWNĘTRZNA, D600, H1800",432,"1-ZE-10",0.16666666666666666,2,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070601","OE - Cadre extérieur, P600, H1800","OE - Outer frame, D600, H1800","OE- MARCO LATERAL EXTERIOR, D600, H1800","ZENERGY - KÜLSŐ KERET, D600, H1800"]
["07061","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D600, H1800",432,"1-ZE-10",3.3333333333333333E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070618","OE - Cadre extérieur, double perforation, P600, H1800","OE - Outer frame, double perforation, D600, H1800","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D600, H1800","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D600, H1800"]
["07062","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D600, H1800",442.8,"1-ZE-10",3.3333333333333333E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070625","OE - Cadre intérieur, double, P600, H1800","OE - Inner frame, double, D600, H1800","OE- MARCO LATERAL INTERIOR DOBLE, D600, H1800","ZENERGY - BELSŐ KERET, DUPLA, D600, H1800"]
["07080","ZENERGY - RAMKA ZEWNĘTRZNA, D800, H1800",484,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070809","OE - Cadre extérieur, P800, H1800","OE - Outer frame, D800, H1800","OE- MARCO LATERAL EXTERIOR, D800, H1800","ZENERGY - KÜLSŐ KERET, D800, H1800"]
["07081","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D800, H1800",484,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070816","OE - Cadre extérieur, double perforation, P800, H1800","OE - Outer frame, double perforation, D800, H1800","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D800, H1800","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D800, H1800"]
["07082","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D800, H1800",493.9,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988070823","OE - Cadre intérieur, double, P800, H1800","OE - Inner frame, double, D800, H1800","OE- MARCO LATERAL INTERIOR DOBLE, D800, H1800","ZENERGY - BELSŐ KERET, DUPLA, D800, H1800"]
["08010","ZENERGY - RAMKA ZEWNĘTRZNA, D1000, H2000",607.20000000000005,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988080105","OE - CADRE EXTÉRIEUR, P1000, H2000","OE - Outer frame, D1000, H2000","*OE - MARCO EXTERIOR, D1000, H2000","ZENERGY - KÜLSŐ KERET, D1000, H2000"]
["08011","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D1000, H2000",607.20000000000005,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988080112","OE - CADRE EXTÉRIEUR, DOUBLE PERFORATION, P1000, H2000","OE - Outer frame, DOUBLE PERFORATION, D1000, H2000","*OE - MARCO EXTERIOR, DOBLE PERFORACIÓN, D1000, H2000","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D1000, H2000"]
["08012","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D1000, H2000",643.5,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988080129","OE - CADRE INTERNE, DOUBLE, P1000, H2000","OE - INTERNAL FRAME, DOUBLE, D1000, H2000","*OE - MARCO INTERNO, DOBLE, D1000, H2000","ZENERGY - BELSŐ KERET, DUPLÁS, D1000, H2000"]
["08020","ZENERGY - RAMKA ZEWNĘTRZNA, D230, H2000",229.9,"1-ZE-10",8.3333333333333329E-2,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080204","OE - Cadre extérieur, P230, H2000","OE - Outer frame, D230, H2000","OE- MARCO LATERAL EXTERIOR, D230, H2000","ZENERGY - KÜLSŐ KERET, D230, H2000"]
["08021","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D230, H2000",229.9,"1-ZE-10",0.01,1,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080211","OE - Cadre extérieur, double perforation, P230, H2000","OE - Outer frame, double perforation, D230, H2000","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D230, H2000","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D230, H2000"]
["08022","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D230, H2000",251.9,"1-ZE-10",0.01,1,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080228","OE - Cadre intérieur, double, P230, H2000","OE - Inner frame, double, D230, H2000","OE- MARCO LATERAL INTERIOR DOBLE, D230, H2000","ZENERGY - BELSŐ KERET, DUPLA, D230, H2000"]
["08030","ZENERGY - RAMKA ZEWNĘTRZNA, D300, H2000",253,"1-ZE-10",0.54166666666666663,5,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080303","OE - Cadre extérieur, P300, H2000","OE - Outer frame, D300, H2000","OE- MARCO LATERAL EXTERIOR, D300, H2000","ZENERGY - KÜLSŐ KERET, D300, H2000"]
["08031","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D300, H2000",253,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080310","OE - Cadre extérieur, double perforation, P300, H2000","OE - Outer frame, double perforation, D300, H2000","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D300, H2000","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D300, H2000"]
["08032","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D300, H2000",284.89999999999998,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080327","OE - Cadre intérieur, double, P300, H2000","OE - Inner frame, double, D300, H2000","OE- MARCO LATERAL INTERIOR DOBLE, D300, H2000","ZENERGY - BELSŐ KERET, DUPLA, D300, H2000"]
["08040","ZENERGY - RAMKA ZEWNĘTRZNA, D400, H2000",273.2,"1-ZE-10",4.1500000000000004,8,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080402","OE - Cadre extérieur, P400, H2000","OE - Outer frame, D400, H2000","OE- MARCO LATERAL EXTERIOR, D400, H2000","ZENERGY - KÜLSŐ KERET, D400, H2000"]
["08041","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D400, H2000",273.2,"1-ZE-10",0.3,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080419","OE - Cadre extérieur, double perforation, P400, H2000","OE - Outer frame, double perforation, D400, H2000","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D400, H2000","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D400, H2000"]
["08042","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D400, H2000",286.2,"1-ZE-10",0.3,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080426","OE - Cadre intérieur, double, P400, H2000","OE - Inner frame, double, D400, H2000","OE- MARCO LATERAL INTERIOR DOBLE, D400, H2000","ZENERGY - BELSŐ KERET, DUPLA, D400, H2000"]
["08060","ZENERGY - RAMKA ZEWNĘTRZNA, D600, H2000",385.6,"1-ZE-10",5,11,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080600","OE - Cadre extérieur, P600, H2000","OE - Outer frame, D600, H2000","OE- MARCO LATERAL EXTERIOR, D600, H2000","ZENERGY - KÜLSŐ KERET, D600, H2000"]
["08061","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D600, H2000",385.6,"1-ZE-10",0.41666666666666669,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080617","OE - Cadre extérieur, double perforation, P600, H2000","OE - Outer frame, double perforation, D600, H2000","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D600, H2000","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D600, H2000"]
["08062","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D600, H2000",409.3,"1-ZE-10",0.24166666666666667,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080624","OE - Cadre intérieur, double, P600, H2000","OE - Inner frame, double, D600, H2000","OE- MARCO LATERAL INTERIOR DOBLE, D600, H2000","ZENERGY - BELSŐ KERET, DUPLA, D600, H2000"]
["08080","ZENERGY - RAMKA ZEWNĘTRZNA, D800, H2000",440,"1-ZE-10",1.5833333333333333,7,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080808","OE - Cadre extérieur, P800, H2000","OE - Outer frame, D800, H2000","OE- MARCO LATERAL EXTERIOR, D800, H2000","ZENERGY - KÜLSŐ KERET, D800, H2000"]
["08081","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D800, H2000",440,"1-ZE-10",0.19166666666666668,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080815","OE - Cadre extérieur, double perforation, P800, H2000","OE - Outer frame, double perforation, D800, H2000","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D800, H2000","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D800, H2000"]
["08082","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D800, H2000",467.5,"1-ZE-10",0.30833333333333335,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988080822","OE - Cadre intérieur, double, P800, H2000","OE - Inner frame, double, D800, H2000","OE- MARCO LATERAL INTERIOR DOBLE, D800, H2000","ZENERGY - BELSŐ KERET, DUPLA, D800, H2000"]
["08200","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-30",159.4,"1-ZE-09",0.16666666666666666,2,"OM_HORIZONTAL_COVER","08200","SZT","85389099","27.12.40.0",null,"5901988082000","OM - Couvercle horizontal L800 IP-30","OM - Two Horizontal W800 IP-30 Lids","OM- TECHO /SUELO (2UDS) W800 IP30 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-30"]
["08201","produkt wycofany (ZENERGY OM - COKÓŁ W800 IP-30)",293.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08201","SZT","85389099","27.12.40.0",null,"5901988082017","produit invalidé OM - Socle L800 IP-30","product cancelled OM - W800 IP-30 plinth","OM- ZOCALO W800 IP30","kivont termék (ZENERGY OM - PLINTH W800 IP-30)"]
["08203","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",159.4,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08203","SZT","85389099","27.12.40.0",null,"5901988082031","OM - Couvercle horizontal L800 IP-30 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W800 IP-30 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W800 IP30  CON AGUJERO 81X222 ","ZENERGY OM - KÉT BORÍTÓVÍZSZINTES W800 IP-30 81X222 LYUKAL IP-55 LÖVEDEKHEZ"]
["08204","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",159.4,"1-ZE-09",0.10833333333333334,2,"OM_HORIZONTAL_COVER","08204","SZT","85389099","27.12.40.0",null,"5901988082048","OM - Couvercle horizontal L800 IP-30 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal W800 IP-30 Lids with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W800 IP30  CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-30 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["08205","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",159.4,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08205","SZT","85389099","27.12.40.0",null,"5901988082055","OM - Couvercle horizontal L800 IP-30 avec trois trous 81x222 sous IP-55 Pass","OM - Two Horizontal W800 IP-30 Lids with THREE holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W800 IP30  CON TRES AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-30 HÁROM LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["08206","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W800 IP-30",150.1,"1-ZE-09",0.01,1,"OM_EXTENSION","08206","SZT","85389099","27.12.40.0",null,"5901988082062","OM - Amélioration du niveau horizontal - L800 IP-30","OM - Horizontal Extension Cover - W800 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W800 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W800 IP-30"]
["08207","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W800 D230 IP-30",159.4,"1-ZE-09",0.11666666666666667,2,"OM_HORIZONTAL_COVER","08207","SZT","85389099","27.12.40.0",null,"5901988082079","OM - Couvercle horizontal socle L800 P230 IP-30","OM - Two Horizontal Plinth Covers W800 D230 IP-30","OM - TAPA HORIZONTAL ZOCALO (2 UN.) W800 D230 IP-30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W800 D230 IP-30"]
["08209","ZENERGY OM - POKRYWA TYLNA W800 H550 9M IP-30",199.8,"1-ZE-09",null,null,"OM_BACK_COVER","08209","SZT","85389099","27.12.40.0",null,"5901988082093","OM - Couvercle arrière L800 H550 9M IP-30","OM - Rear Cover W800 H550 9M IP-30","OM- PANEL TRASERO W800 H550 9M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H550 9M IP-30"]
["08212","ZENERGY OM - POKRYWA TYLNA W800 H700 12M IP-30",218,"1-ZE-09",0.15833333333333333,2,"OM_BACK_COVER","08212","SZT","85389099","27.12.40.0",null,"5901988082123","OM - Couvercle arrière L800 H700 12M IP-30","OM - Rear Cover W800 H700 12M IP-30","OM- PANEL TRASERO W800 H700 12M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H700 12M IP-30"]
["08215","ZENERGY OM - POKRYWA TYLNA W800 H850 15M IP-30",230,"1-ZE-09",0.15833333333333333,2,"OM_BACK_COVER","08215","SZT","85389099","27.12.40.0",null,"5901988082154","OM - Couvercle arrière L800 H850 15M IP-30","OM - Rear Cover W800 H850 15M IP-30","OM- PANEL TRASERO W800 H850 15M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H850 15M IP-30"]
["08218","ZENERGY OM - POKRYWA TYLNA W800 H1000 18M IP-30",253.8,"1-ZE-09",0.05,4,"OM_BACK_COVER","08218","SZT","85389099","27.12.40.0",null,"5901988082185","OM - Couvercle arrière L800 H1000 18M IP-30","OM - Rear Cover W800 H1000 18M IP-30","OM- PANEL TRASERO W800 H1000 18M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1000 18M IP-30"]
["08221","ZENERGY OM - POKRYWA TYLNA W800 H1150 21M IP-30",264.60000000000002,"1-ZE-09",0.01,1,"OM_BACK_COVER","08221","SZT","85389099","27.12.40.0",null,"5901988082215","OM - Couvercle arrière L800 H1150 21M IP-30","OM - Rear Cover W800 H1150 21M IP-30","OM- PANEL TRASERO W800 H1150 21M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1150 21M IP-30"]
["08224","ZENERGY OM - POKRYWA TYLNA W800 H1300 24M IP-30",276.5,"1-ZE-09",5.8333333333333334E-2,2,"OM_BACK_COVER","08224","SZT","85389099","27.12.40.0",null,"5901988082246","OM - Couvercle arrière L800 H1300 24M IP-30","OM - Rear Cover W800 H1300 24M IP-30","OM- PANEL TRASERO W800 H1300 24M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1300 24M IP-30"]
["08227","ZENERGY OM - POKRYWA TYLNA W800 H1450 27M IP-30",286.2,"1-ZE-09",5.8333333333333334E-2,2,"OM_BACK_COVER","08227","SZT","85389099","27.12.40.0",null,"5901988082277","OM - Couvercle arrière L800 H1450 27M IP-30","OM - Rear Cover W800 H1450 27M IP-30","OM- PANEL TRASERO W800 H1450 27M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1450 27M IP-30"]
["08228","ZENERGY OM - POKRYWA TYLNA W800 H1600 28M IP-30",463.3,"1-ZE-09",0.01,1,"OM_BACK_COVER","08228","SZT","85389099","27.12.40.0",null,"5901988082284","OM - Couvercle arrière L800 H1600 28M IP-30","OM - Rear Cover W800 H1600 28M IP-30","OM- PANEL TRASERO W800 H1600 28M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1600 28M IP-30"]
["08229","ZENERGY OM - POKRYWA TYLNA W800 H1550 29M IP-30",312.10000000000002,"1-ZE-09",null,null,"OM_BACK_COVER","08229","SZT","85389099","27.12.40.0",null,"5901988082291","OM - Couvercle arrière L800 H1550 29M IP-30","OM - Rear Cover W800 H1550 29M IP-30","OM- PANEL TRASERO W800 H1550 29M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1550 29M IP-30"]
["08230","ZENERGY OM - POKRYWA TYLNA W800 H1700 30M IP-30",479.5,"1-ZE-09",4.1666666666666664E-2,4,"OM_BACK_COVER","08230","SZT","85389099","27.12.40.0",null,"5901988082307","OM - Couvercle arrière L800 H1700 30M IP-30","OM - Rear Cover W800 H1700 30M IP-30","OM- PANEL TRASERO W800 H1700 30M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1700 30M IP-30"]
["08233","ZENERGY OM - POKRYWA TYLNA W800 H1850 33M IP-30",624.6,"1-ZE-09",0.1,5,"OM_BACK_COVER","08233","SZT","85389099","27.12.40.0",null,"5901988082338","OM - Couvercle arrière L800 H1850 33M IP-30","OM - Rear Cover W800 H1850 33M IP-30","OM- PANEL TRASERO W800 H1850 33M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1850 33M IP-30"]
["08236","ZENERGY OM - POKRYWA TYLNA W800 H2000 36M IP-30",672.5,"1-ZE-09",0.19166666666666668,5,"OM_BACK_COVER","08236","SZT","85389099","27.12.40.0",null,"5901988082369","OM - Couvercle arrière L800 H2000 36M IP-30","OM - Rear Cover W800 H2000 36M IP-30","OM- PANEL TRASERO W800 H2000 36M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H2000 36M IP-30"]
["08239","ZENERGY OM - POKRYWA TYLNA W800 H2150 39M IP-30",724.7,"1-ZE-09",5.8333333333333334E-2,1,"OM_BACK_COVER","08239","SZT","85389099","27.12.40.0",null,"5901988082390","OM - Couvercle arrière L800 H2150 39M IP-30","OM - Rear Cover W800 H2150 39M IP-30","OM- PANEL TRASERO W800 H2150 39M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W800 H2150 39M IP-30"]
["08240","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-30",185.1,"1-ZE-09",0.20833333333333334,4,"OM_HORIZONTAL_COVER","08240","SZT","85389099","27.12.40.0",null,"5901988082406","OM - Deux couvercles horizontaux L800 P300 P300 IP-30","OM - Two Horizontal Covers W800 D300 IP-30","OM- TECHO/SUELO HORIZ. W800 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-30"]
["08241","produkt wycofany (ZENERGY OM - COKÓŁ W800 D300 IP-30)",340.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08241","SZT","85389099","27.12.40.0",null,"5901988082413","produit invalidé OM - Socle L800 P300 P300 IP-30","product cancelled OM - W800 D300 IP-30 plinth","OM- ZOCALO W800 D300 IP30 ","kivont termék (ZENERGY OM - PLINTH W800 D300 IP-30)"]
["08243","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",185.1,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08243","SZT","85389099","27.12.40.0",null,"5901988082437","OM - Deux couvercles horizontaux L800 P300 IP-30 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W800 D300 IP-30 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W800 D300 IP30 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["08244","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",185.1,"1-ZE-09",0.19166666666666668,4,"OM_HORIZONTAL_COVER","08244","SZT","85389099","27.12.40.0",null,"5901988082444","OM - Deux couvercles horizontaux L800 P300 IP-30 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W800 D300 IP-30 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W800 D300 IP30 CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-30 KÉT LYUKAL 81X222 IP-55 LÖVEDEKHEZ"]
["08245","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",185.1,"1-ZE-09",3.3333333333333333E-2,2,"OM_HORIZONTAL_COVER","08245","SZT","85389099","27.12.40.0",null,"5901988082451","OM - Deux couvercles horizontaux L800 P300 IP-30 avec TROIS trous 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W800 D300 IP-30 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W800 D300 IP30 CON TRES 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-30 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["08246","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W800 D300 IP-30",173.9,"1-ZE-09",null,null,"OM_EXTENSION","08246","SZT","85389099","27.12.40.0",null,"5901988082468","OM - Couvercle d'expansion horizontal - Ponceau L800 P300 IP-30","OM - Horizontal Extension Cover - W800 D300 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ. -W800 D300 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W800 D300 IP-30"]
["08247","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W800 D300 IP-30",185.1,"1-ZE-09",3.3333333333333333E-2,1,"OM_HORIZONTAL_COVER","08247","SZT","85389099","27.12.40.0",null,"5901988082475","OM - Couvercle horizontal socle L800 P300 IP-30","OM - Two Horizontal Plinth Covers W800 D300 IP-30","OM- TECHO/SUELO (2UDS) W800 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W800 D300 IP-30"]
["08300","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-55",188.3,"1-ZE-09",1.6666666666666666E-2,2,"OM_HORIZONTAL_COVER","08200","SZT","85389099","27.12.40.0",null,"5901988083007","OM - Couvercle horizontal L800 IP-55","OM - Two Horizontal W800 IP-55 Lids","OM- TECHO /SUELO (2UDS) W800  IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-55"]
["08301","produkt wycofany (ZENERGY OM - COKÓŁ W800 IP-55)",313.5,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08301","SZT","85389099","27.12.40.0",null,"5901988083014","produit invalidé OM - Socle L800 IP-55","product cancelled OM - W800 IP-55 plinth","OM- ZOCALO W800 IP55","kivont termék (ZENERGY OM - PLINTH W800 IP-55)"]
["08303","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",188.3,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","08203","SZT","85389099","27.12.40.0",null,"5901988083038","OM - Couvercle horizontal L800 IP-55 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W800 IP-55 Covers with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W800  IP55 CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["08304","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",188.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08204","SZT","85389099","27.12.40.0",null,"5901988083045","OM - Couvercle horizontal L800 IP-55 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal W800 IP-55 Lids with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W800  IP55 CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-55 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["08305","ZENERGY OM - DWIE POKRYWY POZIOME W800 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",188.3,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","08205","SZT","85389099","27.12.40.0",null,"5901988083052","OM - Couvercle horizontal L800 IP-55 avec TROIS trous 81x222 sous IP-55 pass","OM - Two Horizontal W800 IP-55 Lids with THREE openings 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W800  IP55 CON TRES AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 IP-55 HÁROM LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["08306","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W800 IP-55",184.7,"1-ZE-09",null,null,"OM_EXTENSION","08206","SZT","85389099","27.12.40.0",null,"5901988083069","OM - Extension de grille horizontale - Passe-câble L800 IP-55","OM - Horizontal Extension Cover - W800 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. W800 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W800 IP-55"]
["08307","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W800 D230 IP-55",188.3,"1-ZE-09",1.6666666666666666E-2,4,"OM_HORIZONTAL_COVER","08307","SZT","85389099","27.12.40.0",null,"5901988083076","OM - Couvercle horizontal socle L800 P230 IP-55","OM - Two Horizontal Plinth Covers W800 D230 IP-55","OM - TAPA HORIZONTAL ZOCALO (2 UN.) W800 D230 IP-55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W800 D230 IP-55"]
["08309","ZENERGY OM - POKRYWA TYLNA W800 H550 9M IP-55",339.1,"1-ZE-09",null,null,"OM_BACK_COVER","08209","SZT","85389099","27.12.40.0",null,"5901988083090","OM - Couvercle arrière L800 H550 9M IP-55","OM - Rear Cover W800 H550 9M IP-55","OM- PANEL TRASERO W800 H550 9M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H550 9M IP-55"]
["08312","ZENERGY OM - POKRYWA TYLNA W800 H700 12M IP-55",357.5,"1-ZE-09",null,null,"OM_BACK_COVER","08212","SZT","85389099","27.12.40.0",null,"5901988083120","OM - Couvercle arrière L800 H700 12M IP-55","OM - Rear Cover W800 H700 12M IP-55","OM- PANEL TRASERO W800 H700 12M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H700 12M IP-55"]
["08315","ZENERGY OM - POKRYWA TYLNA W800 H850 15M IP-55",397.4,"1-ZE-09",null,null,"OM_BACK_COVER","08215","SZT","85389099","27.12.40.0",null,"5901988080150","OM - Couvercle arrière L800 H850 15M IP-55","OM - Rear Cover W800 H850 15M IP-55","OM- PANEL TRASERO W800 H850 15M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H850 15M IP-55"]
["08318","ZENERGY OM - POKRYWA TYLNA W800 H1000 18M IP-55",523.79999999999995,"1-ZE-09",1.6666666666666666E-2,1,"OM_BACK_COVER","08218","SZT","85389099","27.12.40.0",null,"5901988083182","OM - Couvercle arrière L800 H1000 18M IP-55","OM - Rear Cover W800 H1000 18M IP-55","OM- PANEL TRASERO W800 H1000 18M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1000 18M IP-55"]
["08321","ZENERGY OM - POKRYWA TYLNA W800 H1150 21M IP-55",456.8,"1-ZE-09",null,null,"OM_BACK_COVER","08221","SZT","85389099","27.12.40.0",null,"5901988083212","OM - Couvercle arrière L800 H1150 21M IP-55","OM - Rear Cover W800 H1150 21M IP-55","OM- PANEL TRASERO W800 H1150 21M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1150 21M IP-55"]
["08324","ZENERGY OM - POKRYWA TYLNA W800 H1300 24M IP-55",486,"1-ZE-09",3.3333333333333333E-2,4,"OM_BACK_COVER","08224","SZT","85389099","27.12.40.0",null,"5901988083243","OM - Couvercle arrière L800 H1300 24M IP-55","OM - Rear Cover W800 H1300 24M IP-55","OM- PANEL TRASERO W800 H1300 24M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1300 24M IP-55"]
["08327","ZENERGY OM - POKRYWA TYLNA W800 H1450 27M IP-55",511.9,"1-ZE-09",0.01,1,"OM_BACK_COVER","08227","SZT","85389099","27.12.40.0",null,"5901988083274","OM - Couvercle arrière L800 H1450 27M IP-55","OM - Rear Cover W800 H1450 27M IP-55","OM- PANEL TRASERO W800 H1450 27M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1450 27M IP-55"]
["08328","ZENERGY OM - POKRYWA TYLNA W800 H1600 28M IP-55",648,"1-ZE-09",null,null,"OM_BACK_COVER","08228","SZT","85389099","27.12.40.0",null,"5901988083281","OM - Couvercle arrière L800 H1600 28M IP-55","OM - Rear Cover W800 H1600 28M IP-55","OM- PANEL TRASERO W800 H1600 28M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1600 28M IP-55"]
["08329","ZENERGY OM - POKRYWA TYLNA W800 H1550 29M IP-55",548.6,"1-ZE-09",null,null,"OM_BACK_COVER","08229","SZT","85389099","27.12.40.0",null,"5901988083298","OM - Couvercle arrière L800 H1550 29M IP-55","OM - Rear Cover W800 H1550 29M IP-55","OM- PANEL TRASERO W800 H1550 29M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1550 29M IP-55"]
["08330","ZENERGY OM - POKRYWA TYLNA W800 H1700 30M IP-55",695.5,"1-ZE-09",0.01,1,"OM_BACK_COVER","08230","SZT","85389099","27.12.40.0",null,"5901988083304","OM - Couvercle arrière L800 H1700 30M IP-55","OM - Rear Cover W800 H1700 30M IP-55","OM- PANEL TRASERO W800 H1700 30M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1700 30M IP-55"]
["08333","ZENERGY OM - POKRYWA TYLNA W800 H1850 33M IP-55",800.3,"1-ZE-09",3.3333333333333333E-2,4,"OM_BACK_COVER","08233","SZT","85389099","27.12.40.0",null,"5901988083335","OM - Couvercle arrière L800 H1850 33M IP-55","OM - Rear Cover W800 H1850 33M IP-55","OM- PANEL TRASERO W800 H1850 33M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H1850 33M IP-55"]
["08336","ZENERGY OM - POKRYWA TYLNA W800 H2000 36M IP-55",826.2,"1-ZE-09",1.6666666666666666E-2,2,"OM_BACK_COVER","08236","SZT","85389099","27.12.40.0",null,"5901988083366","OM - Couvercle arrière L800 H2000 36M IP-55","OM - Rear Cover W800 H2000 36M IP-55","OM- PANEL TRASERO W800 H2000 36M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H2000 36M IP-55"]
["08339","ZENERGY OM - POKRYWA TYLNA W800 H2150 39M IP-55",859.7,"1-ZE-09",null,null,"OM_BACK_COVER","08239","SZT","85389099","27.12.40.0",null,"5901988083397","OM - Couvercle arrière L800 H2150 39M IP-55","OM - Rear Cover W800 H2150 39M IP-55","OM- PANEL TRASERO W800 H2150 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W800 H2150 39M IP-55"]
["08340","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-55",218.3,"1-ZE-09",2.5000000000000001E-2,1,"OM_HORIZONTAL_COVER","08240","SZT","85389099","27.12.40.0",null,"5901988083403","OM - Deux couvercles horizontaux L800 P300 P300 IP-55","OM - Two Horizontal Covers W800 D300 IP-55","OM- TECHO/SUELO HORIZ. W800 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-55"]
["08341","produkt wycofany (ZENERGY OM - COKÓŁ W800 D300 IP-55)",363.8,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08341","SZT","85389099","27.12.40.0",null,"5901988083410","produit invalidé OM - Socle L800 P300 P300 IP-55","product cancelled OM - Plinth W800 D300 IP-55","OM- ZOCALO W800 D300 IP55 ","kivont termék (ZENERGY OM - PLINTH W800 D300 IP-55)"]
["08343","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08243","SZT","85389099","27.12.40.0",null,"5901988083434","OM - Deux couvercles horizontaux L800 P300 IP-55 avec trou 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W800 D300 IP-55 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W800 D300 IP55 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["08344","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08244","SZT","85389099","27.12.40.0",null,"5901988083441","OM - Deux couvercles horizontaux L800 P300 IP-55 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W800 D300 IP-55 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W800 D300 IP55 CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-55 KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["08345","ZENERGY OM - DWIE POKRYWY POZIOME W800 D300 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","08245","SZT","85389099","27.12.40.0",null,"5901988083458","OM - Deux couvercles horizontaux L800 P300 IP","OM - Two Horizontal Covers W800 D300 IP-55 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W800 D300 IP55 CON TRES 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W800 D300 IP-55 HÁROM LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["08346","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W800 D300 IP-55",213.8,"1-ZE-09",null,null,"OM_EXTENSION","08246","SZT","85389099","27.12.40.0",null,"5901988083465","OM - Couvercle d'expansion horizontal - Ponceau L800 P300 IP-55","OM - Horizontal Extension Cover - W800 D300 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ. -W800 D300 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W800 D300 IP-55"]
["08347","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W800 D300 IP-55",218.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","08347","SZT","85389099","27.12.40.0",null,"5901988083472","OM - Couvercle horizontal socle L800 P300 IP-55","OM - Two Horizontal Plinth Covers W800 D300 IP-55","OM- TECHO/SUELO (2UDS) W800 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W800 D300 IP-55"]
["08400","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-30",181.4,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988084004"]
["08403","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",181.4,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988084035"]
["08404","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",181.4,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988084042"]
["08405","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",181.4,null,0.01,1,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988084059"]
["08406","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W900 IP-30",169.6,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988084066"]
["08407","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W900 D230 IP-30",181.4,null,0.01,1,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988084073"]
["08409","ZENERGY OM - POKRYWA TYLNA W900 H550 9M IP-30",224.6,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084097"]
["08412","ZENERGY OM - POKRYWA TYLNA W900 H700 12M IP-30",244.1,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084127"]
["08415","ZENERGY OM - POKRYWA TYLNA W900 H850 15M IP-30",257,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084158"]
["08418","ZENERGY OM - POKRYWA TYLNA W900 H1000 18M IP-30",286.2,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084189"]
["08421","ZENERGY OM - POKRYWA TYLNA W900 H1150 21M IP-30",298.10000000000002,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084219"]
["08424","ZENERGY OM - POKRYWA TYLNA W900 H1300 24M IP-30",312.10000000000002,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084240"]
["08427","ZENERGY OM - POKRYWA TYLNA W900 H1450 27M IP-30",322.89999999999998,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084271"]
["08428","ZENERGY OM - POKRYWA TYLNA W900 H1600 28M IP-30",522.70000000000005,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084288"]
["08429","ZENERGY OM - POKRYWA TYLNA W900 H1550 29M IP-30",352.1,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084295"]
["08430","ZENERGY OM - POKRYWA TYLNA W900 H1700 30M IP-30",541.1,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084301"]
["08433","ZENERGY OM - POKRYWA TYLNA W900 H1850 33M IP-30",698.8,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084332"]
["08436","ZENERGY OM - POKRYWA TYLNA W900 H2000 36M IP-30",756,null,0.01,1,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084363"]
["08439","ZENERGY OM - POKRYWA TYLNA W900 H2150 39M IP-30",818.6,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988084394"]
["08500","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-55",213.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988085001"]
["08503","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",213.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988085032"]
["08504","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",213.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988085049"]
["08505","ZENERGY OM - DWIE POKRYWY POZIOME W900 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",213.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988085056"]
["08506","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W900 IP-55",208.4,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988085063"]
["08507","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W900 D230 IP-55",213.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988085070"]
["08509","ZENERGY OM - POKRYWA TYLNA W900 H550 9M IP-55",382.3,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085094"]
["08512","ZENERGY OM - POKRYWA TYLNA W900 H700 12M IP-55",403.9,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085124"]
["08515","ZENERGY OM - POKRYWA TYLNA W900 H850 15M IP-55",448.2,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085155"]
["08518","ZENERGY OM - POKRYWA TYLNA W900 H1000 18M IP-55",572.4,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085186"]
["08521","ZENERGY OM - POKRYWA TYLNA W900 H1150 21M IP-55",515.20000000000005,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085216"]
["08524","ZENERGY OM - POKRYWA TYLNA W900 H1300 24M IP-55",548.6,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085247"]
["08527","ZENERGY OM - POKRYWA TYLNA W900 H1450 27M IP-55",577.79999999999995,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085278"]
["08528","ZENERGY OM - POKRYWA TYLNA W900 H1600 28M IP-55",732.2,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085285"]
["08529","ZENERGY OM - POKRYWA TYLNA W900 H1550 29M IP-55",619.9,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085292"]
["08530","ZENERGY OM - POKRYWA TYLNA W900 H1700 30M IP-55",785.2,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085308"]
["08533","ZENERGY OM - POKRYWA TYLNA W900 H1850 33M IP-55",904,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085339"]
["08536","ZENERGY OM - POKRYWA TYLNA W900 H2000 36M IP-55",933.1,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085360"]
["08539","ZENERGY OM - POKRYWA TYLNA W900 H2150 39M IP-55",970.9,null,null,null,"OM_BACK_COVER",null,null,"85389099",null,null,"5901988085391"]
["08580","ZENERGY - RAMKA ZEWNĘTRZNA, D850, H2000",496.8,"1-ZE-10",1.6666666666666666E-2,1,"OE_SKD_PARTS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - KÜLSŐ KERET, D850, H2000"]
["09010","ZENERGY - RAMKA ZEWNĘTRZNA, D1000, H2200",661.1,"1-ZE-10",0.25833333333333336,2,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090104","OE - CADRE EXTÉRIEUR, P1000, H2200","OE - Outer frame, D1000, H2200","*OE - MARCO EXTERIOR, D1000, H2200","ZENERGY - KÜLSŐ KERET, D1000, H2200"]
["09011","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D1000, H2200",673.2,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090111","OE - CADRE EXTÉRIEUR, DOUBLE PERFORATION, P1000, H2200","OE - Outer frame, DOUBLE PERFORATION, D1000, H2200","*OE - MARCO EXTERIOR, DOBLE PERFORACIÓN, D1000, H2200","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D1000, H2200"]
["09012","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D1000, H2200",706.2,"1-ZE-10",0.45833333333333331,4,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090128","OE - CADRE INTERNE, DOUBLE, P1000, H2200","OE - INTERNAL FRAME, DOUBLE, D1000, H2200","*OE - MARCO INTERNO, DOBLE, D1000, H2200","ZENERGY - BELSŐ KERET, DUPLA, D1000, H2200"]
["09020","ZENERGY - RAMKA ZEWNĘTRZNA, D230, H2200",273.89999999999998,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090203","OE - Cadre extérieur, P230, H2200","OE - Outer frame, D230, H2200","OE- MARCO LATERAL EXTERIOR, D230, H2200","ZENERGY - KÜLSŐ KERET, D230, H2200"]
["09021","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D230, H2200",273.89999999999998,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090210","OE - Cadre extérieur, double perforation, P230, H2200","OE - Outer frame, double perforation, D230, H2200","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D230, H2200","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D230, H2200"]
["09022","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D230, H2200",294.8,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090227","OE - Cadre intérieur, double, P230, H2200","OE - Inner frame, double, D230, H2200","OE- MARCO LATERAL INTERIOR DOBLE, D230, H2200","ZENERGY - BELSŐ KERET, DUPLA, D230, H2200"]
["09030","ZENERGY - RAMKA ZEWNĘTRZNA, D300, H2200",294.8,"1-ZE-10",4.1666666666666664E-2,2,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090302","OE - Cadre extérieur, P300, H2200","OE - Outer frame, D300, H2200","OE- MARCO LATERAL EXTERIOR, D300, H2200","ZENERGY - KÜLSŐ KERET, D300, H2200"]
["09031","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D300, H2200",294.8,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090319","OE - Cadre extérieur, double perforation, P300, H2200","OE - Outer frame, double perforation, D300, H2200","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D300, H2200","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D300, H2200"]
["09032","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D300, H2200",315.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090326","OE - Cadre intérieur, double, P300, H2200","OE - Inner frame, double, D300, H2200","OE- MARCO LATERAL INTERIOR DOBLE, D300, H2200","ZENERGY - BELSŐ KERET, DUPLA, D300, H2200"]
["09040","ZENERGY - RAMKA ZEWNĘTRZNA, D400, H2200",336.6,"1-ZE-10",0.44166666666666665,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988090401","OE - Cadre extérieur, P400, H2200","OE - Outer frame, D400, H2200","OE- MARCO LATERAL EXTERIOR, D400, H2200","ZENERGY - KÜLSŐ KERET, D400, H2200"]
["09041","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D400, H2200",336.6,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090418","OE - Cadre extérieur, double perforation, P400, H2200","OE - Outer frame, double perforation, D400, H2200","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D400, H2200","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D400, H2200"]
["09042","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D400, H2200",357.5,"1-ZE-10",4.1666666666666664E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090425","OE - Cadre intérieur, double, P400, H2200","OE - Inner frame, double, D400, H2200","OE- MARCO LATERAL INTERIOR DOBLE, D400, H2200","ZENERGY - BELSŐ KERET, DUPLA, D400, H2200"]
["09060","ZENERGY - RAMKA ZEWNĘTRZNA, D600, H2200",473,"1-ZE-10",1.5,5,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090609","OE - Cadre extérieur, P600, H2200","OE - Outer frame, D600, H2200","OE- MARCO LATERAL EXTERIOR, D600, H2200","ZENERGY - KÜLSŐ KERET, D600, H2200"]
["09061","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D600, H2200",473,"1-ZE-10",0.1,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090616","OE - Cadre extérieur, double perforation, P600, H2200","OE - Outer frame, double perforation, D600, H2200","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D600, H2200","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D600, H2200"]
["09062","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D600, H2200",449.9,"1-ZE-10",0.05,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090623","OE - Cadre intérieur, double, P600, H2200","OE - Inner frame, double, D600, H2200","OE- MARCO LATERAL INTERIOR DOBLE, D600, H2200","ZENERGY - BELSŐ KERET, DUPLA, D600, H2200"]
["09080","ZENERGY - RAMKA ZEWNĘTRZNA, D800, H2200",521.4,"1-ZE-10",1.9416666666666667,8,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090807","OE - Cadre extérieur, P800, H2200","OE - Outer frame, D800, H2200","OE- MARCO LATERAL EXTERIOR, D800, H2200","ZENERGY - KÜLSŐ KERET, D800, H2200"]
["09081","ZENERGY - RAMKA ZEWNĘTRZNA, PODWÓJNA PERFORACJA, D800, H2200",521.4,"1-ZE-10",8.3333333333333329E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090814","OE - Cadre extérieur, double perforation, P800, H2200","OE - Outer frame, double perforation, D800, H2200","OE- MARCO LATERAL EXTERIOR, DOBLE PERFORACION, D800, H2200","ZENERGY - KÜLSŐ KERET, DUPLÁS PERFORÁCIÓ, D800, H2200"]
["09082","ZENERGY - RAMKA WEWNĘTRZNA, PODWÓJNA, D800, H2200",562.1,"1-ZE-10",4.1666666666666664E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,"5901988090821","OE - Cadre intérieur, double, P800, H2200","OE - Inner frame, double, D800, H2200","OE- MARCO LATERAL INTERIOR DOBLE, D800, H2200","ZENERGY - BELSŐ KERET, DUPLA, D800, H2200"]
["09200","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-30",188.3,"1-ZE-09",0.16666666666666666,4,"OM_HORIZONTAL_COVER","09200","SZT","85389099","27.12.40.0",null,"5901988092009","OM - Couvercle horizontal L1000 IP-30","OM - Two Horizontal W1000 IP-30 Lids","OM- TECHO /SUELO (2UDS) W1000 IP30 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-30"]
["09201","produkt wycofany (ZENERGY OM - COKÓŁ W1000 IP-30)",324.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09201","SZT","85389099","27.12.40.0",null,"5901988092016","produit invalidé OM - Socle L1000 IP-30","product cancelled OM - W1000 IP-30 plinth","OM- ZOCALO W1000 IP30 ","megszűnt termék (ZENERGY OM - PLINTH W1000 IP-30)"]
["09203","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",188.3,"1-ZE-09",0.15,2,"OM_HORIZONTAL_COVER","09203","SZT","85389099","27.12.40.0",null,"5901988092030","OM - Couvercle horizontal L1000 IP-30 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W1000 IP-30 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1000 IP30  CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["09204","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",188.3,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09204","SZT","85389099","27.12.40.0",null,"5901988092047","OM - Couvercle horizontal IP-30 L1000 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal W1000 IP-30 Lids with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1000 IP30  CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-30 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["09205","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",186.6,"1-ZE-09",2.5000000000000001E-2,2,"ON_HORIZONTAL_COVER","09205","SZT","85389099","27.12.40.0",null,"5901988092054","OM - Couvercle horizontal L1000 IP-30 avec trois trous 81x222 sous le passage IP-55","OM - Two Horizontal Covers W1000 IP-30 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1000 IP30  CON TRES AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-30 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["09206","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W1000 IP-30",178.2,"1-ZE-09",null,null,"OM_EXTENSION","09206","SZT","85389099","27.12.40.0",null,"5901988092061","OM - Extension de grille horizontale - Passe-câble L1000 IP-30","OM - Horizontal Extension Cover - W1000 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ.  W1000 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W1000 IP-30"]
["09207","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1000 D230 IP-30",188.3,"1-ZE-09",0.21666666666666667,6,"OM_HORIZONTAL_COVER","09207","SZT","85389099","27.12.40.0",null,"5901988092078","OM - Couvercle horizontal socle L1000 P230 IP-30","OM - Two Horizontal Plinth Covers W1000 D230 IP-30","OM- TECHO/SUELO (2UDS) W1000 D230 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1000 D230 IP-30"]
["09209","ZENERGY OM - POKRYWA TYLNA W1000 H550 9M IP-30",240.8,"1-ZE-09",null,null,"OM_BACK_COVER","09209","SZT","85389099","27.12.40.0",null,"5901988092092","OM - Couvercle arrière L1000 H550 9M IP-30","OM - Rear Cover W1000 H550 9M IP-30","OM- PANEL TRASERO W1000 H550 9M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H550 9M IP-30"]
["09212","ZENERGY OM - POKRYWA TYLNA W1000 H700 12M IP-30",252.7,"1-ZE-09",null,null,"OM_BACK_COVER","09212","SZT","85389099","27.12.40.0",null,"5901988092122","OM - Couvercle arrière L1000 H700 12M IP-30","OM - Rear Cover W1000 H700 12M IP-30","OM- PANEL TRASERO W1000 H700 12M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H700 12M IP-30"]
["09215","ZENERGY OM - POKRYWA TYLNA W1000 H850 15M IP-30",273.2,"1-ZE-09",0.01,1,"OM_BACK_COVER","09215","SZT","85389099","27.12.40.0",null,"5901988092153","OM - Couvercle arrière L1000 H850 15M IP-30","OM - Rear Cover W1000 H850 15M IP-30","OM- PANEL TRASERO W1000 H850 15M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H850 15M IP-30"]
["09218","ZENERGY OM - POKRYWA TYLNA W1000 H1000 18M IP-30",304.60000000000002,"1-ZE-09",0.05,5,"OM_BACK_COVER","09218","SZT","85389099","27.12.40.0",null,"5901988092184","OM - Couvercle arrière L1000 H1000 18M IP-30","OM - Rear Cover W1000 H1000 18M IP-30","OM- PANEL TRASERO W1000 H1000 18M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1000 18M IP-30"]
["09221","ZENERGY OM - POKRYWA TYLNA W1000 H1150 21M IP-30",320.8,"1-ZE-09",4.1666666666666664E-2,4,"OM_BACK_COVER","09221","SZT","85389099","27.12.40.0",null,"5901988092214","OM - Couvercle arrière L1000 H1150 21M IP-30","OM - Rear Cover W1000 H1150 21M IP-30","OM- PANEL TRASERO W1000 H1150 21M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1150 21M IP-30"]
["09224","ZENERGY OM - POKRYWA TYLNA W1000 H1300 24M IP-30",338,"1-ZE-09",5.8333333333333334E-2,2,"OM_BACK_COVER","09224","SZT","85389099","27.12.40.0",null,"5901988092245","OM - Couvercle arrière L1000 H1300 24M IP-30","OM - Rear Cover W1000 H1300 24M IP-30","OM- PANEL TRASERO W1000 H1300 24M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1300 24M IP-30"]
["09227","ZENERGY OM - POKRYWA TYLNA W1000 H1450 27M IP-30",352.1,"1-ZE-09",0.01,1,"OM_BACK_COVER","09227","SZT","85389099","27.12.40.0",null,"5901988092276","OM - Couvercle arrière L1000 H1450 27M IP-30","OM - Rear Cover W1000 H1450 27M IP-30","OM- PANEL TRASERO W1000 H1450 27M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1450 27M IP-30"]
["09228","ZENERGY OM - POKRYWA TYLNA W1000 H1600 28M IP-30",575.6,"1-ZE-09",4.1666666666666664E-2,5,"OM_BACK_COVER","09228","SZT","85389099","27.12.40.0",null,"5901988092283","OM - Couvercle arrière L1000 H1600 28M IP-30","OM - Rear Cover W1000 H1600 28M IP-30","OM- PANEL TRASERO W1000 H1600 28M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1600 28M IP-30"]
["09229","ZENERGY OM - POKRYWA TYLNA W1000 H1550 29M IP-30",383.4,"1-ZE-09",null,null,"OM_BACK_COVER","09229","SZT","85389099","27.12.40.0",null,"5901988092290","OM - Couvercle arrière L1000 H1550 29M IP-30","OM - Rear Cover W1000 H1550 29M IP-30","OM- PANEL TRASERO W1000 H1550 29M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1550 29M IP-30"]
["09230","ZENERGY OM - POKRYWA TYLNA W1000 H1700 30M IP-30",607,"1-ZE-09",3.3333333333333333E-2,1,"OM_BACK_COVER","09230","SZT","85389099","27.12.40.0",null,"5901988092306","OM - Couvercle arrière L1000 H1700 30M IP-30","OM - Rear Cover W1000 H1700 30M IP-30","OM- PANEL TRASERO W1000 H1700 30M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1700 30M IP-30"]
["09233","ZENERGY OM - POKRYWA TYLNA W1000 H1850 33M IP-30",810.9,"1-ZE-09",0.31666666666666665,4,"OM_BACK_COVER","09233","SZT","85389099","27.12.40.0",null,"5901988092337","OM - Couvercle arrière L1000 H1850 33M IP-30","OM - Rear Cover W1000 H1850 33M IP-30","OM- PANEL TRASERO W1000 H1850 33M IP30","ZENERGY OM -HÁTSÓ BURKOLAT W1000 H1850 33M IP-30"]
["09236","ZENERGY OM - POKRYWA TYLNA W1000 H2000 36M IP-30",846.7,"1-ZE-09",1.6666666666666666E-2,2,"OM_BACK_COVER","09236","SZT","85389099","27.12.40.0",null,"5901988092368","OM - Couvercle arrière L1000 H2000 36M IP-30","OM - Rear Cover W1000 H2000 36M IP-30","OM- PANEL TRASERO W1000 H2000 36M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H2000 36M IP-30"]
["09239","ZENERGY OM - POKRYWA TYLNA W1000 H2150 39M IP-30",942.9,"1-ZE-09",0.20833333333333334,4,"OM_BACK_COVER","09239","SZT","85389099","27.12.40.0",null,"5901988092399","OM - Couvercle arrière L1000 H2150 39M IP-30","OM - Rear Cover W1000 H2150 39M IP-30","OM- PANEL TRASERO W1000 H2150 39M IP30","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H2150 39M IP-30"]
["09240","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-30",218.3,"1-ZE-09",5.8333333333333334E-2,2,"OM_HORIZONTAL_COVER","09240","SZT","85389099","27.12.40.0",null,"5901988092405","OM - Deux couvercles horizontaux L1000 P300 IP-30","OM - Two Horizontal Covers W1000 D300 IP-30","OM- TECHO/SUELO HORIZ. W1000 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-30"]
["09241","produkt wycofany (ZENERGY OM - COKÓŁ W1000 D300 IP-30)",376.6,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09241","SZT","85389099","27.12.40.0",null,"5901988092412","produit invalidé OM - Socle L1000 P300 P300 IP-30","product cancelled OM - W1000 D300 IP-30 plinth","OM- ZOCALO W1000 D300 IP30 ","kivont termék (ZENERGY OM - PLINTH W1000 D300 IP-30)"]
["09243","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-30 Z OTWOREM 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","09243","SZT","85389099","27.12.40.0",null,"5901988092436","OM - Deux couvercles horizontaux L1000 P300 IP-30 avec ouverture 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1000 D300 IP-30 with a 81x222 opening for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W1000 D300 IP30 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-30 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["09244","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-30 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",1.6666666666666666E-2,2,"OM_HORIZONTAL_COVER","09244","SZT","85389099","27.12.40.0",null,"5901988092443","OM - Deux couvercles horizontaux L1000 P300 IP-30 avec trous DWOMA 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1000 D300 IP-30 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W1000 D300 IP30 CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-30 KÉT LYUKAL 81X222 IP-55 LÖVEDEKHEZ"]
["09245","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-30 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",218.3,"1-ZE-09",6.6666666666666666E-2,4,"OM_HORIZONTAL_COVER","09245","SZT","85389099","27.12.40.0",null,"5901988092450","OM - Deux couvercles horizontaux L1000 P300 IP-30 avec TROIS trous 81x222 pour pénétration IP-55","OM - Two Horizontal Covers W1000 D300 IP-30 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W1000 D300 IP30 CON TRES 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-30 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["09246","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W1000 D300 IP-30",206.3,"1-ZE-09",3.3333333333333333E-2,4,"OM_EXTENSION","09246","SZT","85389099","27.12.40.0",null,"5901988092467","OM - Couvercle d'expansion horizontal - L1000 P300 IP-30 ponceau L1000 P300","OM - Horizontal Extension Cover - W1000 D300 IP-30 Grommet","OM- TECHO DE MODULO AUX. HORIZ.  W1000 D300 IP30","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W1000 D300 IP-30"]
["09247","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1000 D300 IP-30",218.3,"1-ZE-09",0.1,7,"OM_HORIZONTAL_COVER","09247","SZT","85389099","27.12.40.0",null,"5901988092474","OM - Couvercle horizontal socle L1000 P300 IP-30","OM - Two Horizontal Plinth Covers W1000 D300 IP-30","OM- TECHO/SUELO (2UDS) W1000 D300 IP30","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1000 D300 IP-30"]
["09300","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-55",226.8,"1-ZE-09",0.11666666666666667,6,"OM_HORIZONTAL_COVER","09200","SZT","85389099","27.12.40.0",null,"5901988093006","OM - Couvercle horizontal L1000 IP-55","OM - Two Horizontal W1000 IP-55 Lids","OM- TECHO /SUELO (2UDS) W1000  IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-55"]
["09301","produkt wycofany (ZENERGY OM - COKÓŁ W1000 IP-55)",351,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09301","SZT","85389099","27.12.40.0",null,"5901988093013","produit invalidé OM - Socle L1000 IP-55","product cancelled OM - W1000 IP-55 plinth","OM- ZOCALO W1000 IP55","megszűnt termék (ZENERGY OM - PLINTH W1000 IP-55)"]
["09303","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",226.8,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09303","SZT","85389099","27.12.40.0",null,"5901988093037","OM - Couvercle horizontal L1000 IP-55 avec ouverture 81x222 sous IP-55","OM - Two Horizontal W1000 IP-55 Lids with a 81x222 opening for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1000  IP55 CON AGUJERO 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["09304","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",226.8,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09204","SZT","85389099","27.12.40.0",null,"5901988093044","OM - Couvercle horizontal IP-55 L1000 avec DEUX trous 81x222 sous IP-55","OM - Two Horizontal W1000 IP-55 Lids with TWO holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1000  IP55 CON DOS AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-55 KÉT LYUKÚ 81X222 AZ IP-55 GOLYÓHOZ"]
["09305","ZENERGY OM - DWIE POKRYWY POZIOME W1000 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",226.8,"1-ZE-09",0.01,2,"OM_HORIZONTAL_COVER","09205","SZT","85389099","27.12.40.0",null,"5901988093051","OM - Couvercle horizontal IP-55 L1000 avec TROIS trous 81x222 sous IP-55","OM - Two Horizontal W1000 IP-55 Lids with THREE holes 81x222 for the IP-55 bushing","OM- TECHO /SUELO (2UDS) W1000  IP55 CON TRES AGUJEROS 81X222 ","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 IP-55 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["09306","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W1000 IP-55",221.4,"1-ZE-09",null,null,"OM_EXTENSION","09206","SZT","85389099","27.12.40.0",null,"5901988093068","OM - Couvercle d'extension horizontale - Glande L1000 IP-55","OM - Horizontal Extension Cover - W1000 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ.  W1000 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W1000 IP-55"]
["09307","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1000 D230 IP-55",226.8,"1-ZE-09",8.3333333333333329E-2,4,"OM_HORIZONTAL_COVER","09307","SZT","85389099","27.12.40.0",null,"5901988093075","OM - Couvercle horizontal socle L1000 P230 IP-55","OM - Two Horizontal Plinth Covers W1000 D230 IP-55","OM- TECHO/SUELO (2UDS) W1000 D230 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1000 D230 IP-55"]
["09309","ZENERGY OM - POKRYWA TYLNA W1000 H550 9M IP-55",398.5,"1-ZE-09",null,null,"OM_BACK_COVER","09209","SZT","85389099","27.12.40.0",null,"5901988093099","OM - Couvercle arrière L1000 H550 9M IP-55","OM - Rear Cover W1000 H550 9M IP-55","OM- PANEL TRASERO W1000 H550 9M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H550 9M IP-55"]
["09312","ZENERGY OM - POKRYWA TYLNA W1000 H700 12M IP-55",418,"1-ZE-09",null,null,"OM_BACK_COVER","09212","SZT","85389099","27.12.40.0",null,"5901988093129","OM - Couvercle arrière L1000 H700 12M IP-55","OM - Rear Cover W1000 H700 12M IP-55","OM- PANEL TRASERO W1000 H700 12M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H700 12M IP-55"]
["09315","ZENERGY OM - POKRYWA TYLNA W1000 H850 15M IP-55",460.1,"1-ZE-09",null,null,"OM_BACK_COVER","09215","SZT","85389099","27.12.40.0",null,"5901988093150","OM - Couvercle arrière L1000 H850 15M IP-55","OM - Rear Cover W1000 H850 15M IP-55","OM- PANEL TRASERO W1000 H850 15M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H850 15M IP-55"]
["09318","ZENERGY OM - POKRYWA TYLNA W1000 H1000 18M IP-55",588.6,"1-ZE-09",1.6666666666666666E-2,2,"OM_BACK_COVER","09218","SZT","85389099","27.12.40.0",null,"5901988093181","OM - Couvercle arrière L1000 H1000 18M IP-55","OM - Rear Cover W1000 H1000 18M IP-55","OM- PANEL TRASERO W1000 H1000 18M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1000 18M IP-55"]
["09321","ZENERGY OM - POKRYWA TYLNA W1000 H1150 21M IP-55",527,"1-ZE-09",4.1666666666666664E-2,4,"OM_BACK_COVER","09221","SZT","85389099","27.12.40.0",null,"5901988093211","OM - Couvercle arrière L1000 H1150 21M IP-55","OM - Rear Cover W1000 H1150 21M IP-55","OM- PANEL TRASERO W1000 H1150 21M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1150 21M IP-55"]
["09324","ZENERGY OM - POKRYWA TYLNA W1000 H1300 24M IP-55",560.5,"1-ZE-09",5.8333333333333334E-2,2,"OM_BACK_COVER","09224","SZT","85389099","27.12.40.0",null,"5901988093242","OM - Couvercle arrière L1000 H1300 24M IP-55","OM - Rear Cover W1000 H1300 24M IP-55","OM- PANEL TRASERO W1000 H1300 24M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1300 24M IP-55"]
["09327","ZENERGY OM - POKRYWA TYLNA W1000 H1450 27M IP-55",590.79999999999995,"1-ZE-09",0.01,1,"OM_BACK_COVER","09227","SZT","85389099","27.12.40.0",null,"5901988093273","OM - Couvercle arrière L1000 H1450 27M IP-55","OM - Rear Cover W1000 H1450 27M IP-55","OM- PANEL TRASERO W1000 H1450 27M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1450 27M IP-55"]
["09328","ZENERGY OM - POKRYWA TYLNA W1000 H1600 28M IP-55",779.8,"1-ZE-09",0.01,1,"OM_BACK_COVER","09228","SZT","85389099","27.12.40.0",null,"5901988093280","OM - Couvercle arrière L1000 H1600 28M IP-55","OM - Rear Cover W1000 H1600 28M IP-55","OM- PANEL TRASERO W1000 H1600 28M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1600 28M IP-55"]
["09329","ZENERGY OM - POKRYWA TYLNA W1000 H1550 29M IP-55",631.79999999999995,"1-ZE-09",null,null,"OM_BACK_COVER","09229","SZT","85389099","27.12.40.0",null,"5901988093297","OM - Couvercle arrière L1000 H1550 29M IP-55","OM - Rear Cover W1000 H1550 29M IP-55","OM- PANEL TRASERO W1000 H1550 29M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1550 29M IP-55"]
["09330","ZENERGY OM - POKRYWA TYLNA W1000 H1700 39M IP-55",818.6,"1-ZE-09",4.1666666666666664E-2,2,"OM_BACK_COVER","09230","SZT","85389099","27.12.40.0",null,"5901988093303","OM - Couvercle arrière L1000 H1700 39M IP-55","OM - Rear Cover W1000 H1700 39M IP-55","OM- PANEL TRASERO W1000 H1700 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1700 39M IP-55"]
["09333","ZENERGY OM - POKRYWA TYLNA W1000 H1850 33M IP-55",962.3,"1-ZE-09",null,null,"OM_BACK_COVER","09233","SZT","85389099","27.12.40.0",null,"5901988093334","OM - Couvercle arrière L1000 H1850 33M IP-55","OM - Rear Cover W1000 H1850 33M IP-55","OM- PANEL TRASERO W1000 H1850 33M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H1850 33M IP-55"]
["09336","ZENERGY OM - POKRYWA TYLNA W1000 H2000 36M IP-55",1012,"1-ZE-09",3.3333333333333333E-2,2,"OM_BACK_COVER","09236","SZT","85389099","27.12.40.0",null,"5901988093365","OM - Couvercle arrière L1000 H2000 36M IP-55","OM - Rear Cover W1000 H2000 36M IP-55","OM- PANEL TRASERO W1000 H2000 36M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H2000 36M IP-55"]
["09339","ZENERGY OM - POKRYWA TYLNA W1000 H2150 39M IP-55",1051.9000000000001,"1-ZE-09",0.11666666666666667,1,"OM_BACK_COVER","09239","SZT","85389099","27.12.40.0",null,"5901988093396","OM - Couvercle arrière L1000 H2150 39M IP-55","OM - Rear Cover W1000 H2150 39M IP-55","OM- PANEL TRASERO W1000 H2150 39M IP55","ZENERGY OM - HÁTSÓ BURKOLAT W1000 H2150 39M IP-55"]
["09340","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-55",263.2,"1-ZE-09",5.8333333333333334E-2,2,"OM_HORIZONTAL_COVER","09240","SZT","85389099","27.12.40.0",null,"5901988093402","OM - Deux couvercles horizontaux L1000 P300 IP-55","OM - Two Horizontal Lids W1000 D300 IP-55","OM- TECHO/SUELO HORIZ. W1000 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-55"]
["09341","produkt wycofany (ZENERGY OM - COKÓŁ W1000 D300 IP-55)",407.7,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09341","SZT","85389099","27.12.40.0",null,"5901988093419","produit invalidé OM - Socle L1000 P300 P300 IP-55","product cancelled OM - Plinth W1000 D300 IP-55","OM- ZOCALO W1000 D300 IP55 ","kivont termék (ZENERGY OM - PLINTH W1000 D300 IP-55)"]
["09343","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-55 Z OTWOREM 81X222 POD PRZEPUST IP-55",263.2,"1-ZE-09",null,null,"OM_HORIZONTAL_COVER","09243","SZT","85389099","27.12.40.0",null,"5901988093433","OM - Deux couvercles horizontaux L1000 P300 IP-55 avec trou 81x222 pour ponceau IP-55","OM - Two Horizontal Covers W1000 D300 IP-55 with an opening 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W1000 D300 IP55 CON 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-55 81X222 LYUKAL AZ IP-55 LÖVEDEKHEZ"]
["09344","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-55 Z DWOMA OTWORAMI 81X222 POD PRZEPUST IP-55",263.2,"1-ZE-09",1.6666666666666666E-2,2,"OM_HORIZONTAL_COVER","09244","SZT","85389099","27.12.40.0",null,"5901988093440","OM - Deux couvercles horizontaux L1000 P300 IP-55 avec trous DWOMA 81x222 pour pénétration IP-55","OM - Two Horizontal Covers W1000 D300 IP-55 with TWO holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W1000 D300 IP55 CON DOS 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-55 KÉT LYUKAL 81X222 AZ IP-55 GOLYÓHOZ"]
["09345","ZENERGY OM - DWIE POKRYWY POZIOME W1000 D300 IP-55 Z TRZEMA OTWORAMI 81X222 POD PRZEPUST IP-55",263.2,"1-ZE-09",0.01,1,"OM_HORIZONTAL_COVER","09245","SZT","85389099","27.12.40.0",null,"5901988093457","OM - Deux couvercles horizontaux L1000 P300 IP-55 avec TROIS trous 81x222 pour pénétration IP-55","OM - Two Horizontal Lids W1000 D300 IP-55 with THREE holes 81x222 for the IP-55 bushing","OM- TECHO/SUELO (2UDS) W1000 D300 IP55 CON TRES 81X222 PARA MEMBRANA IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT W1000 D300 IP-55 HÁROM LYUKÚ 81X222 AZ IP-55 LÖVEDEKHEZ"]
["09346","ZENERGY OM - POKRYWA POZIOMA ROZSZERZENIA - PRZEPUST W1000 D300 IP-55",257,"1-ZE-09",0.01,1,"OM_EXTENSION","09246","SZT","85389099","27.12.40.0",null,"5901988093464","OM - Couvercle d'expansion horizontal - L1000 P300 IP-55 - ponceau L1000 P300","OM - Horizontal Extension Cover - W1000 D300 IP-55 Grommet","OM- TECHO DE MODULO AUX. HORIZ.  W1000 D300 IP55","ZENERGY OM - BŐVÍTÉSI SZINT BURKOLAT - BULLET W1000 D300 IP-55"]
["09347","ZENERGY OM - DWIE POKRYWY POZIOME COKOŁU W1000 D300 IP-55",263.2,"1-ZE-09",1.6666666666666666E-2,4,"OM_HORIZONTAL_COVER","09347","SZT","85389099","27.12.40.0",null,"5901988093471","OM - Couvercle horizontal socle L1000 P300 IP-55","OM - Two Horizontal Plinth Covers W1000 D300 IP-55","OM- TECHO/SUELO (2UDS) W1000 D300 IP55","ZENERGY OM - KÉT VÍZSZINTES BURKOLAT A LÁZBAHOZ W1000 D300 IP-55"]
["10027","AlCubar - Profil anodowany H27, 277mm2, 1 rowek Cu 8mm, 630A dt 55C",130.69999999999999,"1-ZE-08",19.541666666666668,11,"OE_BUSBARS_ALCUBAR","20022","M","76042990","24.42.22.0",null,"5901988100278","AlCubar - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C","AlCubar - Aluminum anodized busbar profile Al-Cu H27, 360 mm2, 1 Copper row, 8 mm, 630A dt 39C, 800A dt 57C","*AlCubar - Perfil H27 anodizado, 277mm2, 1 ranura Cu 8mm, 630A dt 55C","AlCubar - Eloxált profil H27, 277mm2, 1 Cu horony 8mm, 630A dt 55C"]
["10050","AlCubar - Profil anodowany H50R, 670mm2, 2 rowki Cu, 8mm/12mm, 1250A dt 55C",231.6,"1-ZE-08",0.49166666666666664,5,"OE_BUSBARS_ALCUBAR","10050","M","76042990","24.42.22.0",null,"5901988100506","AlCubar - Profilé anodisé AlCubar H50R, 2 rainures en Cu, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C","AlCubar - Anodized busbar profile Al-Cu H50R, 670mm2, 2 Copper rows, 8/12 mm, 1250A dt 55C","*AlCubar - Perfil anodizado H50R, 670mm2, 2 ranuras Cu, 8mm/12mm, 1250A dt 55C","AlCubar - Eloxált profil H50R, 670mm2, 2 Cu horony, 8mm/12mm, 1250A dt 55C"]
["10051","AlCubar - Profil anodowany H50, 480mm2, 1 rowek Cu, 1000A dt 55C",194.7,"1-ZE-08",0.31666666666666665,1,"OE_BUSBARS_ALCUBAR","10051","M","76042990","24.42.22.0",null,"5901988100513","AlCubar - Profilé anodisé H50, 480 mm2, 1 gorge Cu, 1000A dt 55C","AlCubar - Aluminum anodized busbar profile Al-Cu H50 480 mm2, 1 copper groove, 1000A dt 55C","*AlCubar - Perfil anodizado H50, 480mm2, 1 ranura Cu, 1000A dt 55C","AlCubar - H50 eloxált profil, 480mm2, 1 Cu horony, 1000A dt 55C"]
["10052","AlCubar - Profil anodowany H50, 480mm2, 2 rowki Cu 8mm, 1000A dt 55C",222.6,"1-ZE-08",1.7250000000000001,5,"OE_BUSBARS_ALCUBAR","10052","M","7604299000",null,null,"5901988100520","AlCubar - Profilé anodisé H50, 480 mm2, 2 gorge Cu 8mm, 1000A dt 55C","AlCubar - Aluminum anodized busbar profile Al-Cu H50 480 mm2, 2 copper groove 8mm, 1000A dt 55C","*AlCubar - Perfil anodizado H50, 480mm2, 2 ranura Cu 8mm, 1000A dt 55C","AlCubar - Eloxált profil H50, 480mm2, 2 Cu horony 8mm, 1000A dt 55C"]
["10053","AlCu - Osłona mostu 3P H50 AlCubar, rozstaw 105mm, poliwęglan",69.400000000000006,"1-ZE-08",0.01,1,"OE_SEPARATION_BUSBAR","10053","SZT","8538909900",null,"230703RT","5901988100537","AlCu - Couvercle de pont 3P H50 AlCubar, polycarbonate","AlCu - AlCubar H50 3P bridge cover, distance 105mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H50 3P, POLICARBONATO","AlCu - Hídburkolat 3P H50 AlCubar, távolság 105mm, polikarbonát"]
["10054","AlCu - Osłona mostu 4P H50 AlCubar, rozstaw 75mm, poliwęglan",80.599999999999994,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10054","SZT","8538909900",null,"230703RT","5901988100544","AlCu - Couvercle de pont 4P H50 AlCubar, polycarbonate","AlCu - AlCubar H50 4P bridge cover, distance 75mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H50 4P, POLICARBONATO","AlCu - Hídburkolat 4P H50 AlCubar, távolság 75mm, polikarbonát"]
["10073","AlCu - Osłona mostu 3P H75 AlCubar, rozstaw 105mm, poliwęglan",90.2,"1-ZE-08",3.3333333333333333E-2,1,"OE_SEPARATION_BUSBAR","10073","SZT","8538909900",null,"230703RT","5901988100735","AlCu - Couvercle de pont 3P H75 AlCubar, polycarbonate","AlCu - AlCubar H75 3P bridge cover, distance 105mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H75 3P, POLICARBONATO","AlCu - Hídburkolat 3P H75 AlCubar, távolság 105mm, polikarbonát"]
["10074","AlCu - Osłona mostu 4P H75 AlCubar, rozstaw 75mm, poliwęglan",105.3,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10074","SZT","8538909900",null,"230703RT","5901988100742","AlCu - Couvercle de pont 4P H75 AlCubar, polycarbonate","AlCu - AlCubar H75 4P bridge cover, distance 75mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H75 4P, POLICARBONATO","AlCu - Hídburkolat 4P H75 AlCubar, távolság 75mm, polikarbonát"]
["10075","AlCubar - Profil anodowany H75, 1100 mm2, 2 rowki Cu, 1600A dt 55C",348.5,"1-ZE-08",3.8416666666666668,8,"OE_BUSBARS_ALCUBAR","10075","M","76042990","24.42.22.0",null,"5901988100759","AlCubar - Profilé anodisé AlCubar H75, 1100 mm2, 2 rainures en Cu, 1600A dt 55C","ALCubar - Aluminum anodized busbar profile Al-Cu  H75, 1100 mm2, 2 Copper rows, 1600A dt 55C","*AlCubar - Perfil anodizado H75, 1100 mm2, 2 ranuras Cu, 1600A dt 55C","AlCubar - H75 eloxált profil, 1100 mm2, 2 Cu horony, 1600A dt 55C"]
["10076","AlCubar - Łącznik Cu 1600A, typu L1, 125x75x10mm",152.30000000000001,"1-ZE-08",0.25,4,"OE_BUSBARS_ALCUBAR","10076","SZT","7407290000",null,"230412PW","5901988100766","AlCu - Connecteur Cu 1600 A, type L1, 125x75x10mm","AlCu - Cu 1600 A connector, type L1, 125x75x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO L1, 125X75X10MM","AlCubar - Cu csatlakozó 1600A, L1 típus, 125x75x10mm"]
["10077","AlCubar - Łącznik Cu 1600A, typu L2, 145x75x10mm",179.2,"1-ZE-08",0.21666666666666667,5,"OE_BUSBARS_ALCUBAR","10077","SZT","7407290000",null,"230412PW","5901988100773","AlCu - Connecteur Cu 1600 A, type L2, 145x75x10mm","AlCu - Cu 1600 A connector, type L2, 145x75x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO L2, 145X75X10MM","AlCubar - Cu csatlakozó 1600A, L2 típus, 145x75x10mm"]
["10078","AlCubar - Łącznik Cu 1600A, typu I, 215x75x10mm",251.1,"1-ZE-08",0.5,4,"OE_BUSBARS_ALCUBAR","10078","SZT","7407290000",null,"230412PW","5901988100780","AlCu - Connecteur Cu 1600 A, type I, 165x75x10mm","AlCu - Cu 1600 A connector, type I, 165x75x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO I, 165X75X10MM","AlCubar - Cu csatlakozó 1600A, I-es típus, 215x75x10mm"]
["10079","AlCubar - Łącznik Cu 1600A, typu T, 240x75x10mm",289,"1-ZE-08",0.13333333333333333,2,"OE_BUSBARS_ALCUBAR","10079","SZT","74072900",null,"230412PW","5901988100797","AlCu - Connecteur Cu 1600 A, type T, 240x75x10mm","AlCu - Cu 1600 A connector, type T, 240x75x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO T, 240X75X10MM","AlCubar - Cu csatlakozó 1600A, T-típus, 240x75x10mm"]
["10100","AlCubar - Profil anodowany H100R, 2490mm2, 2 rowki Cu, 8mm/12mm, 2500A dt 55C",594,"1-ZE-08",4.45,11,"OE_BUSBARS_ALCUBAR","10100","M","7604299000","24.42.22.0",null,"5901988101008","AlCubar - Profilé anodisé AlCubar H100R, 2490mm2, 2 rainures en Cu, 8 mm et 12 mm, 2500A dt 50C","AlCubar - Aluminum anodized busbar profile Al-Cu H100R, 2490mm2, 2 Copper rows, 8 mm & 12 mm, 2500A dt 50C","*AlCubar - Perfil anodizado H100R, 2490mm2, 2 ranuras Cu, 8mm/12mm, 2500A dt 55C","AlCubar - Eloxált profil H100R, 2490mm2, 2 Cu horony, 8mm/12mm, 2500A dt 55C"]
["10102","AlCubar - Profil anodowany H100, 2500 mm2, 2 rowki Cu 8mm, 2500A dt 53C",601.20000000000005,"1-ZE-08",4.3250000000000002,10,"OE_BUSBARS_ALCUBAR","10102","M","76042990","24.42.22.0",null,"5901988101022","AlCubar - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 53C","AlCubar - Aluminum anodized busbar profile Al-Cu H100, 2500 mm2, 2 copper grooves, 2500A dt 53C","*AlCubar - Perfil anodizado H100, 2500 mm2, 2 ranuras Cu, 2500A dt 53C","AlCubar - Eloxált profil H100, 2500 mm2, 2 Cu horony 8 mm, 2500A dt 53C"]
["10103","AlCu - Osłona mostu 3P H100 AlCubar, rozstaw 105mm, poliwęglan",111.4,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10103","SZT","8538909900",null,"230703RT","5901988101039","AlCu - Couvercle de pont 3P H100 AlCubar, polycarbonate","AlCu - AlCubar H100 3P bridge cover, distance 105mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H100 3P, POLICARBONATO","AlCu - Hídburkolat 3P H100 AlCubar, távolság 105mm, polikarbonát"]
["10104","AlCu - Osłona mostu 4P H100 AlCubar, rozstaw 75mm, poliwęglan",129.9,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10104","SZT","8538909900",null,"230703RT","5901988101046","AlCu - Couvercle de pont 4P H100 AlCubar, polycarbonate","AlCu - AlCubar H100 4P bridge cover, distance 75mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H100 4P, POLICARBONATO","AlCu - Hídburkolat 4P H100 AlCubar, távolság 75mm, polikarbonát"]
["10106","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H400 X W600 2X24MOD IP30, 6H MOD, BEZ DRZWI",429.3,"1-ZE-03",8.3333333333333329E-2,5,"PT_ENCLOSURES","10106","SZT","85381000","27.12.40.0",null,"5901988101060","PT - 2x24MOD IP40, appareillage caché MOD, Portes pleine H400 x L600","PT - H400 x W600 2x24MOD IP40, 6H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL. H400 x W600 2x24MOD IP40, 6H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H400 X W600 2X24MOD IP30, 6H MOD, AJTÓ NÉLKÜL"]
["10109","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H550 X W600 3X24MOD IP30, 9H MOD, BEZ DRZWI",518.29999999999995,"1-ZE-03",0.39166666666666666,8,"PT_ENCLOSURES","10109","SZT","85381000","27.12.40.0",null,"5901988101091","PT - 3 appareillages cachés MOD, IP40, 9x24MOD, Portes pleine H550 x L600","PT - H550 x W600 3x24MOD IP40, 9H MOD, in-wall distribution board, without door","ON- EMPOTRAR METAL. H550 x W600 3x24MOD IP40, 9H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H550 X W600 3X24MOD IP30, 9H MOD, AJTÓ NÉLKÜL"]
["10112","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H700 X W600 4X24MOD IP30, 12H MOD, BEZ DRZWI",602.1,"1-ZE-03",1.5,12,"PT_ENCLOSURES","10112","SZT","85381000","27.12.40.0",null,"5901988101121","PT - Distributeur à encastrer 4x24MOD IP40, MOD 12H, Portes pleine H700 x L600","PT - H700 x W600 4x24MOD IP40, 12H MOD, without door distribution board","ON- EMPOTRAR METAL. H700 x W600 4x24MOD IP40, 12H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H700 X W600 4X24MOD IP30, 12H MOD, AJTÓ NÉLKÜL"]
["10115","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H850 X W600 5X24MOD IP30, 15H MOD, BEZ DRZWI",712.3,"1-ZE-03",1.1916666666666667,12,"PT_ENCLOSURES","10115","SZT","85381000","27.12.40.0",null,"5901988101152","PT - Appareillage encastrable 5x24MOD IP40, MOD 15H, Portes pleine H850 x L600","PT - H850 x W600 5x24MOD IP40, 15H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL. H850 x W600 5x24MOD IP40, 15H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H850 X W600 5X24MOD IP30, 15H MOD, AJTÓ NÉLKÜL"]
["10118","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1000 X W600 6X24MOD IP30, 18H MOD, BEZ DRZWI",822.6,"1-ZE-03",0.59166666666666667,11,"PT_ENCLOSURES","10118","SZT","85381000","27.12.40.0",null,"5901988101183","PT - 6x24MOD IP40, Appareillage caché MOD 18H, Portes pleine H1000 x L600","PT - H1000 x W600 6x24MOD IP40, 18H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL. H1000 x W600 6x24MOD IP40, 18H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLÁZAT H1000 X W600 6X24MOD IP30, 18H MOD, AJTÓ NÉLKÜL"]
["10121","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1150 X W600 7X24MOD IP30, 21H MOD, BEZ DRZWI",938.1,"1-ZE-03",0.38333333333333336,8,"PT_ENCLOSURES","10121","SZT","85381000","27.12.40.0",null,"5901988101213","PT - Distributeur à encastrer 7x24MOD IP40, 21H MOD, Portes pleine H1150 x L600","PT - H1150 x W600 7x24MOD IP40, 21H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL. H1150 x W600 7x24MOD IP40, 21H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1150 X W600 7X24MOD IP30, 21H MOD, AJTÓ NÉLKÜL"]
["10124","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1300 X W600 8X24MOD IP30, 24H MOD, BEZ DRZWI",1045.2,"1-ZE-03",8.3333333333333329E-2,7,"PT_ENCLOSURES","10124","SZT","85381000","27.12.40.0",null,"5901988101244","PT - Appareillage caché 8x24MOD IP40, MOD 24H, Portes pleine H1300 x L600","PT - H1300 x W600 8x24MOD IP40, 24H MOD, without door switchgear","ON- EMPOTRAR METAL. H1300 x W600 8x24MOD IP40, 24H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1300 X W600 8X24MOD IP30, 24H MOD, AJTÓ NÉLKÜL"]
["10127","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1450 X W600 9X24MOD IP30, 27H MOD, BEZ DRZWI",1148,"1-ZE-03",0.01,1,"PT_ENCLOSURES","10127","SZT","85381000","27.12.40.0",null,"5901988101275","PT - Appareillage dissimulé 9x24MOD IP40, MOD 27H, Portes pleine H1450 x L600","PT - H1450 x W600 9x24MOD IP40, 27H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL. H1450 x W600 9x24MOD IP40, 27H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1450 X W600 9X24MOD IP30, 27H MOD, AJTÓ NÉLKÜL"]
["10130","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1600 X W600 10X24MOD IP30, 30H MOD, BEZ DRZWI",1423.6,"1-ZE-03",0.05,4,"PT_ENCLOSURES","10130","SZT","85381000","27.12.40.0",null,"5901988101305","PT - Appareillage dissimulé 10x24MOD IP40, MOD 30H, Portes pleine H1600 x L600","PT - H1600 x W600 10x24MOD IP40, 30H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL. H1600 x W600 10x24MOD IP40, 30H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1600 X W600 10X24MOD IP30, 30H MOD, AJTÓ NÉLKÜL"]
["10150","AlCubar - Profil anodowany H150R, 3727mm2, 3 rowki Cu, 8mm i 12mm, 3400A dt 55C",912,"1-ZE-08",3.1166666666666667,6,"OE_BUSBARS_ALCUBAR","10150","M","76042990","24.42.22.0",null,"5901988101503","AlCubar - Profilé anodisé AlCubar H150R, 3727mm2, 3 rainures en Cu, 8 mm et 12 mm, 3400A dt 55C","Aluminum anodized busbar profile Al-Cu AlCubar H150R, 3727mm2, 3 Copper rows, 8 mm & 12 mm, 3400A dt 55C","*AlCubar - Perfil anodizado H150R, 3727mm2, 3 ranuras Cu, 8mm y 12mm, 3400A dt 55C","AlCubar - Eloxált profil H150R, 3727mm2, 3 Cu horony, 8mm és 12mm, 3400A dt 55C"]
["10151","AlCubar - Łącznik Cu 3200A,  typu L2 H150 z H100 pion, 2x(190x75x10mm)",436.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10151","SZT",null,null,"240702LK","5901988101510","AlCubar - Connecteur Cu 3200A, type L2 H150 avec H100 verticale, 2x(190x75x10mm)","AlCubar - Cu connector 3200A, type L2 H150 with H100 vertical, 2x(190x75x10mm)","*AlCubar - Conector Cu 3200A, tipo L2 H150 de H100 vertical, 2x(190x75x10mm)","AlCubar - Cu 3200A csatlakozó, L2 H150 típus, H100 függőleges, 2x (190x75x10mm)"]
["10153","AlCu - Osłona mostu 3P H150 AlCubar, rozstaw 105mm, poliwęglan",156.80000000000001,"1-ZE-08",0.31666666666666665,4,"OE_SEPARATION_BUSBAR","10153","SZT","8538909900",null,"230629RT","5901988101534","AlCu - Couvercle de pont 3P H150 AlCubar, polycarbonate","AlCu - AlCubar H150 3P bridge cover, distance 105mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H150 3P, POLICARBONATO","AlCu - Hídburkolat 3P H150 AlCubar, távolság 105mm, polikarbonát"]
["10154","AlCubar - Profil anodowany H150, 3427mm2, 4 rowki Cu 8mm, 3200A dt 55C",801.9,"1-ZE-08",2.1333333333333333,8,"OE_BUSBARS_ALCUBAR","10154","M","76042990","24.42.22.0",null,"5901988101541","AlCubar - Profilé anodisé AlCubar H150, 3427mm2, 4 rainures en Cu, 8 mm.  3200A dt 55C","Aluminum anodized busbar profile Al-Cu AlCubar H150, 3427mm2, 4 Copper rows, 8 mm, 3200A dt 55C","ALCUB- PERFIL ALCUBAR H150, 4CU 3200A L=1000MM","AlCubar - Eloxált profil H150, 3427mm2, 4 horony Cu 8mm, 3200A dt 55C"]
["10155","AlCu - Osłona mostu 4P H150 AlCubar, rozstaw 75mm, poliwęglan",184.8,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10155","SZT","8538909900",null,"230629RT","5901988101558","AlCu - Couvercle de pont 4P H150 AlCubar, polycarbonate","AlCu - AlCubar H150 4P bridge cover, distance 75mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H150 4P, POLICARBONATO","AlCu - Hídburkolat 4P H150 AlCubar, távolság 75mm, polikarbonát"]
["10156","AlCubar - Łącznik Cu 3200A,  typu L1, 2x(240x75x10mm)",597,"1-ZE-08",0.43333333333333335,5,"OE_BUSBARS_ALCUBAR","10156","SZT","74072900",null,null,"5901988101565","AlCubar - Connecteur Cu 3200A, type L1, 2x(240x75x10mm)","AlCubar - Cu connector 3200A, type L1, 2x(240x75x10mm)","*AlCubar - Conector Cu 3200A, tipo L1, 2x(240x75x10mm)","AlCubar - Cu csatlakozó 3200A, L1 típus, 2x (240x75x10mm)"]
["10157","AlCubar - Łącznik Cu 3200A,  typu I, 2x(260x75x10mm)",609.29999999999995,"1-ZE-08",1.2416666666666667,8,"OE_BUSBARS_ALCUBAR","10157","SZT","74072900",null,null,"5901988101572","AlCubar - Connecteur Cu 3200A, type I, 2x(210x75x10mm)","AlCubar - Cu connector 3200A, type I, 2x(210x75x10mm)","*AlCubar - Conector Cu 3200A, tipo I, 2x(210x75x10mm)","AlCubar - Cu csatlakozó 3200A, I-es típus, 2x (260x75x10mm)"]
["10158","AlCubar - Łącznik Cu 3200A,  typu T, 2x(370x75x10mm)",873.6,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10158","SZT","74072900",null,null,"5901988101589","AlCubar - Connecteur Cu 3200A, type T, 2x(370x75x10mm)","AlCubar - Cu connector 3200A, type T, 2x(370x75x10mm)","*AlCubar - Conector Cu 3200A, tipo T, 2x(370x75x10mm)","AlCubar - Cu csatlakozó 3200A, T-típus, 2x (370x75x10mm)"]
["10159","AlCubar - Łącznik Cu 3200A, tupu I ,rozłącznik listwowy dla H150R, 2x(345x75x10mm)",764.6,"1-ZE-08",1.6666666666666666E-2,1,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,null,null,null,null,"AlCubar - Cu 3200A csatlakozó, I. típusú, szalagos szakaszoló H150R-hez, 2x (345x75x10mm)"]
["10160","AlCubar - Łącznik Cu 3200A, typu I, H150R, M12, 300x125x10mm",581,null,null,null,"OE_BUSBARS_ALCUBAR",null,null,"74072900",null,null,"5901988101602"]
["10203","AlCu - Osłona mostu 3P H200 AlCubar, rozstaw 105mm, poliwęglan",196,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10203","SZT","8538909900",null,"230703RT","5901988102036","AlCu - Couvercle de pont 3P H200 AlCubar, polycarbonate","AlCu - AlCubar H200 3P bridge cover, distance 105mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H200 3P, POLICARBONATO","AlCu - Hídburkolat 3P H200 AlCubar, távolság 105mm, polikarbonát"]
["10204","AlCu - Osłona mostu 4P H200 AlCubar, rozstaw 75mm, poliwęglan",229.6,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR","10204","SZT","8538909900",null,"230703RT","5901988102043","AlCu - Couvercle de pont 4P H200 AlCubar, polycarbonate","AlCu - AlCubar H200 4P bridge cover, distance 75mm, polycarbonate","ALCUB- TAPA PUENTE ALCUB- H200 4P, POLICARBONATO","AlCu - Hídburkolat 4P H200 AlCubar, távolság 75mm, polikarbonát"]
["10206","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H400 X W800 x D180 2X35MOD IP30, 6H MOD, BEZ DRZWI",550.1,"1-ZE-03",null,null,"PT_ENCLOSURES","10206","SZT","85381000",null,null,"5901988102067","PT - 2x35MOD IP40, appareillage caché MOD, Portes pleine H400 x L800","PT - H400 x W800 x D180 2x35MOD IP40, 6H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL.H400 x W800 x D180 2x35MOD IP40, 6H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H400 X W800 x D180 2X35MOD IP30, 6H MOD, AJTÓ NÉLKÜL"]
["10209","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H550 X W800 x D180 3X35MOD IP30, 9H MOD, BEZ DRZWI",676.3,"1-ZE-03",0.01,1,"PT_ENCLOSURES","10209","SZT","85381000",null,null,"5901988102098","PT - 3 appareillages cachés MOD, IP40, 9x35MOD, Portes pleine H550 x L800","PT - H550 x W800 x D180 3x35MOD IP40, 9H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL.H550 x W800 x D180 3x35MOD IP40, 9H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H550 X W800 x D180 3X35MOD IP30, 9H MOD, AJTÓ NÉLKÜL"]
["10212","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H700 X W800 x D180 4X35MOD IP30, 12H MOD, BEZ DRZWI",797.1,"1-ZE-03",null,null,"PT_ENCLOSURES","10212","SZT","85381000",null,null,"5901988102128","PT - Distributeur à encastrer 4x35MOD IP40, MOD 12H, Portes pleine H700 x L800","PT - H700 x W800 x D180 4x35MOD IP40, 12H MOD, without door, flush-mounted distribution board","ON- EMPOTRAR METAL.H700 x W800 x D180 4x35MOD IP40, 12H MOD, SIN PUERTA","ZENERGY PT - H7 SÜLTETETT KAPCSOLÓTÁBLA00 X W800 x D180 4X35MOD IP30, 12H MOD, AJTÓ NÉLKÜL"]
["10215","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H850 X W800 x D180 5X35MOD IP30, 15H MOD, BEZ DRZWI",948.7,"1-ZE-03",0.01,1,"PT_ENCLOSURES","10215","SZT","85381000",null,null,"5901988102159","PT - Appareillage encastrable 5x35MOD IP40, MOD 15H, Portes pleine H850 x L800","PT - H850 x W800 x D180 5x35MOD IP40, 15H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL.H850 x W800 x D180 5x35MOD IP40, 15H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H850 X W800 x D180 5X35MOD IP30, 15H MOD, AJTÓ NÉLKÜL"]
["10218","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1000 X W800 x D180 6X35MOD IP30, 18H MOD, BEZ DRZWI",1100.3,"1-ZE-03",0.01,1,"PT_ENCLOSURES","10218","SZT","85381000",null,null,"5901988102180","PT - 6x35MOD IP40, Appareillage caché MOD 18H, Portes pleine H1000 x L800","PT - H1000 x W800 x D180 6x35MOD IP40, 18H MOD, flush-mounted distribution board, without door","ON- EMPOTRAR METAL.H1000 x W800 x D180 6x35MOD IP40, 18H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1000 X W800 x D180 6X35MOD IP30, 18H MOD, AJTÓ NÉLKÜL"]
["10221","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1150 X W800 x D180 7X35MOD IP30, 21H MOD, BEZ DRZWI",1257.2,"1-ZE-03",1.6666666666666666E-2,1,"PT_ENCLOSURES","10221","SZT","85381000",null,null,"5901988102210","PT - Distributeur à encastrer 7x35MOD IP40, 21H MOD, Portes pleine H1150 x L800","PT - H1150 x W800 x D180 7x35MOD IP40, 21H MOD, without door, distribution board","ON- EMPOTRAR METAL.H1150 x W800 x D180 7x35MOD IP40, 21H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLÁZAT H1150 X W800 x D180 7X35MOD IP30, 21H MOD, AJTÓ NÉLKÜL"]
["10224","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1300 X W800 x D180 8X35MOD IP30, 24H MOD, BEZ DRZWI",1405.6,"1-ZE-03",null,null,"PT_ENCLOSURES","10224","SZT","85381000",null,null,"5901988102241","PT - Appareillage caché 8x35MOD IP40, MOD 24H, Portes pleine H1300 x L800","PT - H1300 x W800 x D180 8x35MOD IP40, 24H MOD, without door, distribution board","ON- EMPOTRAR METAL.H1300 x W800 x D180 8x35MOD IP40, 24H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1300 X W800 x D180 8X35MOD IP30, 24H MOD, AJTÓ NÉLKÜL"]
["10227","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1450 X W800 x D180 9X35MOD IP30, 27H MOD, BEZ DRZWI",1555,"1-ZE-03",0.01,1,"PT_ENCLOSURES","10227","SZT","85381000",null,null,"5901988102272","PT - Appareillage dissimulé 9x35MOD IP40, MOD 27H, Portes pleine H1450 x L800","PT - H1450 x W800 x D180 9x35MOD IP40, 27H MOD, without door, distribution board","ON- EMPOTRAR METAL.H1450 x W800 x D180 9x35MOD IP40, 27H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1450 X W800 x D180 9X35MOD IP30, 27H MOD, AJTÓ NÉLKÜL"]
["10230","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1600 X W800 x D180 10X35MOD IP30, 30H MOD, BEZ DRZWI",1799.9,"1-ZE-03",6.6666666666666666E-2,5,"PT_ENCLOSURES","10230","SZT","85381000",null,null,"5901988102302","PT - Appareillage dissimulé 10x35MOD IP40, MOD 30H, Portes pleine H1600 x L800","PT - H1600 x W800 x D180 10x35MOD IP40, 30H MOD, without door, distribution board","ON- EMPOTRAR METAL.H1600 x W800 x D180 10x35MOD IP40, 30H MOD, SIN PUERTA","ZENERGY PT - SÜLÉKBESZERELŐ KAPCSOLÓTÁBLA H1600 X W800 x D180 10X35MOD IP30, 30H MOD, AJTÓ NÉLKÜL"]
["12010","OE - Osłona czołowa pełna W400, 1M / 250",37.700000000000003,"1-ZE-01",null,null,"01_PLAIN_COVERS","12010","SZT","85389099","27.12.40.0","230614RT","5901988120108","OE - Couverture avant complète L400, 1M / 250","OE - Plain Front cover W400, 1M / 250","OE- TAPA CIEGA W400, 1M (H 50MM)","OE - Teljes első burkolat W400, 1M / 250"]
["12020","OE - Osłona czołowa pełna W400, 2M / 250",41.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12020","SZT","85389099","27.12.40.0","230614RT","5901988120207","OE - Couverture avant complète L400, 2M / 250","OE - Plain Front cover W400, 2M / 250","OE- TAPA CIEGA W400, 2M (H 100MM)","OE - Teljes első burkolat W400, 2M / 250"]
["12025","OE - Osłona aparatury modułowej W400, 2M / 250, 11 mod",42.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12025","SZT","85389099",null,"230614RT","5901988120252","OE - Couverture d'appareil modulaire L400, 2M / 250, 11 mod","OE - Modular equipment cover W400, 2M / 250, 11 mod","OE-TAPA MODULAR W400, 2M (H 100MM) 11 MOD","OE - W400 moduláris berendezés burkolat, 2M / 250, 11 mod"]
["12028","OE - Osłona czołowa perforowana W400, 2M / 250",50.7,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12028","SZT","85389099",null,"230614RT","5901988120283","OE - Couvercle avant perforé L400, 2M / 250","OE - Perforated Front cover W400, 2M / 250","OE- TAPA FRONTAL VENTILADA W400, 2M (H 100MM)","OE - Perforált előlap W400, 2M / 250"]
["12030","OE - Osłona czołowa pełna W400, 3M / 250",43.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","12030","SZT","85389099","27.12.40.0","230614RT","5901988120306","OE - Couverture avant complète L400, 3M / 250","OE - Plain Front cover W400, 3M / 250","OE- TAPA CIEGA W400, 3M (H 150MM)","OE - Teljes első burkolat W400, 3M / 250"]
["12031","OE - Osłona czołowa W400, 3M / 250, otw. 92x92",44.7,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12031","SZT","85389099","27.12.40.0","230614RT","5901988120313","OE - Cache avant complet L400, 3M / 250, ouvert 92x92","OE - W400, 3M / 250 Front cover, hole 92x92","OE- TAPA CIEGA W400, 3M (H 150MM) CON AGUJERO 92X92","OE - Első burkolat W400, 3M / 250, nyitható 92x92"]
["12032","OE - Osłona czołowa wgłębiona, W400, 3M / 250",162.80000000000001,"1-ZE-01",null,null,"01_PLAIN_COVERS","12032","SZT","85389099",null,"230614RT","5901988120320","OE - Couvercle avant profond de, L400,  3M / 250","OE - Recessed front hood, W400, 3M / 250","OE- TAPA FRONTAL EMPOTRADA W400, 3M / 250","OE - Süllyesztett előlap, W400, 3M / 250"]
["12035","OE - Osłona aparatury modułowej W400, 3M / 250, 11 mod",44.7,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12035","SZT","85389099","27.12.40.0","230614RT","5901988120351","OE - Couverture d'appareil modulaire L400, 3M / 250, 11 mod","OE - Modular equipment cover W400, 3M / 250, 11 mod","OE-TAPA MODULAR W400, 3M (H 150MM) 11 MOD","OE - W400 moduláris berendezés burkolat, 3M / 250, 11 mod"]
["12038","OE - Osłona czołowa perforowana W400, 3M / 250",52.9,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12038","SZT","85389099","27.12.40.0","230614RT","5901988120382","OE - Couvercle avant perforé L400, 3M / 250","OE - Perforated Front cover W400, 3M / 250","OE- TAPA FRONTAL VENTILADA W400, 3M (H 150MM)","OE - Perforált első burkolat W400, 3M / 250"]
["12039","OE - Osłona czołowa przeźroczysta W400, 3M / 250",166.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12039","SZT","85389099","27.12.40.0","230614RT","5901988120399","OE - Couvercle transparent L400, 3M / 250","OE - Transparent Front cover W400, 3M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 3M ","OE - Átlátszó előlap W400, 3M / 250"]
["12040","OE - Osłona czołowa pełna W400, 4M / 250",47.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12040","SZT","85389099","27.12.40.0","230614RT","5901988120405","OE - Couverture avant complète L400, 4M / 250","OE - Plain Front cover W400, 4M / 250","OE- TAPA CIEGA W400, 4M (H 200MM)","OE - Teljes első burkolat W400, 4M / 250"]
["12042","OE - Osłona czołowa wgłębiona, W400, 4M / 250",166.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","12042","SZT","85389099",null,"230614RT","5901988120429","OE - Ecran facial encastré, L400, 4M / 250","OE - Recessed front hood, W400, 4M / 250","OE- TAPA FRONTAL EMPOTRADA W400, 4M / 250","OE - Süllyesztett előlap, W400, 4M / 250"]
["12045","OE - Osłona aparatury modułowej W400, 4M / 250, 11 mod",49.4,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12045","SZT","85389099","27.12.40.0","230616RT","5901988120450","OE - Couverture d'appareil modulaire L400, 4M / 250, 11 mod","OE - Modular equipment cover W400, 4M / 250, 11 mod","OE-TAPA MODULAR W400, 4M (H 200MM) 11 MOD","OE - W400 moduláris berendezés burkolat, 4M / 250, 11 mod"]
["12048","OE - Osłona czołowa perforowana W400, 4M / 250",57.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12048","SZT","85389099","27.12.40.0","230616RT","5901988120481","OE - Couvercle avant perforé L400, 4M / 250","OE - Perforated Front cover W400, 4M / 250","OE- TAPA FRONTAL VENTILADA W400, 4M (H 200MM)","OE - Perforált előlap W400, 4M / 250"]
["12049","OE - Osłona czołowa przeźroczysta W400, 4M / 250",176,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12049","SZT","85389099","27.12.40.0","230616RT","5901988120498","OE - Couvercle transparent L400, 4M / 250","OE - Transparent Front cover W400, 4M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 4M ","OE - Átlátszó előlap W400, 4M / 250"]
["12050","OE - Osłona czołowa pełna W400, 5M / 250",51,"1-ZE-01",null,null,"01_PLAIN_COVERS","12050","SZT","85389099","27.12.40.0","230616RT","5901988120504","OE - Couverture avant complète L400, 5M / 250","OE - Plain Front cover W400, 5M / 250","OE- TAPA CIEGA W400, 5M (H 250MM)","OE - Teljes első burkolat W400, 5M / 250"]
["12052","OE - Osłona czołowa wgłębiona, W400, 5M / 250",169.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12052","SZT","85389099",null,"230616RT","5901988120528","OE - Ecran facial encastré, L400, 5M / 250","OE - Recessed front hood, W400, 5M / 250","OE- TAPA FRONTAL EMPOTRADA W400, 5M / 250","OE - Süllyesztett előlap, W400, 5M / 250"]
["12055","OE - Osłona aparatury modułowej W400, 5M / 250, 11 mod",56.3,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12055","SZT","85389099","27.12.40.0","230616RT","5901988120559","OE - Couverture d'appareil modulaire L400, 5M / 250, 11 mod","OE - Modular equipment cover W400, 5M / 250, 11 mod","OE-TAPA MODULAR W400, 5M (H 250MM) 11 MOD","OE - W400 moduláris berendezés burkolat, 5M / 250, 11 mod"]
["12058","OE - Osłona czołowa perforowana W400, 5M / 250",61.4,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12058","SZT","85389099",null,"230616RT","5901988120580","OE - Couvercle avant perforé L400, 5M / 250","OE - Perforated Front cover W400, 5M / 250","OE- TAPA FRONTAL VENTILADA W400, 5M (H 250MM)","OE - Perforált előlap W400, 5M / 250"]
["12059","OE - Osłona czołowa przeźroczysta W400, 6M / 250",188.6,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12059","SZT","85389099","27.12.40.0","230616RT","5901988120597","OE - Couverture transparente L400, 6M / 250","OE - Transparent Front cover W400, 6M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 6M ","OE - Átlátszó előlap W400, 6M / 250"]
["12060","OE - Osłona czołowa pełna W400, 6M / 250",52.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12060","SZT","85389099","27.12.40.0","230616RT","5901988120603","OE - Couverture avant complète L400, 6M / 250","OE - Plain Front cover W400, 6M / 250","OE- TAPA CIEGA W400, 6M (H 300MM)","OE - Teljes első burkolat W400, 6M / 250"]
["12062","OE - Osłona czołowa wgłębiona, W400, 6M / 250",172.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","12062","SZT","85389099",null,"230616RT","5901988120627","OE - Ecran facial encastré, L400, 6M / 250","OE - Recessed front hood, W400, 6M / 250","OE- TAPA FRONTAL EMPOTRADA W400, 6M / 250","OE - Süllyesztett előlap, W400, 6M / 250"]
["12068","OE - Osłona czołowa perforowana W400, 6M / 250",63.6,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12068","SZT","85389099",null,"230616RT","5901988120689","OE - Couvercle avant perforé L400, 6M / 250","OE - Perforated Front cover W400, 6M / 250","OE- TAPA FRONTAL VENTILADA W400, 6M (H 300MM)","OE - Perforált előlap W400, 6M / 250"]
["12069","OE - Osłona czołowa przeźroczysta W400, 8M / 250",201.3,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12069","SZT","85389099","27.12.40.0","230619RT","5901988120696","OE - Couverture transparente L400, 8M / 250","OE - Transparent Front cover W400, 8M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 8M ","OE - Átlátszó előlap W400, 8M / 250"]
["12070","OE - Osłona czołowa pełna W400, 7M / 250",75.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","12070","SZT","85389099","27.12.40.0","230616RT","5901988120702","OE - Couverture avant complète L400, 7M / 250","OE - Plain Front cover W400, 7M / 250","OE- TAPA CIEGA W400, 7M (H 350MM)","OE - Teljes első burkolat W400, 7M / 250"]
["12079","OE - Osłona czołowa przeźroczysta W400, 9M / 250",210.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12079","SZT","85389099",null,"230616RT","5901988120795","OE - Couverture transparente L400, 9M / 250","OE - Transparent Front cover W400, 9M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 9M ","OE - Átlátszó előlap W400, 9M / 250"]
["12080","OE - Osłona czołowa pełna W400, 8M / 250",81.400000000000006,"1-ZE-01",null,null,"01_PLAIN_COVERS","12080","SZT","85389099","27.12.40.0","230616RT","5901988120801","OE - Couverture avant complète L400, 8M / 250","OE - Plain Front cover W400, 8M / 250","OE- TAPA CIEGA W400, 8M (H 400MM)","OE - Teljes első burkolat W400, 8M / 250"]
["12089","OE - Osłona czołowa przeźroczysta W400, 10M / 250",217.4,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12089","SZT","85389099","27.12.40.0","230616RT","5901988120894","OE - Couverture transparente L400, 10M / 250","OE - Transparent Front cover W400, 10M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 10M ","OE - Átlátszó előlap W400, 10M / 250"]
["12090","OE - Osłona czołowa pełna W400, 9M / 250",85,"1-ZE-01",null,null,"01_PLAIN_COVERS","12090","SZT","85389099","27.12.40.0","230616RT","5901988120900","OE - Couverture avant complète L400, 9M / 250","OE - Plain Front cover W400, 9M / 250","OE- TAPA CIEGA W400, 9M (H 450MM)","OE - Teljes első burkolat W400, 9M / 250"]
["12091","OE - Osłona czołowa pełna W400, 10M / 250",87.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","12091","SZT","85389099","27.12.40.0","230616RT","5901988120917","OE - Couverture avant complète L400, 10M / 250","OE - Plain Front cover W400, 10M / 250","OE- TAPA CIEGA W400, 10M (H 500MM)","OE - Teljes első burkolat W400, 10M / 250"]
["12092","OE - Osłona czołowa pełna W400, 11M / 250",90.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12092","SZT","85389099",null,"230616RT","5901988120924","OE - Couverture avant complète L400, 11M / 250","OE - Plain Front cover W400, 11M / 250","OE- TAPA CIEGA W400, 11M (H 550MM)","OE - Teljes első burkolat W400, 11M / 250"]
["12093","OE - Osłona czołowa pełna W400, 12M / 250",94.6,"1-ZE-01",null,null,"01_PLAIN_COVERS","12093","SZT","85389099","27.12.40.0","230619RT","5901988120931","OE - Couverture avant complète L400, 12M / 250","OE - Plain Front cover W400, 12M / 250","OE- TAPA CIEGA W400, 12M (H 600MM)","OE - Teljes első burkolat W400, 12M / 250"]
["12099","OE - Osłona czołowa przeźroczysta W400, 12M / 250",227.7,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12099","SZT","85389099",null,"230619RT","5901988120993","OE - Couverture transparente L400, 12M / 250","OE - Transparent Front cover W400, 12M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 12M ","OE - Átlátszó előlap W400, 12M / 250"]
["12231","OM - Osłona czołowa pełna W300, 1M / 200",35,"1-ZE-01",null,null,"01_PLAIN_COVERS","12231","SZT",null,null,"230626RT","5901988122317","OM - Couverture avant complète L300, 1M / 200","OM - Plain Front cover W300, 1M / 200","OM- TAPA CIEGA W300, 1M (H 50MM)","OM - Teljes előlap W300, 1M / 200"]
["12232","OM - Osłona czołowa pełna W300, 2M / 200",38.6,"1-ZE-01",null,null,"01_PLAIN_COVERS","12232","SZT","85389099",null,"230626RT","5901988122324","OM - Couverture avant complète L300, 2M / 200","OM - Plain Front cover W300, 2M / 200","OM- TAPA CIEGA W300, 2M (H 100MM)","OM - Teljes előlap W300, 2M / 200"]
["12233","OM - Osłona czołowa pełna W300, 3M / 200",42.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","12233","SZT","85389099",null,"230626RT","5901988122331","OM - Couverture avant complète L300, 3M / 200","OM - Plain Front cover W300, 3M / 200","OM- TAPA CIEGA W300, 3M (H 150MM)","OM - Teljes előlap W300, 3M / 200"]
["12234","OM - Osłona czołowa pełna W300, 4M / 200",45.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12234","SZT",null,null,"230626RT","5901988122348","OM - Couverture avant complète L300, 4M / 200","OM - Plain Front cover W300, 4M / 200","OM- TAPA CIEGA W300, 4M (H 200MM)","OM - Teljes előlap W300, 4M / 200"]
["12235","OM - Osłona czołowa pełna W300, 5M / 200",47.3,"1-ZE-01",null,null,"01_PLAIN_COVERS","12235","SZT",null,null,"230626RT","5901988122355","OM - Couverture avant complète L300, 5M / 200","OM - Plain Front cover W300, 5M / 200","OM- TAPA CIEGA W300, 5M (H 250MM)","OM - Teljes előlap W300, 5M / 200"]
["12236","OM - Osłona czołowa pełna W300, 6M / 200",49.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","12236","SZT",null,null,"230626RT","5901988122362","OM - Couverture avant complète L300, 6M / 200","OM - Plain Front cover W300, 6M / 200","OM- TAPA CIEGA W300, 6M (H 300MM)","OM - Teljes előlap W300, 6M / 200"]
["12237","OM - Osłona czołowa pełna W300, 7M / 200",73.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","12237","SZT",null,null,"230626RT","5901988122379","OM - Couverture avant complète L300, 7M / 200","OM - Plain Front cover W300, 7M / 200","OM- TAPA CIEGA W300, 7M (H 350MM)","OM - Teljes előlap W300, 7M / 200"]
["12238","OM - Osłona czołowa pełna W300, 8M / 200",78.900000000000006,"1-ZE-01",null,null,"01_PLAIN_COVERS","12238","SZT",null,null,"230626RT","5901988122386","OM - Couverture avant complète L300, 8M / 200","OM - Plain Front cover W300, 8M / 200","OM- TAPA CIEGA W300, 8M (H 400MM)","OM - Teljes előlap W300, 8M / 200"]
["12239","OM - Osłona czołowa pełna W300, 9M / 200",84.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12239","SZT",null,null,"230626RT","5901988122393","OM - Couverture avant complète L300, 9M / 200","OM - Plain Front cover W300, 9M / 200","OM- TAPA CIEGA W300, 9M (H 450MM)","OM - Teljes előlap W300, 9M / 200"]
["12240","OM - Osłona czołowa pełna W300, 10M / 200",85.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12240","SZT","85389099",null,"230626RT","5901988122409","OM - Couverture avant complète L300, 10M / 200","OM - Plain Front cover W300, 10M / 200","OM- TAPA CIEGA W300, 10M (H 500MM)","OM - Teljes előlap W300, 10M / 200"]
["12241","OM - Osłona czołowa pełna W300, 11M / 200",87.6,"1-ZE-01",null,null,"01_PLAIN_COVERS","12241","SZT",null,null,"230626RT","5901988122416","OM - Couverture avant complète L300, 11M / 200","OM - Plain Front cover W300, 11M / 200","OM- TAPA CIEGA W300, 11M (H 550MM)","OM - Teljes előlap W300, 11M / 200"]
["12242","OM - Osłona czołowa pełna W300, 12M / 200",89.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12242","SZT",null,null,"230626RT","5901988122423","OM - Couverture avant complète L300, 12M / 200","OM - Plain Front cover W300, 12M / 200","OM- TAPA CIEGA W300, 12M (H 600MM)","OM - Teljes előlap W300, 12M / 200"]
["12250","OM - Osłona aparatury modułowej W300, 2M / 200, 8 mod",41,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12250","SZT",null,null,"230626RT","5901988122508","OM - Couverture d'appareil modulaire L300, 2M / 150, 8 mod","OM - Modular equipment cover W300, 2M / 200, 8 mod","OM-TAPA MODULAR W300, 2M (H 100MM) 8 MOD","OM - fedél W300 moduláris berendezéshez, 2M / 200, 8 modul"]
["12252","OM - Osłona aparatury modułowej W300, 3M / 200, 8 mod",44.7,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12252","SZT",null,null,"230626RT","5901988122522","OM - Couverture d'appareil modulaire L300, 3M / 150, 8 mod","OM - Modular equipment cover W300, 3M / 200, 8 mod","OM-TAPA MODULAR W300, 3M (H 150MM) 8 MOD","OM - fedél W300 moduláris berendezéshez, 3M / 200, 8 modul"]
["12253","OM - Osłona aparatury modułowej W300, 4M / 200, 8 mod",46.4,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12253","SZT",null,null,"230626RT","5901988122539","OM - Couverture d'appareil modulaire L300, 4M / 150, 8 mod","OM - Modular equipment cover W300, 4M / 200, 8 mod","OM-TAPA MODULAR W300, 4M (H 200MM) 8 MOD","OM - Moduláris berendezés burkolata W300, 4M / 200, 8 mod"]
["12254","OM - Osłona aparatury modułowej W300, 5M / 200, 8 mod",48.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12254","SZT",null,null,"230626RT","5901988122546","OM - Couverture d'appareil modulaire L300, 5M / 150, 8 mod","OM - Modular equipment cover W300, 5M / 200, 8 mod","OM-TAPA MODULAR W300, 5M (H 250MM) 8 MOD","OM - W300 moduláris berendezés burkolat, 5M / 200, 8 mod"]
["12510","OE - Osłona czołowa pełna W450, 1M / 300",39.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12510","SZT","85389099","27.12.40.0","230619RT","5901988125103","OE - Couverture avant complète L450, 1M / 300","OE - Plain Front cover W450, 1M / 300","OM-TAPA CIEGA W450, 1M (H 50MM)","OE - Teljes első burkolat W450, 1M / 300"]
["12520","OE - Osłona czołowa pełna W450, 2M / 300",41.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12520","SZT","85389099","27.90.20.0","230619RT","5901988125202","OE - Couverture avant complète L450, 2M / 300","OE - Plain Front cover W450, 2M / 300","OM-TAPA CIEGA W450, 2M (H 100MM)","OE - Teljes első burkolat W450, 2M / 300"]
["12525","OE - Osłona aparatury modułowej W450, 2M / 300, 14 mod",42.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12525","SZT","85389099",null,"230619RT","5901988125257","OE - Couverture d'appareil modulaire L450, 2M / 300, 14 mod","OE - Modular equipment cover W450, 2M / 300, 14 mod","OM-TAPA MODULAR W450, 2M (H 100MM) 14 MOD","OE - W450 moduláris berendezés burkolat, 2M / 300, 14 mod"]
["12528","OE - Osłona czołowa perforowana W450, 2M / 300",52.9,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12528","SZT","85389099",null,"230619RT","5901988125288","OE - Panneau avant perforé L450, 2M / 300","OE - Perforated Front cover W450, 2M / 300","OE- TAPA FRONTAL VENTILADA W450, 2M (H 100MM)","OE - Perforált előlap W450, 2M / 300"]
["12530","OE - Osłona czołowa pełna W450, 3M / 300",43.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","12530","SZT","85389099","27.12.40.0","230619RT","5901988125301","OE - Couverture avant complète L450, 3M / 300","OE - Plain Front cover W450, 3M / 300","OM-TAPA CIEGA W450, 3M (H 150MM)","OE - Teljes első burkolat W450, 3M / 300"]
["12531","OE - Osłona czołowa W450, 3M / 300, otw. 92x92",45.8,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12531","SZT","85389099",null,"230619RT","5901988125318","OE - Cache avant complet L450, 3M / 300, ouvert 92x92","OE - Front cover W450, 3M / 300, open. 92x92","OE- TAPA TROQ. W450, 3M/300, ABIERTA. 92X92","OE - Első burkolat W450, 3M / 300, nyitott 92x92"]
["12532","OE - Osłona czołowa wgłębiona, W450, 3M / 300",174.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12532","SZT","85389099",null,"230619RT","5901988125325","OE - Couvercle avant profond de, L450,  3M / 300","OE - Recessed front hood, W450, 3M / 300","OE- TAPA FRONTAL EMPOTRADA W450, 3M / 300","OE - Süllyesztett előlap, W450, 3M / 300"]
["12535","OE - Osłona aparatury modułowej W450, 3M / 300, 14 mod",43.9,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12535","SZT","85389099","27.12.40.0","230619RT","5901988125356","OE - Couverture d'appareil modulaire L450, 3M / 300, 14 mod","OE - Modular equipment cover W450, 3M / 300, 14 mod","OM-TAPA MODULAR W450, 3M (H 150MM) 14 MOD","OE - W450 moduláris berendezés burkolat, 3M / 300, 14 mod"]
["12538","OE - Osłona czołowa perforowana W450, 3M / 300",57.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12538","SZT","85389099",null,"230619RT","5901988125387","OE - Panneau avant perforé L450, 3M / 300","OE - Perforated Front cover W450, 3M / 300","OE- TAPA FRONTAL VENTILADA W450, 3M (H 150MM)","OE - Perforált előlap W450, 3M / 300"]
["12539","OE - Osłona czołowa przeźroczysta W450, 3M / 300",176,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12539","SZT","85389099",null,"230619RT","5901988125394","OE - Couvercle avant, transparent L450, 3M / 300","OE - Transparent Front cover W450, 3M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 3M ","OE - Átlátszó előlap W450, 3M / 300"]
["12540","OE - Osłona czołowa pełna W450, 4M / 300",47.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12540","SZT","85389099","27.12.40.0","230619RT","5901988125400","OE - Couverture avant complète L450, 4M / 300","OE - Plain Front cover W450, 4M / 300","OM-TAPA CIEGA W450, 4M (H 200MM)","OE - Teljes első burkolat W450, 4M / 300"]
["12541","OE - Osłona czołowa W450, 4M / 300, otw. 92x92",50.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12541","SZT","85389099",null,"230619RT","5901988125417","OE - Cache avant complet L450, 4M / 300, ouvert 92x92","OE - Front cover W450, 4M / 300, open. 92x92","OE- TAPA FRONTAL W450, 4M/300, CON AGUJERO 92X92","OE - Első burkolat W450, 4M / 300, nyitható 92x92"]
["12542","OE - Osłona czołowa wgłębiona, W450, 4M / 300",178.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12542","SZT","85389099",null,"230619RT","5901988125424","OE - Ecran facial encastré, L450, 4M / 300","OE - Recessed front hood, W450, 4M / 300","OE- EMPOTRADA, W450, 4M / 300","OE - Süllyesztett előlap, W450, 4M / 300"]
["12545","OE - Osłona aparatury modułowej W450, 4M / 300, 14 mod",48.4,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12545","SZT","85389099","27.12.40.0","230619RT","5901988125455","OE - Couverture d'appareil modulaire L450, 4M / 300, 14 mod","OE - Modular equipment cover W450, 4M / 300, 14 mod","OM-TAPA MODULAR W450, 4M (H 200MM) 14 MOD","OE - Moduláris berendezések burkolata W450, 4M / 300, 14 mod"]
["12548","OE - Osłona czołowa perforowana W450, 4M / 300",61.4,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12548","SZT","85389099",null,"230619RT","5901988125486","OE - Panneau avant perforé L450, 4M / 300","OE - Perforated Front cover W450, 4M / 300","OE- TAPA FRONTAL VENTILADA W450, 4M (H 200MM)","OE - Perforált előlap W450, 4M / 300"]
["12549","OE - Osłona czołowa przeźroczysta W450, 4M / 300",185.2,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12549","SZT","85389099",null,"230619RT","5901988125493","OE - Couverture, L450, 4M / 300","OE - Transparent Front cover W450, 4M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 4M ","OE - Átlátszó előlap W450, 4M / 300"]
["12550","OE - Osłona czołowa pełna W450, 5M / 300",52.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12550","SZT","85389099","27.12.40.0","230619RT","5901988125509","OE - Couverture avant complète L450, 5M / 300","OE - Plain Front cover W450, 5M / 300","OM-TAPA CIEGA W450, 5M (H 250MM)","OE - Teljes első burkolat W450, 5M / 300"]
["12551","OE - Osłona czołowa W450, 5M / 300, otw. 92x92",55.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12551","SZT","85389099",null,"230619RT","5901988125516","OE - Cache avant complet L450, 5M / 300, ouvert 92x92","OE - Front cover W450, 5M / 300, open. 92x92","OE- TAPA TROQ. W450, 5M/300, ABIERTA. 92X92","OE - Első burkolat W450, 5M / 300, nyitható 92x92"]
["12552","OE - Osłona czołowa wgłębiona, W450, 5M / 300",181.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12552","SZT","85389099",null,"230619RT","5901988125523","OE - Ecran facial encastré, L450, 5M / 300","OE - Recessed front hood, W450, 5M / 300","OE- TAPA FRONTAL EMPOTRADA W450, 5M / 300","OE - Süllyesztett előlap, W450, 5M / 300"]
["12555","OE - Osłona aparatury modułowej W450, 5M / 300, 14 mod",59.4,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12555","SZT","85389099","27.12.40.0","230619RT","5901988125554","OE - Couverture d'appareil modulaire L450, 5M / 300, 14 mod","OE - Modular equipment cover W450, 5M / 300, 14 mod","OM-TAPA MODULAR W450, 5M (H 250MM) 14 MOD","OE - W450 moduláris berendezés burkolat, 5M / 300, 14 mod"]
["12558","OE - Osłona czołowa perforowana W450, 5M / 300",63.6,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12558","SZT","85389099",null,"230619RT","5901988125585","OE - Panneau avant perforé L450, 5M / 300","OE - Perforated Front cover W450, 5M / 300","OE- TAPA FRONTAL VENTILADA W450, 5M (H 250MM)","OE - Perforált előlap W450, 5M / 300"]
["12559","OE - Osłona czołowa przeźroczysta W450, 6M / 300",197.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12559","SZT","85389099",null,"230619RT","5901988125592","OE - Couverture, L450, 6M / 300","OE - Transparent Front cover W450, 6M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 6M ","OE - Átlátszó előlap W450, 6M / 300"]
["12560","OE - Osłona czołowa pełna W450, 6M / 300",54.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12560","SZT","85389099","27.12.40.0","230619RT","5901988125608","OE - Couverture avant complète L450, 6M / 300","OE - Plain Front cover W450, 6M / 300","OM-TAPA CIEGA W450, 6M (H 300MM)","OE - Teljes első burkolat W450, 6M / 300"]
["12562","OE - Osłona czołowa wgłębiona, W450, 6M / 300",185.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12562","SZT","85389099",null,"230619RT","5901988125622","OE - Ecran facial encastré, L450, 6M / 300","OE - Recessed Front cover, W450, 6M / 300","OE- TAPA FRONTAL EMPOTRADA W450, 6M / 300","OE - Süllyesztett előlap, W450, 6M / 300"]
["12568","OE - Osłona czołowa perforowana W450, 6M / 300",67.8,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12568","SZT","85389099",null,"230619RT","5901988125684","OE - Panneau avant perforé L450, 6M / 300","OE - Perforated Front cover W450, 6M / 300","OE- TAPA FRONTAL VENTILADA W450, 6M (H 300MM)","OE - Perforált előlap W450, 6M / 300"]
["12569","OE - Osłona czołowa przeźroczysta W450, 8M / 300",215.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12569","SZT","85389099",null,"230619RT","5901988125691","OE - Couverture, L450, 8M / 300","OE - Transparent Front cover W450, 8M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 8M ","OE - Átlátszó előlap W450, 8M / 300"]
["12570","OE - Osłona czołowa pełna W450, 7M / 300",81.400000000000006,"1-ZE-01",null,null,"01_PLAIN_COVERS","12570","SZT","85389099","27.12.40.0","230619RT","5901988125707","OE - Couverture avant complète L450, 7M / 300","OE - Plain Front cover W450, 7M / 300","OM-TAPA CIEGA W450, 7M (H 350MM)","OE - Teljes első burkolat W450, 7M / 300"]
["12579","OE - Osłona czołowa przeźroczysta W450, 9M / 300",220.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12579","SZT","85389099",null,"230619RT","5901988125790","OE - Couverture, L450, 9M / 300","OE - Transparent Front cover W450, 9M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 9M ","OE - Átlátszó előlap W450, 9M / 300"]
["12580","OE - Osłona czołowa pełna W450, 8M / 300",85,"1-ZE-01",null,null,"01_PLAIN_COVERS","12580","SZT","85389099","27.12.40.0","230619RT","5901988125806","OE - Couverture avant complète L450, 8M / 300","OE - Plain Front cover W450, 8M / 300","OM-TAPA CIEGA W450, 8M (H 400MM)","OE - Teljes első burkolat W450, 8M / 300"]
["12589","OE - Osłona czołowa przeźroczysta W450, 10M / 300",227.7,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12589","SZT","85389099",null,"230619RT","5901988125899","OE - Couverture, L450, 10M / 300","OE - Transparent Front cover W450, 10M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 10M ","OE - Átlátszó előlap W450, 10M / 300"]
["12590","OE - Osłona czołowa pełna W450, 9M / 300",89,"1-ZE-01",null,null,"01_PLAIN_COVERS","12590","SZT","85389099","27.12.40.0","230619RT","5901988125905","OE - Couverture avant complète L450, 9M / 300","OE - Plain Front cover W450, 9M / 300","OM-TAPA CIEGA W450, 9M (H 450MM)","OE - Teljes első burkolat W450, 9M / 300"]
["12591","OE - Osłona czołowa pełna W450, 10M / 300",90.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12591","SZT","85389099","27.12.40.0","230619RT","5901988125912","OE - Couverture avant complète L450, 10M / 300","OE - Plain Front cover W450, 10M / 300","OM-TAPA CIEGA W450, 10M (H 500MM)","OE - Teljes első burkolat W450, 10M / 300"]
["12592","OE - Osłona czołowa pełna W450, 11M / 300",96.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12592","SZT","85389099","27.12.40.0","230619RT","5901988125929","OE - Couverture avant complète L450, 11M / 300","OE - Plain Front cover W450, 11M / 300","OM-TAPA CIEGA W450, 11M (H 550MM)","OE - Teljes első burkolat W450, 11M / 300"]
["12593","OE - Osłona czołowa pełna W450, 12M / 300",100.3,"1-ZE-01",null,null,"01_PLAIN_COVERS","12593","SZT","85389099","27.12.40.0","230619RT","5901988125936","OE - Couverture avant complète L450, 12M / 300","OE - Plain Front cover W450, 12M / 300","OM-TAPA CIEGA W450, 12M (H 600MM)","OE - Teljes első burkolat W450, 12M / 300"]
["12595","OM-VSD - Osłona aparatury modułowej, układ pionowy W450, 9M / 300, 1x24 mod",119.6,"1-ZE-01",null,null,"OM_VSD_PLATES","12595","SZT","85389099",null,"230619RT","5901988125950","OM-VSD - Couvercle modulaire, vertical L450, 9M / 300, 1x24 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W450, 9M / 300, 1x24 mod","OM-VSD- TAPA MODULAR VERTIC. W450, 9M/300, 1X24 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W450, 9M / 300, 1x24 mod"]
["12596","OM-VSD - Osłona aparatury modułowej, układ pionowy W450, 10M / 300, 1x26 mod",120.8,"1-ZE-01",null,null,"OM_VSD_PLATES","12596","SZT","85389099",null,"230619RT","5901988125967","OM-VSD - Couvercle modulaire pour appareils, vertical L450, 10M / 300, 1x26 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W450, 10M / 300, 1x26 mod","OM-VSD- TAPA MODULAR VERTIC. W450, 10M / 300, 1X26 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W450, 10M / 300, 1x26 mod"]
["12597","OM-VSD - Osłona aparatury modułowej, układ pionowy W450, 11M / 300, 1x29 mod",126.5,"1-ZE-01",null,null,"OM_VSD_PLATES","12597","SZT","85389099",null,"230619RT","5901988125974","OM-VSD - Couvercle modulaire, vertical L450, 11M / 300, 1x29 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W450, 11M / 300, 1x29 mod","OM-VSD- TAPA MODULAR VERTIC. W450, 11M / 300, 1X29 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W450, 11M / 300, 1x29 mod"]
["12598","OM-VSD - Osłona aparatury modułowej, układ pionowy W450, 12M / 300, 1x32 mod",131.1,"1-ZE-01",null,null,"OM_VSD_PLATES","12598","SZT","85389099",null,"230619RT","5901988125981","OM-VSD - Couvercle modulaire, vertical L450, 12M / 300, 1x32 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W450, 12M / 300, 1x32 mod","OM-VSD- TAPA MODULAR VERTIC. W450, 12M/300, 1X32 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W450, 12M / 300, 1x32 mod"]
["12599","OE - Osłona czołowa przeźroczysta W450, 12M / 300",241.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12599","SZT","85389099",null,"230619RT","5901988125998","OE - Couvercle avant, transparent L450, 12M / 300","OE - Transparent Front cover W450, 12M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 12M ","OE - Átlátszó előlap W450, 12M / 300"]
["12710","OE - Osłona czołowa pełna W650, 1M / 500",40.299999999999997,"1-ZE-01",null,null,"01_PLAIN_COVERS","12710","SZT","85389099","27.12.40.0","230612RT","5901988127107","OE - Couverture avant complète L650, 1M / 500","OE - Plain Front cover W650, 1M / 500","OE- TAPA CIEGA W650, 1M (H 50MM) ","OE - Teljes első burkolat W650, 1M / 500"]
["12718","OE - Osłona czołowa perforowana W650, 1M / 500",52.9,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12718","SZT","85389099",null,"230612RT","5901988127183","OE - Couvercle avant perforé L650, 1M / 500","OE - Perforated Front cover W650, 1M / 500","OE- TAPA FRONTAL VENTILADA W650, 1M (H 50MM) ","OE - Perforált előlap W650, 1M / 500"]
["12720","OE - Osłona czołowa pełna W650, 2M / 500",40.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12720","SZT","85389099","27.12.40.0","230612RT","5901988127206","OE - Couverture avant complète L650, 2M / 500","OE - Plain Front cover W650, 2M / 500","OE- TAPA CIEGA W650, 2M (H 100MM) ","OE - Teljes első burkolat W650, 2M / 500"]
["12725","OE - Osłona aparatury modułowej W650, 2M / 500, 25 mod",44.5,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12725","SZT","85389099","27.12.40.0","230605RT","5901988127251","OE - Couverture d'appareil modulaire L650, 2M / 500, 25 mod","OE - Modular equipment cover W650, 2M / 500, 25 mod","OE- TAPA MODULAR W650, 2M (H 100MM) 25 MOD","OE - W650 moduláris berendezés burkolat, 2M / 500, 25 mod"]
["12726","OE - Osłona aparatury modułowej W650, 2.5M / 500, 25 mod",49.5,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12726","SZT","85389099",null,"230612RT","5901988127268","OE - Couverture d'appareil modulaire L650, 2,5M / 500, 25 mod","OE - Modular equipment cover W650, 2.5M / 500, 25 mod","OE- TAPA MODULAR W650, 2,5M (H 125MM) 25 MOD","OE - W650 moduláris berendezés burkolat, 2,5M / 500, 25 mod"]
["12728","OE - Osłona czołowa perforowana W650, 2M / 500",57.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12728","SZT","85389099","27.12.40.0","230612RT","5901988127282","OE - Couvercle avant perforé L650, 2M / 500","OE - Perforated Front cover W650, 2M / 500","OE- TAPA FRONTAL VENTILADA W650, 2M (H 100MM) ","OE -Perforált előlap W650, 2M / 500"]
["12730","OE - Osłona czołowa pełna W650, 3M / 500",40.799999999999997,"1-ZE-01",null,null,"01_PLAIN_COVERS","12730","SZT","85389099","27.12.40.0","230612RT","5901988127305","OE - Couverture avant complète L650, 3M / 500","OE - Plain Front cover W650, 3M / 500","OE- TAPA CIEGA W650, 3M (H 150MM) ","OE - Teljes első burkolat W650, 3M / 500"]
["12731","OE - Osłona czołowa W650, 3M / 500, otw. 92x92",60,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12731","SZT","85389099","27.12.40.0","230612RT","5901988127312","OE - Cache avant complet L650, 3M / 500, ouvert 92x92","OE - W650, 3M / 500 Front cover, hole 92x92","OE- TAPA CIEGA W650, 3M (H 150MM) CON AGUJERO 92X92","OE - Első burkolat W650, 3M / 500, nyitott 92x92"]
["12732","OE - Osłona czołowa wgłębiona, W650, 3M / 500",202.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12732","SZT","85389099",null,"230612RT","5901988127329","OE - Couvercle avant profond de, L650,  3M / 500","OE - Recessed front hood, W650, 3M / 500","OE- TAPA FRONTAL EMPOTRADA W650, 3M / 500","OE - Süllyesztett előlap, W650, 3M / 500"]
["12735","OE - Osłona aparatury modułowej W650, 3M / 500, 25 mod",45.7,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12735","SZT","85389099","27.12.40.0","230605RT","5901988127350","OE - Couverture d'appareil modulaire L650, 3M / 500, 25 mod","OE - Modular equipment cover W650, 3M / 500, 25 mod","OE- TAPA MODULAR W650, 3M (H 150MM) 25 MOD","OE - W650 moduláris berendezés burkolat, 3M / 500, 25 mod"]
["12736","OE - Osłona aparatury modułowej, otwór przesunięty W650, 3.5M / 500, 25 mod",52.6,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12736","SZT","85389099","27.12.40.0","230612RT","5901988127367","OE - Couverture d'appareil modulaire L650, 3.5M / 500, 25 mod","OE - Modular apparatus cover, offset hole W650, 3.5M / 500, 25 mod","OE- TAPA MODULAR ORIFICIO DESPLAZADO W650, 3.5M / 500, 25 MOD","OE - Moduláris berendezésfedél, eltolt nyitás W650, 3,5M / 500, 25 mod"]
["12738","OE - Osłona czołowa perforowana W650, 3M / 500",65.599999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12738","SZT","85389099","27.12.40.0","230612RT","5901988127381","OE - Panneau avant perforé L650, 3M / 500","OE - Perforated Front cover W650, 3M / 500","OE- TAPA FRONTAL VENTILADA W650, 3M (H 150MM) ","OE - Perforált előlap W650, 3M / 500"]
["12739","OE - Osłona czołowa przeźroczysta W650, 3M / 500",197.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12739","SZT","85389099",null,"230612RT","5901988127398","OE - Couverture avant, L650, 3M / 500","OE - Transparent Front cover W650, 3M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 3M ","OE - Átlátszó előlap W650, 3M / 500"]
["12740","OE - Osłona czołowa pełna W650, 4M / 500",51.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","12740","SZT","85389099","27.12.40.0","230612RT","5901988127404","OE - Couverture avant complète L650, 4M / 500","OE - Plain Front cover W650, 4M / 500","OE- TAPA CIEGA W650, 4M (H 200MM) ","OE - Teljes első burkolat W650, 4M / 500"]
["12741","OE - Osłona czołowa W650, 4M / 500, otw. 92x92",59.5,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12741","SZT","85389099","27.12.40.0","230612RT","5901988127411","OE - Cache avant complet L650, 4M / 500, ouvert 92x92","OE - W650, 4M / 500 Front cover, open. 92x92","OE- TAPA CIEGA W650, 4M (H 200MM) CON AGUJERO 92X92","OE - Első burkolat W650, 4M / 500, nyitható 92x92"]
["12742","OE - Osłona czołowa wgłębiona, W650, 4M / 500",209,"1-ZE-01",null,null,"01_PLAIN_COVERS","12742","SZT","85389099",null,"230612RT","5901988127428","OE - Ecran facial encastré, L650, 4M / 500","OE - Recessed front hood, W650, 4M / 500","OE- TAPA FRONTAL EMPOTRADA W650, 4M / 500","OE - Süllyesztett előlap, W650, 4M / 500"]
["12745","OE - Osłona aparatury modułowej W650, 4M / 500, 25 mod",53.6,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12745","SZT","85389099","27.12.40.0","230605RT","5901988127459","OE - Couverture d'appareil modulaire L650, 4M / 500, 25 mod","OE - Modular equipment cover W650, 4M / 500, 25 mod","OE- TAPA MODULAR W650, 4M (H 200MM) 25 MOD","OE - W650 moduláris berendezés burkolat, 4M / 500, 25 mod"]
["12748","OE - Osłona czołowa perforowana W650, 4M / 500",74.099999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12748","SZT","85389099","27.12.40.0","230612RT","5901988127480","OE - Panneau avant perforé L650, 4M / 500","OE - Perforated Front cover W650, 4M / 500","OE- TAPA FRONTAL VENTILADA W650, 4M (H 200MM) ","OE - Perforált előlap W650, 4M / 500"]
["12749","OE - Osłona czołowa przeźroczysta W650, 4M / 500",215.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12749","SZT","85389099","27.12.40.0","230612RT","5901988127497","OE - Couverture avant, L650, 4M / 500","OE - Transparent Front cover W650, 4M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 4M ","OE - Átlátszó előlap W650, 4M / 500"]
["12750","OE - Osłona czołowa pełna W650, 5M / 500",66.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12750","SZT","85389099","27.12.40.0","230612RT","5901988127503","OE - Couverture avant complète L650, 5M / 500","OE - Plain Front cover W650, 5M / 500","OE- TAPA CIEGA W650, 5M (H 250MM) ","OE - Teljes első burkolat W650, 5M / 500"]
["12751","OE - Osłona czołowa W650, 5M / 500, otw. 92x92",76.7,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12751","SZT","85389099",null,"230612RT","5901988127510","OE - Cache avant complet L650, 5M / 500, ouvert 92x92","OE - Front cover W650, 5M / 500, open. 92x92","OE- TAPA CIEGA W650, 5M (H 250MM) CON AGUJERO 92X92","OE - Első burkolat W650, 5M / 500, nyitható 92x92"]
["12752","OE - Osłona czołowa wgłębiona, W650, 5M / 500",213.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12752","SZT","85389099",null,"230612RT","5901988127527","OE - Ecran facial encastré, L650, 5M / 500","OE - Recessed front hood, W650, 5M / 500","OE- TAPA FRONTAL EMPOTRADA W650, 5M / 500","OE - Süllyesztett előlap, W650, 5M / 500"]
["12755","OE - Osłona aparatury modułowej W650, 5M / 500, 25 mod",68.7,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12755","SZT","85389099","27.12.40.0","230605RT","5901988127558","OE - Couverture d'appareil modulaire L650, 5M / 500, 25 mod","OE - Modular equipment cover W650, 5M / 500, 25 mod","OE- TAPA MODULAR W650, 5M (H 250MM) 25 MOD","OE - W650 moduláris berendezés burkolat, 5M / 500, 25 mod"]
["12758","OE - Osłona czołowa perforowana W650, 5M / 500",80.400000000000006,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12758","SZT","85389099","27.12.40.0","230612RT","5901988127589","OE - Panneau avant perforé L650, 5M / 500","OE - Perforated Front cover W650, 5M / 500","OE- TAPA FRONTAL VENTILADA W650, 5M (H 250MM) ","OE - Perforált előlap W650, 5M / 500"]
["12759","OE - Osłona czołowa przeźroczysta W650, 6M / 500",241.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12759","KPL","85389099",null,"230612RT","5901988127596","OE - Couverture avant, L650, 6M / 500","OE - Transparent Front cover W650, 6M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 6M ","OE - Átlátszó előlap W650, 6M / 500"]
["12760","OE - Osłona czołowa pełna W650, 6M / 500",70.099999999999994,"1-ZE-01",null,null,"01_PLAIN_COVERS","12760","SZT","85389099","27.12.40.0","230612RT","5901988127602","OE - Couverture avant complète L650, 6M / 500","OE - Plain Front cover W650, 6M / 500","OE- TAPA CIEGA W650, 6M (H 300MM) ","OE - Teljes első burkolat W650, 6M / 500"]
["12762","OE - Osłona czołowa wgłębiona, W650, 6M / 500",217.8,"1-ZE-01",null,null,"01_PLAIN_COVERS","12762","SZT","85389099",null,"230612RT","5901988127626","OE - Ecran facial encastré, L650, 6M / 500","OE - Recessed Front cover, W650, 6M / 500","OE- TAPA FRONTAL EMPOTRADA W650, 6M / 500","OE - Süllyesztett előlap, W650, 6M / 500"]
["12768","OE - Osłona czołowa perforowana W650, 6M / 500",84.5,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12768","SZT","85389099","27.12.40.0","230612RT","5901988127688","OE - Panneau avant perforé L650, 6M / 500","OE - Perforated Front cover W650, 6M / 500","OE- TAPA FRONTAL VENTILADA W650, 6M (H 300MM) ","OE - Perforált előlap W650, 6M / 500"]
["12769","OE - Osłona czołowa przeźroczysta W650, 8M / 500",263.39999999999998,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12769","SZT","85389099","27.12.40.0","230612RT","5901988127695","OE - Couverture avant, L650, 8M / 500","OE - Transparent Front cover W650, 8M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 8M ","OE - Átlátszó előlap W650, 8M / 500"]
["12770","OE - Osłona czołowa pełna W650, 7M / 500",96.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12770","SZT","85389099","27.12.40.0","230612RT","5901988127701","OE - Couverture avant complète L650, 7M / 500","OE - Plain Front cover W650, 7M / 500","OE- TAPA CIEGA W650, 7M (H 350MM) ","OE - Teljes első burkolat W650, 7M / 500"]
["12779","OE - Osłona czołowa przeźroczysta W650, 9M / 500",277.2,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12779","SZT","85389099",null,"230612RT","5901988127794","OE - Couverture, L650, 9M / 500","OE - Transparent Front cover W650, 9M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 9M ","OE - Átlátszó előlap W650, 9M / 500"]
["12780","OE - Osłona czołowa pełna W650, 8M / 500",104.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12780","SZT","85389099","27.12.40.0","230612RT","5901988127800","OE - Couverture avant complète L650, 8M / 500","OE - Plain Front cover W650, 8M / 500","OE- TAPA CIEGA W650, 8M (H 400MM) ","OE - Teljes első burkolat W650, 8M / 500"]
["12789","OE - Osłona czołowa przeźroczysta W650, 10M / 500",288.7,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12789","SZT","85389099","27.12.40.0","230612RT","5901988127893","OE - Couverture, L650, 10M / 500","OE - Transparent Front cover W650, 10M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 10M ","OE - Átlátszó előlap W650, 10M / 500"]
["12790","OE - Osłona czołowa pełna W650, 9M / 500",105.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12790","SZT","85389099","27.12.40.0","230612RT","5901988127909","OE - Couverture avant complète L650, 9M / 500","OE - Plain Front cover W650, 9M / 500","OE- TAPA CIEGA W650, 9M (H 450MM) ","OE - Teljes első burkolat W650, 9M / 500"]
["12791","OE - Osłona czołowa pełna W650, 10M / 500",118.8,"1-ZE-01",null,null,"01_PLAIN_COVERS","12791","SZT","85389099","27.12.40.0","230612RT","5901988127916","OE - Couverture avant complète L650, 10M / 500","OE - Plain Front cover W650, 10M / 500","OE- TAPA CIEGA W650, 10M (H 500MM) ","OE - Teljes első burkolat W650, 10M / 500"]
["12792","OE - Osłona czołowa pełna W650, 11M / 500",123.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12792","SZT","85389099","27.12.40.0","230612RT","5901988127923","OE - Couverture avant complète L650, 11M / 500","OE - Plain Front cover W650, 11M / 500","OE- TAPA CIEGA W650, 11M (H 550MM) ","OE - Teljes első burkolat W650, 11M / 500"]
["12793","OE - Osłona czołowa pełna W650, 12M / 500",128.69999999999999,"1-ZE-01",null,null,"01_PLAIN_COVERS","12793","SZT","85389099","27.12.40.0","230612RT","5901988127930","OE - Couverture avant complète L650, 12M / 500","OE - Plain Front cover W650, 12M / 500","OE- TAPA CIEGA W650, 12M (H 600MM) ","OE - Teljes első burkolat W650, 12M / 500"]
["12794","OE - Osłona czołowa pełna W650, 13M / 500",136.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12794","SZT","85389099","27.12.40.0","230612RT","5901988127947","OE - Couverture avant complète L650, 13M / 500","OE - Plain Front cover W650, 13M / 500","OE- TAPA CIEGA W650, 13M (H 650MM) ","OE - Teljes első burkolat W650, 13M / 500"]
["12795","OM-VSD - Osłona aparatury modułowej, układ pionowy W650, 9M / 500, 2x24 mod",144.9,"1-ZE-01",null,null,"OM_VSD_PLATES","12795","SZT","85389099",null,"230612RT","5901988127954","OM-VSD - Couvercle modulaire pour appareils, vertical L650, 9M / 500, modulaire 2x24","OM-VSD - Modular equipment cover, Vertical layout W650, 9M / 500, 2x24 mod","OM-VSD- TAPA MODULAR VERTIC. W650, 9M/500, 2X24 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W650, 9M / 500, 2x24 mod"]
["12796","OM-VSD - Osłona aparatury modułowej, układ pionowy W650, 10M / 500, 2x26 mod",150.69999999999999,"1-ZE-01",null,null,"OM_VSD_PLATES","12796","SZT","85389099",null,"230612RT","5901988127961","OM-VSD - Couvercle modulaire, vertical L650, 10M / 500, 2x26 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W650, 10M / 500, 2x26 mod","OM-VSD- TAPA MODULAR VERTIC. W650, 10M/500, 2X26 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W650, 10M / 500, 2x26 mod"]
["12797","OM-VSD - Osłona aparatury modułowej, układ pionowy W650, 11M / 500, 2x29 mod",155.30000000000001,"1-ZE-01",null,null,"OM_VSD_PLATES","12797","SZT","85389099",null,"230612RT","5901988127978","OM-VSD - Couvercle modulaire, vertical L650, 11M / 500, 2x29 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W650, 11M / 500, 2x29 mod","OM-VSD- TAPA MODULAR VERTIC. W650, 11M/500, 2X29 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W650, 11M / 500, 2x29 mod"]
["12798","OM-VSD - Osłona aparatury modułowej, układ pionowy W650, 12M / 500, 2x32 mod",161,"1-ZE-01",null,null,"OM_VSD_PLATES","12798","SZT","85389099",null,"230612RT","5901988127985","OM-VSD - Couvercle modulaire pour appareils, vertical L650, 12M / 500, modulaire 2x32","OM-VSD - Modular apparatus cover, Vertical layout W650, 12M / 500, 2x32 mod","OM-VSD- TAPA MODULAR VERTIC. W650, 12M/500, 2X32 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W650, 12M / 500, 2x32 mod"]
["12799","OE - Osłona czołowa przeźroczysta W650, 12M / 500",312.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12799","SZT","85389099","27.12.40.0","230612RT","5901988127992","OE - Couverture avant, L650, 12M / 500","OE - Transparent Front cover W650, 12M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 12M ","OE - Átlátszó előlap W650, 12M / 500"]
["12910","OE - Osłona czołowa pełna W850, 1M / 700",47.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","12910","SZT","85389099","27.12.40.0","230619RT","5901988129101","OE - Couverture avant complète L850, 1M / 700","OE - Plain Front cover W850, 1M / 700","OE- TAPA CIEGA W850, 1M (H 50MM)","OE - Teljes első burkolat W850, 1M / 700"]
["12912","OE - Osłona aparatury modułowej W850, 12M / 700, 4x36 mod",178.1,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12912","SZT","85389099",null,"230619RT","5901988129125","OE - Couverture d'appareil modulaire L850, 12M / 700, 4x36 mod","OE - Modular equipment cover W850, 12M / 700, 4x36 mod","OE- TAPA MODULAR W850, 12M/700, 4X36 MOD","OE - fedél moduláris berendezéshez W850, 12M / 700, 4x36 mod"]
["12918","OE - Osłona czołowa perforowana W850, 1M / 700",59,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12918","SZT","85389099",null,"230619RT","5901988129187","OE - Panneau avant perforé L850, 1M / 700","OE - Perforated Front cover W850, 1M / 700","OE- TAPA FRONTAL VENTILADA W850, 1M (H 50MM)","OE - Perforált előlap W850, 1M / 700"]
["12920","OE - Osłona czołowa pełna W850, 2M / 700",54.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","12920","SZT","85389099","27.12.40.0","230619RT","5901988129200","OE - Couverture avant complète L850, 2M / 700","OE - Plain Front cover W850, 2M / 700","OE- TAPA CIEGA W850, 2M (H 100MM)","OE - Teljes első burkolat W850, 2M / 700"]
["12925","OE - Osłona aparatury modułowej W850, 2M / 700, 36 mod",55.9,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12925","SZT","85389099","27.12.40.0","230619RT","5901988129255","OE - Couverture d'appareil modulaire L850, 2M / 700, 36 mod","OE - Modular equipment cover W850, 2M / 700, 36 mod","OE- TAPA MODULAR W850, 2M (H 100MM) 36 MOD","OE - Moduláris berendezés burkolata W850, 2M / 700, 36 mod"]
["12928","OE - Osłona czołowa perforowana W850, 2M / 700",65.599999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12928","SZT","85389099","27.12.40.0","230619RT","5901988129286","OE - Panneau avant perforé L850, 2M / 700","OE - Perforated Front cover W850, 2M / 700","OE- TAPA FRONTAL VENTILADA W850, 2M (H 100MM)","OE - Perforált előlap W850, 2M / 700"]
["12930","OE - Osłona czołowa pełna W850, 3M / 700",62.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12930","SZT","85389099","27.12.40.0","230619RT","5901988129309","OE - Couverture avant complète L850, 3M / 700","OE - Plain Front cover W850, 3M / 700","OE- TAPA CIEGA W850, 3M (H 150MM)","OE - Teljes első burkolat W850, 3M / 700"]
["12931","OE - Osłona czołowa W850, 3M / 700, otw. 92x92",64,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12931","SZT","85389099",null,"230619RT","5901988129316","OE - Protection frontale L850, 3M / 700, ouverte 92x92","OE - W850, 3M / 700 Front cover, hole 92x92","OE- W850, TAPA TROQ. 3M / 700, ORIFICIO 92X92","OE - Első burkolat W850, 3M / 700, nyitott 92x92"]
["12932","OE - Osłona czołowa wgłębiona, W850, 3M / 700",220,"1-ZE-01",null,null,"01_PLAIN_COVERS","12932","SZT","85389099",null,"230619RT","5901988129323","OE - Couvercle avant profond de, L850,  3M / 700","OE - Recessed front hood, W850, 3M / 700","OE- TAPA FRONTAL EMPOTRADA W850, 3M / 700","OE - Süllyesztett előlap, W850, 3M / 700"]
["12935","OE - Osłona aparatury modułowej W850, 3M / 700, 36 mod",63.6,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12935","SZT","85389099","27.12.40.0",null,"5901988129354","OE - Couverture d'appareil modulaire L850, 3M / 700, 36 mod","OE - Modular equipment cover W850, 3M / 700, 36 mod","OE- TAPA MODULAR W850, 3M (H 150MM) 36 MOD","OE - Moduláris berendezések burkolata W850, 3M / 700, 36 mod"]
["12938","OE - Osłona czołowa perforowana W850, 3M / 700",74.099999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12938","SZT","85389099","27.12.40.0","230619RT","5901988129385","OE - Panneau avant perforé L850, 3M / 700","OE - Perforated Front cover W850, 3M / 700","OE- TAPA FRONTAL VENTILADA W850, 3M (H 150MM)","OE - Perforált előlap W850, 3M / 700"]
["12939","OE - Osłona czołowa przeźroczysta W850, 3M / 700",223.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12939","SZT","85389099","27.12.40.0","230619RT","5901988129392","OE - Couverture avant, L850, 3M / 700","OE - Transparent Front cover W850, 3M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 3M ","OE - Átlátszó előlap W850, 3M / 700"]
["12940","OE - Osłona czołowa pełna W850, 4M / 700",70.099999999999994,"1-ZE-01",null,null,"01_PLAIN_COVERS","12940","SZT","85389099","27.12.40.0","230619RT","5901988129408","OE - Couverture avant complète L850, 4M / 700","OE - Plain Front cover W850, 4M / 700","OE- TAPA CIEGA W850, 4M (H 200MM)","OE - Teljes első burkolat W850, 4M / 700"]
["12941","OE - Osłona czołowa W850, 4M / 700, otw. 92x92",71.5,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12941","SZT","85381000","27.12.40.0","230619RT","5901988129415","OE - Protection frontale L850, 4M / 700, ouverte 92x92","OE - W850, 4M / 700 Front cover, hole 92x92","OE/OM - TAPA CIEGA W850 4M (H 200MM) CON AGUJERO 92X92","OE - Első burkolat W850, 4M / 700, nyitható 92x92"]
["12942","OE - Osłona czołowa wgłębiona, W850, 4M / 700",231,"1-ZE-01",null,null,"01_PLAIN_COVERS","12942","SZT","85389099",null,"230619RT","5901988129422","OE - Ecran facial encastré, L850, 4M / 700","OE - Recessed front hood, W850, 4M / 700","OE- TAPA FRONTAL EMPOTRADA W850, 4M / 700","OE - Süllyesztett előlap, W850, 4M / 700"]
["12945","OE - Osłona aparatury modułowej W850, 4M / 700, 36 mod",71.3,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12945","SZT","85389099","27.12.40.0",null,"5901988129453","OE - Couverture d'appareil modulaire L850, 4M / 700, 36 mod","OE - Modular equipment cover W850, 4M / 700, 36 mod","OE- TAPA MODULAR W850, 4M (H 200MM) 36 MOD","OE - Moduláris berendezés burkolata W850, 4M / 700, 36 mod"]
["12948","OE - Osłona czołowa perforowana W850, 4M / 700",82.6,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12948","SZT","85389099","27.12.40.0","230619RT","5901988129484","OE - Panneau avant perforé L850, 4M / 700","OE - Perforated Front cover W850, 4M / 700","OE- TAPA FRONTAL VENTILADA W850, 4M (H 200MM)","OE - Perforált előlap W850, 4M / 700"]
["12949","OE - Osłona czołowa przeźroczysta W850, 4M / 700",245,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12949","SZT","85389099","27.12.40.0","230619RT","5901988129491","OE - Couverture avant, L850, 4M / 700","OE - Transparent Front cover W850, 4M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 4M ","OE - Átlátszó előlap W850, 4M / 700"]
["12950","OE - Osłona czołowa pełna W850, 5M / 700",77.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","12950","SZT","85389099","27.12.40.0","230619RT","5901988129507","OE - Couverture avant complète L850, 5M / 700","OE - Plain Front cover W850, 5M / 700","OE- TAPA CIEGA W850, 5M (H 250MM)","OE - Teljes első burkolat W850, 5M / 700"]
["12951","OE - Osłona czołowa W850, 5M / 700, otw. 92x92",80,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","12951","SZT","85389099",null,"230619RT","5901988129514","OE - Protection frontale L850, 5M / 700, ouverte 92x92","OE - W850, 5M / 700 Front cover, hole 92x92","OE- W850, 5M / 700 TAPA TROQ. AGUJERO 92X92","OE - Első burkolat W850, 5M / 700, nyitható 92x92"]
["12952","OE - Osłona czołowa wgłębiona, W850, 5M / 700",247.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12952","SZT","85389099",null,"230619RT","5901988129521","OE - Ecran facial encastré, L850, 5M / 700","OE - Recessed front hood, W850, 5M / 700","OE- TAPA FRONTAL EMPOTRADA W850, 5M / 700","OE - Süllyesztett előlap, W850, 5M / 700"]
["12955","OE - Osłona aparatury modułowej W850, 5M / 700, 36 mod",79.099999999999994,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12955","SZT","85389099","27.12.40.0","230619RT","5901988129552","OE - Couverture d'appareil modulaire L850, 5M / 700, 36 mod","OE - Modular equipment cover W850, 5M / 700, 36 mod","OE- TAPA MODULAR W850, 5M (H 250MM) 36 MOD","OE - W850 moduláris berendezés burkolat, 5M / 700, 36 mod"]
["12958","OE - Osłona czołowa perforowana W850, 5M / 700",95.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12958","SZT","85389099","27.12.40.0","230619RT","5901988129583","OE - Couvercle avant perforé L850, 5M / 700","OE - Perforated Front cover W850, 5M / 700","OE- TAPA FRONTAL VENTILADA W850, 5M (H 250MM)","OE - Perforált előlap W850, 5M / 700"]
["12959","OE - Osłona czołowa przeźroczysta W850, 6M / 700",280.60000000000002,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12959","KPL","85389099","27.12.40.0","230620RT","5901988129590","OE - Couverture avant, L850, 6M / 700","OE - Transparent Front cover W850, 6M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 6M ","OE - Átlátszó előlap W850, 6M / 700"]
["12960","OE - Osłona czołowa pełna W850, 6M / 700",83.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12960","SZT","85389099","27.12.40.0","230620RT","5901988129606","OE - Couverture avant complète L850, 6M / 700","OE - Plain Front cover W850, 6M / 700","OE- TAPA CIEGA W850, 6M (H 300MM)","OE - Teljes első burkolat W850, 6M / 700"]
["12962","OE - Osłona czołowa wgłębiona, W850, 6M / 700",258.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","12962","SZT","85389099",null,"230620RT","5901988129620","OE - Ecran facial encastré, L850, 6M / 700","OE - Recessed Front cover, W850, 6M / 700","OE- TAPA FRONTAL EMPOTRADA W850, 6M / 700","OE - Süllyesztett előlap, W850, 6M / 700"]
["12965","OE - Osłona aparatury modułowej W850, 6M / 700, 36 mod",84.9,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","12965","SZT","85389099",null,"230620RT","5901988129651","OE - Couverture d'appareil modulaire L850, 6M / 700, 36 mod","OE - Modular equipment cover W850, 6M / 700, 36 mod","OE- TAPA MODULAR W850, 6M (H 300MM) 36 MOD","OE - Moduláris berendezés burkolata W850, 6M / 700, 36 mod"]
["12968","OE - Osłona czołowa perforowana W850, 6M / 700",101.5,"1-ZE-01",null,null,"01_PERFORATED_COVERS","12968","SZT","85389099","27.12.40.0","230620RT","5901988129682","OE - Panneau avant perforé L850, 6M / 700","OE - Perforated Front cover W850, 6M / 700","OE- TAPA FRONTAL VENTILADA W850, 6M (H 300MM)","OE - Perforált előlap W850, 6M / 700"]
["12969","OE - Osłona czołowa przeźroczysta W850, 8M / 700",312.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12969","SZT","85389099","27.12.40.0","230620RT","5901988129699","OE - Couverture avant, L850, 8M / 700","OE - Transparent Front cover W850, 8M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 8M ","OE - Átlátszó előlap W850, 8M / 700"]
["12970","OE - Osłona czołowa pełna W850, 7M / 700",113.3,"1-ZE-01",null,null,"01_PLAIN_COVERS","12970","SZT","85389099","27.12.40.0","230620RT","5901988129705","OE - Couverture avant complète L850, 7M / 700","OE - Plain Front cover W850, 7M / 700","OE- TAPA CIEGA W850, 7M (H 350MM)","OE - Teljes első burkolat W850, 7M / 700"]
["12979","OE - Osłona czołowa przeźroczysta W850, 9M / 700",330.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12979","SZT","85389099",null,"230620RT","5901988129798","OE - Couverture avant, L850, 9M / 700","OE - Transparent Front cover W850, 9M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 9M ","OE - Átlátszó előlap W850, 9M / 700"]
["12980","OE - Osłona czołowa pełna W850, 8M / 700",118.8,"1-ZE-01",null,null,"01_PLAIN_COVERS","12980","SZT","85389099","27.12.40.0","230620RT","5901988129804","OE - Couverture avant complète L850, 8M / 700","OE - Plain Front cover W850, 8M / 700","OE- TAPA CIEGA W850, 8M (H 400MM)","OE - Teljes első burkolat W850, 8M / 700"]
["12989","OE - Osłona czołowa przeźroczysta W850, 10M / 700",347.3,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12989","SZT","85389099","27.12.40.0","230620RT","5901988129897","OE - Couverture avant, L850, 10M / 700","OE - Transparent Front cover W850, 10M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 10M ","OE - Átlátszó előlap W850, 10M / 700"]
["12990","OE - Osłona czołowa pełna W850, 9M / 700",128.69999999999999,"1-ZE-01",null,null,"01_PLAIN_COVERS","12990","SZT","85389099","27.12.40.0","230620RT","5901988129903","OE - Couverture avant complète L850, 9M / 700","OE - Plain Front cover W850, 9M / 700","OE- TAPA CIEGA W850, 9M (H 450MM)","OE - Teljes első burkolat W850, 9M / 700"]
["12991","OE - Osłona czołowa pełna W850, 10M / 700",136.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","12991","SZT","85389099","27.12.40.0","230620RT","5901988129910","OE - Couverture avant complète L850, 10M / 700","OE - Plain Front cover W850, 10M / 700","OE- TAPA CIEGA W850, 10M (H 500MM)","OE - Teljes első burkolat W850, 10M / 700"]
["12992","OE - Osłona czołowa pełna W850, 11M / 700",146.30000000000001,"1-ZE-01",null,null,"01_PLAIN_COVERS","12992","SZT","85389099","27.12.40.0","230620RT","5901988129927","OE - Couverture avant complète L850, 11M / 700","OE - Plain Front cover W850, 11M / 700","OE- TAPA CIEGA W850, 11M (H 550MM)","OE - Teljes első burkolat W850, 11M / 700"]
["12993","OE - Osłona czołowa pełna W850, 12M / 700",149.6,"1-ZE-01",null,null,"01_PLAIN_COVERS","12993","SZT","85389099","27.12.40.0","230620RT","5901988129934","OE - Couverture avant complète L850, 12M / 700","OE - Plain Front cover W850, 12M / 700","OE- TAPA CIEGA W850, 12M (H 600MM)","OE - Teljes első burkolat W850, 12M / 700"]
["12994","OE - Osłona czołowa pełna W850, 13M / 700",157.30000000000001,"1-ZE-01",null,null,"01_PLAIN_COVERS","12994","SZT","85389099",null,"230620RT","5901988129941","OE - Couverture avant complète L850, 13M / 700","OE - Plain Front cover W850, 13M / 700","OE- TAPA CIEGA W850, 13M (H 650MM)","OE - Teljes első burkolat W850, 13M / 700"]
["12995","OM-VSD - Osłona aparatury modułowej, układ pionowy W850, 9M / 700, 3x24 mod",161,"1-ZE-01",null,null,"OM_VSD_PLATES","12995","SZT","85389099",null,"230620RT","5901988129958","OM-VSD - Couvercle modulaire, vertical L850, 9M / 700, modulaire 3x24","OM-VSD - Modular equipment cover, Vertical layout W850, 9M / 700, 3x24 mod","OM-VSD- TAPA MODULAR VERTIC. W850, 9M / 700, 3X24 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W850, 9M / 700, 3x24 mod"]
["12996","OM-VSD - Osłona aparatury modułowej, układ pionowy W850, 10M / 700, 3x26 mod",169.1,"1-ZE-01",null,null,"OM_VSD_PLATES","12996","SZT","85389099",null,"230620RT","5901988129965","OM-VSD - Couvercle modulaire, vertical L850, 10M / 700, modulaire 3x26","OM-VSD - Modular equipment cover, Vertical layout W850, 10M / 700, 3x26 mod","OM-VSD- TAPA MODULAR VERTIC. W850, 10M/700, 3X26 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W850, 10M / 700, 3x26 mod"]
["12997","OM-VSD - Osłona aparatury modułowej, układ pionowy W850, 11M / 700, 3x29 mod",178.3,"1-ZE-01",null,null,"OM_VSD_PLATES","12997","SZT","85389099",null,"230620RT","5901988129972","OM-VSD - Couvercle modulaire, vertical L850, 11M / 700, modulaire 3x29","OM-VSD - Modular equipment cover, Vertical layout W850, 11M / 700, 3x29 mod","OM-VSD- TAPA MODULAR VERTIC. W850, 11M/700, 3X29 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W850, 11M / 700, 3x29 mod"]
["12998","OM-VSD - Osłona aparatury modułowej, układ pionowy W850, 12M / 700, 3x32 mod",182.9,"1-ZE-01",null,null,"OM_VSD_PLATES","12998","SZT","85389099",null,"230620RT","5901988129989","OM-VSD - Couvercle modulaire, vertical L850, 12M / 700, modulaire 3x32","OM-VSD - Modular equipment cover, Vertical layout W850, 12M / 700, 3x32 mod","OM-VSD- TAPA MODULAR VERTIC. W850, 12M/700, 3X32 MOD","OM-VSD - Moduláris berendezés burkolat, függőleges elrendezés W850, 12M / 700, 3x32 mod"]
["12999","OE - Osłona czołowa przeźroczysta W850, 12M / 700",381.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","12999","SZT","85389099","27.12.40.0","230620RT","5901988129996","OE - Couverture avant, L850, 12M / 700","OE - Transparent Front cover W850, 12M / 700","OE- TAPA FRONTAL TRANSPARENTE W850, 12M ","OE - Átlátszó előlap W850, 12M / 700"]
["14042","OE - Osłona czołowa dla NSX400-630 3P i analizatora 92x92mm, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14042","SZT","85389099",null,"230620RT","5901988140427","OE - Flasque avant pour analyseur NSX400-630 3P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for NSX400-630 3P and 92x92mm, W650, 4M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA ANALIZADOR NSX400-630 3P,  Y 92X92MM, W650, 4M/500, HORIZ. ","OE - Elülső burkolat NSX400-630 3P és analizátorhoz 92x92mm, W650, 4M / 500, vízszintes, kar"]
["14047","OE - Osłona czołowa Ochronnika Przepięciowego B+C z zabezpieczeniem bezpiecznikowym 160A W650, 3M / 500",61.2,"1-ZE-01",null,null,"03_SWITCHES_COVERS","14047","SZT","85389099",null,"230620RT","5901988140472","OE - capot avant du parasurtenseur B + C avec protection de fusible 160A L650, 3M / 500","OE - Front cover of surge arrester B + C with fuse 160A W650, 3M / 500","OE- TAPA TROQ. DE SOBRETENSIONES B+C CON FUSIBLE 160A W650, 3M/500","OE - B+C túlfeszültségvédő elülső burkolata biztosítékvédelemmel 160A W650, 3M / 500"]
["14050","OE - Osłona czołowa dla UCB100 3P i analizatora 92x92mm, W650, 3M / 500, poziomo, dźwignia",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14050","SZT","85389099",null,"230620RT","5901988140502","OE - Couvercle frontal pour analyseur UCB100 3P et 92x92mm, L650, 3M / 500, horizontal, à levier","OE - Front cover for UCB100 3P and 92x92mm, W650, 3M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UCB100 3P Y ANALIZADOR DE REDES  92X92MM, W650, 3M/500, HORIZ. ","OE - Elülső burkolat UCB100 3P és analizátorhoz 92x92mm, W650, 3M / 500, vízszintes, kar"]
["14051","OE - Osłona czołowa dla UCB100 4P i analizatora 92x92mm, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14051","SZT","85389099",null,"230620RT","5901988140519","OE - Couvercle frontal pour analyseur UCB100 4P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for UCB100 4P and 92x92mm, W650, 4M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UCB100 4P Y ANALIZADOR DE REDES 92X92MM, W650, 4M/500, HORIZ. ","OE - Elülső burkolat UCB100 4P és analizátorhoz 92x92mm, W650, 4M / 500, vízszintes, kar"]
["14052","OE - Osłona czołowa dla UCB160-250 3P i analizatora 92x92mm, W650, 3M / 500, poziomo, dźwignia",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14052","SZT","85389099",null,"230620RT","5901988140526","OE - Couvercle frontal pour analyseur UCB160-250 3P et 92x92mm, L650, 3M / 500, horizontal, à levier","OE - Front cover for UCB160-250 3P and analyzer 92x92mm, W650, 3M / 500, Horizontal, Lever","OE- TAPA TROQ. PARA UCB160-250 3P,  Y ANALIZ. 92X92MM, W650, 3M/500, HORIZ. ","OE - Elülső burkolat UCB160-250 3P és analizátorhoz 92x92mm, W650, 3M / 500, vízszintes, kar"]
["14053","OE - Osłona czołowa dla UCB160-250 4P i analizatora 92x92mm, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14053","SZT","85389099",null,"230620RT","5901988140533","OE - Couvercle frontal pour analyseur UCB160-250 4P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for UCB160-250 4P and analyzer 92x92mm, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB160-250 4P  Y ANALIZADOR DE REDES 92X92MM, W650, 4M/500, HORIZ. ","OE - Elülső burkolat UCB160-250 4P és analizátorhoz 92x92mm, W650, 4M / 500, vízszintes, kar"]
["14054","OE - Osłona czołowa dla UCB400 3P i analizatora 92x92mm, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14054","SZT","85389099",null,"230620RT","5901988140540","OE - Blindage frontal pour analyseur UCB400 3P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for UCB400 3P and 92x92mm, W650, 4M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UCB400 3P Y ANALIZADOR DE REDES 92X92MM, W650, 4M/500, HORIZ. ","OE - Elülső burkolat UCB400 3P és analizátorhoz 92x92mm, W650, 4M / 500, vízszintes, kar"]
["14055","OE - Osłona czołowa dla UCB400 4P i analizatora 92x92mm, W650, 5M / 500, poziomo, dźwignia",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14055","SZT","85389099",null,"230620RT","5901988140557","OE - Flasque avant pour UCB400 4P et 92x92mm, L650, analyseur 5M / 500, horizontal, à levier","OE - Front cover for UCB400 4P and 92x92mm, W650, 5M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UCB400 4P  Y ANALIZADOR DE REDES 92X92MM, W650, 5M/500, HORIZ. ","OE - Elülső burkolat UCB400 4P és analizátorhoz 92x92mm, W650, 5M / 500, vízszintes, kar"]
["14060","OE - Osłona czołowa dla UPB100-250 3P i analizatora 92x92mm, W650, 3M / 500, poziomo, dźwignia",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14060","SZT","85389099",null,"230620RT","5901988140601","OE - Couvercle frontal pour analyseur UPB100-250 3P et 92x92mm, L650, 3M / 500, horizontal, à levier","OE - Front cover for UPB100-250 3P and 92x92mm, W650, 3M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UPB100-250 3P Y ANALIZADOR DE REDES 92X92MM, W650, 3M/500, HORIZ. ","OE - Elülső burkolat UPB100-250 3P-hez és analizátorhoz 92x92mm, W650, 3M / 500, vízszintes, kar"]
["14061","OE - Osłona czołowa dla UPB100-250 4P i analizatora 92x92mm, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14061","SZT","85389099",null,"230620RT","5901988140618","OE - Couvercle frontal pour analyseur UPB100-250 4P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for UPB100-250 4P and 92x92mm, W650, 4M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UPB100-250 4P  Y ANALIZADOR DE REDES 92X92MM, W650, 4M/500, HORIZ. ","OE - Elülső burkolat UPB100-250 4P és analizátorhoz 92x92mm, W650, 4M / 500, vízszintes, kar"]
["14062","OE - Osłona czołowa dla UPB400-630 3P i analizatora 92x92mm, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14062","SZT","85389099",null,"230620RT","5901988140625","OE - Ecran frontal pour analyseur UPB400-630 3P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for UPB400-630 3P and 92x92mm, W650, 4M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UPB400-630 3P Y ANALIZADOR DE REDES 92X92MM, W650, 4M/500, HORIZ. ","OE - Elülső burkolat UPB400-630 3P és analizátorhoz 92x92mm, W650, 4M / 500, vízszintes, kar"]
["14063","OE - Osłona czołowa dla UPB400-630 4P i analizatora 92x92mm, W650, 5M / 500, poziomo, dźwignia",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14063","SZT","85389099",null,"230620RT","5901988140632","OE - Flasque avant pour analyseur UPB400-630 4P et 92x92mm, L650, 5M / 500, horizontal, à levier","OE - Front cover for UPB400-630 4P and 92x92mm, W650, 5M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UPB400-630 4P  Y ANALIZ. 92X92MM, W650, 5M/500, HORIZ. ","OE - Elülső burkolat UPB400-630 4P és analizátorhoz 92x92mm, W650, 5M / 500, vízszintes, kar"]
["14072","OE - Osłona czołowa dla NSX400-630 3P i analizatora 92x92mm, W850, 4M / 700, poziomo, dźwignia",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14072","SZT","85389099",null,"230620RT","5901988140724","OE - Flasque avant pour analyseur NSX400-630 3P et 92x92mm, L850, 4M / 700, horizontal, à levier","OE - Front cover for NSX400-630 3P and 92x92mm, W850, 4M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA NSX400-630 3P Y 92X92MM, W850, 4M/700, HORIZ. ","OE - Elülső burkolat NSX400-630 3P és analizátorhoz 92x92mm, W850, 4M / 700, vízszintes, kar"]
["14073","OE - Osłona czołowa dla NSX400-630 4P i analizatora 92x92mm, W850, 5M / 700, poziomo, dźwignia",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14073","SZT","85389099",null,"230620RT","5901988140731","OE - Adaptateur universel pour appareils de mesure + capot avant L650, 3M / 500","OE - Front cover for NSX400-630 4P and 92x92mm, W850, 5M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA NSX400-630 4P Y 92X92MM, W850, 5M/700, HORIZ. ","OE - Elülső burkolat NSX400-630 4P és analizátorhoz 92x92mm, W850, 5M / 700, vízszintes, kar"]
["14084","OE - Osłona czołowa dla UCB400 3P i analizatora 92x92mm, W850, 4M / 700, poziomo, dźwignia",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","14084","SZT","85389099",null,"230620RT","5901988140847","OE - Flasque avant pour analyseur UCB400 3P et 92x92mm, L850, 4M / 700, horizontal, à levier","OE - Front cover for UCB400 3P and 92x92mm, W850, 4M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UCB400 3P Y 92X92MM, W850, 4M/700, HORIZ. ","OE - Elülső burkolat UCB400 3P és analizátorhoz 92x92mm, W850, 4M / 700, vízszintes, kar"]
["14085","OE - Osłona czołowa dla UCB400 4P i analizatora 92x92mm, W850, 5M / 700, poziomo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14085","SZT","85389099",null,"230620RT","5901988140854","OE - Flasque avant pour UCB400 4P et 92x92mm, L850, analyseur 5M / 700, horizontal, à levier","OE - Front cover for UCB400 4P and 92x92mm, W850, 5M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UCB400 4P Y ANALIZ. 92X92MM, W850, 5M/700, HORIZ. ","OE - Elülső burkolat UCB400 4P és analizátorhoz 92x92mm, W850, 5M / 700, vízszintes, kar"]
["14092","OE - Osłona czołowa dla UPB400-630 3P i analizatora 92x92mm, W850, 4M / 700, poziomo, dźwignia",85,"1-ZE-01",null,null,"OE_MCCB_COVERS","14092","SZT","85389099",null,"230620RT","5901988140922","OE - Couvercle avant pour analyseur UPB400-630 3P et 92x92mm, L850, 4M / 700, horizontal, à levier","OE - Front cover for UPB400-630 3P and 92x92mm, W850, 4M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UPB400-630 3P Y ANALIZ. 92X92MM, W850, 4M/700, HORIZ. ","OE - Elülső burkolat UPB400-630 3P és analizátorhoz 92x92mm, W850, 4M / 700, vízszintes, kar"]
["14093","OE - Osłona czołowa dla UPB400-630 4P i analizatora 92x92mm, W850, 5M / 700, poziomo, dźwignia",87.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14093","SZT","85389099",null,"230620RT","5901988140939","OE - Adaptateur universel pour appareils de mesure + capot avant L850, 3M / 700","OE - Front cover for UPB400-630 4P and 92x92mm, W850, 5M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UPB400-630 4P Y ANALIZ. 92X92MM, W850, 5M/700, HORIZ. ","OE - Elülső burkolat UPB400-630 4P és analizátorhoz 92x92mm, W850, 5M / 700, vízszintes, kar"]
["14411","OE - Osłona czołowa INS/INV100-250, W400, 5M / 250, pionowo",68.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14411","SZT","85389099",null,"230620RT","5901988144111","OE - capot avant INS / INV100-250, L400, 5M / 250, vertical","OE - INS / INV100-250, W400, 5M / 250 front visor, Vertical","OE- TAPA TROQ. INS / INV100-250, W400, 5M / 250, VERT.","OE - Első burkolat INS/INV100-250, W400, 5M / 250, függőleges"]
["14412","OE - Osłona czołowa INS/INV100-250, W400, 4M / 250, poziomo",59.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14412","SZT","85389099",null,"230620RT","5901988144128","OE - Couvercle avant NS1600 3 / 4P, L650, 8M / 500, entraînement rotatif, en permanence","OE - INS / INV100-250, W400, 4M / 250 front visor, Horizontal","OE- TAPA TROQ. INS / INV100-250, W400, 4M / 250, HORIZ.","OE - Elülső burkolat INS/INV100-250, W400, 4M / 250, vízszintes"]
["14413","OE - Osłona czołowa INS/INV320-630, W400, 7M / 250, pionowo",89.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14413","SZT","85389099",null,"230620RT","5901988144135","OE - capot avant INS / INV320-630, L400, 7M / 250, vertical","OE - INS / INV320-630 Front cover, W400, 7M / 250, Vertical","OE- TAPA TROQ. INS / INV320-630, W400, 7M / 250, VERT.","OE - Első burkolat INS/INV320-630, W400, 7M / 250, függőleges"]
["14414","OE - Osłona czołowa INS/INV320-630, W400, 5M / 250, poziomo",68.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14414","SZT","85389099",null,"230620RT","5901988144142","OE - Couvercle avant NS1600 3 / 4P, L650, 8M / 500, entraînement par moteur, permanent","OE - INS / INV320-630 Front cover, W400, 5M / 250, Horizontal","OE- TAPA TROQ. INS / INV320-630, W400, 5M / 250 , HORIZ.","OE - Első burkolat INS/INV320-630, W400, 5M / 250, vízszintes"]
["14433","OE - Osłona czołowa NSX100-250 3/4P, W400, 5M / 250, pionowo, dźwignia",68.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14433","SZT","85389099","27.12.40.0","230620RT","5901988144333","OE - capot avant NSX100-250 3 / 4P, L400, 5M / 250, vertical, levier","OE - NSX100-250 3 / 4P Front Hood, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. NSX100-250 3 / 4P, W400, 5M / 250, VERT.","OE - Első burkolat NSX100-250 3/4P, W400, 5M / 250, függőleges, kar"]
["14434","OE - Osłona czołowa NSX100-250 3/4P, W400, 5M / 250, pionowo, silnik, obrotowy",68.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14434","SZT","85389099",null,"230620RT","5901988144340","OE - capot avant NSX100-250 3 / 4P, L400, 5M / 250, vertical, moteur, rotatif","OE - NSX100-250 3 / 4P Front Hood, W400, 5M / 250, Vertical, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3 / 4P, W400, 5M / 250, VERT. MOTOR,","OE - Első burkolat NSX100-250 3/4P, W400, 5M / 250, függőleges, motoros, forgatható"]
["14435","OE - Osłona czołowa NSX100-250 VIGI 3/4P, W400, 7M / 250, pionowo, dźwignia",89.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14435","SZT","85389099",null,"230622RT","5901988144357","OE - capot avant NSX100-250 VIGI 3 / 4P, L400, 7M / 250, vertical, levier","OE - Front cover NSX100-250 VIGI 3 / 4P, W400, 7M / 250, Vertical, Lever","OE- TAPA TROQ. NSX100-250 VIGI 3/4P, W400, 7M/250, VERT.","OE - Első burkolat NSX100-250 VIGI 3/4P, W400, 7M / 250, függőleges, kar"]
["14456","OE - Osłona czołowa NSX400-630 3/4P, W400, 9M / 250, pionowo, dźwignia",99.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14456","SZT","85389099","27.12.40.0","230622RT","5901988144562","OE - capot avant NSX400-630 3 / 4P, L400, 9M / 250, vertical, levier","OE - Front cover NSX400-630 3 / 4P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. NSX400-630 3/4P, W400, 9M/250, VERT.","OE -Előlap NSX400-630 3/4P, W400, 9M / 250, függőleges, kar"]
["14457","OE - Osłona czołowa NSX400-630 3/4P, W400, 9M / 250, pionowo, silnik, obrotowy, wysuwny",99.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14457","SZT","85389099",null,"230622RT","5901988144579","OE - capot avant NSX400-630 3 / 4P, L400, 9M / 250, vertical, moteur, rotatif, dĂ©brochable","OE - Front cover NSX400-630 3 / 4P, W400, 9M / 250, Vertical, Motor, Rotary, Drawout","OE- TAPA TROQ. NSX400-630 3 / 4P, W400, 9M / 250, VERT. MOTOR, EXTRAÍBLE","OE - Előlap NSX400-630 3/4P, W400, 9M / 250, függőleges, motoros, forgatható, kihúzható"]
["14458","OE - Osłona czołowa NSX400-630 VIGI 3/4P, W400, 9M / 250, pionowo, dźwignia",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","14458","SZT","85389099",null,"230622RT","5901988144586","OE - capot avant NSX400-630 VIGI 3 / 4P, L400, 9M / 250, vertical, levier","OE - Front cover NSX400-630 VIGI 3 / 4P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. NSX400-630 VIGI 3/4P, W400, 9M/250, VERT.","OE - Első burkolat NSX400-630 VIGI 3/4P, W400, 9M / 250, függőleges, kar"]
["14483","OE - Osłona czołowa NS1600 3P, W400, 8M / 250, pionowo, dźwignia, na stałe",105.8,"1-ZE-01",null,null,"OE_ACB_COVERS","14483","SZT","85389099",null,"230622RT","5901988144838","OE - capot avant NS1600 3P, L400, 8M / 250, vertical, levier, de mani?re permanente","OE - NS1600 3P Front Hood, W400, 8M / 250, Vertical, Lever, Fixed","OE- TAPA TROQ. NS1600 3P, W400, 8M / 250, VERT. FIJO","OE - Előlap NS1600 3P, W400, 8M / 250, függőleges, kar, fix"]
["14484","OE - Osłona czołowa NS1600 3P, W400, 8M / 250, pionowo, silnik, na stałe",105.8,"1-ZE-01",null,null,"OE_ACB_COVERS","14484","SZT","85389099",null,"230622RT","5901988144845","OE - capot avant NS1600 3P, L400, 8M / 250, vertical, moteur, permanent","OE - NS1600 3P Front Hood, W400, 8M / 250, Vertical, Motor, Fixed","OE- TAPA TROQ. NS1600 3P, W400, 8M / 250, VERT. MOTOR, FIJO","OE - Első burkolat NS1600 3P, W400, 8M / 250, függőleges, motoros, fix"]
["14485","OE - Osłona czołowa NS1600 3P, W400, 8M / 250, pionowo, napęd obrotowy, na stałe",105.8,"1-ZE-01",null,null,"OE_ACB_COVERS","14485","SZT","85389099",null,"230622RT","5901988144852","OE - capot avant NS1600 3P, L400, 8M / 250, vertical, entraĂ®nement rotatif, permanent","OE - NS1600 3P Front Hood, W400, 8M / 250, Vertical, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3P, W400, 8M / 250, VERT. FIJO","OE - Elülső burkolat NS1600 3P, W400, 8M / 250, függőleges, forgó hajtás, fix"]
["14490","OE - Osłona czołowa NT16 3P, W400, 7M / 250, na stałe",97.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14490","SZT","85389099",null,"230622RT","5901988144906","OE - Couvercle avant NW40, L850, 9M / 700, vertical, amovible","OE - Front cover NT16 3P, W400, 7M / 250, permanent","OE- TAPA TROQ. NT16 3P, W400, 7M/250, FIJA","OE - Előlap NT16 3P, W400, 7M / 250, állandó"]
["14511","OE - Osłona czołowa INS/INV100-250, W450, 5M / 300, pionowo",72.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","14511","SZT","85389099",null,"230622RT","5901988145118","OE - capot avant INS / INV100-250, L450, 5M / 300, vertical","OE - INS / INV100-250, W450, 5M / 300 front visor, Vertical","OE- TAPA TROQ. INS / INV100-250, W450, 5M / 300, VERT.","OE - Első burkolat INS/INV100-250, W450, 5M / 300, függőleges"]
["14512","OE - Osłona czołowa INS/INV100-250, W450, 4M / 300, poziomo",62,"1-ZE-01",null,null,"OE_MCCB_COVERS","14512","SZT","85389099",null,"230622RT","5901988145125","OE - capot avant INS / INV100-250, L450, 4M / 300, horizontal","OE - INS / INV100-250 Front cover, W450, 4M / 300, Horizontal","OE- TAPA TROQ. INS / INV100-250, W450, 4M / 300, HORIZ.","OE - Első burkolat INS/INV100-250, W450, 4M / 300, vízszintes"]
["14513","OE - Osłona czołowa INS/INV320-630, W450, 7M / 300, pionowo",95.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","14513","SZT","85389099","27.12.40.0","230622RT","5901988145132","OE - capot avant INS / INV320-630, L450, 7M / 300, vertical","OE - INS / INV320-630 front shield, W450, 7M / 300, Vertical","OE- TAPA TROQ. INS / INV320-630, W450, 7M / 300, VERT.","OE - Első burkolat INS/INV320-630, W450, 7M / 300, függőleges"]
["14514","OE - Osłona czołowa INS/INV320-630, W450, 5M / 300, poziomo",72.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","14514","SZT","85389099",null,"230622RT","5901988145149","OE - capot avant INS / INV320-630, L450, 5M / 300, horizontal","OE - INS / INV320-630, W450, 5M / 300 Front cover, Horizontal","OE- TAPA TROQ. INS/INV320-630, W450, 5M/300, HORIZ.","OE - Első burkolat INS/INV320-630, W450, 5M / 300, vízszintes"]
["14533","OE - Osłona czołowa 2/1x NSX100-250 3/4P, W450, 5M / 300, pionowo, dźwignia",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","14533","SZT","85389099","27.12.40.0","230622RT","5901988145330","OE - capot avant 2 / 1x NSX100-250 3 / 4P, L450, 5M / 300, vertical, levier","OE - Front cover 2 / 1x NSX100-250 3 / 4P, W450, 5M / 300, Vertical, Lever","OE- TAPA TROQ. 2 / 1X NSX100-250 3 / 4P, W450, 5M / 300, VERT.","OE - Első burkolat 2/1x NSX100-250 3/4P, W450, 5M / 300, függőleges, kar"]
["14534","OE - Osłona czołowa 2x NSX100-250 3P, W450, 5M / 300, pionowo, silnik, obrotowy",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","14534","SZT","85389099",null,"230622RT","5901988145347","OE - capot avant 2 / 1x NSX100-250 3 / 4P, L450, 5M / 300, vertical, moteur, rotatif","OE - Front Hood 2 / 1x NSX100-250 3 / 4P, W450, 5M / 300, Vertical, Motor, Rotary","OE- TAPA TROQ. 2X NSX100-250 3P, W450, 5M / 300, VERT. MOTOR","OE - Első burkolat 2x NSX100-250 3P, W450, 5M / 300, függőleges, motoros, forgatható"]
["14535","OE - Osłona czołowa 2/1x NSX100-250 VIGI 3/4P, W450, 7M / 300, pionowo, dźwignia",95.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","14535","SZT","85389099",null,"230622RT","5901988145354","OE - capot avant 2 / 1x NSX100-250 VIGI 3 / 4P, L450, 7M / 300, vertical, levier","OE - Front cover 2 / 1x NSX100-250 VIGI 3 / 4P, W450, 7M / 300, Vertical, Lever","OE- TAPA TROQ. 2 / 1X NSX100-250 VIGI 3 / 4P, W450, 7M / 300, VERT.","OE - Első burkolat 2/1x NSX100-250 VIGI 3/4P, W450, 7M / 300, függőleges, kar"]
["14536","OE - Osłona czołowa 1x NSX100-250 4P, W450, 5M / 300, pionowo, silnik, obrotowy",64.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14536","SZT","85389099",null,"230622RT","5901988145361","OE - Capot avant 1x NSX100-250 4P, L450, 5M / 300, vertical, moteur, rotatif","OE - 1x NSX100-250 4P Front Hood, W450, 5M / 300, Vertical, Motor, Rotary","OE- 1X NSX100-250 4P COFRE DELANTERO, W450, 5M / 300, VERT. MOTOR","OE - Első burkolat 1x NSX100-250 4P, W450, 5M / 300, függőleges, motoros, forgatható"]
["14537","OE - Osłona czołowa NSX100-250 3P, W450, 3M / 300, poziomo, dźwignia",59.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14537","SZT","85389099",null,"230622RT","5901988145378","OE - capot avant NSX100-250 3P, L450, 3M / 300, horizontal, levier","OE - NSX100-250 3P Front Hood, W450, 3M / 300, Horizontal, Lever","OE- NSX100-250 3P  W450, 3M / 300, HORIZ.","OE - Első burkolat NSX100-250 3P, W450, 3M / 300, vízszintes, kar"]
["14538","OE - Osłona czołowa NSX100-250 3P, W450, 3M / 300, poziomo, silnik, obrotowy",59.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14538","SZT","85389099",null,"230622RT","5901988145385","OE - capot avant NSX100-250 3P, L450, 3M / 300, horizontal, moteur, rotatif","OE - NSX100-250 3P Front Hood, W450, 3M / 300, Horizontal, Motor, Rotary","OE- NSX100-250 3P  W450, 3M / 300, HORIZ. MOTOR, ","OE - Első burkolat NSX100-250 3P, W450, 3M / 300, vízszintes, motoros, forgatható"]
["14541","OE - Osłona czołowa NSX100-250 4P, W450, 4M / 300, poziomo, dźwignia",62,"1-ZE-01",null,null,"OE_MCCB_COVERS","14541","SZT","85389099",null,"230622RT","5901988145415","OE - capot avant NSX100-250 4P, L450, 4M / 300, horizontal, levier","OE - NSX100-250 4P Front Hood, W450, 4M / 300, Horizontal, Lever","OE- NSX100-250 4P  W450, 4M / 300, HORIZ.","OE - Első burkolat NSX100-250 4P, W450, 4M / 300, vízszintes, kar"]
["14542","OE - Osłona czołowa NSX100-250 4P, W450, 4M / 300, poziomo, silnik, obrotowy",62,"1-ZE-01",null,null,"OE_MCCB_COVERS","14542","SZT","85389099",null,"230622RT","5901988145422","OE - capot avant NSX100-250 4P, L450, 4M / 300, horizontal, moteur, rotatif","OE - NSX100-250 4P Front Hood, W450, 4M / 300, Horizontal, Motor, Rotary","OE- NSX100-250 4P  W450, 4M / 300, HORIZ. MOTOR, ","OE - Első burkolat NSX100-250 4P, W450, 4M / 300, vízszintes, motoros, forgatható"]
["14546","OE - Osłona czołowa 2x NSX100-250 3/4P SZR, W450, 8M / 300, blokada płytowa, poziomo, silnik",104.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","14546","SZT","85389099",null,"230622RT","5901988145460","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L450, 8M / 300, verrouillage de plaque, horizontal, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W450, 8M / 300, plate lock, Horizontal, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W450, 8M/300,  HORIZ.  MOTOR","OE - Első burkolat 2x NSX100-250 3/4P SZR, W450, 8M / 300, lemezzár, vízszintes, motor"]
["14556","OE - Osłona czołowa NSX400-630 3/4P, W450, 9M / 300, pionowo, dźwignia",113.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","14556","SZT","85389099","27.12.40.0","230622RT","5901988145569","OE - capot avant NSX400-630 3 / 4P, L450, 9M / 300, vertical, levier","OE - NSX400-630 3 / 4P Front Hood, W450, 9M / 300, Vertical, Lever","OE- NSX400-630 3 / 4P  W450, 9M / 300, VERT.","OE - Első burkolat NSX400-630 3/4P, W450, 9M / 300, függőleges, kar"]
["14557","OE - Osłona czołowa NSX400-630 3/4P, W450, 9M / 300, pionowo, silnik, obrotowy, wysuwny",113.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","14557","SZT","85389099",null,"230622RT","5901988145576","OE - capot avant NSX400-630 3 / 4P, L450, 9M / 300, vertical, moteur, rotatif, dĂ©brochable","OE - Front cover NSX400-630 3 / 4P, W450, 9M / 300, Vertical, Motor, rotatable, withdrawable","OE- TAPA TROQ. NSX400-630 3 / 4P, W450, 9M / 300, VERT. MOTOR, EXTRAÍBLE","OE - Előlap NSX400-630 3/4P, W450, 9M / 300, függőleges, motoros, forgatható, kihúzható"]
["14558","OE - Osłona czołowa NSX400-630 VIGI 3/4P, W450, 11M / 300, pionowo, dźwignia",121,"1-ZE-01",null,null,"OE_MCCB_COVERS","14558","SZT","85389099",null,"230622RT","5901988145583","OE - capot avant NSX400-630 VIGI 3 / 4P, L450, 9M / 300, vertical, levier","OE - Front cover NSX400-630 VIGI 3 / 4P, W450, 11M / 300, Vertical, Lever","OE- TAPA TROQ. NSX400-630 VIGI 3/4P, W450, 11M/300, VERT.","OE - Első burkolat NSX400-630 VIGI 3/4P, W450, 11M / 300, függőleges, kar"]
["14562","OE - Osłona czołowa NSX400-630 3P, W450, 4M / 300, poziomo, dźwignia",62,"1-ZE-01",null,null,"OE_MCCB_COVERS","14562","SZT","85389099",null,"230622RT","5901988145620","OE - capot avant NSX400-630 3P, L450, 4M / 300, horizontal, levier","OE - NSX400-630 3P Front Hood, W450, 4M / 300, Horizontal, Lever","OE- PLACA MONTAJE NSX400-630 3P  W450, 4M / 300, HORIZ.","OE - Első burkolat NSX400-630 3P, W450, 4M / 300, vízszintes, kar"]
["14566","OE - Osłona czołowa NSX400-630 4P, W450, 5M / 300, poziomo, dźwignia",72.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","14566","SZT","85389099",null,"230622RT","5901988145668","OE - capot avant NSX400-630 4P, L450, 5M / 300, horizontal, levier","OE - NSX400-630 4P Front Hood, W450, 5M / 300, Horizontal, Lever","OE- PLACA MONTAJE NSX400-630 4P  W450, 5M / 300, HORIZ.","OE - Első burkolat NSX400-630 4P, W450, 5M / 300, vízszintes, kar"]
["14583","OE - Osłona czołowa NS1600 3/4P, W450, 8M / 300, pionowo, dźwignia, na stałe",113.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14583","SZT","85389099","27.12.40.0","230622RT","5901988145835","OE - capot avant NS1600 3 / 4P, L450, 8M / 300, vertical, levier, en permanence","OE - NS1600 3 / 4P Front Shield, W450, 8M / 300, Vertical, Lever, Fixed","OE- TAPA TROQ. NS1600 3 / 4P W450, 8M / 300, VERT. FIJO","OE - Első burkolat NS1600 3/4P, W450, 8M / 300, függőleges, kar, fix"]
["14584","OE - Osłona czołowa NS1600 3/4P, W450, 8M / 300, pionowo, silnik, na stałe",113.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14584","SZT","85389099","27.12.40.0","230622RT","5901988145842","OE - capot avant NS1600 3 / 4P, L450, 8M / 300, vertical, moteur, permanent","OE - NS1600 3 / 4P Front Hood, W450, 8M / 300, Vertical, Motor, Fixed","OE- TAPA TROQ. NS1600 3 / 4P W450, 8M / 300, VERT. MOTOR, FIJO","OE - Első burkolat NS1600 3/4P, W450, 8M / 300, függőleges, motoros, fix"]
["14585","OE - Osłona czołowa NS1600 3/4P, W450, 8M / 300, pionowo, napęd obrotowy, na stałe",113.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14585","SZT","85389099","27.12.40.0","230622RT","5901988145859","OE - capot avant NS1600 3 / 4P, L450, 8M / 300, vertical, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W450, 8M / 300, Vertical, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P W450, 8M / 300, VERT. ACCIONAMIENTO , FIJO","OE - Elülső burkolat NS1600 3/4P, W450, 8M / 300, függőleges, forgó hajtás, fix"]
["14589","OE - Osłona czołowa NS1600/NT16 3P, W450, 10M / 300, wysuwny",126.5,"1-ZE-01",null,null,"OE_ACB_COVERS","14589","SZT","85389099","27.12.40.0","230622RT","5901988145897","OE - Face avant NS1600/NT16 3P, L450, 10M / 300, coulissant","OE - Front cover NS1600 / NT16 3P, W450, 10M / 300, withdrawable","OE- TAPA TROQ. NS1600/NT16 3P, W450, 10M/300, EXTRAÍBLE","OE - Előlap NS1600/NT16 3P, W450, 10M / 300, kihúzható"]
["14590","OE - Osłona czołowa NT16 3/4P, W450, 7M / 300, na stałe",109.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14590","SZT","85389099",null,"230622RT","5901988145903","OE - capot avant NT16 3 / 4P, L450, 7M / 300, en permanence","OE - Front cover NT16 3 / 4P, W450, 7M / 300, permanent","OE- TAPA TROQ. NT16 3/4P, W450, 7M/300, FIJA","OE - Elülső burkolat NT16 3/4P, W450, 7M / 300, állandó"]
["14711","OE - Osłona czołowa 3x INS/INV100-250, W650, 5M / 500, pionowo",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14711","SZT","85389099","27.12.40.0","230622RT","5901988147112","OE - capot avant 3x INS / INV100-250, L650, 5M / 500, vertical","OE - Front cover 3x INS / INV100-250, W650, 5M / 500, Vertical","OE- TAPA TROQ. 3X INS / INV100-250, W650, 5M / 500, VERT.","OE - Első burkolat 3x INS/INV100-250, W650, 5M / 500, függőleges"]
["14712","OE - Osłona czołowa INS/INV100-250, W650, 4M / 500, poziomo",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14712","SZT","85389099","27.12.40.0","230622RT","5901988147129","OE - capot avant INS / INV100-250, L650, 4M / 500, horizontal","OE - INS / INV100-250, W650, 4M / 500 Front cover, Horizontal","OE- TAPA TROQ. INS / INV100-250, W650, 4M / 500,  HORIZ.","OE - Elülső burkolat INS/INV100-250, W650, 4M / 500, vízszintes"]
["14713","OE - Osłona czołowa 2x INS/INV320-630, 1x INS/INV320-630 RZR, W650, 7M / 500, pionowo",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14713","SZT","85389099","27.12.40.0","230622RT","5901988147136","OE - capot avant 2x INS / INV320-630, L650, 1x INS/INV320-630 RZR, 7M / 500, vertical","OE - Front cover 2x INS / INV320-630, 1x INS / INV320-630 RZR, W650, 7M / 500, Vertical","OE- TAPA TROQ. 2X INS / INV320-630, 1X INS / INV320-630 RZR, W650, 7M / 500, VERT.","OE - Első burkolat 2x INS/INV320-630, 1x INS/INV320-630 RZR, W650, 7M / 500, függőleges"]
["14714","OE - Osłona czołowa INS/INV320-630, W650, 5M / 500, poziomo",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14714","SZT","85389099","27.12.40.0","230622RT","5901988147143","OE - capot avant INS / INV320-630, L650, 5M / 500, horizontal","OE - INS / INV320-630, W650, 5M / 500 Front cover, Horizontal","OE- TAPA TROQ. INS/INV320-630, W650, 5M/500, HORIZ.","OE - Elülső burkolat INS/INV320-630, W650, 5M / 500, vízszintes"]
["14718","OE - Osłona czołowa 2x INS/INV100-250 RZR, W650, 5M / 500, pionowo, dźwignia",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14718","SZT","85389099","27.12.40.0","230622RT","5901988147181","OE - capot avant 2x INS / INV100-250 RZR, L650, 5M / 500, vertical, levier","OE - Front cover 2x INS / INV100-250 RZR, W650, 5M / 500, Vertical, Lever","OE- TAPA TROQ. 2X INS / INV100-250 RZR, W650, 5M / 500, VERT.","OE - Első burkolat 2x INS/INV100-250 RZR, W650, 5M / 500, függőleges, kar"]
["14733","OE - Osłona czołowa 4/3x NSX100-250 3/4P, W650, 5M / 500, pionowo, dźwignia",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14733","SZT","85389099","27.12.40.0","230622RT","5901988147334","OE - capot avant 4 / 3x NSX100-250 3 / 4P, L650, 5M / 500, vertical, levier","OE - Front cover 4 / 3x NSX100-250 3 / 4P, W650, 5M / 500, Vertical, Lever","OE- TAPA TROQ. 4 / 3X NSX100-250 3 / 4P, W650, 5M / 500, VERT.","OE - Első burkolat 4/3x NSX100-250 3/4P, W650, 5M / 500, függőleges, kar"]
["14734","OE - Osłona czolowa 4x NSX100-250 3P, W650, 5M / 500, pionowo, silnik, obrotowy",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14734","SZT","85389099","27.12.40.0","230622RT","5901988147341","OE - capot avant 4x NSX100-250 3P, L650, 5M / 500, vertical, moteur, rotatif","OE - Front Shield 4 / 3x NSX100-250 3 / 4P, W650, 5M / 500, Vertical, Motor, Rotary","OE- TAPA TROQ. 4X NSX100-250 3P, W650, 5M / 500, VERT. MOTOR, ","OE - Első burkolat 4x NSX100-250 3P, W650, 5M / 500, függőleges, motoros, forgatható"]
["14735","OE - Osłona czołowa 4/3x NSX100-250 VIGI 3/4P, W650, 7M / 500, pionowo, dźwignia",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14735","SZT","85389099","27.12.40.0","230622RT","5901988147358","OE - capot avant 4 / 3x NSX100-250 VIGI 3 / 4P, L650, 7M / 500, vertical, levier","OE - Front cover 4 / 3x NSX100-250 VIGI 3 / 4P, W650, 7M / 500, Vertical, Lever","OE- TAPA TROQ. 4 / 3X NSX100-250 VIGI 3 / 4P, W650, 7M / 500, VERT.","OE - Első burkolat 4/3x NSX100-250 VIGI 3/4P, W650, 7M / 500, függőleges, kar"]
["14736","OE - Osłona czołowa 3x NSX100-250 4P, W650, 5M / 500, pionowo, silnik, obrotowy",70.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","14736","SZT","85389099",null,"230622RT","5901988147365","OE - Capot avant 3x NSX100-250 4P, L650, 5M / 500, vertical, moteur, rotatif","OE - Front cover 3x NSX100-250 4P, W650, 5M / 500, Vertical, Motor, Rotary","OE- TAPA TROQ. 3X NSX100-250 4P, W650, 5M / 500, VERT. MOTOR, ","OE - Első burkolat 3x NSX100-250 4P, W650, 5M / 500, függőleges, motoros, forgatható"]
["14737","OE - Osłona czołowa NSX100-250 3P, W650, 3M / 500, poziomo, dźwignia",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14737","SZT","85389099","27.12.40.0","230622RT","5901988147372","OE - capot avant NSX100-250 3P, L650, 3M / 500, horizontal, levier","OE - NSX100-250 3P Front Hood, W650, 3M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 3P  W650, 3M / 500, HORIZ.","OE - Első burkolat NSX100-250 3P, W650, 3M / 500, vízszintes, kar"]
["14738","OE - Osłona czołowa NSX100-250 3P, W650, 3M / 500, poziomo, silnik, obrotowy",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14738","SZT","85389099","27.12.40.0","230622RT","5901988147389","OE - capot avant NSX100-250 3P, L650, 3M / 500, horizontal, moteur, rotatif","OE - NSX100-250 3P Front Hood, W650, 3M / 500, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3P  W650, 3M / 500, HORIZ., MOTOR, ","OE - Első burkolat NSX100-250 3P, W650, 3M / 500, vízszintes, motoros, forgatható"]
["14739","OE - Osłona czołowa NSX100-250 VIGI 3P, W650, 3M / 500, poziomo, dźwignia",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14739","SZT","85389099","27.12.40.0","230622RT","5901988147396","OE - capot avant NSX100-250 VIGI 3P, L650, 3M / 500, horizontal, levier","OE - Front cover NSX100-250 VIGI 3P, W650, 3M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 VIGI 3P, W650, 3M/500, HORIZ.","OE - Első burkolat NSX100-250 VIGI 3P, W650, 3M / 500, vízszintes, kar"]
["14740","OE - Osłona czołowa NSX100-250 3P, W650, 4M / 500, poziomo, wysuwny",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14740","SZT","85389099","27.12.40.0","230622RT","5901988147402","OE - capot avant NSX100-250 3P, L650, 4M / 500, horizontal, dĂ©brochable","OE - Front cover NSX100-250 3P, W650, 4M / 500, Horizontal, Sliding","OE- TAPA TROQ. NSX100-250 3P  W650, 4M / 500, HORIZ., DESLIZANTE","OE - Előlap NSX100-250 3P, W650, 4M / 500, vízszintes, kihúzható"]
["14741","OE - Osłona czołowa NSX100-250 4P, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14741","SZT","85389099","27.12.40.0","230622RT","5901988147419","OE - capot avant NSX100-250 4P, L650, 4M / 500, horizontal, levier","OE - NSX100-250 4P Front Hood, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 4P  W650, 4M / 500, HORIZ.","OE - Első burkolat NSX100-250 4P, W650, 4M / 500, vízszintes, kar"]
["14742","OE - Osłona czołowa NSX100-250 4P, W650, 4M / 500, poziomo, silnik, obrotowy",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14742","SZT","85389099","27.12.40.0","230622RT","5901988147426","OE - capot avant NSX100-250 4P, L650, 4M / 500, horizontal, moteur, rotatif","OE - NSX100-250 4P, W650, 4M / 500 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 4P, W650, 4M / 500, HORIZ., MOTOR, ","OE - Első burkolat NSX100-250 4P, W650, 4M / 500, vízszintes, motoros, forgatható"]
["14743","OE - Osłona czołowa NSX100-250 VIGI 4P, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14743","SZT","85389099","27.12.40.0","230622RT","5901988147433","OE - capot avant NSX100-250 VIGI 4P, L650, 4M / 500, horizontal, levier","OE - Front cover NSX100-250 VIGI 4P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 VIGI 4P, W650, 4M/500, HORIZ.","OE - Első burkolat NSX100-250 VIGI 4P, W650, 4M / 500, vízszintes, kar"]
["14744","OE - Osłona czołowa NSX100-250 4P, W650, 5M / 500, poziomo, wysuwny",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14744","SZT","85389099","27.12.40.0","230622RT","5901988147440","OE - capot avant NSX100-250 4P, L650, 5M / 500, horizontal, dĂ©brochable","OE - NSX100-250 4P front visor, W650, 5M / 500, Horizontal, sliding","OE- TAPA TROQ. NSX100-250 4P, W650, 5M/500, HORIZ., DESLIZANTE","OE - Előlap NSX100-250 4P, W650, 5M / 500, vízszintes, kihúzható"]
["14745","OE - Osłona czołowa 2x NSX100-250 3/4P SZR, W650, 7M / 500, blokada płytowa, pionowo, silnik",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14745","SZT","85389099","27.12.40.0","230622RT","5901988147457","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L650, 7M / 500, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W650, 7M / 500, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W650, 7M/500, VERT. MOTOR","OE - Első burkolat 2x NSX100-250 3/4P SZR, W650, 7M / 500, lemezzár, függőleges, motor"]
["14746","OE - Osłona czołowa 2x NSX100-250 3/4P SZR, W650, 8M / 500, blokada płytowa, poziomo, silnik",127.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14746","SZT","85389099","27.12.40.0","230622RT","5901988147464","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L650, 8M / 500, verrou de plaque, horizontal, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W650, 8M / 500, plate lock, Horizontal, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W650, 8M/500,  HORIZ., MOTOR","OE - Első burkolat 2x NSX100-250 3/4P SZR, W650, 8M / 500, lemezzár, vízszintes, motor"]
["14756","OE - Osłona czołowa 1x NSX400-630 3/4P, W650, 9M / 500, pionowo, dźwignia",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14756","SZT","85389099",null,"230622RT","5901988147563","OE - capot avant 1x NSX400-630 3 / 4P, L650, 9M / 500, vertical, levier","OE - 1x NSX400-630 3 / 4P Front cover, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. 1X NSX400-630 3/4P, W650, 9M/500, VERT.","OE - Első burkolat 1x NSX400-630 3/4P, W650, 9M / 500, függőleges, kar"]
["14757","OE - Osłona czołowa 1x NSX400-630 3/4P, W650, 9M / 500, pionowo, silnik, obrotowy, wysuwny",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14757","SZT","85389099",null,"230622RT","5901988147570","OE - capot avant 1x NSX400-630 3 / 4P, L650, 9M / 500, vertical, moteur, rotatif, dĂ©brochable","OE - Front cover 1x NSX400-630 3 / 4P, W650, 9M / 500, Vertical, Motor, rotatable, withdrawable","OE- TAPA TROQ. 1X NSX400-630 3 / 4P, W650, 9M / 500, VERT. MOTOR, EXTRAÍBLE","OE - Előlap 1x NSX400-630 3/4P, W650, 9M / 500, függőleges, motoros, forgatható, kihúzható"]
["14758","OE - Osłona czołowa 1x NSX400-630 VIGI 3/4P, W650, 11M / 500, pionowo, dźwignia",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14758","SZT","85389099",null,"230622RT","5901988147587","OE - capot avant 1x NSX400-630 VIGI 3 / 4P, L650, 11M / 500, vertical, levier","OE - Front cover 1x NSX400-630 VIGI 3 / 4P, W650, 11M / 500, Vertical, Lever","OE- TAPA TROQ. 1X NSX400-630 VIGI 3 / 4P, W650, 11M / 500, VERT.","OE - Első burkolat 1x NSX400-630 VIGI 3/4P, W650, 11M / 500, függőleges, kar"]
["14759","OE - Osłona czołowa 2x NSX400-630 3/4P, W650, 9M / 500, pionowo, dźwignia",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14759","SZT","85389099","27.12.40.0","230622RT","5901988147594","OE - capot avant 2x NSX400-630 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 2x NSX400-630 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. 2X NSX400-630 3/4P, W650, 9M/500, VERT.","OE - Első burkolat 2x NSX400-630 3/4P, W650, 9M / 500, függőleges, kar"]
["14760","OE - Osłona czołowa 2x NSX400-630 3/4P, W650, 9M / 500, pionowo, silnik, obrotowy",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14760","SZT","85389099","27.12.40.0","230622RT","5901988147600","OE - capot avant 2x NSX400-630 3 / 4P, L650, 9M / 500, vertical, moteur, rotatif","OE - Front cover 2x NSX400-630 3 / 4P, W650, 9M / 500, Vertical, Motor, rotary","OE- TAPA TROQ. 2X NSX400-630 3/4P, W650, 9M/500, VERT. MOTOR, ROTATIVO","OE - Első burkolat 2x NSX400-630 3/4P, W650, 9M / 500, függőleges, motoros, forgatható"]
["14761","OE - Osłona czołowa 2x NSX400-630 VIGI 3/4P, W650, 11M / 500, pionowo, dźwignia",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14761","SZT","85389099","27.12.40.0","230622RT","5901988147617","OE - capot avant 2x NSX400-630 VIGI 3/4 P, L650, 9M / 500, vertical, levier","OE - Front cover 2x NSX400-630 VIGI 3 / 4P, W650, 11M / 500, Vertical, Lever","OE- TAPA TROQ. 2X NSX400-630 VIGI 3 / 4P, W650, 11M / 500, VERT.","OE - Első burkolat 2x NSX400-630 VIGI 3/4P, W650, 11M / 500, függőleges, kar"]
["14762","OE - Osłona czołowa NSX400-630 3P, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14762","SZT","85389099","27.12.40.0","230622RT","5901988147624","OE - capot avant NSX400-630 3P, L650, 4M / 500, horizontal, levier","OE - NSX400-630 3P Front Hood, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 3P  W650, 4M / 500, HORIZ.","OE - Első burkolat NSX400-630 3P, W650, 4M / 500, vízszintes, kar"]
["14763","OE - Osłona czołowa NSX400-630 3P, W650, 4M / 500, poziomo, silnik, obrotowy",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14763","SZT","85389099","27.12.40.0","230622RT","5901988147631","OE - capot avant NSX400-630 3P, L650, 4M / 500, horizontal, moteur, rotatif","OE - NSX400-630 3P, W650, 4M / 500 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 3P, W650, 4M / 500, HORIZ., MOTOR, ","OE - Első burkolat NSX400-630 3P, W650, 4M / 500, vízszintes, motoros, forgatható"]
["14764","OE - Osłona czołowa NSX400-630 VIGI 3P, W650, 4M / 500, poziomo, dźwignia",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14764","SZT","85389099","27.12.40.0","230622RT","5901988147648","OE - capot avant NSX400-630 VIGI 3P, L650, 4M / 500, horizontal, levier","OE - Front cover NSX400-630 VIGI 3P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 VIGI 3P, W650, 4M/500, HORIZ.","OE - Első burkolat NSX400-630 VIGI 3P, W650, 4M / 500, vízszintes, kar"]
["14765","OE - Osłona czołowa NSX400-630 3P, W650, 6M / 500, poziomo, wysuwny, silnik",88.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14765","SZT","85389099","27.12.40.0","230622RT","5901988147655","OE - capot avant NSX400-630 3P, L650, 6M / 500, horizontal, dĂ©brochable, moteur","OE - Front cover NSX400-630 3P, W650, 6M / 500, Horizontal, extendable, engine","OE- TAPA TROQ. NSX400-630 3P, W650, 6M/500, HORIZ., EXTENSIBLE, MOTOR","OE - Első burkolat NSX400-630 3P, W650, 6M / 500, vízszintes, kihúzható, motor"]
["14766","OE - Osłona czołowa NSX400-630 4P, W650, 5M / 500, poziomo, dźwignia",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14766","SZT","85389099","27.12.40.0","230622RT","5901988147662","OE - capot avant NSX400-630 4P, L650, 5M / 500, horizontal, levier","OE - NSX400-630 4P Front Hood, W650, 5M / 500, Horizontal, Lever","OE-TAPA TROQ.  NSX400-630 4P  W650, 5M / 500, HORIZ.","OE - Első burkolat NSX400-630 4P, W650, 5M / 500, vízszintes, kar"]
["14767","OE - Osłona czołowa NSX400-630 4P, W650, 5M / 500, poziomo, silnik, obrotowy",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14767","SZT","85389099","27.12.40.0","230622RT","5901988147679","OE - capot avant NSX400-630 4P, L650, 5M / 500, horizontal, moteur, rotatif","OE - NSX400-630 4P, W650, 5M / 500 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 4P, W650, 5M / 500, HORIZ., MOTOR, ","OE - Első burkolat NSX400-630 4P, W650, 5M / 500, vízszintes, motoros, forgatható"]
["14768","OE - Osłona czołowa NSX400-630 VIGI 4P, W650, 5M / 500, poziomo, dźwignia",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","14768","SZT","85389099","27.12.40.0","230622RT","5901988147686","OE - capot avant NSX400-630 VIGI 4P, L650, 5M / 500, horizontal, levier","OE - Front cover NSX400-630 VIGI 4P, W650, 5M / 500, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 VIGI 4P, W650, 5M/500, HORIZ.","OE - Első burkolat NSX400-630 VIGI 4P, W650, 5M / 500, vízszintes, kar"]
["14769","OE - Osłona czołowa NSX400-630 4P, W650, 7M / 500, poziomo, wysuwny, silnik",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","14769","SZT","85389099","27.12.40.0","230622RT","5901988147693","OE - capot avant NSX400-630 4P, L650, 7M / 500, horizontal, dĂ©brochable, moteur","OE - Front cover NSX400-630 4P, W650, 7M / 500, Horizontal, Extendable, Motor","OE- TAPA TROQ. NSX400-630 4P, W650, 7M/500, HORIZ., EXTENSIBLE, MOTOR","OE - Első burkolat NSX400-630 4P, W650, 7M / 500, vízszintes, kihúzható, motor"]
["14770","OE - Osłona czołowa 2x NSX400-630 3/4P SZR, W650, 9M / 500, blokada płytowa, pionowo, silnik",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14770","SZT","85389099","27.12.40.0","230622RT","5901988147709","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L650, 9M / 500, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W650, 9M / 500, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX400-630 3/4P SZR, W650, 9M/500,  VERT. MOTOR","OE - Első burkolat 2x NSX400-630 3/4P SZR, W650, 9M / 500, lemezzár, függőleges, motor"]
["14771","OE - Osłona czołowa 2x NSX400-630 3/4P SZR, W650, 10M / 500, blokada płytowa, poziomo, silnik",150.69999999999999,"1-ZE-01",null,null,"OE_MCCB_COVERS","14771","SZT","85389099","27.12.40.0","230622RT","5901988147716","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L650, 10M / 500, verrou de plaque, horizontal, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W650, 10M / 500, plate lock, Horizontal, Motor","OE- TAPA TROQ. 2x NSX400-630 3/4P SZR, W650, 10M/500,  HORIZ., MOTOR","OE - Első burkolat 2x NSX400-630 3/4P SZR, W650, 10M / 500, lemezzár, vízszintes, motor"]
["14773","OE - Osłona czołowa UA/BA, W650, 4M / 500",73.099999999999994,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","14773","SZT","85389099",null,"230622RT","5901988147730","OE - Capot avant UA/BA, L650, 4M / 500","OE - Front visor UA / BA, W650, 4M / 500","OE- TAPA TROQ. UA/BA, W650, 4M/500","OE - Előlap UA/BA, W650, 4M / 500"]
["14783","OE - Osłona czołowa NS1600 3/4P, W650, 8M / 500, pionowo, dźwignia, na stałe",144.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14783","SZT","85389099","27.12.40.0","230622RT","5901988147839","OE - capot avant NS1600 3 / 4P, L650, 8M / 500, vertical, ? levier, de mani?re permanente","OE - NS1600 3 / 4P Front Hood, W650, 8M / 500, Vertical, Lever, Fixed","OE- TAPA TROQ. NS1600 3 / 4P W650, 8M / 500, VERT. FIJO","OE - Előlap NS1600 3/4P, W650, 8M / 500, függőleges, kar, fix"]
["14784","OE - Osłona czołowa NS1600 3/4P, W650, 8M / 500, pionowo, silnik, na stałe",144.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14784","SZT","85389099","27.12.40.0","230622RT","5901988147846","OE - capot avant NS1600 3 / 4P, L650, 8M / 500, vertical, moteur, permanent","OE - NS1600 3 / 4P Front Hood, W650, 8M / 500, Vertical, Motor, Fixed","OE- TAPA TROQ. NS1600 3 / 4P  W650, 8M / 500, VERT. MOTOR, FIJO","OE - Borító részvezeték NS1600 3/4P, W650, 8M / 500, függőleges, motoros, fix"]
["14785","OE - Osłona czołowa NS1600 3/4P, W650, 8M / 500, pionowo, napęd obrotowy, na stałe",144.9,"1-ZE-01",null,null,"OE_ACB_COVERS","14785","SZT","85389099","27.12.40.0","230622RT","5901988147853","OE - capot avant NS1600 3 / 4P, L650, 8M / 500, vertical, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W650, 8M / 500, Vertical, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P TAPA TROQ., W650, 8M / 500, VERT. ACCIONAMIENTO , FIJO","OE - Elülső burkolat NS1600 3/4P, W650, 8M / 500, függőleges, forgó hajtás, fix"]
["14786","OE - Osłona czołowa NS1600 3/4P, W650, 7M / 500, poziomo, dźwignia, na stałe",134.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14786","SZT","85389099","27.12.40.0","230622RT","5901988147860","OE - capot avant NS1600 3 / 4P, L650, 7M / 500, horizontal, levier, en permanence","OE - NS1600 3 / 4P front visor, W650, 7M / 500, Horizontal, Lever, fixed","OE- TAPA TROQ. NS1600 3 / 4P, W650, 7M / 500, HORIZ., FIJA","OE - Előlap NS1600 3/4P, W650, 7M / 500, vízszintes, kar, fix"]
["14787","OE - Osłona czołowa NS1600 3/4P, W650, 7M / 500, poziomo, silnik, na stałe",134.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14787","SZT","85389099","27.12.40.0","230622RT","5901988147877","OE - capot avant NS1600 3 / 4P, L650, 8M / 500, horizontal, moteur, permanent","OE - NS1600 3 / 4P Front Hood, W650, 7M / 500, Horizontal, Motor, Fixed","OE- TAPA TROQ. NS1600 3 / 4P  W650, 7M / 500, HORIZ., MOTOR, FIJO","OE - Első burkolat NS1600 3/4P, W650, 7M / 500, vízszintes, motoros, fix"]
["14788","OE - Osłona czołowa NS1600 3/4P, W650, 7M / 500, poziomo, napęd obrotowy, na stałe",134.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14788","SZT","85389099","27.12.40.0","230622RT","5901988147884","OE - capot avant NS1600 3 / 4P, L650, 7M / 500, horizontal, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W650, 7M / 500, Horizontal, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P, W650, 7M / 500, HORIZ., UNIDAD ROTATIVA, FIJA","OE - Előlap NS1600 3/4P, W650, 7M / 500, vízszintes, forgó hajtás, fix"]
["14789","OE - Osłona czołowa NS1600/NT16 3/4P, W650, 7M / 500, wysuwny",153,"1-ZE-01",null,null,"OE_ACB_COVERS","14789","SZT","85389099","27.12.40.0","230622RT","5901988147891","OE - Face avant NS1600/NT16 3/4P, L650, 7M / 500, coulissant","OE - Front cover NS1600 / NT16 3 / 4P, W650, 7M / 500, withdrawable","OE- TAPA TROQ. NS1600/NT16 3/4P, W650, 7M/500, EXTRAÍBLE","OE - Előlap NS1600/NT16 3/4P, W650, 7M / 500, kihúzható"]
["14790","OE - Osłona czołowa NT16 3/4P, W650, 7M / 500, na stałe",153,"1-ZE-01",null,null,"OE_ACB_COVERS","14790","SZT","85389099","27.12.40.0","230622RT","5901988147907","OE - capot avant NT16 3 / 4P, L650, 7M / 500, en permanence","OE - Front cover NT16 3 / 4P, W650, 7M / 500, permanent","OE- TAPA TROQ. NT16 3/4P, W650, 7M/500, FIJA","OE - Előlap NT16 3/4P, W650, 7M / 500, állandó"]
["14791","OE - Osłona czołowa NW40 3/4P, W650, 9M / 500, pionowo, wysuwny",261.10000000000002,"1-ZE-01",null,null,"OE_ACB_COVERS","14791","SZT","85389099","27.12.40.0","230622RT","5901988147914","OE - capot avant NW40 3 / 4P, L650, 9M / 500, vertical, débrochable","OE - NW40 3 / 4P, W650, 9M / 500 Front cover, Vertical, withdrawable","OE- TAPA TROQ. NW40 3/4P, W650, 9M/500 TAPA TROQ., VERT. EXTRAÍBLE","OE - Előlap NW40 3/4P, W650, 9M / 500, függőleges, kihúzható"]
["14792","OE - Osłona czołowa NW40 3/4P, W650, 8M / 500, pionowo, na stałe",240.4,"1-ZE-01",null,null,"OE_ACB_COVERS","14792","SZT","85389099","27.12.40.0","230622RT","5901988147921","OE - capot avant NW40 3 / 4P, L650, 8M / 500, vertical, permanent","OE - NW40 3 / 4P, W650, 8M / 500 front visor, Vertical, fixed","OE- TAPA TROQ. NW40 3/4P, W650, 8M/500, VERT. FIJA","OE - Előlap NW40 3/4P, W650, 8M / 500, függőleges, fix"]
["14793","OE - Osłona czołowa NW40b-63 3/4P, W1200, 9M / 500, pionowo, wysuwny",272.60000000000002,"1-ZE-01",null,null,"OE_ACB_COVERS","14793","SZT","85389099",null,"230622RT","5901988347932","OE - Capot avant NW40b-63 3 / 4P, L1200, 9M / 500, vertical, débrochable","OE - NW40b-63 3 / 4P, W1200, 9M / 500 Front cover, Vertical, sliding","OE- TAPA TROQ. NW40B-63 3 / 4P, W1200, 9M / 500 TAPA TROQ., VERT. DESLIZANTE","OE - Előlap NW40b-63 3/4P, W1200, 9M / 500, függőleges, kihúzható"]
["14820","OE - Osłona czołowa pełna W800, 2M / 650",52.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","14820","SZT","85389099",null,"230622RT","5901988148201","OE - Couverture avant complète L800, 2M / 650","OE - Plain Front cover W800, 2M / 650","OE- TAPA CIEGA W800, 2M / 650","OE - Teljes első burkolat W800, 2M / 650"]
["14825","OE - Osłona aparatury modułowej W800, 2M / 650, 33 mod",53.6,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","14825","SZT","85389099",null,"230622RT","5901988148256","OE - Couverture d'appareil modulaire L800, 2M / 650, 33 mod","OE - Modular equipment cover W800, 2M / 650, 33 mod","OE- TAPA MODULAR W800, 2M / 650, 33 MOD","OE - W800 moduláris berendezés burkolat, 2M / 650, 33 mod"]
["14828","OE - Osłona czołowa perforowana W800, 2M / 650",62.9,"1-ZE-01",null,null,"01_PERFORATED_COVERS","14828","SZT","85389099",null,"230622RT","5901988148287","OE - Panneau avant perforé L800, 2M / 650","OE - Perforated Front cover W800, 2M / 650","OE- TAPA TROQ.  W800, 2M / 650","OE - Perforált előlap W800, 2M / 650"]
["14830","OE - Osłona czołowa pełna W800, 3M / 650",60.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","14830","SZT","85389099",null,"230622RT","5901988148300","OE - Couverture avant complète L800, 3M / 650","OE - Plain Front cover W800, 3M / 650","OE- TAPA TROQ. CIEGA W800, 3M / 650","OE - Teljes első burkolat W800, 3M / 650"]
["14835","OE - Osłona aparatury modułowej W800, 3M / 650, 33 mod",61.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","14835","SZT","85389099",null,"230622RT","5901988148355","OE - Couvercle pour appareil modulaire L800, 3M / 650, 33 mod","OE - Modular equipment cover W800, 3M / 650, 33 mod","OE- TAPA MODULAR W800, 3M / 650, 33 MOD","OE - W800 moduláris berendezés burkolat, 3M / 650, 33 mod"]
["14838","OE - Osłona czołowa perforowana W800, 3M / 650",71.099999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","14838","SZT","85389099",null,"230622RT","5901988148386","OE - Panneau avant perforé L800, 3M / 650","OE - Perforated Front cover W800, 3M / 650","OE- TAPA TROQ.  W800, 3M / 650","OE - Perforált előlap W800, 3M / 650"]
["14839","OE - Osłona czołowa przeźroczysta W800, 3M / 650",215.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14839","SZT","85389099",null,"230622RT","5901988148393","OE - Couverture transparente L800, 3M / 650","OE - Transparent Front cover W800, 3M / 650","OE- TAPA TROQ. TRANSP. W800, 3M / 650","OE - Átlátszó előlap W800, 3M / 650"]
["14840","OE - Osłona czołowa pełna W800, 4M / 650",67.3,"1-ZE-01",null,null,"01_PLAIN_COVERS","14840","SZT","85389099",null,"230622RT","5901988148409","OE - Couverture avant complète L800, 4M / 650","OE - Plain Front cover W800, 4M / 650","OE- TAPA TROQ. CIEGA W800, 4M / 650","OE - Teljes első burkolat W800, 4M / 650"]
["14845","OE - Osłona aparatury modułowej W800, 4M / 650, 33 mod",68.5,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","14845","SZT","85389099",null,"230622RT","5901988148454","OE - Couvercle pour appareil modulaire L800, 4M / 650, 33 mod","OE - Modular equipment cover W800, 4M / 650, 33 mod","OE- TAPA MODULAR W800, 4M / 650, 33 MOD","OE - W800 moduláris berendezés burkolat, 4M / 650, 33 mod"]
["14848","OE - Osłona czołowa perforowana W800, 4M / 650",79.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS","14848","SZT","85389099",null,"230622RT","5901988148485","OE - Panneau avant perforé L800, 4M / 650","OE - Perforated Front cover W800, 4M / 650","OE- TAPA TROQ.  W800, 4M / 650","OE - Perforált előlap W800, 4M / 650"]
["14849","OE - Osłona czołowa przeźroczysta W800, 4M / 650",235.8,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14849","SZT","85389099",null,"230622RT","5901988148492","OE - Couvercle transparent L800, 4M / 650","OE - Transparent Front cover W800, 4M / 650","OE- TAPA TROQ. TRANSP. W800, 4M / 650","OE - Átlátszó előlap W800, 4M / 650"]
["14850","OE - Osłona czołowa pełna W800, 5M / 650",74.599999999999994,"1-ZE-01",null,null,"01_PLAIN_COVERS","14850","SZT","85389099",null,"230622RT","5901988148508","OE - Couverture avant complète L800, 5M / 650","OE - Plain Front cover W800, 5M / 650","OE- TAPA TROQ. CIEGA W800, 5M / 650","OE - Teljes első burkolat W800, 5M / 650"]
["14855","OE - Osłona aparatury modułowej W800, 5M / 650, 33 mod",75.900000000000006,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","14855","SZT","85389099",null,"230622RT","5901988148553","OE - Blindage d'équipement modulaire L800, 5M / 650, 33 mod","OE - Modular equipment cover W800, 5M / 650, 33 mod","OE- TAPA MODULAR W800, 5M / 650, 33 MOD","OE - W800 moduláris berendezés burkolat, 5M / 650, 33 mod"]
["14858","OE - Osłona czołowa perforowana W800, 5M / 650",91.3,"1-ZE-01",null,null,"01_PERFORATED_COVERS","14858","SZT","85389099",null,"230622RT","5901988148584","OE - Panneau avant perforé L800, 5M / 650","OE - Perforated Front cover W800, 5M / 650","OE- TAPA TROQ.  W800, 5M / 650","OE - Perforált előlap W800, 5M / 650"]
["14859","OE - Osłona czołowa przeźroczysta W800, 6M / 650",269.10000000000002,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14859","SZT","85389099",null,"230622RT","5901988148591","OE - Couverture transparente L800, 6M / 650","OE - Transparent Front cover W800, 6M / 650","OE- TAPA TROQ. TRANSP. W800, 6M / 650","OE - Átlátszó előlap W800, 6M / 650"]
["14860","OE - Osłona czołowa pełna W800, 6M / 650",79.8,"1-ZE-01",null,null,"01_PLAIN_COVERS","14860","SZT","85389099",null,"230622RT","5901988148607","OE - Couverture avant complète L800, 6M / 650","OE - Plain Front cover W800, 6M / 650","OE- TAPA TROQ. CIEGA W800, 6M / 650","OE - Teljes első burkolat W800, 6M / 650"]
["14865","OE - Osłona aparatury modułowej W800, 6M / 650, 33 mod",81.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","14865","SZT","85389099",null,"230622RT","5901988148652","OE - Couverture d'appareil modulaire L800, 6M / 650, 33 mod","OE - Modular equipment cover W800, 6M / 650, 33 mod","OE- TAPA MODULAR W800, 6M / 650, 33 MOD","OE - W800 moduláris berendezés burkolat, 6M / 650, 33 mod"]
["14868","OE - Osłona czołowa perforowana W800, 6M / 650",97.5,"1-ZE-01",null,null,"01_PERFORATED_COVERS","14868","SZT","85389099",null,"230622RT","5901988148683","OE - Panneau avant perforé L800, 6M / 650","OE - Perforated Front cover W800, 6M / 650","OE- TAPA TROQ.  W800, 6M / 650","OE - Perforált előlap W800, 6M / 650"]
["14869","OE - Osłona czołowa przeźroczysta W800, 8M / 650",300.2,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14869","SZT","85389099",null,"230622RT","5901988148690","OE - Couverture transparente L800, 8M / 650","OE - Transparent Front cover W800, 8M / 650","OE- TAPA TROQ. TRANSP. W800, 8M / 650","OE - Átlátszó előlap W800, 8M / 650"]
["14870","OE - Osłona czołowa pełna W800, 7M / 650",108.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","14870","SZT","85389099",null,"230622RT","5901988148706","OE - Couverture avant complète L800, 7M / 650","OE - Plain Front cover W800, 7M / 650","OE- TAPA TROQ. CIEGA W800, 7M / 650","OE - Teljes első burkolat W800, 7M / 650"]
["14879","OE - Osłona czołowa przeźroczysta W800, 9M / 650",317.39999999999998,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14879","SZT","85389099",null,"230622RT","5901988148799","OE - Couverture transparente L800, 9M / 650","OE - Transparent Front cover W800, 9M / 650","OE- TAPA TROQ. TRANSP. W800, 9M / 650","OE - Átlátszó előlap W800, 9M / 650"]
["14880","OE - Osłona czołowa pełna W800, 8M / 650",114.4,"1-ZE-01",null,null,"01_PLAIN_COVERS","14880","SZT","85389099",null,"230622RT","5901988148805","OE - Couverture avant complète L800, 8M / 650","OE - Plain Front cover W800, 8M / 650","OE- TAPA TROQ. CIEGA W800, 8M / 650","OE - Teljes első burkolat W800, 8M / 650"]
["14889","OE - Osłona czołowa przeźroczysta W800, 10M / 650",333.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14889","SZT","85389099",null,"230622RT","5901988148898","OE - Couverture transparente L800, 10M / 650","OE - Transparent Front cover W800, 10M / 650","OE- TAPA TROQ. TRANSP. W800, 10M / 650","OE - Átlátszó előlap W800, 10M / 650"]
["14890","OE - Osłona czołowa pełna W800, 9M / 650",123.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","14890","SZT","85389099",null,"230622RT","5901988148904","OE - Couverture avant complète L800, 9M / 650","OE - Plain Front cover W800, 9M / 650","OE- TAPA TROQ. CIEGA W800, 9M / 650","OE - Teljes első burkolat W800, 9M / 650"]
["14891","OE - Osłona czołowa pełna W800, 10M / 650",130.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","14891","SZT","85389099",null,"230622RT","5901988148911","OE - Couverture avant complète L800, 10M / 650","OE - Plain Front cover W800, 10M / 650","OE- TAPA TROQ. CIEGA W800, 10M / 650","OE - Teljes első burkolat W800, 10M / 650"]
["14892","OE - Osłona czołowa pełna W800, 11M / 650",139.69999999999999,"1-ZE-01",null,null,"01_PLAIN_COVERS","14892","SZT","85389099",null,"230622RT","5901988148928","OE - Couverture avant complète L800, 11M / 650","OE - Plain Front cover W800, 11M / 650","OE- TAPA TROQ. CIEGA W800, 11M / 650","OE - Teljes első burkolat W800, 11M / 650"]
["14893","OE - Osłona czołowa pełna W800, 12M / 650",143,"1-ZE-01",null,null,"01_PLAIN_COVERS","14893","SZT","85389099",null,null,"5901988348939","OE - Couverture avant complète L800, 12M / 650","OE - Plain Front cover W800, 12M / 650","OE- TAPA TROQ. CIEGA W800, 12M / 650","OE - Teljes első burkolat W800, 12M / 650"]
["14894","OE - Osłona czołowa pełna W800, 13M / 650",150.69999999999999,"1-ZE-01",null,null,"01_PLAIN_COVERS","14894","SZT","85389099",null,"230622RT","5901988148942","OE - Couverture avant complète L800, 13M / 650","OE - Plain Front cover W800, 13M / 650","OE- TAPA TROQ. CIEGA W800, 13M / 650","OE - Teljes első burkolat W800, 13M / 650"]
["14899","OE - Osłona czołowa przeźroczysta W800, 12M / 650",366.9,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","14899","SZT","85389099",null,"230622RT","5901988148997","OE - Couvercle transparent L800, 12M / 650","OE - Transparent Front cover W800, 12M / 650","OE- TAPA TROQ. TRANSP. W800, 12M / 650","OE - Átlátszó előlap W800, 12M / 650"]
["14911","OE - Osłona czołowa 4x INS/INV100-250, W850, 5M / 700, pionowo",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14911","SZT","85389099","27.12.40.0","230622RT","5901988149116","OE - couverture avant 4x INS / INV100-250, L850, 5M / 700, verticale","OE - Front cover 4x INS / INV100-250, W850, 5M / 700, Vertical","OE- TAPA TROQ. 4X INS / INV100-250, W850, 5M / 700, VERT.","OE - Első burkolat 4x INS/INV100-250, W850, 5M / 700, függőleges"]
["14912","OE - Osłona czołowa INS/INV100-250, W850, 4M / 700, poziomo",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14912","SZT","85389099","27.12.40.0","230622RT","5901988149123","OE - capot avant INS / INV100-250, L850, 4M / 700, horizontal","OE - INS / INV100-250, W850, 4M / 700 Front cover, Horizontal","OE- TAPA TROQ. INS / INV100-250, W850, 4M / 700,  HORIZ.","OE - Elülső burkolat INS/INV100-250, W850, 4M / 700, vízszintes"]
["14913","OE - Osłona czołowa 3x INS/INV320-630, 1x INS/INV320-630 RZR, W850, 7M / 700, pionowo",133.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14913","SZT","85389099","27.12.40.0","230622RT","5901988149130","OE - 3 x couvercle frontal INS / INV320-630, 1x INS/INV320-630 RZR, L850, 7M / 700, vertical","OE - Front cover 3x INS / INV320-630, 1x INS / INV320-630 RZR, W850, 7M / 700, Vertical","OE- TAPA TROQ. 3X INS / INV320-630, 1X INS / INV320-630 RZR, W850, 7M / 700, VERT.","OE - Első burkolat 3x INS/INV320-630, 1x INS/INV320-630 RZR, W850, 7M / 700, függőleges"]
["14914","OE - Osłona czołowa INS/INV320-630, W850, 5M / 700, poziomo",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14914","SZT","85389099","27.12.40.0","230622RT","5901988149147","OE - capot avant INS / INV320-630, L850, 5M / 700, horizontal","OE - INS / INV320-630, W850, 5M / 700 Front cover, Horizontal","OE- TAPA TROQ. INS / INV320-630, W850,  5M / 700, HORIZ.","OE - Első burkolat INS/INV320-630, W850, 5M / 700, vízszintes"]
["14918","OE - Osłona czołowa 2x INS/INV100-250 RZR, W850, 5M / 700, pionowo, dźwignia",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14918","SZT","85389099",null,"230622RT","5901988149185","OE - capot avant 2x INS / INV100-250 RZR, L850, 5M / 700, vertical, levier","OE - Front cover 2x INS / INV100-250 RZR, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. 2X INS / INV100-250 RZR, W850, 5M / 700, VERT.","OE - Első burkolat 2x INS/INV100-250 RZR, W850, 5M / 700, függőleges, kar"]
["14933","OE - Osłona czołowa 6/4x NSX100-250 3/4P, W850, 5M / 700, pionowo, dźwignia",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14933","SZT","85389099",null,"230622RT","5901988149338","OE - capot avant 6 / 4x NSX100-250 3 / 4P, L850, 5M / 700, vertical, levier","OE - Front cover 6 / 4x NSX100-250 3 / 4P, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. 6 / 4X NSX100-250 3 / 4P, W850, 5M / 700, VERT.","OE - Első burkolat 6/4x NSX100-250 3/4P, W850, 5M / 700, függőleges, kar"]
["14934","OE - Osłona czołowa 6x NSX100-250 3P, W850, 5M / 700, pionowo, silnik, obrotowy",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14934","SZT","85389099",null,"230622RT","5901988149345","OE - capot avant 6 / 4x NSX100-250 3 / 4P, L850, 5M / 700, vertical, moteur, rotatif","OE - Front Hood 6 / 4x NSX100-250 3 / 4P, W850, 5M / 700, Vertical, Motor, Rotary","OE- TAPA TROQ. 6X NSX100-250 3P, W850, 5M / 700, VERT. MOTOR, ","OE - Első burkolat 6x NSX100-250 3P, W850, 5M / 700, függőleges, motoros, forgatható"]
["14935","OE - Osłona czołowa 6/4x NSX100-250 VIGI 3/4P, W850, 7M / 700, pionowo, dźwignia",133.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14935","SZT","85389099","27.12.40.0","230622RT","5901988149352","OE - capot avant 6 / 4x NSX100-250 VIGI 3 / 4P, L850, 7M / 700, vertical, levier","OE - Front cover 6 / 4x NSX100-250 VIGI 3 / 4P, W850, 7M / 700, Vertical, Lever","OE- TAPA TROQ. 6 / 4X NSX100-250 VIGI 3 / 4P, W850, 7M / 700, VERT.","OE - Első burkolat 6/4x NSX100-250 VIGI 3/4P, W850, 7M / 700, függőleges, kar"]
["14936","OE - Osłona czołowa 4x NSX100-250 4P, W850, 5M / 700, pionowo, silnik, obrotowy",84.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","14936","SZT","85389099",null,"230622RT","5901988149369","OE - Capot avant 4x NSX100-250 4P, L850, 5M / 700, vertical, moteur, rotatif","OE - Front cover 4x NSX100-250 4P, W850, 5M / 700, Vertical, Motor, Rotary","OE- TAPA TROQ. 4X NSX100-250 4P, W850, 5M / 700, VERT. MOTOR, ","OE - Első burkolat 4x NSX100-250 4P, W850, 5M / 700, függőleges, motoros, forgatható"]
["14937","OE - Osłona czołowa NSX100-250 3P, W850, 3M / 700, poziomo, dźwignia",79,"1-ZE-01",null,null,"OE_MCCB_COVERS","14937","SZT","85389099","27.12.40.0","230622RT","5901988149376","OE - capot avant NSX100-250 3P, L850, 3M / 700, horizontal, levier","OE - NSX100-250 3P Front Hood, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 3P, W850, 3M/700, HORIZ.","OE - Első burkolat NSX100-250 3P, W850, 3M / 700, vízszintes, kar"]
["14938","OE - Osłona czołowa NSX100-250 3P, W850, 3M / 700, poziomo, silnik, obrotowy",79,"1-ZE-01",null,null,"OE_MCCB_COVERS","14938","SZT","85389099",null,"230622RT","5901988149383","OE - capot avant NSX100-250 3P, L850, 3M / 700, horizontal, moteur, rotatif","OE - NSX100-250 3P Front Hood, W850, 3M / 700, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3P  W850, 3M / 700, HORIZ., MOTOR, ","OE - Első burkolat NSX100-250 3P, W850, 3M / 700, vízszintes, motoros, forgatható"]
["14939","OE - Osłona czołowa NSX100-250 VIGI 3P, W850, 3M / 700, poziomo, dźwignia",79,"1-ZE-01",null,null,"OE_MCCB_COVERS","14939","SZT","85389099","27.12.40.0","230622RT","5901988149390","OE - capot avant NSX100-250 VIGI 3P, L850, 3M / 700, horizontal, levier","OE - Front cover NSX100-250 VIGI 3P, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 VIGI 3P, W850, 3M/700, HORIZ.","OE - Első burkolat NSX100-250 VIGI 3P, W850, 3M / 700, vízszintes, kar"]
["14940","OE - Osłona czołowa NSX100-250 3P, W850, 4M / 700, poziomo, wysuwny",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14940","SZT","85389099","27.12.40.0","230622RT","5901988149406","OE - capot avant NSX100-250 3P, L850, 4M / 700, horizontal, dĂ©brochable","OE - NSX100-250 3P, W850, 4M / 700 Front cover, Horizontal, sliding","OE- TAPA TROQ. NSX100-250 3P, W850, 4M / 700, HORIZ., DESLIZANTE","OE - Előlap NSX100-250 3P, W850, 4M / 700, vízszintes, kihúzható"]
["14941","OE - Osłona czołowa NSX100-250 4P, W850, 4M / 700, poziomo, dźwignia",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14941","SZT","85389099",null,"230622RT","5901988149413","OE - capot avant NSX100-250 4P, L850, 4M / 700, horizontal, levier","OE - NSX100-250 4P Front cover, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 4P  W850, 4M / 700, HORIZ.","OE - Első burkolat NSX100-250 4P, W850, 4M / 700, vízszintes, kar"]
["14942","OE - Osłona czołowa NSX100-250 4P, W850, 4M / 700, poziomo, silnik, obrotowy",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14942","SZT","85389099",null,"230622RT","5901988149420","OE - capot avant NSX100-250 4P, L850, 4M / 700, horizontal, moteur, rotatif","OE - NSX100-250 4P, W850, 4M / 700 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 4P, W850, 4M / 700 COFRE DELANTERO, HORIZ., MOTOR, ","OE - Első burkolat NSX100-250 4P, W850, 4M / 700, vízszintes, motoros, forgatható"]
["14943","OE - Osłona czołowa NSX100-250 VIGI 4P, W850, 4M / 700, poziomo, dźwignia",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14943","SZT","85389099",null,"230622RT","5901988149437","OE - capot avant NSX100-250 VIGI 4P, L850, 4M / 700, horizontal, levier","OE - Front cover NSX100-250 VIGI 4P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX100-250 VIGI 4P, W850, 4M/700, HORIZ.","OE - Első burkolat NSX100-250 VIGI 4P, W850, 4M / 700, vízszintes, kar"]
["14944","OE - Osłona czołowa NSX100-250 4P, W850, 5M / 700, poziomo, wysuwny",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14944","SZT","85389099",null,"230622RT","5901988149444","OE - capot avant NSX100-250 4P, L850, 5M / 700, horizontal, dĂ©brochable","OE - NSX100-250 4P Front cover, W850, 5M / 700, Horizontal, Sliding","OE- TAPA TROQ. NSX100-250 4P, W850, 5M/700, HORIZ.","OE - Előlap NSX100-250 4P, W850, 5M / 700, vízszintes, kihúzható"]
["14945","OE - Osłona czołowa 2x NSX100-250 3/4P SZR, W850, 7M / 700, blokada płytowa, pionowo, silnik",133.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14945","SZT","85389099",null,"230622RT","5901988149451","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L850, 7M / 700, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W850, 7M / 700, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W850, 7M/700, VERT. MOTOR","OE - Első burkolat 2x NSX100-250 3/4P SZR, W850, 7M / 700, lemezzár, függőleges, motor"]
["14946","OE - Osłona czołowa 2x NSX100-250 3/4P SZR, W850, 8M / 700, blokada płytowa, poziomo, silnik",139.69999999999999,"1-ZE-01",null,null,"OE_MCCB_COVERS","14946","SZT","85389099",null,"230623RT","5901988149468","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L850, 8M / 700, verrouillage de plaque, horizontal, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W850, 8M / 700, plate lock, Horizontal, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W850, 8M/700,  HORIZ., MOTOR","OE - Első burkolat 2x NSX100-250 3/4P SZR, W850, 8M / 700, lemezzár, vízszintes, motor"]
["14959","OE - Osłona czołowa 3x NSX400-630 3/4P, W850, 9M / 700, pionowo, dźwignia",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14959","SZT","85389099",null,"230623RT","5901988149598","OE - capot avant 3x NSX400-630 3 / 4P, L850, 9M / 700, vertical, levier","OE - Front cover 3x NSX400-630 3 / 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. 3X NSX400-630 3/4P, W850, 9M/700, VERT.","OE - Első burkolat 3x NSX400-630 3/4P, W850, 9M / 700, függőleges, kar"]
["14960","OE - Osłona czołowa 3x NSX400-630 3/4P, W850, 9M / 700, pionowo, silnik, obrotowy",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14960","SZT","85389099",null,"230623RT","5901988149604","OE - capot avant 3x NSX400-630 3 / 4P, L850, 9M / 700, vertical, moteur, rotatif","OE - Front cover 3x NSX400-630 3 / 4P, W850, 9M / 700, Vertical, Motor, Rotary","OE- TAPA TROQ. 3X NSX400-630 3 / 4P, W850, 9M / 700, VERT. MOTOR, ","OE - Első burkolat 3x NSX400-630 3/4P, W850, 9M / 700, függőleges, motoros, forgatható"]
["14961","OE - Osłona czołowa 3x NSX400-630 VIGI 3/4P, W850, 9M / 700, pionowo, dźwignia",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14961","SZT","85389099",null,"230623RT","5901988149611","OE - capot avant 3x NSX400-630 VIGI 3/4 P, L850, 9M / 700, vertical, levier","OE - Front cover 3x NSX400-630 VIGI 3 / 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. 3X NSX400-630 VIGI 3 / 4P, W850, 9M / 700, VERT.","OE - Első burkolat 3x NSX400-630 VIGI 3/4P, W850, 9M / 700, függőleges, kar"]
["14962","OE - Osłona czołowa NSX400-630 3P, W850, 4M / 700, poziomo, dźwignia",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14962","SZT","85389099",null,"230623RT","5901988149628","OE - capot avant NSX400-630 3P, L850, 4M / 700, horizontal, levier","OE - Front cover NSX400-630 3P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 3P  W850, 4M / 700, HORIZ.","OE - Első burkolat NSX400-630 3P, W850, 4M / 700, vízszintes, kar"]
["14963","OE - Osłona czołowa NSX400-630 3P, W850, 4M / 700, poziomo, silnik, obrotowy",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14963","SZT","85389099",null,"230623RT","5901988149635","OE - capot avant NSX400-630 3P, L850, 4M / 700, horizontal, moteur, rotatif","OE - NSX400-630 3P, W850, 4M / 700 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 3P, W850, 4M / 700, HORIZ., MOTOR, ","OE - Első burkolat NSX400-630 3P, W850, 4M / 700, vízszintes, motoros, forgatható"]
["14964","OE - Osłona czołowa NSX400-630 VIGI 3P, W850, 4M / 700, poziomo, dźwignia",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","14964","SZT","85389099",null,"230623RT","5901988149642","OE - capot avant NSX400-630 VIGI 3P, L850, 4M / 700, horizontal, levier","OE - Front cover NSX400-630 VIGI 3P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 VIGI 3P, W850, 4M/700, HORIZ.","OE - Első burkolat NSX400-630 VIGI 3P, W850, 4M / 700, vízszintes, kar"]
["14965","OE - Osłona czołowa NSX400-630 3P, W850, 6M / 700, poziomo, wysuwny, silnik",106.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","14965","SZT","85389099",null,"230623RT","5901988149659","OE - capot avant NSX400-630 3P, L850, 6M / 700, horizontal, dĂ©brochable, moteur","OE - Front cover NSX400-630 3P, W850, 6M / 700, Horizontal, Extendable, Motor","OE- TAPA TROQ. NSX400-630 3P, W850, 6M/700, HORIZ., EXTRAIBLE, MOTOR","OE - Első burkolat NSX400-630 3P, W850, 6M / 700, vízszintes, kihúzható, motor"]
["14966","OE - Osłona czołowa NSX400-630 4P, W850, 5M / 700, poziomo, dźwignia",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14966","SZT","85389099",null,"230623RT","5901988149666","OE - capot avant NSX400-630 4P, L850, 5M / 700, horizontal, levier","OE - NSX400-630 4P Front cover, W850, 5M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 4P, W850, 5M / 700, HORIZ.","OE - Első burkolat NSX400-630 4P, W850, 5M / 700, vízszintes, kar"]
["14967","OE - Osłona czołowa NSX400-630 4P, W850, 5M / 700, poziomo, silnik, obrotowy",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14967","SZT","85389099",null,"230623RT","5901988149673","OE - capot avant NSX400-630 4P, L850, 5M / 700, horizontal, moteur, rotatif","OE - NSX400-630 4P, W850, 5M / 700 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 4P, W850, 5M / 700, HORIZ., MOTOR, ","OE - Első burkolat NSX400-630 4P, W850, 5M / 700, vízszintes, motoros, forgatható"]
["14968","OE - Osłona czołowa NSX400-630 VIGI 4P, W850, 5M / 700, poziomo, dźwignia",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14968","SZT","85389099",null,"230623RT","5901988149680","OE - capot avant NSX400-630 VIGI 4P, L850, 5M / 700, horizontal, levier","OE - Front cover NSX400-630 VIGI 4P, W850, 5M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 VIGI 4P, W850, 5M/700, HORIZ.","OE - Első burkolat NSX400-630 VIGI 4P, W850, 5M / 700, vízszintes, kar"]
["14969","OE - Osłona czołowa NSX400-630 4P, W850, 7M / 700, poziomo, wysuwny, silnik",133.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14969","SZT","85389099",null,"230623RT","5901988149697","OE - capot avant NSX400-630 4P, L850, 7M / 700, horizontal, dĂ©brochable, moteur","OE - Front cover NSX400-630 4P, W850, 7M / 700, Horizontal, Extendable, Motor","OE- TAPA TROQ. NSX400-630 4P, W850, 7M/700, HORIZ., EXTENSIBLE, MOTOR","OE - Első burkolat NSX400-630 4P, W850, 7M / 700, vízszintes, kihúzható, motor"]
["14970","OE - Osłona czołowa 2x NSX400-630 3/4P SZR, W850, 9M / 700, blokada płytowa, pionowo, silnik",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","14970","SZT","85389099",null,"230623RT","5901988149703","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L850, 9M / 700, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W850, 9M / 700, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX400-630 3/4P SZR, W850, 9M/700, VERT. MOTOR","OE - Első burkolat 2x NSX400-630 3/4P SZR, W850, 9M / 700, lemezzár, függőleges, motor"]
["14971","OE - Osłona czołowa 2x NSX400-630 3/4P SZR, W850, 10M / 700, blokada płytowa, poziomo, silnik",171.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","14971","SZT","85389099",null,"230623RT","5901988149710","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L850, 10M / 700, verrouillage de plaque, horizontal, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W850, 10M / 700, plate lock, Horizontal, Motor","OE- TAPA TROQ. 2X NSX400-630 3/4P SZR, W850, 10M/700,  HORIZ., MOTOR","OE - Első burkolat 2x NSX400-630 3/4P SZR, W850, 10M / 700, lemezzár, vízszintes, motor"]
["14983","OE - Osłona czołowa NS1600 3/4P, W850, 8M / 700, pionowo, dźwignia, na stałe",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14983","SZT","85389099",null,"230623RT","5901988149833","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, vertical, levier, en permanence","OE - NS1600 3 / 4P Front Hood, W850, 8M / 700, Vertical, Lever, Fixed","OE- TAPA TROQ. NS1600 3 / 4P W850, 8M / 700, VERT. FIJO","OE - Előlap NS1600 3/4P, W850, 8M / 700, függőleges, kar, fix"]
["14984","OE - Osłona czołowa NS1600 3/4P, W850, 8M / 700, pionowo, silnik, na stałe",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14984","SZT","85389099",null,"230623RT","5901988149840","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, vertical, moteur, permanent","OE - NS1600 3 / 4P Front Hood, W850, 8M / 700, Vertical, Motor, Fixed","OE- TAPA TROQ. NS1600 3 / 4P  W850, 8M / 700, VERT. MOTOR, FIJO","OE - Első burkolat NS1600 3/4P, W850, 8M / 700, függőleges, motoros, fix"]
["14985","OE - Osłona czołowa NS1600 3/4P, W850, 8M / 700, pionowo, napęd obrotowy, na stałe",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14985","SZT","85389099",null,"230623RT","5901988149857","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, vertical, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W850, 8M / 700, Vertical, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P, W850, 8M / 700, VERT. ACCIONAMIENTO , FIJO","OE - Elülső burkolat NS1600 3/4P, W850, 8M / 700, függőleges, forgó hajtás, fix"]
["14986","OE - Osłona czołowa NS1600 3/4P, W850, 8M / 700, poziomo, dźwignia, na stałe",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14986","SZT","85389099",null,"230623RT","5901988149864","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, horizontal, levier, en permanence","OE - NS1600 3 / 4P front visor, W850, 8M / 700, Horizontal, Lever, fixed","OE- TAPA TROQ. NS1600 3/4P, W850, 8M/700, HORIZ. FIJO","OE - Előlap NS1600 3/4P, W850, 8M / 700, vízszintes, kar, fix"]
["14987","OE - Osłona czołowa NS1600 3/4P, W850, 8M / 700, poziomo, silnik, na stałe",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14987","SZT","85389099",null,"230623RT","5901988149871","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, horizontal, moteur, permanent","OE - NS1600 3 / 4P Front Shield, W850, 8M / 700, Horizontal, Motor, Fixed","OE- TAPA TROQ. NS1600 3 / 4P,  W850, 8M / 700, HORIZ. MOTOR, FIJO","OE - Első burkolat NS1600 3/4P, W850, 8M / 700, vízszintes, motoros, fix"]
["14988","OE - Osłona czołowa NS1600 3/4P, W850, 8M / 700, poziomo, napęd obrotowy, na stałe",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14988","SZT","85389099",null,"230623RT","5901988149888","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, horizontal, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W850, 8M / 700, Horizontal, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P, W850, 8M / 700, HORIZ. FIJO","OE - Előlap NS1600 3/4P, W850, 8M / 700, vízszintes, forgó hajtás, fix"]
["14989","OE - Osłona czołowa NS1600/NT16 3/4P, W850, 7M / 700, wysuwny",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","14989","SZT","85389099",null,"230623RT","5901988149895","OE - Face avant NS1600/NT16 3/4P, L850, 7M / 700, coulissant","OE - Front cover NS1600 / NT16 3 / 4P, W850, 7M / 700, withdrawable","OE- TAPA TROQ. NS1600/NT16 3/4P, W850, 7M/700, EXTRAÍBLE","OE - Előlap NS1600/NT16 3/4P, W850, 7M/700, kivehető"]
["14990","OE - Osłona czołowa NT16 3/4P, W850, 7M / 700, na stałe",143,"1-ZE-01",null,null,"OE_MCCB_COVERS","14990","SZT","85389099",null,"230623RT","5901988149901","OE - capot avant NT16 3 / 4P, L850, 7M / 700, en permanence","OE - Front cover NT16 3 / 4P, W850, 7M / 700, permanent","OE- TAPA TROQ. NT16 3/4P, W850, 7M/700, FIJA","OE - Előlap NT16 3/4P, W850, 7M / 700, állandó"]
["14991","OE - Osłona czołowa NW40 3/4P, W850, 9M / 700, pionowo, wysuwny",294.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","14991","SZT","85389099",null,"230623RT","5901988149918","OE - capot avant NW40 3 / 4P, L850, 9M / 700, vertical, dĂ©brochable","OE - NW40 3 / 4P, W850, 9M / 700 Front cover, Vertical, withdrawable","OE- TAPA TROQ. NW40 3/4P, W850, 9M/700, VERT. EXTRAÍBLE","OE - Előlap NW40 3/4P, W850, 9M / 700, függőleges, kihúzható"]
["14992","OE - Osłona czołowa NW40 3/4P, W850, 8M / 700, pionowo, na stałe",299,"1-ZE-01",null,null,"OE_ACB_COVERS","14992","SZT","85389099",null,"230623RT","5901988149925","OE - capot avant NW40 3 / 4P, L850, 8M / 700, vertical, permanent","OE - NW40 3 / 4P, W850, 8M / 700 front visor, Vertical, fixed","OE- TAPA TROQ. NW40 3/4P, W850, 8M/700, VERT. FIJO","OE - Előlap NW40 3/4P, W850, 8M / 700, függőleges, fix"]
["14993","OE - Osłona czołowa NW40b 3P, W850, 8M / 700, pionowo, na stałe",299,"1-ZE-01",null,null,"OE_ACB_COVERS","14993","SZT","85389099",null,"230623RT","5901988149932","OE - capot avant NW40b 3P, L850, 8M / 700, vertical, permanent","OE - NW40b 3P, W850, 8M / 700 Front cover, Vertical, fixed","OE- TAPA TROQ. NW40B 3P, W850, 8M/700, VERT. FIJO","OE - Előlap NW40b 3P, W850, 8M / 700, függőleges, fix"]
["15737","OE - Osłona czołowa NSX100-250 3P, W650, 3M / 500, poziomo, dźwignia+ pomiar",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","15737","SZT","85389099",null,"230623RT","5901988157371","OE - capot avant NSX100-250 3P, L650, 3M / 500, horizontal, levier + mesure","OE - Front cover NSX100-250 3P, W650, 3M / 500, Horizontal, Lever + measurement","OE- TAPA TROQ. NSX100-250 3P, W650, 3M/500, HORIZ. + MEDIDA","OE - Előlap NSX100-250 3P, W650, 3M / 500, vízszintes, kar + mérés"]
["15738","OE - Osłona czołowa NSX100-250 3P, W650, 3M / 500, poziomo, silnik+pomiar",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","15738","SZT","85389099",null,"230623RT","5901988157388","OE - capot avant NSX100-250 3P, L650, 3M / 500, horizontal, moteur + mesure","OE - Front cover NSX100-250 3P, W650, 3M / 500, Horizontal, Motor + Measurement","OE- TAPA TROQ. NSX100-250 3P, W650, 3M/500, HORIZ. + MOTOR + MEDIDA","OE - Első burkolat NSX100-250 3P, W650, 3M / 500, vízszintes, motor + mérés"]
["15741","OE - Osłona czołowa NSX100-250 4P, W650, 4M / 500, poziomo, dźwignia+pomiar",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","15741","SZT","85389099",null,"230623RT","5901988157418","OE - capot avant NSX100-250 4P, L650, 4M / 500, horizontal, levier + mesure","OE - Front cover NSX100-250 4P, W650, 4M / 500, Horizontal, Lever + measurement","OE- TAPA TROQ. NSX100-250 4P, W650, 4M/500, HORIZ. + MEDIDA","OE - Első burkolat NSX100-250 4P, W650, 4M / 500, vízszintes, kar+mérés"]
["15742","OE - Osłona czołowa NSX100-250 4P, W650, 4M / 500, poziomo, silnik+pomiar",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","15742","SZT","85389099",null,"230623RT","5901988157425","OE - capot avant NSX100-250 4P, L650, 4M / 500, horizontal, moteur + mesure","OE - Front cover NSX100-250 4P, W650, 4M / 500, Horizontal, Motor + Measurement","OE- TAPA TROQ. NSX100-250 4P, W650, 4M/500, HORIZ. + MOTOR + MEDIDA","OE - Első burkolat NSX100-250 4P, W650, 4M / 500, vízszintes, motor + mérés"]
["15762","OE - Osłona czołowa NSX400-630 3P, W650, 4M / 500, poziomo, dźwignia+motor",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","15762","SZT","85389099",null,"230623RT","5901988157623","OE - capot avant NSX400-630 3P, L650, 4M / 500, horizontal, levier + mesure","OE - Front cover NSX400-630 3P, W650, 4M / 500, Horizontal, Lever + Motor","OE- TAPA TROQ. NSX400-630 3P, W650, 4M/500, HORIZ. + MOTOR","OE - Első burkolat NSX400-630 3P, W650, 4M / 500, vízszintes, kar+motor"]
["15763","OE - Osłona czołowa NSX400-630 3P, W650, 4M / 500, poziomo, silnik+pomiar",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","15763","SZT","85389099",null,"230623RT","5901988157630","OE - capot avant NSX400-630 3P, L650, 4M / 500, horizontal, moteur + mesure","OE - Front cover NSX400-630 3P, W650, 4M / 500, Horizontal, Motor + Measurement","OE- TAPA TROQ. NSX400-630 3P, W650, 4M/500, HORIZ. + MOTOR + MEDIDA","OE - Első burkolat NSX400-630 3P, W650, 4M / 500, vízszintes, motor + mérés"]
["15766","OE - Osłona czołowa NSX400-630 4P, W650, 5M / 500, poziomo, dźwignia+pomiar",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","15766","SZT","85389099",null,"230623RT","5901988157661","OE - capot avant NSX400-630 4P, L650, 5M / 500, horizontal, levier + mesure","OE - Front cover NSX400-630 4P, W650, 5M / 500, Horizontal, Lever + measurement","OE- TAPA TROQ. NSX400-630 4P, W650, 5M/500, HORIZ. + MEDIDA","OE - Első burkolat NSX400-630 4P, W650, 5M / 500, vízszintes, kar+mérés"]
["15767","OE - Osłona czołowa NSX400-630 4P, W650, 5M / 500, poziomo, motor+pomiar",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","15767","SZT","85389099",null,"230623RT","5901988157678","OE - capot avant NSX400-630 4P, L650, 5M / 500, horizontal, moteur + mesure","OE - Front cover NSX400-630 4P, W650, 5M / 500, Horizontal, Motor + measurement","OE- TAPA TROQ. NSX400-630 4P, W650, 5M/500, HORIZ. + MOTOR + MEDIDA","OE - Előlap NSX400-630 4P, W650, 5M / 500, vízszintes, motor + mérés"]
["15786","OE - Osłona czołowa dla NSb i analizatora 92x92mm W650, 7M / 500",139.19999999999999,"1-ZE-01",null,null,"OE_ACB_COVERS","15786","SZT","85389099",null,"230623RT","5901988357863","OE - capot avant pour analyseur NSb et 92x92mm L650, 7M / 500","OE - Front cover for NSb and 92x92mm W650, 7M / 500 analyzer","OE- TAPA TROQ. PARA ANALIZADOR NSB Y 92X92MM W650, 7M/500","OE - Elülső burkolat NSb-hez és analizátorhoz 92x92mm W650, 7M / 500"]
["16460","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 160A, W400, 6M / 250, pionowo",60,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16460","SZT","85389099",null,"230623RT","5901988164607","OE - interrupteur-couvercle-sectionneur EFEN 160, L400, 6M, vertical","OE - Cover EFEN NT-IN 160A, W400, 6M / 250, Vertical","OE- TAPA, CAJA DE CONEXIONES EFEN NT-IN 160A, W400, 6M/250, VERT.","OE - EFEN NT-IN 160A, W400, 6M / 250, függőleges szakaszolódoboz burkolata"]
["16550","OE - Osłona rozłącznik skrzynkowy 2x EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, pionowo",57.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16550","SZT","85389099",null,"230623RT","5901988165505","OE - Déconnecteur 2x EFEN 100, L450, 6M, verticalement","OE - Cover box switch box 2x EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, Vertical","OE- CAJA TAPA CAJA INTERRUPTOR 2X EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, VERT.","OE - fedél a szakaszolódobozhoz 2x EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, függőleges"]
["16560","OE - Osłona rozłącznik skrzynkowy 2x EFEN NT-IN 160A, W450, 6M / 300, pionowo",62.9,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16560","SZT","85389099",null,"230623RT","5901988165604","OE - Déconnecteur 2x EFEN 160, L450, 6M, verticalement","OE - Cover box switch box 2x EFEN NT-IN 160A, W450, 6M / 300, Vertical","OE- TAPA BASE PORTAFUSIBLES  2X160, W450, 6M, VERT.","OE - Szakaszoló fedél 2x EFEN NT-IN 160A, W450, 6M / 300, függőleges"]
["16570","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 250A, W450, 9M / 300, pionowo",83.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16570","SZT","85389099",null,"230623RT","5901988165703","OE - Sectionneur de couvercle EFEN 250, L450, 9M, vertical","OE - Cover EFEN NT-IN 250A, W450, 9M / 300 switch box, Vertical","OE- TAPA BASE PORTAFUSIBLES 250, W450, 9M, VERT.","OE - EFEN NT-IN 250A, W450, 9M / 300, függőleges szakaszolódoboz burkolata"]
["16580","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 400A, W450, 9M / 300, pionowo",83.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16580","SZT","85389099",null,"230623RT","5901988165802","OE - Couvercle de disjoncteur EFEN NT-IN 400A, L450, 9M / 300, vertical","OE - Cover EFEN NT-IN 400A, W450, 9M / 300 switch box, Vertical","OE- TAPA, CAJA DE CONEXIONES EFEN NT-IN 400A, W450, 9M/300, VERT.","OE - EFEN NT-IN 400A, W450, 9M / 300, függőleges szakaszolódoboz burkolata"]
["16650","OE - Osłona rozłącznik skrzynkowy 5x EFEN NT-IN; SCHN LV4 100A, W650, 6M / 500, pionowo",85.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16650","SZT","85389099","27.12.40.0","230623RT","5901988166502","OE - Sectionneur de boîte de recouvrement 5x EFEN 100, L650, 6M, verticalement","OE - Shield switch box 5x EFEN NT-IN; SCHN LV4 100A, W650, 6M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  5X100, W650, 6M, VERT.","OE - Fedele a szakaszolódobozhoz 5x EFEN NT-IN; SCHN LV4 100A, W650, 6M / 500, függőleges"]
["16660","OE - Osłona rozłącznik skrzynkowy 4x EFEN NT-IN 160A, W650, 6M / 500, pionowo",81.2,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16660","SZT","85389099","27.12.40.0","230623RT","5901988166601","OE - Déconnecteur 4x EFEN 160, L650, 6M, verticalement","OE - Cover, switch box 4x EFEN NT-IN 160A, W650, 6M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  4X160, W650, 6M, VERT.","OE - szakaszoló fedél 4x EFEN NT-IN 160A, W650, 6M / 500, függőleges"]
["16661","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 160A + ochronnik, W650, 3M / 500, poziomo",69.900000000000006,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16661","SZT","85389099","27.12.40.0","230623RT","5901988166618","OE - Couvercle de disjoncteur EFEN NT-IN 160A + protecteur, L650, 3M / 500, horizontal","OE - Cover EFEN NT-IN 160A switch disconnector + arrester, W650, 3M / 500, Horizontal","OE- TAPA EFEN NT-IN 160A SECCIONADOR + DESCARGADOR, W650, 3M/500, HORIZ.","OE - EFEN NT-IN 160A doboz leválasztó kapcsoló fedél + védő, W650, 3M / 500, vízszintes"]
["16662","OE - Osłona rozłącznik skrzynkowy EFEN SILAS; SCHN LV4 160A + ochronnik, W650, 3M / 500, poziomo",69.900000000000006,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16662","SZT","85389099","27.12.40.0","230623RT","5901988166625","OE - Couvercle pour interrupteurs-sectionneurs EFEN SILAS ; SCHN LV4 160A + protecteur, L650, 3M / 500, horizontal","OE - Cover EFEN SILAS switch box; SCHN LV4 160A + arrester, W650, 3M / 500, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 160A + LIMITADOR SOBRET. W650, 3M/500, HORIZ.","OE - EFEN SILAS doboz megszakító kapcsoló fedele; SCHN LV4 160A + levezető, W650, 3M / 500, vízszintes"]
["16665","OE - Osłona rozłącznik skrzynkowy 4x EFEN SILAS; SCHN LV4 160A, W650, 6M / 500, pionowo",81.2,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16665","SZT","85389099","27.12.40.0","230623RT","5901988166656","OE - Déconnecteur 4x EFEN SILAS 160, L650, 6M, verticalement","OE - Cover, switch box 4x EFEN SILAS; SCHN LV4 160A, W650, 6M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  4XSILAS 160, W650, 6M, VERT.","OE - Fedele a szakaszolódobozhoz 4x EFEN SILAS; SCHN LV4 160A, W650, 6M / 500, függőleges"]
["16670","OE - Osłona rozłącznik skrzynkowy 2x EFEN NT-IN 250A, W650, 9M / 500, pionowo",109.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16670","SZT","85389099",null,"230623RT","5901988166700","OE - Sectionneur de protection 2x EFEN 250, L650, 9M, verticalement","OE - Cover box switch box 2x EFEN NT-IN 250A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2X250, W650, 9M, VERT.","OE - Szakaszoló fedél 2x EFEN NT-IN 250A, W650, 9M / 500, függőleges"]
["16671","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 250A + ochronnik, W650, 5M / 500, poziomo",69.900000000000006,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16671","SZT","85389099",null,"230623RT","5901988166717","OE - Couvercle de disjoncteur EFEN NT-IN 250A + protection, L650, 5M / 500, horizontal","OE - Cover EFEN NT-IN 250A switch disconnector + arrester, W650, 5M / 500, Horizontal","OE- TAPA SECCIONADOR EFEN NT-IN 250A + LIMITADOR SOBRET. W650, 5M/500, HORIZ.","OE - EFEN NT-IN 250A doboz leválasztó kapcsoló fedél + védő, W650, 5M / 500, vízszintes"]
["16672","OE - Osłona rozłącznik skrzynkowy EFEN SILAS; SCHN LV4 250A, W650, 5M / 500, poziomo",69.900000000000006,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16672","SZT","85389099",null,"230623RT","5901988166724","OE - Couvercle pour interrupteurs-sectionneurs EFEN SILAS ; SCHN LV4 250A, L650, 5M / 500, horizontal","OE - Cover EFEN SILAS switch box; SCHN LV4 250A, W650, 5M / 500, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 250A, W650, 5M / 500, HORIZ.","OE - EFEN SILAS doboz megszakító kapcsoló fedele; SCHN LV4 250A, W650, 5M / 500, vízszintes"]
["16675","OE - Osłona rozłącznik skrzynkowy 2x EFEN SILAS; SCHN LV4 250A, W650, 9M / 500, pionowo",109.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16675","SZT","85389099",null,"230623RT","5901988166755","OE - Boîte de dérivation 2x EFEN SILAS 250, L650, 9M, à la verticale","OE - Cover, switch box 2x EFEN SILAS; SCHN LV4 250A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2XSILAS 250, W650, 9M, VERT.","OE - fedél a szakaszolódobozhoz 2x EFEN SILAS; SCHN LV4 250A, W650, 9M / 500, függőleges"]
["16680","OE - Osłona rozłącznik skrzynkowy 2x EFEN NT-IN 400A, W650, 9M / 500, pionowo",109.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16680","SZT","8538909900",null,"230623RT","5901988166809","OE - Déconnecteur 2x EFEN 400, L650, 9M, verticalement","OE - Cover box switch box 2x EFEN NT-IN 400A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2X400, W650, 9M, VERT.","OE - fedél kapcsolódobozhoz 2x EFEN NT-IN 400A, W650, 9M / 500, függőleges"]
["16681","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 400A, W650, 5M / 500, poziomo",69.900000000000006,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16681","SZT","85389099",null,"230623RT","5901988166816","OE - Couvercle pour interrupteurs-sectionneurs EFEN NT-IN 400A, L650, 5M / 500, horizontal","OE - Cover EFEN NT-IN 400A, W650, 5M / 500, Horizontal switch disconnector","OE- TAPA, CAJA DE CONEXIONES EFEN NT-IN 400A, W650, 5M / 500, HORIZ.","OE - EFEN NT-IN 400A, W650, 5M / 500, vízszintes szakaszolódoboz fedele"]
["16683","OE - Osłona rozłącznik listwowy 9x EFEN 160, W650, 11M / 500, rozstaw szyn 100mm",116.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16683","SZT","85389099","27.12.40.0","230623RT","5901988166830","OE - Interrupteur-cache-contacteur 9x EFEN 160, L650, 11M, écartement de voie 100mm","OE - Cover rail switch disconnector 9x EFEN 160, W650, 11M / 500, bar spacing 100mm","OE- TAPA BASE FUSIBLES 9X160, W650, 11M, SEPARACION BARRAS  100MM","OE - Fedél a szalagos megszakítóhoz 9x EFEN 160, W650, 11M / 500, gyűjtősín távolság 100 mm"]
["16684","OE - Osłona rozłącznik skrzynkowy EFEN SILAS; SCHN LV4 400A, W650, 5M / 500, poziomo",69.900000000000006,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16684","SZT","85389099",null,"230623RT","5901988166847","OE - Couvercle pour interrupteurs-sectionneurs EFEN SILAS ; SCHN LV4 400A, L650, 5M / 500, horizontal","OE - Cover EFEN SILAS switch box; SCHN LV4 400A, W650, 5M / 500, Horizontal","OE- TAPA BASE PORTAFUSIBLES 250 + PROTECC. W650, 5M, HORIZ.","OE - EFEN SILAS doboz megszakító kapcsoló fedele; SCHN LV4 400A, W650, 5M / 500, vízszintes"]
["16685","OE - Osłona rozłącznik skrzynkowy 2x EFEN SILAS; SCHN LV4 400A, W650, 9M / 500, pionowo",109.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16685","SZT","85389099","27.12.40.0","230623RT","5901988166854","OE - Boîte de dérivation 2x EFEN SILAS 400, L650, 9M, à la verticale","OE - Cover, switch box 2x EFEN SILAS; SCHN LV4 400A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2XSILAS 400, W650, 9M, VERT.","OE - fedél a szakaszolódobozhoz 2x EFEN SILAS; SCHN LV4 400A, W650, 9M / 500, függőleges"]
["16690","OE - Osłona rozłącznik skrzynkowy 1x EFEN NT-IN 630A, W650, 9M / 500, pionowo",116.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16690","SZT","85389099",null,"230623RT","5901988166908","OE - Déconnecteur 1x EFEN 630, L650, 9M, verticalement","OE - Cover, switch box 1x EFEN NT-IN 630A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  1X630, W650, 9M, VERT.","OE - szakaszoló fedél 1x EFEN NT-IN 630A, W650, 9M / 500, függőleges"]
["16691","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 630A, W650, 6M / 500, poziomo",81.2,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16691","SZT","85389099","27.90.12.0","230623RT","5901988166915","OE - Couvercle pour interrupteurs-sectionneurs EFEN NT-IN 630A, L650, 6M / 500, horizontal","OE - Cover EFEN NT-IN 630A, W650, 6M / 500 switch box, Horizontal","OE- TAPA EFEN NT-IN 630A, W650, 6M/500, SECCIONADOR HORIZ.","OE - EFEN NT-IN 630A, W650, 6M / 500, vízszintes szakaszolódoboz fedele"]
["16694","OE - Osłona rozłącznik skrzynkowy EFEN SILAS; SCHN LV4 630A, W650, 6M / 500, poziomo",81.2,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16694","SZT","85389099","27.90.12.0","230623RT","5901988166946","OE - Couvercle pour interrupteurs-sectionneurs EFEN SILAS ; SCHN LV4 630A, L650, 6M / 500, horizontal","OE - Cover EFEN SILAS switch box; SCHN LV4 630A, W650, 6M / 500, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 630A, W650, 6M / 500, HORIZ.","OE - EFEN SILAS doboz megszakító kapcsoló fedele; SCHN LV4 630A, W650, 6M / 500, vízszintes"]
["16695","OE - Osłona rozłącznik skrzynkowy 1x EFEN SILAS; SCHN LV4 630A, W650, 9M / 500, pionowo",116.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16695","SZT","85389099",null,"230623RT","5901988166953","OE - Couvercle interrupteur-sectionneur 1x EFEN SILAS ; SCHN LV4 630A, L650, 9M / 500, vertical","OE - Cover box switch box 1x EFEN SILAS; SCHN LV4 630A, W650, 9M / 500, Vertical","OE- CAJA TAPA CAJA DE INTERRUPTORES 1X EFEN SILAS; SCHN LV4 630A, W650, 9M / 500, VERT.","OE - fedél a szakaszolódobozhoz 1x EFEN SILAS; SCHN LV4 630A, W650, 9M / 500, függőleges"]
["16950","OE - Osłona rozłącznik skrzynkowy 7x EFEN NT-IN; SCHN LV4 100A, W850, 6M / 700, pionowo",97.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16950","SZT","85389099",null,"230623RT","5901988169503","OE - Sectionneur de boîte de protection 7x EFEN 100, L850, 6M, verticalement","OE - Cover box switch disconnector 7x EFEN NT-IN; SCHN LV4 100A, W850, 6M / 700, Vertical","OE- TAPA BASE PORTAFUSIBLES  7X100, W850, 6M, VERT.","OE - Fedele a szakaszolódobozhoz 7x EFEN NT-IN; SCHN LV4 100A, W850, 6M / 700, függőleges"]
["16960","OE - Osłona rozłącznik skrzynkowy 6x EFEN NT-IN 160A, W850, 6M / 700, pionowo",97.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16960","SZT","85389099",null,"230623RT","5901988169602","OE - Sectionneur de boîte de protection 6x EFEN 160, L850, 6M, vertical","OE - Cover, switch box 6x EFEN NT-IN 160A, W850, 6M / 700, Vertical","OE- TAPA BASE PORTAFUSIBLES  6X160, W850, 6M, VERT.","OE - fedél a szakaszolódobozhoz 6x EFEN NT-IN 160A, W850, 6M / 700, függőleges"]
["16961","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 160A + ochronnik, W850, 3M / 700, poziomo",75.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16961","SZT","85389099",null,"230623RT","5901988169619","OE - Couvercle interrupteur-sectionneur EFEN 160 + protecteur, L850, 3M, horizontalement","OE - Cover EFEN NT-IN 160A switch disconnector + arrester, W850, 3M / 700, Horizontal","OE- TAPA EFEN NT-IN 160A SECCIONADOR + DESCARGADOR, W850, 3M/700, HORIZ.","OE - EFEN NT-IN 160A doboz leválasztó kapcsoló fedél + védő, W850, 3M / 700, vízszintes"]
["16962","OE - Osłona rozłącznik skrzynkowy EFEN SILAS; SCHN LV4 160A + ochronnik, W850, 3M / 700, poziomo",75.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16962","SZT","8538909900",null,"230623RT","5901988169626","OE - Couvercle interrupteur-sectionneur EFEN SILAS ; SCHN LV4 160A + protecteur, L850, 3M / 700, horizontalement","OE - Cover EFEN SILAS switch box; SCHN LV4 160A + arrester, W850, 3M / 700, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 160A + LIMITADOR SOBRET. W850, 3M/700, HORIZ.","OE - EFEN SILAS doboz megszakító kapcsoló fedele; SCHN LV4 160A + levezető, W850, 3M / 700, vízszintes"]
["16965","OE - Osłona rozłącznik skrzynkowy 6x EFEN SILAS; SCHN LV4 160A, W850, 6M / 700, pionowo",97.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16965","SZT","85389099",null,"230623RT","5901988169657","OE - Couvercle interrupteur-sectionneur 6x EFEN SILAS ; SCHN LV4 160A, L850, 6M / 700, vertical","OE - Cover, switch box 6x EFEN SILAS; SCHN LV4 160A, W850, 6M / 700, Vertical","OE- TAPA, CAJA DE INTERRUPTORES 6X EDEN SILAS; SCHN LV4 160A, W850, 6M / 700, VERT.","OE - fedél a szakaszolódobozhoz 6x EFEN SILAS; SCHN LV4 160A, W850, 6M / 700, függőleges"]
["16970","OE - Osłona rozłącznik skrzynkowy 3x EFEN NT-IN 250A, W850, 9M / 700, pionowo",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16970","SZT","85389099",null,"230623RT","5901988169701","OE - Sectionneur de boîte de recouvrement 3x EFEN 250, L850, 9M, vertical","OE - Cover, switch box 3x EFEN NT-IN 250A, W850, 9M / 700, Vertical","OE- TAPA BASE PORTAFUSIBLES  3X250, W850, 9M, VERT.","OE - fedél a szakaszolódobozhoz 3x EFEN NT-IN 250A, W850, 9M / 700, függőleges"]
["16971","OE - Osłona rozłącznik skrzynkowy EFEN NT-IN 250A + ochronnik, W850, 5M / 700, poziomo",91.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16971","SZT","85389099",null,"230623RT","5901988169718","OE - Couvercle interrupteur-sectionneur EFEN 250 + protecteur, L850, 5M, horizontalement","OE - Cover EFEN NT-IN 250A switch disconnector + arrester, W850, 5M / 700, Horizontal","OE- TAPA, CAJA DE CONEXIONES EFEN NT-IN 250A + LIMITADOR SOBRET. W850, 5M / 700, HORIZ.","OE - EFEN NT-IN 250A doboz leválasztó kapcsoló fedél + védő, W850, 5M / 700, vízszintes"]
["16975","OE - Osłona rozłącznik skrzynkowy 3x EFEN SILAS; SCHN LV4 250A, W850, 9M / 700, pionowo",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16975","SZT","85389099",null,"230623RT","5901988169756","OE - Couvercle interrupteur-sectionneur 3x EFEN SILAS ; SCHN LV4 250A, L850, 9M / 700, vertical","OE - Cover box switch disconnector 3x EFEN SILAS; SCHN LV4 250A, W850, 9M / 700, Vertical","OE- CAJA TAPA SECCIONADOR 3X FEEN SILAS; SCHN LV4 250A, W850, 9M / 700, VERT.","OE - Fedele a szakaszolódobozhoz 3x EFEN SILAS; SCHN LV4 250A, W850, 9M / 700, függőleges"]
["16980","OE - Osłona rozłącznik skrzynkowy 3x EFEN NT-IN 400A, W850, 9M / 700, pionowo",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16980","SZT","85389099",null,"230623RT","5901988169800","OE - Sectionneur de boîte de recouvrement 3x EFEN 250, L850, 9M, vertical","OE - Cover, switch box 3x EFEN NT-IN 400A, W850, 9M / 700, Vertical","OE- TAPA BASE PORTAFUSIBLES  3X250, W850, 9M, VERT.","OE - fedél a szakaszolódobozhoz 3x EFEN NT-IN 400A, W850, 9M / 700, függőleges"]
["16983","OE - Osłona rozłącznik listwowy 13x EFEN 160, W850, 11M / 700, rozstaw szyn 100mm",137.19999999999999,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16983","SZT","85389099",null,"230623RT","5901988169831","OE - Interrupteur-cache couvercle 13x EFEN 160, L850, 11M, écartement de voie 100mm","OE - Cover rail switch disconnector 13x EFEN 160, W850, 11M / 700, busbar spacing 100mm","OE- TAPA BASE FUSIBLES 13X160, W850, 11M, SEPARACION BARRAS  100MM","OE - 13x EFEN 160, W850, 11M / 700 szalagos leválasztó kapcsoló burkolata, gyűjtősín távolság 100 mm"]
["16985","OE - Osłona rozłącznik skrzynkowy 3x EFEN SILAS; SCHN LV4 400A, W850, 9M / 700, pionowo",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16985","SZT","85389099",null,"230623RT","5901988169855","OE - Couvercle interrupteur-sectionneur 3x EFEN SILAS ; SCHN LV4 400A, L850, 9M / 700, vertical","OE - Cover box switch disconnector 3x EFEN SILAS; SCHN LV4 400A, W850, 9M / 700, Vertical","OE- CAJA TAPA SECCIONADOR 3X FEEN SILAS; SCHN LV4 400A, W850, 9M / 700, VERT.","OE - Fedele a szakaszolódobozhoz 3x EFEN SILAS; SCHN LV4 400A, W850, 9M / 700, függőleges"]
["16990","OE - Osłona rozłącznik skrzynkowy 2x EFEN NT-IN 630A, W850, 9M / 700, pionowo",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16990","SZT","85389099",null,"230623RT","5901988169909","OE - Couvercle interrupteur-sectionneur 2x EFEN 630, L850, 9M, verticalement","OE - Cover box switch box 2x EFEN NT-IN 630A, W850, 9M / 700, Vertical","OE- TAPA BASE PORTAFUSIBLES  2X630, W850, 9M, VERT.","OE - Szakaszoló fedél 2x EFEN NT-IN 630A, W850, 9M / 700, függőleges"]
["16994","OE - Osłona rozłącznik skrzynkowy EFEN SILAS; SCHN LV4 630A, W850, 6M / 700, poziomo",97.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16994","SZT","85389099",null,"230623RT","5901988169947","OE - Couvercle interrupteur-sectionneur EFEN SILAS ; SCHN LV4 630A, L850, 6M / 700, horizontalement","OE - Cover EFEN SILAS switch box; SCHN LV4 630A, W850, 6M / 700, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 630A, W850, 6M / 700, HORIZ.","OE - EFEN SILAS doboz megszakító kapcsoló fedele; SCHN LV4 630A, W850, 6M / 700, vízszintes"]
["16995","OE - Osłona rozłącznik skrzynkowy 2x EFEN SILAS; SCHN LV4 630A, W850, 9M / 700, pionowo",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","16995","SZT","85389099",null,"230623RT","5901988169954","OE - Couvercle interrupteur-sectionneur 2x EFEN SILAS ; SCHN LV4 630A, L850, 9M / 700, vertical","OE - Cover, switch box 2x EFEN SILAS; SCHN LV4 630A, W850, 9M / 700, Vertical","OE- CAJA TAPA CAJA INTERRUPTOR 2X FEEN SILAS; SCHN LV4 630A, W850, 9M / 700, VERT.","OE - fedél a szakaszolódobozhoz 2x EFEN SILAS; SCHN LV4 630A, W850, 9M / 700, függőleges"]
["17065","Zenergy MCC - Poprzeczka ramy MCC W650",460,"1-ZE-01",0.85833333333333328,1,"OE_MCC","17065","SZT","85389099",null,null,"5901988170653","MCC - Barre transversale du cadre L650","MCC - Crossbar of the MCC W650 frame","MCC - TRAVESA?O DEL CUADRO MCC W650","Zenergy MCC - MCC W650 keret kereszttartó"]
["17066","Zenergy MCC - Poprzeczka ramy do drzwi MCC W650",163.30000000000001,"1-ZE-01",null,null,"OE_MCC","17066","SZT","85389099",null,null,"5901988170660","MCC - Traverse pour le cadre de porte L650","MCC - Crossbar for the MCC W650 door frame","MCC - TRAVESA?O PARA PUERTA MCC W650","Zenergy MCC - Keretkeresztrúd MCC W650 ajtókhoz"]
["17165","Zenergy MCC - Listwy maskujące zabudowe do osłon czołowych W650",52.1,"1-ZE-01",null,null,"OE_MCC","17165","SZT","85389099",null,null,"5901988171650","MCC - Bandes de protection dissimulées pour couvertures avant L650","MCC - Covering strips for the W650 Front covers","MCC - TIRAS DE COBERTURA PARA LAS CUBIERTAS FRONTALES W650","Zenergy MCC - Takarócsíkok W650 előlapokhoz"]
["17203","Zenergy MCC - Drzwi pełne IP40, 3 mod, H150 x W650",126.5,"1-ZE-03",null,null,"OE_MCC","17203","SZT","85389099",null,"190118LK","5901988172039","MCC - Porte pleine IP40, 3MOD H150 x L650","MCC - Full door IP40, 3 mod, H150 x W650","MCC - PUERTA OPACA IP40, 3 MOD, H150 x W650","Zenergy MCC - Teljes ajtó IP40, 3 mód, H150 x W650"]
["17204","Zenergy MCC - Drzwi pełne IP40, 4 mod, H200 x W650",133.4,"1-ZE-03",null,null,"OE_MCC","17204","SZT","85389099",null,"190118LK","5901988172046","MCC - Porte pleine IP40, 4MOD H200 x L650","MCC - Plain door IP40, 4 mod, H200 x W650","MCC - PUERTA OPACA IP40, 4 MOD, H200 x W650","Zenergy MCC - Teljes ajtó IP40, 4 mód, H200 x W650"]
["17205","Zenergy MCC - Drzwi pełne IP40, 5 mod, H250 x W650",149.5,"1-ZE-03",null,null,"OE_MCC","17205","SZT","85389099",null,"190118LK","5901988172053","MCC - Porte pleine IP40, 5MOD H250 x L650","MCC - Full door IP40, 5 mod, H250 x W650","MCC - PUERTA OPACA IP40, 5 MOD, H250 x W650","Zenergy MCC - Teljes ajtó IP40, 5 mód, H250 x W650"]
["17206","Zenergy MCC - Drzwi pełne IP40, 6 mod, H300 x W650",151.80000000000001,"1-ZE-03",null,null,"OE_MCC","17206","SZT","85389099",null,"190118LK","5901988172060","MCC - Porte pleine IP40, 6MOD H300 x L650","MCC - Full door IP40, 6 mod, H300 x W650","MCC - PUERTA OPACA IP40, 6 MOD, H300 x W650","Zenergy MCC - Teljes ajtó IP40, 6 mód, H300 x W650"]
["17207","Zenergy MCC - Drzwi pełne IP40, 7 mod, H350 x W650",151.80000000000001,"1-ZE-03",null,null,"OE_MCC","17207","SZT","85389099",null,"190118LK","5901988172077","MCC - Porte pleine IP40, 7MOD H350 x L650","MCC - Full door IP40, 7 mod, H350 x W650","MCC - PUERTA OPACA IP40, 7 MOD, H350 x W650","Zenergy MCC - Teljes ajtó IP40, 7 mód, H350 x W650"]
["17208","Zenergy MCC - Drzwi pełne IP40, 8 mod, H400 x W650",155.30000000000001,"1-ZE-03",null,null,"OE_MCC","17208","SZT","85389099",null,"190118LK","5901988172084","MCC - Porte pleine IP40, 8MOD H400 x L650","MCC - Full door IP40, 8 mod, H400 x W650","MCC - PUERTA OPACA IP40, 8 MOD, H400 x W650","Zenergy MCC - Teljes ajtó IP40, 8 mód, H400 x W650"]
["17209","Zenergy MCC - Drzwi pełne IP40, 9 mod, H450 x W650",156.4,"1-ZE-03",null,null,"OE_MCC","17209","SZT","85389099",null,"190118LK","5901988172091","MCC - Porte pleine IP40, 9MOD H450 x L650","MCC - Plain door IP40, 9 mod, H450 x W650","MCC - PUERTA OPACA IP40, 9 MOD, H450 x W650","Zenergy MCC - Teljes ajtó IP40, 9 mód, H450 x W650"]
["17210","Zenergy MCC - Drzwi pełne IP40, 10 mod, H500 x W650",169.1,"1-ZE-03",null,null,"OE_MCC","17210","SZT","85389099",null,"190118LK","5901988172107","MCC - Porte pleine IP40, 10MOD H500 x L650","MCC - Full door IP40, 10 mod, H500 x W650","MCC - PUERTA OPACA IP40, 10 MOD, H500 x W650","Zenergy MCC - Teljes ajtó IP40, 10 mod, H500 x W650"]
["17212","Zenergy MCC - Drzwi pełne IP40, 12 mod, H600 x W650",182.9,"1-ZE-03",null,null,"OE_MCC","17212","SZT","85389099",null,"190118LK","5901988172121","MCC - Porte pleine IP40, 12MOD H600 x L650","MCC - Full door IP40, 12 mod, H600 x W650","MCC - PUERTA OPACA IP40, 12 MOD, H600 x W650","Zenergy MCC - Teljes ajtó IP40, 12 mód, H600 x W650"]
["17213","Zenergy MCC - Drzwi pełne IP40, 13 mod, H650 x W650",188.6,"1-ZE-03",null,null,"OE_MCC","17213","SZT","85389099",null,"190118LK","5901988172138","MCC - Porte pleine IP40, 13MOD H650 x L650","MCC - Full door IP40, 13 mod, H650 x W650","MCC - PUERTA OPACA IP40, 13 MOD, H650 x W650","Zenergy MCC - Teljes ajtó IP40, 13 mod, H650 x W650"]
["17215","Zenergy MCC - Drzwi pełne IP40, 15 mod, H750 x W650",208.2,"1-ZE-03",null,null,"OE_MCC","17215","SZT","85389099",null,"190118LK","5901988172152","MCC - Porte pleine IP40, 14MOD H750 x L650","MCC - Full door IP40, 15 mod, H750 x W650","MCC - PUERTA OPACA IP40, 15 MOD, H750 x W650","Zenergy MCC - Teljes ajtó IP40, 15 mod, H750 x W650"]
["17218","Zenergy MCC - Drzwi pełne IP40, 18 mod, H900 x W650",234.6,"1-ZE-03",null,null,"OE_MCC","17218","SZT","85389099",null,"190118LK","5901988172183","MCC - Porte pleine IP40, 18MOD H900 x L650","MCC - Full door IP40, 18 mod, H900 x W650","MCC - PUERTA OPACA IP40, 18 MOD, H900 x W650","Zenergy MCC - Teljes ajtó IP40, 18 mod, H900 x W650"]
["17220","Zenergy MCC - Drzwi pełne IP40, 20 mod, H1000 x W650",261.10000000000002,"1-ZE-03",null,null,"OE_MCC","17220","SZT","85389099",null,"190118LK","5901988172206","MCC - Porte pleine IP40, 20MOD H1000 x L650","MCC - Full door IP40, 18 mod, H1000 x W650","MCC - PUERTA OPACA IP40, 18 MOD, H1000 x W650","Zenergy MCC - Teljes ajtó IP40, 20 mod, H1000 x W650"]
["17263","Zenergy MCC - Kaseta 3P 12M W650, napęd obrotowy MCCB 2x630A",5400,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988172633"]
["17271","Zenergy MCC - Listwa zawiasów MCC H2200",117.3,"1-ZE-01",null,null,"OE_MCC","17271","SZT","85389099",null,"191002LK","5901988172718","MCC - Bande de charnière MCC H2000","MCC - MCC H2200 hinge bar","MCC - Barra de bisagra H2200 (OBSOLETO)","Zenergy MCC - MCC H2200 zsanércsík"]
["17272","Zenergy MCC - Listwa zawiasów MCC H2000",104.2,"1-ZE-01",null,null,"OE_MCC","17272","SZT","85389099",null,"191002LK","5901988172725","MCC - Bande de charnière MCC H2000","MCC - MCC H2000 hinge bar","MCC - Barra de bisagra H2000 (OBSOLETO)","Zenergy MCC - MCC H2000 zsanércsík"]
["17273","Zenergy MCC - Obudowa mostu pionowego 3P MCC H2000",2001,"1-ZE-01",8.3333333333333329E-2,1,"OE_MCC","17273","SZT","85389099",null,null,"5901988172732","MCC - Boîtier de jeu de barres vertical 3P MCC H2000","MCC - 3P MCC H2000 Vertical bridge housing","MCC - CARCASA DE PUENTE VERT. 3P H2000","Zenergy MCC - 3P MCC H2000 függőleges hídház"]
["17274","Zenergy MCC - Obudowa mostu pionowego 4P MCC H2000",2277,"1-ZE-01",null,null,"OE_MCC","17274","SZT","85389099",null,null,"5901988172749","MCC - Boîtier de jeu de barres vertical 4P MCC H2000","MCC - 4P MCC H2000 Vertical bridge housing","MCC - CARCASA DE PUENTE VERT. 4P H2000","Zenergy MCC - Hídburkolatfüggőleges 4P MCC H2000"]
["17275","Zenergy MCC - 100MM KRATOWNICA IP20 - 3P ŻALUZJA SZYN TYLNYCH PIONOWYCH",13.7,"1-ZE-01",2.9666666666666668,1,"OE_MCC",null,"SZT","85469010",null,null,"5901988172756","MCC - Obturateur de rail vertical 100P Truss IP20 - 3P","MCC - 100mm IP20 grating - 3P rear Vertical rail shutter","MCC- Rejilla 100mm IP20 - Persiana riel VERT. posterior 3P","Zenergy MCC - 100mm IP20 RÁCS - 3P HÁTSÓ FÜGGŐLEGES SÍN SZERETŐK"]
["17277","Zenergy MCC - Obudowa mostu pionowego 3P MCC H2000",1728,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988172770"]
["17278","Zenergy MCC - Obudowa mostu pionowego 4P MCC H2000",1965.6,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988172787"]
["17360","Zenergy MCC - Część stała wtykowa 3P 3M W650",695.8,"1-ZE-01",null,null,"OE_MCC","17360","SZT","85389099",null,"200604LK","5901988173609","MCC - Partie fixe enfichable 3P 3M L650","MCC - Fixed plug-in part 3P 3M W650","MCC - PIEZA ENCHUFABLE FIJA 3P 3M W650","Zenergy MCC - Fix plug-in alkatrész 3P 3M W650"]
["17361","Zenergy MCC - Płyta wtykowa 400-630A 3P 3M W650",885.5,"1-ZE-01",null,null,"OE_MCC","17361","SZT","85389099",null,"200604LK","5901988173616","MCC - Étagère enfichable 100-250A 3P 3M L650","MCC - Plug-in board 100-250A 3P 3M W650","MCC - PLACA ENCHUFABLE 100-250A 3P 3M W650","Zenergy MCC - Plug-in kártya 400-630A 3P 3M W650"]
["17362","Zenergy MCC - Część stała kasetowa 3P 3M W650",1380,"1-ZE-01",0.31666666666666665,1,"OE_MCC","17362","SZT","85389099",null,"200604LK","5901988173623","MCC - Partie fixe de la cassette 3P 3M L650","MCC - Fixed cassette part 3P 3M W650","MCC - CASSETTE FIJO PARTE 3P 3M W650","Zenergy MCC - Fix kazettás alkatrész 3P 3M W650"]
["17363","Zenergy MCC - Kaseta 3P 3M W650, napęd obrotowy MCCB 250A",1771,"1-ZE-01",0.31666666666666665,1,"OE_MCC","17363","SZT","85389099",null,"200604LK","5901988173630","MCC - Cassette 3P 3M L650, Entraînement rotatif MCCB 250A","MCC - 3P 3M W650 cassette, MCCB 250A rotary drive","MCC - CASSETTE 3P 3M W650, UNIDAD ROTATIVA MCCB 250A","Zenergy MCC - 3P 3M W650 kazetta, MCCB 250A forgó meghajtó"]
["17364","Zenergy MCC - Część stała kasetowa 3P 3M W650 125A EPIC",749.8,"1-ZE-01",0.25,1,"OE_MCC","17364","SZT","85389099",null,null,"5901988173647","MCC - Partie fixe de la cassette 3P 3M L650 125A EPIC","MCC - Fixed cassette part 3P 3M W650 125A EPIC","MCC - CASSETTE FIJO PARTE 3P 3M W650 125A EPIC","Zenergy MCC - Fix kazettás alkatrész 3P 3M W650 125A EPIC"]
["17365","Zenergy MCC - Kaseta 3P 3M W650, napęd obrotowy MCCB 125A EPIC",1644.5,"1-ZE-01",0.25,1,"OE_MCC","17365","SZT","85389099",null,null,"5901988173654","MCC - Cassette 3P 3M L650, Entraînement rotatif MCCB 125A EPIC","MCC - 3P 3M W650 cassette, MCCB 125A EPIC rotary drive","MCC - CASSETTE 3P 3M W650, UNIDAD ROTATIVA MCCB 125A EPIC","Zenergy MCC - 3P 3M W650 kazetta, MCCB 125A EPIC forgó hajtás"]
["17366","Zenergy MCC - Kaseta uziemiająca 3P 3M W650 250A",2052,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988173661"]
["17367","Zenergy MCC - Kaseta uziemiająca 3P 3M W650, EPIC",1890,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988173678"]
["17393","OE - OSŁONA CZOŁOWA HGP 400-630 3/4P, W400, 9M / 250, PIONOWO, DŹWIGNIA",98.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","17393","SZT",null,null,"230626RT","5901988173937","OE - COUVERCLE AVANT HGP 400-630 3/4P, L400, 9M / 250, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W400, 9M / 250, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W400, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 400-630 3/4P, W400, 9M / 250, FÜGGŐLEGES, KAR"]
["17394","OE - OSŁONA CZOŁOWA HGP 800 3P, W400, 9M / 250, PIONOWO, DŹWIGNIA",98.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","17394","SZT",null,null,"230626RT","5901988173944","OE - COUVERCLE AVANT HGP 800 3P, L400, 9M / 250, VERTICAL, LEVIER","OE - Front cover HGP 800 3P, W400, 9M / 250, Vertical, Lever","ZEN- TAPA TROQ. HGP 800 3P, W400, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 800 3P, W400, 9M / 250, FÜGGŐLEGES, KAR"]
["17400","Zenergy MCC - Blacha dzieląca część stałą kasety 4M",211.6,"1-ZE-01",null,null,"OE_MCC","17400","SZT","85389099",null,"200604LK","5901988174002","MCC - Plaque métallique divisant la partie fixe de la cassette 4M","MCC - Metal plate dividing the fixed part of the 4M cassette","MCC - PLACA METÁLICA QUE DIVIDE LA PARTE FIJA DEL CASSETTE 4M","Zenergy MCC - A 4M kazetta rögzített részét elválasztó lap"]
["17401","Zenergy MCC - Moduł zasilania 2-wtyki 50A EPIC LAPP",126.5,"1-ZE-01",null,null,"OE_MCC","17401","SZT","85389099",null,"200604LK","5901988174019","MCC - Module d'alimentation 2 broches EPIC LAPP 50A","MCC - 50A EPIC LAPP 2-pin power supply module","MCC - MODULO DE FUENTE DE ALIMENTACIÓN 50A EPIC LAPP DE 2 PINES","Zenergy MCC - Tápmodul 2-pólusú 50A EPIC LAPP"]
["17402","Zenergy MCC - Moduł zasilania 3-wtyki 50A EPIC LAPP",162.19999999999999,"1-ZE-01",null,null,"OE_MCC","17402","SZT","85389099",null,"200604LK","5901988174026","MCC - Module d'alimentation 3 broches EPIC LAPP 50A","MCC - 50A EPIC LAPP 3-pin power supply module","MCC - MODULO DE FUENTE DE ALIMENTACIÓN 50A EPIC LAPP DE 3 PINES","Zenergy MCC - Tápmodul 3 tűs 50A EPIC LAPP"]
["17408","Zenergy MCC - Drzwi transparentne IP40, 8 mod, H400 x W650",286.39999999999998,"1-ZE-03",null,null,"OE_MCC","17408","SZT","85389099",null,"190118LK","5901988174088","MCC - Porte transparentes IP40, 8MOD H400 x L650","MCC - Transparent door IP40, 8 mod, H400 x W650","MCC - PUERTA TRANSP. IP40, 8 MOD, H400 x W650","Zenergy MCC - IP40 átlátszó ajtó, 8 mód, H400 x W650"]
["17409","Zenergy MCC - Drzwi transparentne IP40, 9 mod, H450 x W650",293.3,"1-ZE-03",null,null,"OE_MCC","17409","SZT","85389099",null,"190118LK","5901988174095","MCC - Porte transparentes IP40, 9MOD H450 x L650","MCC - Transparent door IP40, 9 mod, H450 x W650","MCC - PUERTA TRANSP. IP40, 9 MOD, H450 x W650","Zenergy MCC - IP40 átlátszó ajtó, 9 mód, H450 x W650"]
["17411","Zenergy MCC - Drzwi transparentne IP40, 11 mod, H550 x W650",303.60000000000002,"1-ZE-03",null,null,"OE_MCC","17411","SZT","85389099",null,"190118LK","5901988174118","MCC - Porte transparentes IP40, 11MOD H550 x L650","MCC - Transparent door IP40, 11 mod, H550 x W650","*MCC - Puerta transparente IP40, 11 mods, H550 x W650","Zenergy MCC - IP40 átlátszó ajtó, 11 mód, H550 x W650"]
["17412","Zenergy MCC - Drzwi transparentne IP40, 12 mod, H600 x W650",312.8,"1-ZE-03",null,null,"OE_MCC","17412","SZT","85389099",null,"190118LK","5901988174125","MCC - Porte transparentes IP40, 12MOD H600 x L650","MCC - Transparent door IP40, 12 mod, H600 x W650","MCC - PUERTA TRANSP. IP40, 12 MOD, H600 x W650","Zenergy MCC - IP40 átlátszó ajtó, 12 mód, H600 x W650"]
["17413","Zenergy MCC - Drzwi transparentne IP40, 13 mod, H650 x W650",323.2,"1-ZE-03",null,null,"OE_MCC","17413","SZT","85389099",null,"190118LK","5901988174132","MCC - Porte transparentes IP40, 13MOD H650 x L650","MCC - Transparent door IP40, 13 mod, H650 x W650","MCC - PUERTA TRANSP. IP40, 13 MOD, H650 x W650","Zenergy MCC - IP40 átlátszó ajtó, 13 mód, H650 x W650"]
["17450","Zenergy MCC - Część stała wtykowa 4P 4M W650",738.3,"1-ZE-01",null,null,"OE_MCC","17450","SZT","85389099",null,"200604LK","5901988174507","MCC - Partie fixe enfichable 4P 4M L650","MCC - Fixed plug-in part 4P 4M W650","MCC - PIEZA ENCHUFABLE FIJA 4P 4M W650","Zenergy MCC - Plug-in fix alkatrész 4P 4M W650"]
["17451","Zenergy MCC - Płyta wtykowa 100-250A 4P 4M W650",914.3,"1-ZE-01",null,null,"OE_MCC","17451","SZT","85389099",null,"200604LK","5901988174514","MCC - Étagère enfichable 100-250A 4P 4M L650","MCC - Plug-in board 100-250A 4P 4M W650","MCC - TARJETA ENCHUFABLE 100-250A 4P 4M W650","Zenergy MCC - Plug-in kártya 100-250A 4P 4M W650"]
["17460","Zenergy MCC - Część stała wtykowa 3P 4M W650",738.3,"1-ZE-01",null,null,"OE_MCC","17460","SZT","85389099",null,"200604LK","5901988174606","MCC - Partie fixe enfichable 3P 4M L650","MCC - Fixed plug-in part 3P 4M W650","MCC - PIEZA ENCHUFABLE FIJA 3P 4M W650","Zenergy MCC - Plug-in fix alkatrész 3P 4M W650"]
["17461","Zenergy MCC - Płyta wtykowa 400-630A 3P 4M W650",914.3,"1-ZE-01",null,null,"OE_MCC","17461","SZT","85389099",null,"200604LK","5901988174613","MCC - Étagère enfichable 400-630A 3P 4M L650","MCC - Plug-in board 400-630A 3P 4M W650","MCC - TARJETA ENCHUFABLE 400-630A 3P 4M W650","Zenergy MCC - Plug-in kártya 400-630A 3P 4M W650"]
["17462","Zenergy MCC - Część stała kasetowa 3P 4M W650",809.6,"1-ZE-01",0.1,1,"OE_MCC","17462","SZT","85389099",null,"200604LK","5901988174620","MCC - Partie fixe de la cassette 3P 4M L650","MCC - Fixed cassette part 3P 4M W650","MCC - CASSETTE FIJO PARTE 3P 4M W650","Zenergy MCC - Fix kazettás alkatrész 3P 4M W650"]
["17463","Zenergy MCC - Kaseta 3P 4M W650, napęd obrotowy MCCB 630A",1897.5,"1-ZE-01",0.1,1,"OE_MCC","17463","SZT","85389099",null,"200604LK","5901988174637","MCC - Cassette 3P 4M L650, Entraînement rotatif MCCB 630A","MCC - 3P 4M W650 cassette, MCCB 630A rotary drive","MCC-  CASETE 3P 4M W650, UNIDAD ROTATIVA MCCB 630A","Zenergy MCC - 3P 4M W650 kazetta, MCCB 630A forgó meghajtó"]
["17464","Zenergy MCC - Część stała kasetowa dzielona 4P 4M W650",1437.5,"1-ZE-01",1.6666666666666666E-2,1,"OE_MCC","17464","SZT","85389099",null,"200604LK","5901988174644","MCC - Partie fixe de la cassette fractionnée 4P 4M L650","MCC - Fixed cassette section 4P 4M W650","MCC - CASSETTE FIJO 4P 4M W650","Zenergy MCC - Fix kazettás rész osztott 4P 4M W650"]
["17465","Zenergy MCC - Kaseta 3P 4M W650, napęd obrotowy MCCB 630A EPIC",1620,null,1.6666666666666666E-2,1,"OE_MCC",null,null,"85389099",null,null,"5901988174651"]
["17466","Zenergy MCC - Kaseta uziemiająca 3P 4M W650",2160,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988174668"]
["17467","Zenergy MCC - Kaseta uziemiająca 3P 4M W650, EPIC",1998,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988174675"]
["17471","MCC - Płyta dzieląca część stałą kasety 17464",302.39999999999998,null,null,null,"OE_MCC",null,null,"85389099",null,null,""]
["17472","Zenergy MCC - Kaseta 1/2 4M W650, napęd obrotowy GV4L 3P 100A",1834.3,"1-ZE-01",null,null,"OE_MCC","17472","SZT","85389099",null,"200604LK","5901988174729","MCC - Cassette 1/2 4M L650, Entraînement rotatif GV2P 3P 2x50A","MCC - Cassette 1/2 4M W650, rotary drive GV2P 3P 2x50A","MCC - CASSETTE 1/2 4M W650, ACCIONAMIENTO ROTATIVO GV2P 3P 2X50A","Zenergy MCC - 1/2 4M W650 kazetta, GV4L 3P 100A forgó hajtás"]
["17473","Zenergy MCC - Kaseta 1/3 4M W650, napęd obrotowy GV2P 3P 100A",1620,null,null,null,"OE_MCC",null,null,"85389099",null,null,""]
["17474","Zenergy MCC - Kaseta 1/4 4M W650, napęd obrotowy GV2P 3P 50A",1688.2,"1-ZE-01",null,null,"OE_MCC","17474","SZT","85389099",null,"200604LK","5901988174743","MCC - Cassette 1/4 4M L650, Entraînement rotatif GV2P 3P 50A","MCC - 1/4 4M W650 cassette, GV2P 3P 50A rotary drive","MCC - CASSETTE 1/4 4M W650, ACCIONAMIENTO ROTATIVO GV2P 3P 50A","Zenergy MCC - 1/4 4M W650 kazetta, GV2P 3P 50A forgó hajtás"]
["17475","ZENERGY MCC - 100MM KRATOWNICA IP20 - 4P ŻALUZJA SZYN TYLNYCH PIONOWYCH",21.2,"1-ZE-01",null,null,"OE_MCC",null,"SZT","85469010",null,null,"5901988174750","MCC - GRILLE IP20 100 MM - PERSIENNE DE RAIL ARRIÈRE VERTICAL 4P","MCC - 100mm IP20 4P Back Vertical busbars grill","*MCC - REJILLA 100MM IP20 - PERSIA VERTICAL TRASERA 4P","ZENERGY MCC - 100 mm-es GRID IP20 - 4P HÁTSÓ FÜGGŐLEGES SÍN SZERETŐK"]
["17550","Zenergy MCC - Część stała wtykowa 4P 5M W650",938.4,"1-ZE-01",null,null,"OE_MCC","17550","SZT","85389099",null,"200604LK","5901988175504","MCC - Partie fixe enfichable 4P 5M L650","MCC - Fixed plug-in part 4P 5M W650","MCC - PIEZA ENCHUFABLE FIJA 4P 5M W650","Zenergy MCC - Plug-in fix alkatrész 4P 5M W650"]
["17551","Zenergy MCC - Płyta wtykowa 400-630A 4P 5M W650",1173,"1-ZE-01",null,null,"OE_MCC","17551","SZT","85389099",null,"200604LK","5901988175511","MCC - Étagère enfichable 400-630A 4P 5M L650","MCC - Plug-in board 400-630A 4P 5M W650","MCC - PLACA DE CONEXIÓN 400-630A 4P 5M W650","Zenergy MCC - Plug-in kártya 400-630A 4P 5M W650"]
["17562","Zenergy MCC - Część stała kasetowa 3P 5M W650",1495,"1-ZE-01",9.166666666666666E-2,1,"OE_MCC","17562","SZT","85389099",null,"200604LK","5901988175627","MCC - Partie fixe de la cassette 3P 5M L650","MCC - Fixed cassette part 3P 5M W650","MCC - CASSETTE FIJO PARTE 3P 5M W650","Zenergy MCC - Fix kazettás alkatrész 3P 5M W650"]
["17563","Zenergy MCC - Kaseta 3P 5M W650, napęd obrotowy MCCB 630A",1960.8,"1-ZE-01",9.166666666666666E-2,1,"OE_MCC","17563","SZT","85389099",null,"200604LK","5901988175634","MCC - Cassette 3P 5M L650, Entraînement rotatif MCCB 630A","MCC - 3P 5M W650 cassette, MCCB 630A rotary drive","MCC- CASETE 3P 5M W650, UNIDAD ROTATIVA MCCB 630A","Zenergy MCC - 3P 5M W650 kazetta, MCCB 630A forgó meghajtó"]
["17566","Zenergy MCC - Kaseta uziemiająca 3P 5M W650",2160,null,null,null,"OE_MCC",null,null,"85389099",null,null,"5901988175665"]
["17593","OE - OSŁONA CZOŁOWA HGP 400-630 3/4P, W450, 9M / 300, PIONOWO, DŹWIGNIA",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","17593","SZT",null,null,"230626RT","5901988175931","OE - COUVERCLE AVANT HGP 400-630 3/4P, L450, 9M / 300, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W450, 9M / 300, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W450, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 400-630 3/4P, W450, 9M / 300, FÜGGŐLEGES, KAR"]
["17594","OE - OSŁONA CZOŁOWA HGP 800 3P, W450, 9M / 300, PIONOWO, DŹWIGNIA",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","17594","SZT",null,null,"230626RT","5901988175948","OE - COUVERCLE AVANT HGP 800 3P, L450, 9M / 300, VERTICAL, LEVIER","OE - Front cover HGP 800 3P, W450, 9M / 300, Vertical, Lever","ZEN- TAPA TROQ. HGP 800 3P, W450, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 800 3P, W450, 9M / 300, FÜGGŐLEGES, KAR"]
["17662","Zenergy MCC - Część stała kasetowa 3P 6M W650",807.3,"1-ZE-01",null,null,"OE_MCC","17662","SZT","85389099",null,null,"5901988176624","MCC - Partie fixe de la cassette 3P 6M L650","MCC - Fixed cassette part 3P 6M W650","MCC - CASSETTE FIJO PARTE 3P 6M W650","Zenergy MCC - Fix kazettás alkatrész 3P 6M W650"]
["17663","Zenergy MCC - Kaseta 3P 6M W650, napęd obrotowy MCCB 630A",2024,"1-ZE-01",null,null,"OE_MCC","17663","SZT","85389099",null,"200604LK","5901988176631","MCC - Cassette 3P 6M L650, Entraînement rotatif MCCB 630A","MCC - 3P 6M W650 cassette, MCCB 630A rotary drive","MCC- CASETE 3P 6M W650, UNIDAD ROTATIVA MCCB 630A","Zenergy MCC - 3P 6M W650 kazetta, MCCB 630A forgó meghajtó"]
["17710","Zenergy MCC - Adaptery MCC-10M do zabudowy osłon czołowych 9M",155.30000000000001,"1-ZE-01",null,null,"OE_MCC","17710","SZT","85389099",null,"210306LK","5901988177102","MCC - Adaptateurs MCC-10M pour le montage des caches avant 9M","MCC - MCC-10M adapters for the installation of 9M Front covers","MCC- ADAPTADOR MCC-10M PARA LA INSTALACIÓN DE TAPAS FRONTALES 9M","Zenergy MCC - MCC-10M adapterek 9M előlapok felszereléséhez"]
["17711","Zenergy MCC - Adaptery MCC-11M do zabudowy osłon czołowych 10M",169.1,"1-ZE-01",null,null,"OE_MCC","17711","SZT","85389099",null,"210306LK","5901988177119","MCC - Adaptateurs MCC-11M pour le montage des caches avant 10M","MCC - MCC-11M adapters for building 10M Front covers","MCC- ADAPTADOR MCC-11M PARA LA CONSTRUCCIÓN DE CUBIERTAS FRONTALES DE 10M","Zenergy MCC - MCC-11M adapterek 10M előlapok felszereléséhez"]
["17712","Zenergy MCC - Adaptery MCC-12M do zabudowy osłon czołowych 11M",182.9,"1-ZE-01",null,null,"OE_MCC","17712","SZT","85389099",null,"210306LK","5901988177126","MCC - Adaptateurs MCC-12M pour le montage des caches avant 11M","MCC - MCC-12M adapters for mounting 11M Front covers","MCC- ADAPTADOR MCC-12M PARA MONTAR TAPAS FRONTALES 11M","Zenergy MCC - MCC-12M adapterek 11M előlapok felszereléséhez"]
["17713","Zenergy MCC - Adaptery MCC-13M do zabudowy osłon czołowych 12M",196.7,"1-ZE-01",null,null,"OE_MCC","17713","SZT","85389099",null,"210306LK","5901988177133","MCC - Adaptateurs MCC-13M pour le montage des caches avant 12M","MCC - MCC-13M adapters for mounting 12M Front covers","MCC- ADAPTADOR MCC-13M PARA LA INSTALACIÓN DE TAPAS FRONTALES DE 12M","Zenergy MCC - MCC-13M adapterek 12M előlapok felszereléséhez"]
["17714","Zenergy MCC - Adaptery MCC-14M do zabudowy osłon czołowych 13M",211.6,"1-ZE-01",null,null,"OE_MCC","17714","SZT","85389099",null,"210306LK","5901988177140","MCC - Adaptateurs MCC-14M pour le montage des caches avant 13M","MCC - MCC-14M adapters for mounting 13M Front covers","MCC- ADAPTADOR MCC-14M PARA MONTAR TAPAS FRONTALES 13M","Zenergy MCC - MCC-14M adapterek 13M előlapok felszereléséhez"]
["17715","Zenergy MCC - Adaptery MCC-15M do zabudowy osłon czołowych 14M",225.4,"1-ZE-01",null,null,"OE_MCC","17715","SZT","85389099",null,"210306LK","5901988177157","MCC - Adaptateurs MCC-15M pour le montage des caches avant 14M","MCC - MCC-15M adapters for mounting 14M Front covers","MCC- ADAPTADOR MCC-15M PARA MONTAR TAPAS FRONTALES 14M","Zenergy MCC - MCC-15M adapterek 14M előlapok felszereléséhez"]
["17718","Zenergy MCC - Adaptery MCC-18M do zabudowy osłon czołowych 17M",268,"1-ZE-01",null,null,"OE_MCC","17718","SZT","85389099",null,"210306LK","5901988177188","MCC - Adaptateurs MCC-18M pour le montage des caches avant 17M","MCC - MCC-18M adapters for mounting 17M Front covers","MCC- ADAPTADOR MCC-18M PARA MONTAR TAPAS FRONTALES 17M","Zenergy MCC - MCC-18M adapterek 17M előlapok felszereléséhez"]
["17730","Zenergy MCC - Adaptery MCC-3M do zabudowy osłon czołowych 2M",70.400000000000006,"1-ZE-01",null,null,"OE_MCC","17730","SZT","85389099",null,"210306LK","5901988177300","MCC - Adaptateurs MCC-3M pour le montage des caches avant 2M","MCC - MCC-3M adapters for mounting 2M Front covers","MCC- ADAPTADOR MCC-3M PARA MONTAR TAPAS FRONTALES 2M","Zenergy MCC - MCC-3M adapterek 2M előlapok felszereléséhez"]
["17740","Zenergy MCC - Adaptery MCC-4M do zabudowy osłon czołowych 3M",70.400000000000006,"1-ZE-01",null,null,"OE_MCC","17740","SZT","85389099",null,"210306LK","5901988177409","MCC - Adaptateurs MCC-4M pour le montage des caches avant 3M","MCC - MCC-4M adapters for mounting 3M Front covers","MCC- ADAPTADOR MCC-4M PARA MONTAR TAPAS FRONTALES 3M","Zenergy MCC - MCC-4M adapterek 3M előlapok felszereléséhez"]
["17748","OE - OSŁONA CZOŁOWA HGP 400-630 3P, W650, 4M / 500, POZIOMO, DŹWIGNIA",66.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","17748","SZT",null,null,"230626RT","5901988177485","OE - COUVERCLE AVANT HGP 400-630 3P, L650, 4M / 500, HORIZONTAL, LEVIER","OE - Front cover HGP 400-630 3P, W650, 4M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP 400-630 3P, W650, 4M (200mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 400-630 3P, W650, 4M / 500, VÍZSZINTES, KAR"]
["17750","Zenergy MCC - Adaptery MCC-5M do zabudowy osłon czołowych 4M",78.2,"1-ZE-01",null,null,"OE_MCC","17750","SZT","85389099",null,null,"5901988177508","MCC - Adaptateurs MCC-5M pour le montage des caches avant 4M","MCC - MCC-5M adapters for mounting 4M Front covers","MCC- ADAPTADOR MCC-5M PARA MONTAR TAPAS FRONTALES DE 4M","Zenergy MCC - MCC-5M adapterek 4M előlapok felszereléséhez"]
["17758","OE - OSŁONA CZOŁOWA HGP 400-630 4P, W650, 5M / 500, POZIOMO, DŹWIGNIA",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","17758","SZT",null,null,"230626RT","5901988177584","OE - COUVERCLE AVANT HGP 400-630 4P, L650, 5M / 500, HORIZONTAL, LEVIER","OE - Front cover HGP 400-630 4P, W650, 5M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP 400-630 4P, W650, 5M (250mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 400-630 4P, W650, 5M / 500, VÍZSZINTES, KAR"]
["17760","Zenergy MCC - Adaptery MCC-6M do zabudowy osłon czołowych 5M",98.6,"1-ZE-01",null,null,"OE_MCC","17760","SZT","85389099",null,"210306LK","5901988177607","MCC - Adaptateurs MCC-6M pour le montage des caches avant 5M","MCC - MCC-6M adapters for mounting 5M Front covers","MCC- ADAPTADOR MCC-6M PARA MONTAR TAPAS FRONTALES DE 5M","Zenergy MCC - MCC-6M adapterek 5M előlapok felszereléséhez"]
["17764","Zenergy MCC - Kaseta 4P 7M W650, napęd obrotowy MCCB 800A-1000A",3258,"1-ZE-01",null,null,"OE_MCC","17764","SZT","85389099",null,null,"5901988177645","MCC - Cassette 4P 7M L650, Entraînement rotatif MCCB 800A-1000A","MCC - 4P 7M W650 cassette, MCCB 800A-1000A rotary drive","MCC- CASETE 4P 7M W650, UNIDAD ROTATIVA MCCB 800A-1000A","Zenergy MCC - 4P 7M W650 kazetta, MCCB 800A-1000A forgó meghajtó"]
["17769","OE - OSŁONA CZOŁOWA HGP 800 3P, W650, 6M / 500, POZIOMO, DŹWIGNIA",92.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","17769","SZT","85389099","27.12.40.0","230626RT","5901988177690","OE - COUVERCLE AVANT HGP 800 3P, L650, 6M / 500, HORIZONTAL, LEVIER","OE - Front cover HGP 800 3P, W650, 6M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP 800 3P, W650, 6M (300mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 800 3P, W650, 6M / 500, VÍZSZINTES, KAR"]
["17770","Zenergy MCC - Adaptery MCC-7M do zabudowy osłon czołowych 6M",104.2,"1-ZE-01",null,null,"OE_MCC","17770","SZT","85389099",null,null,"5901988177706","MCC - Adaptateurs MCC-7M pour le montage des caches avant 6M","MCC - MCC-7M adapters for mounting 6M Front covers","MCC- ADAPTADOR MCC-7M PARA MONTAR TAPAS FRONTALES 6M","Zenergy MCC - MCC-7M adapterek 6M előlapok felszereléséhez"]
["17779","OE - OSŁONA CZOŁOWA HGP 800 4P, W650, 7M / 500, POZIOMO, DŹWIGNIA",113.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","17779","SZT",null,null,"230626RT","5901988177799","OE - COUVERCLE AVANT HGP 800 4P, L650, 7M / 500, HORIZONTAL, LEVIER","OE - Front cover HGP 800 4P, W650, 7M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP 800 4P, W650, 7M (350mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 800 4P, W650, 7M / 500, VÍZSZINTES, KAR"]
["17780","Zenergy MCC - Adaptery MCC-8M do zabudowy osłon czołowych 7M",126.5,"1-ZE-01",null,null,"OE_MCC","17780","SZT","85389099",null,"210306LK","5901988177805","MCC - Adaptateurs MCC-8M pour le montage des caches avant 7M","MCC - MCC-8M adapters for mounting 7M Front covers","MCC- ADAPTADOR MCC-8M PARA MONTAR TAPAS FRONTALES 7M","Zenergy MCC - MCC-8M adapterek 7M előlapok felszereléséhez"]
["17790","Zenergy MCC - Adaptery MCC-9M do zabudowy osłon czołowych 8M",140.30000000000001,"1-ZE-01",null,null,"OE_MCC","17790","SZT","85389099",null,"210306LK","5901988177904","MCC - Adaptateurs MCC-9M pour le montage des caches avant 8M","MCC - MCC-9M adapters for mounting 8M Front covers","MCC- ADAPTADOR MCC-9M PARA MONTAR TAPAS FRONTALES 8M","Zenergy MCC - MCC-9M adapterek 8M előlapok felszereléséhez"]
["17793","OE - OSŁONA CZOŁOWA HGP 400-630 3/4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","17793","SZT",null,null,"230626RT","5901988177935","OE - COUVERCLE AVANT HGP 400-630 3/4P, L650, 9M / 500, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W650, 9M (450mm)VERT.","OE - ELSŐ BURKOLAT HGP 400-630 3/4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["17794","OE - OSŁONA CZOŁOWA HGP 800 3P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","17794","SZT",null,null,"230626RT","5901988177942","OE - COUVERCLE AVANT HGP 800 3P, L650, 9M / 500, VERTICAL, LEVIER","OE - Front cover HGP 800 3P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGP 800 3P, W650, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 800 3P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["17795","OE - OSŁONA CZOŁOWA HGP 800 4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","17795","SZT",null,null,"230626RT","5901988177959","OE - COUVERCLE AVANT HGP 800 4P, L650, 9M / 500, VERTICAL, LEVIER","OE - Front cover HGP 800 4P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGP 800 4P, W650, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 800 4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["17948","OE - OSŁONA CZOŁOWA HGP 400-630 3P, W850, 4M / 700, POZIOMO, DŹWIGNIA",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","17948","SZT",null,null,"230626RT","5901988179489","OE - COUVERCLE AVANT HGP 400-630 3P, L850, 4M / 700, HORIZONTAL, LEVIER","OE - Front cover HGP 400-630 3P, W850, 4M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP 400-630 3P, W850, 4M (200mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 400-630 3P, W850, 4M / 700, VÍZSZINTES, KAR"]
["17958","OE - OSŁONA CZOŁOWA HGP 400-630 4P, W850, 5M / 700, POZIOMO, DŹWIGNIA",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","17958","SZT",null,null,"230626RT","5901988179588","OE - COUVERCLE AVANT HGP 400-630 4P, L850, 5M / 700, HORIZONTAL, LEVIER","OE - Front cover HGP 400-630 4P, W850, 5M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP 400-630 4P, W850, 5M (250mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 400-630 4P, W850, 5M / 700, VÍZSZINTES, KAR"]
["17969","OE - OSŁONA CZOŁOWA HGP 800 3P, W850, 6M / 700, POZIOMO, DŹWIGNIA",107.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","17969","SZT","85389099","27.12.40.0","230626RT","5901988179694","OE - COUVERCLE AVANT HGP 800 3P, L850, 6M / 700, HORIZONTAL, LEVIER","OE - Front cover HGP 800 3P, W850, 6M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP 800 3P, W850, 6M (300mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 800 3P, W850, 6M / 700, VÍZSZINTES, KAR"]
["17979","OE - OSŁONA CZOŁOWA HGP 800 4P, W850, 7M / 700, POZIOMO, DŹWIGNIA",130.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","17979","SZT",null,null,"230626RT","5901988179793","OE - COUVERCLE AVANT HGP 800 4P, L850, 7M / 700, HORIZONTAL, LEVIER","OE - Front cover HGP 800 4P, W850, 7M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP 800 4P, W850, 7M (350mm) HORIZ. ","OE - ELSŐ BURKOLAT HGP 800 4P, W850, 7M / 700, VÍZSZINTES, KAR"]
["17993","OE - OSŁONA CZOŁOWA HGP 400-630 3/4P, W850, 9M / 700, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","17993","SZT",null,null,"230626RT","5901988179939","OE - COUVERCLE AVANT HGP 400-630 3/4P, L850, 9M / 700, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W850, 9M / 700, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W850, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 400-630 3/4P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["17994","OE - OSŁONA CZOŁOWA HGP 800 3P, W850, 9M / 700, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","17994","SZT",null,null,"230626RT","5901988179946","OE - COUVERCLE AVANT HGP 800 3P, L850, 9M / 700, VERTICAL, LEVIER","OE - Front cover HGP 800 3P, W850, 9M / 700, Vertical, Lever","ZEN- TAPA TROQ. HGP 800 3P, W850, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT HGP 800 3P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["17995","OE - OSŁONA CZOŁOWA 2X HGP 800 4P, W850, 9M / 700, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","17995","SZT",null,null,"230626RT","5901988179953","OE - COUVERCLE AVANT 2X HGP 800 4P, L850, 9M / 700, VERTICAL, LEVIER","OE - Front cover 2X HGP 800 4P, W850, 9M / 700, Vertical, Lever","ZEN- TAPA TROQ. 2X HGP 800 4P, W850, 9M (450mm) VERT.","OE - ELSŐ BURKOLAT 2X HGP 800 4P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["18235","OE - Osłona czołowa HGP 250, UPB 100-250 3P, W400, 3M / 250, poziomo, dźwignia",49.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","18235","SZT","85389099",null,"230623RT","5901988182359","OE - Couvercle avant HGP 250, UPB 100-250 3P, L400, 3M / 250, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 3P, W400, 3M / 250, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 3P, W400, 3M (150MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 3P, W400, 3M / 250, vízszintes, kar"]
["18245","OE - Osłona czołowa HGP 250, UPB 100-250 4P, W400, 4M / 250, poziomo, dźwignia",52.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18245","SZT","85389099",null,"230623RT","5901988182458","OE - Couvercle avant HGP 250, UPB 100-250 4P, L400, 4M / 250, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 4P, W400, 4M / 250, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 4P, W400, 4M (200MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 4P, W400, 4M / 250, vízszintes, kar"]
["18250","OE - Osłona czołowa HGP 250, UPB 100-250 3/4P, W400, 5M / 250, pionowo, dźwignia",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18250","SZT","85389099","27.12.40.0","230623RT","5901988182502","OE - Couvercle avant HGP 250, UPB 100-250 3 / 4P, L400, 5M / 250, vertical, levier","OE - Front visor HGP 250, UPB 100-250 3 / 4P, W400, 5M / 250, Vertical, Lever","ZEN- TAPA TROQ. HGP250 3/4P, W400, 5M (250MM) VERT.","OE - Első burkolat HGP 250, UPB 100-250 3/4P, W400, 5M / 250, függőleges, kar"]
["18291","OE - Osłona czołowa UPB 400-630 3/4P, W400, 9M / 250, pionowo, dźwignia",93.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","18291","SZT","85389099",null,"230623RT","5901988182915","OE - Panneau avant UPB 400-630 3 / 4P, L400, 9M / 250, vertical, levier","OE - Front visor UPB 400-630 3 / 4P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. UPB 400-630 3/4P, W400, 9M (450MM)  VERT.","OE - Első burkolat UPB 400-630 3/4P, W400, 9M / 250, függőleges, kar"]
["18323","OE - Osłona czołowa UCB 1000-1250 4P, W400, 12M / 250, pionowo, dźwignia",104.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","18323","SZT","85389099",null,"230623RT","5901988183233","OE - Capot avant UCB 1000-1250 4P, L400, 12M / 250, vertical, levier","OE - Front cover UCB 1000-1250 4P, W400, 12M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 4P, W400, 12M (600MM)  VERT.","OE - Előlap UCB 1000-1250 4P, W400, 12M / 250, függőleges, kar"]
["18334","OE - Osłona czołowa UCB 100 3P, W400, 3M / 250, poziomo, dźwignia",49.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","18334","SZT","85389099",null,"230623RT","5901988183349","OE - Capot avant UCB 100 3P, L400, 3M / 250, horizontal, levier","OE - Front cover UCB 100 3P, W400, 3M / 250, Horizontal, Lever","OE- TAPA TROQ. UCB 100 3P, W400, 3M (150MM)  HORIZ.","OE - Előlap UCB 100 3P, W400, 3M / 250, vízszintes, kar"]
["18335","OE - Osłona czołowa UCB 160-250 3P, W400, 3M / 250, poziomo, dźwignia",49.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","18335","SZT","85389099",null,"230623RT","5901988183356","OE - Capot avant UCB 160-250 3P, L400, 3M / 250, horizontal, levier","OE - Front cover UCB 160-250 3P, W400, 3M / 250, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 3P, W400, 3M (150MM)  HORIZ.","OE - Előlap UCB 160-250 3P, W400, 3M / 250, vízszintes, kar"]
["18344","OE - Osłona czołowa UCB 100 4P, W400, 4M / 250, poziomo, dźwignia",52.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18344","SZT","85389099",null,"230623RT","5901988183448","OE - Capot avant UCB 100 4P, L400, 4M / 250, horizontal, levier","OE - Front cover UCB 100 4P, W400, 4M / 250, Horizontal, Lever","OE- TAPA TROQ. UCB 100 4P, W400, 4M (200MM)  HORIZ.","OE - Előlap UCB 100 4P, W400, 4M / 250, vízszintes, kar"]
["18345","OE - Osłona czołowa UCB 160-250 4P, W400, 4M / 250, poziomo, dźwignia",52.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18345","SZT","85389099",null,"230623RT","5901988183455","OE - Capot avant UCB 160-250 4P, L400, 4M / 250, horizontal, levier","OE - Front cover UCB 160-250 4P, W400, 4M / 250, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 4P, W400, 4M (200MM)  HORIZ.","OE - Előlap UCB 160-250 4P, W400, 4M / 250, vízszintes, kar"]
["18349","OE - Osłona czołowa UCB 100 4P, W400, 5M / 250, pionowo, dźwignia",59,"1-ZE-01",null,null,"OE_MCCB_COVERS","18349","SZT","85389099","27.12.40.0","230623RT","5901988183493","OE - Couvercle avant UCB 100 4P, L400, 5M / 250, vertical, levier","OE - Front visor UCB 100 4P, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 100 3/4P, W400, 5M (250MM)  VERT.","OE - Előlap UCB 100 4P, W400, 5M / 250, függőleges, kar"]
["18350","OE - Osłona czołowa UCB 160-250 3P, W400, 5M / 250, pionowo, dźwignia",59,"1-ZE-01",null,null,"OE_MCCB_COVERS","18350","SZT","85371098","27.12.31.0","230623RT","5901988183509","OE - Capot avant UCB 160-250 3P, L400, 5M / 250, vertical, levier","OE - Front cover UCB 160-250 3P, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 160-250 3P, W400, 5M (250MM)  VERT.","OE - Előlap UCB 160-250 3P, W400, 5M / 250, függőleges, kar"]
["18390","OE - Osłona czołowa UCB 400 3P, W400, 9M / 250, pionowo, dźwignia",93.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","18390","SZT","85371098","27.12.31.0","230623RT","5901988183905","OE - Couvercle avant UCB 400 3P, L400, 9M / 250, vertical, levier","OE - Front visor UCB 400 3P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 400 3P, W400, 9M / 250, VERT.","OE - Előlap UCB 400 3P, W400, 9M / 250, függőleges, kar"]
["18391","OE - Osłona czołowa UCB 400 4P, W400, 9M / 250, pionowo, dźwignia",98.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18391","SZT","85371098","27.12.31.0","230623RT","5901988183912","OE - Couvercle avant UCB 400 4P, L400, 9M / 250, vertical, levier","OE - Front visor UCB 400 4P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 400 4P, W400, 9M (450MM)  VERT.","OE - Előlap UCB 400 4P, W400, 9M / 250, függőleges, kar"]
["18392","OE - Osłona czołowa UCB 630-800 3P, W400, 9M / 250, pionowo, dźwignia",98.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18392","SZT","85371098","27.12.31.0","230623RT","5901988183929","OE - Couvercle avant UCB 630-800 3P, L400, 9M / 250, vertical, levier","OE - Front cover UCB 630-800 3P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 630-800 3P, W400, 9M (450MM)  VERT.","OE - Előlap UCB 630-800 3P, W400, 9M / 250, függőleges, kar"]
["18435","OE - Osłona czołowa HGP 250, UPB 100-250 3P, W450, 3M / 300, poziomo, dźwignia",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18435","SZT","85389099","27.12.40.0","230626RT","5901988184353","OE - Couvercle avant HGP 250, UPB 100-250 3P, L450, 3M / 300, horizontal, levier","OE - Front hood HGP 250, UPB 100-250 3P, W450, 3M / 300, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 3P, W450, 3M (150MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 3P, W450, 3M / 300, vízszintes, kar"]
["18445","OE - Osłona czołowa HGP 250, UPB 100-250 4P, W450, 4M / 300, poziomo, dźwignia",58.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18445","SZT","85389099","27.12.40.0","230626RT","5901988184452","OE - Couvercle avant HGP 250, UPB 100-250 4P, L450, 4M / 300, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 4P, W450, 4M / 300, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 4P, W450, 4M (200MM) HORIZ. ","OE - Előlap HGP 250, UPB 100-250 4P, W450, 4M / 300, vízszintes, kar"]
["18450","OE - Osłona czołowa HGP 250, UPB 100-250 3/4P, W450, 5M / 300, pionowo, dźwignia",65.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","18450","SZT","85389099","27.12.40.0","230626RT","5901988184506","OE - Couvercle avant HGP 250, UPB 100-250 3 / 4P, L450, 5M / 300, vertical, levier","OE - Front visor HGP 250, UPB 100-250 3 / 4P, W450, 5M / 300, Vertical, Lever","ZEN- TAPA TROQ. HGP250 3/4P, W450, 5M (250MM) VERT.","OE - Első burkolat HGP 250, UPB 100-250 3/4P, W450, 5M / 300, függőleges, kar"]
["18491","OE - Osłona czołowa UPB 400-630 3/4P, W450, 9M / 300, pionowo, dźwignia",111.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18491","SZT","85389099","27.12.40.0","230626RT","5901988184919","OE - Panneau avant UPB 400-630 3 / 4P, L450, 9M / 300, vertical, levier","OE - Front visor UPB 400-630 3 / 4P, W450, 9M / 300, Vertical, Lever","OM- TAPA TROQ. UPB 400-630 3/4P, W450, 9M (450MM) VERT.","OE - Első burkolat UPB 400-630 3/4P, W450, 9M / 300, függőleges, kar"]
["18522","OE - Osłona czołowa UCB 1000-1250 3P, W450, 12M / 300, pionowo, dźwignia",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","18522","SZT","85389099","27.12.40.0","230626RT","5901988185220","OE - Capot avant UCB 1000-1250 3P, L450, 12M / 300, vertical, levier","OE - Front cover UCB 1000-1250 3P, W450, 12M / 300, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 3P, W450, 12M (600MM) VERT.","OE - Első burkolat UCB 1000-1250 3P, W450, 12M / 300, függőleges, kar"]
["18534","OE - Osłona czołowa UCB 100 3P, W450, 3M / 300, poziomo, dźwignia",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18534","SZT","85389099","27.12.40.0","230626RT","5901988185343","OE - Capot avant UCB 100 3P, L450, 3M / 300, horizontal, levier","OE - Front Shield UCB 100 3P, W450, 3M / 300, Horizontal, Lever","OM- TAPA TROQ. UCB 100 3P, W450, 3M (150MM) HORIZ.","OE - Előlap UCB 100 3P, W450, 3M / 300, vízszintes, kar"]
["18535","OE - Osłona czołowa UCB 160-250 3P, W450, 3M / 300, poziomo, dźwignia",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18535","SZT","85389099","27.12.40.0","230626RT","5901988185350","OE - Capot avant UCB 160-250 3P, L450, 3M / 300, horizontal, levier","OE - Front cover UCB 160-250 3P, W450, 3M / 300, Horizontal, Lever","OM- TAPA TROQ. UCB 160-250 3P, W450, 3M (150MM) HORIZ.","OE - Előlap UCB 160-250 3P, W450, 3M / 300, vízszintes, kar"]
["18544","OE - Osłona czołowa UCB 100 4P, W450, 4M / 300, poziomo, dźwignia",58.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18544","SZT","85389099","27.12.40.0","230626RT","5901988185442","OE - Capot avant UCB 100 4P, L450, 4M / 300, horizontal, levier","OE - Front cover UCB 100 4P, W450, 4M / 300, Horizontal, Lever","OM- TAPA TROQ. UCB 100 4P, W450, 4M (200MM) HORIZ.","OE - Előlap UCB 100 4P, W450, 4M / 300, vízszintes, kar"]
["18545","OE - Osłona czołowa UCB 160-250 4P, W450, 4M / 300, poziomo, dźwignia",58.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18545","SZT","85389099","27.12.40.0","230626RT","5901988185459","OE - Capot avant UCB 160-250 4P, L450, 4M / 300, horizontal, effet de levier","OE - Front cover UCB 160-250 4P, W450, 4M / 300, Horizontal, Lever","OM- TAPA TROQ. UCB 160-250 4P, W450, 4M (200MM) HORIZ.","OE - Előlap UCB 160-250 4P, W450, 4M / 300, vízszintes, kar"]
["18549","OE - Osłona czołowa UCB 100 3/4P, W450, 5M / 300, pionowo, dźwignia",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","18549","SZT","85389099","27.12.40.0","230626RT","5901988185497","OE - Capot avant UCB 100 3 / 4P, L450, 5M / 300, vertical, levier","OE - Front cover UCB 100 3 / 4P, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. UCB 100 3/4P, W450, 5M (250MM) VERT.","OE - Előlap UCB 100 3/4P, W450, 5M / 300, függőleges, kar"]
["18550","OE - Osłona czołowa UCB 160-250 3P, W450, 5M / 300, pionowo, dźwignia",65.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","18550","SZT","85389099","27.12.40.0","230626RT","5901988185503","OE - Capot avant UCB 160-250 3P, L450, 5M / 300, vertical, levier","OE - Front cover UCB 160-250 3P, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. UCB 160-250 3P, W450, 5M (250MM) VERT.","OE - Előlap UCB 160-250 3P, W450, 5M / 300, függőleges, kar"]
["18590","OE - Osłona czołowa UCB 400 3P, W450, 9M / 300, pionowo, dźwignia",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","18590","SZT","85389099","27.12.40.0","230626RT","5901988185909","OE - Capot avant UCB 400 3P, L450, 9M / 300, vertical, levier","OE - UCB 400 3P, W450, 9M / 300 front visor, Vertical, Lever","OM- TAPA TROQ. UCB 400 3P, W450, 9M (450MM) VERT.","OE - Előlap UCB 400 3P, W450, 9M / 300, függőleges, kar"]
["18591","OE - Osłona czołowa UCB 400 4P, W450, 9M / 300, pionowo, dźwignia",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","18591","SZT","85389099","27.12.40.0","230626RT","5901988185916","OE - Couvercle avant UCB 400 4P, L450, 9M / 300, vertical, levier","OE - UCB 400 4P, W450, 9M / 300 front visor, Vertical, Lever","OM- TAPA TROQ. UCB 400 4P, W450, 9M (450MM) VERT.","OE - Első burkolat UCB 400 4P, W450, 9M / 300, függőleges, kar"]
["18592","OE - Osłona czołowa UCB 630-800 3P, W450, 9M / 300, pionowo, dźwignia",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","18592","SZT","85389099","27.12.40.0","230626RT","5901988185923","OE - Capot avant UCB 630-800 3P, L450, 9M / 300, vertical, levier","OE - Front cover UCB 630-800 3P, W450, 9M / 300, Vertical, Lever","OM- TAPA TROQ. UCB 630-800 3P, W450, 9M (450MM) VERT.","OE - Előlap UCB 630-800 3P, W450, 9M / 300, függőleges, kar"]
["18635","OE - Osłona czołowa HGP 250, UPB 100-250 3P, W650, 3M / 500, poziomo, dźwignia",63.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18635","SZT","85389099","27.12.40.0","230626RT","5901988186357","OE - Couvercle avant HGP 250, UPB 100-250 3P, L650, 3M / 500, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 3P, W650, 3M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 3P, W650, 3M (150MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 3P, W650, 3M / 500, vízszintes, kar"]
["18642","OE - Osłona czołowa UAB 100 3/4P, W650, 4M / 500, pionowo, dźwignia",76.5,"1-ZE-01",null,null,"OE_ACB_COVERS","18642","SZT","85389099","27.12.40.0","230626RT","5901988186425","OE - Couvercle avant UAB 100 3 / 4P, L650, 4M / 500, vertical, levier","OE - Front visor UAB 100 3 / 4P, W650, 4M / 500, Vertical, Lever","OE- TAPA TROQ. UAB 100 3/4P, W650, 4M / 500, VERT.","OE - Első burkolat UAB 100 3/4P, W650, 4M / 500, függőleges, kar"]
["18645","OE - Osłona czołowa HGP 250, UPB 100-250 4P, W650, 4M / 500, poziomo, dźwignia",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","18645","SZT","85389099","27.12.40.0","230626RT","5901988186456","OE - Couvercle avant HGP 250, UPB 100-250 4P, L650, 4M / 500, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 4P, W650, 4M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 4P, W650, 4M (200MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 4P, W650, 4M / 500, vízszintes, kar"]
["18646","OE - Osłona czołowa UPB 400-630 3P, W650, 4M / 500, poziomo, dźwignia",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","18646","SZT","85389099","27.12.40.0","230626RT","5901988186463","OE - Panneau avant UPB 400-630 3P, L650, 4M / 500, horizontal, levier","OE - Front cover UPB 400-630 3P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. UPB 400-630 3P, W650, 4M (200MM)  HORIZ.","OE - Első burkolat UPB 400-630 3P, W650, 4M / 500, vízszintes, kar"]
["18650","OE - Osłona czołowa HGP 250, UPB 100-250 3/4P, W650, 5M / 500, pionowo, dźwignia",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18650","SZT","85389099","27.12.40.0","230626RT","5901988186500","OE - Couvercle avant HGP 250, UPB 100-250 3 / 4P, L650, 5M / 500, vertical, levier","OE - Front visor HGP 250, UPB 100-250 3 / 4P, W650, 5M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGP250 3/4P, W650, 5M (250MM) VERT.","OE - Első burkolat HGP 250, UPB 100-250 3/4P, W650, 5M / 500, függőleges, kar"]
["18652","OE - OSŁONA CZOŁOWA UAB 100 3/4P, W650, 5M / 500, PIONOWO, DŹWIGNIA",85.3,"1-ZE-01",null,null,"OE_ACB_COVERS","18652","SZT","85389099","27.12.40.0","230626RT","5901988186524","OE - CAPOT AVANT UAB 100 3/4P, L650, 5M / 500, VERTICAL, LEVIER","OE - Front cover UAB 100 3/4P, W650, 5M / 500, Vertical, Lever","*OE - TAPA DELANTERA UAB 100 3/4P, W650, 5M / 500, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT UAB 100 3/4P, W650, 5M / 500, FÜGGŐLEGES, KAR"]
["18656","OE - Osłona czołowa UPB 400-630 4P, W650, 5M / 500, poziomo, dźwignia",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18656","SZT","85389099","27.12.40.0","230626RT","5901988186562","OE - Panneau avant UPB 400-630 4P, L650, 5M / 500, horizontal, levier","OE - Front cover UPB 400-630 4P, W650, 5M / 500, Horizontal, Lever","OE- TAPA TROQ. UPB 400-630 4P, W650, 5M (250MM)  HORIZ.","OE - Első burkolat UPB 400-630 4P, W650, 5M / 500, vízszintes, kar"]
["18690","OE - Osłona czołowa 1x UPB 400-630 3/4P, W650, 9M / 500, pionowo, dźwignia",125.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18690","SZT","85389099","27.12.40.0","230626RT","5901988186906","OE - Panneau avant 1x UPB 400-630 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 1x UPB 400-630 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. 1X UPB 400-630 3/4P, W650, 9M/500, VERTIC. ","OE - Első burkolat 1x UPB 400-630 3/4P, W650, 9M / 500, függőleges, kar"]
["18691","OE - Osłona czołowa 2x UPB 400-630 3/4P, W650, 9M / 500, pionowo, dźwignia",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18691","SZT","85389099","27.12.40.0","230626RT","5901988186913","OE - Panneau avant 2x UPB 400-630 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 2x UPB 400-630 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. UPB 400-630 3/4P, W650, 9M (450MM)  VERT.","OE - Előlap 2x UPB 400-630 3/4P, W650, 9M / 500, függőleges, kar"]
["18706","OE - Osłona czołowa UCB 1000-1250 3/4P, W650, 12M / 500, pionowo, silnik",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18706","SZT","85389099","27.12.40.0","230626RT","5901988187064","OE - Capot avant UCB 1000-1250 3 / 4P, L650, 10M / 500, verticalement, moteur","OE - Front cover UCB 1000-1250 3 / 4P, W650, 12M / 500, Vertical, engine","OE- TAPA TROQ. UCB 1000-1250 3/4P, W650, 10M (500MM)  VERT.","OE - Első burkolat UCB 1000-1250 3/4P, W650, 12M / 500, függőleges, motor"]
["18709","OE - Osłona czołowa UAN 06-32 3/4P, A, W650, 10M / 500, wysuwny",157.6,"1-ZE-01",null,null,"OE_ACB_COVERS","18709","SZT","85389099","27.12.40.0","230626RT","5901988187095","OE - Couvercle avant UAN 06-32 3 / 4P, A, L650, 10M / 500, débrochable","OE - Front cover UAN 06-32 3 / 4P, A, W650, 10M / 500, withdrawable","OE- TAPA TROQ. UAN TIPO A 06-32 3/4P, W650, 10M (500MM)  EXTR.","OE - Előlap UAN 06-32 3/4P, A, W650, 10M / 500, kihúzható"]
["18710","OE - Osłona czołowa UAN 06-32 3/4P, B, W650, 10M / 500, wysuwny",157.6,"1-ZE-01",null,null,"OE_ACB_COVERS","18710","SZT","85389099","27.12.40.0","230626RT","5901988187101","OE - Couvercle avant UAN 06-32 3 / 4P, B, L650, 10M / 500, débrochable","OE - Front cover UAN 06-32 3 / 4P, B, W650, 10M / 500, Removable","OE- TAPA TROQ. UAN TIPO B 06-32 3/4P, W650, 10M (500MM)  EXTR.","OE - Előlap UAN 06-32 3/4P, B, W650, 10M / 500, kihúzható"]
["18722","OE - Osłona czołowa UCB/UCD 1000-1250 3P, W650, 12M / 500, pionowo, dźwignia",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","18722","SZT","85389099","27.12.40.0","230626RT","5901988187224","OE - Capot avant UCB 1000-1250 3P, L650, 12M / 500, vertical, levier","OE - Front cover UCB / UCD 1000-1250 3P, W650, 12M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 3P, W650, 12M (600MM)  VERT.","OE - Előlap UCB/UCD 1000-1250 3P, W650, 12M / 500, függőleges, kar"]
["18734","OE - Osłona czołowa UCB 100 3P, W650, 3M / 500, poziomo, dźwignia",63.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18734","SZT","85389099","27.12.40.0","230626RT","5901988187347","OE - Capot avant UCB 100 3P, L650, 3M / 500, horizontal, levier","OE - Front cover UCB 100 3P, W650, 3M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 100 3P, W650, 3M (150MM)  HORIZ.","OE - Előlap UCB 100 3P, W650, 3M / 500, vízszintes, kar"]
["18735","OE - Osłona czołowa UCB 160-250 3P, W650, 3M / 500, poziomo, dźwignia",63.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18735","SZT","85389099","27.12.40.0","230626RT","5901988187354","OE - Capot avant UCB 160-250 3P, L650, 3M / 500, horizontal, levier","OE - Front cover UCB 160-250 3P, W650, 3M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 3P, W650, 3M (150MM)  HORIZ.","OE - Előlap UCB 160-250 3P, W650, 3M / 500, vízszintes, kar"]
["18744","OE - Osłona czołowa UCB 100 4P, W650, 4M / 500, poziomo, dźwignia",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","18744","SZT","85389099","27.12.40.0","230626RT","5901988187446","OE - Capot avant UCB 100 4P, L650, 4M / 500, horizontal, levier","OE - Front cover UCB 100 4P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 100 4P, W650, 4M (200MM)  HORIZ.","OE - Előlap UCB 100 4P, W650, 4M / 500, vízszintes, kar"]
["18745","OE - Osłona czołowa UCB 160-250 4P, W650, 4M / 500, poziomo, dźwignia",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","18745","SZT","85389099","27.12.40.0","230626RT","5901988187453","OE - Capot avant UCB 160-250 4P, L650, 4M / 500, horizontal, effet de levier","OE - Front cover UCB 160-250 4P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 4P, W650, 4M (200MM)  HORIZ.","OE - Előlap UCB 160-250 4P, W650, 4M / 500, vízszintes, kar"]
["18746","OE - Osłona czołowa UCB 400 3P, W650, 4M / 500, poziomo, dźwignia",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","18746","SZT","85389099","27.12.40.0","230626RT","5901988187460","OE - Capot avant UCB 400 3P, L650, 4M / 500, horizontal, levier","OE - Front cover UCB 400 3P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 400 3P, W650, 4M (200MM)  HORIZ.","OE - Előlap UCB 400 3P, W650, 4M / 500, vízszintes, kar"]
["18749","OE - Osłona czołowa UCB 100 3/4P, W650, 5M / 500, pionowo, dźwignia",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18749","SZT","85389099","27.12.40.0","230626RT","5901988187491","OE - Couvercle avant UCB 100 3 / 4P, L650, 5M / 500, vertical, levier","OE - Front cover UCB 100 3 / 4P, W650, 5M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 100 3/4P, W650, 5M (250MM)  VERT.","OE - Előlap UCB 100 3/4P, W650, 5M / 500, függőleges, kar"]
["18750","OE - Osłona czołowa UCB 160-250 3/4P, W650, 5M / 500, pionowo, dźwignia",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18750","SZT","85389099","27.12.40.0","230626RT","5901988187507","OE - Couvercle avant UCB 160-250 3 / 4P, L650, 5M / 500, vertical, levier","OE - Front cover UCB 160-250 3 / 4P, W650, 5M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 160-250 3/4P, W650, 5M (250MM)  VERT.","OE - Előlap UCB 160-250 3/4P, W650, 5M / 500, függőleges, kar"]
["18756","OE - Osłona czołowa UCB 400 4P, W650, 5M / 500, poziomo, dźwignia",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18756","SZT","85389099","27.12.40.0","230626RT","5901988187569","OE - Couvercle avant UCB 400 4P, L650, 5M / 500, horizontal, levier","OE - Front Shield UCB 400 4P, W650, 5M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 400 4P, W650, 5M (250MM)  HORIZ.","OE - Előlap UCB 400 4P, W650, 5M / 500, vízszintes, kar"]
["18767","OE - Osłona czołowa UCB 630-800 3P, W650, 6M / 500, poziomo, dźwignia",82.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","18767","SZT","85389099","27.12.40.0","230626RT","5901988187675","OE - Capot avant UCB 630-800 3P, L650, 6M / 500, horizontal, levier","OE - Front cover UCB 630-800 3P, W650, 6M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 630-800 3P, W650, 6M (300MM)  HORIZ.","OE - Előlap UCB 630-800 3P, W650, 6M / 500, vízszintes, kar"]
["18768","OE - Osłona czołowa UCB 1000-1250 3P, W650, 6M / 500, poziomo, dźwignia",82.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","18768","SZT","85389099","27.12.40.0","230626RT","5901988187682","OE - Capot avant UCB 1000-1250 3P, L650, 6M / 500, horizontal, effet de levier","OE - Front cover UCB 1000-1250 3P, W650, 6M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 1000-1250 3P, W650, 6M (300MM)  HORIZ.","OE - Előlap UCB 1000-1250 3P, W650, 6M / 500, vízszintes, kar"]
["18769","OE - Osłona czołowa UCB 630-800 3P, W650, 6M / 500, poziomo, silnik",82.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","18769","SZT","85389099","27.12.40.0","230626RT","5901988187699","OE - Capot avant UCB 630-800 3P, L650, 6M / 500, horizontal, moteur","OE - Front cover UCB 630-800 3P, W650, 6M / 500, Horizontal, Engine","OE- TAPA TROQ. UCB 630-800 3P, W650, 6M (300MM)  HORIZ.","OE - Első burkolat UCB 630-800 3P, W650, 6M / 500, vízszintes, motor"]
["18777","OE - Osłona czołowa UCB 630-800 4P, W650, 7M / 500, poziomo, dźwignia",108.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18777","SZT","85389099","27.12.40.0","230626RT","5901988187774","OE - Capot avant UCB 630-800 4P, L650, 7M / 500, horizontal, effet de levier","OE - Front cover UCB 630-800 4P, W650, 7M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 630-800 4P, W650, 7M (350MM)  HORIZ.","OE - Előlap UCB 630-800 4P, W650, 7M / 500, vízszintes, kar"]
["18778","OE - Osłona czołowa UCB 1000-1250 4P, W650, 7M / 500, poziomo, dźwignia",108.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18778","SZT","85389099","27.12.40.0","230626RT","5901988187781","OE - Capot avant UCB 1000-1250 4P, L650, 7M / 500, horizontal, effet de levier","OE - Front cover UCB 1000-1250 4P, W650, 7M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 1000-1250 4P, W650, 7M (350MM)  HORIZ.","OE - Előlap UCB 1000-1250 4P, W650, 7M / 500, vízszintes, kar"]
["18779","OE - Osłona czołowa UCB 630-800 4P, W650, 7M / 500, poziomo, silnik",108.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","18779","SZT","85389099","27.12.40.0","230626RT","5901988187798","OE - Capot avant UCB 630-800 4P, L650, 7M / 500, horizontal, moteur","OE - Front cover UCB 630-800 4P, W650, 7M / 500, Horizontal, Engine","OE- TAPA TROQ. UCB 630-800 4P, W650, 7M (350MM)  HORIZ.","OE - Első burkolat UCB 630-800 4P, W650, 7M / 500, vízszintes, motor"]
["18787","OE - Osłona czołowa UCB 1000-1250 3P, W650, 6M / 500, poziomo, silnik",79,"1-ZE-01",null,null,"OE_MCCB_COVERS","18787","SZT","85389099","27.12.40.0","230626RT","5901988187873","OE - Couvercle avant UCB 1000-1250 3P, L650, 6M / 500, horizontal, moteur","OE - Front cover UCB 1000-1250 3P, W650, 6M / 500, Horizontal, Engine","OE- TAPA TROQ. UCB 1000-1250 3P, W650, 6M (300MM)  HORIZ.","OE - Első burkolat UCB 1000-1250 3P, W650, 6M / 500, vízszintes, motor"]
["18790","OE - Osłona czołowa 1x UCB 400 3/4P, W650, 9M / 500, pionowo, dźwignia",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18790","SZT","85389099","27.12.40.0","230626RT","5901988187903","OE - Couvercle avant 1x UCB 400 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 1x UCB 400 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. 1X UCB 400 3/4P, W650, 9M/500, VERTIC. ","OE - Első burkolat 1x UCB 400 3/4P, W650, 9M / 500, függőleges, kar"]
["18791","OE - Osłona czołowa 2x UCB 400 3/4P, W650, 9M / 500, pionowo, dźwignia",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18791","SZT","85389099","27.12.40.0","230626RT","5901988187910","OE - Couvercle avant 2x UCB 400 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 2x UCB 400 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 400 3/4P, W650, 9M (450MM)  VERT.","OE - Első burkolat 2x UCB 400 3/4P, W650, 9M / 500, függőleges, kar"]
["18792","OE - Osłona czołowa UCB 630-800 3P, W650, 9M / 500, pionowo, dźwignia",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18792","SZT","85389099","27.12.40.0","230626RT","5901988187927","OE - Capot avant UCB 630-800 3P, L650, 9M / 500, vertical, levier","OE - Front cover UCB 630-800 3P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 630-800 3P, W650, 9M (450MM)  VERT.","OE - Előlap UCB 630-800 3P, W650, 9M / 500, függőleges, kar"]
["18793","OE - Osłona czołowa UCB 630-800 4P, W650, 9M / 500, pionowo, dźwignia",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18793","SZT","85389099","27.12.40.0","230626RT","5901988187934","OE - Couvercle avant UCB 630-800 4P, L650, 9M / 500, vertical, levier","OE - Front cover UCB 630-800 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 630-800 4P, W650, 9M (450MM)  VERT.","OE - Első burkolat UCB 630-800 4P, W650, 9M / 500, függőleges, kar"]
["18794","OE - Osłona czołowa UAN 06-20 3/4P, A, W650, 9M / 500, na stałe",157.6,"1-ZE-01",null,null,"OE_ACB_COVERS","18794","SZT","85389099","27.12.40.0","230626RT","5901988187941","OE - Couvercle avant UAN 06-20 3 / 4P, A, L650, 9M / 500, fixe","OE - Front cover UAN 06-20 3 / 4P, A, W650, 9M / 500, permanent","OE- TAPA TROQ. UAN 06-20 3/4P, A, W650, 9M (450MM)  FIJO","OE - Előlap UAN 06-20 3/4P, A, W650, 9M / 500, állandó"]
["18795","OE - Osłona czołowa UAN 08-40 3/4P, B, W650, 9M / 500, na stałe",157.6,"1-ZE-01",null,null,"OE_ACB_COVERS","18795","SZT","85389099","27.12.40.0","230626RT","5901988187958","OE - Couvercle avant UAN 08-40 3 / 4P, B, L650, 9M / 500, fixe","OE - Front cover UAN 08-40 3 / 4P, B, W650, 9M / 500, permanent","OE- TAPA TROQ. UAN 08-40 3/4P, B, W650, 9M (450MM)  FIJO","OE - Előlap UAN 08-40 3/4P, B, W650, 9M / 500, állandó"]
["18835","OE - Osłona czołowa HGP 250, UPB 100-250 3P, W850, 3M / 700, poziomo, dźwignia",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","18835","SZT","85389099","27.12.40.0","230626RT","5901988188351","OE - Couvercle avant HGP 250, UPB 100-250 3P, L850, 3M / 700, horizontal, levier","OE - Front hood HGP 250, UPB 100-250 3P, W850, 3M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 3P, W850, 3M (150MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 3P, W850, 3M / 700, vízszintes, kar"]
["18845","OE - Osłona czołowa HGP 250, UPB 100-250 4P, W850, 4M / 700, poziomo, dźwignia",85,"1-ZE-01",null,null,"OE_MCCB_COVERS","18845","SZT","85389099","27.12.40.0","230626RT","5901988188450","OE - Capot avant HGP 250, UPB 100-250 4P, L850, 4M / 700, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 4P, W850, 4M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 4P, W850, 4M (200MM) HORIZ. ","OE - Első burkolat HGP 250, UPB 100-250 4P, W850, 4M / 700, vízszintes, kar"]
["18846","OE - Osłona czołowa UPB 400-630 3P, W850, 4M / 700, poziomo, dźwignia",85,"1-ZE-01",null,null,"OE_MCCB_COVERS","18846","SZT","85389099","27.12.40.0","230626RT","5901988188467","OE - Couvercle avant UPB 400-630 3P, L850, 4M / 700, horizontal, levier","OE - Front cover UPB 400-630 3P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. UPB 400-630 3P, W850, 4M (200MM)  HORIZ.","OE - Első burkolat UPB 400-630 3P, W850, 4M / 700, vízszintes, kar"]
["18850","OE - Osłona czołowa HGP 250, UPB 100-250 3/4P, W850, 5M / 700, pionowo, dźwignia",87.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","18850","SZT","85389099","27.12.40.0","230626RT","5901988188504","OE - Couvercle avant HGP 250, UPB 100-250 3 / 4P, L850, 5M / 700, vertical, levier","OE - Front visor HGP 250, UPB 100-250 3 / 4P, W850, 5M / 700, Vertical, Lever","ZEN- TAPA TROQ. HGP250 3/4P, W850, 5M (250MM) VERT.","OE - Első burkolat HGP 250, UPB 100-250 3/4P, W850, 5M / 700, függőleges, kar"]
["18856","OE - Osłona czołowa UPB 400-630 4P, W850, 5M / 700, poziomo, dźwignia",87.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","18856","SZT","85389099","27.12.40.0","230626RT","5901988188566","OE - Capot avant UPB 400-630 4P, L850, 5M / 700, horizontal, levier","OE - Front cover UPB 400-630 4P, W850, 5M / 700, Horizontal, Lever","OE- TAPA TROQ. UPB 400-630 4P, W850, 5M (250MM)  HORIZ.","OE - Első burkolat UPB 400-630 4P, W850, 5M / 700, vízszintes, kar"]
["18891","OE - Osłona czołowa UPB 400-630 3/4P, W850, 9M / 700, pionowo, dźwignia",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","18891","SZT","85389099","27.12.40.0","230626RT","5901988188917","OE - Panneau avant UPB 400-630 3 / 4P, L850, 9M / 700, vertical, levier","OE - Front visor UPB 400-630 3 / 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. UPB 400-630 3/4P, W850, 9M (450MM)  VERT.","OE - Első burkolat UPB 400-630 3/4P, W850, 9M / 700, függőleges, kar"]
["18909","OE - Osłona czołowa UAN 06-32 3/4P,A, W850, 10M / 700, wysuwny",176,"1-ZE-01",null,null,"OE_ACB_COVERS","18909","SZT","85389099","27.12.40.0","230626RT","5901988189099","OE - Couvercle avant UAN 06-32 3 / 4P,A, L850, 10M / 700, débrochable","OE - Front cover UAN 06-32 3 / 4P, W850, 10M / 700, Removable","OE- TAPA TROQ. UAN A 06-32 3/4P, W850, 10M (500MM)  EXTR.","OE - Előlap UAN 06-32 3/4P,A, W850, 10M / 700, kihúzható"]
["18910","OE - Osłona czołowa UAN 06-32 3/4P,B, W850, 10M / 700, wysuwny",176,"1-ZE-01",null,null,"OE_ACB_COVERS","18910","SZT","85389099","27.12.40.0","230626RT","5901988189105","OE - Couvercle avant UAN 06-32 3 / 4P,B, L850, 10M / 700, débrochable","OE - Front cover UAN 06-32 3 / 4P, B, W850, 10M / 700, Removable","OE- TAPA TROQ. UAN B 06-32 3/4P, W850, 10M (500MM)  EXTR.","OE - Előlap UAN 06-32 3/4P,B, W850, 10M / 700, kihúzható"]
["18920","OE - Osłona czołowa 2x UCB 1000-1250 3P, W850, 12M / 700, pionowo, dźwignia",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18920","SZT","85389099","27.12.40.0","230626RT","5901988189204","OE - Capot avant 2x UCB 1000-1250 3P, L850, 12M / 700, vertical, levier","OE - Front cover 2x UCB 1000-1250 3P, W850, 12M / 700, Vertical, Lever","OE- TAPA TROQ. 2X UCB 1000-1250 3P, W850, 12M (600MM)  VERT.","OE - Első burkolat 2x UCB 1000-1250 3P, W850, 12M / 700, függőleges, kar"]
["18921","OE - Osłona czołowa 2x UCB 1000-1250 4P, W850, 12M / 700, pionowo, dźwignia",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18920","SZT","85389099","27.12.40.0","230626RT","5901988189211","OE - Capot avant 2x UCB 1000-1250 4P, L850, 12M / 700, vertical, levier","OE - Front cover 2x UCB 1000-1250 4P, W850, 12M / 700, Vertical, Lever","OE- TAPA TROQ. 2X UCB 1000-1250 4P, W850, 12M (600MM)  VERT.","OE - Első burkolat 2x UCB 1000-1250 4P, W850, 12M / 700, függőleges, kar"]
["18922","OE - Osłona czołowa UCB 1000-1250 3P, W850, 12M / 700, pionowo, dźwignia",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18922","SZT","85389099","27.12.40.0","230626RT","5901988189228","OE - Capot avant UCB 1000-1250 3P, L850, 12M / 700, vertical, levier","OE - Front cover UCB 1000-1250 3P, W850, 12M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 3P, W850, 12M (600MM)  VERT.","OE - Előlap UCB 1000-1250 3P, W850, 12M / 700, függőleges, kar"]
["18923","OE - Osłona czołowa UCB 1000-1250 4P, W850, 12M / 700, pionowo, dźwignia",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18922","SZT","85389099","27.12.40.0","230626RT","5901988189235","OE - Capot avant UCB 1000-1250 4P, L850, 12M / 700, vertical, levier","OE - Front cover UCB 1000-1250 4P, W850, 12M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 4P, W850, 12M (600MM)  VERT.","OE - Előlap UCB 1000-1250 4P, W850, 12M / 700, függőleges, kar"]
["18934","OE - Osłona czołowa UCB 100 3P, W850, 3M / 700, poziomo, dźwignia",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","18934","SZT","85389099","27.12.40.0","230626RT","5901988189341","OE - Capot avant UCB 100 3P, L850, 3M / 700, horizontal, levier","OE - Front cover UCB 100 3P, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 100 3P, W850, 3M (150MM)  HORIZ.","OE - Előlap UCB 100 3P, W850, 3M / 700, vízszintes, kar"]
["18935","OE - Osłona czołowa UCB 160-250 3P, W850, 3M / 700, poziomo, dźwignia",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","18935","SZT","85389099","27.12.40.0","230626RT","5901988189358","OE - Capot avant UCB 160-250 3P, L850, 3M / 700, horizontal, levier","OE - Front cover UCB 160-250 3P, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 3P, W850, 3M (150MM)  HORIZ.","OE - Előlap UCB 160-250 3P, W850, 3M / 700, vízszintes, kar"]
["18944","OE - Osłona czołowa UCB 100 4P, W850, 4M / 700, poziomo, dźwignia",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18944","SZT","85389099","27.12.40.0",null,"5901988189440","OE - Capot avant UCB 100 4P, L850, 4M / 700, horizontal, levier","OE - Front cover UCB 100 4P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 100 4P, W850, 4M (200MM)  HORIZ.","OE - Előlap UCB 100 4P, W850, 4M / 700, vízszintes, kar"]
["18945","OE - Osłona czołowa UCB 160-250 4P, W850, 4M / 700, poziomo, dźwignia",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18945","SZT","85389099","27.12.40.0","230626RT","5901988189457","OE - Capot avant UCB 160-250 4P, L850, 4M / 700, horizontal, effet de levier","OE - Front cover UCB 160-250 4P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 4P, W850, 4M (200MM)  HORIZ.","OE - Előlap UCB 160-250 4P, W850, 4M / 700, vízszintes, kar"]
["18946","OE - Osłona czołowa UCB 400 3P, W850, 4M / 700, poziomo, dźwignia",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","18946","SZT","85389099","27.12.40.0","230626RT","5901988189464","OE - Capot avant UCB 400 3P, L850, 4M / 700, horizontal, effet de levier","OE - Front cover UCB 400 3P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 400 3P, W850, 4M (200MM)  HORIZ.","OE - Előlap UCB 400 3P, W850, 4M / 700, vízszintes, kar"]
["18949","OE - Osłona czołowa UCB 100 3/4P, W850, 5M / 700, pionowo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","18949","SZT","85389099","27.12.40.0","230626RT","5901988189495","OE - Couvercle avant UCB 100 3 / 4P, L850, 5M / 700, vertical, levier","OE - Front cover UCB 100 3 / 4P, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 100 3/4P, W850, 5M (250MM)  VERT.","OE - Előlap UCB 100 3/4P, W850, 5M / 700, függőleges, kar"]
["18950","OE - Osłona czołowa UCB 160-250 3/4P, W850, 5M / 700, pionowo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","18950","SZT","85389099","27.12.40.0","230626RT","5901988189501","OE - Couvercle avant UCB 160-250 3 / 4P, L850, 5M / 700, vertical, levier","OE - Front cover UCB 160-250 3 / 4P, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 160-250 3/4P, W850, 5M (250MM)  VERT.","OE - Előlap UCB 160-250 3/4P, W850, 5M / 700, függőleges, kar"]
["18956","OE - Osłona czołowa UCB 400 4P, W850, 5M / 700, poziomo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","18956","SZT","85389099","27.12.40.0","230626RT","5901988189563","OE - Capot avant UCB 400 4P, L850, 5M / 700, horizontal, levier","OE - Front cover UCB 400 4P, W850, 5M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 400 4P, W850, 5M (250MM)  HORIZ.","OE - Előlap UCB 400 4P, W850, 5M / 700, vízszintes, kar"]
["18967","OE - Osłona czołowa UCB 630-800 3P, W850, 6M / 700, poziomo, dźwignia",100.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18967","SZT","85389099","27.12.40.0","230626RT","5901988189679","OE - Capot avant UCB 630-800 3P, L850, 6M / 700, horizontal, levier","OE - Front cover UCB 630-800 3P, W850, 6M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 630-800 3P, W850, 6M (300MM)  HORIZ.","OE - Előlap UCB 630-800 3P, W850, 6M / 700, vízszintes, kar"]
["18968","OE - Osłona czołowa UCB 1000-1250 3P, W850, 6M / 700, poziomo, dźwignia",100.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18968","SZT","85389099","27.12.40.0","230626RT","5901988189686","OE - Capot avant UCB 1000-1250 3P, L850, 6M / 700, horizontal, levier","OE - Front cover UCB 1000-1250 3P, W850, 6M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 1000-1250 3P, W850, 6M (300MM)  HORIZ.","OE - Előlap UCB 1000-1250 3P, W850, 6M / 700, vízszintes, kar"]
["18977","OE - Osłona czołowa UCB 630-800 4P, W850, 7M / 700, poziomo, dźwignia",125.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18977","SZT","85389099","27.12.40.0","230626RT","5901988189778","OE - Capot avant UCB 630-800 4P, L850, 7M / 700, horizontal, levier","OE - Front cover UCB 630-800 4P, W850, 7M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 630-800 4P, W850, 7M (350MM)  HORIZ.","OE - Előlap UCB 630-800 4P, W850, 7M / 700, vízszintes, kar"]
["18978","OE - Osłona czołowa UCB 1000-1250 4P, W850, 7M / 700, poziomo, dźwignia",125.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18978","SZT","85389099","27.12.40.0","230626RT","5901988189785","OE - Capot avant UCB 1000-1250 4P, L850, 7M / 700, horizontal, effet de levier","OE - Front cover UCB 1000-1250 4P, W850, 7M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 1000-1250 4P, W850, 7M (350MM)  HORIZ.","OE - Előlap UCB 1000-1250 4P, W850, 7M / 700, vízszintes, kar"]
["18979","OE - Osłona czołowa UCB 630-800 4P, W850, 7M / 700, poziomo, silnik",125.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","18979","SZT","85389099","27.12.40.0","230626RT","5901988189792","OE - Capot avant UCB 630-800 4P, L850, 7M / 700, horizontal, moteur","OE - Front cover UCB 630-800 4P, W850, 7M / 700, Horizontal, Engine","OE- TAPA TROQ. UCB 630-800 4P, W850, 7M (350MM)  HORIZ.","OE - Előlap UCB 630-800 4P, W850, 7M / 700,vízszintes, motor"]
["18991","OE - Osłona czołowa UCB 400 3/4P, W850, 9M / 700, pionowo, dźwignia",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18991","SZT","85389099","27.12.40.0","230626RT","5901988189914","OE - Couvercle avant UCB 400 3 / 4P, L850, 9M / 700, vertical, levier","OE - Front cover UCB 400 3 / 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 400 3/4P, W850, 9M (450MM)  VERT.","OE - Előlap UCB 400 3/4P, W850, 9M / 700, függőleges, kar"]
["18992","OE - Osłona czołowa UCB 630-800 3P, W850, 9M / 700, pionowo, dźwignia",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18992","SZT","85389099","27.12.40.0","230626RT","5901988189921","OE - Capot avant UCB 630-800 3P, L850, 9M / 700, vertical, levier","OE - Front cover UCB 630-800 3P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 630-800 3P, W850, 9M (450MM)  VERT.","OE - Előlap UCB 630-800 3P, W850, 9M / 700, függőleges, kar"]
["18993","OE - Osłona czołowa UCB 630-800 4P, W850, 9M / 700, pionowo, dźwignia",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","18993","SZT","85389099","27.12.40.0","230626RT","5901988189938","OE - Capot avant UCB 630-800 4P, L850, 9M / 700, vertical, levier","OE - Front cover UCB 630-800 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 630-800 4P, W850, 9M (450MM)  VERT.","OE - Előlap UCB 630-800 4P, W850, 9M / 700, függőleges, kar"]
["18994","OE - Osłona czołowa UAN 06-20 3/4P, A, W850, 9M / 700, na stałe",166.8,"1-ZE-01",null,null,"OE_ACB_COVERS","18994","SZT","85389099","27.12.40.0","230626RT","5901988189945","OE - Couvercle avant UAN 06-20 3 / 4P, A, L850, 9M / 700, permanent","OE - Front cover UAN 06-20 3 / 4P, A, W850, 9M / 700, permanent","OE- TAPA TROQ. UAN 06-20 3/4P, A, W850, 9M (450MM)  FIJO","OE - Előlap UAN 06-20 3/4P, A, W850, 9M / 700, állandó"]
["18996","OE - Osłona czołowa UAN 06-20 3/4P, B, W850, 9M / 700, na stałe",166.8,"1-ZE-01",null,null,"OE_ACB_COVERS","18996","SZT","85389099","27.12.40.0","230626RT","5901988189969","OE - Couvercle avant UAN 06-20 3 / 4P, B, L850, 9M / 700, permanent","OE - Front cover UAN 06-20 3 / 4P, B, W850, 9M / 700, permanent","OE- TAPA TROQ. UAN 06-20 3/4P, B, W850, 9M (450MM)  FIJO","OE - Előlap UAN 06-20 3/4P, B, W850, 9M / 700, állandó"]
["19000","ZENERGY IT - 12 WSPORNIKÓW PORZADKUJĄCYCH KABLE",116.6,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","39269097","22.29.29.0",null,"5901988190002","IT - 12 supports pour nettoyer les câbles","IT - 12 cable organizing brackets","OE IT- 12 SOPORT. PARA ORDENAR CABLES","ZENERGY IT - 12 KÁBELIRÁNYÍTÁSI TÁMOGATÁS"]
["19150","OE - WSPORNIKI BOCZNE RACK 19, 39U  ( 4 szt. ) obudowa D=775 W=600",552,null,null,null,"IT_SUPPORT","19150",null,null,null,"240201PW",null,"OE - Supports latéraux Rack 19, armoire de 39U (4 pcs) D = 775 W = 600","OE - Side brackets Rack 19, 42U (4 pcs) cabinet D = 775 W = 600","OE- Soportes laterales Rack 19, 39U (4 uds) armario D = 775 W = 600","OE - RACK OLDALTARTÓK 19, 39U (4 db) ház D=775 W=600"]
["19151","OE - Wymaskowanie pionowych wsporników bocznych RACK 19, 39U ( dół ) obudowy W=600",52.9,null,6.6666666666666666E-2,1,"IT_SUPPORT","19151",null,null,null,"240205PW",null,"OE - Masquage des supports latéraux verticaux du RACK 19, 39U (bas) du boîtier W=600","OE - Masking the vertical side supports of RACK 19, 39U (bottom) of the W=600 case","OE - Enmascaramiento de los soportes laterales verticales del RACK 19, 39U (inferior) de la carcasa W=600","OE - A W=600 ház RACK 19, 39U (alul) függőleges oldaltámaszainak maszkolása"]
["19152","OE - WSPORNIKI BOCZNE RACK 19, 41U  ( 4 szt. ) obudowa D=775 W=600",563.5,null,6.6666666666666666E-2,1,"IT_SUPPORT","19152",null,null,null,"240205PW",null,"OE - Supports latéraux Rack 19, armoire de 41U (4 pcs) D = 775 W = 600","OE - Side brackets Rack 19, 39U (4 pcs) cabinet D = 775 W = 600","OE- Soportes laterales Rack 19, 41U (4 uds) armario D = 775 W = 600","OE - RACK OLDALTARTÓK 19, 41U (4 db) ház D=775 W=600"]
["19158","IT - WSPORNIK PŁYT MONTAŻOWYCH/IZOLATORÓW H36 RACK 19, D=775",108.1,null,8.3333333333333329E-2,1,"IT_SUPPORT","19158",null,null,null,"240207PW",null,"IT - SUPPORT POUR PLAQUES DE MONTAGE/ISOLANTS H36 RACK 19, D=775","IT - SUPPORT FOR MOUNTING PLATES/INSULATORS H36 RACK 19, D=775","IT - SOPORTE PARA MONTAJE DE PLACAS/AISLANTES H36 RACK 19, D=775","IT - TÁMOGATÁS LEMEZEK/SZIGETELŐK SZERELÉSÉHEZ H36 RACK 19, D=775"]
["19160","ZENERGY - WSPORNIKI BOCZNE RACK 19, 42U  ( 4 SZT ) SZAFA  D=1000 W=650",535.70000000000005,"1-ZE-01",1.6666666666666666E-2,1,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988191603","OE - Supports latéraux Rack 19, armoire de 42U (4 pcs) D = 1000 W = 650","OE - Side brackets Rack 19, 42U (4 pcs) cabinet D = 1000 W = 650","OE- Soportes laterales Rack 19, 42U (4 uds) armario D = 1000 W = 650","ZENERGY - OLDALTÁMASZTÓ RACK 19, 42U (4 DB) SZEKRÉNY D=1000 W=650"]
["19180","ZENERGY - WSPORNIKI BOCZNE RACK 19, 42U  ( 4 SZT ) SZAFA  D=1000 W=800",583.20000000000005,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988191801","OE - Supports latéraux Rack 19, armoire de 42U (4 pcs) D = 1000 W = 800","OE - Side brackets Rack 19, 42U (4 pcs) cabinet D = 1000 W = 800","OE- Soportes laterales Rack 19, 42U (4 uds) armario D = 1000 W = 800","ZENERGY - OLDALTÁMASZTÓ RACK 19, 42U (4 DB) SZEKRÉNY D=1000 W=800"]
["19181","ZENERGY - WSPORNIKI BOCZNE RACK 19, 47U  ( 4 SZT ) SZAFA  D=1000 W=800 H=2250",622.1,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988191818","OE - Supports latéraux Rack 19, armoire de 47U (4 pièces) D = 1000 W = 800 H = 2250","OE - Side brackets Rack 19, 47U (4 pcs) cabinet D = 1000 W = 800 H = 2250","OE- Soportes laterales Rack 19, 47U (4 uds) armario D = 1000 W = 800 H = 2250","ZENERGY - OLDALTÁMASZTÓ RACK 19, 47U (4 DB) SZEKRÉNY D=1000 W=800 H=2250"]
["19191","ZENERGY - IT SZUFLADA BEZPIECZEŃSTWA COKOŁU PRZÓD + TYŁ, H=100, W=800",271.10000000000002,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988191917","OE - Tiroir de sécurité informatique, plinthe avant + arrière, H = 100, L = 800","OE - IT front + back plinth safety drawer, H = 100, W = 800","OE- Cajón de seguridad con ZOCALO frontal + trasero IT, H = 100, W = 800","ZENERGY - IT LÁLTAL BIZTONSÁGI FIÓK ELSŐ + HÁTSÓ, H=100, W=800"]
["19201","IZOLATOR WSPORCZY ROZSTAW 60MM SZYN 30X10MM 3P",19,"1-ZE-01",null,null,"OE_INSULATORS",null,"SZT","85469010",null,"110426LK","5901988192013","Espacement des isolants de soutien Rails 60mm 30x10mm 3P","Support insulator, spacing of 60mm busbars 30x10mm 3P","Aislador soporte, distancia entre barras 60mm 30x10mm 3P","OSZTASZIGETELŐ HELY 60MM BUSZ 30X10MM 3P"]
["19322","OE - OSŁONA CZOŁOWA HGM 1000-1250 3P, W400, 12M / 300, PIONOWO, DŹWIGNIA",110,"1-ZE-01",null,null,"OE_MCCB_COVERS","19322","SZT","85389099",null,"230626RT","5901988193225","OE - CAPOT AVANT HGM 1000-1250 3P, L400, 12M / 300, VERTICAL, LEVIER","OE - Front Cover HGM 1000-1250 3P, W400, 12M / 300, Vertical, Lever","*OE - TAPA DELANTERA HGM 1000-1250 3P, W400, 12M / 300, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 3P, W400, 12M / 300, FÜGGŐLEGES, KAR"]
["19350","OE - Osłona czołowa HGM 100 3/4P, W400, 5M / 250, pionowo, dźwignia",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","19350","SZT","85381000","27.12.40.0","230626RT","5901988193508","OE - Couvercle avant HGM 100 3 / 4P, L400, 5M / 250, vertical, levier","OE - HGM 100 3 / 4P front visor, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 100 3/4P, W400, 5M (250MM)  VERT.","OE - Első burkolat HGM 100 3/4P, W400, 5M / 250, függőleges, kar"]
["19351","OE - Osłona czołowa HGM 125 4P, W400, 5M / 250, pionowo, dźwignia",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","19351","SZT","85381000","27.12.40.0","230626RT","5901988193515","OE - HGM 125 4P, L400, capot avant 5M / 250, vertical, levier","OE - HGM 125 4P front visor, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 125 3/4P, W400, 5M (250MM)  VERT.","OE - Első burkolat HGM 125 4P, W400, 5M / 250, függőleges, kar"]
["19352","OE - Osłona czołowa HGM 160-250 4P, W400, 5M / 250, pionowo, dźwignia",59,"1-ZE-01",null,null,"OE_MCCB_COVERS","19352","SZT","85381000","27.12.40.0","230626RT","5901988193522","OE - Couvercle avant HGM 160-250 4P, L400, 5M / 250, vertical, levier","OE - Front Cover HGM 160-250 4P, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 160-250 3/4P, W400, 5M (250MM)  VERT.","OE - Első burkolat HGM 160-250 4P, W400, 5M / 250, függőleges, kar"]
["19393","OE - Osłona czołowa HGM 400 3/4P, W400, 9M / 250, pionowo, dźwignia",99.9,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19393","SZT","85389099","27.12.40.0","230626RT","5901988193935","OE - Couvercle avant HGM 400 3 / 4P, L400, 9M / 250, vertical, levier","OE - HGM 400 3 / 4P front visor, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 400 3/4P, W400, 9M (450MM)  VERT.","OE - Első burkolat HGM 400 3/4P, W400, 9M / 250, függőleges, kar"]
["19394","OE - Osłona czołowa HGM 630-800 3P, W400, 9M / 250, pionowo, dźwignia",93.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","19394","SZT","85389099",null,"230626RT","5901988193942","OE - Couvercle avant HGM 630-800 3P, L400, 9M / 250, vertical, levier","OE - Front Cover HGM 630-800 3P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 630-800 3P, W400, 9M (450MM)  VERT.","OE - Első burkolat HGM 630-800 3P, W400, 9M / 250, függőleges, kar"]
["19522","OE - OSŁONA CZOŁOWA HGM 1000-1250 3P, W450, 12M / 300, PIONOWO, DŹWIGNIA",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","19522","SZT","85389099",null,"230626RT","5901988195229","OE - COUVERCLE HGM 1000-1250 3P, L450, 12M/300, VERTICAL, LEVIER","OE - Cover HGM 1000-1250 3P, W450, 12M / 300, Vertical, Lever","*OE - CUBIERTA HGM 1000-1250 3P, W450, 12M / 300, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 3P, W450, 12M / 300, FÜGGŐLEGES, KAR"]
["19523","OE - OSŁONA CZOŁOWA HGM 1000-1250 4P, W450, 12M / 300, PIONOWO, DŹWIGNIA",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","19522","SZT","85389099",null,"230626RT","5901988195236","OE - COUVERCLE HGM 1000-1250 4P, L450, 12M/300, VERTICAL, LEVIER","OE - Front Cover HGM 1000-1250 4P, W450, 12M / 300, Vertical, Lever","*OE - CUBIERTA HGM 1000-1250 4P, W450, 12M / 300, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 4P, W450, 12M / 300, FÜGGŐLEGES, KAR"]
["19545","OE - Osłona czołowa HGM 100 4P, W450, 3M / 300, poziomo, dźwignia",57.1,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19545","SZT","85389099",null,"230626RT","5901988195458","OE - Couvercle avant HGM 100 4P, L450, 3M / 300, horizontal, levier","OE - HGM 100 4P Front cover, W450, 3M / 300, Horizontal, Lever","OM- TAPA TROQ. HGM 100 4P, W450, 3M (150MM) HORIZ.","OE - Első burkolat HGM 100 4P, W450, 3M / 300, vízszintes, kar"]
["19546","OE - Osłona czołowa HGM 125 4P, W450, 3M / 300, poziomo, dźwignia",57.1,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19546","SZT","85389099",null,"230626RT","5901988195465","OE - Couvercle avant HGM 125 4P, L450, 3M / 300, horizontal, levier","OE - HGM 125 4P front visor, W450, 3M / 300, Horizontal, Lever","OM- TAPA TROQ. HGM 125 4P, W450, 3M (150MM) HORIZ.","OE - Első burkolat HGM 125 4P, W450, 3M / 300, vízszintes, kar"]
["19547","OE - Osłona czołowa HGM 160-250 4P, W450, 4M / 300, poziomo, dźwignia",59.4,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19547","SZT","85389099",null,"230626RT","5901988195472","OE - Couvercle avant HGM 160-250 4P, L450, 4M / 300, horizontal, levier","OE - Front Cover HGM 160-250 4P, W450, 4M / 300, Horizontal, Lever","OM- TAPA TROQ. HGM 160-250 4P, W450, 4M (200MM) HORIZ.","OE - Első burkolat HGM 160-250 4P, W450, 4M / 300, vízszintes, kar"]
["19550","OE - Osłona czołowa HGM 100 3/4P, W450, 5M / 300, pionowo, dźwignia",63.6,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19550","SZT","85389099","27.12.40.0","230626RT","5901988195502","OE - Couvercle avant HGM 100 3 / 4P, L450, 5M / 300, vertical, levier","OE - HGM 100 3 / 4P front visor, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 100 3/4P, W450, 5M (250MM) VERT.","OE - Első burkolat HGM 100 3/4P, W450, 5M / 300, függőleges, kar"]
["19551","OE - Osłona czołowa HGM 125 4P, W450, 5M / 300, pionowo, dźwignia",66.599999999999994,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19551","SZT","85389099","27.12.40.0","230626RT","5901988195519","OE - Couvercle avant HGM 125 4P, L450, 5M / 300, vertical, levier","OE - HGM 125 4P front visor, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 125 3/4P, W450, 5M (250MM) VERT.","OE - Első burkolat HGM 125 4P, W450, 5M / 300, függőleges, kar"]
["19552","OE - Osłona czołowa HGM 160-250 4P, W450, 5M / 300, pionowo, dźwignia",66.599999999999994,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19552","SZT","85389099","27.12.40.0","230626RT","5901988195526","OE - Couvercle avant HGM 160-250 4P, L450, 5M / 300, vertical, levier","OE - Front visor HGM 160-250 4P, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 160-250 3/4P, W450, 5M (250MM) VERT.","OE - Első burkolat HGM 160-250 4P, W450, 5M / 300, függőleges, kar"]
["19593","OE - Osłona czołowa HGM 400 3/4P, W450, 9M / 300, pionowo, dźwignia",108.1,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19593","SZT","85389099","27.12.40.0","230626RT","5901988195939","OE - Couvercle avant HGM 400 3 / 4P, L450, 9M / 300, vertical, levier","OE - HGM 400 3 / 4P front visor, W450, 9M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 400 3/4P, W450, 9M (450MM) VERT.","OE - Első burkolat HGM 400 3/4P, W450, 9M / 300, függőleges, kar"]
["19595","OE - Osłona czołowa HGM 630-800 4P, W450, 9M / 300, pionowo, dźwignia",108.1,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19595","SZT","85389099","27.12.40.0","230626RT","5901988195953","OE - Couvercle avant HGM 630-800 4P, L450, 9M / 300, vertical, levier","OE - HGM 630-800 4P front visor, W450, 9M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 630-800 3/4P, W450, 9M (450MM) VERT.","OE - Első burkolat HGM 630-800 4P, W450, 9M / 300, függőleges, kar"]
["19702","OE - OSŁONA CZOŁOWA HGM 125 3P + ANALIZATOR 92X92mm, W650, 3M / 500, POZIOMO",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","19702","SZT","85389099",null,"230626RT","5901988197025","OE - CAPOT AVANT HGM 125 3P + ANALYSEUR 92X92mm, L650, 3M / 500, HORIZONTAL","OE - Front Cover HGM 125 3P + analyzer 92X92mm, W650, 3M / 500, Horizontal","ZEN- TAPA TROQ. HGM 125 3P + ANALIZ. DE REDES 92X92mm, W650, 3M / 500, HORIZ.","OE - ELSŐ BURKOLAT HGM 125 3P + ELEMZŐ 92X92mm, W650, 3M / 500, VÍZSZINTES"]
["19703","OE - OSŁONA CZOŁOWA HGM 125 4P + ANALIZATOR 92X92mm, W650, 3M / 500, POZIOMO",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","19703","SZT","85389099",null,"230626RT","5901988197032","OE - CAPOT AVANT HGM 125 4P + ANALYSEUR 92X92mm, L650, 3M / 500, HORIZONTAL","OE - Front Cover HGM 125 4P + analyzer 92X92mm, W650, 3M / 500, Horizontal","*OE - TAPA FRONTAL HGM 125 4P + ANALIZADOR 92X92mm, W650, 3M / 500, HORIZONTAL","OE - ELSŐ BURKOLAT HGM 125 4P + ELEMZŐ 92X92mm, W650, 3M / 500, VÍZSZINTES"]
["19704","OE - OSŁONA CZOŁOWA HGM 160-250 3P + ANALIZATOR 92X92mm, W650, 3M / 500, POZIOMO",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","19704","SZT","85389099",null,"230626RT","5901988197049","OE - CAPOT AVANT HGM 160-250 3P + ANALYSEUR 92X92mm, L650, 3M / 500, HORIZONTAL","OE - Front Cover HGM 160-250 3P + analyzer 92X92mm, W650, 3M / 500, Horizontal","ZEN- TAPA TROQ. HGM 160-250 3P + ANALIZ. DE REDES 92X92mm, W650, 3M / 500, HORIZ.","OE - ELSŐ BURKOLAT HGM 160-250 3P + ELEMZŐ 92X92mm, W650, 3M / 500, VÍZSZINTES"]
["19705","OE - OSŁONA CZOŁOWA HGM 160-250 4P + ANALIZATOR 92X92mm, W650, 4M / 500, POZIOMO",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","19705","SZT","85389099",null,"230626RT","5901988197056","OE - CAPOT AVANT HGM 160-250 4P + ANALYSEUR 92X92mm, L650, 4M / 500, HORIZONTAL","OE - Front Cover HGM 160-250 4P + analyzer 92X92mm, W650, 4M / 500, Horizontal","*OE - TAPA FRONTAL HGM 160-250 4P + ANALIZADOR 92X92mm, W650, 4M/500, HORIZONTAL","OE - ELSŐ BURKOLAT HGM 160-250 4P + ELEMZŐ 92X92mm, W650, 4M / 500, VÍZSZINTES"]
["19706","OE - OSŁONA CZOŁOWA HGM 400 3P + ANALIZATOR 92X92mm, W650, 4M / 500, POZIOMO",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","19706","SZT","85389099",null,"230626RT","5901988197063","OE - CAPOT AVANT HGM 400 3P + ANALYSEUR 92X92mm, L650, 4M / 500, HORIZONTAL","OE - Front Cover HGM 400 3P + analyzer 92X92mm, W650, 4M / 500, Horizontal","*OE - TAPA FRONTAL HGM 400 3P + ANALIZADOR 92X92mm, W650, 4M / 500, HORIZONTAL","OE - ELSŐ BURKOLAT HGM 400 3P + ELEMZŐ 92X92mm, W650, 4M / 500, VÍZSZINTES"]
["19722","OE - OSŁONA CZOŁOWA HGM 1000-1250 3P, W650, 12M / 500, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","19722","SZT","85389099",null,"230626RT","5901988197223","OE - COUVERCLE HGM 1000-1250 3P, L650, 12M/500, VERTICAL, LEVIER","OE - Cover HGM 1000-1250 3P, W650, 12M / 500, Vertical, Lever","*OE - CUBIERTA HGM 1000-1250 3P, W650, 12M / 500, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 3P, W650, 12M / 500, FÜGGŐLEGES, KAR"]
["19723","OE - OSŁONA CZOŁOWA HGM 1000-1250 4P, W650, 12M / 500, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","19722","SZT","85389099",null,"230626RT","5901988197230","OE - CAPOT AVANT HGM 1000-1250 4P, L650, 12M / 500, VERTICAL, LEVIER","OE - Front Cover HGM 1000-1250 4P, W650, 12M / 500, Vertical, Lever","*OE - TAPA DELANTERA HGM 1000-1250 4P, W650, 12M / 500, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 4P, W650, 12M / 500, FÜGGŐLEGES, KAR"]
["19736","OE - Osłona czołowa HGM 125 3P, W650, 3M / 500, poziomo, dźwignia",63.6,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19736","SZT","85389099",null,"230626RT","5901988197360","OE - Couvercle avant HGM 125 3P, L650, 3M / 500, horizontal, levier","OE - HGM 125 3P front visor, W650, 3M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 125 3P, W650, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 125 3P, W650, 3M / 500, vízszintes, kar"]
["19737","OE - Osłona czołowa HGM 160-250 3P, W650, 3M / 500, poziomo, dźwignia",63.6,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19737","SZT","85389099",null,"230626RT","5901988197377","OE - Couvercle avant HGM 160-250 3P, L650, 3M / 500, horizontal, levier","OE - Front Cover HGM 160-250 3P, W650, 3M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 160-250 3P, W650, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 160-250 3P, W650, 3M / 500, vízszintes, kar"]
["19745","OE - Osłona czołowa HGM 100 3/4P, W650, 3M / 500, poziomo, dźwignia",63.6,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19745","SZT","85389099","27.12.40.0","230626RT","5901988197452","OE - Couvercle avant HGM 100 4P, L650, 3M / 500, horizontal, levier","OE - HGM 100 4P, W650, 3M / 500 Front cover, Horizontal, Lever","ZEN- TAPA TROQ. HGM 100 4P, W650, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 100 3/4P, W650, 3M / 500, vízszintes, kar"]
["19746","OE - Osłona czołowa HGM 125 4P, W650, 3M / 500, poziomo, dźwignia",66.599999999999994,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19746","SZT","85389099","27.12.40.0","230626RT","5901988197469","OE - Couvercle avant HGM 125 4P, L650, 3M / 500, horizontal, levier","OE - HGM 125 4P front visor, W650, 3M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 125 4P, W650, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 125 4P, W650, 3M / 500, vízszintes, kar"]
["19747","OE - Osłona czołowa HGM 160-250 4P, W650, 4M / 500, poziomo, dźwignia",71.2,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19747","SZT","85389099","27.12.40.0","230626RT","5901988197476","OE - Couvercle avant HGM 160-250 4P, L650, 4M / 500, horizontal, levier","OE - Front Cover HGM 160-250 4P, W650, 4M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 160-250 4P, W650, 4M (200MM)  HORIZ.","OE - Első burkolat HGM 160-250 4P, W650, 4M / 500, vízszintes, kar"]
["19748","OE - Osłona czołowa HGM 400 3P, W650, 4M / 500, poziomo, dźwignia",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","19748","SZT","85389099",null,"230626RT","5901988197483","OE - Couvercle avant HGM 400 3P, L650, 4M / 500, horizontal, levier","OE - HGM 400 3P front visor, W650, 4M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 400 3P, W650, 4M (200MM)  HORIZ.","OE - Első burkolat HGM 400 3P, W650, 4M / 500, vízszintes, kar"]
["19750","OE - Osłona czołowa HGM 100 3/4P, W650, 5M / 500, pionowo, dźwignia",77.7,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19750","SZT","85389099","27.12.40.0","230626RT","5901988197506","OE - Couvercle avant HGM 100 3 / 4P, L650, 5M / 500, vertical, levier","OE - HGM 100 3 / 4P front visor, W650, 5M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 100 3/4P, W650, 5M (250MM)  VERT.","OE - Első burkolat HGM 100 3/4P, W650, 5M / 500, függőleges, kar"]
["19751","OE - Osłona czołowa HGM 125 3/4P, W650, 5M / 500, pionowo, dźwignia",77.7,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19751","SZT","85389099","27.12.40.0","230626RT","5901988197513","OE - Couvercle avant HGM 125 3 / 4P, L650, 5M / 500, vertical, levier","OE - HGM 125 3 / 4P front visor, W650, 5M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 125 3/4P, W650, 5M (250MM)  VERT.","OE - Első burkolat HGM 125 3/4P, W650, 5M / 500, függőleges, kar"]
["19752","OE - Osłona czołowa HGM 160-250 3/4P, W650, 5M / 500, pionowo, dźwignia",77.7,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19752","SZT","85389099","27.12.40.0","230626RT","5901988197520","OE - Couvercle avant HGM 160-250 3 / 4P, L650, 5M / 500, vertical, levier","OE - Front Cover HGM 160-250 3 / 4P, W650, 5M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 160-250 3/4P, W650, 5M (250MM)  VERT.","OE - Első burkolat HGM 160-250 3/4P, W650, 5M / 500, függőleges, kar"]
["19758","OE - Osłona czołowa HGM 400 4P, W650, 5M / 500, poziomo, dźwignia",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","19758","SZT","85389099","27.12.40.0","230626RT","5901988197582","OE - Couvercle avant HGM 400 4P, L650, 5M / 500, horizontal, levier","OE - HGM 400 4P front visor, W650, 5M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 400 4P, W650, 5M (250MM)  HORIZ.","OE - Első burkolat HGM 400 4P, W650, 5M / 500, vízszintes, kar"]
["19769","OE - Osłona czołowa HGM 630-800 3P, W650, 6M / 500, poziomo, dźwignia",79,"1-ZE-01",null,null,"OE_MCCB_COVERS","19769","SZT","85389099","27.12.40.0","230626RT","5901988197698","OE - Couvercle avant HGM 630-800 3P, L650, 6M / 500, horizontal, levier","OE - Front Cover HGM 630-800 3P, W650, 6M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 630-800 3P, W650, 6M (300MM)  HORIZ.","OE - Első burkolat HGM 630-800 3P, W650, 6M / 500, vízszintes, kar"]
["19779","OE - Osłona czołowa HGM 630-800 4P, W650, 7M / 500, poziomo, dźwignia",103.8,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19779","SZT","85389099","27.12.40.0","230626RT","5901988197797","OE - Couvercle avant HGM 630-800 4P, L650, 7M / 500, horizontal, levier","OE - Front Cover HGM 630-800 4P, W650, 7M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 630-800 4P, W650, 7M (350MM)  HORIZ.","OE - Első burkolat HGM 630-800 4P, W650, 7M / 500, vízszintes, kar"]
["19793","OE - Osłona czołowa HGM 400 3/4P, W650, 9M / 500, pionowo, dźwignia",137.80000000000001,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19793","SZT","85389099","27.12.40.0","230626RT","5901988197933","OE - Couvercle avant HGM 400 3 / 4P, L650, 9M / 500, vertical, levier","OE - HGM 400 3 / 4P front visor, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 400 3/4P, W650, 9M (450MM)  VERT.","OE - Első burkolat HGM 400 3/4P, W650, 9M / 500, függőleges, kar"]
["19794","OE - Osłona czołowa HGM 630-800 3P, W650, 9M / 500, pionowo, dźwignia",128.69999999999999,"1-ZE-01",null,null,"OE_MCCB_COVERS","19794","SZT","85389099","27.12.40.0","230626RT","5901988197940","OE - Couvercle avant HGM 630-800 3P, L650, 9M / 500, vertical, levier","OE - HGM 630-800 3P front visor, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 630-800 3P, W650, 9M (450MM)  VERT.","OE - Első burkolat HGM 630-800 3P, W650, 9M / 500, függőleges, kar"]
["19795","OE - Osłona czołowa HGM 630-800 4P, W650, 9M / 500, pionowo, dźwignia",137.80000000000001,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19795","SZT","85389099","27.12.40.0","230626RT","5901988197957","OE - Couvercle avant HGM 630-800 4P, L650, 9M / 500, vertical, levier","OE - Front Cover HGM 630-800 4P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 630-800 4P, W650, 9M (450MM)  VERT.","OE - Első burkolat HGM 630-800 4P, W650, 9M / 500, függőleges, kar"]
["19920","OE - Osłona czołowa 2x HGM 1000-1250 3/4P, W850, 12M / 700, pionowo, dźwignia",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","19920","SZT","85389099",null,"230626RT","5901988199203","OE - Capot avant 2x HGM 1000-1250 3/4P, L850, 12M / 700, vertical, levier","OE - Front cover 2x HGM 1000-1250 3/4P, W850, 12M / 700, Vertical, Lever","*OE- Tapa troq. 2x HGM 1000-1250 3/4P, W850, 12M (600mm)  vert.","OE - Első burkolat 2x HGM 1000-1250 3/4P, W850, 12M / 700, függőleges, kar"]
["19922","OE - OSŁONA CZOŁOWA HGM 1000-1250 3P, W850, 12M / 700, PIONOWO, DŹWIGNIA",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","19922","SZT","85389099",null,"230626RT","5901988199227","OE - CAPOT AVANT HGM 1000-1250 3P, L850, 12M / 700, VERTICAL, LEVIER","OE - Front Cover HGM 1000-1250 3P, W850, 12M / 700, Vertical, Lever","*OE - TAPA DELANTERA HGM 1000-1250 3P, W850, 12M / 700, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 3P, W850, 12M / 700, FÜGGŐLEGES, KAR"]
["19923","OE - OSŁONA CZOŁOWA HGM 1000-1250 4P, W850, 12M / 700, PIONOWO, DŹWIGNIA",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","19922","SZT","85389099",null,"230626RT","5901988199234","OE - CAPOT AVANT HGM 1000-1250 4P, L850, 12M / 700, VERTICAL, LEVIER","OE - Front Cover HGM 1000-1250 4P, W850, 12M / 700, Vertical, Lever","*OE - TAPA DELANTERA HGM 1000-1250 4P, W850, 12M / 700, VERTICAL, PALANCA","OE - ELSŐ BURKOLAT HGM 1000-1250 4P, W850, 12M / 700, FÜGGŐLEGES, KAR"]
["19936","OE - Osłona czołowa HGM 125 3P, W850, 3M / 700, poziomo, dźwignia",70.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","19936","SZT","85389099",null,"230626RT","5901988199364","OE - Couvercle avant HGM 125 3P, L850, 3M / 700, horizontal, levier","OE - HGM 125 3P front visor, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 125 3P, W850, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 125 3P, W850, 3M / 700, vízszintes, kar"]
["19937","OE - Osłona czołowa HGM 160-250 3P, W850, 3M / 700, poziomo, dźwignia",70.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","19937","SZT","85389099",null,"230626RT","5901988199371","OE - Couvercle avant HGM 160-250 3P, L850, 3M / 700, horizontal, levier","OE - Front Cover HGM 160-250 3P, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 160-250 3P, W850, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 160-250 3P, W850, 3M / 700, vízszintes, kar"]
["19945","OE - Osłona czołowa HGM 100 4P, W850, 3M / 700, poziomo, dźwignia",71.900000000000006,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19945","SZT","85389099","27.12.40.0","230626RT","5901988199456","OE - Couvercle avant HGM 100 4P, L850, 3M / 700, horizontal, levier","OE - HGM 100 4P, W850, 3M / 700 Front cover, Horizontal, Lever","OE- TAPA TROQ. HGM 100 4P, W850, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 100 4P, W850, 3M / 700, vízszintes, kar"]
["19946","OE - Osłona czołowa HGM 125 4P, W850, 3M / 700, poziomo, dźwignia",71.900000000000006,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19946","SZT","85389099","27.12.40.0","230626RT","5901988199463","OE - Couvercle avant HGM 125 4P, L850, 3M / 700, horizontal, levier","OE - HGM 125 4P Front cover, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 125 4P, W850, 3M (150MM)  HORIZ.","OE - Első burkolat HGM 125 4P, W850, 3M / 700, vízszintes, kar"]
["19947","OE - Osłona czołowa HGM 160-250 4P, W850, 4M / 700, poziomo, dźwignia",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","19947","SZT","85381000","27.12.40.0","230626RT","5901988199470","OE - Couvercle avant HGM 160-250 4P, L850, 4M / 700, horizontal, levier","OE - Front Cover HGM 160-250 4P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 160-250 4P, W850, 4M (200MM)  HORIZ.","OE - Első burkolat HGM 160-250 4P, W850, 4M / 700, vízszintes, kar"]
["19948","OE - Osłona czołowa HGM 400 3P, W850, 4M / 700, poziomo, dźwignia",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","19948","SZT","85381000","27.12.40.0","230626RT","5901988199487","OE - Couvercle avant HGM 400 3P, L850, 4M / 700, horizontal, levier","OE - HGM 400 3P, W850, 4M / 700 Front cover, Horizontal, Lever","OE- TAPA TROQ. HGM 400 3P, W850, 4M (200MM)  HORIZ.","OE - Első burkolat HGM 400 3P, W850, 4M / 700, vízszintes, kar"]
["19950","OE - Osłona czołowa HGM 100 3/4P, W850, 5M / 700, pionowo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","19950","SZT","85381000","27.12.40.0","230626RT","5901988199500","OE - Couvercle avant HGM 100 3 / 4P, L850, 5M / 700, vertical, levier","OE - HGM 100 3 / 4P front visor, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 100 3/4P, W850, 5M (250MM)  VERT.","OE - Első burkolat HGM 100 3/4P, W850, 5M / 700, függőleges, kar"]
["19951","OE - Osłona czołowa HGM 125 3/4P, W850, 5M / 700, pionowo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","19951","SZT","85381000","27.12.40.0","230626RT","5901988199517","OE - Couvercle avant HGM 125 3 / 4P, L850, 5M / 700, vertical, levier","OE - HGM 125 3 / 4P front visor, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 125 3/4P, W850, 5M (250MM)  VERT.","OE - Első burkolat HGM 125 3/4P, W850, 5M / 700, függőleges, kar"]
["19952","OE - Osłona czołowa HGM 160-250 3/4P, W850, 5M / 700, pionowo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","19952","SZT","85381000","27.12.40.0","230626RT","5901988199524","OE - Couvercle avant HGM 160-250 3 / 4P, L850, 5M / 700, vertical, levier","OE - Front Cover HGM 160-250 3 / 4P, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 160-250 3/4P, W850, 5M (250MM)  VERT.","OE - Első burkolat HGM 160-250 3/4P, W850, 5M / 700, függőleges, kar"]
["19958","OE - Osłona czołowa HGM 400 4P, W850, 5M / 700, poziomo, dźwignia",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","19958","SZT","85381000","27.12.40.0","230626RT","5901988199586","OE - Capot avant HGM 400 4P, L850, 5M / 700, horizontal, effet de levier","OE - HGM 400 4P Front cover, W850, 5M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 400 4P, W850, 5M (250MM)  HORIZ.","OE - Első burkolat HGM 400 4P, W850, 5M / 700, vízszintes, kar"]
["19969","OE - Osłona czołowa HGM 630-800 3P, W850, 6M / 700, poziomo, dźwignia",95.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","19969","SZT","85389099",null,"230626RT","5901988199692","OE - Couvercle avant HGM 630-800 3P, L850, 6M / 700, horizontal, levier","OE - Front Cover HGM 630-800 3P, W850, 6M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 630-800 3P, W850, 6M (300MM)  HORIZ.","OE - Első burkolat HGM 630-800 3P, W850, 6M / 700, vízszintes, kar"]
["19979","OE - Osłona czołowa HGM 630-800 4P, W850, 7M / 700, poziomo, dźwignia",118.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","19979","SZT","85381000","27.12.40.0","230626RT","5901988199791","OE - Couvercle avant HGM 630-800 4P, L850, 7M / 700, horizontal, levier","OE - Front Cover HGM 630-800 4P, W850, 7M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 630-800 4P, W850, 7M (350MM)  HORIZ.","OE - Első burkolat HGM 630-800 4P, W850, 7M / 700, vízszintes, kar"]
["19993","OE - Osłona czołowa HGM 400 3/4P, W850, 9M / 700, pionowo, dźwignia",155.69999999999999,"1-ZE-01",null,null,"03_SWITCHES_COVERS","19993","SZT","85389099","27.12.40.0","230626RT","5901988199937","OE - Couvercle avant HGM 400 3 / 4P, L850, 9M / 700, vertical, levier","OE - HGM 400 3 / 4P front visor, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 400 3/4P, W850, 9M (450MM)  VERT.","OE - Első burkolat HGM 400 3/4P, W850, 9M / 700, függőleges, kar"]
["19994","OE - Osłona czołowa HGM 630-800 3P, W850, 9M / 700, pionowo, dźwignia",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","19994","SZT","85389099",null,"230626RT","5901988199944","OE - Couvercle avant HGM 630-800 3P, L850, 9M / 700, vertical, levier","OE - HGM 630-800 3P front hood, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 630-800 3P, W850, 9M (450MM)  VERT.","OE - Első burkolat HGM 630-800 3P, W850, 9M / 700, függőleges, kar"]
["19995","OE - Osłona czołowa HGM 630-800 4P, W850, 9M / 700, pionowo, dźwignia",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","19995","SZT","85381000","27.12.40.0","230626RT","5901988199951","OE - Couvercle avant HGM 630-800 4P, L850, 9M / 700, vertical, levier","OE - Front Cover HGM 630-800 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 630-800 4P, W850, 9M (450MM)  VERT.","OE - Első burkolat HGM 630-800 4P, W850, 9M / 700, függőleges, kar"]
["20011","ALCUBAR - PRZYŁĄCZE M10 x 3, M12 x 1, Cu 185x80x5mm",129.9,"1-ZE-08",0.15,2,"OE_BUSBARS_ALCUBAR","20011","SZT","73181595","25.94.11.0",null,"5901988200114","AlCu - Connexion M10 x 3, M12 x 1, Cu 185x80x5mm","AlCu - M10 x 3, M12 x 1, Cu 185x80x5mm","ALCUB- CONEXION M10 X 4, CU 185X80X5MM","AlCubar- CSATLAKOZTATÁS M10 x 3, M12 x 1, Cu 185x80x5mm"]
["20012","ALCUBAR - PRZYŁĄCZE M10 x 4, M12 x 2, Cu 275x80x5mm",194.9,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20012","SZT","73181595","25.94.11.0",null,"5901988200121","AlCu - Connexion M10 x 4, M12 x 2, Cu 275x80x5mm","AlCu - M10 x 4, M12 x 2, Cu 275x80x5mm","ALCUB- CONEXION M10 X 6, CU 275X80X5MM","AlCubar - CSATLAKOZÁS M10 x 4, M12 x 2, Cu 275x80x5mm"]
["20013","ALCUBAR - PRZYŁĄCZE M10 x 5, M12 x 3, Cu 375x80x5mm",256.5,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20013","SZT","73181595","25.94.11.0",null,"5901988200138","AlCu - Connexion M10 x 5, M12 x 3, Cu 365x80x5mm","AlCu - M10 x 5, M12 x 3, Cu 365x80x5mm","ALCUB- CONEXION M10 X 8, CU 365X80X5MM","AlCubar - CSATLAKOZTATÁS M10 x 5, M12 x 3, Cu 375x80x5mm"]
["20014","ALCUBAR - PRZYŁĄCZE M10 x 6, M12 x 4, Cu 455x80x5mm",306.89999999999998,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20014","SZT","73181595","25.94.11.0",null,"5901988200145","AlCu - Connexion M10 x 16, M12 x 4, Cu 455x80x5mm","AlCu - M10 x 6, M12 x 4, Cu 455x80x5mm","ALCUB- CONEXION M10 X 10, CU 455X80X5MM","AlCubar - CSATLAKOZTATÁS M10 x 6, M12 x 4, Cu 455x80x5mm"]
["20021","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C",246,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20022","M","76042990","24.42.22.0",null,"5901988200213","AlCu - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C","ALCUB-PERFIL AL-CU H27  1CU 6MM, 630A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFIL ALCUBAR H27, 360 MM2, 1 CU HORVÁNY, 6 MM, 630A DT 39C, 800A DT 57C"]
["20022","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C",246,"1-ZE-08",0.26666666666666666,8,"OE_BUSBARS_ALCUBAR","20022","M","76042990","24.42.22.0",null,"5901988200220","AlCu - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C","AlCu - Anodized profile AlCubar H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C","ALCUB-PERFIL AL-CU H27  1CU 8MM, 630A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C"]
["20023","ALCUBAR - PROFIL ALUMINIOWY ALCUBAR H27 PE, 1 ROWEK, 8 MM, 630A",181.6,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"M","76042990","24.42.22.0",null,"5901988200237","AlCu - Profilé en aluminium AlCubar H27 PE, 1 rainure, 8 mm, 630A","AlCu - AlCubar H27 PE aluminum profile, 1 groove, 8 mm, 630A","ALCUB-PERFIL AL-CU H27 H27 PE, 1  CU 8 MM, 630A UNIDAD L=1METRO","AlCubar - ALUMÍNIUM PROFIL ALCUBAR H27 PE, 1 VONÁS, 8 MM, 630A"]
["20026","ALCUBAR - ODPOWIEDNIK REF. ZENE20028",43.5,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988200268","AlCu - Connecteur Cu 630 A, type L1, 60x30x10mm","AlCu - equivalent to ref. ZENE20028","ALCUB-UNION CU PARA ALCUB 630A, TIPO L1, 60X30X10MM","AlCubar – MEGFELELŐ A REF. ZENE20028"]
["20028","ALCUBAR - ŁĄCZNIK CU 630 A, TYPU I / L1, 55X30X10MM",32.299999999999997,"1-ZE-08",1.8916666666666666,7,"OE_BUSBARS_ALCUBAR","20028","SZT","74072900","24.44.22.0",null,"5901988200282","AlCu - Connecteur Cu 630 A, type I, 55x30x10mm","AlCu - Cu 630 A connector, I / L1 type, 55x30x10mm","ALCUB-UNION CU PARA ALCUB 630A, TIPO I, 55X30X10MM","AlCubar - CSATLAKOZÓ CU 630 A, I. TÍPUS / L1, 55X30X10MM"]
["20030","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C",388,"1-ZE-08",5.3833333333333337,8,"OE_BUSBARS_ALCUBAR","20030","M","7604299000","24.42.22.0",null,"5901988200305","AlCu - Profilé anodisé AlCubar H50R, 2 rainures en Cu, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C","ALCUB-PERFIL AL-CU H50  2CU 1000A L CU, 8 MM I 12 MM, 1000A UNIDAD L=1METRO","AlCubar – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C"]
["20031","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 1 ROWEK CU, 1000A DT 40C, 1250A DT 58C",366,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20032","M","7604299000","24.42.22.0",null,"5901988200312","AlCu - Profilé anodisé AlCubar H50, 670 mm2, 1 gorge Cu, 1000A dt 40C, 1250A dt 58C","AlCu - AlCubar Anodized profile H50, 670 mm2, 1 Cu groove, 1000A dt 40C, 1250A dt 58C","ALCUB-PERFIL AL-CU H50  1CU 1000A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFILOS ALCUBAR H50, 670 MM2, 1 CU GROOVE, 1000A DT 40C, 1250A DT 58C"]
["20032","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 2 ROWKI CU, 1000A DT 40C, 1250A DT 58C",418,"1-ZE-08",7.4999999999999997E-2,1,"OE_BUSBARS_ALCUBAR","20032","M","76042990","24.42.22.0",null,"5901988200329","AlCu - Profilé anodisé AlCubar H50, 670 mm2, 2 rainures en Cu, 1000A dt 40C, 1250A dt 58C","AlCu - Anodized profile AlCubar H50, 670 mm2, 2 Cu grooves, 1000A dt 40C, 1250A dt 58C","ALCUB-PERFIL AL-CU H50  2CU 1000A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFILOS ALCUBAR H50, 670 MM2, 2 CU HORVÁZAT, 1000A DT 40C, 1250A DT 58C"]
["20035","ALCUBAR - ŁĄCZNIK CU 1000 A, TYPU I ,ROZŁĄCZNIK LISTWOWY DLA ALCUBAR H50R, 245X50X10mm",199.4,"1-ZE-08",0.05,1,"OE_BUSBARS_ALCUBAR","20035","SZT","74072900",null,null,"5901988200350","AlCu - Connecteur Cu 1000 A, type I, sectionneur à bande pour AlCubar H50R, 245x50x10mm","AlCu - Coupler Cu 1000 A, type I, switch disconnector for AlCubar H50R, 245x50x10mm","*AlCu - Conector Cu 1000 A, tipo I, seccionador de riel para AlCubar H50R, 245x50x10mm","ALCUBAR - CU 1000 A CSATLAKOZÓ, I. TÍPUS, SZALAGOS KAPCSOLÓ ALCUBAR H50R-HOZ, 245X50X10mm"]
["20036","ALCUBAR - ŁĄCZNIK CU 1000 A, TYPU L1, 100X50X10MM",88.9,"1-ZE-08",1.2083333333333333,10,"OE_BUSBARS_ALCUBAR","20036","SZT","74072900","24.44.22.0",null,"5901988200367","AlCu - Connecteur Cu 1000 A, type L1, 100x50x10mm","AlCu - Cu 1000 A connector, type L1, 100x50x10mm","ALCUB-UNION CU PARA ALCUB 1000A, TIPO L1, 100X50X10MM","AlCubar - CU CSATLAKOZÓ 1000 A, L1 TÍPUS, 100X50X10MM"]
["20038","ALCUBAR - ŁĄCZNIK CU 1000 A, TYPU I, 155X50X10MM",118.7,"1-ZE-08",1.8833333333333333,10,"OE_BUSBARS_ALCUBAR","20038","SZT","74072900","24.44.22.0",null,"5901988200381","AlCu - Connecteur Cu 1000 A, type I, 105x50x10mm","AlCu - Cu 1000 A connector, type I, 105x50x10mm","ALCUB-UNION CU PARA ALCUB 1000A, TIPO I, 105X50X10MM","AlCubar - CU CSATLAKOZÓ 1000 A, I. TÍPUS, 155X50X10MM"]
["20039","ALCUBAR - ŁĄCZNIK CU 1000 A, TYPU T, 160X50X10MM",113.1,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20039","SZT","74072900","24.44.22.0",null,"5901988200398","AlCu - Connecteur Cu 1000 A, type T, 160x50x10mm","AlCu - Cu 1000 A connector, T type, 160x50x10mm","ALCUB-UNION CU PARA ALCUB 1000A, TIPO T, 160X50X10MM","AlCubar - CU CSATLAKOZÓ 1000 A, T-TÍPUS, 160X50X10MM"]
["20041","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 1 ROWEK CU, 1600A DT 47C, 2000A DT 69C",476,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"M","76042990","24.42.22.0",null,"5901988200411","AlCu - Profilé anodisé AlCubar H80, 1280 mm2, 1 rainure Cu, 1600A dt 47C, 2000A dt 69C","AlCu - Anodized profile AlCubar H80, 1280 mm2, 1 Cu groove, 1600A dt 47C, 2000A dt 69C","ALCUB-PERFIL AL-CU H50  1CU 1600A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFILOS ALCUBAR H80, 1280 MM2, 1 CU HORVÁNY, 1600A DT 47C, 2000A DT 69C"]
["20042","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C",522,"1-ZE-08",0.01,1,"OE_BUSBARS_ALCUBAR","20042","M","76042990","24.42.22.0",null,"5901988200428","AlCu - Profilé anodisé AlCubar H80, 1280 mm2, 2 rainures en Cu, 1600A dt 47C, 2000A dt 69C","AlCu - Profile, anodized AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C","ALCUB-PERFIL AL-CU H80  2CU 1600A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU BAROVE, 1600A DT 47C, 2000A DT 69C"]
["20043","ALCUBAR - ŁĄCZNIK CU 3200 A (2X1600A), TYPU L1, 2X(210X80X10MM)",508.5,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20043","SZT","74072900","24.44.22.0",null,"5901988200435","AlCu - Connecteur Cu 3200 A (2x1600A), type L1, 2x (210x80x10mm)","AlCu - Connector Cu 3200 A (2x1600A), type L1, 2x (210x80x10mm)","ALCUB- UNION CU PARA ALCUB 3200 A (2X1600A), TIPO L1","AlCubar – CU CSATLAKOZÓ 3200 A (2X1600A), L1 TÍPUS, 2X (210X80X10MM)"]
["20044","ALCUBAR - ŁĄCZNIK CU 3200 A (2X1600A), TYPU L2, 2X(235X80X10MM)",560,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20044","SZT","74072900","24.44.22.0",null,"5901988200442","AlCu - Connecteur Cu 3200 A (2x1600A), type L2, 2x (235x80x10mm)","AlCu - Connector Cu 3200 A (2x1600A), L2 type, 2x (235x80x10mm)","ALCUB- UNION CU PARA ALCUB 3200 A (2X1600A), TIPO L2","AlCubar – CU CSATLAKOZÓ 3200 A (2X1600A), L2 TÍPUS, 2X (235X80X10MM)"]
["20045","ALCUBAR - ŁĄCZNIK CU 3200 A (2X1600A), TYPU T, 2X(330X80X10MM)",791.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20045","SZT","74072900","24.44.22.0",null,"5901988200459","AlCu - Connecteur Cu 3200 A (2x1600A), type T, 2x (330x80x10mm)","AlCu - Connector Cu 3200 A (2x1600A), type T, 2x (330x80x10mm)","ALCUB- UNION CU PARA ALCUB 3200 A (2X1600A), TIPO T","AlCubar – CU CONNECTOR 3200 A (2X1600A), T-TYPE, 2X (330X80X10MM)"]
["20046","ALCUBAR - ŁĄCZNIK CU 1600 A, TYPU L1, 130X80X10MM",145.6,"1-ZE-08",4.1666666666666664E-2,1,"OE_BUSBARS_ALCUBAR","20046","SZT","74072900","24.44.22.0",null,"5901988200466","AlCu - Connecteur Cu 1600 A, type L1, 130x80x10mm","AlCu - Cu 1600 A connector, type L1, 130x80x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO L1, 130X80X10MM","AlCubar – CSATLAKOZÓ CU 1600 A, L1 TÍPUS, 130X80X10MM"]
["20047","ALCUBAR - ŁĄCZNIK CU 1600 A, TYPU L2, 155X80X10MM",174.7,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20047","SZT","74072900","24.44.22.0",null,"5901988200473","AlCu - Connecteur Cu 1600 A, type L2, 155x80x10mm","AlCu - Cu 1600 A connector, L2 type, 155x80x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO L2, 155X80X10MM","AlCubar - CU CSATLAKOZÓ 1600 A, L2 TÍPUS, 155X80X10MM"]
["20048","ALCUBAR - ŁĄCZNIK CU 1600 A, TYPU I, 165X80X10MM",188.2,"1-ZE-08",0.01,1,"OE_BUSBARS_ALCUBAR","20048","SZT","74072900","24.44.22.0",null,"5901988200480","AlCu - Connecteur Cu 1600 A, type I, 165x80x10mm","AlCu - Cu 1600 A connector, type I, 165x80x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO I, 165X80X10MM","AlCubar - CSATLAKOZÓ CU 1600 A, I. TÍPUS, 165X80X10MM"]
["20049","ALCUBAR - ŁĄCZNIK CU 1600 A, TYPU T, 250X80X10MM",285.60000000000002,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20049","SZT","74072900","24.44.22.0",null,"5901988200497","AlCu - Connecteur Cu 1600 A, type T, 250x80x10mm","AlCu - Cu 1600 A connector, T type, 250x80x10mm","ALCUB-UNION CU PARA ALCUB 1600A, TIPO T, 250X80X10MM","AlCubar - CU CSATLAKOZÓ 1600 A, T-TYPE, 250X80X10MM"]
["20050","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C",956,"1-ZE-08",0.05,1,"OE_BUSBARS_ALCUBAR","20050","M","7604299000","24.42.22.0",null,"5901988200503","AlCu - Profilé anodisé AlCubar H100R, 2 rainures en Cu, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C","ALCUB-PERFIL AL-CU H100  2CU, 8 MM Y 12 MM, 2500A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C"]
["20051","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 1 ROWEK CU, 2500A DT 55C",934,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20052","M","76042990","24.42.22.0",null,"5901988200510","AlCu - Profilé anodisé AlCubar H100, 2500 mm2, 1 rainure Cu, 2500A dt 55C","AlCu - Anodized profile AlCubar H100, 2500 mm2, 1 Cu groove, 2500A dt 55C","ALCUB-PERFIL AL-CU H100  1CU 2500A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFILOS ALCUBAR H100, 2500 MM2, 1 CU BARNA, 2500A DT 55C"]
["20052","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C",1004,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20052","M","76042990","24.42.22.0",null,"5901988200527","AlCu - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 55C","AlCu - Anodized profile AlCubar H100, 2500 mm2, 2 Cu grooves, 2500A dt 55C","ALCUB-PERFIL AL-CU H100  2CU 2500A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFILOS ALCUBAR H100, 2500 MM2, 2 CU BAROVE, 2500A DT 55C"]
["20053","ALCUBAR - ŁĄCZNIK CU 4000 A (2X2500A), TYPU L1, 2X(260X100X10MM)",719,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20053","SZT","74072900","24.44.22.0",null,"5901988200534","AlCu - Connecteur Cu 4000 A (2x2500A), type L1, 2x (260x100x10mm)","AlCu - Connector Cu 4000 A (2x2500A), type L1, 2x (260x100x10mm)","ALCUB- UNION CU PARA ALCUB 4000 A (2X2500A), TIPO L1","AlCubar – CU CSATLAKOZÓ 4000 A (2X2500A), L1 TÍPUS, 2X (260X100X10MM)"]
["20054","ALCUBAR - ŁĄCZNIK CU 4000 A (2X2500A), TYPU L2, 2X(290X100X10MM)",734.7,"1-ZE-08",0.05,2,"OE_BUSBARS_ALCUBAR","20054","KPL","74072900","24.44.22.0",null,"5901988200541","AlCu - Connecteur Cu 4000 A (2x2500A), type L2, 2x (290x100x10mm)","AlCu - Connector Cu 4000 A (2x2500A), L2 type, 2x (290x100x10mm)","ALCUB- UNION CU PARA ALCUB 4000 A (2X2500A), TIPO L2","AlCubar – CU CSATLAKOZÓ 4000 A (2X2500A), L2 TÍPUS, 2X (290X100X10MM)"]
["20055","ALCUBAR - ŁĄCZNIK CU 4000 A (2X2500A), TYPU T, 2X(410X100X10MM)",1234.2,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20055","SZT","74072900","24.44.22.0",null,"5901988200558","AlCu - connecteur Cu 4000 A (2x2500A), type T, 2x (410x100x10mm)","AlCu - Connector Cu 4000 A (2x2500A), type T, 2x (410x100x10mm)","ALCUB- UNION CU PARA ALCUB 4000 A (2X2500A), TIPO T","AlCubar – CU CSATLAKOZÓ 4000 A (2X2500A), T-TYPE, 2X (410X100X10MM)"]
["20056","ALCUBAR - ŁĄCZNIK CU 2500 A, TYPU L1, 160X100X10MM",234.1,"1-ZE-08",0.28333333333333333,5,"OE_BUSBARS_ALCUBAR","20056","SZT","74072900","24.44.22.0",null,"5901988200565","AlCu - Connecteur Cu 2500 A, type L1, 160x100x10mm","AlCu - Cu 2500 A connector, type L1, 160x100x10mm","ALCUB- UNION CU PARA ALCUB 2500A, TIPO L1, 160X100X10MM","AlCubar - CU CSATLAKOZÓ 2500 A, L1 TÍPUS, 160X100X10MM"]
["20057","ALCUBAR - ŁĄCZNIK CU 2500 A, TYPU L2, 190X100X10MM",255.4,"1-ZE-08",0.40833333333333333,8,"OE_BUSBARS_ALCUBAR","20057","SZT","7407290000","24.44.22.0",null,"5901988200572","AlCu - Connecteur Cu 2500 A, type L2, 190x100x10mm","AlCu - Cu 2500 A connector, L2 type, 190x100x10mm","ALCUB- UNION CU PARA ALCUB 2500A, TIPO L2, 190X100X10MM","AlCubar - CU CSATLAKOZÓ 2500 A, L2 TÍPUS, 190X100X10MM"]
["20058","ALCUBAR - ŁĄCZNIK CU 2500 A, TYPU I,   250X100X10MM",376.3,"1-ZE-08",1.4,7,"OE_BUSBARS_ALCUBAR","20058","SZT","74072900","24.44.22.0",null,"5901988200589","AlCu - Connecteur Cu 2500 A, type I, 200x100x10mm","AlCu - Cu 2500 A connector, type I, 200x100x10mm","ALCUB-UNION CU PARA ALCUB 2500A, TIPO I, 200X100X10MM","AlCubar - CU CSATLAKOZÓ 2500 A, I. TÍPUS, 250X100X10MM"]
["20059","ALCUBAR - ŁĄCZNIK CU 2500 A, TYPU T,   310X100X10MM",452.5,"1-ZE-08",0.05,1,"OE_BUSBARS_ALCUBAR","20059","SZT","74072900","24.44.22.0",null,"5901988200596","AlCu - Connecteur Cu 2500 A, type T, 310x100x10mm","AlCu - Cu 2500 A connector, T type, 310x100x10mm","ALCUB-UNION CU PARA ALCUB 2500A, TIPO T, 310X100X10MM","AlCubar - CU CSATLAKOZÓ 2500 A, T-TYPE, 310X100X10MM"]
["20060","ALCUBAR - PODPORA SZYNY PIONOWEJ ALCUBAR H27, KPL.100SZT",545.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","85472000","27.33.14.0",null,"5901988200602","AlCu - Support de rail vertical AlCubar H27 set100 articles","AlCu - Support of the Vertical rail AlCubar H27 set 100 pcs","ALCUB-/CU- TOPE ANTIDESLIZ. PARA BARRA ALCUB- 630A 1UND ","ALCUBAR – FÜGGŐLEGES SÍN TÁMOGATÁS ALCUBAR H27, 100 DB KÉSZLET"]
["20061","ALCUBAR - PRZYŁĄCZE M10 x 3, M12 x 1, Cu 185x100x5mm",187,"1-ZE-08",0.1,1,"OE_BUSBARS_ALCUBAR","20061","SZT","74072900","24.44.22.0",null,"5901988200619","AlCu - Connexion M10 x 3, M12 x 1, Cu 185x100x5mm","AlCu - M10 x 3, M12 x 1, Cu 185x100x5mm","ALCUB- CONEXION M10 X 4, CU 185X100X5MM","AlCubar - CSATLAKOZTATÁS M10 x 3, M12 x 1, Cu 185x100x5mm"]
["20062","ALCUBAR - PRZYŁĄCZE M10 x 4, M12 x 2, Cu 275x100x5mm",226.2,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20062","SZT","74072900","24.44.22.0",null,"5901988200626","AlCu - Connexion M10 x 4, M12 x 2, Cu 275x100x5mm","AlCu - M10 x 4, M12 x 2, Cu 275x100x5mm","ALCUB- CONEXION M10 X 6, CU 275X100X5MM","AlCubar - CSATLAKOZÁS M10 x 4, M12 x 2, Cu 275x100x5mm"]
["20063","ALCUBAR - PRZYŁĄCZE M10 x 5, M12 x 3, Cu 365x100x5mm",264.3,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20063","SZT","74072900","24.44.22.0",null,"5901988200633","AlCu - Connexion M10 x 5, M12 x 3, Cu 365x100x5mm","AlCu - M10 x 5, M12 x 3, Cu 365x100x5mm","ALCUB- CONEXION M10 X 8, CU 365X100X5MM","AlCubar - CSATLAKOZÁS M10 x 5, M12 x 3, Cu 365x100x5mm"]
["20064","ALCUBAR - PRZYŁĄCZE M10 x 6, M12 x 4, Cu 455x100x5MM",340.5,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20064","SZT","74072900","24.44.22.0",null,"5901988200640","AlCu - Connexion M10 x 6, M12 x 4, Cu 455x100x5mm","AlCu - M10 x 6, M12 x 4, Cu 455x100x5mm","ALCUB- CONEXION M10 X 10, CU 455X100X5MM","AlCubar - CSATLAKOZTATÁS M10 x 6, M12 x 4, Cu 455x100x5MM"]
["20065","ALCUBAR 100R - ŁĄCZNIK CU 2500 A, TYPU I, M12mm, 250X100X10MM",376.3,"1-ZE-08",0.35,7,"OE_BUSBARS_ALCUBAR","20065","SZT","74072900","24.44.22.0",null,"5901988200657","AlCubar 100R - Connecteur Cu 2500 A, type I, 6x M12mm, 200x100x10mm","AlCubar 100R - Cu 2500 A connector, type I, 6x M12mm, 200x100x10mm","ALCUB- 100R- CONECTOR CU 2500 A, TIPO I, 6X M12MM, 200X100X10MM","ALCUBAR 100R - CU CSATLAKOZÓ 2500 A, I. TÍPUS, M12mm, 250X100X10MM"]
["20068","AlCubar - Śruba zamkowa M8x25 dla AlCubarH27 (630A), kl 8.8  + podkładki, nakrętki,  kpl.100szt, wsuwane od końca profila",165.8,"1-ZE-08",0.54166666666666663,10,"OE_BUSBARS_ALCUBAR","20068","SZT","73181595","24.44.22.0",null,"5901988200688","AlCu - Vis coulissantes 1x M8x27 pour AlCubar H27 (630A) + rondelles, écrous, jeu de 25 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 1x M8x27 for AlcubarH27 (630A) + washers, nuts, set of 25, inserted from the end of the profile","ALCUB- CONEXION M12 X 8, CU 365X100X5MM","AlCubar - M8x25 kocsicsavar AlCubarH27-hez (630A), 8.8 osztály + alátétek, anyák, 100 db-os készlet, a profil végétől behelyezve"]
["20070","ALCUBAR - PODPORA SZYNY PIONOWEJ ALCUBAR H50, H80, H100, KPL.100SZT",545.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20070","SZT","73182200","25.94.12.0","230908LK","5901988200701","AlCu - Support de rail vertical AlCubar H50, H80, H100, set100 articles","AlCu - Support of the Vertical rail AlCubar H50, H80, H100, set of 100 pcs","ALCUB-/CU TOPE ANTIDESLIZ. PARA BARRA ALCUB- ?1000A 1UND","AlCubar - FÜGGŐLEGES SÍN TÁMOGATÁS ALCUBAR H50, H80, H100, SZETT 100 DB"]
["20071","ALCUBAR - PODKŁADKA SPRĘŻYSTA, SŁONECZKOWA 6/14, KPL.1000SZT, PRZEBIJAJĄCA",342.4,"1-ZE-08",null,null,"OE_SUPPORT","20071","KPL","7318159500","25.94.12.0","230912LK","5901988200718","AlCu - Rondelle élastique solaire 6/14, ensemble de 1000 pièces, piercing","AlCu - Spring washer, sun 6/14, set 1000 pcs, piercing","ALCUB- ARANDELA ELASTICA, 6/14, 1000UDS ","AlCubar - RUGÓS ALATÓ, SOLAR 6/14, 1000 db-os SZETT, TELJESÍTŐ"]
["20072","ALCUBAR - PODKŁADKA SPRĘŻYSTA, SŁONECZKOWA 6/14, KPL.100SZT.",35.6,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73182200","25.94.12.0",null,"5901988200725","AlCu - Rondelle élastique solaire 6/14, set100 articles","AlCu - Solar spring washer 6/14, set of 100 pcs.","ALCUB- ARANDELA ELASTICA, 6/14, 100UDS","AlCubar - TAVASZI MOSÓ, SUNNY 6/14, 100 DB-OS SZETT."]
["20073","ALCUBAR - PODKŁADKA SPRĘŻYSTA, SŁONECZKOWA 8/18, KPL.100SZT.",61.5,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73182200","25.94.12.0",null,"5901988200732","AlCu - rondelle élastique, solaire 8/18, set100 articles","AlCu - Solar spring washer 8/18, set of 100 pcs.","ALCUB- ARANDELA ELASTICA, 8/18, 100UDS","AlCubar - TAVASZI MOSÓ, SUNNY 8/18, 100 DB-OS SZETT."]
["20074","ALCUBAR - PODKŁADKA SPRĘŻYSTA, SŁONECZKOWA 10/22, KPL.100SZT.",66.3,"1-ZE-08",0.01,1,"OE_BUSBARS_ALCUBAR",null,"KPL","73182200","25.94.12.0",null,"5901988200749","AlCu - rondelle élastique, dim 10/22, set 100 pièces","AlCu - Solar spring washer 10/22, set of 100 pcs.","ALCUB- ARANDELA ELASTICA, 10/22, 100UDS","AlCubar - RUGÓS MOSÓ, SUNNY 10/22, 100 DB-OS SZETT."]
["20075","ALCUBAR - PODKŁADKA SPRĘŻYSTA, SŁONECZKOWA 12/27, KPL.100SZT.",80.5,"1-ZE-08",0.01,1,"OE_BUSBARS_ALCUBAR","20075","KPL","73182200","25.94.12.0","230926LK","5901988200756","AlCu - rondelle élastique 12/27, set100, solaire","AlCu - Solar spring washer 12/27, set of 100 pcs.","ALCUB- ARANDELA ELASTICA, 12/27, 100UDS","AlCubar - TAVASZI MOSÓ, SUNNY 12/27, 100 DB-OS SZETT."]
["20076","ALCUBAR - PODKŁADKA SPRĘŻYSTA, SŁONECZKOWA 16/32, KPL.100SZT.",144.5,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73182200","25.94.12.0",null,"5901988200763","AlCu - rondelle élastique 16/32 solaire, set100 articles","AlCu - Solar spring washer 16/32, set of 100 pcs.","ALCUB- ARANDELA ELASTICA, 16/32, 100UDS","AlCubar - TAVASZI MOSÓ, SUNNY 16/32, 100 DB-OS SZETT."]
["20077","ALCUBAR - PODKŁADKA STALOWA-OCYNK, POWIĘKSZONA, 8/24, KPL.100SZT",75.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73182200","25.94.12.0",null,"5901988200770","AlCu - Acier zingué, agrandi, 8/24, set de 100 pièces","AlCu - Steel-Galvanized washer, enlarged, 8/24, set of 100 pieces","ALCUB- ARANDELA ACERO-GALVANIZADO, 8/24, 100UDS","AlCubar - ACÉL-HANGANYOZOTT ALATÓ, NAGYÍTÁS, 8/24, 100 DB-OS SZETT"]
["20078","ALCUBAR - PODKŁADKA STALOWA-OCYNK, POWIĘKSZONA, 8/28, KPL.100SZT",82.9,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73182200","25.94.12.0",null,"5901988200787","AlCu - acier galvanisé, élargi, 8/28, set100 articles","AlCu - Steel-Galvanized washer, enlarged, 8/28, set of 100 pcs","ALCUB- ARANDELA ACERO-GALVANIZADO, 8/28, 100UDS","AlCubar - ACÉL-HANGANYOZOTT ALATÓ, NAGYÍTÁS, 8/28, 100 DB-OS SZETT"]
["20079","ALCUBAR - PODKŁADKA CU M8/20 POD KOŃCÓWKI KABLOWE <25MM2, KPL.100SZT",187,"1-ZE-08",0.40833333333333333,2,"OE_BUSBARS_ALCUBAR","20079","KPL","74072900","25.94.12.0","230320LK","5901988200794","AlCu - Rondelle Cu M8 / 20 sous cosses de câble <25mm2, set 100p","AlCu - Cu M8 / 20 washer for cable terminals <25mm2, 100 pcs set","ALCUB- ARANDELA CU M8/20 PARA TERMINALES <25MM2, 100UDS","AlCubar - CU M8/20 ALÁTÉK 25MM2-nél kisebb KÁBELTERMÉKEKHEZ, 100 DB KÉSZLET"]
["20080","ALCUBAR - ZACISK U16/6, 16MM2, DO ROWKA 6MM ALCUBAR 630A, KPL.100SZT, MONTAŻ W DOWOLNYM MIEJSCU",308,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988200800","AlCu - Collier U16 / 6, 16mm2, pour rainure de 6mm AlCubar 630A, set 100p, montage possible","AlCu - Clamp U16 / 6, 16mm2, for a 6mm groove AlCubar 630A, 100 pcs set, installation in any place","ALCUB- CONECTOR TIPO U PARA ALCUB- 630A, RANURA 6MM 100UDS ","AlCubar - U16/6, 16MM2, 6MM-ES VONÁZÁSÚ ALCUBAR 630A-HOZ, 100 DB-OS KÉSZLET, TELEPÍTÉS BÁRHOL"]
["20081","ALCUBAR - ZACISK U16/8, 16MM2, DO ROWKA 8MM ALCUBAR 630A, KPL.100SZT, MONTAŻ W DOWOLNYM MIEJSCU",308,"1-ZE-08",0.5,1,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988200817","AlCu - Pince U16 / 8, 16mm2, pour gorge AlCubar 630A de 8mm, set 100p, montage possible","AlCu - Clamp U16 / 8, 16mm2, for 8mm groove AlCubar 630A, 100 pcs set, installation in any place","ALCUB- CONECTOR TIPO U PARA ALCUB- 630A, RANURA 8MM 100UND ","AlCubar - CAMP U16/8, 16MM2, 8MM VONÁZÁSHOZ ALCUBAR 630A, 100 DB-OS KÉSZLET, TELEPÍTÉS BÁRHOL"]
["20082","ALCUBAR - ŚRUBY PRZESUWNE 2X M8X27 + PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",98.2,"1-ZE-08",2.1083333333333334,8,"OE_BUSBARS_ALCUBAR","20082","KPL","73181595","25.94.11.0",null,"5901988200824","AlCu - Vis coulissantes 2x M8x27 + rondelles, écrous, jeu de 10 pièces, glissées à partir de l'extrémité du profilé","AlCu - Sliding screws 2x M8x27 + washers, nuts, 10 pcs set, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. PARA UNION BARRAS 2X M8X27 10UDS","AlCubar - CSÚSZTÓ CSAVAROK 2X M8X27 + ALLATÉTTEK, ANYÁK, SZETT 10 DB, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20083","ALCUBAR - ŚRUBY PRZESUWNE 3X M8X27 + PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",121,"1-ZE-08",0.64166666666666672,4,"OE_BUSBARS_ALCUBAR","20083","KPL","73181595","25.94.11.0",null,"5901988200831","AlCu - Vis coulissantes 3x M8x27 + rondelles, écrous, jeu de 10 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 3x M8x27 + washers, nuts, set of 10, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. PARA UNION BARRAS 3X M8X27 10UDS","AlCubar - 3X M8X27 CSÚSZTÓ CSAVAR + ALLATÁTÉTEK, ANYÁK, 10 db-os SZETT, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20084","ALCUBAR - ŚRUBY PRZESUWNE 4X M8X27 + PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",144.5,"1-ZE-08",2.0499999999999998,10,"OE_BUSBARS_ALCUBAR","20084","KPL","73181595","25.94.11.0",null,"5901988200848","AlCu - Vis coulissantes 4x M8x27 + rondelles, écrous, jeu de 10 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 4x M8x27 + washers, nuts, 10 pcs set, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. PARA UNION BARRAS 4X M8X27 10UDS","AlCubar - 4X M8X27 CSÚSZTÓ CSAVAR + ALLATÁTÉTEK, ANYÁK, 10 db-os SZETT, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20085","ALCUBAR - ZACISK U16/8, 16MM2, DO ROWKA 8MM ALCUBAR 1000A+, KPL.100SZT, MONTAŻ W DOWOLNYM MIEJSCU",308,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20085","KPL","73181595","25.94.11.0","230321PK","5901988200855","AlCu - Pince U16 / 8, 16mm2, pour rainure de 8mm AlCubar 1000A +, jeu 100p, montage possible","AlCu - Clamp U16 / 8, 16mm2, for 8mm groove AlCubar 1000A +, 100 pcs set, installation in any place","ALCUB- CONECTOR TIPO U PARA ALCUB- 1000,1600,2500A 100UDS","AlCubar - CLAMP U16/8, 16MM2, 8MM GROOVE ALCUBAR 1000A+, 100 DB-OS KÉSZLET, TELEPÍTÉS BÁRHOL"]
["20086","ALCUBAR - ŚRUBA ZAMKOWA M6X16, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",109.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988200862","AlCu - Vis de blocage M6x16, classe 8.8, + rondelles, écrous, jeu de 100 pièces, insérées à partir de l'extrémité du profilé","AlCu - Square bolt M6x16, class 8.8, + washers, nuts, set of 100 pieces, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M6X16, 100UDS","AlCubar - SZÁLLÍTÓ CSAVAR M6X16, 8.8 OSZTÁLY, + ALTÁTÉKOK, ANYÁK, 100 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20088","ALCUBAR - ŚRUBA ZAMKOWA M8X30 DLA ALCUBAR 1000A+, KL 8.8  + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",188.2,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","73181595",null,null,"5901988200886","AlCu - VIS DE BLOCAGE M8X30 POUR ALCUBAR 1000A+, KL 8.8 + RONDELLES, ÉCROUS, JEU DE 100 PCS, GLISSER DE L'EXTRÉMITÉ DU PROFIL","AlCu - Lock bolt M8X30 for AlCubar 1000A+, KL 8.8 + washers, nuts, set 100 PCS, slide from the end of the profile","*AlCu - TORNILLO DE BLOQUEO M8X30 PARA ALCUBAR 1000A+, KL 8.8 + ARANDELAS, TUERCAS, JUEGO 100 UDS, DESLIZAMIENTO DEL EXTREMO DEL PERFIL","AlCubar - M8X30 HORDOZÓ CSAVAR ALCUBAR 1000A+, 8.8 OSZTÁLYHOZ + ALTÁTÉKOK, DIÁK, 100 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20089","ALCUBAR - PODKŁADKA CU M12/40 POD KOŃCÓWKI KABLOWE, KPL.100SZT",828.8,"1-ZE-08",0.05,2,"OE_BUSBARS_ALCUBAR","20089","SZT","73182200",null,"230320LK","5901988200794","AlCu - Rondelle Cu M12/40 sous cosses de câble, set 100p","AlCu - Cu M12/40 washer for cable terminals, 100 pcs set","ALCUB- ARANDELA CU M12/40 PARA TERMINALES, 100UDS","AlCubar - CU M12/40 ALMÁT KÁBELTERMÁKHOZ, 100 DÉS KÉSZLET"]
["20090","ALCUBAR - ŚRUBA ZAMKOWA M6X20, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",112,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","73181595","25.94.11.0",null,"5901988200909","AlCu - Vis à tête cylindrique M6x20, classe 8.8, + rondelles, écrous, jeu de 100 pièces, glissées à partir de l'extrémité du profilé","AlCu - Square bolt M6x20, class 8.8, + washers, nuts, set of 100 pieces, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M6X20, 100UDS","AlCubar - SZÁLLÍTÓ CSAVAR M6X20, 8.8 OSZTÁLY, + ALTÁTÉKOK, ANYÁK, 100 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20091","ALCUBAR - ŚRUBA ZAMKOWA M8X20 DLA ALCUBAR 1000A+, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",171.4,"1-ZE-08",0.10833333333333334,2,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988200916","AlCu - Vis à tête cylindrique M8x20, classe 8.8, + rondelles, écrous, jeu de 100 pièces, insérés à partir de l'extrémité du profil","AlCu - Square bolt M8x20, class 8.8, + washers, nuts, 100 pcs set, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M8X20, 100UDS","AlCubar - M8X20 HORDOZÓ CSAVAR ALCUBAR 1000A+, 8.8 OSZTÁLYHOZ, + ALTÁTÉKOK, DIÁK, 100 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20092","ALCUBAR - ŚRUBA ZAMKOWA M8X25 DLA ALCUBAR 1000A+, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",180.3,"1-ZE-08",0.13333333333333333,4,"OE_BUSBARS_ALCUBAR","20092","SZT","73181595","25.94.11.0","230908LK","5901988200923","AlCu - Vis à tête cylindrique M8x25, classe 8.8, + rondelles, écrous, jeu de 100 pièces, glissés à partir de l'extrémité du profilé","AlCu - Square head bolt M8x25, class 8.8, + washers, nuts, 100 pcs set, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M8X25, 100UDS","AlCubar - M8X25 HORDOZÓ CSAVAR ALCUBAR 1000A+, 8.8 OSZTÁLYHOZ + ALTÁTÉKOK, DIÁK, 100 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20093","ALCUBAR - ŚRUBA ZAMKOWA M8X35 DLA ALCUBAR 1000A+, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",199.4,"1-ZE-08",0.24166666666666667,5,"OE_BUSBARS_ALCUBAR",null,"SZT","73181595","25.94.11.0",null,"5901988200930","AlCu - Vis de blocage M8x35, classe 8.8, + rondelles, écrous, jeu de 100 pièces, glissés à partir de l'extrémité du profilé","AlCu - Square bolt M8x35, class 8.8, + washers, nuts, set of 100 pieces, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M8X35, 100UDS","AlCubar - M8X35 HORDOZÓ CSAVAR ALCUBAR 1000A+, 8.8 OSZTÁLYHOZ, + ALTÁTÉKOK, ANYA, KÉSZLET 100 DB, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20094","ALCUBAR - ŚRUBA ZAMKOWA M12X30, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",347.2,"1-ZE-08",0.35,7,"OE_BUSBARS_ALCUBAR","20094","SZT","73181595","25.94.11.0","230914LK","5901988200947","AlCu - Vis de blocage M12x30, classe 8.8, + rondelles, écrous, jeu de 100 pièces, glissés à partir de l'extrémité du profilé","AlCu - Square bolt M12x30, class 8.8, + washers, nuts, set of 100 pieces, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M12X30, 100UDS","AlCubar - HORDOZÓ CSAVAR M12X30, KL 8.8, + ALÁTÉTI, NUTS, 100 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20095","ALCUBAR - ŚRUBA ZAMKOWA M12X35, KL 8.8, + PODKŁADKI, NAKRĘTKI,  KPL.100SZT, WSUWANE OD KOŃCA PROFILA",394.2,"1-ZE-08",0.1,2,"OE_BUSBARS_ALCUBAR","20095","SZT","73181595","25.94.11.0","230914LK","5901988200954","AlCu - Vis de blocage M12x35, classe 8.8, + rondelles, écrous, set de 100 pièces, glissées à partir de l'extrémité du profilé","AlCu - Square bolt M12x35, class 8.8, + washers, nuts, 100 pcs set, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. CABEZA PLANA M12X35, 100UDS","AlCubar - HORDOZÓ CSAVAR M12X35, 8.8 OSZTÁLY, + ALTÁTÉKOK, ANYÁK, KÉSZLET 100 DB, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20096","ALCUBAR - ŚRUBA PRZESUWNA, MŁOTKOWA Z KULKĄ M8X25 DO ROWKA 8MM, + PODKŁADKI, NAKRĘTKI, KPL.20SZT, MAX 630A",138.9,"1-ZE-08",13.3,2,"OE_BUSBARS_ALCUBAR","20096","KPL","73181595","25.94.11.0","230320LK","5901988200961","AlCu - Vis coulissante, marteau à bille M8x25 pour rainure de 8mm, + rondelles, écrou, lot de 20pcs, max. 630A","AlCu - Sliding hammer screw with a ball M8x25 for a 8mm groove, + washers, nuts, set of 20 pieces, max 630A","ALCUB-TORNILLO CABEZA MARTILLO M8X25, 630A 20UDS","AlCubar - CSÚSZTÓ, KAPCSOLATOS CSAVAR GOLYÓVAL M8X25 8MM-ES VONÁZHOZ, + ALTÁTÉKOK, ANYA, 20 DB-OS SZETT, MAX 630A"]
["20097","ALCUBAR - ŚRUBA PRZESUWNA, MŁOTKOWA Z KULKĄ M8X39 DO ROWKA 8MM, + PODKŁADKI, NAKRĘTKI, KPL.20SZT, MAX 630A",151.19999999999999,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20097","KPL","73181595","25.94.11.0","230320LK","5901988200978","AlCu - Vis coulissante, marteau à bille rainure M8x39 à 8mm, + rondelles, écrous, jeu de 20pcs, max 630A","AlCu - Sliding hammer screw with a ball M8x39 for a 8mm groove, + washers, nuts, set of 20 pieces, max 630A","ALCUB-TORNILLO CABEZA MARTILLO M8X35, 630A 20UDS","AlCubar - CSÚSZTÓ, KAPCSOLATOS CSAVAR GOLYÓVAL M8X39 8MM RÉDÉKHEZ, + ALTÁTÉKOK, ANYA, 20 DB-OS SZETT, MAX 630A"]
["20098","ALCUBAR - ŚRUBA PRZESUWNA, MŁOTKOWA Z KULKĄ M12X30 DO ROWKA 12MM, + PODKŁADKI, NAKRĘTKI, KPL.20SZT.",180.3,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20098","KPL","73181595","25.94.11.0","230320LK","5901988200985","AlCu - Vis coulissante, marteau avec boule M12x30 pour rainure de 12mm, + rondelles, écrous, lot de 20pcs.","AlCu - Sliding hammer screw with a ball M12x30 for a 12mm groove, + washers, nuts, set of 20 pcs.","ALCUB-TORNILLO CABEZA MARTILLO M12X30, 2500A 20UDS","AlCubar - M12X30 GOLYÓS CSAVAR 12MM VONÁZHOZ, + ALTÁTÉKOK, ANYÁK, 20 DB-OS SZETT."]
["20099","ALCUBAR - ŚRUBA PRZESUWNA, MŁOTKOWA Z KULKĄ M12X35 DO ROWKA 12MM, + PODKŁADKI, NAKRĘTKI, KPL.20SZT.",209.4,"1-ZE-08",4.1666666666666664E-2,1,"OE_BUSBARS_ALCUBAR","20099","SZT","73181595","25.94.11.0",null,"5901988200992","AlCu - Vis coulissante, marteau avec boule M12x35 pour rainure de 12mm, + rondelles, écrous, lot de 20pcs.","AlCu - Sliding hammer screw with a ball M12x35 for a 12mm groove, + washers, nuts, set of 20 pcs.","ALCUB-TORNILLO CABEZA MARTILLO M12X35, 2500A 20UDS","AlCubar - CSÚSZTÓ, M12X35 GOLYÓS KALACÁS CSAVAR 12MM-ES VONÁZHOZ, + ALTÁTÉKOK, ANYÁK, 20 DB-OS SZETT."]
["20100","ALCUBAR / CU - IZOLATOR 1P, D200, MOST PIONOWY Z BOKU",124.3,"1-ZE-01",null,null,"OE_INSULATOR_D400","20100","SZT","85469010","27.90.12.0",null,"5901988201005","AlCu/Cu - Isolateur 1P, P200, pont vertical sur le côté","AlCu/Cu - 1P, D200 insulator, Vertical bridge on the side","ALCUB / CU- SOPORTE 1P, D200, EMB. VERT. LATERAL","AlCubar / CU - SZIGETELŐ 1P, D200, OLDALSÓ FÜGGŐLEGES HÍD"]
["20101","ALCUBAR / CU - IZOLATOR 1P, D400, MOST PIONOWY Z BOKU",237.4,"1-ZE-01",3.3333333333333333E-2,1,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201012","AlCu/Cu - Isolateur 1P, P400, pont vertical sur le côté","AlCu/Cu - 1P, D400 insulator, Vertical bridge on the side","ALCUB / CU- SOPORTE 1P, D400, EMB. VERT. LATERAL","AlCubar / CU - SZIGETELŐ 1P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20103","ALCUBAR / CU - IZOLATOR 3P, D400, MOST PIONOWY Z BOKU",266.60000000000002,"1-ZE-08",0.40833333333333333,2,"OE_INSULATOR_D400","20103","SZT","85469010","27.90.12.0",null,"5901988201036","AlCu/Cu - Isolateur 3P, P400, pont vertical sur le côté","AlCu/Cu - Insulator 3P, D400, Vertical bridge on the side","ALCUB/CU- SOPORTE 3P D400 PARA EMB. VERTICAL LATERAL","ALCUBAR / CU - 3P SZIGETELŐ, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20104","ALCUBAR / CU - IZOLATOR 4P, D400, MOST PIONOWY Z BOKU",297.89999999999998,"1-ZE-08",8.3333333333333329E-2,2,"OE_INSULATOR_D400","20104","SZT","85469010","27.90.12.0",null,"5901988201043","AlCu/Cu - Isolateur 4P, P400, pont vertical sur le côté","AlCu/Cu - 4P, D400 insulator, Vertical bridge on the side","ALCUB/CU- SOPORTE 4P D400 PARA EMB. VERTICAL LATERAL","AlCubar / CU - SZIGETELŐ 4P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20105","ALCUBAR / CU - IZOLATOR 3P, TYŁ, MOST POZIOMY NA PLECACH",245.3,"1-ZE-08",null,null,"OE_INSULATOR_D400",null,"SZT","85469010",null,null,"5901988201050","AlCu/Cu - ISOLANT 3P, ARRIÈRE, PONT HORIZONTAL À L'ARRIÈRE","AlCu/Cu - 3P INSULATOR, REAR, Horizontal BRIDGE ON THE BACK","*AlCu/Cu - AISLADOR 3P TRASERO PUENTE HORIZONTAL POSTERIOR","AlCubar / CU - 3P SZIGETELŐ, HÁTSÓ, VÍZSZINTES HÍD A HÁTSON"]
["20106","ALCUBAR / CU - IZOLATOR 4P, TYŁ, MOST POZIOMY NA PLECACH",273.3,"1-ZE-08",null,null,"OE_INSULATOR_D400",null,"SZT","85469010",null,null,"5901988201067","AlCu/Cu - ISOLANT 4P, ARRIÈRE, PONT HORIZONTAL À L'ARRIÈRE","AlCu/Cu - 4P INSULATOR, REAR, Horizontal BRIDGE ON THE BACK","*AlCu/Cu - AISLADOR 4P TRASERO PUENTE HORIZONTAL POSTERIOR","AlCubar / CU - 4P SZIGETELŐ, HÁTSÓ, VÍZSZINTES HÍD A HÁTSON"]
["20108","ALCUBAR / CU - IZOLATOR 3P, DOIZOLOWANIE SZYN PIONOWYCH",320.3,"1-ZE-08",null,null,"OE_INSULATOR_D400","20108","SZT","85469010","27.90.12.0",null,"5901988201081","AlCu/Cu - Isolant 3P, isolation des rails verticaux","AlCu/Cu - 3P insulator, insulation of Vertical busbars","ALCUB / CU- SOPORTE 3P, PARA REFORZAR EMB. VERT.","ALCUBAR / CU - 3P SZIGETELŐ, FÜGGŐLEGES SÍNEK SZIGETELÉS"]
["20109","ALCUBAR / CU - IZOLATOR 4P, DOIZOLOWANIE SZYN PIONOWYCH",402.1,"1-ZE-08",null,null,"OE_INSULATOR_D400","20109","SZT","85469010","27.90.12.0",null,"5901988201098","AlCu/Cu - Isolateur 4P, isolation des rails verticaux","AlCu/Cu - 4P insulator, insulation of Vertical busbars","ALCUB / CU- SOPORTE 4P, PARA REFORZAR EMB. VERT.","ALCUBAR / CU - 4P SZIGETELŐ, FÜGGŐLEGES SÍNEK SZIGETELÉS"]
["20110","AlCubar / Cu - Izolator 2x3P inox, D800, most poziomy",369.6,"1-ZE-01",null,null,"OE_INSULATOR_D400","20110","SZT","85469010",null,null,"5901988201104","AlCu/Cu - Isolateur 2x3P inox, P800, pont horizontal","AlCu/Cu - 2x3P inox insulator, D800, Horizontal bridge","ALCUB / CU- SOPORTE 1P, EMB. HORIZ. FONDO PARA UNION BARRAS","AlCubar / Cu - Szigetelő 2x3P inox, D800, vízszintes híd"]
["20111","ALCUBAR / CU - IZOLATOR 1P, D400, MOST POZIOMY",237.4,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201111","AlCu/Cu - Isolateur 1P, P400, pont horizontal","AlCu/Cu - 1P, D400 insulator, Horizontal bridge","ALCUB / CU- SOPORTE 1P, D400, EMB. HORIZ.","AlCubar / CU - SZIGETELŐ 1P, D400, VÍZSZINTES HÍD"]
["20112","AlCubar / Cu - Izolator 2P inox, D800, most poziomy",369.6,null,0.45,5,"OE_INSULATOR_DEPTH","20112",null,null,null,"240205PW",null,"AlCubar / Cu - Isolateur inox 2P, D800, jeu de barres horizontal","AlCubar / Cu - 2P inox insulator, D800, horizontal busbar","AlCubar / Cu - Aislador inox 2P, D800, embarrado horizontal","AlCubar / Cu - 2P inox szigetelő, D800, vízszintes híd"]
["20113","ALCUBAR / CU - IZOLATOR 3P, D400, MOST POZIOMY",320.3,"1-ZE-08",0.24166666666666667,4,"OE_INSULATOR_D400","20113","SZT","85469010","27.90.12.0",null,"5901988201135","AlCu/Cu - Isolateur 3P, P400, pont horizontal","AlCu/Cu - Insulator 3P, D400, Horizontal bridge","ALCUB/CU- SOPORTE 3P D400 PARA EMB. HORIZ.","AlCubar / CU - 3P SZIGETELŐ, D400, VÍZSZINTES HÍD"]
["20114","ALCUBAR / CU - IZOLATOR 4P, D400, MOST POZIOMY",402.1,"1-ZE-08",null,null,"OE_INSULATOR_D400","20114","SZT","85469010","27.90.12.0",null,"5901988201142","AlCu/Cu - Isolateur 4P, P400, pont horizontal","AlCu/Cu - 4P, D400 insulator, Horizontal bridge","ALCUB/CU- SOPORTE 4P D400 PARA EMB. HORIZ.","AlCubar / CU - ISOLATOR 4P, D400, VÍZSZINTES HÍD"]
["20115","AlCubar / Cu - Izolator 3P inox, D1000, most poziomy",441.3,"1-ZE-01",null,null,"OE_INSULATOR_D400","20115","SZT","85469010",null,null,"5901988201159","AlCu/Cu - Isolateur 3P inox, P1000, pont horizontal","AlCu/Cu - 3P inox insulator, D1000, Horizontal bridge","ALCUB/CU- SOPORTE INOX 3P, D1000, EMB. HORIZ.","AlCubar / Cu - 3P inox szigetelő, D1000, vízszintes híd"]
["20116","AlCubar / Cu - Izolator 1P inox, D1000, most poziomy",346.1,"1-ZE-01",null,null,"OE_INSULATOR_D400","20116","SZT","85469010",null,null,"5901988201166","AlCu/Cu - Isolateur 1P inox, P1000, pont horizontal","AlCu/Cu - 1P inox insulator, D1000, Horizontal bridge","ALCUB/CU- SOPORTE INOX 1P, D1000, EMB. HORIZ.","AlCubar / Cu - Insulator 1P inox, D1000, vízszintes híd"]
["20117","ALCUBAR / CU - IZOLATOR, DOIZOLOWANIE SZYN POZIOMYCH POLA NAROŻNEGO",249.8,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010",null,null,"5901988201173","AlCu/Cu - ISOLANT, ISOLANT SUPPLÉMENTAIRE DES BARRES HORIZONTALES DES BARRES D'ANGLE","AlCu/Cu - INSULATOR, ADDITIONAL INSULATION OF Horizontal BARS OF CORNER BARS","*AlCu/Cu - AISLADOR, AISLAMIENTO ADICIONAL DE BARRAS HORIZONTALES DE BARRAS DE ESQUINA","AlCubar / CU - IZOLÁTOR, A SAROKTERÜLET VÍZSZINTES SÍNÉNEK SZIGETELÉSE"]
["20118","ALCUBAR / CU - IZOLATOR 3P, DOIZOLOWANIE SZYN POZIOMYCH",320.3,"1-ZE-08",null,null,"OE_INSULATOR_D400","20118","SZT","85469010","27.90.12.0",null,"5901988201180","AlCu/Cu - Isolateur 3P, isolation des rails horizontaux","AlCu/Cu - 3P insulator, insulation of Horizontal busbars","ALCUB / CU- SOPORTE 3P, REFUERZO EMB. HORIZ. ","ALCUBAR / CU - 3P SZIGETELŐ, VÍZSZINTES RÚDAK SZIGETELÉSE"]
["20119","ALCUBAR / CU - IZOLATOR 4P, DOIZOLOWANIE SZYN POZIOMYCH",402.1,"1-ZE-08",null,null,"OE_INSULATOR_D400","20119","SZT","85469010",null,null,"5901988201197","AlCu/Cu - Isolateur 4P, isolation des rails horizontaux","AlCu/Cu - 4P insulator, insulation of Horizontal busbars","ALCUB / CU- SOPORTE 4P, REFUERZO EMB. HORIZ.","ALCUBAR / CU - 4P SZIGETELŐ, VÍZSZINTES BUSZSZIGETELÉS"]
["20120","ALCUBAR / CU - IZOLATOR 1P, D200, MOST POZIOMY, DLA ŁĄCZNIKA SZYN",124.3,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201203","AlCu - Isolateur 1P, P200, horizontal, pour connecteur de jeu de barres","AlCu/Cu - 1P, D200 insulator, Horizontal bridge, for busbar connector","ALCUB- SOPORTE 1P, D200, HORIZ. PARA UNION BARRAS","AlCubar / CU - SZIGETELŐ 1P, D200, VÍZSZINTES HÍD, BUSZ CSATLAKOZÁSHOZ"]
["20122","ALCUBAR / CU - IZOLATOR 1P, D400, MOST POZIOMY, DLA ŁĄCZNIKA SZYN",237.4,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201227","AlCu - Isolateur 1P, P400, horizontal, pour connecteur de jeu de barres","AlCu/Cu - 1P, D400 insulator, Horizontal bridge, for busbar connector","ALCUB- SOPORTE 1P, D400, HORIZ. PARA UNION BARRAS","AlCubar / CU - SZIGETELŐ 1P, D400, VÍZSZINTES HÍD, BUSZ CSATLAKOZTATÁSHOZ"]
["20123","ALCUBAR - IZOLATOR 3P, D400, POZIOMO, DLA ŁĄCZNIKA SZYN",320.3,"1-ZE-08",3.3333333333333333E-2,2,"OE_INSULATOR_D400","20123","SZT","85469010","27.90.12.0",null,"5901988201234","AlCu - Isolateur 3P, P400, horizontal, pour connecteur de jeu de barres","AlCu - Insulator 3P, D400, Horizontal, for rail connector","ALCUB/CU-SOPORTE 3P, D400 PARA PLETINA DE UNION HORIZ. ","AlCubar - 3P SZIGETELŐ, D400, VÍZSZINTES, BUSZ CSATLAKOZÁSHOZ"]
["20124","ALCUBAR - IZOLATOR 4P, D400, POZIOMO, DLA ŁĄCZNIKA SZYN",402.1,"1-ZE-08",null,null,"OE_INSULATOR_D400","20124","SZT","85469010","27.90.12.0",null,"5901988201241","AlCu - Isolateur 4P, P400, horizontal, pour raccord de rail","AlCu - Insulator 4P, D400, Horizontal, for rail connector","ALCUB/CU-SOPORTE 4P, D400 PARA PLETINA DE UNION HORIZ. ","AlCubar - SZIGETELŐ 4P, D400, VÍZSZINTES, BUSZ CSATLAKOZÁSHOZ"]
["20125","Cu - Wspornik izolatora, D400, most poziomy tylko Miedź",106.4,"1-ZE-08",2,5,"OE_INSULATOR_DEPTH","20125","SZT","85469010",null,"230807LK","5901988201258","AlCu/Cu - Isolant, P400, pont horizontal","Cu - Insulator support, D400, Horizontal bridge only for Copper","ALCUB / CU- SOPORTE, D400, EMB. HORIZ.","Cu - Szigetelő tartó, D400, csak vízszintes híd Réz"]
["20126","ALCUBAR / CU - IZOLATOR 4P INOX, D600, MOST POZIOMY",425.6,"1-ZE-08",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201265","AlCu/Cu - Isolant 4P inox, P600, pont horizontal","AlCu/Cu - 4P inox insulator, D600, Horizontal bridge","ALCUB / CU- SOPORTE 4P INOX, D600, EMB. HORIZ.","AlCubar / CU - 4P INOX SZIGETELŐ, D600, VÍZSZINTES HÍD"]
["20127","ALCUBAR / CU - IZOLATOR 3P INOX, D800, MOST POZIOMY",414.4,"1-ZE-08",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201272","AlCu/Cu - Isolant 3P inox, P800, pont horizontal","AlCu/Cu - 3P inox insulator, D800, Horizontal bridge","ALCUB / CU- SOPORTE 3P INOX, D800, EMB. HORIZ.","AlCubar / CU - 3P INOX SZIGETELŐ, D800, VÍZSZINTES HÍD"]
["20128","ALCUBAR / CU - IZOLATOR 4P INOX, D800, MOST POZIOMY",497.3,"1-ZE-08",1.6666666666666666E-2,1,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201289","AlCu/Cu - Isolateur 4P inox, P800, pont horizontal","AlCu/Cu - 4P inox insulator, D800, Horizontal bridge","ALCUB / CU- SOPORTE 4P INOX, D800, EMB. HORIZ.","AlCubar / CU - 4P INOX SZIGETELŐ, D800, VÍZSZINTES HÍD"]
["20129","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, ROZSTAW 50,61MM, POLIWĘGLAN 15X240X2000MM",356.2,"1-ZE-08",0.4,2,"OE_SEPARATION_BUSBAR","20129","SZT","85389099","27.33.14.0",null,"5901988201296","AlCu - Couvercle de pont AlCubar H27, polycarbonate de 40x240mmx2000mm","AlCu - AlCubar H27 bridge cover, distance 50.61mm, polycarbonate 15x240x2000mm","ALCUB-TAPA PROTECC. PARA EMBARRADO ALCUB- 630A L=500MM","AlCubar - ALCUBAR H27 HÍDBURKOLAT, TÉR 50,61MM, POLICARBONÁT 15X240X2000MM"]
["20130","ALCUBAR / CU - WSPORNIK IZOLATORA MOST POZIOMY, INOX, 2M, ROZSTAW 100MM",258.7,"1-ZE-01",0.13333333333333333,1,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201302","AlCu/Cu - Support isolant, pont horizontal, 2 m, espacement 100mm","AlCu/Cu - Insulator bracket, Horizontal bridge, inox, 2m, spacing 100mm","ALCUB / CU-SOPORTE EMB. HORIZ., INOX, 2M, DIST. 100MM","AlCubar / CU - SZIGETELŐ TÁMASZ VÍZSZINTES HÍD, INOX, 2M, HELY 100 mm"]
["20131","ALCUBAR / CU - WSPORNIK IZOLATORA MOST PIONOWY, INOX, 2M, ROZSTAW 100MM",271,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201319","AlCu/Cu - Support isolant vertical, pont de 2 m, espacement de 100mm","AlCu/Cu - Insulator support Vertical bridge, inox, 2m, spacing 100mm","ALCUB / CU-SOPORTE EMB. VERT., INOX, 2M, DIST. 100MM","AlCubar / CU - SZIGETELT TARTÓ, FÜGGŐLEGES HÍD, INOX, 2M, HELY 100MM"]
["20132","ALCUBAR / CU - ELEMENT GÓRNY IZOLATORA, INOX, 1P",61.3,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85389099","27.90.12.0",null,"5901988201326","AlCu/Cu - Elément supérieur isolant, inox, 1P","AlCu/Cu - Insulator top piece, inox, 1P","ALCUB / CU- PARTE SUPERIOR SOPORTE, INOX, 1P","AlCubar / CU - FELSŐ SZIGETELŐELEM, INOX, 1P"]
["20133","ALCUBAR / CU - ELEMENT GÓRNY IZOLATORA, INOX, 3P, ROZSTAW 100MM",82.4,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85389099","27.90.12.0",null,"5901988201333","AlCu/Cu - Elément supérieur d'isolateur, 3P, Espacement 100mm","AlCu/Cu - Upper insulator, inox, 3P, spacing 100mm","ALCUB / CU- PARTE SUPERIOR SOPORTE, INOX, 3P, DIST. 100MM","AlCubar / CU - FELSŐ SZIGETELŐELEM, INOX, 3P, HELY 100mm"]
["20134","ALCUBAR / CU - ELEMENT GÓRNY IZOLATORA, INOX, 4P, ROZSTAW 100MM",91.8,"1-ZE-01",0.4,4,"OE_INSULATOR_D400",null,"SZT","85389099","27.90.12.0",null,"5901988201340","AlCu/Cu - Élément supérieur d'isolateur, 4P, espacement 100mm","AlCu/Cu - Upper insulator, inox, 4P, spacing 100mm","ALCUB / CU- PARTE SUPERIOR SOPORTE, INOX, 4P, DIST. 100MM","AlCubar / CU - SZIGETELŐ FELSŐ ELEM, INOX, 4P, HELY 100mm"]
["20135","ALCUBAR / CU - WSPORNIK IZOLATORA MOST POZIOMY, OCYNK, 2M, ROZSTAW 100MM",233,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201357","AlCu/Cu - Support isolant, pont horizontal, galvanisé, espacement de 2m, 100mm","AlCu/Cu - Insulator support, Horizontal bridge, Galvanized, 2m, spacing 100mm","ALCUB / CU-SOPORTE EMB. HORIZ. 2M, DIST. 100MM","AlCubar / CU - SZIGETELŐ TÁMASZ VÍZSZINTES HÍD, HONGGANYOZOTT, 2M, HELY 100MM"]
["20136","ALCUBAR / CU - WSPORNIK IZOLATORA MOST PIONOWY, OCYNK, 2M, ROZSTAW 100MM",245.3,"1-ZE-01",0.01,1,"OE_INSULATOR_D400","20136","SZT","85469010","27.90.12.0",null,"5901988201364","AlCu/Cu - Support d'isolateur, pont vertical, galvanisé, espacement de 2m, 100mm","AlCu/Cu - Insulator support Vertical bridge, Galvanized, 2m, spacing 100mm","ALCUB / CU-SOPORTE EMB. VERT., 2M, DIST. 100MM","AlCubar / CU - SZIGETELŐ TARTÓ, FÜGGŐLEGES HÍD, HOGAGYZAT, 2M, HELY 100MM"]
["20137","ALCUBAR / CU - ELEMENT GÓRNY IZOLATORA, OCYNK, 1P",56.4,"1-ZE-01",1.05,1,"OE_INSULATOR_D400",null,"SZT","85389099","27.90.12.0",null,"5901988201371","AlCu/Cu - Elément supérieur isolant, galvanisé, 1P","AlCu/Cu - Top insulator, Galvanized, 1P","ALCUB / CU- PARTE SUPERIOR SOPORTE, 1P","AlCubar / CU - FELSŐ SZIGETELŐELEM, HORGANYOZOTT, 1P"]
["20138","ALCUBAR / CU - ELEMENT GÓRNY IZOLATORA, OCYNK, 3P, ROZSTAW 100MM",75.400000000000006,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85389099","27.90.12.0",null,"5901988201388","AlCu/Cu - Elément supérieur isolant, galvanisé, 3P, écartement 100mm","AlCu/Cu - Top insulator, Galvanized, 3P, spacing 100mm","ALCUB / CU- PARTE SUPERIOR SOPORTE, 3P, DIST. 100MM","AlCubar / CU - FELSŐ SZIGETELŐELEM, HORGANYOZOTT, 3P, HELY 100MM"]
["20139","ALCUBAR / CU - ELEMENT GÓRNY IZOLATORA, OCYNK, 4P, ROZSTAW 100MM",82.4,"1-ZE-01",null,null,"OE_INSULATOR_D400","20139","SZT","85389099","27.90.12.0",null,"5901988201395","AlCu/Cu - Elément supérieur isolant, galvanisé, 4P, écartement 100mm","AlCu/Cu - Top insulator, Galvanized, 4P, spacing 100mm","ALCUB / CU- PARTE SUPERIOR SOPORTE, 4P, DIST. 100MM","AlCubar / CU - SZIGETELŐ FELSŐ ELEM, HONGGANYOZOTT, 4P, HELY 100 mm"]
["20140","ALCUBAR - WSPORNIK IZOLATORA 630A, MOST POZIOMY, OCYNK, 2M, ROZSTAW 50MM",233,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","85389099","27.90.12.0",null,"5901988201401","AlCu - Support isolant 630A, pont horizontal, galvanisé, espacement de 2m, 50mm","AlCu - Insulator support 630A, Horizontal bridge, Galvanized, 2m, 50mm spacing","ALCUB-SOPORTE 630A, EMB. HORIZ. 2M, DIST. 50MM","AlCubar - SZIGETELŐTÁMASZTÓ 630A, VÍZSZINTES HÍD, HORGANYOZOTT, 2M, TÉR 50MM"]
["20141","ALCUBAR - WSPORNIK IZOLATORA 630A, MOST PIONOWY, OCYNK, 2M, ROZSTAW 50MM",245.3,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","85389099","27.90.12.0",null,"5901988201418","AlCu - Support isolant 630A, pont vertical, galvanisé, espacement de 2m, 50mm","AlCu - Insulator support 630A, Vertical bridge, Galvanized, 2m, 50mm spacing","ALCUB-SOPORTE 630A, EMB. VERT., 2M, DIST. 50MM","AlCubar - SZIGETELŐTÁMASZTÓ 630A, FÜGGŐLEGES HÍD, HORGANYOZOTT, 2M, TÉR 50MM"]
["20142","ALCUBAR - ELEMENT GÓRNY IZOLATORA 630A, OCYNK, 1P",56.3,"1-ZE-01",null,null,"OM_SUPPORT",null,"SZT","85389099","27.90.12.0",null,"5901988201425","AlCu - Elément supérieur d'isolateur 630A, galvanisé, 1P","AlCu - Insulator top piece 630A, Galvanized, 1P","ALCUB- PARTE SUPERIOR SOPORTE 630A, 1P","AlCubar - 630A SZIGETELŐ FELSŐ ELEME, HOGAGYZAT, 1P"]
["20143","ALCUBAR - ELEMENT GÓRNY IZOLATORA 630A, OCYNK, 3P, ROZSTAW 50MM",75.2,"1-ZE-01",null,null,"OM_SUPPORT",null,"SZT","85389099","27.90.12.0",null,"5901988201432","AlCu - Elément supérieur d'isolateur 630A, galvanisé, 3P, espacement de 50mm","AlCu - Top element of insulator 630A, Galvanized, 3P, spacing 50mm","ALCUB- PARTE SUPERIOR SOPORTE 630A, 3P, DIST. 50MM","AlCubar - 630A SZIGETELŐ FELSŐ ELEM, HORGANYOZOTT, 3P, TÉR 50MM"]
["20144","ALCUBAR - ELEMENT GÓRNY IZOLATORA 630A, OCYNK, 4P, ROZSTAW 50MM",82.4,"1-ZE-01",null,null,"OM_SUPPORT",null,"SZT","85389099","27.90.12.0",null,"5901988201449","AlCu - Elément supérieur d'isolateur 630A, galvanisé, 4P, espacement de 50mm","AlCu - Top element of insulator 630A, Galvanized, 4P, spacing 50mm","ALCUB- PARTE SUPERIOR SOPORTE 630A, 4P, DIST. 50MM","AlCubar - 630A SZIGETELŐ FELSŐ ELEM, HORGANYOZOTT, 4P, TÉR 50MM"]
["20145","ALCUBAR - ZAŚLEPKA ALCUBAR H27 1SZT",1.7,"1-ZE-01",19,5,"OM_SUPPORT","20145","SZT","85389099","27.33.14.0",null,"5901988201456","AlCu - Embout AlCubar H27 1pcs","AlCu - End cap AlCubar H27 1 pc","ALCUB- TAPON ALCUB H27 1UND.","ALCUBAR - ALCUBAR H27 PLUG 1DB"]
["20146","ALCUBAR / CU - IZOLATOR 1P, MOST POZIOMY NA PLECACH",124.3,"1-ZE-01",0.64166666666666672,10,"OE_INSULATOR_D400","20146","SZT","85469010",null,null,"5901988201463","AlCu/Cu - Isolant 1P, pont horizontal à l'arrière","AlCu/Cu - 1P insulator, Horizontal bridge on the back","ALCUB / CU- SOPORTE 1P, EMB. HORIZ. FONDO","ALCUBAR / CU - 1P SZIGETELŐ, VÍZSZINTES HÍD A HÁTSON"]
["20147","ALCUBAR / CU - IZOLATOR 1P, MOST POZIOMY NA PLECACH, DLA ŁĄCZNIKA SZYN",124.3,"1-ZE-01",5.8333333333333334E-2,4,"OE_INSULATOR_D400","20147","SZT","85469010","27.90.12.0",null,"5901988201470","AlCu/Cu - Isolant 1P, pont horizontal ? l'arri?re, pour raccord de rail","AlCu/Cu - 1P insulator, Horizontal bridge on the back, for a rail connector","ALCUB/CU- SOPORTE 1P, EMB. HORIZ. EN LA PARTE TRASERA","AlCubar / CU - 1P SZIGETELŐ, VÍZSZINTES HÍD A HÁTSON, SÍN CSATLAKOZÓHOZ"]
["20148","ALCUBAR / CU - IZOLATOR 3P, MOST POZIOMY NA PLECACH",320.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988201487","AlCu/Cu - Isolant 3P, pont horizontal à l'arrière","AlCu/Cu - 3P insulator, Horizontal bridge on the back","ALCUB / CU- SOPORTE 3P, EMB. HORIZ. FONDO","AlCubar / CU - 3P SZIGETELŐ, VÍZSZINTES HÍD A HÁTSON"]
["20149","ALCUBAR / CU - IZOLATOR 4P, MOST POZIOMY NA PLECACH",402.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20149","SZT","85469010","27.90.12.0",null,"5901988201494","AlCu/Cu - Isolateur 4P, pont horizontal à l'arrière","AlCu/Cu - 4P insulator, Horizontal bridge on the back","ALCUB / CU- SOPORTE 4P, EMB. HORIZ. FONDO","AlCubar / CU - 4P SZIGETELŐ, VÍZSZINTES HÍD A HÁTSON"]
["20150","ALCUBAR - IZOLATOR 630A 1P, D200, MOST PIONOWY Z BOKU",56.4,"1-ZE-08",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988201500","AlCu - Isolateur 630A 1P, P200, pont vertical sur le côté","AlCu - 630A 1P, D200 insulator, Vertical bridge on the side","ALCUB- SOPORTE 630A 1P, D200, EMB. VERT. LATERAL","AlCubar - SZIGETELŐ 630A 1P, D200, OLDALSÓ FÜGGŐLEGES HÍD"]
["20152","ALCUBAR - IZOLATOR 630A 3P, D400, MOST PIONOWY Z BOKU, ROZSTAW 105MM",124.3,"1-ZE-01",4.1666666666666664E-2,1,"OE_INSULATOR_D400","20152","SZT","85469010",null,null,"5901988201524","AlCu - 630A 3P, isolateur P400, pont vertical sur le côté, distance 105mm","AlCu - Insulator 630A 3P, D400, Vertical bridge on the side, spacing 105mm","ALCUB- SOPORTE 3P,  630A, D400, EMB. VERTIC. LATERAL","AlCubar - SZIGETELŐ 630A 3P, D400, OLDALSÓ FÜGGŐLEGES HÍD, HELY 105mm"]
["20153","ALCUBAR - IZOLATOR 630A 3P, D400, MOST PIONOWY Z BOKU",133.30000000000001,"1-ZE-08",1.1166666666666667,6,"OE_INSULATOR_D400","20153","SZT","85469010",null,null,"5901988201531","AlCu - Isolateur 630A 3P, P400, pont vertical sur le côté","AlCu - Insulator 630A 3P, D400, Vertical bridge on the side","ALCUB- SOPORTE 630A 3P, D400, EMB. VERT. LATERAL","AlCubar - SZIGETELŐ 630A 3P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20154","ALCUBAR - IZOLATOR 630A 4P, D400, MOST PIONOWY Z BOKU",164.6,"1-ZE-08",1.1166666666666667,6,"OE_INSULATOR_D400","20154","SZT","85469010",null,null,"5901988201548","AlCu - Isolateur 630A 4P, P400, pont vertical sur le côté","AlCu - Insulator 630A 4P, D400, Vertical bridge on the side","ALCUB- SOPORTE 630A 4P, D400, EMB. VERT. LATERAL","AlCubar - SZIGETELŐ 630A 4P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20155","ALCUBAR - ŁĄCZNIK CU 4000 A (2X2500A) H100-H100, MOSTEK ŁĄCZĄCY (140X50X5MM)",53.9,"1-ZE-08",0.41666666666666669,2,"OE_BUSBARS_ALCUBAR","20155","SZT","74072900","24.44.22.0",null,"5901988201555","AlCu - Connecteur Cu 4000 A (2X2500A) H100-H100, (140X50X5MM)","AlCu - COUPLER CU 4000A (2X2500A) H100-H100, CONNECTING BRIDGE (140X50X5mm)","Alcubar UNION Cu para Alcubar 2500A en paralelo 4000A","AlCubar – CU CSATLAKOZÓ 4000 A (2X2500A) H100-H100, CSATLAKOZÓ HÍD (140X50X5MM)"]
["20156","ALCUBAR - ŁĄCZNIK CU 3200 A (2x1600A) H80-H80, (2x2500A) H100-H100R, MOSTEK ŁĄCZĄCY tył (110x50x5mm)",49.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20156","SZT","74072900","24.44.22.0",null,"5901988201562","AlCu - Connecteur Cu 3200 A (2x1600A) H80-H80, (2x2500A) H100-H100R, (110x50x5mm)","AlCu - CONNECTOR CU 3200 A (2x1600A) H80-H80, (2x2500A) H100-H100R, BRIDGE CONNECTING rear (110x50x5mm)","ALCUB- CONECTOR CU 3200 A (2X1600A) H80-H80, (2X2500A) H100-H100R ","AlCubar - CSATLAKOZÓ CU 3200 A (2x1600A) H80-H80, (2x2500A) H100-H100R, HÍD CSATLAKOZÁS hátul (110x50x5mm)"]
["20157","ALCUBAR - ŁĄCZNIK CU 1000A H50R (M12mm), TYPU I, 155X50X10MM",118.7,"1-ZE-08",0.81666666666666665,12,"OE_BUSBARS_ALCUBAR","20157","SZT","74072900","24.44.22.0",null,"5901988201579","AlCubar 50R - Connecteur Cu 1000 A, type I, M12mm, 105x50x10mm","AlCubar 50R - Cu 1000 A connector, type I, M12mm, 105x50x10mm","ALCUB- 50R- CONECTOR CU 1000 A, TIPO I, M12MM, 105X50X10MM","AlCubar – CSATLAKOZÓ CU 1000A H50R (M12mm), I. TÍPUS, 155X50X10MM"]
["20158","ALCUBAR - ŁĄCZNIK CU 2500 A, TYPU I ,ROZŁĄCZNIK LISTWOWY DLA ALCUBAR H100R, 340X100X10MM",488.3,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20158","SZT","74072900","24.44.22.0",null,"5901988201586","AlCu - connecteur Cu 2500 A, type I, sectionneur à bande pour AlCubar 100R, 340x100x10mm","AlCu - Coupler Cu 2500 A, type I, switch disconnector for AlCubar 100R, 340x100x10mm","ALCUB- CONECTOR CU 2500 A, TIPO I, PARA ALCUB- 100R, 340X100X10MM","ALCUBAR - CU 2500 A CSATLAKOZÓ, I. TÍPUS, SZALAGOS KAPCSOLÓ ALCUBAR H100R-HOZ, 340X100X10MM"]
["20159","ALCUBAR 100R - ŁĄCZNIK CU 2500 A, TYPU I DLA ALCUBAR H100-H100R, 250X100X10MM",376.3,"1-ZE-08",0.01,1,"OE_BUSBARS_ALCUBAR","20159","SZT","74072900",null,null,"5901988201593","AlCubar 100R - Connecteur Cu 2500A, type I, AlCubar H100-H100R, 200x100x10mm","AlCubar 100R - Cu 2500A connector, type I, for AlCubar H100-H100R, 200x100x10mm","ALCUB- 100R- CONECTOR CU 2500A, TIPO I, PARA ALCUB- H100-H100R","ALCUBAR 100R - CU CSATLAKOZÓ 2500 A, I. TÍPUS ALCUBA H100-H100R-HOZ, 250X100X10MM"]
["20160","ALCUBAR - ŁĄCZNIK CU 1000A H50-H50R (M8-M12mm), TYPU I, 155X50X10MM",118.7,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20160","SZT","74072900",null,null,"5901988201609","AlCu - Connecteur Cu 1000A H50-H50R (M8-M12mm), type I, 105X50X10MM","AlCu - 630A 1P insulator, Horizontal bridge on the back","ALCUB- SOPORTE 630A 1P, EMB. HORIZ. FONDO","AlCubar – CSATLAKOZÓ CU 1000A H50-H50R (M8-M12mm), I. TÍPUS, 155X50X10MM"]
["20161","ALCUBAR - IZOLATOR 630A 1P, MOST POZIOMY NA PLECACH",52.2,"1-ZE-08",0.43333333333333335,8,"OE_INSULATOR_D400","20161","SZT","85469010","27.90.12.0",null,"5901988201616","AlCu - Isolateur 630A 1P, pont horizontal à l'arrière","AlCu - 630A 1P insulator, Horizontal bridge on the back","ALCUB- AISLADOR 630A 1P, EMB. HORIZ. EN LA PARTE TRASERA","AlCubar - SZIGETELŐ 630A 1P, HÁLÁN VÍZSZINTES HÍD"]
["20163","ALCUBAR - IZOLATOR 630A 3P, D400, MOST POZIOMY",124.3,"1-ZE-08",null,null,"OE_INSULATOR_D400","20163","SZT","85469010","27.90.12.0",null,"5901988201630","AlCu - Isolateur 630A 3P, P400, pont horizontal","AlCu - 630A 3P, D400 insulator, Horizontal bridge","ALCUB- SOPORTE 630A 3P, D400, EMB. HORIZ.","AlCubar - SZIGETELŐ 630A 3P, D400, VÍZSZINTES HÍD"]
["20164","ALCUBAR - IZOLATOR 630A 4P, D400, MOST POZIOMY",164.6,"1-ZE-08",0.24166666666666667,2,"OE_INSULATOR_D400","20164","SZT","85469010","27.90.12.0",null,"5901988201647","AlCu - Isolateur 630A 4P, P400, pont horizontal","AlCu - 630A 4P, D400 insulator, Horizontal bridge","ALCUB- SOPORTE 630A 4P, D400, EMB. HORIZ.","AlCubar - ISOLATOR 630A 4P, D400, VÍZSZINTES HÍD"]
["20165","ALCUBAR 100R - ŁĄCZNIK CU 2500A, TYPU L, 175X100X10MM",245.3,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20165","SZT","74072900",null,null,"5901988201654","AlCubar 100R - Connecteur Cu 2500A, type L, 175x100x10mm","AlCubar 100R - Cu 2500A connector, L type, 175x100x10mm","ALCUB- 100R- CONECTOR CU 2500A, TIPO L, 175X100X10MM","ALCUBAR 100R - CU 2500A CSATLAKOZÓ, L-TÍPUS, 175X100X10MM"]
["20166","ZENERGY - MIEDZIANE PRZYŁĄCZE UZIEMIAJĄCE OCHRONNIKA, 40x40x5mm",13.5,null,null,null,null,null,null,"74072900",null,null,"5901988201661"]
["20167","ALCUBAR - ŁĄCZNIK CU 4000 A (2X2500A) H100-H100R, MOSTEK ŁĄCZĄCY przód (155X50X5MM)",59.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20167","SZT","74072900",null,null,"5901988201678","AlCu - Connecteur Cu 4000 A (2X2500A) H100-H100, de face (140X50X5MM)","AlCu - CONNECTOR CU 4000 A (2X2500A) H100-H100R, BRIDGE, CONNECTING FRONT (155X50X5mm)","ALCUB- CONECTOR Cu 4000 A (2X2500A) H100-H100R, FRONTAL","AlCubar - CU CONNECTOR 4000 A (2X2500A) H100-H100R, CSATLAKOZÓ HÍD elöl (155X50X5MM)"]
["20168","ALCUBAR - IZOLATOR 630A 3P, D400, DOIZOLOWANIE SZYN POZIOMYCH",133.30000000000001,"1-ZE-01",null,null,"OE_INSULATOR_D400","20168","SZT","85469010","27.90.12.0",null,"5901988201685","AlCu - Isolateur 630A 3P, P400, isolation des rails horizontaux","AlCu - 630A 3P, D400 insulator, insulation of Horizontal rails","ALCUB- SOPORTE 630A 3P, D400, REFUERZO EMB. HORIZ. ","AlCubar - SZIGETELŐ 630A 3P, D400, VÍZSZINTES RÚDAK SZIGETELÉSE"]
["20169","ALCUBAR - IZOLATOR 630A 4P, D400, DOIZOLOWANIE SZYN POZIOMYCH",175.8,"1-ZE-01",null,null,"OE_INSULATOR_D400","20169","SZT","85469010","27.90.12.0",null,"5901988201692","AlCu - Isolateur 630A 4P, P400, isolation des rails horizontaux","AlCu - 630A 4P, D400 insulator, insulation of Horizontal rails","ALCUB- SOPORTE 630A 4P, D400, REFUERZO EMB. HORIZ. ","AlCubar - SZIGETELŐ 630A 4P, D400, VÍZSZINTES RUDOK SZIGETELÉSE"]
["20170","ALCUBAR - IZOLATOR 630A 3P, W1000, MOST PIONOWY NA PLECACH",160.19999999999999,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20170","SZT","85469010","27.90.12.0",null,"5901988201708","AlCu - Isolateur 630A 3P, L1000, pont vertical à l'arrière","AlCu - 630A 3P insulator, W1000, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W1000, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W1000, FÜGGŐLEGES HÍD A HÁTÁN"]
["20171","ALCUBAR - IZOLATOR 630A 3P, W1200, MOST PIONOWY NA PLECACH",168,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20171","SZT","85469010","27.90.12.0",null,"5901988201715","AlCu - Isolateur 630A 3P, L1200, pont vertical à l'arrière","AlCu - 630A 3P insulator, W1200, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W1200, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W1200, FÜGGŐLEGES HÍD A HÁTSON"]
["20172","ALCUBAR - IZOLATOR 630A 3P, W1300, MOST PIONOWY NA PLECACH",173.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20172","SZT","85469010","27.90.12.0",null,"5901988201722","AlCu - Isolateur 630A 3P, L1300, pont vertical à l'arrière","AlCu - 630A 3P insulator, W1300, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W1300, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W1300, FÜGGŐLEGES HÍD A HÁTSON"]
["20174","ALCUBAR - IZOLATOR 630A 3P, W400, MOST PIONOWY NA PLECACH",133.30000000000001,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20174","SZT","85469010","27.90.12.0",null,"5901988201746","AlCu - Isolateur 630A 3P, L400, pont vertical à l'arrière","AlCu - 630A 3P insulator, W400, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W400, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W400, FÜGGŐLEGES HÍD A HÁLÁN"]
["20175","ALCUBAR - IZOLATOR 630A 3P, W450, MOST PIONOWY NA PLECACH",135.5,"1-ZE-01",0.05,2,"OE_INSULATOR_WIDTH","20175","SZT","85469010","27.90.12.0",null,"5901988201753","AlCu - Isolateur 630A 3P, L450, pont vertical à l'arrière","AlCu - 630A 3P insulator, W450, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W450, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W450, FÜGGŐLEGES HÍD A HÁLÁN"]
["20176","ALCUBAR - IZOLATOR 630A 3P, W600, MOST PIONOWY NA PLECACH",143.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20176","SZT","85469010","27.90.12.0",null,"5901988201760","AlCu - Isolateur 630A 3P, L600, pont vertical à l'arrière","AlCu - 630A 3P, W600 insulator, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W600, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W600, FÜGGŐLEGES HÍD A HÁLÁN"]
["20177","ALCUBAR - IZOLATOR 630A 3P, W650, MOST PIONOWY NA PLECACH",145.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20177","SZT","85469010","27.90.12.0",null,"5901988201777","AlCu - Isolateur 630A 3P, L650, pont vertical à l'arrière","AlCu - 630A 3P insulator, W650, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W650, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W650, FÜGGŐLEGES HÍD A HÁTSON"]
["20178","ALCUBAR - IZOLATOR 630A 3P, W800, MOST PIONOWY NA PLECACH",150.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20178","SZT","85469010","27.90.12.0",null,"5901988201784","AlCu - Isolateur 630A 3P, L800, pont vertical à l'arrière","AlCu - 630A 3P insulator, W800, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W800, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W800, FÜGGŐLEGES HÍD A HÁLÁN"]
["20179","ALCUBAR - IZOLATOR 630A 3P, W850, MOST PIONOWY NA PLECACH",155.69999999999999,"1-ZE-01",4.1666666666666664E-2,1,"OE_INSULATOR_WIDTH","20179","SZT","85469010","27.90.12.0",null,"5901988201791","AlCu - Isolateur 630A 3P, L850, pont vertical à l'arrière","AlCu - 630A 3P insulator, W850, Vertical bridge on the back","ALCUB- SOPORTE 630A 3P, W850, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 3P, W850, FÜGGŐLEGES HÍD A HÁLÁN"]
["20180","ALCUBAR - IZOLATOR 630A 4P, W1000, MOST PIONOWY NA PLECACH",206.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20180","SZT","85469010","27.90.12.0",null,"5901988201807","AlCu - Isolateur 630A 4P, L1000, pont vertical à l'arrière","AlCu - 630A 4P insulator, W1000, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W1000, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W1000, FÜGGŐLEGES HÍD PL-reECACH"]
["20181","ALCUBAR - IZOLATOR 630A 4P, W1200, MOST PIONOWY NA PLECACH",212.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20181","SZT","85469010","27.90.12.0",null,"5901988201814","AlCu - Isolateur 630A 4P, L1200, pont vertical à l'arrière","AlCu - 630A 4P insulator, W1200, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W1200, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W1200, FÜGGŐLEGES HÍD A HÁLÁN"]
["20182","ALCUBAR - IZOLATOR 630A 4P, W1300, MOST PIONOWY NA PLECACH",218.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20182","SZT","85469010","27.90.12.0",null,"5901988201821","AlCu - Isolateur 630A 4P, L1300, pont vertical à l'arrière","AlCu - 630A 4P insulator, W1300, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W1300, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W1300, FÜGGŐLEGES HÍD A HÁTSON"]
["20184","ALCUBAR - IZOLATOR 630A 4P, W400, MOST PIONOWY NA PLECACH",175.8,"1-ZE-01",0.19166666666666668,4,"OE_INSULATOR_WIDTH","20184","SZT","85469010","27.90.12.0",null,"5901988201845","AlCu - Isolateur 630A 4P, L400, pont vertical à l'arrière","AlCu - Insulator 630A 4P, W400, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W400, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W400, FÜGGŐLEGES HÍD A HÁLÁN"]
["20185","ALCUBAR - IZOLATOR 630A 4P, W450, MOST PIONOWY NA PLECACH",178.1,"1-ZE-01",3.3333333333333333E-2,1,"OE_INSULATOR_WIDTH","20185","SZT","85469010","27.90.12.0",null,"5901988201852","AlCu - Isolateur 630A 4P, L450, pont vertical à l'arrière","AlCu - 630A 4P, W450 insulator, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W450, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W450, FÜGGŐLEGES HÍD A HÁLÁN"]
["20186","ALCUBAR - IZOLATOR 630A 4P, W600, MOST PIONOWY NA PLECACH",183.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20186","SZT","85469010","27.90.12.0",null,"5901988201869","AlCu - Isolateur 630A 4P, L600, pont vertical à l'arrière","AlCu - 630A 4P, W600 insulator, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W600, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W600, FÜGGŐLEGES HÍD A HÁLÁN"]
["20187","ALCUBAR - IZOLATOR 630A 4P, W650, MOST PIONOWY NA PLECACH",188.2,"1-ZE-01",6.6666666666666666E-2,2,"OE_INSULATOR_WIDTH","20187","SZT","85469010","27.90.12.0",null,"5901988201876","AlCu - Isolateur 630A 4P, L650, pont vertical à l'arrière","AlCu - Insulator 630A 4P, W650, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W650, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W650, FÜGGŐLEGES HÍD A HÁLÁN"]
["20188","ALCUBAR - IZOLATOR 630A 4P, W800, MOST PIONOWY NA PLECACH",194.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20188","SZT","85469010","27.90.12.0",null,"5901988201883","AlCu - Isolateur 630A 4P, L800, pont vertical à l'arrière","AlCu - 630A 4P, W800 insulator, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W800, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W800, FÜGGŐLEGES HÍD A HÁTÁN"]
["20189","ALCUBAR - IZOLATOR 630A 4P, W850, MOST PIONOWY NA PLECACH",200.5,"1-ZE-01",0.10833333333333334,2,"OE_INSULATOR_WIDTH","20189","SZT","85469010","27.90.12.0",null,"5901988201890","AlCu - Isolateur 630A 4P, L850, pont vertical à l'arrière","AlCu - Insulator 630A 4P, W850, Vertical bridge on the back","ALCUB- SOPORTE 630A 4P, W850, EMB. VERT. FONDO","AlCubar - SZIGETELŐ 630A 4P, W850, FÜGGŐLEGES HÍD A HÁLÁN"]
["20190","produkt wycofany (ALCUBAR - IZOLATOR 630A 3P, MOST POZIOMY NA PLECACH LUB PŁYCIE MONTAŻOWEJ, ROZSTAW 61MM)",124.3,"1-ZE-08",4.1666666666666664E-2,1,"OE_INSULATOR_WIDTH","20190","SZT","85469010","27.90.20.0",null,"5901988201906","AlCu - Isolateur 630A 3P, pont horizontal à l'arrière ou plaque de montage","AlCu - 630A 3P insulator, Horizontal bridge on the back or Mounting plate, 61mm spacing","ALCUB- 630A SOPORTE 3P, EMB. HORIZ. EN LA PARTE POSTERIOR","kivont termék (AlCubar - ISOLATOR 630A 3P, VÍZSZINTES HÍD A HÁTRA VAGY SZERELŐLAP, HELY 61MM)"]
["20191","ALCUBAR - WPUST PRZESUWNY M5 DO ROWKA 5MM + ŚRUBA M5X16 + PODKŁADKI, NAKRĘTKI, KPL.10SZT",154.6,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988201913","AlCu - clé coulissante M5 pour rainure de 5mm + vis M5x16 + rondelles, écrous, jeu de 10 pièces","AlCu - M5 slot nut for 5mm groove + M5x16 screw + washers, nuts, set of 10","ALCUB- TUERCA DESLIZ. M5 PARA RANURA 5MM + TORNILLO M5X16 10UDS","AlCubar - M5 CSÚSZTÓ KENNEL 5 MM-ES VONÁZHOZ + M5X16 CSAVAR + ALÁTÉTEK, ANYÁK, SZETT 10 DB"]
["20192","ALCUBAR - WPUST PRZESUWNY M5 DO ROWKA 8MM + ŚRUBA M5X16 + PODKŁADKI, NAKRĘTKI, KPL.10SZT",115.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988201920","AlCu - clé coulissante M5 pour rainure de 8 mm + vis M5x16 + rondelles, écrous, jeu de 10 pièces","AlCu - M5 slot key for 8mm groove + M5x16 screw + washers, nuts, set of 10","ALCUB- TUERCA DESLIZ. M5 PARA RANURA 8MM + TORNILLO M5X16 10UDS","AlCubar - M5 CSÚSZTÓ KENNEL 8 MM-ES VONÁZHOZ + M5X16 CSAVAR + ALÁTÉTEK, ANYÁK, 10 DB-OS KÉSZLET"]
["20193","ALCUBAR - WPUST PRZESUWNY M6 DO ROWKA 8MM + ŚRUBA M6X16 + PODKŁADKI, NAKRĘTKI, KPL.10SZT",115.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988201937","AlCu - rainure de clavette coulissante M6 pour rainure de 8mm + vis M6x16 + rondelles, écrous, jeu de 10pcs","AlCu - M6 slot key for 8mm groove + M6x16 screw + washers, nuts, set of 10","ALCUB- TUERCA DESLIZ. M6 PARA RANURA 8MM + TORNILLO M6X16 10UDS","AlCubar - M6 CSÚSZTÓ KENNEL 8 MM-ES VONÁZHOZ + M6X16 CSAVAR + ALÁTÉTEK, ANYÁK, 10 DB-OS KÉSZLET"]
["20194","ALCUBAR - WPUST PRZESUWNY M8 DO ROWKA 8MM + ŚRUBA M8X25 + PODKŁADKI, NAKRĘTKI, KPL.10SZT",115.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988201944","AlCu - clé coulissante M8 pour rainure de 8 mm + vis M8x25 + rondelles, écrous, jeu de 10 pièces","AlCu - M8 slot nut for 8mm groove + M8x25 screw + washers, nuts, set of 10","ALCUB- TUERCA DESLIZ. M8 PARA RANURA 8MM + TORNILLO M8X25 10UDS","AlCubar - M8 CSÚSZTÓ KENNEL 8 MM-ES VONÁZHOZ + M8X25 CSAVAR + ALÁTÉTEK, ANYÁK, SZETT 10 DB"]
["20195","ALCUBAR - WPUST PRZESUWNY M8 DO ROWKA 10MM + ŚRUBA M8X30 + PODKŁADKI, NAKRĘTKI, KPL.10SZT",221.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988201951","AlCu - clé coulissante M8 pour rainure de 10 mm + vis M8x30 + rondelles, écrous, jeu de 10 pièces","AlCu - M8 slot for a 10mm groove + M8x30 screw + washers, nuts, set of 10","ALCUB- TUERCA DESLIZ. M8 PARA RANURA 10MM + TORNILLO M8X30 10UDS","AlCubar - M8 CSÚSZTÓ KENNEL 10 MM-ES VONÁZHOZ + M8X30 CSAVAR + ALÁTÉTEK, ANYÁK, 10 DB-OS KÉSZLET"]
["20196","ALCUBAR - WPUST PRZESUWNY M10 DO ROWKA 10MM + ŚRUBA M10X30 + PODKŁADKI, NAKRĘTKI, KPL.10SZT",221.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"KPL","73181595","25.94.11.0",null,"5901988201968","AlCu - clé coulissante M10 pour rainure de 10 mm + vis M10x30 + rondelles, écrous, lot de 10 pièces","AlCu - M10 slot key for 10mm groove + M10x30 screw + washers, nuts, set of 10","ALCUB- TUERCA DESLIZ. M10 PARA RANURA 10MM + TORNILLO M10X30 10UDS","AlCubar - M10 CSÚSZTÓ KENNEL 10 MM-ES VONÁZHOZ + M10X30 CSAVAR + ALÁTÉTEK, ANYÁK, 10 DB-OS KÉSZLET"]
["20197","ALCUBAR - IZOLATOR 630A 4P, MOST POZIOMY NA PLECACH LUB PŁYCIE MONTAŻOWEJ, ROZSTAW 50MM",164.6,"1-ZE-08",9.166666666666666E-2,4,"OE_INSULATOR_WIDTH","20197","SZT","85469010","27.90.12.0",null,"5901988201975","AlCu - Isolateur 630A 4P, pont horizontal à l'arrière ou plaque de montage","AlCu - 630A 4P insulator, Horizontal bridge on the back or Mounting plate, 50mm spacing","ALCUB- 630A SOPORTE 4P, EMB. HORIZ. EN LA PARTE TRASERA ","AlCubar - SZIGETELŐ 630A 4P, VÍZSZINTES HÍD A HÁTRA VAGY SZERELŐLEMEZ, HELY 50MM"]
["20198","ALCUBAR - IZOLATOR 630A 3P, MOST POZIOMY NA PLECACH LUB PŁYCIE MONTAŻOWEJ, ROZSTAW 75MM",124.3,"1-ZE-08",0.35833333333333334,2,"OE_INSULATOR_WIDTH","20198","SZT","85469010","27.90.12.0",null,"5901988201982","AlCu - Isolateur 630A 3P, pont horizontal à l'arrière ou plaque de montage","AlCu - 630A 3P insulator, Horizontal bridge on the back or Mounting plate, 75mm spacing","ALCUB- SOPORTE 630A 3P, EMB. HORIZ. FONDO O PLACA MONTAJE","AlCubar - SZIGETELŐ 630A 3P, VÍZSZINTES HÍD A HÁTRA VAGY SZERELŐLEMEZ, HELY 75MM"]
["20199","ALCUBAR - IZOLATOR 630A 4P, MOST POZIOMY NA PLECACH LUB PŁYCIE MONTAŻOWEJ, ROZSTAW 61MM",164.6,"1-ZE-08",4.95,7,"OE_INSULATOR_WIDTH","20199","SZT","85469010",null,null,"5901988201999","AlCu - Isolateur 630A 4P, pont horizontal à l'arrière ou plaque de montage","AlCu - Insulator 630A 4P, Horizontal bridge on the back or Mounting plate, spacing 61mm","ALCUB- SOPORTE 630A 4P, EMB. HORIZ. FONDO O PLACA MONTAJE","AlCubar - SZIGETELŐ 630A 4P, VÍZSZINTES HÍD A HÁTRA VAGY SZERELŐLEMEZ, HELY 61MM"]
["20200","ALCUBAR / CU - IZOLATOR 3P, W1000, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",319.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202002","AlCu/Cu - Isolateur 3P, L1000, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W1000, Horizontally, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W1000, VERT. FONDO","ALCUBAR / CU - 3P SZIGETELŐ, W1000, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20201","ALCUBAR / CU - IZOLATOR 3P, W1200, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",329.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988202019","AlCu/Cu - Isolateur 3P, L1200, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W1200, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W1200, VERT. FONDO","AlCubar / CU - 3P SZIGETELŐ, W1200, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20202","ALCUBAR / CU - IZOLATOR 3P, W1300, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",339.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202026","AlCu/Cu - Isolateur 3P, L1300, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W1300, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W1300, VERT. FONDO","ALCUBAR / CU - 3P SZIGETELŐ, W1300, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20206","ALCUBAR / CU - IZOLATOR 3P, W600, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",282.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202064","AlCu/Cu - Isolateur 3P, L600, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W600, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W600, VERT. FONDO","ALCUBAR / CU - 3P SZIGETELŐ, W600, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20207","ALCUBAR / CU - IZOLATOR 3P, W650, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",287.8,"1-ZE-01",0.01,1,"OE_INSULATOR_WIDTH","20207","SZT","85469010","27.90.12.0",null,"5901988202071","AlCu/Cu - Isolateur 3P, L650, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W650, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W650, VERT. FONDO","ALCUBAR / CU - 3P SZIGETELŐ, W650, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20208","ALCUBAR / CU - IZOLATOR 3P, W800, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",302.39999999999998,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202088","AlCu/Cu - Isolateur 3P, L800, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W800, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W800, VERT. FONDO","AlCubar / CU - 3P SZIGETELŐ, W800, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20209","ALCUBAR / CU - IZOLATOR 3P, W850, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",310.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20209","SZT","85469010","27.90.12.0",null,"5901988202095","AlCu/Cu - Isolateur 3P, L850, verticalement à l'arrière","AlCu/Cu - Insulator 3P, W850, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W850, VERT. FONDO","AlCubar / CU - 3P SZIGETELŐ, W850, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20210","ALCUBAR / CU - IZOLATOR 4P, W1000, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",392,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20210","SZT","85469010","27.90.12.0",null,"5901988202101","AlCu/Cu - Isolateur 4P, L1000, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W1000, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1000, VERT. FONDO","AlCubar / CU - SZIGETELŐ 4P, W1000, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20211","ALCUBAR / CU - IZOLATOR 4P, W1200, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",402.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20211","SZT","85469010","27.90.12.0",null,"5901988202118","AlCu/Cu - Isolateur 4P, L1200, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W1200, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1200, VERT. FONDO","AlCubar / CU - SZIGETELŐ 4P, W1200, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20212","ALCUBAR / CU - IZOLATOR 4P, W1300, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",412.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202125","AlCu/Cu - Isolateur 4P, L1300, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W1300, Horizontally, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1300, VERT. FONDO","AlCubar / CU - SZIGETELŐ 4P, W1300, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20216","ALCUBAR / CU - IZOLATOR 4P, W600, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",351.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202163","AlCu/Cu - Isolateur 4P, L600, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W600, Horizontally, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W600, VERT. FONDO","AlCubar / CU - SZIGETELŐ 4P, W600, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20217","ALCUBAR / CU - IZOLATOR 4P, W650, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",357.3,"1-ZE-01",1.6666666666666666E-2,1,"OE_INSULATOR_WIDTH","20217","SZT","85469010","27.90.12.0",null,"5901988202170","AlCu/Cu - Isolateur 4P, L650, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W650, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W650, VERT. FONDO","ALCUBAR / CU - SZIGETELŐ 4P, W650, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20218","ALCUBAR / CU - IZOLATOR 4P, W800, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",373,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202187","AlCu/Cu - Isolateur 4P, L800, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W800, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W800, VERT. FONDO","AlCubar / CU - SZIGETELŐ 4P, W800, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20219","ALCUBAR / CU - IZOLATOR 4P, W850, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",383,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20219","SZT","85469010","27.90.12.0",null,"5901988202194","AlCu/Cu - Isolateur 4P, L850, verticalement à l'arrière","AlCu/Cu - Insulator 4P, W850, Horizontal, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W850, VERT. FONDO","AlCubar / CU - SZIGETELŐ 4P, W850, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20220","ALCUBAR / CU - IZOLATOR 2x3P, W1000, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",406.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20220","SZT","85469010",null,null,"5901988202200","AlCu/Cu - Isolateur 2x3P, L1000, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 2x3P, W1000, Vertically, adjustable depth, spacing 130mm","ALCUB / CU- SOPORTE 3P, W1000, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 2x3P, W1000, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20221","ALCUBAR / CU - IZOLATOR 3P+N, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, Rozstaw 230mm + N 240mm",370.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20221","SZT","85469010","27.90.12.0",null,"5901988202217","Cu 6300A - Isolateur 3P+N, L1200, verticalement à l'arrière, profondeur réglable, espacement 230mm + N 240mm","Cu 6300A - Insulator 3P + N, W1200, Vertical, adjustable depth, spacing 230mm + N 240mm","ALCUB / CU- SOPORTE 3P, W1200, VERT. FONDO, REGUL. PROF.","ALCUBAR / CU - SZIGETELŐ 3P+N, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, Távolság 230mm + N 240mm"]
["20222","ALCUBAR / CU - IZOLATOR 3P, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",380.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20222","SZT","85469010",null,null,"5901988202224","AlCubar 6300A - Isolateur 3P+N, L1200, verticalement à l'arrière, profondeur réglable, espacement 230mm + N 240mm","AlCubar 6300A - Insulator 3P + N, W1200, Vertically, adjustable depth, spacing 230mm + N 240mm","ALCUB / CU- SOPORTE 3P, W1300, VERT. FONDO, REGUL. PROF.","ALCUBAR / CU - 3P SZIGETELŐ, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20225","ALCUBAR / CU - IZOLATOR 3P, W450, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",323.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202255","AlCu/Cu - ISOLANT 3P, L450, VERTICAL, RÉGLABLE EN PROFONDEUR, ESPACEMENT 115-125-115MM","AlCu/Cu - 3P INSULATOR, W450, Vertical, DEPTH ADJUSTABLE, SPACING 115-125-115mm","*AlCu/Cu - AISLADOR 3P, W450, VERTICAL, REGULABLE EN PROFUNDIDAD, ESPACIO 115-125-115MM","AlCubar / CU - 3P SZIGETELŐ, W450, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20226","ALCUBAR / CU - IZOLATOR 3P, W600, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",328.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202262","AlCu/Cu - Isolateur 3P, L600, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 3P, W600, Vertically, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W600, VERT. FONDO, REGUL. PROF.","ALCUBAR / CU - 3P SZIGETELŐ, W600, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20227","ALCUBAR / CU - IZOLATOR 3P, W650, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",333.8,"1-ZE-01",4.1666666666666664E-2,1,"OE_INSULATOR_WIDTH","20227","SZT","85469010","27.90.12.0",null,"5901988202279","AlCu/Cu - Isolateur 3P, L650, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 3P, W650, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W650, VERT. FONDO, REGUL. PROF.","ALCUBAR / CU - 3P SZIGETELŐ, W650, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20228","ALCUBAR / CU - IZOLATOR 3P, W800, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",342.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202286","AlCu/Cu - Isolateur 3P, L800, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 3P, W800, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W800, VERT. FONDO, REGUL. PROF.","ALCUBAR / CU - 3P SZIGETELŐ, W800, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20229","ALCUBAR / CU - IZOLATOR 3P, W850, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",351.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20229","SZT","85469010","27.90.12.0",null,"5901988202293","AlCu/Cu - Isolateur 3P, L850, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 3P, W850, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W850, VERT. FONDO, REGUL. PROF.","ALCUBAR / CU - 3P SZIGETELŐ, W850, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20230","ALCUBAR / CU - IZOLATOR 4P, W1000, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",431.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20230","SZT","85469010","27.90.12.0",null,"5901988202309","AlCu/Cu - Isolateur 4P, L1000, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W1000, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1000, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W1000, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20231","ALCUBAR / CU - IZOLATOR 4P, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",441.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202316","AlCu/Cu - Isolateur 4P, L1200, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W1200, Vertically, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1200, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20232","ALCUBAR / CU - IZOLATOR 4P, W1300, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",451.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202323","AlCu/Cu - Isolateur 4P, L1300, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W1300, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1300, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W1300, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20236","ALCUBAR / CU - IZOLATOR 4P, W600, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",398.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202361","AlCu/Cu - Isolateur 4P, L600, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W600, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W600, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W600, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20237","ALCUBAR / CU - IZOLATOR 4P, W650, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",402.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20237","SZT","8546901000","27.90.12.0",null,"5901988202378","AlCu/Cu - Isolateur 4P, L650, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W650, Vertical, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W650, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W650, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20238","ALCUBAR / CU - IZOLATOR 4P, W800, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",414.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202385","AlCu/Cu - Isolateur 4P, L800, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W800, Vertically, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W800, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W800, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20239","ALCUBAR / CU - IZOLATOR 4P, W850, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 115-125-115MM",422.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20239","SZT","85469010","27.90.12.0",null,"5901988202392","AlCu/Cu - Isolateur 4P, L850, verticalement à l'arrière, profondeur réglable","AlCu/Cu - Insulator 4P, W850, Vertically, adjustable depth, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W850, VERT. FONDO, REGUL. PROF.","AlCubar / CU - SZIGETELŐ 4P, W850, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 115-125-115MM"]
["20240","ALCUBAR / CU - IZOLATOR 3P, W1000, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",360.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20240","SZT","85469010","27.90.12.0",null,"5901988202408","AlCu/Cu - Isolateur 3P, L1000, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W1000, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W1000, FONDO, REGUL. ALTURA","AlCubar / CU - 3P SZIGETELŐ, W1000, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 115-125-115MM TÉR"]
["20241","ALCUBAR / CU - IZOLATOR 3P, W1200, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",370.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202415","AlCu/Cu - Isolateur 3P, L1200, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W1200, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W1200, FONDO, REGUL. ALTURA","AlCubar / CU - 3P SZIGETELŐ, W1200, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 115-125-115MM"]
["20242","ALCUBAR / CU - IZOLATOR 3P, W1300, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",380.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202422","AlCu/Cu - Isolateur 3P, L1300, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W1300, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W1300, FONDO, REGUL. ALTURA","AlCubar / CU - 3P SZIGETELŐ, W1300, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 115-125-115MM TÉR"]
["20246","ALCUBAR / CU - IZOLATOR 3P, W600, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",328.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202460","AlCu/Cu - Isolateur 3P, L600, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W600, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W600, FONDO, REGUL. ALTURA","ALCUBAR / CU - 3P SZIGETELŐ, W600, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 115-125-115MM HELY."]
["20247","ALCUBAR / CU - IZOLATOR 3P, W650, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",333.8,"1-ZE-01",0.01,1,"OE_INSULATOR_WIDTH","20247","SZT","85469010","27.90.12.0",null,"5901988202477","AlCu/Cu - Isolateur 3P, L650, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W650, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W650, FONDO, REGUL. ALTURA","AlCubar / CU - 3P SZIGETELŐ, W650, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 115-125-115MM"]
["20248","ALCUBAR / CU - IZOLATOR 3P, W800, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",342.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202484","AlCu/Cu - Isolateur 3P, L800, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W800, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W800, FONDO, REGUL. ALTURA","AlCubar / CU - 3P SZIGETELŐ, W800, TÁMASZTÁS/FÜGGŐLEGES A HÁTSON, ÁLLÍTHATÓ MAGASSÁG, HELYSZÍR 115-125-115MM"]
["20249","ALCUBAR / CU - IZOLATOR 3P, W850, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",351.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20249","SZT","85469010","27.90.12.0",null,"5901988202491","AlCu/Cu - Isolateur 3P, L850, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 3P, W850, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 3P, W850, FONDO, REGUL. ALTURA","AlCubar / CU - 3P SZIGETELŐ, W850, TÁMASZTÁS/FÜGGŐLEGES HÁTÁN, ÁLLÍTHATÓ MAGASSÁG, 115-125-115MM HELY."]
["20250","ALCUBAR / CU - IZOLATOR 4P, W1000, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",431.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202507","AlCu/Cu - Isolateur 4P, L1000, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W1000, support / Vertical on the back, adjustable height, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1000, FONDO, REGUL. ALTURA","ALCUBAR / CU - 4P SZIGETELŐ, W1000, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 115-125-115MM HELY."]
["20251","ALCUBAR / CU - IZOLATOR 4P, W1200, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",441.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202514","AlCu/Cu - Isolateur 4P, L1200, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W1200, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1200, FONDO, REGUL. ALTURA","AlCubar / CU - 4P SZIGETELŐ, W1200, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 115-125-115MM"]
["20252","ALCUBAR / CU - IZOLATOR 4P, W1300, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",451.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202521","AlCu/Cu - Isolateur 4P, L1300, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W1300, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W1300, FONDO, REGUL. ALTURA","AlCubar / CU - 4P SZIGETELŐ, W1300, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELYSZÁM 115-125-115MM"]
["20256","ALCUBAR / CU - IZOLATOR 4P, W600, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",398.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202569","AlCu/Cu - Isolateur 4P, L600, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W600, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W600, FONDO, REGUL. ALTURA","AlCubar / CU - IZOLATOR 4P, W600, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 115-125-115MM"]
["20257","ALCUBAR / CU - IZOLATOR 4P, W650, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",402.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20257","SZT","85469010","27.90.12.0",null,"5901988202576","AlCu/Cu - Isolateur 4P, L650, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W650, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W650, FONDO, REGUL. ALTURA","AlCubar / CU - 4P SZIGETELŐ, W650, TÁMASZTÁS/FÜGGŐLEGES HÁTÁN, ÁLLÍTHATÓ MAGASSÁG, HELY 115-125-115MM"]
["20258","ALCUBAR / CU - IZOLATOR 4P, W800, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",414.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202583","AlCu/Cu - Isolateur 4P, L800, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W800, support / Vertical on the back, height adjustable, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W800, FONDO, REGUL. ALTURA","AlCubar / CU - 4P SZIGETELŐ, W800, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELYSZÍR 115-125-115MM"]
["20259","ALCUBAR / CU - IZOLATOR 4P, W850, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 115-125-115MM",422.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20259","SZT","85469010","27.90.12.0",null,"5901988202590","AlCu/Cu - Isolateur 4P, L850, appui à l'arrière, hauteur réglable","AlCu/Cu - Insulator 4P, W850, support / Vertical on the back, adjustable height, spacing 115-125-115mm","ALCUB / CU- SOPORTE 4P, W850, FONDO, REGUL. ALTURA","AlCubar / CU - 4P SZIGETELŐ, W850, TÁMASZTÁS/FÜGGŐLEGES HÁTÁN, ÁLLÍTHATÓ MAGASSÁG, 115-125-115MM HELY."]
["20261","AlCubar / Cu - Płyta montażowa / izolator 1P dla AlCubar H50R, most na płycie montażowej",216.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20261","SZT","85469010","27.90.12.0",null,"5901988202613","AlCu/Cu - Plaque de montage / Isolateur 1P pour AlCubar H50R, pont sur plaque de montage","AlCu/Cu - Mounting plate / 1P insulator for AlCubar H50R, bridge on Mounting plate","*AlCu/Cu - Placa de montaje / Aislante 1P para AlCubar H50R, puente sobre placa de montaje","AlCubar / Cu - Szerelőlap / 1P szigetelő AlCubar H50R-hez, híd a szerelőlapon"]
["20264","AlCubar / Cu - Płyta montażowa / izolator 4P dla AlCubar H50R, most na płycie montażowej",666.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202644","AlCu/Cu - Plaque de montage / Isolateur 4P pour AlCubar H50R, pont sur plaque de montage","AlCu/Cu - Mounting plate / 4P insulator for AlCubar H50R, bridge on Mounting plate","*AlCu/Cu - Placa de montaje / Aislante 4P para AlCubar H50R, puente sobre placa de montaje","AlCubar / Cu - Szerelőlap / 4P szigetelő AlCubar H50R-hez, híd a szerelőlapon"]
["20267","ALCUBAR / CU - IZOLATOR SZYNOPRZEWODU 3P+PEN, ROZSTAW 105MM",268.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988202675","AlCu/Cu - Isolateur 3200-4000A 3P, L650, commutateur - pont, complet","AlCu/Cu - 3P + PEN busbar insulator, 105mm spacing","ALCUB / CU- SOPORTE 3200-4000A 3P, W650, INTERRUPTOR - EMB.","AlCubar / CU - BUSZSZIGETELŐ 3P+TOLL, HELY 105MM"]
["20269","ALCUBAR / CU - IZOLATOR SZYNOPRZEWODU 4P, ROZSTAW 105MM",336,"1-ZE-01",0.49166666666666664,4,"OE_INSULATOR_WIDTH","20269","SZT","85469010","27.90.12.0",null,"5901988202699","AlCu/Cu - Isolateur 3200-4000A 3P, L850, commutateur - pont, complet","AlCu/Cu - 4P busbar insulator, 105mm spacing","ALCUB / CU- SOPORTE 3200-4000A 3P, W850, INTERRUPTOR - EMB.","AlCubar / CU - BUSZSZIGETELŐ 4P, HELY 105MM"]
["20270","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 1P, D200, MOST POZIOMY",75.400000000000006,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202705","AlCu/Cu - Support d'isolateur + élément supérieur 1P, P200, pont horizontal","AlCu/Cu - Insulator support + 1P top piece, D200, Horizontal bridge","ALCUB / CU-SOPORTE + PARTE SUPERIOR 1P, D200, EMB. HORIZ.","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 1P, D200, VÍZSZINTES HÍD"]
["20271","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 1P, D400, MOST POZIOMY",162.4,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202712","AlCu/Cu - Support isolant + élément supérieur 1P, P400, pont horizontal","AlCu/Cu - Insulator support + 1P top piece, D400, Horizontal bridge","ALCUB / CU-SOPORTE + PARTE SUPERIOR 1P, D400, EMB. HORIZ.","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 1P, D400, VÍZSZINTES HÍD"]
["20272","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 3P, D400, MOST POZIOMY",183.7,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202729","AlCu/Cu - Support isolant + élément supérieur 3P, P400, pont horizontal","AlCu/Cu - Insulator support + 3P top piece, D400, Horizontal bridge","ALCUB / CU-SOPORTE + PARTE SUPERIOR 3P, D400, EMB. HORIZ.","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 3P, D400, VÍZSZINTES HÍD"]
["20273","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 4P, D400, MOST POZIOMY",220.6,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202736","AlCu/Cu - Support isolant + élément supérieur 4P, P400, pont horizontal","AlCu/Cu - Insulator support + top piece 4P, D400, Horizontal bridge","ALCUB / CU-SOPORTE + PARTE SUPERIOR 4P, D400, EMB. HORIZ.","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 4P, D400, VÍZSZINTES HÍD"]
["20280","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 1P, D200, MOST PIONOWY Z BOKU",75.400000000000006,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202804","AlCu/Cu - Support isolant + élément supérieur 1P, P200, pont vertical sur le côté","AlCu/Cu - Insulator support + 1P top piece, D200, Vertical bridge on the side","ALCUB / CU-SOPORTE + PARTE SUPERIOR 1P, D200, EMB. VERT. LATERAL","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 1P, D200, OLDALSÓ FÜGGŐLEGES HÍD"]
["20281","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 1P, D400, MOST PIONOWY Z BOKU",162.4,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202811","AlCu/Cu - Support isolant + élément supérieur 1P, P400, pont vertical sur le côté","AlCu/Cu - Insulator support + 1P top piece, D400, Vertical bridge on the side","ALCUB / CU-SOPORTE + PARTE SUPERIOR 1P, D400, EMB. VERT. LATERAL","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 1P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20282","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 3P, D400, MOST PIONOWY Z BOKU",183.7,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202828","AlCu/Cu - Support isolant + élément supérieur 3P, P400, pont vertical sur le côté","AlCu/Cu - Insulator support + 3P top piece, D400, Vertical bridge on the side","ALCUB / CU-SOPORTE + PARTE SUPERIOR 3P, D400, EMB. VERT. LATERAL","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 3P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20283","ALCUBAR / CU - WSPORNIK IZOLATORA + ELEMENT GÓRNY 4P, D400, MOST PIONOWY Z BOKU",220.6,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010","27.90.12.0",null,"5901988202835","AlCu/Cu - Support isolant + élément supérieur 4P, P400, pont vertical sur le côté","AlCu/Cu - Insulator support + top piece 4P, D400, Vertical bridge on the side","ALCUB / CU-SOPORTE + PARTE SUPERIOR 4P, D400, EMB. VERT. LATERAL","AlCubar / CU - SZIGETELŐ KONZER + FELSŐ ELEM 4P, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["20292","AlCubar - Śruba zamkowa M8x50 dla AlCubar 1000A+, kl 8.8, + podkładki, nakrętki,  kpl.100szt, wsuwane od końca profila",231.1,null,0.1,2,"OE_BUSBARS_ALCUBAR",null,null,"73181595",null,null,"5901988202927"]
["20293","AlCubar - Śruba zamkowa M12x54 dla AlCubar 1000A+, kl 8.8, + podkładki, nakrętki,  kpl.100szt, wsuwane od końca profila",453.6,null,1.6666666666666666E-2,2,"OE_BUSBARS_ALCUBAR",null,null,"73181595",null,null,"5901988202934"]
["20296","ALCUBAR - ŚRUBY PRZESUWNE 2X M8X27 DLA ALCUBAR R I ROZŁĄCZNIKA LISTWOWEGO NH-00+ PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",200.5,"1-ZE-08",0.23333333333333334,4,"OE_BUSBARS_ALCUBAR","20296","SZT","73181595","27.90.51.0",null,"5901988202965","AlCu - Vis coulissantes 2x M8x27 pour interrupteur-sectionneur à lamelles AlCubar R et NH-00 + rondelles, écrous, jeu de 10 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 2x M8x27 for AlCubar R and NH-00 rail switch disconnector + washers, nuts, set of 10, inserted from the end of the profile","ALCUB- TORNILLOS DESLIZANTES 2X M8X27 ","AlCubar - CSÚSZTÓ CSAVAROK 2X M8X27 AlCubar R-HOZ ÉS NH-00+ CSATLAKOZÓHOZ ALÁTÉTÉK, ANYA, 10 DÉS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20297","ALCUBAR - ŚRUBY PRZESUWNE 2X M8X27 DLA ALCUBAR H50R+ PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",200.5,"1-ZE-08",0.23333333333333334,4,"OE_BUSBARS_ALCUBAR","20297","SZT","73181595","25.94.11.0",null,"5901988202972","AlCu - Vis coulissantes 2x M8x27 pour AlCubar H50R + rondelles, écrous, jeu de 10 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 2x M8x27 for AlCubar H50R + washers, nuts, set of 10, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. 2X M8X27 PARA ALCUB- H50R+ 10UDS","ALCUBAR - 2X M8X27 CSÚSZTÓ CSAVAR ALCUBA H50R+ ALÁTÉTHOZ, ANYA, 10 DÉS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20298","ALCUBAR - ŚRUBY PRZESUWNE 4X M8X27 DLA ALCUBAR R I ROZŁĄCZNIKA LISTWOWEGO NH-00+ PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",401,"1-ZE-08",0.10833333333333334,4,"OE_BUSBARS_ALCUBAR","20298","SZT","73181595","25.94.11.0",null,"5901988202989","AlCu - Vis coulissantes 4x M8x27 pour interrupteur-sectionneur à lamelles AlCubar R et NH-00 + rondelles, écrous, jeu de 10 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 4x M8x27 for AlCubar R and NH-00 rail switch disconnector + washers, nuts, set of 10 pieces, inserted from the end of the profile","ALCUB- TORNILLOS DESLIZANTES 4X M8X27 ","AlCubar - CSÚSZTÓ CSAVAROK 4X M8X27 ALCUBAR R-HOZ ÉS NH-00+ CSATLAKOZÓHOZ ALÁTÉTEK, ANYÁK, 10-ES KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20299","ALCUBAR - ŚRUBY PRZESUWNE 4X M8X27 DLA ALCUBAR H100R+ PODKŁADKI, NAKRĘTKI, KPL.10SZT, WSUWANE OD KOŃCA PROFILA",401,"1-ZE-08",0.10833333333333334,2,"OE_BUSBARS_ALCUBAR","20299","SZT","73181595","25.94.11.0",null,"5901988202996","AlCu - Vis coulissantes 4x M8x27 pour AlCubar H100R + rondelles, écrous, jeu de 10 pièces, insérées à partir de l'extrémité du profilé","AlCu - Sliding screws 4x M8x27 for AlCubar H100R + washers, nuts, set of 10, inserted from the end of the profile","ALCUB- TORNILLO DESLIZ. 4X M8X27 PARA ALCUB- H100R+ 10UDS","AlCubar - CSÚSZTÓ CSAVAROK 4X M8X27 ALKUBAR H100R+ ALÁTÉTEKHEZ, ANYA, 10 DB-OS KÉSZLET, A PROFIL VÉGÉRŐL BEHELYEZVE"]
["20303","ZENERGY - WSPORNIK PŁYTY MONTAŻOWEJ / IZOLATORÓW 3P, D600 WZMOCNIONY",93,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988203030","OE - Plaque de montage / support isolant 3P, P600 renforcé","OE - Bracket for Mounting plate / insulators 3P, D600 reinforced","OE- Soporte para PLACA MONTAJE / aisladores 3P, D600 reforzado","ZENERGY - SZERELŐLEMEZ TÁMASZTÁSA / 3P SZIGETELŐK, D600 MEGERŐSÍTETT"]
["20304","ZENERGY - WSPORNIK PŁYTY MONTAŻOWEJ / IZOLATORÓW 4P, D600 WZMOCNIONY",93,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988203047","OE - Support de plaque de montage / Isolateur 4P, P600 renforcé","OE - Bracket Mounting plate / insulators 4P, D600 reinforced","OE- Soporte para PLACA MONTAJE / aisladores 4P, D600 reforzado","ZENERGY - SZERELŐLEMEZ / 4P SZIGETELŐ TÁMASZTÁS, D600 MEGERŐSÍTETT"]
["20310","ALCUBAR / CU - IZOLATOR 1P, W1000, MOST PIONOWY NA PLECACH",220.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20310","SZT","85469010",null,null,"5901988203108","AlCu/Cu - Isolateur 1P, L1000, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W1000, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W1000, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W1000, FÜGGŐLEGES HÍD A HÁTSON"]
["20311","ALCUBAR / CU - IZOLATOR 1P, W1200, MOST PIONOWY NA PLECACH",225.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20311","SZT","85469010",null,null,"5901988203115","AlCu/Cu - Isolateur 1P, L1200, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W1200, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W1200, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W1200, FÜGGŐLEGES HÍD A HÁTSON"]
["20312","ALCUBAR / CU - IZOLATOR 1P, W1300, MOST PIONOWY NA PLECACH",228.5,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20312","SZT","85469010",null,null,"5901988203122","AlCu/Cu - Isolateur 1P, L1300, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W1300, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W1300, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W1300, FÜGGŐLEGES HÍD A HÁTSON"]
["20313","ALCUBAR / CU - IZOLATOR 1P, W300, MOST PIONOWY NA PLECACH",190.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20313","SZT","85469010",null,null,"5901988203139","AlCu/Cu - Isolateur 1P, L300, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W300, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W300, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W300, FÜGGŐLEGES HÍD A HÁTSON"]
["20314","ALCUBAR / CU - IZOLATOR 1P, W400, MOST PIONOWY NA PLECACH",193.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20314","SZT","85469010",null,null,"5901988203146","AlCu/Cu - Isolateur 1P, L400, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W400, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W400, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W400, FÜGGŐLEGES HÍD A HÁTSON"]
["20315","ALCUBAR / CU - IZOLATOR 1P, W450, MOST PIONOWY NA PLECACH",197.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20315","SZT","85469010",null,null,"5901988203153","AlCu/Cu - Isolateur 1P, L450, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W450, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W450, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W450, FÜGGŐLEGES HÍD A HÁTSON"]
["20316","ALCUBAR / CU - IZOLATOR 1P, W600, MOST PIONOWY NA PLECACH",201.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20316","SZT","85469010",null,null,"5901988203160","AlCu/Cu - Isolateur 1P, L600, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W600, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W600, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W600, FÜGGŐLEGES HÍD A HÁTSON"]
["20317","ALCUBAR / CU - IZOLATOR 1P, W650, MOST PIONOWY NA PLECACH",207.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20317","SZT","85389099","27.12.40.0",null,"5901988203177","AlCu/Cu - Isolateur 1P, L650, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W650, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W650, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W650, FÜGGŐLEGES HÍD A HÁTSON"]
["20318","ALCUBAR / CU - IZOLATOR 1P, W800, MOST PIONOWY NA PLECACH",210.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20318","SZT","85469010",null,null,"5901988203184","AlCu/Cu - Isolateur 1P, L800, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W800, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W800, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W800, FÜGGŐLEGES HÍD A HÁTSON"]
["20319","ALCUBAR / CU - IZOLATOR 1P, W850, MOST PIONOWY NA PLECACH",213.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20319","SZT","85469010",null,null,"5901988203191","AlCu/Cu - Isolateur 1P, L850, pont vertical à l'arrière","AlCu/Cu - 1P insulator, W850, Vertical bridge on the back","ALCUB/CU- SOPORTE 1P, W850, EMB. VERTIC. PARTE POSTERIOR","AlCubar / CU - SZIGETELŐ 1P, W850, FÜGGŐLEGES HÍD A HÁTSON"]
["20328","ALCUBAR - OSŁONA MOSTU ALCUBAR H27",0,"1-ZE-08",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988203283","AlCu - Couverture de pont AlCubar H27","AlCu - AlCubar H27 bridge cover","AlCubar - Cubierta puente AlCubar H27","ALCUBAR - ALCUBAR H27 HÍDBURKOLAT"]
["20329","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, ROZSTAW 80MM, POLIWĘGLAN 15X330X2000MM",377.4,"1-ZE-08",9.166666666666666E-2,2,"OE_SEPARATION_BUSBAR","20329","SZT","85389099","27.33.14.0",null,"5901988203290","AlCu - couvre pont AlCubar H27, espacement 80 mm, polycarbonate 40x330x2000mm","AlCu - AlCubar H27 bridge cover, 80mm distance, polycarbonate 15x330x2000mm","ALCUB- TAPA EMB. ALCUB- H27, DIST. 80MM, POLICARBONATO","AlCubar - ALCUBAR H27 HÍDBURKOLAT, HELY 80MM, POLIKARBONÁT 15X330X2000MM"]
["20340","H27",0,"1-ZE-08",null,null,null,null,"SZT",null,null,null,null,null,null,null,"H27"]
["20341","H50",0,"1-ZE-08",null,null,null,null,"SZT",null,null,null,null,null,null,null,"H50"]
["20343","H75",0,"1-ZE-08",null,null,null,null,"SZT",null,null,null,null,null,null,null,"H75"]
["20344","AlCubar - Połaczenie miedziane mostu poziomego AlCubar H100 pola narożnego, Cu 100x10 - komplet L1, L2, L3, N",3153.9,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988203443","AlCubar - Raccordement cuivre du pont horizontal AlCubar H100 de la travée d'angle, Cu 100x10 - set L1, L2, L3, N","AlCubar - Copper connection of the Horizontal bridge AlCubar H100 of the corner bay, Cu 100x10 - set L1, L2, L3, N","*AlCubar - Empalme de cobre del puente horizontal AlCubar H100 de la crujía, Cu 100x10 - set L1, L2, L3, N","AlCubar - AlCubar H100 vízszintes híd rézcsatlakozása a sarokterületen, Cu 100x10 - L1, L2, L3, N készlet"]
["20346","H150",0,"1-ZE-08",null,null,null,null,"SZT",null,null,null,null,null,null,null,"H150"]
["20350","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (15X5) 4 SZT. 160A - 500MM",248,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203504","AlCu - rails en cuivre perforés (15x5) 4 pcs. 160A - 500mm","AlCu - Opened copper bars (15x5) 4 pcs. 160A - 500mm","ALCUBAR - PLETINAS CU PERFORADAS (15X5) 4 UDS 160A  L=500MM","AlCubar - NYITOTT RÉZSÍNEK (15X5) 4 DB. 160A - 500MM"]
["20351","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (20X5) 4 SZT. 250A - 500MM",300,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203511","AlCu - rails en cuivre perforés (20x5) 4 pcs. 250A - 500mm","AlCu - Opened copper bars (20x5) 4 pcs. 250A - 500mm","ALCUBAR - PLETINAS CU PERFORADAS (20X5) 4 UDS 250A  L=500MM","AlCubar - NYITOTT RÉZSÍNEK (20X5) 4 DB. 250A - 500MM"]
["20352","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (30X5) 4 SZT. 400A - 500MM",439,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203528","AlCu - rails en cuivre perforés (30x5) 4 pcs. 400A - 500mm","AlCu - Opened copper bars (30x5) 4 pcs. 400A - 500mm","ALCUBAR - PLETINAS CU PERFORADAS (30X5) 4 UDS 400A  L=500MM","AlCubar - NYITOTT RÉZSÍNEK (30X5) 4 DB. 400A - 500MM"]
["20353","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (30x10) 4 SZT. 630A - 500MM",876,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203535","AlCu - rails en cuivre perforés () 4 pcs. 630A - 500mm","AlCu - Opened copper bars () 4 pcs. 630A - 500mm","AlCubar - Barras de cobre abiertas () 4 piezas 630A - 500mm","AlCubar - NYITOTT RÉZSÍNEK (30x10) 4 DB. 630A - 500MM"]
["20360","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (15X5) 4 SZT. 160A - 1000MM",491,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203603","AlCu - rails en cuivre perforés (15x5) 4 pcs. 160A - 1000mm","AlCu - Opened copper bars (15x5) 4 pcs. 160A - 1000mm","ALCUBAR - PLETINAS CU PERFORADAS (15X5) 4 UDS 160A  L=1000MM","AlCubar - NYITOTT RÉZSÍNEK (15X5) 4 DB. 160A - 1000MM"]
["20361","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (20X5) 4 SZT. 250A - 1000MM",586,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203610","AlCu - rails en cuivre perforés (20x5) 4 pcs. 250A - 1000mm","AlCu - Opened copper bars (20x5) 4 pcs. 250A - 1000mm","ALCUBAR - PLETINAS CU PERFORADAS (20X5) 4 UDS 250A  L=1000MM","AlCubar - NYITOTT RÉZSÍNEK (20X5) 4 DB. 250A - 1000MM"]
["20362","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (30X5) 4 SZT. 400A - 1000MM",879,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203627","AlCu - rails en cuivre perforés (30x5) 4 pcs. 400A - 1000mm","AlCu - Opened copper bars (30x5) 4 pcs. 400A - 1000mm","ALCUBAR - PLETINAS CU PERFORADAS (30X5) 4 UDS 400A  L=1000MM","AlCubar - NYITOTT RÉZSÍNEK (30X5) 4 DB. 400A - 1000MM"]
["20363","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (30x10) 4 SZT. 630A - 1000MM",1760,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900","24.44.22.0",null,"5901988203634","AlCu - rails en cuivre perforés () 4 pcs. 630A - 1000mm","AlCu - Opened copper bars () 4 pcs. 630A - 1000mm","AlCubar - Barras de cobre abiertas () 4 piezas 630A - 1000mm","AlCubar - NYITOTT RÉZSÍNEK (30x10) 4 DB. 630A - 1000MM"]
["20370","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (15X5) 4 SZT. 160A - 2000mm",1008,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988203702","AlCu - BARRES DE CUIVRE OUVERTES (15X5) 4 PCS. 160A - 2000mm","AlCu - OPEN COPPER BARS (15X5) 4 PCS. 160A - 2000mm","*AlCu - BARRAS DE COBRE ABIERTAS (15X5) 4 UDS. 160A - 2000mm","AlCubar - NYITOTT RÉZSÍNEK (15X5) 4 DB. 160A - 2000mm"]
["20371","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (20X5) 4 SZT. 250A - 2000mm",1203,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988203719","AlCu - BARRES DE CUIVRE OUVERTES (20X5) 4 PCS. 250A - 2000mm","AlCu - OPEN COPPER BARS (20X5) 4 PCS. 250A - 2000mm","*AlCu - BARRAS DE COBRE ABIERTO (20X5) 4 UDS. 250A - 2000mm","AlCubar - NYITOTT RÉZSÍNEK (20X5) 4 DB. 250A - 2000mm"]
["20372","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (30X5) 4 SZT. 400A - 2000mm",1880,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988203726","AlCu - BARRES DE CUIVRE OUVERTES (30X5) 4 PCS. 400A - 2000mm","AlCu - OPEN COPPER BARS (30X5) 4 PCS. 400A - 2000mm","*AlCu - BARRAS DE COBRE ABIERTO (30X5) 4 UDS. 400A - 2000mm","AlCubar - NYITOTT RÉZSÍNEK (30X5) 4 DB. 400A - 2000mm"]
["20373","ALCUBAR - OTWOROWANE SZYNY MIEDZIANE (30x10) 4 SZT. 630A - 2000mm",3693,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988203733","AlCu - BARRES DE CUIVRE OUVERTES (30x10) 4 PCS. 630A - 2000mm","AlCu - OPEN COPPER BARS (30x10) 4 PCS. 630A - 2000mm","*AlCu - BARRAS DE COBRE ABIERTAS (30x10) 4 UDS. 630A - 2000mm","AlCubar - NYITOTT RÉZSÍNEK (30x10) 4 DB. 630A - 2000mm"]
["20400","Zenergy - Wspornik płyt montażowych/izolatorów, D1000 Tył wzmocniony",136.1,"1-ZE-01",null,null,"OE_SUPPORT","20400","SZT","85389099",null,null,"5901988204006","OE - Support pour plaques de montage / isolateurs, renforcé P1000","OE - Bracket for Mounting plates / insulators, D1000 Reinforced rear","OE- SOPORTE PARA PLACAS DE MONTAJE / SOPORTES, D1000 ","Zenergy - Szerelőlap/szigetelőtartó, D1000 Megerősített hátlap"]
["20401","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH, D1000 WZMOCNIONY",194.4,"1-ZE-01",0.31666666666666665,4,"OE_SUPPORT","20401","SZT","85389099",null,null,"5901988204013","OE - Support de plaque de montage/isolateurs, P1000 renforcé ACB 6300A","OE - Bracket for Mounting plates / insulators, D1000 reinforced with ACB 6300A","OE- SOPORTE PARA PLACAS DE MONTAJE / SOPORTES, D1000  ACB 6300A","ZENERGY - SZERELŐLEMEZ TARTÓ, D1000 MEGERŐSÍTETT"]
["20402","ZENERGY - WSPORNIK IZOLATORÓW TYŁ, D200 POLA D600",65.2,"1-ZE-01",null,null,"OE_SUPPORT","20402","SZT","8538909900","27.90.20.0",null,"5901988204020","OE - Support pour plaques de montage / isolateurs, renforcé par P200","OE - Bracket for insulators rear, D200 fields D600","OE- SOPORTE PARA AISLADORES TRASERO, CAMPOS D200 D600","ZENERGY - HÁTSÓ SZIGETELŐ KONZER, D200 POLA D600"]
["20403","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH/IZOLATORÓW, D1000 WZMOCNIONY",125.3,"1-ZE-01",0.9,4,"OE_SUPPORT","20403","SZT","85389099","27.12.40.0",null,"5901988204037","OE - Support pour plaques de montage / isolateurs, renforcé P1000 ACB","OE - Bracket for Mounting plates / insulators, D1000 reinforced with ACB","OE- SOPORTE PARA PLACAS DE MONTAJE / AISLADORES, D1000 ","ZENERGY - TÁMASZTÁS SZERELÉSI LEMEZEKHEZ/SZIGETELŐKHOZ, D1000 MEGERŐSÍTETT"]
["20404","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH/IZOLATORÓW H36, D400 TYŁ WZMOCNIONY",81.599999999999994,"1-ZE-01",1.05,2,"OE_SUPPORT","20404","SZT","85389099","27.90.20.0",null,"5901988204044","OE - Support de plaque de montage/isolateurs, P400 renforcé à l'arrière","OE - Bracket for Mounting plates / insulators, D400 rear reinforced","OE- SOPORTE PLACA MONTAJE/SOP. BARRAS D400 DETRAS ","ZENERGY - TÁMASZTÁS A LEMEZEK/SZIGETELŐK SZERELÉSÉHEZ H36, D400 MEGERŐSÍTETT HÁTSÓ"]
["20405","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH/IZOLATORÓW H36, D400 WZMOCNIONY, FORMA 4B - KRÓTSZY",81.599999999999994,"1-ZE-01",null,null,"OE_SUPPORT","20405","SZT","85389099","27.90.20.0",null,"5901988204051","OE - Support de plaque de montage/isolateurs, P400 renforcé, Forme 4b - plus court","OE - Bracket for Mounting plates / insulators, D400 reinforced, Form 4b - shorter","OE- SOPORTE PLACA MONTAJE  INOX D400, REFORZADO","ZENERGY - SZERELÉSI LEMEZEK/SZIGETELŐ TÁMASZTÁSA H36, D400 MEGERŐSÍTETT, 4B FORMA - RÖVIDEBB"]
["20406","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH/IZOLATORÓW H36, D600 WZMOCNIONY",91.9,"1-ZE-01",2.4833333333333334,2,"OE_SUPPORT","20406","SZT","85389099","27.12.40.0",null,"5901988204068","OE - Support de plaque de montage/isolateurs, P600 renforcé","OE - Bracket for Mounting plates / insulators, D600 reinforced","OE- SOPORTE PLACA MONTAJE  INOX D600, REFORZADO","ZENERGY - SZERELÉSI LEMEZEK/SZIGETELŐ TÁMASZTÁSA H36, D600 MEGERŐSÍTETT"]
["20408","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH/IZOLATORÓW H36, D800 WZMOCNIONY",102.1,"1-ZE-01",3.7833333333333332,5,"OE_SUPPORT","20408","SZT","85389099","27.12.40.0",null,"5901988204082","OE - Support pour plaques de montage / isolateurs, renforcé P1000","OE - Bracket for Mounting plates / insulators, D800 reinforced","OE- SOPORTE PLACA MONTAJE/SOP. BARRAS D800 REFORZADO","ZENERGY - SZERELÉSI LEMEZEK/SZIGETELŐ TÁMASZTÁSA H36, D800 MEGERŐSÍTETT"]
["20409","ZENERGY - MOSTEK MIEDZIANY PEN ALCUBAR 100R DO PE ALCUBAR 50R",172.5,"1-ZE-01",null,null,"OE_ACB_TRANSFER","20409","SZT","74072900",null,null,"5901988204099","OE - Pont en cuivre PEN Alcubar 100R pour PE AlCubar 50R","OE - Copper PEN Alcubar 100R bridge for PE AlCubar 50R","ALCUB- PUENTE DE Cu PEN ALCUB- 100R PARA PE ALCUB- 50R","ZENERGY - COPPER BRIDGE PEN ALCUBAR 100R FOR PE ALCUBAR 50R"]
["20410","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH, D800 WZMOCNIONY",186.8,"1-ZE-01",null,null,"OE_SUPPORT","20410","SZT","85389099",null,null,"5901988204105","OE - Support de plaque de montage/isolateurs, P800 renforcé ACB 6300A","OE - Bracket for Mounting plates / insulators, D800 reinforced with ACB 6300A","OE- Conexión de cobre 06-10","ZENERGY - SZERELŐLEMEZ TARTÓ, D800 MEGERŐSÍTETT"]
["20411","Zenergy - Wspornik płyt montażowych/izolatorów H36, D1000 wzmocniony",136.1,"1-ZE-01",0.71666666666666667,4,"OE_SUPPORT","20411","SZT",null,null,"240518PW","5901988204112","OE - Plaque de montage/support d'isolateur H36, D1000 renforcé","OE - Mounting plate/insulator bracket H36, D1000 hardened","OE - Placa de montaje/soporte aislante H36, D1000 reforzado","Zenergy - Tartólemezek/szigetelők H36, D1000, megerősített"]
["20412","OE - Wspornik izolatorów D200 pola D1000",71.3,null,1.6166666666666667,4,"OE_SUPPORT","20412",null,null,null,"240619PW","5901988204129","OE - Support d'isolateur D200 pour baie D1000","OE - D200 insulator support for D1000 bay","Soporte aislante D200 para bahía D1000","OE - D200 szigetelő támogatás D1000 rekeszekhez"]
["20417","ZENERGY - POŁĄCZENIE MIEDZIANE 12",0,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988204174","OE - Raccord en cuivre 12","OE - Copper connection 12","OE- Conexión de cobre 12","ZENERGY - RÉZ CSATLAKOZTATÁS 12"]
["20424","ZENERGY - POŁĄCZENIE MIEDZIANE 16",0,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988204242","OE - Raccord en cuivre 16","OE - Copper connection 16","OE- Conexión de cobre 16","ZENERGY - RÉZ CSATLAKOZTATÁS 16"]
["20430","ALCUBAR - POŁĄCZENIE MIEDZIANE MOSTU PIONOWEGO ALCUBAR DO ROZŁĄCZNIKÓW LISTWOWYCH H50R 1000A",398.7,"1-ZE-01",9.166666666666666E-2,5,"OE_BUSBARS_ALCUBAR","20430","SZT","74072900",null,null,"5901988204303","AlCu - Connexion en cuivre du pont vertical AlCubar aux sectionneurs de rail H50R 1000A","AlCu - Copper connection of the AlCubar Vertical bridge for H50R 1000A rail disconnectors","ALCUB- CONEXIÓN Cu EMB. VERTIC. ALCUB- H50R 1000A","AlCubar – AlCubar FÜGGŐLEGES HÍD RÉZ CSATLAKOZTATÁSA H50R 1000A SZALAK KAPCSOLÓHOZ"]
["20431","ZENERGY - POŁĄCZENIE MIEDZIANE 20",0,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988204310","OE - Raccord en cuivre 20","OE - Copper connection 20","OE- Conexión de cobre 20","ZENERGY - RÉZ CSATLAKOZTATÁS 20"]
["20438","ZENERGY - POŁĄCZENIE MIEDZIANE 4X2X 80X10 WYŁĄCZNIKA UAN25B3S DO KABLI NAD DACH",4941.6000000000004,"1-ZE-01",null,null,"OE_ACB_TRANSFER","20438","SZT","74072900",null,null,"5901988204389","OE - Connexion en cuivre 4x2x 80x10 UAN25B3S Disjoncteur pour cĂ˘bles au-dessus du toit","OE - 4x2x 80x10 copper connection of UAN25B3S switch for cables above the roof","OE- CONEXIÓN Cu 4X2X 80X10 DEL INT. UAN25B3S ","ZENERGY - RÉZ CSATLAKOZÁS 4X2X 80X10 UAN25B3S TETŐFÖLTI KÁBELSZAKÍTÓ"]
["20440","ALCUBAR - POŁĄCZENIE MIEDZIANE MOSTU PIONOWEGO ALCUBAR DO ROZŁĄCZNIKÓW LISTWOWYCH H50R 1400A",898.2,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR","20440","SZT","74072900",null,null,"5901988204402","AlCu - Connexion en cuivre du pont vertical AlCubar aux sectionneurs de rail H50R 1400A","AlCu - Copper connection of the AlCubar Vertical bridge for H50R 1400A rail disconnectors","ALCUB- CONEXIÓN Cu EMB. VERTIC. ALCUB-  H50R 1400A","AlCubar – AZ AlCubar FÜGGŐLEGES HÍD RÉZ CSATLAKOZTATÁSA H50R 1400A SZALAK KAPCSOLÓKHOZ"]
["20441","ZENERGY - POŁĄCZENIE MIEDZIANE 3X2X 80X10 WYŁĄCZNIKA UAN25B3S Z ALCUBAR H100R DO ROZŁĄCZNIKÓW LISTWOWYCH",5276.2,"1-ZE-01",null,null,"OE_ACB_TRANSFER","20441","SZT","74072900",null,null,"5901988204419","OE - Connexion en cuivre Disjoncteur UAN25B3S 3x2x 80x10 avec AlCubar H100R pour sectionneurs ? bande","OE - 3x2x 80x10 copper connection of UAN25B3S circuit breaker with AlCubar H100R for switch disconnectors","ALCUB- CONEXIÓN Cu 3X2X 80X10 DE INT. AUT. UAN25B3S, ALCUB- H100R ","ZENERGY - RÉZ CSATLAKOZÓS 3X2X 80X10 UAN25B3S ÁRAMKAPCSOLÓ ALKUBARRAL H100R SZALAK KAPCSOLÓHOZ"]
["20445","ZENERGY - POŁĄCZENIE MIEDZIANE 32",0,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988204457","OE - Raccord en cuivre 32","OE - Copper connection 32","OE- Conexión de cobre 32","ZENERGY - RÉZ CSATLAKOZTATÁS 32"]
["20450","ALCUBAR - POŁĄCZENIE MIEDZIANE MOSTU PIONOWEGO ALCUBAR DO ROZŁĄCZNIKÓW LISTWOWYCH H100R 2500A",1854.7,"1-ZE-01",9.166666666666666E-2,5,"OE_BUSBARS_ALCUBAR","20450","SZT","74072900",null,null,"5901988204501","AlCu - Connexion en cuivre du pont vertical AlCubar aux sectionneurs de rail H100R 2500A","AlCu - Copper connection of the AlCubar Vertical bridge for H100R 2500A rail disconnectors","ALCUB- CONEXIÓN Cu DEL EMB. VERTIC. ALCUB- H100R 2500A","AlCubar – AlCubar FÜGGŐLEGES HÍD RÉZ CSATLAKOZTATÁSA A H100R 2500A SZALAK KAPCSOLÓHOZ"]
["20452","OE - Połączenie miedziane 40",0,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","7407290000",null,null,"5901988204525","OE - Raccord en cuivre 40","OE - Copper connection 40","OE- Conexión de cobre 40","OE - Réz csatlakozás 40"]
["20460","ALCUBAR - POŁĄCZENIE MIEDZIANE MOSTU PIONOWEGO ALCUBAR DO ROZŁĄCZNIKÓW LISTWOWYCH H150R 3200A",3175.2,"1-ZE-01",9.166666666666666E-2,4,"OE_INSULATOR_WIDTH",null,"SZT","7407290000",null,null,null,null,null,null,"AlCubar – AZ AlCubar FÜGGŐLEGES HÍD RÉZ CSATLAKOZTATÁSA A LI KAPCSOLÓKHOZSTWOWYCH H150R 3200A"]
["20463","ALCUBAR / 3XCU - IZOLATOR REGULOWANY 3200-4000A 3P, W650, WYŁĄCZNIK - MOST PIONOWY",336,"1-ZE-01",4.1666666666666664E-2,1,"OE_INSULATOR_WIDTH","20463","SZT","85469010",null,null,"5901988204631","AlCubar / 3xCu - Isolateur réglable 3200-4000A 3P, L650, interrupteur - pont vertical","AlCubar / 3xCu - Adjustable insulator 3200-4000A 3P, W650, circuit breaker - Vertical bridge","ALCUB- / 3XCU- SOPORTE REG. 3200-4000A 3P, W650, VERTIC.","AlCubar / 3XCU - ÁLLÍTHATÓ SZIGETELŐ 3200-4000A 3P, W650, MEGSZAKÍTÓ - FÜGGŐLEGES HÍD"]
["20464","ALCUBAR / 3XCU - IZOLATOR REGULOWANY 3200-4000A 4P, W650, WYŁĄCZNIK - MOST PIONOWY",392,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20464","SZT","85469010","27.90.12.0",null,"5901988204648","AlCubar / 3xCu - Isolant ajustable 3200-4000A 4P, L650, commutateur - pont vertical","AlCubar / 3xCu - Adjustable insulator 3200-4000A 4P, W650, circuit breaker - Vertical bridge","ALCUB- / 3XCU- SOPORTE REG. 3200-4000A 4P, W650, VERTIC.","AlCubar / 3XCU - ÁLLÍTHATÓ SZIGETELŐ 3200-4000A 4P, W650, MEGSZAKÍTÓ - FÜGGŐLEGES HÍD"]
["20470","Zenergy - Połączenie miedziane wyłącznika UAN16A 4x 2x80X5 na plecy (obudowa D600) - Vertical Type",3808.8,"1-ZE-01",null,null,"OE_ACB_TRANSFER",null,"SZT","74072900",null,null,"5901988204709","OE - Connexion Cuivre UAN16A 4x 2x80X5 pour l'arrière (boitier P600) - Type Vertical","OE - Copper connection UAN16A 4x 2x80X5 for the back (D600 housing) - Vertical Type","*OE - Conexión de cobre UAN16A 4x 2x80X5 para la parte posterior (carcasa D600) - Tipo vertical","Zenergy - UAN16A kapcsoló réz csatlakozása 4x 2x80X5 hátul (D600 ház) - Függőleges típus"]
["20471","Zenergy - Połączenie miedziane wyłącznika UAN25B 4x 2x80X10 na plecy (obudowa D600) - Vertical Type",6982.8,"1-ZE-01",null,null,"OE_ACB_TRANSFER",null,"SZT","74072900",null,null,"5901988204716","OE - Connexion Cuivre UAN25B 4x 2x80X10 pour l'arrière (boîtier P600) - Type Vertical","OE - Copper connection UAN25B 4x 2x80X10 for the back (D600 housing) - Vertical Type","*OE - Conexión de cobre UAN25B 4x 2x80X10 para la parte posterior (carcasa D600) - Tipo vertical","Zenergy - UAN25B kapcsoló réz csatlakozása 4x 2x80X10 hátul (D600 ház) - Függőleges típus"]
["20474","Zenergy - Połączenie miedziane wyłącznika UAN16A 4x 2x80X5 na plecy, 4x 2x50X10 do mostu poziomego w przedziale D400 za wyłącznikem (obudowa D800) - Vertical Type/Upper + Horizontal Type/Lower",6982.8,"1-ZE-01",null,null,"OE_ACB_TRANSFER",null,"SZT","74072900",null,null,"5901988204747","OE - Connexion en cuivre du disjoncteur UAN16A 4x 2x80X5 à l'arrière, 4x 2x50X10 au pont horizontal dans le compartiment P400 derrière le disjoncteur (enveloppe P800) - Type vertical/supérieur + Type horizontal/inférieur","OE - Copper connection of the circuit breaker UAN16A 4x 2x80X5 to the back, 4x 2x50X10 to the Horizontal bridge in the D400 compartment behind the circuit breaker (D800 enclosure) - Vertical Type/Upper + Horizontal Type/Lower","*OE - Conexión de cobre del interruptor automático UAN16A 4x 2x80X5 hacia atrás, 4x 2x50X10 al puente horizontal en el compartimiento D400 detrás del interruptor automático (carcasa D800) - Tipo vertical/superior + Tipo horizontal/inferior","Zenergy - UAN16A megszakító réz csatlakozása 4x 2x80X5 hátul, 4x 2x50X10 a vízszintes hídhoz a D400 rekeszben a megszakító mögött (D800 ház) - Függőleges típus/Felső + Vízszintes típus/Alsó"]
["20475","Zenergy - Połączenie miedziane wyłącznika UAN25B 4x 2x80X10 na plecy, 4x 2x80X10 do mostu poziomego w przedziale D400 za wyłącznikiem (obudowa D800) - Vertical Type/Upper + Horizontal Type/Lower",11426.4,"1-ZE-01",null,null,"OE_ACB_TRANSFER",null,"SZT","74072900",null,null,"5901988204754","OE - Connexion en cuivre du disjoncteur UAN25B 4x 2x80X10 à l'arrière, 4x 2x80X10 au pont horizontal dans le compartiment P400 derrière le disjoncteur (enveloppe P800) - Type vertical/supérieur + Type horizontal/inférieur","OE - Copper connection of the circuit breaker UAN25B 4x 2x80X10 to the back, 4x 2x80X10 to the Horizontal bridge in the D400 compartment behind the circuit breaker (D800 enclosure) - Vertical Type/Upper + Horizontal Type/Lower","*OE - Conexión de cobre del interruptor automático UAN25B 4x 2x80X10 a la parte posterior, 4x 2x80X10 al puente horizontal en el compartimiento D400 detrás del interruptor automático (carcasa D800) - Tipo vertical/Superior + Tipo horizontal/Inferior","Zenergy - Az UAN25B megszakító rézcsatlakozása 4x 2x80X10 hátul, 4x 2x80X10 a vízszintes hídhoz a D400 rekeszben a megszakító mögött (D800 ház) - Függőleges típus/Felső + Vízszintes típus/Alsó"]
["20476","Zenergy - Połączenie miedziane wyłącznika UAN25B 4x 2x80X10 do mostów poziomych w przedziale D400 za wyłącznikem (obudowa D800) - Horizontal Type",12272.8,"1-ZE-01",null,null,"OE_ACB_TRANSFER",null,"SZT","74072900",null,null,"5901988204761","OE - Connexion en cuivre du disjoncteur UAN25B 4x 2x80X10 pour les ponts horizontaux dans le compartiment P400 derrière le disjoncteur (enveloppe P800) - Type Horizontal","OE - Copper connection of the circuit breaker UAN25B 4x 2x80X10 for Horizontal bridges in the D400 compartment behind the circuit breaker (D800 enclosure) - Horizontal Type","*OE - Conexión de cobre del interruptor automático UAN25B 4x 2x80X10 para puentes horizontales en el compartimento D400 detrás del interruptor automático (carcasa D800) - Tipo Horizontal","Zenergy - UAN25B megszakító rézcsatlakozása 4x 2x80X10 vízszintes hidakhoz a D400 rekeszben a megszakító mögött (D800 ház) - Vízszintes típus"]
["20477","Zenergy - Połączenie miedziane wyłącznika UAN25B (przyłącza krawędziowe) 4x 2x80X10 do mostu poziomego w przedziale D400 za wyłącznikeim (obudowa D800)",0,"1-ZE-01",null,null,"OE_ACB_TRANSFER",null,"SZT","74072900",null,null,"5901988204778","OE - Connexion en cuivre du disjoncteur UAN25B (connexions de bord) 4x 2x80X10 au pont horizontal dans le compartiment P400 derrière le disjoncteur (coffret P800)","OE - Copper connection of the UAN25B circuit breaker (edge connections) 4x 2x80X10 to the Horizontal bridge in the D400 compartment behind the circuit breaker (D800 enclosure)","*OE - Conexión de cobre del interruptor automático UAN25B (conexiones de borde) 4x 2x80X10 al puente horizontal en el compartimiento D400 detrás del interruptor automático (caja D800)","Zenergy - Az UAN25B megszakító rézcsatlakozása (élcsatlakozások) 4x 2x80X10 a vízszintes hídhoz a D400 rekeszben a megszakítók mögött (D800 ház)"]
["20483","ALCUBAR / 3XCU - IZOLATOR REGULOWANY 3200-4000A 3P, W850, WYŁĄCZNIK - MOST PIONOWY",353.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20483","SZT","85469010",null,null,"5901988204839","AlCubar / 3xCu - Isolateur réglable 3200-4000A 3P, L850, interrupteur - pont vertical","AlCubar / 3xCu - Adjustable insulator 3200-4000A 3P, W850, circuit breaker - Vertical bridge","ALCUB- / 3XCU- SOPORTE REG. 3200-4000A 3P, W850, VERTIC.","AlCubar / 3XCU - ÁLLÍTHATÓ SZIGETELŐ 3200-4000A 3P, W850, MEGSZAKÍTÓ - FÜGGŐLEGES HÍD"]
["20484","ALCUBAR / 3XCU - IZOLATOR REGULOWANY 3200-4000A 4P, W850, WYŁĄCZNIK - MOST PIONOWY",411,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20484","SZT","85469010",null,null,"5901988204846","AlCubar / 3xCu - Isolateur ajustable 3200-4000A 4P, L850, commutateur - pont vertical","AlCubar / 3xCu - Adjustable insulator 3200-4000A 4P, W850, circuit breaker - Vertical bridge","ALCUB- / 3XCU- SOPORTE REG. 3200-4000A 4P, W850, VERTIC.","AlCubar / 3XCU - ÁLLÍTHATÓ SZIGETELŐ 3200-4000A 4P, W850, MEGSZAKÍTÓ - FÜGGŐLEGES HÍD"]
["20493","ALCUBAR / 3XCU - IZOLATOR REGULOWANY 5000-6300A 3P, W1200, WYŁĄCZNIK - MOST PIONOWY",381.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20493","SZT","85469010",null,null,"5901988204938","AlCubar / 3xCu - Isolateur réglable 5000-6300A 3P, L1200, interrupteur - pont vertical","AlCubar / 3xCu - Adjustable insulator 5000-6300A 3P, W1200, circuit breaker - Vertical bridge","ALCUB- / 3XCU- SOPORTE REG. 5000-6300A 3P, W1200, VERTIC.","AlCubar / 3XCU - ÁLLÍTHATÓ SZIGETELŐ 5000-6300A 3P, W1200, MEGSZAKÍTÓ - FÜGGŐLEGES HÍD"]
["20494","ALCUBAR / 3XCU - IZOLATOR REGULOWANY 5000-6300A 4P, W1200, WYŁĄCZNIK - MOST PIONOWY",439,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20494","SZT","85469010",null,null,"5901988204945","AlCubar / 3xCu - Isolateur réglable 5000-6300A 4P, L1200, interrupteur - pont vertical","AlCubar / 3xCu - Adjustable insulator 5000-6300A 4P, W1200, circuit breaker - Vertical bridge","ALCUB- / 3XCU- AISLADOR REG. 5000-6300A 4P, W1200, VERTIC.","AlCubar / 3XCU - ÁLLÍTHATÓ SZIGETELŐ 5000-6300A 4P, W1200, MEGSZAKÍTÓ - FÜGGŐLEGES HÍD"]
["20500","ALCUBAR / CU - IZOLATOR 3P, W1000, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",384.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205003","AlCu/Cu - 3P, isolateur L1000, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W1000, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1000, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W1000, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20501","ALCUBAR / CU - IZOLATOR 3P, W1200, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",395.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205010","AlCu/Cu - 3P, isolateur L1200, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W1200, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1200, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W1200, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20502","ALCUBAR / CU - IZOLATOR 3P, W1300, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",407.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205027","AlCu/Cu - 3P, isolateur L1300, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W1300, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1300, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W1300, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20504","ALCUBAR / CU - IZOLATOR 3P, W400, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",320.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20504","SZT","85469010",null,null,"5901988205041","AlCu/Cu - 3P, isolateur L400, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W400, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W400, HORIZ. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W400, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20505","ALCUBAR / CU - IZOLATOR 3P, W450, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",327,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20505","SZT","85469010",null,null,"5901988205058","AlCu/Cu - 3P, isolateur L450, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W450, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W450, HORIZ. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W450, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20506","ALCUBAR / CU - IZOLATOR 3P, W600, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",339.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205065","AlCu/Cu - 3P, isolateur L600, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W600, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W600, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W600, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20507","ALCUBAR / CU - IZOLATOR 3P, W650, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",346.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20507","SZT","85469010",null,null,"5901988205072","AlCu/Cu - 3P, isolateur L650, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W650, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W650, HORIZ. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W650, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20508","ALCUBAR / CU - IZOLATOR 3P, W800, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",362.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205089","AlCu/Cu - 3P, isolateur L800, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W800, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W800, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W800, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20509","ALCUBAR / CU - IZOLATOR 3P, W850, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",371.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20509","SZT","85469010",null,null,"5901988205096","AlCu/Cu - 3P, isolateur L850, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W850, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W850, HORIZ. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W850, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20510","ALCUBAR / CU - IZOLATOR 4P, W1000, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",470.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205102","AlCu/Cu - 4P, isolateur L1000, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W1000, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1000, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - SZIGETELŐ 4P, W1000, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20511","ALCUBAR / CU - IZOLATOR 4P, W1200, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",482.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205119","AlCu/Cu - 4P, isolateur L1200, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W1200, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1200, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 4P SZIGETELŐ, W1200, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20512","ALCUBAR / CU - IZOLATOR 4P, W1300, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",493.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205126","AlCu/Cu - 4P, isolateur L1300, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W1300, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1300, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - 4P SZIGETELŐ, W1300, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20515","ALCUBAR / CU - IZOLATOR 4P, W450, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",409.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20515","SZT","85469010",null,null,"5901988205157","AlCu/Cu - 4P, isolateur L450, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W450, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W450, HORIZ. REG. PROF. PASO 80MM","AlCubar / CU - SZIGETELŐ 4P, W450, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20516","ALCUBAR / CU - IZOLATOR 4P, W600, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",421.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205164","AlCu/Cu - 4P, isolateur L600, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W600, Horizontally, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W600, HORIZ. REGUL. PROF. PASO  80mm","AlCubar / CU - SZIGETELŐ 4P, W600, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20517","ALCUBAR / CU - IZOLATOR 4P, W650, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",429,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20517","SZT","85469010","27.90.12.0",null,"5901988205171","AlCu/Cu - 4P, isolateur L650, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W650, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W650, HORIZ. REG. PROF. PASO 80MM","AlCubar / CU - SZIGETELŐ 4P, W650, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20518","ALCUBAR / CU - IZOLATOR 4P, W800, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",446.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205188","AlCu/Cu - 4P, isolateur L800, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W800, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W800, HORIZ. REGUL. PROF. PASO  80mm","ALCUBAR / CU - SZIGETELŐ 4P, W800, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20519","ALCUBAR / CU - IZOLATOR 4P, W850, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",459.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20519","SZT","85469010",null,null,"5901988205195","AlCu/Cu - 4P, isolateur L850, horizontal, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W850, Horizontal, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W850, HORIZ. REG. PROF. PASO 80MM","ALCUBAR / CU - 4P SZIGETELŐ, W850, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20520","ALCUBAR / CU - IZOLATOR 3P, W1000, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",433.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205201","AlCu/Cu - 3P, isolateur L1000, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W1000, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1000, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W1000, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20521","ALCUBAR / CU - IZOLATOR 3P, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",444.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205218","AlCu/Cu - 3P, isolateur L1200, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W1200, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1200, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20522","ALCUBAR / CU - IZOLATOR 3P, W1300, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",457,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205225","AlCu/Cu - 3P, isolateur L1300, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W1300, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1300, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W1300, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20524","ALCUBAR / CU - IZOLATOR 3P, W400, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",381.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20524","SZT","85469010",null,null,"5901988205249","AlCu/Cu - 3P, isolateur L400, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W400, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W400, VERTIC. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W400, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20525","ALCUBAR / CU - IZOLATOR 3P, W450, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",388.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20525","SZT","85469010",null,null,"5901988205256","AlCu/Cu - 3P, isolateur L450, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W450, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W450, VERTIC. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W450, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20526","ALCUBAR / CU - IZOLATOR 3P, W600, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",393.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205263","AlCu/Cu - 3P, isolateur L600, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W600, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W600, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W600, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20527","ALCUBAR / CU - IZOLATOR 3P, W650, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",399.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20527","SZT","85469010",null,null,"5901988205270","AlCu/Cu - 3P, isolateur L650, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W650, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W650, VERTIC. REG. PROF. PASO 80MM","ALCUBAR / CU - 3P SZIGETELŐ, W650, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20528","ALCUBAR / CU - IZOLATOR 3P, W800, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",412.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205287","AlCu/Cu - 3P, isolateur L800, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W800, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W800, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - 3P SZIGETELŐ, W800, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20529","ALCUBAR / CU - IZOLATOR 3P, W850, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",421.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20529","SZT","85469010",null,null,"5901988205294","AlCu/Cu - 3P, isolateur L850, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 3P, W850, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 3P, W850, VERTIC. REG. PROF. PASO 80MM","AlCubar / CU - 3P SZIGETELŐ, W850, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20530","ALCUBAR / CU - IZOLATOR 4P, W1000, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",517.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205300","AlCu/Cu - 4P, isolateur L1000, vertical, réglable en profondeur, écartement 80mm","AlCu/Cu - Insulator 4P, W1000, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1000, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - SZIGETELŐ 4P, W1000, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20531","ALCUBAR / CU - IZOLATOR 4P, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",529.79999999999995,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205317","AlCu/Cu - 4P, isolateur L1200, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W1200, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1200, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - SZIGETELŐ 4P, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20532","ALCUBAR / CU - IZOLATOR 4P, W1300, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",541,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205324","AlCu/Cu - 4P, isolateur L1300, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W1300, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1300, VERT., REGUL. PROF. PASO  80mm","ALCUBAR / CU - 4P SZIGETELŐ, W1300, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20535","ALCUBAR / CU - IZOLATOR 4P, W450, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",470.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20535","SZT","85469010",null,null,"5901988205355","AlCu/Cu - 4P, isolateur L450, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W450, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W450, VERTIC. REG. PROF. PASO 80MM","AlCubar / CU - SZIGETELŐ 4P, W450, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20536","ALCUBAR / CU - IZOLATOR 4P, W600, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",478.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205362","AlCu/Cu - 4P, isolateur L600, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W600, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W600, VERT., REGUL. PROF. PASO  80mm","AlCubar / CU - SZIGETELŐ 4P, W600, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20537","ALCUBAR / CU - IZOLATOR 4P, W650, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",482.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20537","SZT","85469010",null,null,"5901988205379","AlCu/Cu - 4P, isolateur L650, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W650, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W650, VERTIC. REG. PROF. PASO 80MM","ALCUBAR / CU - 4P SZIGETELŐ, W650, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20538","ALCUBAR / CU - IZOLATOR 4P, W800, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",497.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205386","AlCu/Cu - 4P, isolateur L800, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W800, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W800, VERT., REGUL. PROF. PASO  80mm","AlCubar / CU - SZIGETELŐ 4P, W800, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20539","ALCUBAR / CU - IZOLATOR 4P, W850, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 80MM",506.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20539","SZT","85469010",null,null,"5901988205393","AlCu/Cu - 4P, isolateur L850, vertical, réglable en profondeur, distance 80mm","AlCu/Cu - Insulator 4P, W850, Vertically, adjustable depth, spacing 80mm","ALCUB/CU- SOPORTE 4P, W850, VERTIC. REG. PROF. PASO 80MM","ALCUBAR / CU - 4P SZIGETELŐ, W850, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 80MM"]
["20540","ALCUBAR / CU - IZOLATOR 3P, W1000, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",433.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205409","AlCu/Cu - 3P, isolateur L1000, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W1000, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1000, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 3P SZIGETELŐ, W1000, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20541","ALCUBAR / CU - IZOLATOR 3P, W1200, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",444.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205416","AlCu/Cu - 3P, isolateur L1200, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W1200, support / Vertical on the back, adjustable height, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1200, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 3P SZIGETELŐ, W1200, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20542","ALCUBAR / CU - IZOLATOR 3P, W1300, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",457,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205423","AlCu/Cu - 3P, isolateur L1300, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W1300, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W1300, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 3P SZIGETELŐ, W1300, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20544","ALCUBAR / CU - IZOLATOR 3P, W400, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",381.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20544","SZT","85469010",null,null,"5901988205447","AlCu/Cu - 3P, isolateur L400, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W400, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W400, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / CU - 3P SZIGETELŐ, W400, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20545","ALCUBAR / CU - IZOLATOR 3P, W450, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",388.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20545","SZT","85469010",null,null,"5901988205454","AlCu/Cu - 3P, isolateur L450, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W450, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W450, SOP/VERT PARTE POSTERIOR, REG. ALT.","ALCUBAR / CU - 3P SZIGETELŐ, W450, TÁMASZTÁS/FÜGGŐLEGES A HÁTSON, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20546","ALCUBAR / CU - IZOLATOR 3P, W600, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",393.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205461","AlCu/Cu - 3P, isolateur L600, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W600, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W600, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 3P SZIGETELŐ, W600, TÁMASZTÁS/FÜGGŐLEGES HÁTTÉL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20547","ALCUBAR / CU - IZOLATOR 3P, W650, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",399.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20547","SZT","85469010",null,null,"5901988205478","AlCu/Cu - 3P, isolateur L650, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W650, support / Vertical on the back, adjustable height, spacing 80mm","ALCUB/CU- SOPORTE 3P, W650, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / CU - 3P SZIGETELŐ, W650, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 80 mm-es tér"]
["20548","ALCUBAR / CU - IZOLATOR 3P, W800, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",412.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988205485","AlCu/Cu - 3P, isolateur L800, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W800, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W800, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 3P SZIGETELŐ, W800, TÁMASZTÁS/FÜGGŐLEGES A HÁTSON, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20549","ALCUBAR / CU - IZOLATOR 3P, W850, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",421.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20549","SZT","85469010",null,null,"5901988205492","AlCu/Cu - 3P, isolateur L850, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 3P, W850, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 3P, W850, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / CU - 3P SZIGETELŐ, W850, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELYSZÍM 80MM"]
["20550","ALCUBAR / CU - IZOLATOR 4P, W1000, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",517.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988205508","AlCu/Cu - 4P, isolateur L1000, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W1000, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1000, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - ISOLATOR 4P, W1000, TÁMOGATÁS/FÜGGŐLEGES A HÁTSON,ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20551","ALCUBAR / CU - IZOLATOR 4P, W1200, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",529.79999999999995,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988205515","AlCu/Cu - 4P, isolateur L1200, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W1200, support / Vertical on the back, adjustable height, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1200, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 4P SZIGETELŐ, W1200, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20552","ALCUBAR / CU - IZOLATOR 4P, W1300, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",541,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988205522","AlCu/Cu - 4P, isolateur L1300, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W1300, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W1300, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm80 mm","AlCubar / CU - 4P SZIGETELŐ, W1300, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20554","AlCubar / Cu - Izolator 4P, W400, podpora/pionowo na plecach, regulowana wysokość, rozstaw 80mm",463.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20554","SZT","85469010","27.90.12.0",null,"5901988205546","AlCu/Cu - 4P, isolateur L400, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W400, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W400, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / Cu - Szigetelő 4P, W400, támasz/függőleges hátul, állítható magasság, távolság 80mm"]
["20555","ALCUBAR / CU - IZOLATOR 4P, W450, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",470.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20555","SZT","85469010","27.90.12.0",null,"5901988205553","AlCu/Cu - 4P, isolateur L450, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W450, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W450, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / CU - 4P SZIGETELŐ, W450, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20556","ALCUBAR / CU - IZOLATOR 4P, W600, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",478.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988205560","AlCu/Cu - 4P, isolateur L600, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W600, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W600, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 4P SZIGETELŐ, W600, TÁMASZTÁS/FÜGGŐLEGES A HÁLON, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20557","ALCUBAR / CU - IZOLATOR 4P, W650, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",482.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20557","SZT","85469010","27.90.12.0",null,"5901988205577","AlCu/Cu - 4P, isolateur L650, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W650, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W650, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / CU - 4P SZIGETELŐ, W650, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20558","ALCUBAR / CU - IZOLATOR 4P, W800, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",497.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010","27.90.12.0",null,"5901988205584","AlCu/Cu - 4P, isolateur L800, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W800, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W800, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm 80 mm","AlCubar / CU - 4P SZIGETELŐ, W800, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 80 mm-es térköz"]
["20559","ALCUBAR / CU - IZOLATOR 4P, W850, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 80MM",506.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20559","SZT","85469010","27.90.12.0",null,"5901988205591","AlCu/Cu - 4P, isolateur L850, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 4P, W850, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 4P, W850, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / CU - 4P SZIGETELŐ, W850, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, HELY 80MM"]
["20567","AlCubar / Cu - Izolator 6P, W650, podpora/pionowo na plecach, regulowana wysokość, rozstaw 80mm",566.70000000000005,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20567","SZT","85469010",null,null,"5901988205676","AlCu/Cu - 6P, isolateur L650, dossier/vertical, réglable en hauteur, écartement 80mm","AlCu/Cu - Insulator 6P, W650, support / Vertical on the back, height adjustable, spacing 80mm","ALCUB/CU- SOPORTE 6P, W650, SOP/VERT PARTE POSTERIOR, REG. ALT.","AlCubar / Cu - Szigetelő 6P, W650, hátul támasztó/függőleges, állítható magasságú, távolság 80mm"]
["20600","ALCUBAR / CU - IZOLATOR 3P, W1000, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",384.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206000","AlCu/Cu - 3P, isolateur L1000, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W1000, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1000, HORIZ. REGUL. PROF. PASO  105mm","ALCUBAR / CU - 3P SZIGETELŐ, W1000, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20601","ALCUBAR / CU - IZOLATOR 3P, W1200, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",395.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206017","AlCu/Cu - 3P, isolateur L1200, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W1200, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1200, HORIZ. REGUL. PROF. PASO  105mm","ALCUBAR / CU - 3P SZIGETELŐ, W1200, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20602","ALCUBAR / CU - IZOLATOR 3P, W1300, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",407.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206024","AlCu/Cu - 3P, isolateur L1300, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W1300, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1300, HORIZ. REGUL. PROF. PASO  105mm","AlCubar / CU - 3P SZIGETELŐ, W1300, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20605","ALCUBAR / CU - IZOLATOR 3P, W450, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",327,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20605","SZT","85469010",null,null,"5901988206055","AlCu/Cu - 3P, isolateur L450, horizontal, réglable en profondeur, espacement 105mm","AlCu/Cu - Insulator 3P, W450, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W450, HORIZ. REG. PROF. PASO 105MM","ALCUBAR / CU - 3P SZIGETELŐ, W450, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20606","ALCUBAR / CU - IZOLATOR 3P, W600, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",339.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206062","AlCu/Cu - 3P, isolateur L600, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W600, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W600, HORIZ. REGUL. PROF. PASO  105mm","ALCUBAR / CU - 3P SZIGETELŐ, W600, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20607","ALCUBAR / CU - IZOLATOR 3P, W650, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",346.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20607","SZT","85469010",null,null,"5901988206079","AlCu/Cu - 3P, isolateur L650, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W650, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W650, HORIZ. REG. PROF. PASO 105MM","ALCUBAR / CU - 3P SZIGETELŐ, W650, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20608","ALCUBAR / CU - IZOLATOR 3P, W800, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",362.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206086","AlCu/Cu - 3P, isolateur L800, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W800, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W800, HORIZ. REGUL. PROF. PASO  105mm","ALCUBAR / CU - 3P SZIGETELŐ, W800, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20609","ALCUBAR / CU - IZOLATOR 3P, W850, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",371.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20609","SZT","85469010",null,null,"5901988206093","AlCu/Cu - 3P, isolateur L850, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W850, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W850, HORIZ. REG. PROF. PASO 105MM","ALCUBAR / CU - 3P SZIGETELŐ, W850, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20610","ALCUBAR / CU - IZOLATOR 4P, W1000, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",470.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206109","AlCu/Cu - 4P, isolateur L1000, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W1000, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1000, HORIZ. REGUL. PROF. PASO  105mm","AlCubar / CU - SZIGETELŐ 4P, W1000, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20611","ALCUBAR / CU - IZOLATOR 4P, W1200, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",482.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206116","AlCu/Cu - 4P, isolateur L1200, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W1200, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1200, HORIZ. REGUL. PROF. PASO  105mm","ALCUBAR / CU - 4P SZIGETELŐ, W1200, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20612","ALCUBAR / CU - IZOLATOR 4P, W1300, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",493.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206123","AlCu/Cu - 4P, isolateur L1300, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W1300, Horizontally, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1300, HORIZ. REGUL. PROF. PASO  105mm","AlCubar / CU - 4P SZIGETELŐ, W1300, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20616","ALCUBAR / CU - IZOLATOR 4P, W600, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",421.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206161","AlCu/Cu - 4P, isolateur L600, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W600, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W600, HORIZ. REGUL. PROF. PASO  105mm","AlCubar / CU - SZIGETELŐ 4P, W600, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20617","ALCUBAR / CU - IZOLATOR 4P, W650, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",429,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20617","SZT","85469010",null,null,"5901988206178","AlCu/Cu - 4P, isolateur L650, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W650, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W650, HORIZ. REG. PROF. PASO 105MM","ALCUBAR / CU - 4P SZIGETELŐ, W650, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20618","ALCUBAR / CU - IZOLATOR 4P, W800, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",446.9,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206185","AlCu/Cu - 4P, isolateur L800, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W800, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W800, HORIZ. REGUL. PROF. PASO  105mm","ALCUBAR / CU - SZIGETELŐ 4P, W800, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20619","ALCUBAR / CU - IZOLATOR 4P, W850, POZIOMO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",459.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20619","SZT","85469010",null,null,"5901988206192","AlCu/Cu - 4P, isolateur L850, horizontal, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W850, Horizontal, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W850, HORIZ. REG. PROF. PASO 105MM","ALCUBAR / CU - 4P SZIGETELŐ, W850, VÍZSZINTES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20620","ALCUBAR / CU - IZOLATOR 3P, W1000, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",433.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206208","AlCu/Cu - 3P, isolateur L1000, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W1000, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1000, VERT. REGUL. PROF. PASO 105mm","ALCUBAR / CU - 3P SZIGETELŐ, W1000, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20621","ALCUBAR / CU - IZOLATOR 3P, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",444.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206215","AlCu/Cu - 3P, isolateur L1200, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W1200, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1200, VERT. REGUL. PROF. PASO 105mm","ALCUBAR / CU - 3P SZIGETELŐ, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20622","ALCUBAR / CU - IZOLATOR 3P, W1300, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",457,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206222","AlCu/Cu - 3P, isolateur L1300, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W1300, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1300, VERT. REGUL. PROF. PASO 105mm","ALCUBAR / CU - 3P SZIGETELŐ, W1300, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20625","ALCUBAR / CU - IZOLATOR 3P, W450, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",388.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20625","SZT","85469010",null,null,"5901988206253","AlCu/Cu - 3P, isolateur L450, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W450, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W450, VERTIC. REG. PROF. PASO 105MM","ALCUBAR / CU - 3P SZIGETELŐ, W450, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20626","ALCUBAR / CU - IZOLATOR 3P, W600, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",393.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206260","AlCu/Cu - 3P, isolateur L600, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W600, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W600, VERT. REGUL. PROF. PASO 105mm","ALCUBAR / CU - 3P SZIGETELŐ, W600, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20627","ALCUBAR / CU - IZOLATOR 3P, W650, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",399.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20627","SZT","85469010",null,null,"5901988206277","AlCu/Cu - 3P, isolateur L650, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W650, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W650, VERTIC. REG. PROF. PASO 105MM","ALCUBAR / CU - 3P SZIGETELŐ, W650, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20628","ALCUBAR / CU - IZOLATOR 3P, W800, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",412.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206284","AlCu/Cu - 3P, isolateur L800, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W800, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W800, VERT. REGUL. PROF. PASO 105mm","ALCUBAR / CU - 3P SZIGETELŐ, W800, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20629","ALCUBAR / CU - IZOLATOR 3P, W850, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",421.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20629","SZT","85469010",null,null,"5901988206291","AlCu/Cu - 3P, isolateur L850, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 3P, W850, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 3P, W850, VERTIC. REG. PROF. PASO 105MM","ALCUBAR / CU - 3P SZIGETELŐ, W850, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20630","ALCUBAR / CU - IZOLATOR 4P, W1000, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",517.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206307","AlCu/Cu - 4P, isolateur L1000, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W1000, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1000, VERT. REGUL. PROF. PASO 105mm","AlCubar / CU - SZIGETELŐ 4P, W1000, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20631","ALCUBAR / CU - IZOLATOR 4P, W1200, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",529.79999999999995,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206314","AlCu/Cu - 4P, isolateur L1200, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W1200, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1200, VERT. REGUL. PROF. PASO 105mm","ALCUBAR / CU - 4P SZIGETELŐ, W1200, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20632","ALCUBAR / CU - IZOLATOR 4P, W1300, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",541,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206321","AlCu/Cu - 4P, isolateur L1300, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W1300, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1300, VERT. REGUL. PROF. PASO 105mm","AlCubar / CU - SZIGETELŐ 4P, W1300, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20636","ALCUBAR / CU - IZOLATOR 4P, W600, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",478.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206369","AlCu/Cu - 4P, isolateur L600, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W600, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W600, VERT. REGUL. PROF. PASO 105mm","AlCubar / CU - SZIGETELŐ 4P, W600, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20637","ALCUBAR / CU - IZOLATOR 4P, W650, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",482.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20637","SZT","85469010",null,null,"5901988206376","AlCu/Cu - 4P, isolateur L650, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W650, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W650, VERTIC. REG. PROF. PASO 105MM","ALCUBAR / CU - 4P SZIGETELŐ, W650, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20638","ALCUBAR / CU - IZOLATOR 4P, W800, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",497.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206383","AlCu/Cu - 4P, isolateur L800, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W800, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W800, VERT. REGUL. PROF. PASO 105mm","AlCubar / CU - SZIGETELŐ 4P, W800, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105MM"]
["20639","ALCUBAR / CU - IZOLATOR 4P, W850, PIONOWO, REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 105MM",506.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20639","SZT","85469010",null,null,"5901988206390","AlCu/Cu - 4P, isolateur L850, vertical, réglable en profondeur, distance 105mm","AlCu/Cu - Insulator 4P, W850, Vertically, adjustable depth, spacing 105mm","ALCUB/CU- SOPORTE 4P, W850, VERTIC. REG. PROF. PASO 105MM","ALCUBAR / CU - 4P SZIGETELŐ, W850, FÜGGŐLEGES, ÁLLÍTHATÓ MÉLYSÉG, HELY 105 mm"]
["20640","ALCUBAR / CU - IZOLATOR 3P, W1000, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",433.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206406","AlCu/Cu - 3P, isolateur L1000, dossier/vertical, réglable en hauteur, écartement 105 mm","AlCu/Cu - Insulator 3P, W1000, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1000, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 3P SZIGETELŐ, W1000, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓ, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20641","ALCUBAR / CU - IZOLATOR 3P, W1200, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",444.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206413","AlCu/Cu - 3P, isolateur L1200, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 3P, W1200, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1200, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 3P SZIGETELŐ, W1200, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20642","ALCUBAR / CU - IZOLATOR 3P, W1300, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",457,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206420","AlCu/Cu - 3P, isolateur L1300, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 3P, W1300, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W1300, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","ALCUBAR / CU - 3P SZIGETELŐ, W1300, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20645","ALCUBAR / CU - IZOLATOR 3P, W450, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",388.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20645","SZT","85469010",null,null,"5901988206451","AlCu/Cu - 3P, isolateur L450, dossier/vertical, réglable en hauteur, écartement 105 mm","AlCu/Cu - Insulator 3P, W450, support / Vertical on the back, adjustable height, spacing 105mm","ALCUB/CU- SOPORTE 3P, W450, SOP/VERTIC. REG. ALTURA PASO 105 MM","AlCubar / CU - 3P SZIGETELŐ, W450, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20646","ALCUBAR / CU - IZOLATOR 3P, W600, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",393.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206468","AlCu/Cu - 3P, isolateur L600, dossier/vertical, réglable en hauteur, écartement 105 mm","AlCu/Cu - Insulator 3P, W600, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W600, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 3P SZIGETELŐ, W600, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105 mm-es tér"]
["20647","ALCUBAR / CU - IZOLATOR 3P, W650, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",399.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20647","SZT","85469010",null,null,"5901988206475","AlCu/Cu - 3P, isolateur L650, dossier/vertical, réglable en hauteur, écartement 105 mm","AlCu/Cu - Insulator 3P, W650, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W650, SOP/VERTIC. REG. ALTURA PASO 105 MM","AlCubar / CU - 3P SZIGETELŐ, W650, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20648","ALCUBAR / CU - IZOLATOR 3P, W800, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",412.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206482","AlCu/Cu - 3P, isolateur L800, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 3P, W800, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W800, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 3P SZIGETELŐ, W800, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105 mm-es tér"]
["20649","ALCUBAR / CU - IZOLATOR 3P, W850, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",421.1,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20649","SZT","85469010",null,null,"5901988206499","AlCu/Cu - 3P, isolateur L850, dossier/vertical, réglable en hauteur, écartement 105 mm","AlCu/Cu - Insulator 3P, W850, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 3P, W850, SOP/VERTIC. REG. ALTURA PASO 105 MM","AlCubar / CU - 3P SZIGETELŐ, W850, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105 mm-es tér"]
["20650","ALCUBAR / CU - IZOLATOR 4P, W1000, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",517.4,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206505","AlCu/Cu - 4P, isolateur L1000, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 4P, W1000, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1000, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","ALCUBAR / CU - 4P SZIGETELŐ, W1000, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20651","ALCUBAR / CU - IZOLATOR 4P, W1200, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",529.79999999999995,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206512","AlCu/Cu - 4P, isolateur L1200, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 4P, W1200, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1200, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm105 mm","AlCubar / CU - 4P SZIGETELŐ, W1200, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20652","ALCUBAR / CU - IZOLATOR 4P, W1300, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",541,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206529","AlCu/Cu - 4P, isolateur L1300, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 4P, W1300, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 4P, W1300, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 4P SZIGETELŐ, W1300, TÁMASZTÁS/FÜGGŐLEGES HÁTÁN, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20656","ALCUBAR / CU - IZOLATOR 4P, W600, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",478.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206567","AlCu/Cu - 4P, isolateur L600, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 4P, W600, support / Vertical on the back, adjustable height, spacing 105mm","ALCUB/CU- SOPORTE 4P, W600, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 4P SZIGETELŐ, W600, TÁMASZTÁS/FÜGGŐLEGES HÁTÁN, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20657","ALCUBAR / CU - IZOLATOR 4P, W650, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",482.7,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20657","SZT","85469010",null,null,"5901988206574","AlCu/Cu - 4P, isolateur L650, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 4P, W650, support / Vertical on the back, adjustable height, spacing 105mm","ALCUB/CU- SOPORTE 4P, W650, SOP/VERTIC. REG. ALTURA PASO 105 MM","AlCubar / CU - 4P SZIGETELŐ, W650, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["20658","ALCUBAR / CU - IZOLATOR 4P, W800, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",497.3,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85469010",null,null,"5901988206581","AlCu/Cu - 4P, isolateur L800, dossier/vertical, réglable en hauteur, distance 105mm","AlCu/Cu - Insulator 4P, W800, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 4P, W800, VERT. POSTERIOR, REGUL. ALTURA, PASO 105mm","AlCubar / CU - 4P SZIGETELŐ, W800, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105 mm-es tér"]
["20659","ALCUBAR / CU - IZOLATOR 4P, W850, PODPORA/PIONOWO NA PLECACH, REGULOWANA WYSOKOŚĆ, ROZSTAW 105MM",506.2,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","20659","SZT","85469010",null,null,"5901988206598","AlCu/Cu - 4P, isolateur L850, dossier/vertical, réglable en hauteur, espacement 105mm","AlCu/Cu - Insulator 4P, W850, support / Vertical on the back, height adjustable, spacing 105mm","ALCUB/CU- SOPORTE 4P, W850, SOP/VERTIC. REG. ALTURA DIST. 105 MM","AlCubar / CU - 4P SZIGETELŐ, W850, TÁMASZTÁS/FÜGGŐLEGES HÁTSÓL, ÁLLÍTHATÓ MAGASSÁG, 105MM HELY"]
["21000","OE - Udarowa przekładnia kątowa 1/4\" Milwaukee + zestaw 10 bitów",140.4,null,null,null,"OE_ACCESSORIES",null,null,"8483405190",null,null,"4058546289027"]
["21001","OE - Bit TX25, 25mm - 1szt.",3,null,null,null,"OE_ACCESSORIES",null,null,"8483405190",null,null,"4002395385423"]
["21076","ZENERGY OM - SZYNA PE W600, L=470 MM, 20 ZACISKÓW 16MM2 + 1 X M6",75.599999999999994,"1-ZE-19",1.6833333333333333,8,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988210762","OM - RAIL PE L600, L=470 MM, 20 BORNES 16MM2 + 1 X M6","OM - PE RAIL W600, L=470 mm, 20 TERMINALS 16mm2 + 1 X M6","*OM - CARRIL PE W600, L=470 MM, 20 TERMINALES 16MM2 + 1 X M6","ZENERGY OM - PE RAIL W600, L=470 MM, 20 TERMINÁL 16MM2 + 1 X M6"]
["21077","ZENERGY OM - SZYNA PE W800, L=470 MM, 20 ZACISKÓW 16MM2 + 1 X M6",101.5,"1-ZE-19",1.6666666666666666E-2,1,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988210779","OM - RAIL PE L800, L=470 MM, 20 BORNES 16MM2 + 1 X M6","OM - PE RAIL W800, L=470 mm, 20 TERMINALS 16mm2 + 1 X M6","*OM - CARRIL PE W800, L=470 MM, 20 TERMINALES 16MM2 + 1 X M6","ZENERGY OM - PE RAIL W800, L=470 MM, 20 TERMINÁL 16MM2 + 1 X M6"]
["21092","ALCUBAR OM - WSPORNIK IZOLATORA SW04300, MOST POZIOMY NA PLECACH - 1 SZT.",49,"1-ZE-08",9.166666666666666E-2,2,"OM_SUPPORT","21092","SZT","85389099","27.12.40.0",null,"5901988210922","AlCubar OM - Support isolant SW04300, pont horizontal ? l'arri?re - 1 pc.","AlCubar OM - Insulator support SW04300, Horizontal bridge on the back - 1 pc.","SOPORTE PARA SW04300 HORIZ. 1UND","ALCUBAR OM - SZIGETELŐ KONZER SW04300, VÍZSZINTES HÍD A HÁTRA - 1 DB."]
["21093","ALCUBAR OM - WSPORNIK IZOLATORA SW04300, W400, MOST PIONOWY NA PLECACH - 1 SZT.",49,"1-ZE-08",null,null,"OM_SUPPORT","21093","SZT","85389099","27.90.12.0",null,"5901988210939","AlCubar OM - Support isolant SW04300, L400, pont vertical ? l'arri?re - 1 pc.","AlCubar OM - Insulator support SW04300, W400, Vertical bridge on the back - 1 pc.","SOPORTE PARA SW04300 VERT. 1UND","ALCUBAR OM - SZIGETELŐ KONZER SW04300, W400, P HÍDION A HÁTSON - 1 DB."]
["21094","ALCUBAR / CU - IZOLATOR WSPORCZY SW04300 4P - 1 SZT.",89.5,"1-ZE-08",null,null,"OM_SUPPORT","21094","SZT","85389099","27.90.12.0",null,"5901988210946","AlCubar OM - Isolant de poteau AlCubar SW04300 4P - 1 pi?ce","AlCubar OM / Cu - Post insulator SW04300 4P - 1 pc.","ALCUB- OM/CU- SOPORTE POSTE SW04300 4P- 1 UD.","ALCUBAR / CU - POST SZIGETELŐ SW04300 4P - 1 DB."]
["21097","ALCUBAR OM - WSPORNIK IZOLATORA ZENE39200, MOST POZIOMY - 1 SZT.",45.6,"1-ZE-08",null,null,"OM_SUPPORT","21097","SZT","85389099","27.90.12.0",null,"5901988210977","AlCubar OM - Support isolant ZENE39200, pont horizontal - 1 pc.","ALCUBAR OM - INSULATOR SUPPORT ZENE39200, Horizontal BRIDGE - 1 PC.","ALCUB- OM- SOPORTE AISLADOR ZENE39200, EMB. HORIZ. 1 UD.","ALCUBAR OM - ZENE39200 SZIGETELŐ KONZER, VÍZSZINTES HÍD - 1 DB."]
["21098","ALCUBAR OM - WSPORNIK IZOLATORA ZENE39200, W400, MOST PIONOWY - 1 SZT.",45.6,"1-ZE-08",null,null,"OM_SUPPORT","21098","SZT","85389099","27.90.12.0",null,"5901988210984","AlCubar OM - Support isolant ZENE39200, L400, pont vertical - 1 pc.","ALCUBAR OM - INSULATOR BRACKET ZENE39200, W400, Vertical BRIDGE - 1 PC.","ALCUB- OM- SOPORTE AISLADOR ZENE39200, W400, EMB. VERTIC.- 1 UD.","ALCUBAR OM - SZIGETELŐ KONZER ZENE39200, W400, FÜGGŐLEGES HÍD - 1 DB."]
["21129","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, DLA IZOLATORA SW04300, POLIWĘGLAN 15X275X2000MM",340.3,"1-ZE-08",null,null,"OM_SUPPORT","21129","SZT","85389099","27.12.40.0",null,"5901988211295","AlCu - couvre-pont AlCubar H27, pour isolateur SW04300, polycarbonate 20x275x2000mm","AlCu - Bridge cover AlCubar H27, for insulator SW04300, polycarbonate 15x275x2000mm","TAPA PROTECC. PARA PROMET-DIS L=500MM","ALCUBAR - ALCUBAR H27 HÍDBURKOLAT, SW04300 SZIGETELŐHEZ, POLIKARBONÁT 15X275X2000MM"]
["21130","ALCUBAR OM - WSPORNIK OSŁONY MOSTU ALCUBAR H27 (SW04300) - 1 SZT.",11.1,"1-ZE-08",0.11666666666666667,1,"OM_SUPPORT","21130","SZT","85389099","27.12.40.0",null,"5901988211301","AlCubar OM - Support de couvre-pont AlCubar H27 (SW04300) - 1 pi?ce","AlCubar OM - AlCubar H27 bridge cover bracket (SW04300) - 1 pc.","SOPORTE PARA TAPA PROTECC. PROMET-DIS","ALCUBAR OM - ALCUBAR H27 HÍDBURKOLAT (SW04300) - 1 DB."]
["21197","ALCUBAR - IZOLATOR 630A 4P, MOST PIONOWY NA PLECACH REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 50MM + WSPORNIKI",185.7,"1-ZE-08",0.15833333333333333,1,"OE_INSULATOR_WIDTH","21197","SZT",null,null,"240830RT","5901988211974",null,null,null,"AlCubar - SZIGETELŐ 630A 4P, FÜGGŐLEGES HÍD A HÁTÁN, ÁLLÍTHATÓ MÉLYSÉG, HELY 50MM + TÁMASZOK"]
["21198","ALCUBAR - IZOLATOR 630A 3P, MOST PIONOWY NA PLECACH REGULOWANA GŁĘBOKOŚĆ, ROZSTAW 75MM + WSPORNIKI",145.6,"1-ZE-08",null,null,"OE_INSULATOR_WIDTH","21198","SZT",null,null,"240830RT","5901988211981",null,null,null,"AlCubar - SZIGETELŐ 630A 3P, FÜGGŐLEGES HÍD A HÁTSON, ÁLLÍTHATÓ MÉLYSÉG, HELY 75MM + TÁMASZOK"]
["21900","OE - Nakrętka M3, biały ocynk, kl.8.8, DIN 934 - 100 szt.",2.7,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M3 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21901","OE - Nakrętka M4, biały ocynk, kl.8.8, DIN 934 - 100 szt.",4.5999999999999996,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M4 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21902","OE - Nakrętka M5, biały ocynk, kl.8.8, DIN 934 - 100 szt.",6,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M5 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21903","OE - Nakrętka M6, biały ocynk, kl.8.8, DIN 934 - 100 szt.",7.3,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M6 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21904","OE - Nakrętka M8, biały ocynk, kl.8.8, DIN 934 - 100 szt.",16.2,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M8 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21905","OE - Nakrętka M10, biały ocynk, kl.8.8, DIN 934 - 100 szt.",36.700000000000003,"1-ZE-01",0.01,1,null,null,"P","73181595",null,null,null,null,null,null,"OE - M10 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21906","OE - Nakrętka M12, biały ocynk, kl.8.8, DIN 934 - 100 szt.",51.8,"1-ZE-01",0.01,1,null,null,"P","73181595",null,null,null,null,null,null,"OE - M12 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21907","OE - Nakrętka M16, biały ocynk, kl.8.8, DIN 934 - 100 szt.",110.2,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M16 anya, fehérre horganyzott, 8.8 osztály, DIN 934 - 100 db."]
["21913","OE - Nakrętka M6 z kołnierzem ząbkowanym, biały ocynk, kl.8.8, DIN 6923 - 100 szt.",15.8,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M6 anya fogazott gallérral, fehérre horganyzott, 8.8 osztály, DIN 6923 - 100 db."]
["21914","OE - Nakrętka M8 z kołnierzem ząbkowanym, biały ocynk, kl.8.8, DIN 6923 - 100 szt.",28.1,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M8-as anya fogazott gallérral, fehérre horganyzott, 8.8 osztály, DIN 6923 - 100 db."]
["21915","OE - Nakrętka M10 z kołnierzem ząbkowanym, biały ocynk, kl.8.8, DIN 6923 - 100 szt.",47.5,"1-ZE-01",null,null,null,null,"P","73181595",null,null,null,null,null,null,"OE - M10-es anya fogazott gallérral, fehérre horganyzott, 8.8 osztály, DIN 6923 - 100 db."]
["21930","OE - Śruba M8x12, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",65.900000000000006,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219307"]
["21931","OE - Śruba M8x16, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",75.599999999999994,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219314"]
["21932","OE - Śruba M8x20, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",88.6,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219321"]
["21933","OE - Śruba M8x25, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",95,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219338"]
["21934","OE - Śruba M8x30, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",97.2,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219345"]
["21935","OE - Śruba M8x35, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",114.5,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219352"]
["21936","OE - Śruba M8x40, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",151.19999999999999,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219369"]
["21941","OE - Śruba M10x16, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",130.69999999999999,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219413"]
["21944","OE - Śruba M10x30, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",170.6,"1-ZE-01",0.01,1,null,null,null,"73181575",null,null,"5901988219444"]
["21948","OE - Śruba M10x50, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",237.6,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219482"]
["21951","OE - Śruba M10x65, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",298.10000000000002,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219512"]
["21954","OE - Śruba M10x100, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",518.4,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219543"]
["21955","OE - Śruba M10x120, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",637.20000000000005,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219550"]
["21960","OE - Śruba M12x30, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",172.8,"1-ZE-01",0.01,1,null,null,null,"73181575",null,null,"5901988219604"]
["21964","OE - Śruba M12x50, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",334.8,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219642"]
["21967","OE - Śruba M12x100, DIN 933 biały ocynk kl.8.8  6-kąt  - 100szt.",604.79999999999995,"1-ZE-01",null,null,null,null,null,"73181575",null,null,"5901988219673"]
["22009","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 9M,  W1200 H550 D230, WISZĄCA",629.6,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988220099","OM - Boîtier de base IP30, 9M, L1200 H550 P230, suspendu","OM - Basic housing IP30, 9M, W1200 H550 D230, hanging","OM- ARMARIO METAL. IP30, 9M, W1200 H550 D230, MURAL","ZENERGY OM - ALAP HÁZ IP30, 9M, W1200 H550 D230, FÜGG."]
["22021","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 21M,  W1200 H1150 D230, WISZĄCA",827.3,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988220211","OM - Boîtier de base IP30, 21M, L1200 H1150 P230, suspendu","OM - Basic housing IP30, 21M, W1200 H1150 D230, hanging","OM- ARMARIO METAL. IP30, 21M, W1200 H1150 D230, MURAL","ZENERGY OM - ALAP HÁZ IP30, 21M, W1200 H1150 D230, FÜGG."]
["22028","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 28M,  W1200 H1600 D230, COKÓŁ 100MM",1471,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988220280","OM - Boîtier de base IP30, 28M, L1200 H1600 P230, base 100mm","OM - Basic housing IP30, 28M, W1200 H1600 D230, plinth 100mm","OM- ARMARIO METAL. IP30, 28M, W1200 H1600 D230, ZOCALO 100mm","ZENERGY OM - ALAP HÁZ IP30, 28M, W1200 H1600 D230, lábazat 100mm"]
["22033","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 33M,  W1200 H1850 D230, COKÓŁ 100MM",1932.1,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988220334","OM - Boîtier de base IP30, 33M, L1200 H1850 P230, base 100mm","OM - Basic enclosure IP30, 33M, W1200 H1850 D230, plinth 100mm","OM- ARMARIO METAL. IP30, 33M, W1200 H1850 D230, ZOCALO 100 mm","ZENERGY OM - ALAP HÁZ IP30, 33M, W1200 H1850 D230, lábazat 100mm"]
["22036","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 36M,  W1200 H2000 D230, COKÓŁ 100MM",2072.5,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988220365","OM - Boîtier de base IP30, 36M, L1200 H2000 P230, base 100mm","OM - Basic housing IP30, 36M, W1200 H2000 D230, plinth 100mm","OM- ARMARIO METAL. IP30, 36M, W1200 H2000 D230, ZOCALO 100 mm","ZENERGY OM - ALAP HÁZ IP30, 36M, W1200 H2000 D230, lábazat 100mm"]
["22041","ZENERGY OM - SZYNA PROSTA, TYŁ, TS-35D, (H=15MM), W600",32.799999999999997,"1-ZE-09",0.38333333333333336,5,"OM_RAIL_DIN","22041","SZT","85389099","27.12.40.0",null,"5901988220419","OM - Rail droit, arrière, TS-35D, (h = 15mm), L600","OM - Straight rail, rear, TS-35D, (h = 15mm), W600","OM- CARRIL RECTO, FONDO, TS-35D, (H=15MM), W600","ZENERGY OM - EGYENES SÍN, HÁTSÓ, TS-35D, (H=15MM), W600"]
["22045","ZENERGY OM - PŁYTA MONTAŻOWA + OSŁONA ROZŁĄCZNIK SKRZYNKOWY 1X EFEN250 + 6X EFEN 160, W1000, 9M, PIONOWO",455.8,"1-ZE-01",null,null,"OM_FUSE_PLATES",null,"SZT","85389099",null,null,"5901988220457","OM - Plaque de montage + boîtier de protection, boîte de commutation 1x EFEN250 + 6x EFEN 160, L1000, 9M, vertical","OM - Mounting plate + cover switch box 1x EFEN250 + 6x EFEN 160, W1000, 9M, Vertical","OM- PLACA MONTAJE + TAPA BASE PORTAFUSIBLES  1X250 + 6X160, W1000, 9M,","ZENERGY OM - SZERELŐLEMEZ + FEDŐDOBOZ KAPCSOLÓ 1X EFEN250 + 6X EFEN 160, W1000, 9M, FÜGGŐLEGES"]
["22048","ZENERGY OM - PŁYTA MONTAŻOWA + OSŁONA ROZŁĄCZNIK SKRZYNKOWY 4X EFEN250, W1000, 9M, PIONOWO",307.10000000000002,"1-ZE-01",null,null,"OM_FUSE_PLATES",null,"SZT","85389099",null,null,"5901988220488","OM - Plaque de montage + boîtier de protection, boîtier de commutation 4x EFEN250, L1000, 9M, vertical","OM - Mounting plate + cover box switch box 4x EFEN250, W1000, 9M, Vertical","OM- PLACA MONTAJE + TAPA BASE PORTAFUSIBLES  4X250, W1000, 9M, VERT.","ZENERGY OM - SZERELŐLEMEZ + FEDŐDOBOZ KAPCSOLÓ 4X EFEN250, W1000, 9M, FÜGGŐLEGES"]
["22053","ZENERGY OM - SZYNA APARATURY MODUŁOWEJ TS-35D, W300",26.3,"1-ZE-09",null,null,"OM_RAIL_DIN","22053","SZT","85389099","27.12.40.0",null,"5901988220532","OM - Rail pour appareils modulaires TS-35D, L300","OM - Modular apparatus rail TS-35D, W300","OM-CARRIL DIN FIJO, W300, 7 MOD. COMPLETO","ZENERGY OM - MODULÁRIS BERENDEZÉS SÍN TS-35D, W300"]
["22059","ZENERGY OM - SZYNA APARATURY MODUŁOWEJ TS-35D, W1000",42.1,"1-ZE-09",0.25,5,"OM_RAIL_DIN","22059","SZT","85389099","27.12.40.0",null,"5901988220594","OM - Rail d'équipement modulaire TS-35D, L1000","OM - TS-35D, W1000 modular equipment rail","OM-CARRIL DIN FIJO, W1000 46 MOD. COMPLETO","ZENERGY OM - MODULÁRIS BERENDEZÉS SÍN TS-35D, W1000"]
["22061","ZENERGY OM - DWIE WKŁADKI DO ZAMKA TYPU PIÓRKO",54.4,"1-ZE-09",0.3,4,"OM_SUPPORT","22061","SZT","85389099","27.12.40.0",null,"5901988220617","OM - Deux inserts pour le type de plume","OM - Two feather lock inserts","OM- CIERRE DOBLE PELETON 2UDS","ZENERGY OM - KÉT BETÉT EGY TOLLCSIPZÁRHOZ"]
["22064","ZENERGY OM - SZYNA REGULOWANA APARATURY MODUŁOWEJ TS-35D, W400",40,"1-ZE-09",0.01,1,"OM_RAIL_DIN","22064","SZT","85389099","27.12.40.0",null,"5901988220648","OM - Rail réglable d'appareil modulaire TS-35D, L400","OM - Adjustable rail for modular equipment TS-35D, W400","OM- CARRIL DIN REGUL. PROF. W400","ZENERGY OM - ÁLLÍTHATÓ SÍN MODULÁRIS BERENDEZÉSEKHEZ TS-35D, W400"]
["22069","ZENERGY OM - SZYNA REGULOWANA APARATURY MODUŁOWEJ TS-35D, W1000",59.5,"1-ZE-09",0.1,4,"OM_RAIL_DIN","22069","SZT","85389099","27.12.40.0",null,"5901988220693","OM - Rail réglable d'appareil modulaire TS-35D, L1000","OM - Adjustable rail for modular devices TS-35D, W1000","OM- CARRIL DIN REGUL. PROF. W1000","ZENERGY OM - ÁLLÍTHATÓ SÍN MODULÁRIS BERENDEZÉSEKHEZ TS-35D, W1000"]
["22072","ZENERGY OM - DRABINKA KABLOWA - W600",52.4,"1-ZE-09",2.6,6,"OM_SUPPORT","22072","SZT","85389099","27.12.40.0",null,"5901988220723","OM - Échelle à câbles - L600","OM - Cable ladder - W600","OM- SOPORTE FIJACION CABLES -W600","ZENERGY OM - KÁBELLÉTRA - W600"]
["22076","ZENERGY OM - SZYNA PE W600, L=470 MM, 40 ZACISKÓW 16MM2 + 1xM6",95.1,"1-ZE-19",6.6,8,"OM_SUPPORT","22076","SZT","85389099","27.12.40.0",null,"5901988220761","OM - Rail PE, L = 470 mm, 40 bornes 16 mm2 + 1 x M6","OM - PE rail W600, L = 470 mm, 40 terminals 16mm2 + 1 x M6","*OM- Barra PE para armario W=600","ZENERGY OM - PE RAIL W600, L=470 MM, 40 TERMINÁL 16MM2 + 1xM6"]
["22079","ZENERGY OM - DWA IZOLATORY TORU NEUTRALNEGO, DO REFERENCJI 22075-78",22.4,"1-ZE-09",1.8,7,"OM_SUPPORT","22079","SZT","85389099","27.12.40.0",null,"5901988220792","OM - Deux isolateurs de voie neutres, références 22075-78","OM - Two Neutral Insulators, for reference 22075-78","OM- AISLADORES PARA NEUTRO PARA REF. 22075-78 2UDS.","ZENERGY OM - KÉT SEMÜLT SZIGETELŐ, REFERENCIA 22075-78"]
["22082","ZENERGY OM - SZEROKI WSPORNIK KORYTKA KABLOWEGO H30mm",15.1,"1-ZE-09",null,null,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988220822","OM - Support de chemins de câbles large","OM - The wide bracket of the cable tray","OM- SOPORTE ANCHO PARA CANALETA","ZENERGY OM - SZÉLES KÁBELTÁLCA TARTÓ H30mm"]
["22086","ZENERGY OM - CEOWNIK KORYTKA KABLOWEGO W800",14.1,"1-ZE-09",0.11666666666666667,1,"OM_SUPPORT","22086","SZT","85389099","27.12.40.0",null,"5901988220860","OM - Canal du chemin de câbles L800","OM - W800 cable tray channel","OM- CARRIL PARA CANALETA HORIZ. W800","ZENERGY OM - a W800 KÁBELTÁLCA vezérigazgatója"]
["22089","ZENERGY OM - WSPORNIK PŁYT MONTAŻOWYCH, REGULOWANYCH D230 - 1 SZT.",10.1,"1-ZE-09",9.6,2,"OM_SUPPORT","22089","SZT","85389099","27.12.40.0",null,"5901988220891","OM - Support de plaque de support, réglable - 1 pièce","OM - Bracket for Mounting plates, adjustable D230 - 1 pc.","OM- SOPORTE PARA PLACA MONTAJE, REGUL. - 1 UDS.","ZENERGY OM - ÁLLÍTHATÓ SZERELŐLEMEZEK TÁMOGATÁS D230 - 1 DB."]
["22090","ALCUBAR OM - IZOLATOR 630A 3P, W400, MOST PIONOWY NA PLECACH",124.1,"1-ZE-08",null,null,"OM_SUPPORT",null,"SZT","85389099","27.90.12.0",null,"5901988220907","AlCubar OM - Isolateur 630A 3P, L400, pont vertical à l'arrière","AlCubar OM - Insulator 630A 3P, W400, Vertical bridge on the back","ALCUB- OM - SOPORTE  630A 3P, W400, FONDO  ","ALCUBAR OM - ISOLATOR 630A 3P, W400, FÜGGŐLEGES HÍD A HÁTSON"]
["22093","ALCUBAR OM - IZOLATOR 630A 3P, W1000, MOST PIONOWY NA PLECACH",140.19999999999999,"1-ZE-08",null,null,"OM_SUPPORT",null,"SZT","85389099","27.90.12.0",null,"5901988220938","AlCubar OM - Isolateur 630A 3P, L1000, pont vertical à l'arrière","AlCubar OM - 630A 3P insulator, W1000, Vertical bridge on the back","ALCUB- OM - SOPORTE 630A 3P, W1000, EMBARRADO VERT. FONDO","ALCUBAR OM - ISOLATOR 630A 3P, W1000, FÜGGŐLEGES HÍD A HÁTSON"]
["22096","ALCUBAR OM - IZOLATOR 630A 4P, W800, MOST PIONOWY NA PLECACH",176.6,"1-ZE-08",null,null,"OM_SUPPORT",null,"SZT","85389099","27.90.12.0",null,"5901988220969","AlCubar OM - Isolateur 630A 4P, L800, pont vertical à l'arrière","AlCubar OM - Insulator 630A 4P, W800, Vertical bridge on the back","ALCUB- OM - SOPORTE  630A 4P, W800, FONDO  ","ALCUBAR OM - ISOLATOR 630A 4P, W800, FÜGGŐLEGES HÍD A HÁTSON"]
["22100","ZENERGY OM-VSD - PROFIL PRZEDZIAŁU KABLOWEGO L1950MM",192.1,"1-ZE-09",null,null,"OM_VSD_PLATES","22100","SZT","85389099",null,null,"5901988221003","OM-VSD - Profil du compartiment à câbles L1950mm","OM-VSD - Cable compartment profile L1950mm","OM-VSD- PERFIL DE COMPARTIMENTO DE CABLES L1950MM","ZENERGY OM-VSD - KÁBELREKESZ PROFIL L1950MM"]
["22103","ZENERGY OM-VSD - DWA KĄTOWNIKI BOCZNE DO ZENERGY OM D300 L1950MM",100.6,"1-ZE-09",null,null,"OM_VSD_PLATES","22103","SZT","85389099",null,null,"5901988221034","OM-VSD - Deux angles latéraux pour Zenergy OM P300 L1950mm","OM-VSD - Two side angles for Zenergy OM D300 L1950mm","OM-VSD- DOS ÁNGULOS LATERALES PARA OM D300 L1950MM","ZENERGY OM-VSD - KÉT OLDALSZÖG A ZENERGY OM D300 L1950MM-hez"]
["22106","ZENERGY OM-VSD - ZESTAW WSPORNIKA DO ZENERGY OM POKRYWA TYLNA W600 X D300",85.2,"1-ZE-09",null,null,"OM_VSD_PLATES","22106","SZT","85389099",null,null,"5901988221065","OM-VSD - Kit de fixation Zenergy OM Couvercle arrière L600 x P300","OM-VSD - Bracket kit for Zenergy OM Back cover W600 x D300","OM-VSD- KIT DE SOPORTE PARA ZENERGY OM PANEL TRASERO W600XD300","ZENERGY OM-VSD - KONZER KÉSZLET ZENERGY OM HÁTSÓ BURKOLATHOZ W600 X D300"]
["22110","ZENERGY OM-VSD - DOCISK PRZEDZIAŁU KABLOWEGO PROSTY",14,"1-ZE-09",null,null,"OM_VSD_PLATES",null,"SZT","85389099",null,null,"5901988221102","OM-VSD - Compartiment de câble pression simple","OM-VSD - Straight cable compartment clamp","OM-VSD - ABRAZADERA RECTA PARA COMPARTIMENTO DE CABLES","ZENERGY OM-VSD - EGYENES KÁBELREKESZ BIZTOSÍTÓ"]
["22113","ZENERGY OM - SZYNA PE, 12 ZACISKÓW 10MM2",20.5,"1-ZE-19",null,null,"OM_SUPPORT",null,"SZT","85389099",null,null,"5901988221133","OM - rail PE, 12 bornes 10mm2","OM - PE rail, 12 terminals 10mm2","OM- Carril PE, 12 terminales 10mm2","ZENERGY OM - PE RAIL, 12 TERMINÁL 10MM2"]
["22114","Zenergy OM-VSD - Wspornik profili pionowych dla OM Pokrywa tylna D230 L1950mm Slim",70.400000000000006,"1-ZE-09",null,null,"OM_VSD_PLATES","22114","SZT","85389099",null,null,"5901988221140","OM-VSD - Support profilé vertical pour OM Capot arrière Svelte L800 x P230","OM-VSD - Vertical profile support for OM Back cover W800 x D230 Slim","OM-VSD- SOPORTE DE PERFIL VERTIC. PARA OM PANEL TRASERO W800XD230 ","Zenergy OM-VSD - Függőleges profil támogatás az OM hátsó burkolathoz D230 L1950mm Slim"]
["22122","Zenergy OM-VSD - Płyta przedziału kablowego L1950mm Slim&Simple",98.6,"1-ZE-09",null,null,"OM_VSD_PLATES","22122","SZT","85389099",null,null,"5901988221225","OM-VSD - Deux angles latéraux pour Zenergy OM L1950mm Svelte&Simples L800 ","OM-VSD - Cable compartment plate L1950mm W800 Slim & Simple","OM-VSD- PLACA DE COMPARTIMENTO DE CABLES L1950MM W800 ","Zenergy OM-VSD - Kábeltartó lemez L1950mm Slim&Simple"]
["22158","ZENERGY OM - SZYNA APARATURY MODUŁOWEJ TS-35D, W800 D300",43.9,"1-ZE-09",1.5833333333333333,5,"OM_RAIL_DIN","22158","SZT","85389099","27.12.40.0",null,"5901988221584","OM - Bus d'équipement modulaire TS-35D, L800 P300","OM - Modular apparatus rail TS-35D, W800 D300","OM- CARRIL MODULAR PARA APARATOS TS-35D, W800 D300","ZENERGY OM - MODULÁRUS BERENDEZÉS BUSZ TS-35D, W800 D300"]
["22168","ZENERGY OM - SZYNA REGULOWANA APARATURY MODUŁOWEJ TS-35D, W800 D300",60.6,"1-ZE-09",0.39166666666666666,7,"OM_RAIL_DIN","22168","SZT","85389099","27.12.40.0",null,"5901988221683","OM - Rail réglable pour équipement modulaire TS-35D, L800 P300","OM - Adjustable rail for modular devices TS-35D, W800 D300","OM- CARRIL DIN REG. PROF. TS-35D, W800 D300","ZENERGY OM - ÁLLÍTHATÓ SÍN MODULÁRUS BERENDEZÉSEKHEZ TS-35D, W800 D300"]
["22181","ZENERGY OM - WSPORNIK KORYTKA KABLOWEGO H30mm - 2 RAMIONA",10.5,"1-ZE-09",1.6666666666666666E-2,1,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988221812","OM - Support de chemin de câbles - 2 bras","OM - Cable tray bracket - 2 arms","OM- Soporte para bandeja portacables - 2 brazos","ZENERGY OM - KÁBELTÁLCA TARTÓ H30mm - 2 KAROS"]
["22185","ZENERGY OM - WSPORNIK SZYNY PE 22075 - W400 (D230)",41.8,"1-ZE-09",null,null,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988221850","OM - SUPPORT RAIL PE 22075 - L400 (D230)","OM - BAR SUPPORT PE 22075 - W400 (D230)","*OM - SOPORTE RIEL PE 22075 - W400 (D230)","ZENERGY OM - PE RAIL TÁMOGATÁS 22075 - W400 (D230)"]
["22188","ZENERGY OM - WSPORNIK SZYNY PE 22076 - W1000 (D230)",72.3,"1-ZE-09",8.3333333333333329E-2,1,"OM_SUPPORT",null,"SZT","8538909900","27.12.40.0",null,"5901988221881","OM - SUPPORT RAIL PE 22076 - L1000 (D230)","OM - BAR SUPPORT PE 22076 - W1000 (D230)","*OM - SOPORTE RIEL PE 22076 - W1000 (D230)","ZENERGY OM - PE RAIL TÁMOGATÁS 22076 - W1000 (D230)"]
["22197","ZENERGY OM - WSPORNIK SZYNY PE 22076 - W800 (D300)",66.400000000000006,"1-ZE-09",0.55833333333333335,1,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988221973","OM - SUPPORT RAIL PE 22076 - L800 (D300)","OM - BAR SUPPORT PE 22076 - W800 (D300)","*OM - SOPORTE RIEL PE 22076 - W800 (D300)","ZENERGY OM - PE RAIL SUPPORT 22076 - W800 (D300)"]
["22198","ZENERGY OM - WSPORNIK SZYNY PE 22076 - W1000 (D300)",76.3,"1-ZE-09",null,null,"OM_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988221980","OM - SUPPORT RAIL PE 22076 - L1000 (D300)","OM - BAR SUPPORT PE 22076 - W1000 (D300)","*OM - SOPORTE RIEL PE 22076 - W1000 (D300)","ZENERGY OM - PE RAIL TÁMOGATÁS 22076 - W1000 (D300)"]
["22203","ZENERGY OM - PŁYTA MONTAŻOWA W1000 HGM, UCB:100-250 PIONOWO / HGM:100-125, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P POZIOMO",146.30000000000001,"1-ZE-09",null,null,"OM_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988222031","OM - Plaque de montage L1000 HGM, UCB: 100-250 verticalement / HGM:100-125, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P horizontal","OM - Mounting plate W1000 HGM, UCB: 100-250 Vertical / HGM:100-125, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P Horizontal","OM- PLACA MONT. HGM100-250 VERT. / HGM100-125, 160-250 3P; HGP250 3P  W1000 HORIZ.","ZENERGY OM - SZERELŐLEMEZ W1000 HGM, UCB:100-250 FÜGGŐLEGES / HGM:100-125, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P VÍZSZINTES"]
["22206","ZENERGY OM - PŁYTA MONTAŻOWA W1000 HGM, UCB:630-800 PIONOWO / HGM, UCB:630-800 3P POZIOMO",247.5,"1-ZE-09",null,null,"OM_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988222062","OM - Plaque de montage L1000 HGM, UCB: 630-800 verticalement / HGM, UCB: 630-800 3P horizontalement","OM - Mounting plate W1000 HGM, UCB: 630-800 Vertical / HGM, UCB: 630-800 3P Horizontal","OM- PLACA MONTAJE  W1000 HGM 630-800 VERT. HGM,UCB:630-800 3P HORIZ.","ZENERGY OM - SZERELŐLEMEZ W1000 HGM, UCB:630-800 FÜGGŐLEGES / HGM, UCB:630-800 3P VÍZSZINTES"]
["22213","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W1000, 3M / 900",70.2,"1-ZE-09",9.166666666666666E-2,1,"01_PLAIN_COVERS","22213","SZT","85389099","27.12.40.0",null,"5901988222130","OM - Couverture avant complète L1000, 3M / 900","OM - Plain Front cover W1000, 3M / 900","OM- TAPA CIEGA W1000, 3M (H 150MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W1000, 3M / 900"]
["22216","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W1000, 6M / 900",94.7,"1-ZE-09",0.01,1,"01_PLAIN_COVERS","22216","SZT","85389099","27.12.40.0",null,"5901988222161","OM - Couverture avant complète L1000, 6M / 900","OM - Plain Front cover W1000, 6M / 900","OM- TAPA CIEGA W1000, 6M (H 300MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W1000, 6M / 900"]
["22220","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W1000, 10M / 900",152.9,"1-ZE-09",null,null,"01_PLAIN_COVERS","22220","SZT","85389099","27.12.40.0",null,"5901988222208","OM - Écran facial complet L1000, 10M / 900","OM - Plain Front cover W1000, 10M / 900","OM- TAPA CIEGA W1000, 10M (H 500MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W1000, 10M / 900"]
["22223","ZENERGY OM - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 7X EFEN160, W1000 / 900, 6M, PIONOWO",96.7,"1-ZE-09",null,null,"OM_FUSE_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988222239","OM - interrupteur de protection sectionneur 7x EFEN160, L1000 / 900, 6M, vertical","OM - Cover, switch box 7x EFEN160, W1000 / 900, 6M, Vertical","OM- Tapa, caja de interruptores 7x EFN160, W1000 / 900, 6M, VERT.","ZENERGY OM - FEDŐDOBOZ KAPCSOLÓ 7X EFEN160, W1000 / 900, 6M, FÜGGŐLEGES"]
["22226","ZENERGY OM - METALOWA KIESZEŃ NA DOKUMENTACJĘ W400, DLA REF. 22061/22062",46.9,"1-ZE-09",null,null,"OM_SUPPORT","22226","SZT","85389099","27.12.40.0",null,"5901988222260","OM - Pochette en métal pour la documentation L400","OM - Metal document pocket W400, for ref. 22061/22062","OM- PORTADOCUMENTOS MET. L400","ZENERGY OM - FÉM DOKUMENTÁCIÓS ZSEB W400, REF. 22061/22062"]
["22227","ZENERGY OM - METALOWA KIESZEŃ NA DOKUMENTACJĘ W600, DLA REF. 22061/22062",58.5,"1-ZE-09",0.85833333333333328,4,"OM_SUPPORT","22227","SZT","85389099","27.12.40.0",null,"5901988222277","OM - Pochette en métal pour la documentation L600","OM - Metal document pocket W600, for ref. 22061/22062","OM- PORTADOCUMENTOS MET. L600","ZENERGY OM - FÉM DOKUMENTÁCIÓS ZSEB W600, REF. 22061/22062"]
["22231","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W300, 1M / 200",35,"1-ZE-09",null,null,"01_PLAIN_COVERS","22231","SZT","85389099","27.12.40.0",null,"5901988222314","OM - Couverture avant complète L300, 1M / 200","OM - Plain Front cover W300, 1M / 200","OM- TAPA CIEGA W300, 1M (H 50MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W300, 1M / 200"]
["22235","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W300, 5M / 200",47.3,"1-ZE-09",null,null,"01_PLAIN_COVERS","22235","SZT","85389099","27.12.40.0",null,"5901988222352","OM - Couverture avant complète L300, 5M / 200","OM - Plain Front cover W300, 5M / 200","OM- TAPA CIEGA W300, 5M (H 250MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W300, 5M / 200"]
["22238","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W300, 8M / 200",78.900000000000006,"1-ZE-09",null,null,"01_PLAIN_COVERS","22238","SZT","85389099","27.12.40.0",null,"5901988222383","OM - Couverture avant complète L300, 8M / 200","OM - Plain Front cover W300, 8M / 200","OM- TAPA CIEGA W300, 8M (H 400MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W300, 8M / 200"]
["22241","ZENERGY OM - OSŁONA CZOŁOWA PEŁNA W300, 11M / 200",87.6,"1-ZE-09",null,null,"01_PLAIN_COVERS","22241","SZT","85389099","27.12.40.0",null,"5901988222413","OM - Couverture avant complète L300, 11M / 200","OM - Plain Front cover W300, 11M / 200","OM- TAPA CIEGA W300, 11M (H 550MM)","ZENERGY OM - TELJES ELSŐ BURKOLAT W300, 11M / 200"]
["22245","ZENERGY OM - PŁYTA MONTAŻOWA W400 HGM, UCB:400; UPB:400-630 PIONOWO",98,"1-ZE-09",0.1,1,"OM_MCCB_PLATES","22245","SZT","85389099","27.12.40.0",null,"5901988222451","OM - Plaque de montage L400 HGM, UCB: 400; UPB: 400-630 verticalement","OM - Mounting plate W400 HGM, UCB: 400; UPB: 400-630 Vertically","OM- PLACA MONTAJE  W400 HGM 400; UPB:400-630 VERT.","ZENERGY OM - SZERELŐLAP W400 HGM, UCB:400; UPB:400-630 FÜGGŐLEGES"]
["22248","ZENERGY OM - PŁYTA MONTAŻOWA W400 ROZŁĄCZNIK SKRZYNKOWY 2x EFEN 160A, PIONOWO",65.5,"1-ZE-09",4.1666666666666664E-2,1,"OM_FUSE_PLATES","22248","SZT","85389099",null,null,"5901988222482","OM - L400 PLAQUE DE MONTAGE BOÎTE DE DÉCONNEXION 2X EFEN 160A, VERTICAL","OM - W400 Mounting plate DISCONNECT BOX 2X EFEN 160A, Vertical","*OM - W400 PLACA DE MONTAJE CAJA DE DESCONEXIÓN 2X EFEN 160A, VERTICAL","ZENERGY OM - SZERELŐLAP W400 DOBOZ KAPCSOLÓ 2x EFEN 160A, FÜGGŐLEGES"]
["22250","ZENERGY OM - OSŁONA APARATURY MODUŁOWEJ W300, 2M / 200, 7 MOD",41,"1-ZE-09",null,null,"02_DIN_RAIL_COVERS","22250","SZT","85389099","27.12.40.0",null,"5901988222505","OM - Couverture d'appareil modulaire L300, 2M / 150, 7 mod","OM - Modular equipment cover W300, 2M / 200, 7 mod","OM-TAPA MODULAR W300, 2M (H 100MM) 7 MOD","ZENERGY OM - MODULÁRUS BERENDEZÉSBURKOLAT W300, 2M / 200, 7 MOD"]
["22254","ZENERGY OM - OSŁONA APARATURY MODUŁOWEJ W300, 5M / 200, 7 MOD",48.2,"1-ZE-09",null,null,"02_DIN_RAIL_COVERS","22254","SZT","85389099","27.12.40.0",null,"5901988222543","OM - Couverture d'appareil modulaire L300, 5M / 150, 7 mod","OM - Modular equipment cover W300, 5M / 200, 7 mod","OM-TAPA MODULAR W300, 5M (H 250MM) 7 MOD","ZENERGY OM - MODULÁRUS BERENDEZÉSBURKOLAT W300, 5M / 200, 7 MOD"]
["22258","ZENERGY OM - OSŁONA APARATURY MODUŁOWEJ W1000, 4M / 900, 46 MOD",80.3,"1-ZE-09",6.6666666666666666E-2,4,"02_DIN_RAIL_COVERS","22258","SZT","85389099","27.12.40.0",null,"5901988222581","OM - Couverture d'appareil modulaire L1000, 4M / 900, 46 mod","OM - Modular equipment cover W1000, 4M / 900, 46 mod","OM-TAPA MODULAR W1000, 4M (H 200MM) 46 MOD","ZENERGY OM - MODULÁRUS BERENDEZÉSBURKOLAT W1000, 4M / 900, 46 MOD"]
["22262","ZENERGY OM - PŁYTA MONTAŻOWA W600 ROZŁĄCZNIK SKRZYNKOWY 2x EFEN 250A, PIONOWO",95.4,"1-ZE-09",0.05,1,"OM_FUSE_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988222628","OM - Plaque de montage déconnecteur L600 2x EFEN 250A, vertical","OM - Mounting plate W600 box switch disconnector 2x EFEN 250A, Vertical","OM- PLACA MONTAJE CIEGA W600 PARA REGLETAS FUSIBLE 2X250A, VERT.","ZENERGY OM - SZERELŐLEMEZ W600 DOBOZ KAPCSOLÓ 2x EFEN 250A, FÜGGŐLEGES"]
["22265","ZENERGY OM - PŁYTA MONTAŻOWA W600 HGM, UCB:400; UPB:400-630 PIONOWO / HGM, UCB:400 4P; UPB:400-630 4P POZIOMO",137.5,"1-ZE-09",1.6666666666666666E-2,1,"OM_MCCB_PLATES","22265","SZT","85389099","27.12.40.0",null,"5901988222659","OM - Plaque de montage L600 HGM, UCB: 400; UPB: 400-630 verticalement / HGM, UCB: 400 4P; UPB: 400-630 4P horizontal","OM - Mounting plate W600 HGM, UCB: 400; UPB: 400-630 Vertical / HGM, UCB: 400 4P; UPB: 400-630 4P Horizontal","OM- PLACA MONTAJE  W600 HGM 400; UPB:400-630 VERT. HGM 400 4P; UPB:400-63","ZENERGY OM - SZERELŐLAP W600 HGM, UCB:400; UPB:400-630 FÜGGŐLEGES / HGM, UCB:400 4P; UPB:400-630 4P VÍZSZINTES"]
["22268","ZENERGY OM - PŁYTA MONTAŻOWA W600 ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN, SILAS; SCHN LV4 160A + OCHRONNIK, 3M, POZIOMO",79.2,null,null,null,"OM_MCCB_PLATES",null,null,"85389099",null,null,"5901988222680"]
["22278","ZENERGY OM - METALOWA KIESZEŃ NA DOKUMENTACJĘ W800, DLA REF. 22060",68.7,"1-ZE-09",null,null,"OM_SUPPORT","22278","SZT","85389099","27.12.40.0",null,"5901988222789","OM - Pochette métallique pour documentation L800, pour réf. 22060","OM - Metal document pocket W800, for ref. 22060","OM- PORTADOCUMENTOS MET. W800","ZENERGY OM - FÉM DOKUMENTÁCIÓS ZSEB W800, REF. 22060"]
["22281","ZENERGY OM - PŁYTA MONTAŻOWA W800 ROZŁĄCZNIK SKRZYNKOWY 6X EFEN 160A, PIONOWO",115.6,"1-ZE-09",null,null,"OM_FUSE_PLATES","22281","SZT","85389099","27.12.40.0",null,"5901988222819","OM - Plaque de montage déconnexion de boîte L800 6x EFEN 160A, verticale","OM - W800 Mounting plate 6x EFEN 160A box switch disconnector, Vertical","OM- PLACA MONTAJE CIEGA W800 PARA REGLETAS FUSIBLE 6X160A, VERT.","ZENERGY OM - SZERELŐLAP W800 DOBOZ KAPCSOLÓ 6X EFEN 160A, FÜGGŐLEGES"]
["22284","ZENERGY OM - PŁYTA MONTAŻOWA W800 UPB:100-250; HGP250 PIONOWO / HGM, UCB:160-250 4P, 400 3P; UPB:100-250, 400-630 3P; HGP250 POZIOMO",155.1,"1-ZE-09",null,null,"OM_MCCB_PLATES","22284","SZT","85389099","27.12.40.0",null,"5901988222840","OM - Plaque de montage L800 UPB: 100-250 verticalement / HGM, UCB: 160-250 4P, 400 3P; UPB: 100-250, 400-630 3P horizontal","OM - Mounting plate W800 UPB: 100-250 Vertical / HGM, UCB: 160-250 4P, 400 3P; UPB: 100-250, 400-630 3P Horizontal","OM- PLACA MONT. HGP250 VERT. / HGM160-250 4P, 400 3P;  HGP250 W800 HORIZ.","ZENERGY OM - SZERELŐLAP W800 UPB:100-250; HGP250 VERTICAL / HGM, UCB:160-250 4P, 400 3P; UPB: 100-250, 400-630 3P; HGP250 VÍZSZINTES"]
["22285","ZENERGY OM - PŁYTA MONTAŻOWA W800 HGM, UCB:400; UPB:400-630 PIONOWO / HGM, UCB:400 4P; UPB:400-630 4P POZIOMO",188.1,"1-ZE-09",null,null,"OM_MCCB_PLATES","22285","SZT","85389099","27.12.40.0",null,"5901988222857","OM - Plaque de montage L800 HGM, UCB: 400; UPB: 400-630 verticalement / HGM, UCB: 400 4P; UPB: 400-630 4P horizontal","OM - Mounting plate W800 HGM, UCB: 400; UPB: 400-630 Vertical / HGM, UCB: 400 4P; UPB: 400-630 4P Horizontal","OM- PLACA MONTAJE  W800 HGM 400; UPB:400-630 VERT. HGM 400 4P; UPB:400-63","ZENERGY OM - SZERELŐLAP W800 HGM, UCB:400; UPB:400-630 FÜGGŐLEGES / HGM, UCB:400 4P; UPB:400-630 4P VÍZSZINTES"]
["22288","ZENERGY OM - PŁYTA MONTAŻOWA W800 ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN, SILAS; SCHN LV4 160A + OCHRONNIK, 3M, POZIOMO",115.6,null,null,null,"OM_FUSE_PLATES",null,null,"85389099",null,null,"5901988222888"]
["22294","ZENERGY OM - OSŁONA CZOŁOWA WENTYLOWANA W300, 4M / 200",47.5,null,0.15833333333333333,4,null,null,null,"85389099",null,null,"5901988222949"]
["22301","ZENERGY OM - PŁYTA MONTAŻOWA W300, 1M, OCYNK",31.1,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22301","SZT","85389099","27.12.40.0",null,"5901988223014","OM - Plaque de montage L300, 1M, galvanisée","OM - Mounting plate W300, 1M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W300, 1M","ZENERGY OM - SZERELŐLEMEZ W300, 1M, HOGAGYZAT"]
["22304","ZENERGY OM - PŁYTA MONTAŻOWA W300, 4M, OCYNK",46.8,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22304","SZT","85389099","27.12.40.0",null,"5901988223045","OM - Plaque de montage L300, 4M, galvanisée","OM - Mounting plate W300, 4M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W300, 4M","ZENERGY OM - SZERELŐLEMEZ W300, 4M, HORGANYOZ"]
["22309","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W300,   9M, OCYNK",82.2,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22309","SZT","85389099","27.12.40.0",null,"5901988223090","OM - Plaque de montage complète L300, 9M, galvanisée","OM - Plain Mounting plate W300, 9M, galv","OM- PLACA MONTAJE TOTAL W300, 9M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W300, 9M, HORGANYOZ"]
["22312","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W300, 12M, OCYNK",83.1,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22312","SZT","85389099","27.12.40.0",null,"5901988223120","OM - Plaque de montage complète L300, 12M, galvanisée","OM - Plain Mounting plate W300, 12M, galv","OM- PLACA MONTAJE TOTAL W300, 12M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W300, 12M, HORGANYOZ"]
["22315","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W300, 15M, OCYNK",102.4,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22315","SZT","85389099","27.12.40.0",null,"5901988223151","OM - Plaque de montage complète L300, 15M, galvanisée","OM - Plain Mounting plate W300, 15M, galv","OM- PLACA MONTAJE TOTAL W300, 15M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W300, 15M, HORGANYOZ"]
["22324","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W300, 24M, OCYNK",135.9,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22324","SZT","85389099","27.12.40.0",null,"5901988223243","OM - Plaque de montage complète L300, 24M, galvanisée","OM - Plain Mounting plate W300, 24M, galv","OM- PLACA MONTAJE TOTAL W300, 24M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W300, 24M, HORGANYOZ"]
["22329","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W300, 29M, OCYNK",147.69999999999999,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22329","SZT","85389099","27.12.40.0",null,"5901988223298","OM - Plaque de montage complète L300, 29M, galvanisée","OM - Plain Mounting plate W300, 29M, galv","OM- PLACA MONTAJE TOTAL W300, 29M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W300, 29M, HORGANYOZ"]
["22339","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W300, 39M, OCYNK",194.7,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988223397","OM - Plaque de montage complète L300, 39M, galvanisée","OM - Plain Mounting plate W300, 39M, galv","OM- PLACA MONTAJE TOTAL W300, 39M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W300, 39M, HORGANYOZ"]
["22403","ZENERGY OM - PŁYTA MONTAŻOWA W400, 3M, OCYNK",43.4,"1-ZE-09",0.15,5,"OM_PLAIN_PLATES","22403","SZT","85389099","27.12.40.0",null,"5901988224035","OM - Plaque de montage L400, 3M, galvanisée","OM - Mounting plate W400, 3M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W400, 3M","ZENERGY OM - SZERELŐLEMEZ W400, 3M, HOGAGYZAT"]
["22408","ZENERGY OM - PŁYTA MONTAŻOWA W400, 8M, OCYNK",79.7,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22408","SZT","85389099","27.12.40.0",null,"5901988224080","OM - Plaque de montage L400, 8M, galvanisée","OM - Mounting plate W400, 8M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W400, 8M","ZENERGY OM - SZERELŐLEMEZ W400, 8M, HOGAGYZAT"]
["22412","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W400, 12M, OCYNK",90.2,"1-ZE-09",3.3333333333333333E-2,1,"OM_PLAIN_PLATES","22412","SZT","85389099","27.12.40.0",null,"5901988224127","OM - Plaque de montage complète L400, 12M, galvanisée","OM - Plain Mounting plate W400, 12M, galv","OM- PLACA MONTAJE TOTAL W400, 12M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W400, 12M, HORGANYOZ"]
["22421","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W400, 21M, OCYNK",135.9,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22421","SZT","85389099","27.12.40.0",null,"5901988224219","OM - Plaque de montage complète L400, 21M, galvanisée","OM - Plain Mounting plate W400, 21M, galv","OM- PLACA MONTAJE TOTAL W400, 21M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W400, 21M, HORGANYOZ"]
["22424","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W400, 24M, OCYNK",146.6,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22424","SZT","85389099","27.12.40.0",null,"5901988224240","OM - Plaque de montage complète L400, 24M, galvanisée","OM - Plain Mounting plate W400, 24M, galv","OM- PLACA MONTAJE TOTAL W400, 24M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W400, 24M, HORGANYOZ"]
["22429","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W400, 29M, OCYNK",161.6,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22429","SZT","85389099","27.12.40.0",null,"5901988224295","OM - Plaque de montage complète L400, 29M, galvanisée","OM - Plain Mounting plate W400, 29M, galv","OM- PLACA MONTAJE TOTAL W400, 29M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W400, 29M, HORGANYOZ"]
["22436","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W400, 36M, OCYNK",210.8,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988224363","OM - Plaque de montage complète L400, 36M, galvanisée","OM - Plain Mounting plate W400, 36M, galv","OM- PLACA MONTAJE TOTAL W400, 36M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W400, 36M, HORGANYOZ"]
["22453","ZENERGY OM - PŁYTA MONTAŻOWA WGŁĘBIONA W400, 3M, OCYNK",46.4,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988224530","OM - PLAQUE DE MONTAGE À ENCASTRER L400, 3M, GALVANISÉE","OM - Recessed Mounting plate W400, 3M, Galvanized","*OM - PLACA DE EMPOTRAR L400 3M GALVANIZADA","ZENERGY OM - SÜLÉSZTETT SZERELŐLEMEZ W400, 3M, HOGANGOZOTT"]
["22456","ZENERGY OM - PŁYTA MONTAŻOWA WGŁĘBIONA W400, 6M, OCYNK",76.099999999999994,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988224561","OM - PLAQUE À ENCASTRER L400, 6M, GALVANISÉE","OM - Recessed Mounting plate W400, 6M, Galvanized","*OM - PLACA DE EMPOTRAR L400 6M GALVANIZADA","ZENERGY OM - SÜLYÉTETT RÖGZÍTŐLEMEZ W400, 6M, HORGANYOZ"]
["22463","ZENERGY OM - PŁYTA MONTAŻOWA W400, 5M: NSX400-630; INS/INV320-630 PIONOWO / NSX400-630 4P; INS/INV320-630 POZIOMO",98.6,"1-ZE-09",null,null,"OM_MCCB_PLATES","22463","SZT","85389099","27.12.40.0",null,"5901988224639","OM - plaque de montage L400, 5M: NSX400-630; INS320-630 vertical / NSX400-630 4P; INS320-630 horizontal","OM - Mounting plate W400, 5M: NSX400-630; INS320-630 Vertical / NSX400-630 4P; INS320-630 Horizontal","OM - PLACA MONTAJE W400, 5M: NSX400-630; INS320-630 VERT. / NSX400-630 4P; INS320-630 HORIZ.","ZENERGY OM - SZERELŐLAP W400, 5M: NSX400-630; INS/INV320-630 FÜGGŐLEGES / NSX400-630 4P; INS/INV320-630 VÍZSZINTES"]
["22512","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 12M,  W1200 H700 D230, WISZĄCA",935.3,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988225124","OM - Boîtier de base IP55, 12M, L1200 H700 P230, suspendu","OM - Basic housing IP55, 12M, W1200 H700 D230, hanging","OM- ARMARIO METAL. IP55, 12M, W1200 H700 D230, MURAL","ZENERGY OM - ALAP HÁZ IP55, 12M, W1200 H700 D230, FÜGG."]
["22521","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 21M,  W1200 H1150 D230, WISZĄCA",1158.8,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988225216","OM - Boîtier de base IP55, 21M, L1200 H1150 P230, suspendu","OM - Basic housing IP55, 21M, W1200 H1150 D230, hanging","OM- ARMARIO METAL. IP55, 21M, W1200 H1150 D230, MURAL","ZENERGY OM - ALAP HÁZ IP55, 21M, W1200 H1150 D230, FÜGG."]
["22524","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 24M,  W1200 H1300 D230, WISZĄCA",1228,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988225247","OM - Boîtier de base IP55, 24M, L1200 H1300 P230, suspendu","OM - Basic housing IP55, 24M, W1200 H1300 D230, hanging","OM- ARMARIO METAL. IP55, 24M, W1200 H1300 D230, MURAL","ZENERGY OM - ALAP HÁZ IP55, 24M, W1200 H1300 D230, FÜGG."]
["22529","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 29M,  W1200 H1550 D230, WISZĄCA",1431,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988225292","OM - Boîtier de base IP55, 29M, L1200 H1550 P230, suspendu","OM - Basic housing IP55, 29M, W1200 H1550 D230, hanging","OM- ARMARIO METAL. IP55, 29M, W1200 H1550 D230, MURAL","ZENERGY OM - ALAP HÁZ IP55, 29M, W1200 H1550 D230, FÜGG."]
["22536","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 36M,  W1200 H2000 D230, COKÓŁ 100MM",2409.5,"1-ZE-09",null,null,"OM_ENCLOSURES",null,"SZT","85381000","27.12.40.0",null,"5901988225360","OM - Boîtier de base IP55, 36M, L1200 H2000 P230, base 100mm","OM - Basic housing IP55, 36M, W1200 H2000 D230, plinth 100mm","OM- ARMARIO METAL. IP55, 36M, W1200 H2000 D230, ZOCALO 100 mm","ZENERGY OM - ALAP HÁZ IP55, 36M, W1200 H2000 D230, lábazat 100mm"]
["22603","ZENERGY OM - PŁYTA MONTAŻOWA W600, 3M, OCYNK",47,"1-ZE-09",0.15833333333333333,5,"OM_PLAIN_PLATES","22603","SZT","85389099","27.12.40.0",null,"5901988226039","OM - Plaque de montage L600, 3M, galvanisée","OM - Mounting plate W600, 3M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W600, 3M","ZENERGY OM - SZERELŐLEMEZ W600, 3M, HOGAGYZAT"]
["22606","ZENERGY OM - PŁYTA MONTAŻOWA W600, 6M, OCYNK",75.5,"1-ZE-09",5.8333333333333334E-2,1,"OM_PLAIN_PLATES","22606","SZT","85389099","27.12.40.0",null,"5901988226060","OM - Plaque de montage L600, 6M, galvanisée","OM - Mounting plate W600, 6M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W600, 6M","ZENERGY OM - SZERELŐLEMEZ W600, 6M, HORGANYOZ"]
["22611","ZENERGY OM - PŁYTA MONTAŻOWA W600, 11M, OCYNK",98.8,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988226114","OM - Plaque de montage L600, 12M, galvanisée","OM - Mounting plate W600, 11M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W600, 12M","ZENERGY OM - SZERELŐLEMEZ W600, 11M, HOGAGYZAT"]
["22618","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W600, 18M, OCYNK",126.3,"1-ZE-09",0.01,1,"OM_PLAIN_PLATES","22618","SZT","85389099","27.12.40.0",null,"5901988226183","OM - Plaque de montage complète L600, 18M, galvanisée","OM - Plain Mounting plate W600, 18M, galv","OM- PLACA MONTAJE TOTAL W600, 18M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W600, 18M, HORGANYOZ"]
["22624","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W600, 24M, OCYNK",155.19999999999999,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22624","SZT","85389099","27.12.40.0",null,"5901988226244","OM - Plaque de montage complète L600, 24M, galvanisée","OM - Plain Mounting plate W600, 24M, galv","OM- PLACA MONTAJE TOTAL W600, 24M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W600, 24M, HORGANYOZ"]
["22627","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W600, 27M, OCYNK",160.5,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22627","SZT","85389099","27.12.40.0",null,"5901988226275","OM - Plaque de montage complète L600, 27M, galvanisée","OM - Plain Mounting plate W600, 27M, galv","OM- PLACA MONTAJE TOTAL W600, 27M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W600, 27M, HORGANYOZ"]
["22636","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W600, 36M, OCYNK",284.60000000000002,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988226367","OM - Plaque de montage complète L600, 36M, galvanisée","OM - Plain Mounting plate W600, 36M, galv","OM- PLACA MONTAJE TOTAL W600, 36M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W600, 36M, HORGANYOZ"]
["22640","ZENERGY OM - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN 100A, MONTAŻ NA SZYNACH, ROZSTAW 60MM + 2 IZOLATORY, D300",324,null,null,null,null,null,null,"",null,null,""]
["22644","ZENERGY OM - PŁYTA MONTAŻOWA + OSŁONA ROZŁĄCZNIK SKRZYNKOWY 4X EFEN 160, W600, 6M, PIONOWO",138,"1-ZE-09",9.166666666666666E-2,5,"OM_FUSE_PLATES",null,"SZT","85389099",null,null,"5901988226442","OM - Plaque de montage + boîtier de protection, boîtier de commutation 4x EFEN 160, L600, 6M, vertical","OM - Mounting plate + cover box switch box 4x EFEN 160, W600, 6M, Vertical","OM- PLACA MONTAJE CIEGA + TAPA PARA REGLETAS FUSIBLE 4X160, W600, 6M, ","ZENERGY OM - SZERELŐLAP + FEDŐDOBOZ KAPCSOLÓ 4X EFEN 160, W600, 6M, FÜGGŐLEGES"]
["22652","ZENERGY OM - PŁYTA MONTAŻOWA WGŁĘBIONA W600, 2M, OCYNK",46.7,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22652","SZT","85389099","27.12.40.0","231025PW","5901988226527","OM - PLAQUE DE MONTAGE ENCASTRÉ L600, 2M, GALVANISÉE","OM - Recessed Mounting plate W600, 2M, Galvanized","*OM - PLACA DE EMPOTRAR L600 2M GALVANIZADA","ZENERGY OM - SÜLYÉTETT SZERELŐLEMEZ W600, 2M, HORGANYOZ"]
["22656","ZENERGY OM - PŁYTA MONTAŻOWA WGŁĘBIONA W600, 6M, OCYNK",85,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22656","SZT","85389099","27.12.40.0","231025PW","5901988226565","OM - PLAQUE À ENCASTRER L600, 6M, GALVANISÉE","OM - Recessed Mounting plate W600, 6M, Galvanized","*OM - PLACA DE EMPOTRAR L600 6M GALVANIZADA","ZENERGY OM - SÜLYÉTETT SZERELŐLEMEZ W600, 6M, HOGANGZOTT"]
["22663","ZENERGY OM - PŁYTA MONTAŻOWA W600, 5M: NSX400-630; INS/INV320-630 PIONOWO / NSX400-630 4P; INS/INV320-630 POZIOMO",137.5,"1-ZE-09",null,null,"OM_MCCB_PLATES","22663","SZT","85389099","27.12.40.0",null,"5901988226633","OM - Plaque de montage NSX400-630 3 / 4P, L600, 6M, verticalement","OM - Mounting plate W600, 5M: NSX400-630; INS320-630 Vertical / NSX400-630 4P; INS / INV320-630 Horizontal","OM - PLACA MONTAJE W600, 5M: NSX400-630; INS320-630 VERT. / NSX400-630 4P; INS/INV320-630 HORIZ.","ZENERGY OM - SZERELŐLAP W600, 5M: NSX400-630; INS/INV320-630 FÜGGŐLEGES / NSX400-630 4P; INS/INV320-630 VÍZSZINTES"]
["22666","ZENERGY OM - PŁYTA MONTAŻOWA W600, 6M: HGP800 3/4P PIONOWO / HGP800 3P POZIOMO",155.1,"1-ZE-09",null,null,"OM_MCCB_PLATES","22666","SZT","85389099",null,null,"5901988226664","OM - PLAQUE DE MONTAGE L600, 6M: HGP800 3/4P VERTICALEMENT / HGP:800 3P HORIZONTALEMENT","OM - Mounting plate W600, 6M: HGP800 3/4P VerticalLY / HGP800 3P HorizontalLY","OM- PLACA MONT. HGP800 3/4P VERT. / HGP800 3P HORIZ. W600, 6M","ZENERGY OM - SZERELŐLAP W600, 6M: HGP800 3/4P VERTICAL / HGP800 3P HORIZONTAL"]
["22667","ZENERGY OM - PŁYTA MONTAŻOWA W600, 7M: HGP800 4P POZIOMO",177.1,"1-ZE-09",null,null,"OM_MCCB_PLATES","22667","SZT","85389099",null,null,"5901988226671","OM - PLAQUE DE MONTAGE L600, 7M: HGP:800 4P HORIZONTALEMENT","OM - Mounting plate W600, 7M: HGP800 4P HorizontalLY","OM- PLACA MONT. HGP800 4P HORIZ. W600, 7M","ZENERGY OM - SZERELŐLAP W600, 7M: HGP800 4P VÍZSZINTES"]
["22803","ZENERGY OM - PŁYTA MONTAŻOWA W800, 3M, OCYNK",72.2,"1-ZE-09",4.1666666666666664E-2,1,"OM_PLAIN_PLATES","22803","SZT","85389099","27.12.40.0",null,"5901988228033","OM - Plaque de montage L800, 3M, galvanisée","OM - Mounting plate W800, 3M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W800, 3M","ZENERGY OM - SZERELŐLEMEZ W800, 3M, HOGAGYZAT"]
["22808","ZENERGY OM - PŁYTA MONTAŻOWA W800, 8M, OCYNK",131.6,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22808","SZT","85389099","27.12.40.0",null,"5901988228088","OM - Plaque de montage L800, 8M, galvanisée","OM - Mounting plate W800, 8M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W800, 8M","ZENERGY OM - SZERELŐLEMEZ W800, 8M, HOGAGYZAT"]
["22811","ZENERGY OM - PŁYTA MONTAŻOWA W800, 11M, OCYNK",143.4,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988228118","OM - Plaque de montage L800, 12M, galvanisée","OM - Mounting plate W800, 11M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W800, 12M","ZENERGY OM - SZERELŐLEMEZ W800, 11M, HOGAGYZAT"]
["22818","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W800, 18M, OCYNK",179.8,"1-ZE-09",4.1666666666666664E-2,4,"OM_PLAIN_PLATES","22818","SZT","85389099","27.12.40.0",null,"5901988228187","OM - Plaque de montage complète L800, 18M, galvanisée","OM - Plain Mounting plate W800, 18M, galv","OM- PLACA MONTAJE TOTAL W800, 18M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W800, 18M, HORGANYOZ"]
["22828","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W800, 28M, OCYNK",307.10000000000002,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22828","SZT","85389099","27.12.40.0",null,"5901988228286","OM - Plaque de montage complète L800, 28M, galvanisée","OM - Plain Mounting plate W800, 28M, galv","OM- PLACA MONTAJE TOTAL W800, 28M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W800, 28M, HORGANYOZ"]
["22833","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W800, 33M, OCYNK",389.5,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988228330","OM - Plaque de montage complète L800, 33M, galvanisée","OM - Plain Mounting plate W800, 33M, galv","OM- PLACA MONTAJE TOTAL W800, 33M","ZENERGY OM - TELJES RÖGZÍTŐLEMEZ W800, 33M, HOGAGYZAT"]
["22841","ZENERGY OM - PŁYTA MONTAŻOWA LICZNIKOWA 3TL, W800, 8M, OCYNK",400.2,"1-ZE-09",0.01,1,"OM_PLAIN_PLATES","22841","SZT","85389099",null,null,"5901988228415","OM - 3TL, L800, plaque de montage de compteur de 9M, galvanisé","OM - Counter Mounting plate 3TL, W800, 8M, galv","OM- PLACA MONTAJE CIEGA PARA CONTADOR 3TL, W800, 9M","ZENERGYOM - SZÁMLÁLÓ SZERELŐLEMEZ 3TL, W800, 8M, HORGANYOZ"]
["22844","ZENERGY OM - PŁYTA MONTAŻOWA + OSŁONA ROZŁĄCZNIK SKRZYNKOWY 6X EFEN 160, W800, 6M, PIONOWO",178.7,"1-ZE-09",null,null,"OM_FUSE_PLATES",null,"SZT","85389099",null,null,"5901988228446","OM - Plaque de montage + commutateur de boîte de recouvrement 6x EFEN 160, L800, 6M, vertical","OM - Mounting plate + cover switch box 6x EFEN 160, W800, 6M, Vertical","OM- PLACA MONTAJE CIEGA + TAPA PARA REGLETAS FUSIBLE 6X160, W800, 6M, ","ZENERGY OM - SZERELŐLEMEZ + FEDŐDOBOZ KAPCSOLÓ 6X EFEN 160, W800, 6M, FÜGGŐLEGES"]
["22847","ZENERGY OM - PŁYTA MONTAŻOWA + OSŁONA ROZŁĄCZNIK SKRZYNKOWY 3X EFEN250, W800, 9M, PIONOWO",236.5,"1-ZE-09",null,null,"OM_FUSE_PLATES",null,"SZT","85389099",null,null,"5901988228477","OM - Détecteur plaque de montage + couvercle 3x EFEN250, L800, 9M, vertical","OM - Mounting plate + cover 3x EFEN250, W800, 9M box switch disconnector, Vertical","OM- PLACA MONTAJE CIEGA + TAPA PARA REGLETAS FUSIBLE 3X EFEN250, W800,","ZENERGY OM - SZERELŐLEMEZ + FEDŐDOBOZ KAPCSOLÓ 3X EFEN250, W800, 9M, FÜGGŐLEGES"]
["22855","ZENERGY OM - PŁYTA MONTAŻOWA WGŁĘBIONA W800, 5M, OCYNK",109.1,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988228552","OM - PLAQUE DE MONTAGE À ENCASTRER L800, 5M, GALVANISÉE","OM - Recessed Mounting plate W800, 5M, Galvanized","*OM - PLACA DE EMPOTRAR L800 5M GALVANIZADA","ZENERGY OM - SÜLYÉTETT RÖGZÍTŐLEMEZ W800, 5M, HORGANYOZ"]
["22862","ZENERGY OM - PŁYTA MONTAŻOWA W800, 4M: NSX:100-250 4P, 400-630 3P; INS/INV100-250 POZIOMO",154,"1-ZE-09",null,null,"OM_MCCB_PLATES","22862","SZT","85389099","27.12.40.0",null,"5901988228620","OM - Plaque de montage NSX100-250 4P, L800, 4M, horizontale","OM - Mounting plate W800, 4M: NSX: 100-250 4P, 400-630 3P; INS / INV100-250 Horizontal","OM - PLACA MONTAJE W800, 4M: NSX: 100-250 4P, 400-630 3P; INS/INV100-250 HORIZ.","ZENERGY OM - SZERELŐLAP W800, 4M: NSX:100-250 4P, 400-630 3P; INS/INV100-250 VÍZSZINTES"]
["22865","ZENERGY OM - PŁYTA MONTAŻOWA W800, 5M: HGP:400-630 3/4P PIONOWO / HGP:400-630 4P POZIOMO",188.1,"1-ZE-09",null,null,"OM_MCCB_PLATES","22865","SZT","85389099",null,null,"5901988228651","OM - PLAQUE DE MONTAGE L800, 5M : HGP:400-630 3/4P VERTICALEMENT / HGP:400-630 4P HORIZONTALEMENT","OM - Mounting plate W800, 5M: HGP:400-630 3/4P VerticalLY / HGP:400-630 4P HorizontalLY","OM- PLACA MONT. HGP400-630 3/4P VERT. / HGP400-630 4P HORIZ. W800, 5M","ZENERGY OM - SZERELŐLAP W800, 5M: HGP:400-630 3/4P FÜGGŐLEGES / HGP:400-630 4P VÍZSZINTES"]
["22902","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 2M, OCYNK",76.8,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229023","OM - Plaque de montage L1000, 2M, galvanisée","OM - Mounting plate W1000, 2M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W1000, 2M","ZENERGY OM - RÖGZÍTŐLEMEZ W1000, 2M, HORGANYOZ"]
["22906","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 6M, OCYNK",137,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229061","OM - Plaque de montage L1000, 6M, galvanisée","OM - Mounting plate W1000, 6M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W1000, 6M","ZENERGY OM - RÖGZÍTŐLEMEZ W1000, 6M, HORGANYOZ"]
["22910","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 10M, OCYNK",168,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229108","OM - Plaque de montage L1000, 10M, galvanisée","OM - Mounting plate W1000, 10M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W1000, 10M","ZENERGY OM - SZERELŐLEMEZ W1000, 10M, HOGAGYZAT"]
["22911","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 11M, OCYNK",173.3,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229115","OM - Plaque de montage L1000, 12M, galvanisée","OM - Mounting plate W1000, 11M, galv","OM- PLACA MONTAJE CIEGA PARCIAL W1000, 12M","ZENERGY OM - SZERELŐLEMEZ W1000, 11M, HOGANGOZOTT"]
["22918","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W1000, 18M, OCYNK",215.1,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229184","OM - Plaque de montage complète L1000, 18M, galvanisée","OM - Plain Mounting plate W1000, 18M, galv","OM- PLACA MONTAJE TOTAL W1000, 18M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W1000, 18M, HORGANYOZ"]
["22928","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W1000, 28M, OCYNK",380.9,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229283","OM - Plaque de montage complète L1000, 28M, galvanisée","OM - Plain Mounting plate W1000, 28M, galv","OM- PLACA MONTAJE TOTAL W1000, 28M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W1000, 28M, HORGANYOZ"]
["22933","ZENERGY OM - PEŁNA PŁYTA MONTAŻOWA W1000, 33M, OCYNK",492.2,"1-ZE-09",null,null,"OM_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229337","OM - Plaque de montage complète L1000, 33M, galvanisée","OM - Plain Mounting plate W1000, 33M, galv","OM- PLACA MONTAJE TOTAL W1000, 33M","ZENERGY OM - TELJES RÖGZÍTŐ LEMEZ W1000, 33M, HORGANYOZ"]
["22941","ZENERGY OM - PŁYTA MONTAŻOWA LICZNIKOWA 4TL, W1000, 8M, OCYNK",481.5,"1-ZE-09",null,null,"OM_PLAIN_PLATES","22941","SZT","85389099",null,null,"5901988229412","OM - Plaque de connexion 4TL, L1000, 9M, galv","OM - Counter Mounting plate 4TL, W1000, 8M, galv","OM - PLACA MONATJE PARA CONTADOR 4TL, W1000, 8M, GALV","ZENERGY OM - MÉRŐSZERELŐ LEMEZ 4TL, W1000, 8M, HORGANYOZOTT"]
["22963","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 5M: NSX400-630; INS/INV320-630 PIONOWO / NSX400-630 4P; INS/INV320-630 POZIOMO",216.7,"1-ZE-09",3.3333333333333333E-2,1,"OM_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988229634","OM - plaque de montage L1000, 5M: NSX400-630; INS / INV320-630 vertical / NSX400-630 4P; INS / INV320-630 horizontal","OM - Mounting plate W1000, 5M: NSX400-630; INS / INV320-630 Vertical / NSX400-630 4P; INS / INV320-630 Horizontal","OM- W1000, PLACA MONTAJE de 5M: NSX400-630; INS/INV320-630 VERT./NSX400-630 4P; INS/INV320-630 HORIZ.mente","ZENERGY OM - SZERELŐLAP W1000, 5M: NSX400-630; INS/INV320-630 FÜGGŐLEGES / NSX400-630 4P; INS/INV320-630 VÍZSZINTES"]
["22966","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 6M: HGP800 3/4P PIONOWO / HGP800 3P POZIOMO",247.5,"1-ZE-09",null,null,"OM_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988229665","OM - PLAQUE DE MONTAGE L1000, 6M: HGP800 3/4P VERTICALEMENT / HGP:800 3P HORIZONTALEMENT","OM - Mounting plate W1000, 6M: HGP800 3/4P VerticalLY / HGP800 3P HorizontalLY","OM- PLACA MONT. HGP800 3/4P VERT. / HGP800 3P HORIZ. W1000, 6M","ZENERGY OM - W1000 SZERELŐLAP, 6M: HGP800 3/4P FÜGGŐLEGES / HGP800 3P VÍZSZINTES"]
["22967","ZENERGY OM - PŁYTA MONTAŻOWA W1000, 7M: HGP800 4P POZIOMO",270.60000000000002,"1-ZE-09",null,null,"OM_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988229672","OM - PLAQUE DE MONTAGE L1000, 7M: HGP:800 4P HORIZONTALEMENT","OM - Mounting plate W1000, 7M: HGP800 4P Horizontal","OM- PLACA MONT. HGP800 4P HORIZ. W1000, 7M","ZENERGY OM - W1000 SZERELŐLAP, 7M: HGP800 4P VÍZSZINTES"]
["22973","ZENERGY OM - OSŁONA CZOŁOWA 4X INS/INV320-630, W1000, 9M / 900, PIONOWO, DŹWIGNIA",162.80000000000001,"1-ZE-01",null,null,"OM_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988229733","OM - capot avant 4x INS / INV320-630, L1000, 9M / 900, vertical, levier","OM - Front cover 4x INS / INV320-630, W1000, 9M / 900, Vertical, Lever","OM- TAPA TROQ. 4x INS/INV320-630, W1000, 9M/900, VERT., MANETA","ZENERGY OM - ELSŐ BURKOLAT 4X INS/INV320-630, W1000, 9M / 900, FÜGGŐLEGES, KAR"]
["22982","ZENERGY OM - OSŁONA CZOŁOWA NSX100-250 3P, W1000, 3M / 900, POZIOMO, DŹWIGNIA",84,"1-ZE-01",null,null,"OM_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988229825","OM - capot avant NSX100-250 3P, L1000, 3M / 900, horizontal, levier","OM - NSX100-250 3P Front Shield, W1000, 3M / 900, Horizontal, Lever","OM- TAPA TROQ. NSX100-250 3P, W1000, 3M/900, HORIZ. MANETA","ZENERGY OM - ELSŐ BURKOLAT NSX100-250 3P, W1000, 3M / 900, VÍZSZINTES, KAR"]
["22993","ZENERGY OM - OSŁONA CZOŁOWA NSX400-630 4P, W1000, 5M / 900, POZIOMO, DŹWIGNIA",101.8,"1-ZE-01",null,null,"OM_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988229931","OM - capot avant NSX400-630 4P, L1000, 5M / 900, horizontal, levier","OM - NSX400-630 4P, W1000, 5M / 900 front visor, Horizontal, Lever","OM- TAPA TROQ. NSX400-630 4P, W1000, 5M/900, HORIZ. MANETA","ZENERGY OM - ELSŐ BURKOLAT NSX400-630 4P, W1000, 5M / 900, VÍZSZINTES, KAR"]
["23015","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 15 MOD,    H850 X D230 X W300, WISZĄCA",385.6,"1-ZE-09",null,null,"OM_ENCLOSURES","23015","SZT","85381000","27.12.40.0",null,"5901988230159","OM - Boîtier de base IP30, 15 mod, H850 x P230 x L300, suspendu","OM - Basic housing IP30, 15 mod, H850 x D230 x W300, hanging","OM- ARMARIO METAL. IP30, 15 MOD,  H850 x D230 x W300, MURAL","ZENERGY OM - ALAP HÁZ IP30, 15 MOD, H850 X D230 X W300, FÜGG."]
["23024","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 24 MOD,  H1300 X D230 X W300, WISZĄCA",520.6,"1-ZE-09",null,null,"OM_ENCLOSURES","23024","SZT","85381000","27.12.40.0",null,"5901988230241","OM - Boîtier de base IP30, 24 mod, H1300 x P230 x L300, suspendu","OM - Basic housing IP30, 24 mod, H1300 x D230 x W300, hanging","OM- ARMARIO METAL. IP30, 24 MOD,  H1300 x D230 x W300, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP30, 24 MOD, H1300 X D230 X W300, FÜGG."]
["23030","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 30 MOD,  H1700 X D230 X W300, COKÓŁ 100MM",901.8,"1-ZE-09",null,null,"OM_ENCLOSURES","23030","SZT","85381000","27.12.40.0",null,"5901988230302","OM - Boîtier de base IP30, 30 mod, H1700 x P230 x L300, borne 100mm","OM - Basic housing IP30, 30 mod, H1700 x D230 x W300, plinth 100mm","OM- ARMARIO METAL. IP30, 30 MOD,  H1700 x D230 x W300, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 30 MOD, H1700 X D230 X W300, lábazat 100 mm"]
["23039","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 39 MOD,  H2150 X D230 X W300, COKÓŁ 100MM",1218.2,"1-ZE-09",null,null,"OM_ENCLOSURES","23039","SZT","85381000","27.12.40.0",null,"5901988230395","OM - Boîtier de base IP30, 39 mod, H2150 x P230 x L300, base 100mm","OM - Basic housing IP30, 39 mod, H2150 x D230 x W300, plinth 100mm","OM- ARMARIO METAL. IP30, 39 MOD,  H2150 x D230 x W300, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 39 MOD, H2150 X D230 X W300, lábazat 100 mm"]
["23109","ZENERGY OM - ROZSZERZENIE IP30,   9 MOD,    H550 X D230 X W300, WISZĄCA",349.9,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23109","SZT","85381000","27.12.40.0",null,"5901988231095","OM - Extension IP30, 9 mod, H550 x P230 x L300, suspendu","OM - Extension IP30, 9 mod, H550 x D230 x W300, hanging","OM- MODULO AUX. IP30,   9 MOD,  H550 x D230 x W300, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 9 MOD, H550X D230 X W300, FÜGG"]
["23118","ZENERGY OM - ROZSZERZENIE IP30, 18 MOD,  H1000 X D230 X W300, WISZĄCA",465.5,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23118","SZT","85381000","27.12.40.0",null,"5901988231187","OM - Extension IP30, 18 mod, H1000 x P230 x L300, suspendu","OM - Extension IP30, 18 mod, H1000 x D230 x W300, pendant","OM- MODULO AUX. IP30, 18 MOD,  H1000 x D230 x W300, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 18 MOD, H1000 X D230 X W300, LAKÓS"]
["23129","ZENERGY OM - ROZSZERZENIE IP30, 29 MOD,  H1550 X D230 X W300, WISZĄCA",677.2,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23129","SZT","85381000","27.12.40.0",null,"5901988231293","OM - extension IP30, 29 mod, H1550 x P230 x L300, suspendu","OM - Extension IP30, 29 mod, H1550 x D230 x W300, pendant","OM- MODULO AUX. IP30, 29 MOD,  H1550 x D230 x W300, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 29 MOD, H1550 X D230 X W300, LAKÓS"]
["23136","ZENERGY OM - ROZSZERZENIE IP30, 36 MOD,  H2000 X D230 X W300, COKÓŁ 100MM",1147,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23136","SZT","85381000","27.12.40.0",null,"5901988231361","OM - extension IP30, 36 mod, H2000 x P230 x L300, base 100 mm","OM - Extension IP30, 36 mod, H2000 x D230 x W300, plinth 100mm","OM- MODULO AUX. IP30, 36 MOD,  H2000 x D230 x W300, ZOCALO 100MM","ZENERGY OM - IP30 BŐVÍTÉS, 36 MOD, H2000 X D230 X W300, lábazat 100 mm"]
["23212","ZENERGY OM - DRZWI PEŁNE IP30, 12 MOD,    H700 X W300",132.80000000000001,"1-ZE-09",null,null,"OM_DOORS","23212","SZT","85389099","27.12.40.0",null,"5901988232122","OM - Portes pleine IP30, 12 mod., H700 x L300","OM - Plain door IP30, 12 mod, H700 x W300","OM- PUERTA OPACA IP30, 12 MOD,  H700 x W300","ZENERGY OM – TÖMÖR AJTÓ IP30, 12 MOD, H700 X W300"]
["23224","ZENERGY OM - DRZWI PEŁNE IP30, 24 MOD,  H1300 X W300",189,"1-ZE-09",null,null,"OM_DOORS","23224","SZT","85389099","27.12.40.0",null,"5901988232245","OM - Portes pleine IP30, 24 mod., H1300 x L300","OM - Plain door IP30, 24 mod, H1300 x W300","OM- PUERTA OPACA IP30, 24 MOD,  H1300 x W300","ZENERGY OM – TÖMÖR AJTÓ IP30, 24 MOD, H1300 X W300"]
["23229","ZENERGY OM - DRZWI PEŁNE IP30, 29 MOD,  H1550 X W300",284,"1-ZE-09",null,null,"OM_DOORS","23229","SZT","85389099","27.12.40.0",null,"5901988232290","OM - Portes pleine IP30, 29 mod, H1550 x L300","OM - Plain door IP30, 29 mod, H1550 x W300","OM- PUERTA OPACA IP30, 29 MOD,  H1550 x W300","ZENERGY OM – TÖMÖR AJTÓ IP30, 29 MOD, H1550 X W300"]
["23236","ZENERGY OM - DRZWI PEŁNE IP30, 36 MOD,  H1900 X W300",402.8,"1-ZE-09",0.05,4,"OM_DOORS","23236","SZT","85389099","27.12.40.0",null,"5901988232368","OM - Portes pleine IP30, 36 mod, H1900 x L300","OM - Plain door IP30, 36 mod, H1900 x W300","OM- PUERTA OPACA IP30, 36 MOD,  H1900 x W300","ZENERGY OM – TÖMÖR AJTÓ IP30, 36 MOD, H1900 X W300"]
["23239","ZENERGY OM - DRZWI PEŁNE IP30, 39 MOD,  H2050 X W300",446,"1-ZE-09",null,null,"OM_DOORS","23239","SZT","85389099","27.12.40.0",null,"5901988232399","OM - Portes pleine IP30, 39 mod, H2050 x L300","OM - Plain door IP30, 39 mod, H2050 x W300","OM- PUERTA OPACA IP30, 39 MOD,  H2050 x W300","ZENERGY OM – TÖMÖR AJTÓ IP30, 39 MOD, H2050 X W300"]
["23415","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 15 MOD,    H850 X W300",243.8,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23415","SZT","85389099","27.12.40.0",null,"5901988234157","OM - Portes transparentes IP30, 15 mod, H850 x L300","OM - Transparent door IP30, 15 mod, H850 x W300","OM- PUERTA TRANSP. IP30, 15 MOD,  H850 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 15 MOD, H850 X W300"]
["23424","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 24 MOD,  H1300 X W300",361.5,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23424","SZT","85389099","27.12.40.0",null,"5901988234249","OM - Portes transparentes IP30, 24 mod., H1300 x L300","OM - Transparent door IP30, 24 mod, H1300 x W300","OM- PUERTA TRANSP. IP30, 24 MOD,  H1300 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 24 MOD, H1300 X W300"]
["23430","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 30 MOD,  H1600 X W300",445.2,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23430","SZT","85389099","27.12.40.0",null,"5901988234300","OM - Portes transparentes IP30, 30 mod, H1600 x L300","OM - Transparent door IP30, 30 mod, H1600 x W300","OM- PUERTA TRANSP. IP30, 30 MOD,  H1600 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 30 MOD, H1600 X W300"]
["23439","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 39 MOD,  H2050 X W300",610.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23439","SZT","85389099","27.12.40.0",null,"5901988234393","OM - Portes transparentes IP30, 39 mod, H2050 x L300","OM - Transparent door IP30, 39 mod, H2050 x W300","OM- PUERTA TRANSP. IP30, 39 MOD,  H2050 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 39 MOD, H2050 X W300"]
["23518","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 18 MOD,  H1000 X D230 X W300, WISZĄCA",601.6,"1-ZE-09",null,null,"OM_ENCLOSURES","23018","SZT","85381000","27.12.40.0",null,"5901988235185","OM - Boîtier de base IP55, 18 mod, H1000 x P230 x L300, suspendu","OM - Basic housing IP55, 18 mod, H1000 x D230 x W300, hanging","OM- ARMARIO METAL. IP55, 18 MOD,  H1000 x D230 x W300, MURAL","ZENERGY OM - ALAP HÁZ IP55, 18 MOD, H1000 X D230 X W300, FÜGG."]
["23527","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 27 MOD,  H1450 X D230 X W300, WISZĄCA",781.9,"1-ZE-09",null,null,"OM_ENCLOSURES","23027","SZT","85381000","27.12.40.0",null,"5901988235277","OM - Boîtier de base IP55, 27 mod, H1450 x P230 x L300, suspendu","OM - Basic housing IP55, 27 mod, H1450 x D230 x W300, hanging","OM- ARMARIO METAL. IP55, 27 MOD,  H1450 x D230 x W300, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP55, 27 MOD, H1450 X D230 X W300, FÜGG."]
["23530","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 30 MOD,  H1700 X D230 X W300, COKÓŁ 100MM",1102.7,"1-ZE-09",null,null,"OM_ENCLOSURES","23030","SZT","85381000","27.12.40.0",null,"5901988235307","OM - Boîtier de base IP55, 30 mod, H1700 x P230 x L300, base 100mm","OM - Basic housing IP55, 30 mod, H1700 x D230 x W300, plinth 100mm","OM- ARMARIO METAL. IP55, 30 MOD,  H1700 x D230 x W300, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP55, 30 MOD, H1700 X D230 X W300, lábazat 100 mm"]
["23533","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 33 MOD,  H1850 X D230 X W300, COKÓŁ 100MM",1243.0999999999999,"1-ZE-09",null,null,"OM_ENCLOSURES","23033","SZT","85381000","27.12.40.0",null,"5901988235338","OM - Boîtier de base IP55, 33 mod, H1850 x P230 x L300, borne 100mm","OM - Basic housing IP55, 33 mod, H1850 x D230 x W300, plinth 100mm","OM- ARMARIO METAL. IP55, 33 MOD,  H1850 x D230 x W300, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP55, 33 MOD, H1850 X D230 X W300, lábazat 100 mm"]
["23609","ZENERGY OM - ROZSZERZENIE IP55,   9 MOD,    H550 X D230 X W300, WISZĄCA",467.6,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23109","SZT","85381000","27.12.40.0",null,"5901988236090","OM - extension IP55, 9 mod, H550 x P230 x L300, suspendu","OM - Extension IP55, 9 mod, H550 x D230 x W300, hanging","OM- MODULO AUX. IP55,   9 MOD,  H550 x D230 x W300, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 9 MOD, H550 X D230 X W300, LAKÓS"]
["23618","ZENERGY OM - ROZSZERZENIE IP55, 18 MOD,  H1000 X D230 X W300, WISZĄCA",627.5,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23118","SZT","85381000","27.12.40.0",null,"5901988236182","OM - extension IP55, 18 mod, H1000 x P230 x L300, suspendu","OM - Extension IP55, 18 mod, H1000 x D230 x W300, hanging","OM- MODULO AUX. IP55, 18 MOD,  H1000 x D230 x W300, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 18 MOD, H1000 X D230 X W300, LAKÓS"]
["23628","ZENERGY OM - ROZSZERZENIE IP55, 28 MOD,  H1600 X D230 X W300, COKÓŁ 100MM",1074.5999999999999,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23128","SZT","85381000","27.12.40.0",null,"5901988236281","OM - extension de IP55, 28 mod, H1600 x P230 x L300, socle 100mm","OM - Extension IP55, 28 mod, H1600 x D230 x W300, plinth 100mm","OM- MODULO AUX. IP55, 28 MOD,  H1600 x D230 x W300, ZOCALO 100MM","ZENERGY OM – IP55 BŐVÍTÉS, 28 MOD, H1600 X D230 X W300, lábazat 100 mm"]
["23633","ZENERGY OM - ROZSZERZENIE IP55, 33 MOD,  H1850 X D230 X W300, COKÓŁ 100MM",1230.0999999999999,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","23133","SZT","85381000","27.12.40.0",null,"5901988236335","OM - Extension IP55, 33 mod, H1850 x P230 x L300, base de 100 mm","OM - Extension IP55, 33 mod, H1850 x D230 x W300, plinth 100mm","OM- MODULO AUX. IP55, 33 MOD,  H1850 x D230 x W300, ZOCALO 100MM","ZENERGY OM - IP55 BŐVÍTÉS, 33 MOD, H1850 X D230 X W300, lábazat 100 mm"]
["23712","ZENERGY OM - DRZWI PEŁNE IP55, 12 MOD,    H700 X W300",262.39999999999998,"1-ZE-09",null,null,"OM_DOORS","23212","SZT","85389099","27.12.40.0",null,"5901988237127","OM - Portes pleine IP55, 12 mod, H700 x L300","OM - Plain door IP55, 12 mod, H700 x W300","OM- PUERTA OPACA IP55, 12 MOD,  H700 x W300","ZENERGY OM – TÖMÖR AJTÓ IP55, 12 MOD, H700 X W300"]
["23721","ZENERGY OM - DRZWI PEŁNE IP55, 21 MOD,  H1150 X W300",315.39999999999998,"1-ZE-09",null,null,"OM_DOORS","23221","SZT","85389099","27.12.40.0",null,"5901988237219","OM - Portes pleine IP55, 21 mod, H1150 x L300","OM - Plain door IP55, 21 mod, H1150 x W300","OM- PUERTA OPACA IP55, 21 MOD,  H1150 x W300","ZENERGY OM – TÖMÖR AJTÓ IP55, 21 MOD, H1150 X W300"]
["23729","ZENERGY OM - DRZWI PEŁNE IP55, 29 MOD,  H1550 X W300",388.8,"1-ZE-09",null,null,"OM_DOORS","23229","SZT","85389099","27.12.40.0",null,"5901988237295","OM - Portes pleine IP55, 29 mod, H1550 x L300","OM - Plain door IP55, 29 mod, H1550 x W300","OM- PUERTA OPACA IP55, 29 MOD,  H1550 x W300","ZENERGY OM – TÖMÖR AJTÓ IP55, 29 MOD, H1550 X W300"]
["23730","ZENERGY OM - DRZWI PEŁNE IP55, 30 MOD,  H1600 X W300",406.1,"1-ZE-09",null,null,"OM_DOORS","23230","SZT","85389099","27.12.40.0",null,"5901988237301","OM - Portes pleine IP55, 30 mod., H1600 x L300","OM - Plain door IP55, 30 mod, H1600 x W300","OM- PUERTA OPACA IP55, 30 MOD,  H1600 x W300","ZENERGY OM – TÖMÖR AJTÓ IP55, 30 MOD, H1600 X W300"]
["23739","ZENERGY OM - DRZWI PEŁNE IP55, 39 MOD,  H2050 X W300",533.5,"1-ZE-09",null,null,"OM_DOORS","23239","SZT","85389099","27.12.40.0",null,"5901988237394","OM - Portes pleine IP55, 39 mod, H2050 x L300","OM - Plain door IP55, 39 mod, H2050 x W300","OM- PUERTA OPACA IP55, 39 MOD,  H2050 x W300","ZENERGY OM - TELJES AJTÓ IP55, 39 MOD,H2050 X W300"]
["23918","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 18 MOD,  H1100 X W300",324.39999999999998,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23418","SZT","85389099","27.12.40.0",null,"5901988239183","OM - Portes transparentes IP55, 18 mod, H1100 x L300","OM - Transparent door IP55, 18 mod, H1100 x W300","OM- PUERTA TRANSP. IP55, 18 MOD,  H1100 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 18 MOD, H1100 X W300"]
["23927","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 27 MOD,  H1450 X W300",481.2,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23427","SZT","85389099","27.12.40.0",null,"5901988239275","OM - Portes transparentes IP55, 27 mod, H1450 x L300","OM - Transparent door IP55, 27 mod, H1450 x W300","OM- PUERTA TRANSP. IP55, 27 MOD,  H1450 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 27 MOD, H1450 X W300"]
["23930","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 30 MOD,  H1600 X W300",513,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","23430","SZT","85389099","27.12.40.0",null,"5901988239305","OM - Portes transparentes IP55, 30 mod., H1600 x L300","OM - Transparent door IP55, 30 mod, H1600 x W300","OM- PUERTA TRANSP. IP55, 30 MOD,  H1600 x W300","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 30 MOD, H1600 X W300"]
["24009","ZENERGY OM - OBUDOWA PODSTAWOWA IP30,   9 MOD,    H550 X D230 X W400, WISZĄCA",352.1,"1-ZE-09",null,null,"OM_ENCLOSURES","24009","SZT","85381000","27.12.40.0",null,"5901988240097","OM - Boîtier de base IP30, 9 mod., H550 x P230 x L400, suspendu","OM - Basic housing IP30, 9 mod, H550 x D230 x W400, hanging","OM- ARMARIO METAL. IP30,   9 MOD,  H550 x D230 x W400, MURAL","ZENERGY OM - ALAP HÁZ IP30, 9 MOD, H550 X D230 X W400, FÜGG."]
["24018","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 18 MOD,  H1000 X D230 X W400, WISZĄCA",457.9,"1-ZE-09",null,null,"OM_ENCLOSURES","24018","SZT","85381000","27.12.40.0",null,"5901988240189","OM - Boîtier de base IP30, 18 mod, H1000 x P230 x L400, suspendu","OM - Basic housing IP30, 18 mod, H1000 x D230 x W400, hanging","OM- ARMARIO METAL. IP30, 18 MOD,  H1000 x D230 x W400, MURAL","ZENERGY OM - ALAP HÁZ IP30, 18 MOD, H1000 X D230 X W400, FÜGG."]
["24027","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 27 MOD,  H1450 X D230 X W400, WISZĄCA",585.4,"1-ZE-09",null,null,"OM_ENCLOSURES","24027","SZT","85381000","27.12.40.0",null,"5901988240271","OM - Boîtier de base IP30, 27 mod, H1450 x P230 x L400, suspendu","OM - Basic housing IP30, 27 mod, H1450 x D230 x W400, hanging","OM- ARMARIO METAL. IP30, 27 MOD,  H1450 x D230 x W400, MURAL","ZENERGY OM - ALAP HÁZ IP30, 27 MOD, H1450 X D230 X W400, FÜGG."]
["24028","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 28 MOD,  H1600 X D230 X W400, COKÓŁ 100MM",853.2,"1-ZE-09",null,null,"OM_ENCLOSURES","24028","SZT","85381000","27.12.40.0",null,"5901988240288","OM - Boîtier de base IP30, 28 mod, H1600 x P230 x L400, base 100mm","OM - Basic housing IP30, 28 mod, H1600 x D230 x W400, plinth 100mm","OM- ARMARIO METAL. IP30, 28 MOD, H1600XD230XW400, ZOCALO 100 MM","ZENERGY OM - ALAP HÁZ IP30, 28 MOD, H1600 X D230 X W400, lábazat 100 mm"]
["24033","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 33 MOD,  H1850 X D230 X W400, COKÓŁ 100MM",1063.8,"1-ZE-09",null,null,"OM_ENCLOSURES","24033","SZT","85381000","27.12.40.0",null,"5901988240332","OM - Boîtier de base IP30, 33 mod, H1850 x P230 x L400, base 100mm","OM - Basic housing IP30, 33 mod, H1850 x D230 x W400, plinth 100mm","OM- ARMARIO METAL. IP30, 33 MOD,  H1850 x D230 x W400, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 33 MOD, H1850 X D230 X W400, lábazat 100 mm"]
["24112","ZENERGY OM - ROZSZERZENIE IP30, 12 MOD,    H700 X D230 X W400, WISZĄCA",376.9,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24112","SZT","85381000","27.12.40.0",null,"5901988241124","OM - extension IP30, 12 mod, H700 x P230 x L400, suspendu","OM - Extension IP30, 12 mod, H700 x D230 x W400, pendant","OM- MODULO AUX. IP30, 12 MOD,  H700 x D230 x W400, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 12 MOD, H700 X D230 X W400, LAKÓS"]
["24121","ZENERGY OM - ROZSZERZENIE IP30, 21 MOD,  H1150 X D230 X W400, WISZĄCA",538.9,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24121","SZT","85381000","27.12.40.0",null,"5901988241216","OM - extension IP30, 21 mod, H1150 x P230 x L400, suspendu","OM - Extension IP30, 21 mod, H1150 x D230 x W400, pendant","OM- MODULO AUX. IP30, 21 MOD,  H1150 x D230 x W400, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 21 MOD, H1150 X D230 X W400, LAKÓS"]
["24128","ZENERGY OM - ROZSZERZENIE IP30, 28 MOD,  H1600 X D230 X W400, COKÓŁ 100MM",897.5,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24128","SZT","85381000","27.12.40.0",null,"5901988241285","OM - Extension IP30, 28 mod, H1600 x P230 x L400, base 100mm","OM - Extension IP30, 28 mod, H1600 x D230 x W400, plinth 100mm","OM- MODULO AUX. IP30, 28 MOD, H1600XD230XW400, ZOCALO 100 MM","ZENERGY OM - IP30 BŐVÍTÉS, 28 MOD, H1600 X D230 X W400, lábazat 100 mm"]
["24136","ZENERGY OM - ROZSZERZENIE IP30, 36 MOD,  H2000 X D230 X W400, COKÓŁ 100MM",1202,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24136","SZT","85381000","27.12.40.0",null,"5901988241360","OM - extension IP30, 36 mod, H2000 x P230 x L400, base 100 mm","OM - Extension IP30, 36 mod, H2000 x D230 x W400, plinth 100mm","OM- MODULO AUX. IP30, 36 MOD,  H2000 x D230 x W400, ZOCALO 100MM","ZENERGY OM - IP30 BŐVÍTÉS, 36 MOD, H2000 X D230 X W400, lábazat 100 mm"]
["24212","ZENERGY OM - DRZWI PEŁNE IP30, 12 MOD,    H700 X W400",140.4,"1-ZE-09",0.14166666666666666,4,"OM_DOORS","24212","SZT","85389099","27.12.40.0",null,"5901988242121","OM - Portes pleine IP30, 12 mod, H700 x L400","OM - Plain door IP30, 12 mod, H700 x W400","OM- PUERTA OPACA IP30, 12 MOD,  H700 x W400","ZENERGY OM – TÖMÖR AJTÓ IP30, 12 MOD, H700 X W400"]
["24221","ZENERGY OM - DRZWI PEŁNE IP30, 21 MOD,  H1150 X W400",182.5,"1-ZE-09",0.11666666666666667,5,"OM_DOORS","24221","SZT","85389099","27.12.40.0",null,"5901988242213","OM - Portes pleine IP30, 21 mod, H1150 x L400","OM - Plain door IP30, 21 mod, H1150 x W400","OM- PUERTA OPACA IP30, 21 MOD,  H1150 x W400","ZENERGY OM – TÖMÖR AJTÓ IP30, 21 MOD, H1150 X W400"]
["24224","ZENERGY OM - DRZWI PEŁNE IP30, 24 MOD,  H1300 X W400",199.8,"1-ZE-09",0.13333333333333333,2,"OM_DOORS","24224","SZT","85389099","27.12.40.0",null,"5901988242244","OM - Portes pleine IP30, 24 mod., H1300 x L400","OM - Plain door IP30, 24 mod, H1300 x W400","OM- PUERTA OPACA IP30, 24 MOD,  H1300 x W400","ZENERGY OM – TÖMÖR AJTÓ IP30, 24 MOD, H1300 X W400"]
["24229","ZENERGY OM - DRZWI PEŁNE IP30, 29 MOD,  H1550 X W400",315.39999999999998,"1-ZE-09",null,null,"OM_DOORS","24229","SZT","85389099","27.12.40.0",null,"5901988242299","OM - Portes pleine IP30, 29 mod, H1550 x L400","OM - Plain door IP30, 29 mod, H1550 x W400","OM- PUERTA OPACA IP30, 29 MOD H1550XW400","ZENERGY OM – TÖMÖR AJTÓ IP30, 29 MOD, H1550 X W400"]
["24409","ZENERGY OM - DRZWI TRANSPARENTNE IP30,   9 MOD,    H550 X W400",214.1,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24409","SZT","85389099","27.12.40.0",null,"5901988244095","OM - Portes transparentes IP30, 9 mod., H550 x L400","OM - Transparent door IP30, 9 mod, H550 x W400","OM- PUERTA TRANSP. IP30,  9 MOD,  H550 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 9 MOD, H550 X W400"]
["24418","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 18 MOD,  H1000 X W400",305.3,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24418","SZT","85389099","27.12.40.0",null,"5901988244187","OM - Portes transparentes IP30, 18 mod., H1000 x L400","OM - Transparent door IP30, 18 mod, H1000 x W400","OM- PUERTA TRANSP. IP30, 18 MOD,  H1000 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 18 MOD, H1000 X W400"]
["24427","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 27 MOD,  H1450 X W400",464.3,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24427","SZT","85389099","27.12.40.0",null,"5901988244279","OM - Portes transparentes IP30, 27 mod, H1450 x L400","OM - Transparent door IP30, 27 mod, H1450 x W400","OM- PUERTA TRANSP. IP30, 27 MOD,  H1450 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 27 MOD, H1450 X W400"]
["24433","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 33 MOD,  H1750 X W400",561.79999999999995,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24433","SZT","85389099","27.12.40.0",null,"5901988244330","OM - Portes transparentes IP30, 33 mod, H1750 x L400","OM - Transparent door IP30, 33 mod, H1750 x W400","OM- PUERTA TRANSP. IP30, 33 MOD,  H1750 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 33 MOD, H1750 X W400"]
["24509","ZENERGY OM - OBUDOWA PODSTAWOWA IP55,   9 MOD,    H550 X D230 X W400, WISZĄCA",483.8,"1-ZE-09",0.01,1,"OM_ENCLOSURES","24009","SZT","85381000","27.12.40.0",null,"5901988245092","OM - Boîtier de base IP55, 9 mod., H550 x P230 x L400, suspendu","OM - Basic housing IP55, 9 mod, H550 x D230 x W400, hanging","OM- ARMARIO METAL. IP55,   9 MOD,  H550 x D230 x W400, MURAL","ZENERGY OM - ALAP HÁZ IP55, 9 MOD, H550 X D230 X W400, FÜGG."]
["24512","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 12 MOD,    H700 X D230 X W400, WISZĄCA",511.9,"1-ZE-09",null,null,"OM_ENCLOSURES","24012","SZT","85381000","27.12.40.0",null,"5901988245122","OM - Boîtier de base IP55, 12 mod, H700 x P230 x L400, suspendu","OM - Basic housing IP55, 12 mod, H700 x D230 x W400, hanging","OM- ARMARIO METAL. IP55, 12 MOD,  H700 x D230 x W400, MURAL","ZENERGY OM - ALAP HÁZ IP55, 12 MOD, H700 X D230 X W400, FÜGG."]
["24521","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 21 MOD,  H1150 X D230 X W400, WISZĄCA",703.1,"1-ZE-09",null,null,"OM_ENCLOSURES","24021","SZT","85381000","27.12.40.0",null,"5901988245214","OM - Boîtier de base IP55, 21 mod, H1150 x P230 x L400, suspendu","OM - Basic housing IP55, 21 mod, H1150 x D230 x W400, hanging","OM- ARMARIO METAL. IP55, 21 MOD,  H1150 x D230 x W400, MURAL","ZENERGY OM - ALAP HÁZ IP55, 21 MOD, H1150 X D230 X W400, FÜGG."]
["24528","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 28 MOD,  H1600 X D230 X W400, COKÓŁ 100MM",1116.7,"1-ZE-09",null,null,"OM_ENCLOSURES","24028","SZT","85381000","27.12.40.0",null,"5901988245283","OM - Boîtier de base IP55, 28 mod, H1600 x P230 x L400, base 100mm","OM - Basic housing IP55, 28 mod, H1600 x D230 x W400, plinth 100mm","OM- ARMARIO METAL. IP55, 28 MOD, H1600XD230XW400, ZOCALO 100 MM","ZENERGY OM - ALAP HÁZ IP55, 28 MOD, H1600 X D230 X W400, lábazat 100 mm"]
["24536","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 36 MOD,  H2000 X D230 X W400, COKÓŁ 100MM",1378.1,"1-ZE-09",null,null,"OM_ENCLOSURES","24036","SZT","85381000","27.12.40.0",null,"5901988245368","OM - Boîtier de base IP55, 36 mod, H2000 x P230 x L400, base 100mm","OM - Basic housing IP55, 36 mod, H2000 x D230 x W400, plinth 100mm","OM- ARMARIO METAL. IP55, 36 MOD,  H2000 x D230 x W400, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP55, 36 MOD, H2000 X D230 X W400, lábazat 100 mm"]
["24612","ZENERGY OM - ROZSZERZENIE IP55, 12 MOD,    H700 X D230 X W400, WISZĄCA",530.29999999999995,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24112","SZT","85381000","27.12.40.0",null,"5901988246129","OM - extension IP55, 12 mod, H700 x P230 x L400, suspendu","OM - Extension IP55, 12 mod, H700 x D230 x W400, pendant","OM- MODULO AUX. IP55, 12 MOD,  H700 x D230 x W400, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 12 MOD, H700 X D230 X W400, LAKÓS"]
["24621","ZENERGY OM - ROZSZERZENIE IP55, 21 MOD,  H1150 X D230 X W400, WISZĄCA",733.3,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24121","SZT","85381000","27.12.40.0",null,"5901988246211","OM - Extension IP55, 21 mod, H1150 x P230 x L400, suspendu","OM - Extension IP55, 21 mod, H1150 x D230 x W400, pendant","OM- MODULO AUX. IP55, 21 MOD,  H1150 x D230 x W400, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 21 MOD, H1150 X D230 X W400, LAKÓS"]
["24629","ZENERGY OM - ROZSZERZENIE IP55, 29 MOD,  H1550 X D230 X W400, WISZĄCA",952.6,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24129","SZT","85381000","27.12.40.0",null,"5901988246297","OM - Extension IP55, 29 mod, H1550 x P230 x L400, suspendu","OM - Extension IP55, 29 mod, H1550 x D230 x W400, pendant","OM- MODULO AUX. IP55, 29 MOD, H1550XD230XW400, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 29 MOD, H1550 X D230 X W400, LAKÓS"]
["24636","ZENERGY OM - ROZSZERZENIE IP55, 36 MOD,  H2000 X D230 X W400, COKÓŁ 100MM",1371.6,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24136","SZT","85381000","27.12.40.0",null,"5901988246365","OM - extension IP55, 36 mod, H2000 x P230 x L400, base 100 mm","OM - Extension IP55, 36 mod, H2000 x D230 x W400, plinth 100mm","OM- MODULO AUX. IP55, 36 MOD,  H2000 x D230 x W400, ZOCALO 100MM","ZENERGY OM – IP55 BŐVÍTÉS, 36 MOD, H2000 X D230 X W400, lábazat 100 mm"]
["24639","ZENERGY OM - ROZSZERZENIE IP55, 39 MOD,  H2150 X D230 X W400, COKÓŁ 100MM",1473.1,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","24139","SZT","85381000","27.12.40.0",null,"5901988246396","OM - Extension IP55, 39 mod, H2150 x P230 x L400, base 100 mm","OM - Extension IP55, 39 mod, H2150 x D230 x W400, plinth 100mm","OM- MODULO AUX. IP55, 39 MOD,  H2150 x D230 x W400, ZOCALO 100MM","ZENERGY OM - IP55 BŐVÍTÉS, 39 MOD, H2150 X D230 X W400, lábazat 100 mm"]
["24715","ZENERGY OM - DRZWI PEŁNE IP55, 15 MOD,    H850 X W400",216,"1-ZE-09",1.6666666666666666E-2,1,"OM_DOORS","24215","SZT","85389099","27.12.40.0",null,"5901988247157","OM - Portes pleine IP55, 15 mod., H850 x L400","OM - Plain door IP55, 15 mod, H850 x W400","OM- PUERTA OPACA IP55, 15 MOD,  H850 x W400","ZENERGY OM – TÖMÖR AJTÓ IP55, 15 MOD, H850 X W400"]
["24724","ZENERGY OM - DRZWI PEŁNE IP55, 24 MOD,  H1300 X W400",318.60000000000002,"1-ZE-09",4.1666666666666664E-2,2,"OM_DOORS","24224","SZT","85389099","27.12.40.0",null,"5901988247249","OM - Portes pleine IP55, 24 mod., H1300 x L400","OM - Plain door IP55, 24 mod, H1300 x W400","OM- PUERTA OPACA IP55, 24 MOD,  H1300 x W400","ZENERGY OM – TÖMÖR AJTÓ IP55, 24 MOD, H1300 X W400"]
["24730","ZENERGY OM - DRZWI PEŁNE IP55, 30 MOD,  H1600 X W400",440.6,"1-ZE-09",null,null,"OM_DOORS","24230","SZT","85389099","27.12.40.0",null,"5901988247300","OM - Portes pleine IP55, 30 mod., H1600 x L400","OM - Plain door IP55, 30 mod, H1600 x W400","OM- PUERTA OPACA IP55, 30 MOD,  H1600 x W400","ZENERGY OM – TÖMÖR AJTÓ IP55, 30 MOD, H1600 X W400"]
["24739","ZENERGY OM - DRZWI PEŁNE IP55, 39 MOD,  H2050 X W400",553,"1-ZE-09",0.11666666666666667,1,"OM_DOORS","24239","SZT","85389099","27.12.40.0",null,"5901988247393","OM - Portes pleine IP55, 39 mod, H2050 x L400","OM - Plain door IP55, 39 mod, H2050 x W400","OM- PUERTA OPACA IP55, 39 MOD,  H2050 x W400","ZENERGY OM – TÖMÖR AJTÓ IP55, 39 MOD, H2050 X W400"]
["24775","ZENERGY - TRANSFER NA TYŁ 3X2X 60X5 WYŁĄCZNIKA NT12 3P W KASECIE, DO KABLI",822.3,"1-ZE-01",null,null,"OE_ACB_TRANSFER","24775","SZT","74072900",null,null,"5901988247751","OE - Transfert arrière 3x2x 60x5 NT12 Interrupteur 3P en cassette, pour câbles","OE - Back transfer 3x2x 60x5 of NT12 3P switch in cassette, for cables","OE- BACK TRANSFER 3X2X 60X5 DE NT12 3P ","ZENERGY - ÁTHELYEZÉS A HÁTSÓRA 3X2X 60X5 NT12 3P MEGSZAKÍTÓ KAZETTÁBAN, KÁBELHEZ"]
["24778","ZENERGY - POŁĄCZENIE MIEDZIANE 3X2X80X10 WYŁĄCZNIKA NW25 3P W KASECIE, DO KABLI",3619.1,"1-ZE-01",null,null,"OE_ACB_TRANSFER","24778","SZT","74072900",null,null,"5901988247782","OE - Connexion en cuivre 3x2x Disjoncteur 80x10 NW25 3P en boĂ®tier, pour cĂ˘bles","OE - Copper connection 3x2x80x10 NW25 3P switch in a cassette, for cables","OE- CONEXION CU 3X2X80X10 PARA NW25 3P, PARA CABLES","ZENERGY - RÉZ CSATLAKOZÁS 3X2X80X10 NW25 3P SZAKADÓ KAZETTÁBAN, KÁBELHEZ"]
["24782","Zenergy - Połączenie miedziane 3x2x100x10 wyłącznika NW25 3P w kasecie, z mostem AlCubar 6300A",8383.5,"1-ZE-01",null,null,"OE_ACB_TRANSFER","24782","SZT","74072900",null,"191002LK","5901988247829","OE - Connexion en cuivre 3x2x 100x10 NW25 3P dans une cassette, avec un pont AlCubar 6300A","OE - Copper connection 3x2x100x10 NW25 3P circuit breaker in a cassette, with an AlCubar 6300A bridge","OE- CONEXION CU 3X2X100X10 PARA NW25 3P, CON ALCUBAR 6300A","Zenergy - Réz csatlakozás 3x2x100x10 NW25 3P megszakító kazettában, AlCubar 6300A híddal"]
["24803","Zenergy - Połączenie miedziane L 2x125x10 Pionowy do Poziomy tor Neutralny AlCubar 4000A",571.6,"1-ZE-01",null,null,"OE_ACB_TRANSFER","24803","SZT","74072900",null,null,"5901988248031","OE - Connexion cuivre L 2x125x10 Trajet neutre vertical vers horizontal AlCubar 4000A","OE - Copper connection L 2x125x10 Vertical to Horizontal track Neutral AlCubar 4000A","ALCUB- CONEXIÓN Cu L 2X125X10 VERTIC. NEUTRO ALCUB- 4000A","Zenergy - Réz csatlakozás L 2x125x10 függőleges-vízszintes sínhez Semleges AlCubar 4000A"]
["24804","Zenergy - Połączenie miedziane L 2x125x10 Pionowy do Poziomy tor Neutralny AlCubar 6300A",830.3,"1-ZE-01",null,null,"OE_ACB_TRANSFER","24804","SZT","74072900",null,null,"5901988248048","OE - Connexion cuivre L 2x125x10 Trajet neutre vertical vers horizontal AlCubar 6300A","OE - Copper connection L 2x125x10 Vertical to Horizontal track Neutral AlCubar 6300A","ALCUB- CONEXIÓN Cu L 2X125X10 VERTIC. NEUTRO ALCUB- 6300A","Zenergy - Réz csatlakozás L 2x125x10 függőleges-vízszintes sín Semleges AlCubar 6300A"]
["24850","Zenergy - Połączenie miedziane 3x30x10 -  EFEN 160A montaż na szynach",503.8,"1-ZE-09",null,null,"OE_MCCB_TRANSFER","24850","SZT","85389099",null,"200131LK","5901988248505","OE - Connexion cuivre 3x30x10 - EFEN 160A montage sur rails","OE - Copper connection 3x30x10 - EFEN 160A mounting on rails","OE- EMPALME Cu 3X30X10- EDEN 160A MONTAJE SOBRE CARRIL","Zenergy - Réz csatlakozás 3x30x10 - EFEN 160A sínre szerelés"]
["24880","Zenergy - Wygrodzenie toru Neutralnego W650",83.1,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","24880","SZT","85389099",null,"200414LK","5901988248802","OE - Clôturer le Neutre L650","OE - W650 Neutral track fence","OE- SEPARADOR NEUTRO W650","Zenergy - Semleges pályakerítés W650"]
["24890","Zenergy - Wygrodzenie toru Neutralnego W1200",97.3,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","24890","SZT","85389099",null,null,"5901988248901","OE - Clôturer le Neutre L1200","OE - W1200 Neutral track fence","OE- W1200 SEPARADOR NEUTRA","Zenergy - A W1200 Semleges pálya kerítése"]
["24894","Zenergy - Wygrodzenie czołowe W1200 3,5MOD",113.1,"1-ZE-01",0.27083333333333331,4,"OE_SEPARATION_BUSBAR","24894","SZT","85389099",null,null,"5901988248949","OE - Cloison avant L1200 3,5MOD","OE - Front barrier W1200 3.5MOD","OE- PROTECCIÓN EMB. W1200 3.5MOD","Zenergy - Első kerítés W1200 3.5MOD"]
["24897","Zenergy - Wygrodzenie poziome dół/góra przedziału D400 do toru PE",282.2,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","24897","SZT","85389099",null,null,"5901988248970","OE - Clôture horizontale vers le bas / haut du compartiment P400 jusqu'à la piste PE","OE - Horizontal barrier at the bottom / top of the D400 compartment to the PE track","OE- PROTECCIÓN HORIZ. EN LA PARTE INFERIOR/SUPERIOR D400","Zenergy - Vízszintes kerítés a D400-as rekesz alján/felül a PE pályához"]
["24909","ZENERGY OM - DRZWI TRANSPARENTNE IP55,   9 MOD,    H550 X W400",261.8,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24409","SZT","85389099","27.12.40.0",null,"5901988249090","OM - Portes transparentes IP55, 9 mod., H550 x L400","OM - Transparent door IP55, 9 mod, H550 x W400","OM- PUERTA TRANSP. IP55, 9 MOD,  H550 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 9 MOD, H550 X W400"]
["24912","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 12 MOD,    H700 X W400",292.60000000000002,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24412","SZT","85389099","27.12.40.0",null,"5901988249120","OM - Portes transparentes IP55, 12 mod, H700 x L400","OM - Transparent door IP55, 12 mod, H700 x W400","OM- PUERTA TRANSP. IP55, 12 MOD,  H700 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 12 MOD, H700 X W400"]
["24921","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 21 MOD,  H1150 X W400",410.2,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24421","SZT","85389099","27.12.40.0",null,"5901988249212","OM - Portes transparentes IP55, 21 mod., H1150 x L400","OM - Transparent door IP55, 21 mod, H1150 x W400","OM- PUERTA TRANSP. IP55, 21 MOD,  H1150 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 21 MOD, H1150 X W400"]
["24928","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 28 MOD,  H1500 X W400",550.1,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24428","SZT","85389099","27.12.40.0",null,"5901988249281","OM - Portes transparentes IP55, 28 mod, H1500 x L400","OM - Transparent door IP55, 28 mod, H1500 x W400","OM- PUERTA TRANSP. IP55, 28 MOD H1500XW400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 28 MOD, H1500 X W400"]
["24936","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 36 MOD,  H1900 X W400",697.5,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","24436","SZT","85389099","27.12.40.0",null,"5901988249366","OM - Portes transparentes IP55, 36 mod, H1900 x L400","OM - Transparent door IP55, 36 mod, H1900 x W400","OM- PUERTA TRANSP. IP55, 36 MOD,  H1900 x W400","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 36 MOD, H1900 X W400"]
["25212","Zenergy OM - Daszek zewnętrzny obudowy IP55, W1200 x D230",438.5,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988252120"]
["25280","Zenergy OM - Daszek zewnętrzny obudowy IP55, W800 x D230",315.39999999999998,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988252809"]
["25312","Zenergy OM - Daszek zewnętrzny obudowy IP55, W1200 x D300",455.8,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988253127"]
["25360","Zenergy OM - Daszek zewnętrzny obudowy IP55, W600 x D300",276.5,null,3.3333333333333333E-2,1,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988253608"]
["25380","Zenergy OM - Daszek zewnętrzny obudowy IP55, W800 x D300",325.10000000000002,null,null,null,"OM_HORIZONTAL_COVER",null,null,"85389099",null,null,"5901988253806"]
["26012","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 12 MOD,    H700 X D230 X W600, WISZĄCA",371.5,"1-ZE-09",0.11666666666666667,5,"OM_ENCLOSURES","26012","SZT","85381000","27.12.40.0",null,"5901988260125","OM - Boîtier de base IP30, 12 mod., H700 x P230 x L600, suspendu","OM - Basic housing IP30, 12 mod, H700 x D230 x W600, hanging","OM- ARMARIO METAL. IP30, 12 MOD,  H700 x D230 x W600, MURAL","ZENERGY OM - ALAP HÁZ IP30, 12 MOD, H700 X D230 X W600, FÜGG."]
["26024","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 24 MOD,  H1300 X D230 X W600, WISZĄCA",549.70000000000005,"1-ZE-09",4.1666666666666664E-2,5,"OM_ENCLOSURES","26024","SZT","85381000","27.12.40.0",null,"5901988260248","OM - Boîtier de base IP30, 24 mod., H1300 x P230 x L600, suspendu","OM - Basic housing IP30, 24 mod, H1300 x D230 x W600, hanging","OM- ARMARIO METAL. IP30, 24 MOD,  H1300 x D230 x W600, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP30, 24 MOD, H1300 X D230 X W600, FÜGG."]
["26029","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 29 MOD,  H1550 X D230 X W600, WISZĄCA",653.4,"1-ZE-09",1.6666666666666666E-2,2,"OM_ENCLOSURES","26029","SZT","85381000","27.12.40.0",null,"5901988260293","OM - Boîtier de base IP30, 29 mod, H1550 x P230 x L600, suspendu","OM - Basic housing IP30, 29 mod, H1550 x D230 x W600, hanging","OM- ARMARIO METAL. IP30, 29 MOD, H1550XD230XW600, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP30, 29 MOD, H1550 X D230 X W600, FÜGG."]
["26109","ZENERGY OM - ROZSZERZENIE IP30,   9 MOD,    H550 X D230 X W600, WISZĄCA",380.2,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26109","SZT","85381000","27.12.40.0",null,"5901988261092","OM - extension IP30, 9 mod, H550 x P230 x L600, suspendu","OM - Extension IP30, 9 mod, H550 x D230 x W600, pendant","OM- MODULO AUX. IP30, 9 MOD,  H550 x D230 x W600, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 9 MOD, H550 X D230 X W600, LAKÓS"]
["26118","ZENERGY OM - ROZSZERZENIE IP30, 18 MOD,  H1000 X D230 X W600, WISZĄCA",487.1,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26118","SZT","85381000","27.12.40.0",null,"5901988261184","OM - extension IP30, 18 mod, H1000 x P230 x L600, suspendu","OM - Extension IP30, 18 mod, H1000 x D230 x W600, hanging","OM- MODULO AUX. IP30, 18 MOD,  H1000 x D230 x W600, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 18 MOD, H1000 X D230 X W600, LAKÓS"]
["26127","ZENERGY OM - ROZSZERZENIE IP30, 27 MOD,  H1450 X D230 X W600, WISZĄCA",619.9,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26127","SZT","85381000","27.12.40.0",null,"5901988261276","OM - Extension IP30, 27 mod, H1450 x P230 x L600, suspendu","OM - Extension IP30, 27 mod, H1450 x D230 x W600, pendant","OM- MODULO AUX. IP30, 27 MOD,  H1450 x D230 x W600, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 27 MOD, H1450 X D230 X W600, LAKÓS"]
["26130","ZENERGY OM - ROZSZERZENIE IP30, 30 MOD,  H1700 X D230 X W600, COKÓŁ 100MM",1068.0999999999999,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26130","SZT","85381000","27.12.40.0",null,"5901988261306","OM - extension IP30, 30 mod, H1700 x P230 x L600, base 100mm","OM - Extension IP30, 30 mod, H1700 x D230 x W600, plinth 100mm","OM- MODULO AUX. IP30, 30 MOD,  H1700 x D230 x W600, ZOCALO 100MM","ZENERGY OM – IP30 BŐVÍTÉS, 30 MOD, H1700 X D230 X W600, lábazat 100 mm"]
["26133","ZENERGY OM - ROZSZERZENIE IP30, 33 MOD,  H1850 X D230 X W600, COKÓŁ 100MM",1179.4000000000001,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26133","SZT","85381000","27.12.40.0",null,"5901988261337","OM - Extension IP30, 33 mod, H1850 x P230 x L600, base 100mm","OM - Extension IP30, 33 mod, H1850 x D230 x W600, plinth 100mm","OM- MODULO AUX. IP30, 33 MOD,  H1850 x D230 x W600, ZOCALO 100MM","ZENERGY OM - IP30 BŐVÍTÉS, 33 MOD, H1850 X D230 X W600, lábazat 100 mm"]
["26206","ZENERGY OM - DRZWI PEŁNE IP30,   6 MOD,    H400 X W600",124.2,"1-ZE-09",null,null,"OM_DOORS",null,"SZT","85389099","27.12.40.0",null,"5901988262068","OM - Portes pleine IP30, 6 mod., H400 x L600","OM - Plain door IP30, 6 mod, H400 x W600","OM- PUERTA OPACA IP30, 6 mods, H400 x W600","ZENERGY OM – TÖMÖR AJTÓ IP30, 6 MOD, H400 X W600"]
["26218","ZENERGY OM - DRZWI PEŁNE IP30, 18 MOD,  H1000 X W600",173.9,"1-ZE-09",0.39166666666666666,2,"OM_DOORS","26218","SZT","85389099","27.12.40.0",null,"5901988262181","OM - Portes pleine IP30, 18 mod., H1000 x L600","OM - Plain door IP30, 18 mod, H1000 x W600","OM- PUERTA OPACA IP30, 18 MOD,  H1000 x W600","ZENERGY OM – TÖMÖR AJTÓ IP30, 18 MOD, H1000 X W600"]
["26227","ZENERGY OM - DRZWI PEŁNE IP30, 27 MOD,  H1450 X W600",244.1,"1-ZE-09",0.55000000000000004,5,"OM_DOORS","26227","SZT","85389099","27.12.40.0",null,"5901988262273","OM - Portes pleine IP30, 27 mod, H1450 x L600","OM - Plain door IP30, 27 mod, H1450 x W600","OM- PUERTA OPACA IP30, 27 MOD,  H1450 x W600","ZENERGY OM – TÖMÖR AJTÓ IP30, 27 MOD, H1450 X W600"]
["26230","ZENERGY OM - DRZWI PEŁNE IP30, 30 MOD,  H1600 X W600",378,"1-ZE-09",0.3,1,"OM_DOORS","26230","SZT","85389099","27.12.40.0",null,"5901988262303","OM - Portes pleine IP30, 30 mod, H1600 x L600","OM - Plain door IP30, 30 mod, H1600 x W600","OM- PUERTA OPACA IP30, 30 MOD,  H1600 x W600","ZENERGY OM – TÖMÖR AJTÓ IP30, 30 MOD, H1600 X W600"]
["26406","ZENERGY OM - DRZWI TRANSPARENTNE IP30,   6 MOD,    H400 X W600",230,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS",null,"SZT","85389099","27.12.40.0",null,"5901988264062","OM - Portes transparentes IP30, 6 mod., H400 x L600","OM - Transparent door IP30, 6 mod, H400 x W600","OM- Puerta transparente IP30, 6 mods, H400 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 6 MOD, H400 X W600"]
["26415","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 15 MOD,    H850 X W600",321.2,"1-ZE-09",0.01,1,"OM_TRANSPARENT_DOORS","26415","SZT","85389099","27.12.40.0",null,"5901988264154","OM - Portes transparentes IP30, 15 mod., H850 x L600","OM - Transparent door IP30, 15 mod, H850 x W600","OM- PUERTA TRANSP. IP30, 15 MOD,  H850 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 15 MOD, H850 X W600"]
["26424","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 24 MOD,  H1300 X W600",478.1,"1-ZE-09",0.01,1,"OM_TRANSPARENT_DOORS","26424","SZT","85389099","27.12.40.0",null,"5901988264246","OM - Portes transparentes IP30, 24 mod., H1300 x L600","OM - Transparent door IP30, 24 mod, H1300 x W600","OM- PUERTA TRANSP. IP30, 24 MOD,  H1300 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 24 MOD, H1300 X W600"]
["26427","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 27 MOD,  H1450 X W600",558.6,"1-ZE-09",0.01,1,"OM_TRANSPARENT_DOORS","26427","SZT","85389099","27.12.40.0",null,"5901988264277","OM - Portes transparentes IP30, 27 mod, H1450 x L600","OM - Transparent door IP30, 27 mod, H1450 x W600","OM- PUERTA TRANSP. IP30, 27 MOD,  H1450 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 27 MOD, H1450 X W600"]
["26430","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 30 MOD,  H1600 X W600",645.5,"1-ZE-09",3.3333333333333333E-2,2,"OM_TRANSPARENT_DOORS","26430","SZT","85389099","27.12.40.0",null,"5901988264307","OM - Portes transparentes IP30, 30 mod, H1600 x L600","OM - Transparent door IP30, 30 mod, H1600 x W600","OM- PUERTA TRANSP. IP30, 30 MOD,  H1600 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 30 MOD, H1600 X W600"]
["26509","ZENERGY OM - OBUDOWA PODSTAWOWA IP55,   9 MOD,    H550 X D230 X W600, WISZĄCA",527,"1-ZE-09",null,null,"OM_ENCLOSURES","26009","SZT","85381000","27.12.40.0",null,"5901988265090","OM - Boîtier de base IP55, 9 mod., H550 x P230 x L600, suspendu","OM - Basic housing IP55, 9 mod, H550 x D230 x W600, hanging","OM- ARMARIO METAL. IP55, 9 MOD,  H550 x D230 x W600, MURAL","ZENERGY OM - ALAP HÁZ IP55, 9 MOD, H550 X D230 X W600, FÜGG."]
["26518","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 18 MOD,  H1000 X D230 X W600, WISZĄCA",665.3,"1-ZE-09",5.8333333333333334E-2,5,"OM_ENCLOSURES","26018","SZT","85381000","27.12.40.0",null,"5901988265182","OM - Boîtier de base IP55, 18 mod, H1000 x P230 x L600, suspendu","OM - Basic housing IP55, 18 mod, H1000 x D230 x W600, hanging","OM- ARMARIO METAL. IP55, 18 MOD,  H1000 x D230 x W600, MURAL","ZENERGY OM - ALAP HÁZ IP55, 18 MOD, H1000 X D230 X W600, FÜGG."]
["26527","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 27 MOD,  H1450 X D230 X W600, WISZĄCA",844.6,"1-ZE-09",null,null,"OM_ENCLOSURES","26027","SZT","85381000","27.12.40.0",null,"5901988265274","OM - Boîtier de base IP55, 27 mod, H1450 x P230 x L600, suspendu","OM - Basic housing IP55, 27 mod, H1450 x D230 x W600, hanging","OM- ARMARIO METAL. IP55, 27 MOD,  H1450 x D230 x W600, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP55, 27 MOD, H1450 X D230 X W600, FÜGG."]
["26533","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 33 MOD,  H1850 X D230 X W600, COKÓŁ 100MM",1396.4,"1-ZE-09",1.6666666666666666E-2,2,"OM_ENCLOSURES","26033","SZT","85381000","27.12.40.0",null,"5901988265335","OM - Boîtier de base IP55, 33 mod, H1850 x P230 x L600, base 100mm","OM - Basic housing IP55, 33 mod, H1850 x D230 x W600, plinth 100mm","OM- ARMARIO METAL. IP55, 33 MOD,  H1850 x D230 x W600, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP55, 33 MOD, H1850 X D230 X W600, lábazat 100 mm"]
["26609","ZENERGY OM - ROZSZERZENIE IP55,   9 MOD,    H550 X D230 X W600, WISZĄCA",541.1,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26109","SZT","85381000","27.12.40.0",null,"5901988266097","OM - Extension IP55, 9 mod, H550 x P230 x L600, suspendu","OM - Extension IP55, 9 mod, H550 x D230 x W600, pendant","OM- MODULO AUX. IP55, 9 MOD,  H550 x D230 x W600, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 9 MOD, H550 X D230 X W600, LAKÓS"]
["26612","ZENERGY OM - ROZSZERZENIE IP55, 12 MOD,    H700 X D230 X W600, WISZĄCA",572.4,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26112","SZT","85381000","27.12.40.0",null,"5901988266127","OM - extension IP55, 12 mod, H700 x P230 x L600, suspendu","OM - Extension IP55, 12 mod, H700 x D230 x W600, pendant","OM- MODULO AUX. IP55, 12 MOD,  H700 x D230 x W600, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 12 MOD, H700 X D230 X W600, LAKÓS"]
["26628","ZENERGY OM - ROZSZERZENIE IP55, 28 MOD,  H1600 X D230 X W600, COKÓŁ 100MM",1217.2,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26128","SZT","85381000","27.12.40.0",null,"5901988266288","OM - extension de IP55, 28 mod, H1600 x P230 x L600, socle 100mm","OM - Extension IP55, 28 mod, H1600 x D230 x W600, plinth 100mm","OM- MODULO AUX. IP55, 28 MOD, H1600XD230XW600, ZOCALO 100 MM","ZENERGY OM – IP55 BŐVÍTÉS, 28 MOD, H1600 X D230 X W600, lábazat 100 mm"]
["26629","ZENERGY OM - ROZSZERZENIE IP55, 29 MOD,  H1550 X D230 X W600, WISZĄCA",970.9,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26129","SZT","85381000","27.12.40.0",null,"5901988266295","OM - Extension IP55, 29 mod, H1550 x P230 x L600, suspendu","OM - Extension IP55, 29 mod, H1550 x D230 x W600, pendant","OM- MODULO AUX. IP55, 29 MOD, H1550XD230XW600, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 29 MOD, H1550 X D230 X W600, LAKÓS"]
["26639","ZENERGY OM - ROZSZERZENIE IP55, 39 MOD,  H2150 X D230 X W600, COKÓŁ 100MM",1649.2,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","26139","SZT","85381000","27.12.40.0",null,"5901988266394","OM - Extension IP55, 39 mod, H2150 x P230 x L600, base 100mm","OM - Extension IP55, 39 mod, H2150 x D230 x W600, plinth 100mm","OM- MODULO AUX. IP55, 39 MOD,  H2150 x D230 x W600, ZOCALO 100MM","ZENERGY OM - IP55 BŐVÍTÉS, 39 MOD, H2150 X D230 X W600, lábazat 100 mm"]
["26715","ZENERGY OM - DRZWI PEŁNE IP55, 15 MOD,    H850 X W600",312.10000000000002,"1-ZE-09",5.8333333333333334E-2,4,"OM_DOORS","26215","SZT","85389099","27.12.40.0",null,"5901988267155","OM - Portes pleine IP55, 15 mod., H850 x L600","OM - Plain door IP55, 15 mod, H850 x W600","OM- PUERTA OPACA IP55, 15 MOD,  H850 x W600","ZENERGY OM – TÖMÖR AJTÓ IP55, 15 MOD, H850 X W600"]
["26724","ZENERGY OM - DRZWI PEŁNE IP55, 24 MOD,  H1300 X W600",393.1,"1-ZE-09",8.3333333333333329E-2,4,"OM_DOORS","26224","SZT","85389099","27.12.40.0",null,"5901988267247","OM - Portes pleine IP55, 24 mod., H1300 x L600","OM - Plain door IP55, 24 mod, H1300 x W600","OM- PUERTA OPACA IP55, 24 MOD,  H1300 x W600","ZENERGY OM – TÖMÖR AJTÓ IP55, 24 MOD, H1300 X W600"]
["26730","ZENERGY OM - DRZWI PEŁNE IP55, 30 MOD,  H1600 X W600",537.79999999999995,"1-ZE-09",6.6666666666666666E-2,5,"OM_DOORS","26230","SZT","85389099","27.12.40.0",null,"5901988267308","OM - Portes pleine IP55, 30 mod., H1600 x L600","OM - Plain door IP55, 30 mod, H1600 x W600","OM- PUERTA OPACA IP55, 30 MOD,  H1600 x W600","ZENERGY OM – TÖMÖR AJTÓ IP55, 30 MOD, H1600 X W600"]
["26739","ZENERGY OM - DRZWI PEŁNE IP55, 39 MOD,  H2050 X W600",665.3,"1-ZE-09",0.11666666666666667,1,"OM_DOORS","26239","SZT","85389099","27.12.40.0",null,"5901988267391","OM - Portes pleine IP55, 39 mod, H2050 x L600","OM - Plain door IP55, 39 mod, H2050 x W600","OM- PUERTA OPACA IP55, 39 MOD,  H2050 x W600","ZENERGY OM – TÖMÖR AJTÓ IP55, 39 MOD, H2050 X W600"]
["26906","ZENERGY OM - DRZWI TRANSPARENTNE IP55,   6 MOD,    H400 X W600",336,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS",null,"SZT","85389099","27.12.40.0",null,"5901988269067","OM - Portes transparentes IP55, 6 mod., H400 x L600","OM - Transparent door IP55, 6 mod, H400 x W600","OM- Puerta transparente IP55, 6 mod, H400 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 6 MOD, H400 X W600"]
["26915","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 15 MOD,    H850 X W600",451.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","26415","SZT","85389099","27.12.40.0",null,"5901988269159","OM - Portes transparentes IP55, 15 mod., H850 x L600","OM - Transparent door IP55, 15 mod, H850 x W600","OM- PUERTA TRANSP. IP55, 15 MOD,  H850 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 15 MOD, H850 X W600"]
["26924","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 24 MOD,  H1300 X W600",629.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","26424","SZT","85389099","27.12.40.0",null,"5901988269241","OM - Portes transparentes IP55, 24 mod., H1300 x L600","OM - Transparent door IP55, 24 mod, H1300 x W600","OM- PUERTA TRANSP. IP55, 24 MOD,  H1300 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 24 MOD, H1300 X W600"]
["26930","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 30 MOD,  H1600 X W600",796.1,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","26430","SZT","85389099","27.12.40.0",null,"5901988269302","OM - Portes transparentes IP55, 30 mod., H1600 x L600","OM - Transparent door IP55, 30 mod, H1600 x W600","OM- PUERTA TRANSP. IP55, 30 MOD,  H1600 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 30 MOD, H1600 X W600"]
["26939","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 39 MOD,  H2050 X W600",1017.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","26439","SZT","85389099","27.12.40.0",null,"5901988269395","OM - Portes transparentes IP55, 39 mod, H2050 x L600","OM - Transparent door IP55, 39 mod, H2050 x W600","OM- PUERTA TRANSP. IP55, 39 MOD,  H2050 x W600","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 39 MOD, H2050 X W600"]
["27593","ZENERGY - OSŁONA CZOŁOWA HGP 400-630 3/4P, W450, 9M / 300, PIONOWO, DŹWIGNIA",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","27593","SZT","85389099",null,null,"5901988275938","OE - COUVERCLE AVANT HGP 400-630 3/4P, L450, 9M / 300, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W450, 9M / 300, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W450, 9M (450mm) VERT.","ZENERGY - ELSŐ BURKOLAT HGP 400-630 3/4P, W450, 9M / 300, FÜGGŐLEGES, KAR"]
["27758","ZENERGY - OSŁONA CZOŁOWA HGP 400-630 4P, W650, 5M / 500, POZIOMO, DŹWIGNIA",76.3,"1-ZE-01",0.05,2,"OE_MCCB_COVERS","27758","SZT","85389099",null,null,"5901988277581","OE - COUVERCLE AVANT HGP 400-630 4P, L650, 5M / 500, HORIZONTAL, LEVIER","OE - Front cover HGP 400-630 4P, W650, 5M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGP 400-630 4P, W650, 5M (250mm) HORIZ. ","ZENERGY - ELSŐ BURKOLAT HGP 400-630 4P, W650, 5M / 500, VÍZSZINTES, KAR"]
["27793","ZENERGY - OSŁONA CZOŁOWA HGP 400-630 3/4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",5.8333333333333334E-2,2,"OE_MCCB_COVERS","27793","SZT","85389099",null,null,"5901988277932","OE - COUVERCLE AVANT HGP 400-630 3/4P, L650, 9M / 500, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W650, 9M (450mm)VERT.","ZENERGY - ELSŐ BURKOLAT HGP 400-630 3/4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["27794","ZENERGY - OSŁONA CZOŁOWA HGP 800 3P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","27794","SZT","8538909900",null,null,"5901988277949","OE - COUVERCLE AVANT HGP 800 3P, L650, 9M / 500, VERTICAL, LEVIER","OE - Front cover HGP 800 3P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGP 800 3P, W650, 9M (450mm) VERT.","ZENERGY - ELSŐ BURKOLAT HGP 800 3P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["27958","ZENERGY - OSŁONA CZOŁOWA HGP 400-630 4P, W850, 5M / 700, POZIOMO, DŹWIGNIA",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","27958","SZT","85389099",null,null,"5901988279585","OE - COUVERCLE AVANT HGP 400-630 4P, L850, 5M / 700, HORIZONTAL, LEVIER","OE - Front cover HGP 400-630 4P, W850, 5M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP 400-630 4P, W850, 5M (250mm) HORIZ. ","ZENERGY - ELSŐ BURKOLAT HGP 400-630 4P, W850, 5M / 700, VÍZSZINTES, KAR"]
["27993","ZENERGY - OSŁONA CZOŁOWA HGP 400-630 3/4P, W850, 9M / 700, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",1.6666666666666666E-2,1,"OE_MCCB_COVERS","27993","SZT","85389099",null,null,"5901988279936","OE - COUVERCLE AVANT HGP 400-630 3/4P, L850, 9M / 700, VERTICAL, LEVIER","OE - Front cover HGP 400-630 3/4P, W850, 9M / 700, Vertical, Lever","ZEN- TAPA TROQ. HGP 400-630 3/4P, W850, 9M (450mm) VERT.","ZENERGY - ELSŐ BURKOLAT HGP 400-630 3/4P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["28012","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 12 MOD,    H700 X D230 X W800, WISZĄCA",477.4,"1-ZE-09",null,null,"OM_ENCLOSURES","28012","SZT","85381000","27.12.40.0",null,"5901988280123","OM - Boîtier de base IP30, 12 mod., H700 x P230 x L800, suspendu","OM - Basic housing IP30, 12 mod, H700 x D230 x W800, hanging","OM- ARMARIO METAL. IP30, 12 MOD,  H700 x D230 x W800, MURAL","ZENERGY OM - ALAP HÁZ IP30, 12 MOD, H700 X D230 X W800, FÜGG."]
["28021","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 21 MOD,  H1150 X D230 X W800, WISZĄCA",612.4,"1-ZE-09",0.01,1,"OM_ENCLOSURES","28021","SZT","85381000","27.12.40.0",null,"5901988280215","OM - Boîtier de base IP30, 21 mod, H1150 x P230 x L800, suspendu","OM - Basic housing IP30, 21 mod, H1150 x D230 x W800, hanging","OM- ARMARIO METAL. IP30, 21 MOD,  H1150 x D230 x W800, MURAL","ZENERGY OM - ALAP HÁZ IP30, 21 MOD, H1150 X D230 X W800, FÜGG."]
["28030","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 30 MOD,  H1700 X D230 X W800, COKÓŁ 100MM",1193.4000000000001,"1-ZE-09",null,null,"OM_ENCLOSURES","28030","SZT","85381000","27.12.40.0",null,"5901988280307","OM - Boîtier de base IP30, 30 mod, H1700 x P230 x L800, base 100mm","OM - Basic housing IP30, 30 mod, H1700 x D230 x W800, plinth 100mm","OM- ARMARIO METAL. IP30, 30 MOD,  H1700 x D230 x W800, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 30 MOD, H1700 X D230 X W800, lábazat 100 mm"]
["28039","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 39 MOD,  H2150 X D230 X W800, COKÓŁ 100MM",1685.9,"1-ZE-09",0.01,1,"OM_ENCLOSURES","28039","SZT","85381000","27.12.40.0",null,"5901988280390","OM - Boîtier de base IP30, 39 mod, H2150 x P230 x L800, borne 100 mm","OM - Basic housing IP30, 39 mod, H2150 x D230 x W800, plinth 100mm","OM- ARMARIO METAL. IP30, 39 MOD,  H2150 x D230 x W800, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 39 MOD, H2150 X D230 X W800, lábazat 100 mm"]
["28115","ZENERGY OM - ROZSZERZENIE IP30, 15 MOD,    H850 X D230 X W800, WISZĄCA",545.4,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28115","SZT","85381000","27.12.40.0",null,"5901988281151","OM - extension IP30, 15 mod, H850 x P230 x L800, suspendu","OM - Extension IP30, 15 mod, H850 x D230 x W800, hanging","OM- MODULO AUX. IP30, 15 MOD,  H850 x D230 x W800, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 15 MOD, H850 X D230 X W800, LAKÓS"]
["28118","ZENERGY OM - ROZSZERZENIE IP30, 18 MOD,  H1000 X D230 X W800, WISZĄCA",607,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28118","SZT","85381000","27.12.40.0",null,"5901988281182","OM - extension IP30, 18 mod, H1000 x P230 x L800, suspendu","OM - Extension IP30, 18 mod, H1000 x D230 x W800, hanging","OM- MODULO AUX. IP30, 18 MOD,  H1000 x D230 x W800, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 18 MOD, H1000 X D230 X W800, LAKÓS"]
["28127","ZENERGY OM - ROZSZERZENIE IP30, 27 MOD,  H1450 X D230 X W800, WISZĄCA",712.8,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28127","SZT","85381000","27.12.40.0",null,"5901988281274","OM - Extension IP30, 27 mod, H1450 x P230 x L800, suspendu","OM - Extension IP30, 27 mod, H1450 x D230 x W800, hanging","OM- MODULO AUX. IP30, 27 MOD,  H1450 x D230 x W800, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 27 MOD, H1450 X D230 X W800, LAKÓS"]
["28130","ZENERGY OM - ROZSZERZENIE IP30, 30 MOD,  H1700 X D230 X W800, COKÓŁ 100MM",1239.8,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28130","SZT","85381000","27.12.40.0",null,"5901988281304","OM - Extension IP30, 30 mod, H1700 x P230 x L800, base 100 mm","OM - Extension IP30, 30 mod, H1700 x D230 x W800, plinth 100mm","OM- MODULO AUX. IP30, 30 MOD,  H1700 x D230 x W800, ZOCALO 100MM","ZENERGY OM – IP30 BŐVÍTÉS, 30 MOD, H1700 X D230 X W800, lábazat 100 mm"]
["28209","ZENERGY OM - DRZWI PEŁNE IP30,   9 MOD,    H550 X W800",175,"1-ZE-09",3.3333333333333333E-2,2,"OM_DOORS","28209","SZT","85389099","27.12.40.0",null,"5901988282097","OM - Portes pleine IP30, 9 mod., H550 x L800","OM - Plain door IP30, 9 mod, H550 x W800","OM- PUERTA OPACA IP30, 9 MOD,  H550 x W800","ZENERGY OM – TÖMÖR AJTÓ IP30, 9 MOD, H550 X W800"]
["28218","ZENERGY OM - DRZWI PEŁNE IP30, 18 MOD,  H1000 X W800",229,"1-ZE-09",4.1666666666666664E-2,2,"OM_DOORS","28218","SZT","85389099","27.12.40.0",null,"5901988282189","OM - Portes pleine IP30, 18 mod., H1000 x L800","OM - Plain door IP30, 18 mod, H1000 x W800","OM- PUERTA OPACA IP30, 18 MOD,  H1000 x W800","ZENERGY OM – TÖMÖR AJTÓ IP30, 18 MOD, H1000 X W800"]
["28228","ZENERGY OM - DRZWI PEŁNE IP30, 28 MOD,  H1500 X W800",343.4,"1-ZE-09",0.01,1,"OM_DOORS","28228","SZT","85389099","27.12.40.0",null,"5901988282288","OM - Portes pleine IP30, 28 mod, H1500 x L800","OM - Plain door IP30, 28 mod, H1500 x W800","OM- PUERTA OPACA IP30, 28 MOD H1500XW800","ZENERGY OM – TÖMÖR AJTÓ IP30, 28 MOD, H1500 X W800"]
["28233","ZENERGY OM - DRZWI PEŁNE IP30, 33 MOD,  H1750 X W800",476.3,"1-ZE-09",0.10833333333333334,5,"OM_DOORS","28233","SZT","85389099","27.12.40.0",null,"5901988282332","OM - Portes pleine IP30, 33 mod, H1750 x L800","OM - Plain door IP30, 33 mod, H1750 x W800","OM- PUERTA OPACA IP30, 33 MOD,  H1750 x W800","ZENERGY OM – TÖMÖR AJTÓ IP30, 33 MOD, H1750 X W800"]
["28238","Zenergy OM - Drzwi pełne IP30, H1950 X W850 / prostownik Elektra",572.4,null,3.3333333333333333E-2,1,"OM_DOORS",null,null,"85389099",null,null,"5901988282387"]
["28239","ZENERGY OM - DRZWI PEŁNE IP30, 39 MOD,  H2050 X W800",581,"1-ZE-09",0.05,1,"OM_DOORS","28239","SZT","85389099","27.12.40.0",null,"5901988282394","OM - Portes pleine IP30, 39 mod, H2050 x L800","OM - Plain door IP30, 39 mod, H2050 x W800","OM- PUERTA OPACA IP30, 39 MOD,  H2050 x W800","ZENERGY OM – TÖMÖR AJTÓ IP30, 39 MOD, H2050 X W800"]
["28415","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 15 MOD,    H850 X W800",425.1,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","28415","SZT","85389099","27.12.40.0",null,"5901988284152","OM - Portes transparentes IP30, 15 mod, H850 x L800","OM - Transparent door IP30, 15 mod, H850 x W800","OM- PUERTA TRANSP. IP30, 15 MOD,  H850 x W800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 15 MOD, H850 X W800"]
["28427","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 27 MOD,  H1450 X W800",710.2,"1-ZE-09",0.01,1,"OM_TRANSPARENT_DOORS","28427","SZT","85389099","27.12.40.0",null,"5901988284275","OM - Portes transparentes IP30, 27 mod, H1450 x L800","OM - Transparent door IP30, 27 mod, H1450 x W800","OM- PUERTA TRANSP. IP30, 27 MOD,  H1450 x W800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 27 MOD, H1450 X W800"]
["28430","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 30 MOD,  H1600 X W800",790.8,"1-ZE-09",1.6666666666666666E-2,2,"OM_TRANSPARENT_DOORS","28430","SZT","85389099","27.12.40.0",null,"5901988284305","OM - Portes transparentes IP30, 30 mod, H1600 x L800","OM - Transparent door IP30, 30 mod, H1600 x W800","OM- PUERTA TRANSP. IP30, 30 MOD,  H1600 x W800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 30 MOD, H1600 X W800"]
["28437","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 39U,  H1950 X W800",978.5,"1-ZE-09",0.05,1,"OM_TRANSPARENT_DOORS",null,"SZT","85389099","27.12.40.0",null,null,null,null,null,"ZENERGY OM – ÁTLÁTSZÓ AJTÓK IP30, 39U, H1950 X W800"]
["28515","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 15 MOD,    H850 X D230 X W800, WISZĄCA",752.8,"1-ZE-09",null,null,"OM_ENCLOSURES","28015","SZT","85381000","27.12.40.0",null,"5901988285159","OM - Boîtier de base IP55, 15 mod, H850 x P230 x L800, suspendu","OM - Basic housing IP55, 15 mod, H850 x D230 x W800, hanging","OM- ARMARIO METAL. IP55, 15 MOD,  H850 x D230 x W800, MURAL","ZENERGY OM - IP55 ALAP HÁZ, 15 MOD, H850 X D230 X W800, FÜGG."]
["28524","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 24 MOD,  H1300 X D230 X W800, WISZĄCA",911.5,"1-ZE-09",1.6666666666666666E-2,2,"OM_ENCLOSURES","28024","SZT","85381000","27.12.40.0",null,"5901988285241","OM - Boîtier de base IP55, 24 modules, H1300 x P230 x L800, suspendu","OM - Basic housing IP55, 24 mod, H1300 x D230 x W800, hanging","OM- ARMARIO METAL. IP55, 24 MOD,  H1300 x D230 x W800, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP55, 24 MOD, H1300 X D230 X W800, FÜGG."]
["28529","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 29 MOD,  H1550 X D230 X W800, WISZĄCA",1049.8,"1-ZE-09",null,null,"OM_ENCLOSURES","28029","SZT","85381000","27.12.40.0",null,"5901988285296","OM - Boîtier de base IP55, 29 mod, H1550 x P230 x L800, suspendu","OM - Basic housing IP55, 29 mod, H1550 x D230 x W800, hanging","OM- ARMARIO METAL. IP55, 29 MOD, H1550XD230XW800, MURAL","ZENERGY OM - IP55 ALAP HÁZ, 29 MOD, H1550 X D230 X W800, FÜGG."]
["28530","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 30 MOD,  H1700 X D230 X W800, COKÓŁ 100MM",1441.8,"1-ZE-09",0.01,1,"OM_ENCLOSURES","28030","SZT","85381000","27.12.40.0",null,"5901988285302","OM - Boîtier de base IP55, 30 mod, H1700 x P230 x L800, socle 100 mm","OM - Basic housing IP55, 30 mod, H1700 x D230 x W800, plinth 100mm","OM- ARMARIO METAL. IP55, 30 MOD,  H1700 x D230 x W800, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP55, 30 MOD, H1700 X D230 X W800, lábazat 100 mm"]
["28615","ZENERGY OM - ROZSZERZENIE IP55, 15 MOD,    H850 X D230 X W800, WISZĄCA",775.4,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28115","SZT","85381000","27.12.40.0",null,"5901988286156","OM - extension IP55, 15 mod, H850 x P230 x L800, suspendu","OM - Extension IP55, 15 mod, H850 x D230 x W800, hanging","OM- MODULO AUX. IP55, 15 MOD,  H850 x D230 x W800, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 15 MOD, H850 X D230 X W800, LAKÓS"]
["28621","ZENERGY OM - ROZSZERZENIE IP55, 21 MOD,  H1150 X D230 X W800, WISZĄCA",891,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28121","SZT","85381000","27.12.40.0",null,"5901988286217","OM - extension IP55, 21 mod, H1150 x P230 x L800, suspendu","OM - Extension IP55, 21 mod, H1150 x D230 x W800, pendant","OM- MODULO AUX. IP55, 21 MOD,  H1150 x D230 x W800, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 21 MOD, H1150 X D230 X W800, LAKÓS"]
["28628","ZENERGY OM - ROZSZERZENIE IP55, 28 MOD,  H1600 X D230 X W800, COKÓŁ 100MM",1390,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28128","SZT","85381000","27.12.40.0",null,"5901988286286","OM - extension de IP55, 28 mod, H1600 x P230 x L800, socle 100mm","OM - Extension IP55, 28 mod, H1600 x D230 x W800, plinth 100mm","OM- MODULO AUX. IP55, 28 MOD, H1600XD230XW800, ZOCALO 100 MM","ZENERGY OM – IP55 BŐVÍTÉS, 28 MOD, H1600 X D230 X W800, lábazat 100 mm"]
["28633","ZENERGY OM - ROZSZERZENIE IP55, 33 MOD,  H1850 X D230 X W800, COKÓŁ 100MM",1672.9,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS","28133","SZT","85381000","27.12.40.0",null,"5901988286330","OM - extension de IP55, 33 mod, H1850 x P230 x L800, socle 100mm","OM - Extension IP55, 33 mod, H1850 x D230 x W800, plinth 100mm","OM- MODULO AUX. IP55, 33 MOD,  H1850 x D230 x W800, ZOCALO 100MM","ZENERGY OM – IP55 BŐVÍTÉS, 33 MOD, H1850 X D230 X W800, lábazat 100 mm"]
["28712","ZENERGY OM - DRZWI PEŁNE IP55, 12 MOD,    H700 X W800",283,"1-ZE-09",null,null,"OM_DOORS","28212","SZT","85389099","27.12.40.0",null,"5901988287122","OM - Portes pleine IP55, 12 mod, H700 x L800","OM - Plain door IP55, 12 mod, H700 x W800","OM- PUERTA OPACA IP55, 12 MOD,  H700 x W800","ZENERGY OM – TÖMÖR AJTÓ IP55, 12 MOD, H700 X W800"]
["28721","ZENERGY OM - DRZWI PEŁNE IP55, 21 MOD,  H1150 X W800",397.4,"1-ZE-09",null,null,"OM_DOORS","28221","SZT","85389099","27.12.40.0",null,"5901988287214","OM - Portes pleine IP55, 21 mod, H1150 x L800","OM - Plain door IP55, 21 mod, H1150 x W800","OM- PUERTA OPACA IP55, 21 MOD,  H1150 x W800","ZENERGY OM – TÖMÖR AJTÓ IP55, 21 MOD, H1150 X W800"]
["28724","ZENERGY OM - DRZWI PEŁNE IP55, 24 MOD,  H1300 X W800",454.7,"1-ZE-09",4.1666666666666664E-2,4,"OM_DOORS","28224","SZT","85389099","27.12.40.0",null,"5901988287245","OM - Portes pleine IP55, 24 mod., H1300 x L800","OM - Plain door IP55, 24 mod, H1300 x W800","OM- PUERTA OPACA IP55, 24 MOD,  H1300 x W800","ZENERGY OM – TÖMÖR AJTÓ IP55, 24 MOD, H1300 X W800"]
["28729","ZENERGY OM - DRZWI PEŁNE IP55, 29 MOD,  H1550 X W800",583.20000000000005,"1-ZE-09",null,null,"OM_DOORS","28229","SZT","85389099","27.12.40.0",null,"5901988287290","OM - Portes pleine IP55, 29 mod, H1550 x L800","OM - Plain door IP55, 29 mod, H1550 x W800","OM- PUERTA OPACA IP55, 29 MOD, H1550XW800","ZENERGY OM – TÖMÖR AJTÓ IP55, 29 MOD, H1550 X W800"]
["28736","ZENERGY OM - DRZWI PEŁNE IP55, 36 MOD,  H1900 X W800",723.6,"1-ZE-09",5.8333333333333334E-2,4,"OM_DOORS","28236","SZT","85389099","27.12.40.0",null,"5901988287368","OM - Portes pleine IP55, 36 mod, H1900 x L800","OM - Plain door IP55, 36 mod, H1900 x W800","OM- PUERTA OPACA IP55, 36 MOD,  H1900 x W800","ZENERGY OM – TÖMÖR AJTÓ IP55, 36 MOD, H1900 X W800"]
["28912","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 12 MOD,    H700 X W800",455.8,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","28412","SZT","85389099","27.12.40.0",null,"5901988289126","OM - Portes transparentes IP55, 12 mod., H700 x L800","OM - Transparent door IP55, 12 mod, H700 x W800","OM- PUERTA TRANSP. IP55, 12 MOD,  H700 x W800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 12 MOD, H700 X W800"]
["28921","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 21 MOD,  H1150 X W800",612.70000000000005,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","28421","SZT","85389099","27.12.40.0",null,"5901988289218","OM - Portes transparentes IP55, 21 mod, H1150 x L800","OM - Transparent door IP55, 21 mod, H1150 x W800","OM- PUERTA TRANSP. IP55, 21 MOD,  H1150 x W800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 21 MOD, H1150 X W800"]
["28928","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 28 MOD,  H1500 X W800",805.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","28428","SZT","85389099","27.12.40.0",null,"5901988289287","OM - Portes transparentes IP55, 28 mod, H1500 x L800","OM - Transparent door IP55, 28 mod, H1500 x W800","OM- PUERTA TRANSP. IP55, 28 MOD H1500XW800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 28 MOD, H1500 X W800"]
["28936","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 36 MOD,  H1900 X W800",1009.1,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","28436","SZT","85389099","27.12.40.0",null,"5901988289362","OM - Portes transparentes IP55, 36 mod, H1900 x L800","OM - Transparent door IP55, 36 mod, H1900 x W800","OM- PUERTA TRANSP. IP55, 36 MOD,  H1900 x W800","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 36 MOD, H1900 X W800"]
["29009","ZENERGY OM - OBUDOWA PODSTAWOWA IP30,   9 MOD,    H550 X D230 X W1000, WISZĄCA",544.29999999999995,"1-ZE-09",null,null,"OM_ENCLOSURES","29009","SZT","85381000","27.12.40.0",null,"5901988290092","OM - Boîtier de base IP30, 9 mod., H550 x P230 x L1000, suspendu","OM - Basic housing IP30, 9 mod, H550 x D230 x W1000, hanging","OM- ARMARIO METAL. IP30,  9 MOD,  H550 x D230 x W1000, MURAL","ZENERGY OM - ALAP HÁZ IP30, 9 MOD, H550 X D230 X W1000, FÜGG."]
["29012","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 12 MOD,    H700 X D230 X W1000, WISZĄCA",549.70000000000005,"1-ZE-09",null,null,"OM_ENCLOSURES","29012","SZT","85381000","27.12.40.0",null,"5901988290122","OM - Boîtier de base IP30, 12 mod, H700 x P230 x L1000, suspendu","OM - Basic housing IP30, 12 mod, H700 x D230 x W1000, hanging","OM- ARMARIO METAL. IP30, 12 MOD,  H700 x D230 x W1000, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP30, 12 MOD, H700 X D230 X W1000, FÜGG."]
["29021","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 21 MOD,  H1150 X D230 X W1000, WISZĄCA",698.8,"1-ZE-09",null,null,"OM_ENCLOSURES","29021","SZT","85381000","27.12.40.0",null,"5901988290214","OM - Boîtier de base IP30, 21 mod, H1150 x P230 x L1000, suspendu","OM - Basic housing IP30, 21 mod, H1150 x D230 x W1000, hanging","OM- ARMARIO METAL. IP30, 21 MOD,  H1150 x D230 x W1000, MURAL","ZENERGY OM - ALAP HÁZ IP30, 21 MOD, H1150 X D230 X W1000, FÜGG."]
["29028","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 28 MOD,  H1600 X D230 X W1000, COKÓŁ 100MM",1248.5,"1-ZE-09",0.01,1,"OM_ENCLOSURES","29028","SZT","85381000","27.12.40.0",null,"5901988290283","OM - Boîtier de base IP30, 28 mod, H1600 x P230 x L1000, base 100mm","OM - Basic housing IP30, 28 mod, H1600 x D230 x W1000, plinth 100mm","OM- ARMARIO METAL. IP30, 28 MOD,  H1600 x D230 x W1000, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 28 MOD, H1600 X D230 X W1000, lábazat 100 mm"]
["29036","ZENERGY OM - OBUDOWA PODSTAWOWA IP30, 36 MOD,  H2000 X D230 X W1000, COKÓŁ 100MM",1749.6,"1-ZE-09",null,null,"OM_ENCLOSURES","29036","SZT","85381000","27.12.40.0",null,"5901988290368","OM - Boîtier de base IP30, 36 mod, H2000 x P230 x L1000, base 100mm","OM - Basic housing IP30, 36 mod, H2000 x D230 x W1000, plinth 100mm","OM- ARMARIO METAL. IP30, 36 MOD,  H2000 x D230 x W1000, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP30, 36 MOD, H2000 X D230 X W1000, lábazat 100 mm"]
["29112","ZENERGY OM - ROZSZERZENIE IP30, 12 MOD,    H700 X D230 X W1000, WISZĄCA",568.1,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988291129","OM - Extension IP30, 12 mod, H700 x P230 x L1000, suspendu","OM - Extension IP30, 12 mod, H700 x D230 x W1000, hanging","OM- MODULO AUX. IP30, 12 MOD,  H700 x D230 x W1000, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 12 MOD, H700 X D230 X W1000, LAKÓS"]
["29121","ZENERGY OM - ROZSZERZENIE IP30, 21 MOD,  H1150 X D230 X W1000, WISZĄCA",730.1,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988291211","OM - extension IP30, 21 mod, H1150 x P230 x L1000, suspendu","OM - Extension IP30, 21 mod, H1150 x D230 x W1000, pendant","OM- MODULO AUX. IP30, 21 MOD,  H1150 x D230 x W1000, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 21 MOD, H1150 X D230 X W1000, LAKÓS"]
["29129","ZENERGY OM - ROZSZERZENIE IP30, 29 MOD,  H1550 X D230 X W1000, WISZĄCA",891,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988291297","OM - Extension IP30, 29 mod, H1550 x P230 x L1000, suspendu","OM - Extension IP30, 29 mod, H1550 x D230 x W1000, pendant","OM- MODULO AUX. IP30, 29 MOD,  H1550 x D230 x W1000, MURAL","ZENERGY OM - IP30 BŐVÍTÉS, 29 MOD, H1550 X D230 X W1000, LAKÓS"]
["29130","ZENERGY OM - ROZSZERZENIE IP30, 30 MOD,  H1700 X D230 X W1000, COKÓŁ 100MM",1413.7,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988291303","OM - Extension IP30, 30 mod, H1700 x P230 x L1000, base 100mm","OM - Extension IP30, 30 mod, H1700 x D230 x W1000, plinth 100mm","OM- MODULO AUX. IP30, 30 MOD,  H1700 x D230 x W1000, ZOCALO 100MM","ZENERGY OM - IP30 BŐVÍTÉS, 30 MOD, H1700 X D230 X W1000, lábazat 100 mm"]
["29209","ZENERGY OM - DRZWI PEŁNE IP30,   9 MOD,    H550 X W1000",200.9,"1-ZE-09",null,null,"OM_DOORS","29209","SZT","85389099","27.12.40.0",null,"5901988292096","OM - Portes pleine IP30, 9 mod., H550 x L1000","OM - Plain door IP30, 9 mod, H550 x W1000","OM- PUERTA OPACA IP30,   9 MOD,   H550 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP30, 9 MOD, H550 X W1000"]
["29218","ZENERGY OM - DRZWI PEŁNE IP30, 18 MOD,  H1000 X W1000",261.39999999999998,"1-ZE-09",null,null,"OM_DOORS","29218","SZT","85389099","27.12.40.0",null,"5901988292188","OM - Portes pleine IP30, 18 mod., H1000 x L1000","OM - Plain door IP30, 18 mod, H1000 x W1000","OM- PUERTA OPACA IP30, 18 MOD,  H1000 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP30, 18 MOD, H1000 X W1000"]
["29227","ZENERGY OM - DRZWI PEŁNE IP30, 27 MOD,  H1450 X W1000",290.5,"1-ZE-09",null,null,"OM_DOORS","29227","SZT","85389099","27.12.40.0",null,"5901988292270","OM - Portes pleine IP30, 27 mod, H1450 x L1000","OM - Plain door IP30, 27 mod, H1450 x W1000","OM- PUERTA OPACA IP30, 27 MOD,  H1450 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP30, 27 MOD, H1450 X W1000"]
["29233","ZENERGY OM - DRZWI PEŁNE IP30, 33 MOD,  H1750 X W1000",650.20000000000005,"1-ZE-09",null,null,"OM_DOORS","29233","SZT","85389099","27.12.40.0",null,"5901988292331","OM - Portes pleine IP30, 33 mod, H1750 x L1000","OM - Plain door IP30, 33 mod, H1750 x W1000","OM- PUERTA OPACA IP30, 33 MOD,  H1750 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP30, 33 MOD, H1750 X W1000"]
["29409","ZENERGY OM - DRZWI TRANSPARENTNE IP30,   9 MOD,    H550 X W1000",398.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29409","SZT","85389099","27.12.40.0",null,"5901988294090","OM - Portes transparentes IP30, 9 mod., H550 x L1000","OM - Transparent door IP30, 9 mod, H550 x W1000","OM- PUERTA TRANSP. IP30,  9 MOD,  H550 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 9 MOD, H550 X W1000"]
["29421","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 21 MOD,  H1150 X W1000",628.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29421","SZT","85389099","27.12.40.0",null,"5901988294212","OM - Portes transparentes IP30, 21 mod, H1150 x L1000","OM - Transparent door IP30, 21 mod, H1150 x W1000","OM- PUERTA TRANSP. IP30, 21 MOD,  H1150 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 21 MOD, H1150 X W1000"]
["29428","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 28 MOD,  H1500 X W1000",845.9,"1-ZE-09",0.01,1,"OM_TRANSPARENT_DOORS","29428","SZT","85389099","27.12.40.0",null,"5901988294281","OM - Portes transparentes IP30, 28 mod, H1500 x L1000","OM - Transparent door IP30, 28 mod, H1500 x W1000","OM- PUERTA TRANSP. IP30, 28 MOD,  H1500 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 28 MOD, H1500 X W1000"]
["29433","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 33 MOD,  H1750 X W1000",978.4,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29433","SZT","85389099","27.12.40.0",null,"5901988294335","OM - Portes transparentes IP30, 33 mod, H1750 x L1000","OM - Transparent door IP30, 33 mod, H1750 x W1000","OM- PUERTA TRANSP. IP30, 33 MOD,  H1750 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 33 MOD, H1750 X W1000"]
["29436","ZENERGY OM - DRZWI TRANSPARENTNE IP30, 36 MOD,  H1900 X W1000",1071.7,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29436","SZT","85389099","27.12.40.0",null,"5901988294366","OM - Portes transparentes IP30, 36 mod, H1900 x L1000","OM - Transparent door IP30, 36 mod, H1900 x W1000","OM- PUERTA TRANSP. IP30, 36 MOD,  H1900 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP30, 36 MOD, H1900 X W1000"]
["29512","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 12 MOD,    H700 X D230 X W1000, WISZĄCA",786.2,"1-ZE-09",null,null,"OM_ENCLOSURES","29012","SZT","85381000","27.12.40.0",null,"5901988295127","OM - Boîtier de base IP55, 12 mod, H700 x P230 x L1000, suspendu","OM - Basic housing IP55, 12 mod, H700 x D230 x W1000, hanging","OM- ARMARIO METAL. IP55, 12 MOD,  H700 x D230 x W1000, MURAL","ZENERGY OM - ALAP HÁZ IP55, 12 MOD, H700 X D230 X W1000, FÜGG."]
["29521","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 21 MOD,  H1150 X D230 X W1000, WISZĄCA",970.9,"1-ZE-09",3.3333333333333333E-2,2,"OM_ENCLOSURES","29021","SZT","85381000","27.12.40.0",null,"5901988295219","OM - Boîtier de base IP55, 21 mod, H1150 x P230 x L1000, suspendu","OM - Basic housing IP55, 21 mod, H1150 x D230 x W1000, hanging","OM- ARMARIO METAL. IP55, 21 MOD,  H1150 x D230 x W1000, MURAL","ZENERGY OM - ALAPVETŐ HÁZ IP55, 21 MOD, H1150 X D230 X W1000, FÜGG."]
["29529","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 29 MOD,  H1550 X D230 X W1000, WISZĄCA",1172.9000000000001,"1-ZE-09",null,null,"OM_ENCLOSURES","29029","SZT","85381000","27.12.40.0",null,"5901988295295","OM - Boîtier de base IP55, 29 mod, H1550 x P230 x L1000, suspendu","OM - Basic housing IP55, 29 mod, H1550 x D230 x W1000, hanging","OM- ARMARIO METAL. IP55, 29 MOD,  H1550 x D230 x W1000, MURAL","ZENERGY OM - ALAP HÁZ IP55, 29 MOD, H1550 X D230 X W1000, FÜGG."]
["29536","ZENERGY OM - OBUDOWA PODSTAWOWA IP55, 36 MOD,  H2000 X D230 X W1000, COKÓŁ 100MM",2015.3,"1-ZE-09",1.6666666666666666E-2,2,"OM_ENCLOSURES","29036","SZT","85381000","27.12.40.0",null,"5901988295363","OM - Boîtier de base IP55, 36 mod, H2000 x P230 x L1000, base 100mm","OM - Basic housing IP55, 36 mod, H2000 x D230 x W1000, plinth 100mm","OM- ARMARIO METAL. IP55, 36 MOD,  H2000 x D230 x W1000, ZOCALO 100MM","ZENERGY OM - ALAP HÁZ IP55, 36 MOD, H2000 X D230 X W1000, lábazat 100 mm"]
["29615","ZENERGY OM - ROZSZERZENIE IP55, 15 MOD,    H850 X D230 X W1000, WISZĄCA",877,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988296155","OM - extension IP55, 15 mod, H850 x P230 x L1000, suspendu","OM - Extension IP55, 15 mod, H850 x D230 x W1000, hanging","OM- MODULO AUX. IP55, 15 MOD,  H850 x D230 x W1000, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 15 MOD, H850 X D230 X W1000, LAKÓS"]
["29624","ZENERGY OM - ROZSZERZENIE IP55, 24 MOD,  H1300 X D230 X W1000, WISZĄCA",1060.5999999999999,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988296247","OM - extension IP55, 24 mod, H1300 x P230 x L1000, suspendu","OM - Extension IP55, 24 mod, H1300 x D230 x W1000, pendant","OM- MODULO AUX. IP55, 24 MOD,  H1300 x D230 x W1000, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 24 MOD, H1300 X D230 X W1000, LAKÓS"]
["29629","ZENERGY OM - ROZSZERZENIE IP55, 29 MOD,  H1550 X D230 X W1000, WISZĄCA",1212.8,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988296292","OM - Extension IP55, 29 mod, H1550 x P230 x L1000, suspendu","OM - Extension IP55, 29 mod, H1550 x D230 x W1000, hanging","OM- MODULO AUX. IP55, 29 MOD,  H1550 x D230 x W1000, MURAL","ZENERGY OM - IP55 BŐVÍTÉS, 29 MOD, H1550 X D230 X W1000, LAKÓS"]
["29630","ZENERGY OM - ROZSZERZENIE IP55, 30 MOD,  H1700 X D230 X W1000, COKÓŁ 100MM",1637.3,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988296308","OM - Extension IP55, 30 mod, H1700 x P230 x L1000, base 100mm","OM - Extension IP55, 30 mod, H1700 x D230 x W1000, plinth 100mm","OM- MODULO AUX. IP55, 30 MOD,  H1700 x D230 x W1000, ZOCALO 100MM","ZENERGY OM - IP55 BŐVÍTÉS, 30 MOD, H1700 X D230 X W1000, lábazat 100 mm"]
["29639","ZENERGY OM - ROZSZERZENIE IP55, 39 MOD,  H2150 X D230 X W1000, COKÓŁ 100MM",2153.5,"1-ZE-09",null,null,"OM_ENCLOSURES_EXTENSIONS",null,"SZT","85381000","27.12.40.0",null,"5901988296391","OM - Extension IP55, 39 mod, H2150 x P230 x L1000, base 100 mm","OM - Extension IP55, 39 mod, H2150 x D230 x W1000, plinth 100mm","OM- MODULO AUX. IP55, 39 MOD,  H2150 x D230 x W1000, ZOCALO 100MM","ZENERGY OM - IP55 BŐVÍTÉS, 39 MOD, H2150 X D230 X W1000, lábazat 100 mm"]
["29715","ZENERGY OM - DRZWI PEŁNE IP55, 15 MOD,    H850 X W1000",359.6,"1-ZE-09",null,null,"OM_DOORS","29215","SZT","85389099","27.12.40.0",null,"5901988297152","OM - Portes pleine IP55, 15 mod., H850 x L1000","OM - Plain door IP55, 15 mod, H850 x W1000","OM- PUERTA OPACA IP55, 15 MOD,   H850 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP55, 15 MOD, H850 X W1000"]
["29724","ZENERGY OM - DRZWI PEŁNE IP55, 24 MOD,  H1300 X W1000",522.70000000000005,"1-ZE-09",0.05,1,"OM_DOORS","29224","SZT","85389099","27.12.40.0",null,"5901988297244","OM - Portes pleine IP55, 24 mod., H1300 x L1000","OM - Plain door IP55, 24 mod, H1300 x W1000","OM- PUERTA OPACA IP55, 24 MOD,  H1300 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP55, 24 MOD, H1300 X W1000"]
["29733","ZENERGY OM - DRZWI PEŁNE IP55, 33 MOD,  H1750 X W1000",751.7,"1-ZE-09",null,null,"OM_DOORS","29233","SZT","85389099","27.12.40.0",null,"5901988297336","OM - Portes pleine IP55, 33 mod, H1750 x L1000","OM - Plain door IP55, 33 mod, H1750 x W1000","OM- PUERTA OPACA IP55, 33 MOD,  H1750 x W1000","ZENERGY OM – TÖMÖR AJTÓ IP55, 33 MOD, H1750 X W1000"]
["29912","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 12 MOD,    H700 X W1000",523.6,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29412","SZT","85389099","27.12.40.0",null,"5901988299125","OM - Portes transparentes IP55, 12 mod, H700 x L1000","OM - Transparent door IP55, 12 mod, H700 x W1000","OM- PUERTA TRANSP. IP55, 12 MOD,  H700 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 12 MOD, H700 X W1000"]
["29921","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 21 MOD,  H1150 X W1000",702.8,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29421","SZT","85389099","27.12.40.0",null,"5901988299217","OM - Portes transparentes IP55, 21 mod, H1150 x L1000","OM - Transparent door IP55, 21 mod, H1150 x W1000","OM- PUERTA TRANSP. IP55, 21 MOD,  H1150 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 21 MOD, H1150 X W1000"]
["29928","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 28 MOD,  H1500 X W1000",925.4,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29428","SZT","85389099","27.12.40.0",null,"5901988299286","OM - Portes transparentes IP55, 28 mod, H1500 x L1000","OM - Transparent door IP55, 28 mod, H1500 x W1000","OM- PUERTA TRANSP. IP55, 28 MOD,  H1500 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 28 MOD, H1500 X W1000"]
["29929","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 29 MOD,  H1550 X W1000",959.3,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29429","SZT","85389099","27.12.40.0",null,"5901988299293","OM - Portes transparentes IP55, 29 mod, H1550 x L1000","OM - Transparent door IP55, 29 mod, H1550 x W1000","OM- PUERTA TRANSP. IP55, 29 MOD,  H1550 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 29 MOD, H1550 X W1000"]
["29936","ZENERGY OM - DRZWI TRANSPARENTNE IP55, 36 MOD,  H1900 X W1000",1159.5999999999999,"1-ZE-09",null,null,"OM_TRANSPARENT_DOORS","29436","SZT","85389099","27.12.40.0",null,"5901988299361","OM - Portes transparentes IP55, 36 mod, H1900 x L1000","OM - Transparent door IP55, 36 mod, H1900 x W1000","OM- PUERTA TRANSP. IP55, 36 MOD,  H1900 x W1000","ZENERGY OM - ÁTLÁTSZÓ AJTÓK IP55, 36 MOD, H1900 X W1000"]
["30006","ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650+400",257,"1-ZE-01",null,null,"OE_PLINTHS","30015","SZT","85389099","27.12.40.0",null,"5901988300067","OE - Socle H100, couvert avant et arrière, L650 + 400","OE - H100 plinth, ventilated covers front, rear, W650 + 400","OE- ZOCALO H100, VENTILADO, FRONTAL/TRASERO (2UDS) W650+400","ZENERGY - LÁZALAK H100, SZELLŐZŐ BURKOLATOK ELSŐ, HÁTSÓ, W650+400"]
["30012","ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W1200",244.1,"1-ZE-01",null,null,"OE_PLINTHS","30012","SZT","85389099","27.12.40.0",null,"5901988300128","OE - Socle H100, couvertures avant et arrière, L1200","OE - H100 plinth, ventilated covers front, rear, W1200","OE- ZOCALO H100, VENTILADO, FRONTAL/TRASERO (2UDS) W1200","ZENERGY - LÁZALAK H100, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W1200"]
["30016","ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W1150",239.8,"1-ZE-01",null,null,"OE_PLINTHS","30016","SZT","85389099","27.12.40.0",null,"5901988300166","OE - Socle H100, couverture avant et arrière, W1150","OE - H100 plinth, ventilated covers front, rear, W1150","OE- ZOCALO H100, VENTILADO, FRONTAL/TRASERO (2UDS) W1150","ZENERGY - LÁZALAK H100, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W1150"]
["30023","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D230",131.80000000000001,"1-ZE-01",2.2999999999999998,4,"OE_PLINTHS","30023","SZT","85389099","27.12.40.0",null,"5901988300234","OE - Socle H100, écrans latéraux complets, P230","OE - H100 plinth, Plain side covers, D230","OE- ZOCALO H100, LATERAL (2UDS), D230","ZENERGY - LÁZAT H100, TELJES OLDALBURKOLATOK, D230"]
["30033","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D300",146.9,"1-ZE-01",1.1583333333333334,6,"OE_PLINTHS","30033","SZT","85389099","27.12.40.0",null,"5901988300333","OE - Socle H100, écrans latéraux complets, P300","OE - H100 plinth, Plain side covers, D300","OE- ZOCALO H100, LATERAL (2UDS), D300","ZENERGY - LÁZAT H100, TELJES OLDALBURKOLATOK, D300"]
["30043","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D400",150.1,"1-ZE-01",1.5,6,"OE_PLINTHS","30043","SZT","85389099","27.12.40.0",null,"5901988300432","OE - Socle H100, protections latérales complètes, P400","OE - H100 plinth, Plain side covers, D400","OE- ZOCALO H100, LATERAL (2UDS), D400","ZENERGY - LÁZAT H100, TELJES OLDALBURKOLATOK, D400"]
["30045","ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W450",165.2,"1-ZE-01",null,null,"OE_PLINTHS","30045","SZT","85389099","27.12.40.0",null,"5901988300456","OE - Socle H100, avant, arrière, cache L450","OE - H100 plinth, ventilated covers front, rear, W450","OE- ZOCALO H100, VENTILADO, FRONTAL/TRASERO (2UDS) W450","ZENERGY - LÁZALAK H100, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W450"]
["30060","ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W600",173.9,"1-ZE-01",0.11666666666666667,2,"OE_PLINTHS","30060","SZT","85389099","27.12.40.0",null,"5901988300609","OE - Socle H100, couvertures avant et arrière, L600","OE - H100 plinth, ventilated covers front, rear, W600","OE- ZOCALO H100, VENTILADO, FRONTAL/TRASERO (2UDS) W600","ZENERGY - LÁZALOK H100, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W600"]
["30071","Zenergy - Cokół H100, komplet do ramy narożnikowej, D600",396.4,"1-ZE-01",null,null,"OE_PLINTHS","30071","SZT","85389099","27.12.40.0","191002LK","5901988300715","OE - Socle H100, jeu pour cadre d'angle, P600","OE - H100 plinth, set for the corner frame, D600","OE- ZOCALO H100, JUEGO PARA MARCO ANGULAR, D600","Zenergy - Lábazat H100, komplett sarokkerethez, D600"]
["30081","Zenergy - Cokół H100, komplet do ramy narożnikowej, D800",397.4,"1-ZE-01",0.01,1,"OE_PLINTHS",null,"KPL","85389099","27.12.40.0",null,"5901988300814","OE - Socle H100, kit pour cadre d'angle, P800","OE - Plinth H100, set for corner frame, D800","*OE - Zócalo H100, juego para marco de esquina, D800","Zenergy - Lábazat H100, komplett sarokkerethez, D800"]
["30091","Zenergy - Cokół H100, komplet do ramy narożnikowej, D800",429.8,"1-ZE-01",null,null,"OE_PLINTHS","30091","SZT","85389099","27.12.40.0","191002LK","5901988300913","OE - Socle H100, jeu pour cadre d'angle, P800","OE - H100 plinth, set for the corner frame, D800","OE- ZOCALO H100, JUEGO PARA MARCO ANGULAR, D800","Zenergy - Lábazat H100, komplett sarokkerethez, D800"]
["30103","ZENERGY - COKÓŁ H200, PEŁNE OSŁONY BOCZNE, D1000",478.4,"1-ZE-01",0.01,1,"OE_PLINTHS","30103","SZT","85389099","27.12.40.0",null,"5901988301033","OE - Socle H200, écrans latéraux complets, P1000","OE - H200 plinth, Plain side covers, D1000","OE- ZOCALO H200, CIEGO, LATERAL (2UDS), D1000","ZENERGY - LÁZAT H200, TELJES OLDALBURKOLATOK, D1000"]
["30111","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W150+650+300",403.9,"1-ZE-01",null,null,"OE_PLINTHS","30111","SZT","85389099","27.12.40.0",null,"5901988301118","OE - Socle H200, couverture avant et arrière, L150 + 650 + 300","OE - H200 plinth, front and rear cover, W150 + 650 + 300","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W150+650+300","ZENERGY - LÁZALAK H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W150+650+300"]
["30112","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W1200",381.2,"1-ZE-01",0.01,1,"OE_PLINTHS","30112","SZT","85389099","27.12.40.0",null,"5901988301125","OE - Socle H200, avant, arrière, couverture L1200","OE - H200 plinth, front and rear cover, W1200","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W1200","ZENERGY - LÁZALOK H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W1200"]
["30121","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W150+650+400",421.2,"1-ZE-01",null,null,"OE_PLINTHS","30112","SZT","85389099","27.12.40.0",null,"5901988301217","OE - Socle H200, couverture avant et arrière, L150 + 650 + 400","OE - H200 plinth, front and rear cover, W150 + 650 + 400","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W150+650+400","ZENERGY - LÁZALAK H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W150+650+400"]
["30133","ZENERGY - COKÓŁ H200, PEŁNE OSŁONY BOCZNE, D300",251.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_PLINTHS","30133","SZT","85389099","27.12.40.0",null,"5901988301330","OE - Socle H200, écrans latéraux complets, P300","OE - H200 plinth, Plain side covers, D300","OE- ZOCALO H200, CIEGO, LATERAL (2UDS), D300","ZENERGY - LÁZAT H200, TELJES OLDALBURKOLATOK, D300"]
["30143","ZENERGY - COKÓŁ H200, PEŁNE OSŁONY BOCZNE, D400",281.89999999999998,"1-ZE-01",0.44166666666666665,4,"OE_PLINTHS","30143","SZT","85389099","27.12.40.0",null,"5901988301439","OE - Socle H200, protections latérales complètes, P400","OE - H200 plinth, Plain side covers, D400","OE- ZOCALO H200, CIEGO, LATERAL (2UDS), D400","ZENERGY - LÁZAT H200, TELJES OLDALBURKOLATOK, D400"]
["30160","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W600",261.39999999999998,"1-ZE-01",null,null,"OE_PLINTHS","30160","SZT","85389099","27.12.40.0",null,"5901988301606","OE - Socle H200, avant, arrière, couverture L600","OE - H200 plinth, front and rear cover, W600","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W600","ZENERGY - LÁZALOM H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W600"]
["30165","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650",268.89999999999998,"1-ZE-01",null,null,"OE_PLINTHS","30165","SZT","85389099","27.12.40.0",null,"5901988301651","OE - Socle H200, avant, arrière, cache L650","OE - H200 plinth, front and rear cover, W650","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W650","ZENERGY - LÁZALAK H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W650"]
["30183","ZENERGY - COKÓŁ H200, PEŁNE OSŁONY BOCZNE, D800",409.3,"1-ZE-01",null,null,"OE_PLINTHS","30183","SZT","85389099","27.12.40.0",null,"5901988301835","OE - Socle H200, écrans latéraux complets, P800","OE - H200 plinth, Plain side covers, D800","OE- ZOCALO H200, CIEGO, LATERAL (2UDS), D800","ZENERGY - LÁZAT H200, TELJES OLDALBURKOLATOK, D800"]
["30195","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W950",346.7,"1-ZE-01",null,null,"OE_PLINTHS","30195","SZT","85389099","27.12.40.0",null,"5901988301958","OE - Socle H200, avant, arrière, cache W950","OE - H200 plinth, front and rear cover, W950","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W950","ZENERGY - LÁZALAK H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W950"]
["30196","ZENERGY - COKÓŁ H200, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650+300",374.8,"1-ZE-01",null,null,"OE_PLINTHS","30195","SZT","85389099","27.12.40.0",null,"5901988301965","OE - Socle H200, couverture avant et arrière, L650 + 300","OE - H200 plinth, front and rear cover, W650 + 300","OE- ZOCALO H200, VENTILADO, FRONTAL/TRASERO (2UDS) W650+300","ZENERGY - LÁZALAK H200, SZELLŐZTETT BURKOLATOK ELSŐ, HÁTSÓ, W650+300"]
["30212","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W1200, D230, przetłoczenia",306.7,"1-ZE-01",null,null,"OE_COVERS","31212","SZT","85389099",null,null,"5901988302122","OE - Capot supérieur IP30, L1200, P230, ventilation","OE - Top cover IP30, W1200, D230, ventilation","OE- TECHO IP30, W1200, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W1200, D230, dombornyomott"]
["30218","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850+300, D230, przetłoczenia",301.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988302184","OE - Capot supérieur IP30, L850 + 300, P230, ventilation","OE - Top cover IP30, W850 + 300, D230, ventilation","OE- TECHO IP30, W850+300, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850+300, D230, dombornyomott"]
["30222","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W150+650+300, D230, przetłoczenia",294.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988302221","OE - Capot supérieur IP30, L150 + 650 + 300, P230, ventilation","OE - Top cover IP30, W150 + 650 + 300, D230, ventilation","OE- TECHO IP30, W150+650+300, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W150+650+300, D230, dombornyomott"]
["30230","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W300, D230, przetłoczenia",219.2,"1-ZE-01",null,null,"OE_COVERS","31230","SZT","85389099",null,null,"5901988302306","OE - Capot supérieur IP30, L300, P230, ventilation","OE - Top cover IP30, W300, D230, ventilation","OE- TECHO IP30, W300, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ FEDÉL IP30, W300, D230, dombornyomott"]
["30240","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W400, D230, przetłoczenia",229,"1-ZE-01",null,null,"OE_COVERS","31240","SZT","85389099",null,null,"5901988302405","OE - Capot supérieur IP30, L400, P230, ventilation","OE - Top cover IP30, W400, D230, ventilation","OE- TECHO IP30, W400, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W400, D230, dombornyomott"]
["30266","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450+200, D230, przetłoczenia",253.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988302665","OE - Capot supérieur IP30, L450 + 200, P230, ventilation","OE - Top cover IP30, W450 + 200, D230, ventilation","OE- TECHO IP30, W450+200, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450+200, D230, dombornyomott"]
["30280","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W800, D230, przetłoczenia",266.8,"1-ZE-01",null,null,"OE_COVERS","31280","SZT","85389099",null,null,"5901988302801","OE - Capot supérieur IP30, L800, P230, ventilation","OE - Top cover IP30, W800, D230, ventilation","OE- TECHO IP30, W800, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W800, D230, dombornyomott"]
["30281","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+150, D230, przetłoczenia",266.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988302818","OE - Capot supérieur IP30, L650 + 150, P230, ventilation","OE - Top cover IP30, W650 + 150, D230, ventilation","OE- TECHO IP30, W650+150, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+150, D230, dombornyomott"]
["30291","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450+450, D230, przetłoczenia",276.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988302917","OE - Capot supérieur IP30, L450 + 450, P230, ventilation","OE - Top cover IP30, W450 + 450, D230, ventilation","OE- TECHO IP30, W450+450, D230, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450+450, D230, dombornyomott"]
["30311","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+400, D300, przetłoczenia",406.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303112","OE - Capot supérieur IP30, L650 + 400, P300, ventilation","OE - Top cover IP30, W650 + 400, D300, ventilation","OE- TECHO IP30, W650+400, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+400, D300, dombornyomott"]
["30318","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850+300, D300, przetłoczenia",424.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303181","OE - Capot supérieur IP30, L850 + 300, P300, ventilation","OE - Top cover IP30, W850 + 300, D300, ventilation","OE- TECHO IP30, W850+300, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850+300, D300, dombornyomott"]
["30320","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850+450, D300, przetłoczenia",455.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303204","OE - Capot supérieur IP30, L850 + 450, P300, ventilation","OE - Top cover IP30, W850 + 450, D300, ventilation","OE- TECHO IP30, W850+450, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850+450, D300, dombornyomott"]
["30332","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W200+650+300, D300, przetłoczenia",424.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303327","OE - Capot supérieur IP30, L200 + 650 + 300, P300, ventilation","OE - Top cover IP30, W200 + 650 + 300, D300, ventilation","OE- TECHO IP30, W200+650+300, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W200+650+300, D300, dombornyomott"]
["30345","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450, D300, przetłoczenia",287.3,"1-ZE-01",null,null,"OE_COVERS","31345","SZT","85389099",null,null,"5901988303457","OE - Capot supérieur IP30, L450, P300, ventilation","OE - Top cover IP30, W450, D300, ventilation","OE- TECHO IP30, W450, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450, D300, dombornyomott"]
["30366","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450+200, D300, przetłoczenia",327.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303662","OE - Capot supérieur IP30, L450 + 200, P300, ventilation","OE - Top cover IP30, W450 + 200, D300, ventilation","OE- TECHO IP30, W450+200, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450+200, D300, dombornyomott"]
["30371","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W300+400, D300, przetłoczenia",337,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303716","OE - Capot supérieur IP30, L300 + 400, P300, ventilation","OE - Top cover IP30, W300 + 400, D300, ventilation","OE- TECHO IP30, W300+400, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W300+400, D300, dombornyomott"]
["30381","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+150, D300, przetłoczenia",356.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303815","OE - Capot supérieur IP30, L650 + 150, P300, ventilation","OE - Top cover IP30, W650 + 150, D300, ventilation","OE- TECHO IP30, W650+150, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+150, D300, dombornyomott"]
["30391","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450+450, D300, przetłoczenia",376.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988303914","OE - Capot supérieur IP30, L450 + 450, P300, ventilation","OE - Top cover IP30, W450 + 450, D300, ventilation","OE- TECHO IP30, W450+450, D300, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450+450, D300, dombornyomott"]
["30410","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W1000, D400, przetłoczenia",401.8,"1-ZE-01",null,null,"OE_COVERS","31410","SZT","85389099",null,null,"5901988304102","OE - Capot supérieur IP30, L1000, P400, ventilation","OE - Top cover IP30, W1000, D400, ventilation","OE- TECHO IP30, W1000, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ FEDÉL IP30, W1000, D400, dombornyomott"]
["30413","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W1300, D400, przetłoczenia",459,"1-ZE-01",null,null,"OE_COVERS","31413","SZT","85389099",null,null,"5901988304133","OE - Capot supérieur IP30, L1300, P400, ventilation","OE - Top cover IP30, W1300, D400, ventilation","OE- TECHO IP30, W1300, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ FEDÉL IP30, W1300, D400, dombornyomott"]
["30420","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850+450, D400, przetłoczenia",459,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988304201","OE - Capot supérieur IP30, L850 + 450, P400, ventilation","OE - Top cover IP30, W850 + 450, D400, ventilation","OE- TECHO IP30, W850+450, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850+450, D400, dombornyomott"]
["30427","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W150+850+300, D400, przetłoczenia",459,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988304270","OE - Capot supérieur IP30, L150 + 850 + 300, P400, ventilation","OE - Top cover IP30, W150 + 850 + 300, D400, ventilation","OE- TECHO IP30, W150+850+300, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W150+850+300, D400, dombornyomott"]
["30432","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W200+650+300, D400, przetłoczenia",430.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988304324","OE - Capot supérieur IP30, L200 + 650 + 300, P400, ventilation","OE - Top cover IP30, W200 + 650 + 300, D400, ventilation","OE- TECHO IP30, W200+650+300, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W200+650+300, D400, dombornyomott"]
["30433","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W200+650+400, D400, przetłoczenia",449.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988304331","OE - Capot supérieur IP30, L200 + 650 + 400, P400, ventilation","OE - Top cover IP30, W200 + 650 + 400, D400, ventilation","OE- TECHO IP30, W200+650+400, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W200+650+400, D400, dombornyomott"]
["30460","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W600, D400, przetłoczenia",324,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","31460","SZT","85389099",null,null,"5901988304607","OE - Capot supérieur IP30, L600, P400, ventilation","OE - Top cover IP30, W600, D400, ventilation","OE- TECHO IP30, W600, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W600, D400, dombornyomott"]
["30476","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W300+450, D400, przetłoczenia",354.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988304768","OE - Capot supérieur IP30, L300 + 450, P400, ventilation","OE - Top cover IP30, W300 + 450, D400, ventilation","OE- TECHO IP30, W300+450, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ FEDÉL IP30, W300+450, D400, dombornyomott"]
["30485","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850, D400, przetłoczenia",373.7,"1-ZE-01",0.01,1,"OE_COVERS","31485","SZT","85389099",null,null,"5901988304850","OE - Capot supérieur IP30, L850, P400, ventilation","OE - Top cover IP30, W850, D400, ventilation","OE- TECHO IP30, W850, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850, D400, dombornyomott"]
["30495","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+300, D400, przetłoczenia",392,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988304959","OE - Capot supérieur IP30, L650 + 300, P400, ventilation","OE - Top cover IP30, W650 + 300, D400, ventilation","OE- TECHO IP30, W650+300, D400, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+300, D400, dombornyomott"]
["30611","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+400, D600, przetłoczenia",453.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988306113","OE - Capot supérieur IP30, L650 + 400, P600, ventilation","OE - Top cover IP30, W650 + 400, D600, ventilation","OE- TECHO IP30, W650+400, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+400, D600, dombornyomott"]
["30615","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+450, D600, przetłoczenia",462.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988306151","OE - Capot supérieur IP30, L650 + 450, P600, ventilation","OE - Top cover IP30, W650 + 450, D600, ventilation","OE- TECHO IP30, W650+450, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+450, D600, dombornyomott"]
["30620","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850+450, D600, przetłoczenia",508.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988306205","OE - Capot supérieur IP30, L850 + 450, P600, ventilation","OE - Top cover IP30, W850 + 450, D600, ventilation","OE- TECHO IP30, W850+450, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850+450, D600, dombornyomott"]
["30621","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W150+650+400, D600, przetłoczenia",486,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988306212","OE - Capot supérieur IP30, L150 + 650 + 400, P600, ventilation","OE - Top cover IP30, W150 + 650 + 400, D600, ventilation","OE- TECHO IP30, W150+650+400, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W150+650+400, D600, dombornyomott"]
["30630","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W300, D600, przetłoczenia",286.2,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","31630","SZT","85389099",null,null,"5901988306304","OE - Capot supérieur IP30, L300, P600, ventilation","OE - Top cover IP30, W300, D600, ventilation","OE- TECHO IP30, W300, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ FEDÉL IP30, W300, D600, dombornyomott"]
["30641","ZENERGY - POKRYWA GÓRNA IP30, W400, D600, z przepustem kablowym",311,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","30641","SZT","85389099","27.12.40.0",null,"5901988306410","OE - Capot supérieur IP30, L400, P600, avec un presse-étoupe","OE - Top cover IP30, W400, D600, with a cable gland","OE- TECHO IP30, W400, D600, CON PRENSAESTOPAS","ZENERGY - FELSŐ BURKOLAT IP30, W400, D600, kábelbevezetéssel"]
["30660","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W600, D600, przetłoczenia",352.1,"1-ZE-01",null,null,"OE_COVERS","31660","SZT","85389099",null,null,"5901988306601","OE - Capot supérieur IP30, L600, P600, ventilation","OE - Top cover IP30, W600, D600, ventilation","OE- TECHO IP30, W600, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W600, D600, dombornyomott"]
["30666","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450+200, D600, przetłoczenia",364,"1-ZE-01",null,null,"OE_COVERS","31665","SZT","85389099",null,null,"5901988306663","OE - Capot supérieur IP30, L450 + 200, P600, ventilation","OE - Top cover IP30, W450 + 200, D600, ventilation","OE- TECHO IP30, W450+200, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450+200, D600, dombornyomott"]
["30680","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W800, D600, przetłoczenia",396.4,"1-ZE-01",null,null,"OE_COVERS","31680","SZT","85389099",null,null,"5901988306809","OE - Capot supérieur IP30, L800, P600, ventilation","OE - Top cover IP30, W800, D600, ventilation","OE- TECHO IP30, W800, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W800, D600, dombornyomott"]
["30684","ZENERGY - POKRYWA GÓRNA IP30, W850, D600, z przepustem pod kable Lewy",493.6,"1-ZE-01",0.01,1,"OE_COVERS","30684","SZT","85389099","27.12.40.0",null,"5901988306847","OE - Capot supérieur IP30, L850, P600, avec un conduit pour câbles","OE - Top cover IP30, W850, D600, with a cable gland Left","OE- TECHO IP30, W850, D600, CON PRENSAESTOPAS","ZENERGY - FELSŐ BURKOLAT IP30, W850, D600, kábelbemenettel bal"]
["30687","ZENERGY - POKRYWA GÓRNA IP30, W850, D600, z przepustem kablowym Prawy",493.6,"1-ZE-01",null,null,"OE_COVERS","30687","SZT","85389099","27.12.40.0",null,"5901988306878","OE - CAPOT SUPÉRIEUR IP30, L850, P600, avec presse-étoupe Droit","OE - Top cover IP30, W850, D600, with a cable gland Right","OE- TECHO IP30, W650+200, D600, CON ENTRADA PARA CABLES DERECHA","ZENERGY - FELSŐ BURKOLAT IP30, W850, D600, kábelbevezetéssel Jobb"]
["30691","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W450+450, D600, przetłoczenia",419,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988306915","OE - Capot supérieur IP30, L450 + 450, P600, ventilation","OE - Top cover IP30, W450 + 450, D600, ventilation","OE- TECHO IP30, W450+450, D600, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W450+450, D600, dombornyomott"]
["30711","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W1200, D1000",0,null,null,null,"OE_COVERS",null,null,"85389099",null,null,"5901988307110"]
["30715","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W450, D1000",0,null,null,null,"OE_COVERS",null,null,"85389099",null,null,"5901988307158"]
["30718","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W800, D1000",0,null,null,null,"OE_COVERS",null,null,"85389099",null,null,"5901988307189"]
["30721","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W1200, D230",731.2,"1-ZE-01",null,null,"OE_COVERS","30721","SZT","85389099",null,null,"5901988307219","OE - Toit de logement, L1200, P230","OE - Cover canopy, W1200, D230","OE- TEJADILLO, W1200, D230","ZENERGY - KÜLSŐ HÁZ IP55, W1200, D230"]
["30725","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W450, D230",426.6,"1-ZE-01",null,null,"OE_COVERS","30725","SZT","85389099",null,null,"5901988307257","OE - Toit de logement, L450, P230","OE - Housing canopy, W450, D230","OE- TEJADILLO, W450, D230","ZENERGY - KÜLSŐ HÁZ IP55, W450, D230"]
["30728","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W800, D230",526,"1-ZE-01",null,null,"OE_COVERS","30728","SZT","85389099",null,null,"5901988307288","OE - Toit de logement, L800, P230","OE - Housing canopy, W800, D230","OE- TEJADILLO, W800, D230","ZENERGY - KÜLSŐ HÁZ IP55, W800, D230"]
["30729","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W850, D230",615.6,"1-ZE-01",null,null,"OE_COVERS","30729","SZT","85389099",null,null,"5901988307295","OE - Toit de logement, L850, P230","OE - Housing canopy, W850, D230","OE- TEJADILLO, W850, D230","ZENERGY - KÜLSŐ HÁZ IP55, W850, D230"]
["30732","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W1300, D300",777.6,"1-ZE-01",null,null,"OE_COVERS","30732","SZT","85389099",null,null,"5901988307325","OE - Toit de logement, L1300, P300","OE - Housing canopy, W1300, D300","OE- TEJADILLO, W1300, D300","ZENERGY - KÜLSŐ HÁZ IP55, W1300, D300"]
["30735","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W450, D300",441.7,"1-ZE-01",null,null,"OE_COVERS","30735","SZT","85389099",null,null,"5901988307356","OE - Toit de logement, L450, P300","OE - Housing canopy, W450, D300","OE- TEJADILLO, W450, D300","ZENERGY - KÜLSŐ HÁZ IP55, W450, D300"]
["30739","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W850, D300",638.29999999999995,"1-ZE-01",null,null,"OE_COVERS","30739","SZT","85389099",null,null,"5901988307394","OE - Toit de logement, L850, P300","OE - Cover canopy, W850, D300","OE- TEJADILLO, W850, D300","ZENERGY - KÜLSŐ HÁZ IP55, W850, D300"]
["30742","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W1300, D400",805.7,"1-ZE-01",null,null,"OE_COVERS","30742","SZT","85389099",null,null,"5901988307424","OE - Toit de logement, L1300, P400","OE - Housing canopy, W1300, D400","OE- TEJADILLO, W1300, D400","ZENERGY - KÜLSŐ HÁZ IP55, W1300, D400"]
["30745","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W450, D400",455.8,"1-ZE-01",null,null,"OE_COVERS","30745","SZT","85389099",null,null,"5901988307455","OE - Toit de logement, L450, P400","OE - Housing canopy, W450, D400","OE- TEJADILLO, W450, D400","ZENERGY - KÜLSŐ HÁZ IP55, W450, D400"]
["30748","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W800, D400",561.6,"1-ZE-01",null,null,"OE_COVERS","30748","SZT","85389099",null,null,"5901988307486","OE - Toit de logement, L800, P400","OE - Housing canopy, W800, D400","OE- TEJADILLO, W800, D400","ZENERGY - KÜLSŐ HÁZ IP55, W800, D400"]
["30762","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W1300, D600",853.2,"1-ZE-01",null,null,"OE_COVERS","30762","SZT","85389099",null,null,"5901988307622","OE - Toit de logement, L1300, P600","OE - Cover canopy, W1300, D600","OE- TEJADILLO, W1300, D600","ZENERGY - KÜLSŐ HÁZ IP55, W1300, D600"]
["30763","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W300, D600",416.9,"1-ZE-01",null,null,"OE_COVERS","30763","SZT","85389099",null,null,"5901988307639","OE - Toit de logement, L300, P600","OE - Cover canopy, W300, D600","OE- TEJADILLO, W300, D600","ZENERGY - KÜLSŐ HÁZ IP55, W300, D600"]
["30766","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W600, D600",510.8,"1-ZE-01",null,null,"OE_COVERS","30766","SZT","85389099",null,null,"5901988307660","OE - Toit de logement, L600, P600","OE - Cover canopy, W600, D600","OE- TEJADILLO, W600, D600","ZENERGY - KÜLSŐ HÁZ IP55, W600, D600"]
["30769","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W850, D600",721.4,"1-ZE-01",null,null,"OE_COVERS","30769","SZT","85389099",null,null,"5901988307691","OE - Toit de logement, L850, P600","OE - Housing canopy, W850, D600","OE- TEJADILLO, W850, D600","ZENERGY - KÜLSŐ HÁZ IP55, W850, D600"]
["30781","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W1200, D800",897.6,"1-ZE-01",null,null,"OE_COVERS","30781","SZT","85389099",null,null,"5901988307813","OE - Toit de logement, L1200, P800","OE - Cover canopy, W1200, D800","OE- TEJADILLO, W1200, D800","ZENERGY - KÜLSŐ HÁZ IP55, W1200, D800"]
["30784","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W400, D800",480.7,"1-ZE-01",null,null,"OE_COVERS","30784","SZT","85389099",null,null,"5901988307844","OE - Toit de logement, L400, P800","OE - Housing canopy, W400, D800","OE- TEJADILLO, W400, D800","ZENERGY - KÜLSŐ HÁZ IP55, W400, D800"]
["30787","ZENERGY - DASZEK ZEWNĘTRZNY OBUDOWY IP55, W650, D800",605,"1-ZE-01",null,null,"OE_COVERS","30787","SZT","85389099",null,null,"5901988307875","OE - Toit de logement, L650, P800","OE - Housing canopy, W650, D800","OE- TEJADILLO, W650, D800","ZENERGY - KÜLSŐ HÁZ IP55, W650, D800"]
["30811","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+400, D800, przetłoczenia",531.29999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308117","OE - Capot supérieur IP30, L650 + 400, P800, ventilation","OE - Top cover IP30, W650 + 400, D800, ventilation","OE- TECHO IP30, W650+400, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+400, D800, dombornyomott"]
["30815","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+450, D800, przetłoczenia",544.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308155","OE - Capot supérieur IP30, L650 + 450, P800, ventilation","OE - Top cover IP30, W650 + 450, D800, ventilation","OE- TECHO IP30, W650+450, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+450, D800, dombornyomott"]
["30818","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850+300, D800, przetłoczenia",558.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308186","OE - Capot supérieur IP30, L850 + 300, P800, ventilation","OE - Top cover IP30, W850 + 300, D800, ventilation","OE- TECHO IP30, W850+300, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850+300, D800, dombornyomott"]
["30821","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W150+650+400, D800, przetłoczenia",574.20000000000005,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308216","OE - Capot supérieur IP30, L150 + 650 + 400, P800, ventilation","OE - Top cover IP30, W150 + 650 + 400, D800, ventilation","OE- TECHO IP30, W150+650+400, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W150+650+400, D800, dombornyomott"]
["30828","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W150+850+400, D800, przetłoczenia",630.29999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308285","OE - Capot supérieur IP30, L150 + 850 + 400, P800, ventilation","OE - Top cover IP30, W150 + 850 + 400, D800, ventilation","OE- TECHO IP30, W150+850+400, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W150+850+400, D800, dombornyomott"]
["30840","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W400, D800, przetłoczenia",347.6,"1-ZE-01",null,null,"OE_COVERS","31840","SZT","85389099","27.12.40.0",null,"5901988308407","OE - Capot supérieur IP30, L400, P800, ventilation","OE - Top cover IP30, W400, D800, ventilation","OE- TECHO IP30, W400, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W400, D800, dombornyomott"]
["30861","OE - Pokrywa górna perforowana / pełna IP30, W600, D775",396.4,"1-ZE-01",6.6666666666666666E-2,1,"OE_COVERS","30861","SZT",null,null,"240201PW",null,"OE - Capot supérieur perforé/solide IP30, W600, D775","OE - Perforated/solid top cover IP30, W600, D775","OE - Cubierta superior perforada/sólida IP30, W600, D775","OE - Perforált/masszív felső burkolat IP30, W600, D775"]
["30876","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W300+450, D800, przetłoczenia",446.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308766","OE - Capot supérieur IP30, L300 + 450, P800, ventilation","OE - Top cover IP30, W300 + 450, D800, ventilation","OE- TECHO IP30, W300+450, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ FEDÉL IP30, W300+450, D800, dombornyomott"]
["30885","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W850, D800, przetłoczenia",475.2,"1-ZE-01",4.1666666666666664E-2,2,"OE_COVERS","31885","SZT","85389099","27.12.40.0",null,"5901988308858","OE - Capot supérieur IP30, L850, P800, ventilation","OE - Top cover IP30, W850, D800, ventilation","OE- TECHO IP30, W850, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W850, D800, dombornyomott"]
["30892","Zenergy - Pokrywa górna wentylowana IP30, W850, D850 / prostownik Elektra",480.6,null,0.01,1,"OE_COVERS",null,null,"85389099",null,null,"5901988308926"]
["30895","ZENERGY - POKRYWA GÓRNA WENTYLOWANA IP30, W650+300, D800, przetłoczenia",502.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988308957","OE - Capot supérieur IP30, L650 + 300, P800, ventilation","OE - Top cover IP30, W650 + 300, D800, ventilation","OE- TECHO IP30, W650+300, D800, VENTIL.","ZENERGY - SZELLŐZTETT FELSŐ BURKOLAT IP30, W650+300, D800, dombornyomott"]
["30910","ZENERGY - SZYNA PROSTA, PRZÓD, TS-35D, (H=50MM), W1000",52.8,"1-ZE-01",null,null,"OE_RAIL_DIN","30910","SZT","85389099",null,null,"5901988309107","OE - Rail droit, avant, TS-35D, (h = 50mm), L1000","OE - Rail straight, front, TS-35D, (h = 50mm), W1000","OE- CARRIL RECTO, DELANTE, TS-35D, (H=50MM), W1000","ZENERGY - EGYENES SÍN, ELSŐ, TS-35D, (H=50MM), W1000"]
["30914","ZENERGY - SZYNA SKOŚNA TS-35D, NISKA (H=20MM), W1000",55.2,"1-ZE-01",null,null,"OE_RAIL_DIN","30914","SZT","85389099",null,null,"5901988309145","OE - Rail incliné TS-35D, faible (h = 20mm), L1000","OE - TS-35D slant rail, low (h = 20mm), W1000","OE- CARRIL INCLINADO TS-35D, BAJA (H=20MM), W1000","ZENERGY – DÖNTÉSSÍN TS-35D, ALACSONY (H=20MM), W1000"]
["30918","ZENERGY - ZESTAW 6 SZYN TS-35D, 6M, W1000,(H=15MM), + PE 40 ZACISKÓW",285.60000000000002,"1-ZE-01",null,null,"OE_RAIL_DIN",null,"SZT","85389099",null,null,"5901988309183","OE - Jeu de 6 rails TS-35D, 6M, L1000, (h = 15mm), + bornes PE 40","OE - set of 6 rails TS-35D, 6M, W1000, (h = 15mm), + PE 40 clips","OE- JUEGO 6 CARRILES TS-35D, 6M, W1000,(H=15MM), + PE ","ZENERGY - 6 SÍNES SZETT TS-35D, 6M, W1000, (H=15MM), + PE 40 BIZTOSOK"]
["30922","ZENERGY - SZYNA ALUMINIOWA TS-35D (H=15MM) DŁUGOŚĆ 1,5M",46.4,"1-ZE-01",1.6666666666666666E-2,1,"OE_RAIL_DIN","30922","P","76042990",null,null,"5901988309220","OE - Rail en aluminium TS-35D (h = 15mm), longueur 1,5 m","OE - TS-35D aluminum rail (h = 15mm), 1.5m long","OE- BARRA ALUMINIO TS-35D (H=15MM)  L=1,5M","ZENERGY - ALUMÍNIUM SÍN TS-35D (H=15MM) HOSSZ 1,5M"]
["30926","ZENERGY - SZYNA ALUMINIOWA TS-35D (H=15MM) DŁUGOŚĆ 1,6M",49.5,"1-ZE-01",0.01,1,"OE_RAIL_DIN","30926","P","85389099","27.12.40.0",null,"5901988309268","OE - Rail en aluminium TS-35D (h = 15mm), 1,6 m de long","OE - TS-35D aluminum rail (h = 15mm), 1.6m long","OE- BARRA ALUMINIO TS-35D (H=15MM)  L=1,6M","ZENERGY – ALUMÍNIUM SÍN TS-35D (H=15MM) HOSSZ 1,6M"]
["30929","ZENERGY - SZYNA ALUMINIOWA TS-35D (H=15MM) DŁUGOŚĆ 2,5M",77.2,"1-ZE-01",0.01,1,"OE_RAIL_DIN","30929","P","76042990",null,null,"5901988309299","OE - Rail en aluminium TS-35D (h = 15mm), 2,5 m de long","OE - TS-35D aluminum rail (h = 15mm), 2.5m long","OE- BARRA ALUMINIO TS-35D (H=15MM)  L=2,5M","ZENERGY - ALUMÍNIUM SÍN TS-35D (H=15MM) HOSSZ 2,5M"]
["30941","ZENERGY - SZYNA PROSTA, TYŁ, TS-35D, (H=50MM), W400",36.200000000000003,"1-ZE-01",null,null,"OE_RAIL_DIN","30941","SZT","85389099",null,null,"5901988309411","OE - Rail droit, arrière, TS-35D, (h = 50mm), L400","OE - Straight rail, rear TS-35D, (h = 50mm), W400","OE- CARRIL RECTO, DETRAS, TS-35D, (H=50MM), W400","ZENERGY - EGYENES SÍN, HÁTSÓ, TS-35D, (H=50MM), W400"]
["30942","ZENERGY - SZYNA PROSTA, PRZÓD, TS-35D, (H=100MM), W400",39.799999999999997,"1-ZE-01",null,null,"OE_RAIL_DIN","30942","SZT","85389099",null,null,"5901988309428","OE - Rail droit, avant, TS-35D, (h = 100mm), L400","OE - Rail straight, front, TS-35D, (h = 100mm), W400","OE- CARRIL RECTO, DELANTE, TS-35D, (H=100MM), W400","ZENERGY - EGYENES SÍN, ELSŐ, TS-35D, (H=100MM), W400"]
["30945","ZENERGY - SZYNA SKOŚNA TS-35D, WYSOKA, (H=50MM), W400",39.799999999999997,"1-ZE-01",null,null,"OE_RAIL_DIN","30945","SZT","85389099",null,null,"5901988309459","OE - Rail incliné TS-35D, haut, (h = 100mm), L400","OE - TS-35D slant rail, high, (h = 50mm), W400","OE- CARRIL INCLINADO TS-35D, ALTA (H=100MM), W400","ZENERGY – DÖNTÉSSÍN TS-35D, MAGAS, (H=50MM), W400"]
["30952","ZENERGY - SZYNA PROSTA, PRZÓD, TS-35D, (H=100MM), W450",42.1,"1-ZE-01",null,null,"OE_RAIL_DIN","30952","SZT","85389099",null,null,"5901988309527","OE - Rail droit, avant, TS-35D, (h = 100mm), L450","OE - Rail straight, front, TS-35D, (h = 100mm), W450","OE- CARRIL RECTO, DELANTE, TS-35D, (H=100MM), W450","ZENERGY - EGYENES SÍN, ELSŐ, TS-35D, (H=100MM), W450"]
["30955","ZENERGY - SZYNA SKOŚNA TS-35D, WYSOKA, (H=50MM), W450",42.1,"1-ZE-01",null,null,"OE_RAIL_DIN","30955","SZT","85389099",null,null,"5901988309558","OE - Rail incliné TS-35D, hauteur, (h = 100mm), L450","OE - TS-35D slant rail, high, (h = 50mm), W450","OE- CARRIL INCLINADO TS-35D, ALTA (H=100MM), W450","ZENERGY – DÖNTÉSSÍN TS-35D, MAGAS, (H=50MM), W450"]
["30961","ZENERGY - SZYNA PROSTA, TYŁ, TS-35D, (H=50MM), W600",40.9,"1-ZE-01",null,null,"OE_RAIL_DIN","30961","SZT","85389099",null,null,"5901988309619","OE - Rail droit, arrière, TS-35D, (h = 50mm), L600","OE - Straight rail, rear, TS-35D, (h = 50mm), W600","OE- CARRIL RECTO, DETRAS, TS-35D, (H=50MM), W600","ZENERGY - EGYENES SÍN, HÁTSÓ, TS-35D, (H=50MM), W600"]
["30965","ZENERGY - SZYNA SKOŚNA TS-35D, WYSOKA, (H=50MM), W600",44.4,"1-ZE-01",null,null,"OE_RAIL_DIN","30965","SZT","85389099",null,null,"5901988309657","OE - Rail incliné TS-35D, hauteur, (h = 100mm), L600","OE - TS-35D slant rail, high, (h = 50mm), W600","OE- CARRIL INCLINADO TS-35D, ALTA (H=100MM), W600","ZENERGY – DÖNTÉSSÍN TS-35D, MAGAS, (H=50MM), W600"]
["30971","ZENERGY - SZYNA PROSTA, TYŁ, TS-35D, (H=50MM), W650",45.4,"1-ZE-01",3.3333333333333333E-2,1,"OE_RAIL_DIN","30971","SZT","85389099",null,null,"5901988309718","OE - Rail droit, arrière, TS-35D, (h = 50mm), L650","OE - Straight rail, back, TS-35D, (h = 50mm), W650","OE- CARRIL RECTO, DETRAS, TS-35D, (H=50MM), W650","ZENERGY - EGYENES SÍN, HÁTSÓ, TS-35D, (H=50MM), W650"]
["30974","ZENERGY - SZYNA SKOŚNA TS-35D, NISKA (H=20MM), W650",45.4,"1-ZE-01",null,null,"OE_RAIL_DIN","30974","SZT","85389099",null,null,"5901988309749","OE - Rail incliné TS-35D, faible (h = 20mm), L650","OE - TS-35D slant rail, low (h = 20mm), W650","OE- CARRIL INCLINADO TS-35D, BAJA (H=20MM), W650","ZENERGY – DÖNTÉSSÍN TS-35D, ALACSONY (H=20MM), W650"]
["30975","ZENERGY - SZYNA SKOŚNA TS-35D, WYSOKA, (H=50MM), W650",48.8,"1-ZE-01",null,null,"OE_RAIL_DIN","30975","SZT","85389099",null,null,"5901988309756","OE - Rail incliné TS-35D, hauteur, (h = 100mm), L650","OE - TS-35D slant rail, high, (h = 50mm), W650","OE- CARRIL INCLINADO TS-35D, ALTA (H=100MM), W650","ZENERGY – DÖNTÉSSÍN TS-35D, MAGAS, (H=50MM), W650"]
["30981","ZENERGY - SZYNA PROSTA, TYŁ, TS-35D, (H=50MM), W800",46.7,"1-ZE-01",null,null,"OE_RAIL_DIN","30981","SZT","85389099",null,null,"5901988309817","OE - Rail droit, arrière, TS-35D, (h = 50mm), L800","OE - Straight rail, rear, TS-35D, (h = 50mm), W800","OE- CARRIL RECTO, DETRAS, TS-35D, (H=50MM), W800","ZENERGY - EGYENES SÍN, HÁTSÓ, TS-35D, (H=50MM), W800"]
["30985","ZENERGY - SZYNA SKOŚNA TS-35D, WYSOKA, (H=50MM), W800",50.1,"1-ZE-01",null,null,"OE_RAIL_DIN","30985","SZT","85389099",null,null,"5901988309855","OE - Rail incliné TS-35D, hauteur (h = 100mm), L800","OE - TS-35D slant rail, high, (h = 50mm), W800","OE- CARRIL INCLINADO TS-35D, ALTA (H=100MM), W800","ZENERGY – DÖNTÉSSÍN TS-35D, MAGAS, (H=50MM), W800"]
["30991","ZENERGY - SZYNA PROSTA, TYŁ, TS-35D, (H=50MM), W850",50.7,"1-ZE-01",null,null,"OE_RAIL_DIN","30991","SZT","85389099",null,null,"5901988309916","OE - Rail droit, arrière, TS-35D, (h = 50mm), L850","OE - Straight rail, rear, TS-35D, (h = 50mm), W850","OE- CARRIL RECTO, DETRAS, TS-35D, (H=50MM), W850","ZENERGY - EGYENES SÍN, HÁTSÓ, TS-35D, (H=50MM), W850"]
["30994","ZENERGY - SZYNA SKOŚNA TS-35D, NISKA (H=20MM), W850",53,"1-ZE-01",null,null,"OE_RAIL_DIN","30994","SZT","85389099",null,null,"5901988309947","OE - Rail incliné TS-35D, faible (h = 20mm), L850","OE - TS-35D slant rail, low (h = 20mm), W850","OE- CARRIL INCLINADO TS-35D, BAJA (H=20MM), W850","ZENERGY – DÖNTÉSSÍN TS-35D, ALACSONY (H=20MM), W850"]
["30999","ZENERGY - Etykieta samoprzylepna \"Nie myć ciśnieniowo\" średnica 100mm",16.2,"1-ZE-01",null,null,"OE_ACCESSORIES","30999","SZT","85389099",null,"230927LK","5901988309992","Ne pas laver sous pression – Autocollant adhésif 100 mm de diamètre","OE - Self-adhesive label \"Do not pressure wash\" 100mm diameter","*OE - Etiqueta autoadhesiva \"No lavar a presión\" 100 mm de diámetro","ZENERGY - Öntapadós címke \"Ne mossa nyomás alatt\" átmérője 100mm"]
["31002","ZENERGY - WYGRODZENIE TYLNE ODGINANE 2M W650",48.4,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","31002","SZT","85389099","27.12.40.0",null,"5901988310028","OE - Baffle arrière 2M L650","OE - Rear bending fence 2M W650","OE- DEFLECTOR TRASERO ABATIBLE 2M W650","ZENERGY - HÁTSÓ HAJLULÓ KERÍTÉS 2M W650"]
["31010","ZENERGY - UCHWYT REGULOWANY DO WSPORNIKA 310XX",15.9,"1-ZE-01",0.7,1,"OE_SUPPORT","31010","SZT","85389099","27.12.40.0",null,"5901988310103","OE - Support réglable pour support 310xx","OE - Adjustable handle for the 310xx bracket","OE- PIEZA REGULACION PARA SOPORTE 310XX","ZENERGY - ÁLLÍTHATÓ NYÚL A 310XX KONZOLHOZ"]
["31011","OE - Uchwyt regulowany do wspornika wzmocnionego, bocznego 204XX, dla przednich płyt osłonowych",18.7,"1-ZE-01",null,null,"OE_SUPPORT","31011","SZT","85389099",null,null,"5901988310110","OE - Support réglable pour support 204xx","OE - Adjustable handle for the 204xx bracket","OE- PIEZA REGULACION PARA SOPORTE 204XX","OE - Állítható konzol a megerősített oldalsó tartóhoz 204XX, az első fedőlemezekhez"]
["31024","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H36MM D200, ZEWNĘTRZNY",54.6,"1-ZE-01",0.28333333333333333,2,"OE_SUPPORT","31024","SZT","85389099",null,null,"5901988310240","OE - Support de plaque de montage H36mm P200, extérieur","OE - H36mm D200 Mounting plate bracket, external","OE- SOPORTE PARA PLACAS DE MONTAJE H36MM D200, EXTERNO","ZENERGY - SZERELŐLEMEZ TARTÓ H36MM D200, KÜLSŐ"]
["31031","ZENERGY - PRZEDNIE WYGRODZENIE SZYN PIONOWYCH W RAMIE W150, H1400",29.2,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988310318","OE - Clôture avant des rails verticaux dans le cadre L150, H1400","OE - Front partition of Vertical rails in the W150, H1400 frame","OE- TAPA FRONTAL PARA EMBARRADO VERT.  W150, H1400","ZENERGY – ELSŐ SOÁLYA FÜGGŐLEGES SÍNEKHEZ W150, H1400 KERETBEN"]
["31034","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H36MM D300, ZEWNĘTRZNY",58.4,"1-ZE-01",null,null,"OE_SUPPORT","31034","SZT","85389099",null,null,"5901988310349","OE - Support de plaque de montage H36mm P300, externe","OE - H36mm D300 Mounting plate bracket, external","OE- SOPORTE DE PLACA MONTAJE  H36MM D300, EXTERNO","ZENERGY - SZERELŐLEMEZ TARTÓ H36MM D300, KÜLSŐ"]
["31041","ZENERGY - PRZEDNIE WYGRODZENIE SZYN PIONOWYCH W RAMIE W150, H1600",33.4,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988310417","OE - Support horizontal, Forma3 - 1 jeu.","OE - The front barrier of Vertical rails in the W150, H1600 frame","OE- SOPORTE PLACA MONTAJE  H36 D400, EXTERIOR","ZENERGY – ELSŐ SOÁLYA FÜGGŐLEGES SÍNEKHEZ W150, H1600 KERETBEN"]
["31045","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H25MM D400, WEWNĘTRZNY",38.1,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988310455","OE - Support de montage P400, interne","OE - H25mm D400 Mounting plate bracket, internal","OE- SOPORTE PLACA MONTAJE  D400, INTERIOR ","ZENERGY - H25MM D400 SZERELŐLEMEZ TARTÓ, BELSŐ"]
["31049","ZENERGY - WYGRODZENIE BOCZNE; WSPORNIK ŻALUZJI ROZSUWANY, D200, FORMA2",46.7,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988310493","OE - Clôture latérale; Pression de serrage à l'angle 31055 3P / 4P, P400, Forma2","OE - Side fence; Extendable shutter support, D200, separation Form 2","OE- PROTECCION CONEXION PREFABRICADA H=250MM, FORMA 4B","ZENERGY - OLDALKERÍTÉS; KINYÚJTHATÓ REDŐNYEK TÁMASZTÁSA,D200, FORMA2"]
["31050","ZENERGY - WYGRODZENIE POZIOME WYŁĄCZNIKÓW, W650, FORMA3",202.7,"1-ZE-01",0.05,2,"OE_SEPARATION_BUSBAR","31050","SZT","85389099","27.12.40.0",null,"5901988310509","OE - Clôture horizontale pour disjoncteurs, L650, Forma3","OE - Horizontal fencing for circuit breakers, W650, Forma3","OE- PROTECC. EMB HORIZ. DE INT. AUT. W650, FORMA3","ZENERGY - MEGSZAKÍTÓK VÍZSZINTES KERÍTÉSE, W650, FORMA3"]
["31053","ZENERGY - WYGRODZENIE TYLNE POŁĄCZENIA, W650, FORMA4",388.6,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988310530","OE - Support arrière pour interrupteur horizontal, L650, Forma3","OE - Rear Connection Fencing, W650, Forma4","OE- SOPORTE SEPARACION INTERRUPTOR HORIZ. W650, FORMA 3","ZENERGY - HÁTSÓ FÜGG.KERÍTÉS, W650, FORMA4"]
["31056","ZENERGY - WYGRODZENIE BOCZNE; WSPORNIK ŻALUZJI ROZSUWANY 3P, D400, FORMA2",81.3,"1-ZE-01",0.20833333333333334,2,"OE_SEPARATION_BUSBAR","31056","SZT","85389099","27.12.40.0",null,"5901988310561","OE - Clôture latérale; Support pour stores coulissants 3P, P400, Forma2","OE - Side fence; Roller shutter bracket extending 3P, D400, separation Form 2","OE- PROTECC. EMBARRADO LATERAL, SOPORTE PARA CORTINA 3P, D400, FORMA 2","ZENERGY - OLDALKERÍTÉS; KINYÚJTHATÓ REDŐZŐK TÁMASZTÁSA 3P, D400, FORM2"]
["31060","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H25MM D600, ZEWNĘTRZNY",42.8,"1-ZE-01",0.5,2,"OE_SUPPORT","31060","SZT","85389099","27.12.40.0",null,"5901988310608","OE - Support de montage P600, externe","OE - H25mm D600 Mounting plate bracket, external","OE- SOPORTE PLACA MONTAJE  D600, EXTERIOR","ZENERGY - H25MM D600 SZERELŐLEMEZ TARTÓ, KÜLSŐ"]
["31063","ZENERGY - PRZEDNIE WYGRODZENIE SZYN PIONOWYCH W RAMIE W300, H1800",63.4,"1-ZE-01",null,null,"OE_COVERS","31063","SZT","85389099","27.12.40.0",null,"5901988310639","OE - Clôture avant de rails verticaux dans un cadre L300, H1800","OE - The front barrier of Vertical rails in the W300, H1800 frame","OE- TAPA FRONTAL PARA EMBARRADO VERT.  W300, H1800","ZENERGY – ELSŐ SOÁLYA FÜGGŐLEGES SÍNEKHEZ W300, H1800 KERETBEN"]
["31067","ZENERGY - WYGRODZENIE POZIOME TYŁ, W650 D200, FORMA3",75.400000000000006,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","31067","SZT","85389099",null,null,"5901988310660","OE - paroi arrière horizontale, L650 P200, Forme 3","OE - Horizontal rear partition, W650 D200, Forma3","OE- PROTECCIÓN TRASERA HORIZ. W650 D200, FORMA3","ZENERGY - HÁTSÓ VÍZSZINTES KERÍTÉS, W650 D200, FORMA3"]
["31072","ZENERGY - PRZEDNIE WYGRODZENIE SZYN PIONOWYCH W RAMIE W200, H2000",72.099999999999994,"1-ZE-01",5.8333333333333334E-2,1,"OE_COVERS","31072","SZT","85389099","27.12.40.0",null,"5901988310721","OE - Clôture avant de rails verticaux en cadre L200, H2000","OE - The front barrier of Vertical rails in the W200, H2000 frame","OE- TAPA FRONTAL PARA EMBARRADO VERT.  W200, H2000","ZENERGY – ELSŐ SOÁLYA FÜGGŐLEGES SÍNEKHEZ W200, H2000 KERETBEN"]
["31075","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H25MM D800, WEWNĘTRZNY",47.4,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988310752","OE - Support de montage P800, interne","OE - H25mm D800 Mounting plate bracket, internal","OE- SOPORTE PLACA MONTAJE  D800, INTERIOR ","ZENERGY - H25MM D800 SZERELŐLEMEZ TARTÓ, BELSŐ"]
["31076","ZENERGY - PRZEDNIE WYGRODZENIE SZYN PIONOWYCH W RAMIE W400, H2000",123.2,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988310769","OE - BARRIÈRE DE RAIL VERTICAL AVANT DANS CADRE L400, H2000","OE - Front Vertical rail barrier in frame W400, H2000","*OE - BARRERA DE RIEL VERTICAL DELANTERO EN MARCO W400, H2000","ZENERGY – ELSŐ SOÁLYA FÜGGŐLEGES SÍNEKHEZ W400, H2000 KERETBEN"]
["31079","ZENERGY - WYGRODZENIE BOCZNE ODGINANE 5M D200",61.2,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","31079","SZT","85389099","27.12.40.0",null,"5901988310790","OE - Clôture latérale 5M P200","OE - Folding side barrier 5M D200","OE- PROTECC. EMB. LATERAL PLEGABLE 5M D200","ZENERGY - HAJLÍTOTT OLDALKERÍTÉS 5M D200"]
["31082","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY POZIOME 2SZT W1300 2 FORMA",209.4,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988310820","OE - Rails horizontaux pour clôtures - tôle horizontale 2pcs L1300 2 Forme","OE - Horizontal rails fence - Horizontal sheets 2 pcs. W1300 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS HORIZ. W1300 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - VÍZSZINTES LAP 2 DB W1300 2 FORM"]
["31086","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY POZIOME 2SZT W600 2 FORMA",126.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_SEPARATION_BUSBAR","31086","SZT","85389099","27.12.40.0",null,"5901988310868","OE - Rails horizontaux pour clôtures - tôle horizontale 2pcs L600 2 Forme","OE - Horizontal rails fence - Horizontal sheets 2 pcs. W600 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS HORIZ. W600 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - VÍZSZINTES LAP 2 DB W600 2 FORM"]
["31091","ZENERGY - PRZEDNIE WYGRODZENIE SZYN PIONOWYCH W RAMIE W150, H2200",70.7,"1-ZE-01",0.25833333333333336,2,"OE_COVERS","31091","SZT","85389099","27.12.40.0",null,"5901988310912","OE - Clôture avant des rails verticaux dans le cadre L150, H2200","OE - The front barrier of Vertical rails in the W150, H2200 frame","OE- TAPA FRONTAL PARA EMBARRADO VERT.  W150, H2200","ZENERGY – ELSŐ SOÁLYA FÜGGŐLEGES SÍNEKHEZ W150, H2200 KERETBEN"]
["31094","ZENERGY - PRZEDNIE WYGRODZENIE POLA NAROŻNEGO H2200",62.2,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988310943","OE - Clôture avant du champ d'angle H2200","OE - The front part of the corner area H2200","OE- La parte delantera del área de la esquina H2200","ZENERGY - ELSŐ SAROKKERÍTÉS H2200"]
["31098","ZENERGY - WYGRODZENIE BOCZNE ODGINANE 5M D400",71,"1-ZE-01",0.1,2,"OE_SEPARATION_BUSBAR","31098","SZT","85389099","27.12.40.0",null,"5901988310981","OE - Côté courbé 5M P400","OE - Folding side barrier 5M D400","OE- PROTECC. EMB. LATERAL PLEGABLE 5M D400","ZENERGY - HAJLÍTOTT OLDALKERÍTÉS 5M D400"]
["31110","ZENERGY - COKÓŁ H400, OSŁONA PRZÓD,TYŁ, W1000",641.5,"1-ZE-01",0.01,1,"OE_PLINTHS",null,"SZT","85389099",null,null,"5901988311100","OE - Socle H400, avant, arrière, cache L1000","OE - H400 plinth, front and rear cover, W1000","OE- ZOCALO H400, FRONTAL/TRASERO (2UDS) W1000","ZENERGY - LÁZLET H400, BURKOLAT ELSŐ, HÁTSÓ, W1000"]
["31112","ZENERGY - COKÓŁ H400, OSŁONA PRZÓD,TYŁ, W1200",685.8,"1-ZE-01",null,null,"OE_PLINTHS",null,"SZT","85389099",null,null,"5901988311124","OE - Socle H400, couverture avant et arrière, L1200","OE - H400 plinth, front and rear cover, W1200","OE- ZOCALO H400, FRONTAL/TRASERO (2UDS) W1200","ZENERGY - Lábazat H400, BURKOLAT ELSŐ, HÁTSÓ, W1200"]
["31127","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H18MM D230, ZEWNĘTRZNY",32.5,"1-ZE-01",0.14166666666666666,1,"OE_SUPPORT","31126","SZT","85389099",null,null,"5901988311278","OE - SUPPORT DE PLAQUE DE MONTAGE H18MM P230, EXTERNE","OE - H18mm D230 Mounting plate BRACKET, EXTERNAL","*OE - SOPORTE DE PLACA DE MONTAJE H18MM D230, EXTERNO","ZENERGY - H18MM D230 SZERELŐLEMEZ TARTÓ, KÜLSŐ"]
["31136","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H18MM D300, ZEWNĘTRZNY",33.4,"1-ZE-01",0.3,1,"OE_SUPPORT","31136","SZT","85389099",null,null,"5901988311360","OE - Support de plaque de montage H18mm P300, externe","OE - H18mm D300 Mounting plate bracket, external","OE- SOPORTE DE PLACA MONTAJE  H18MM D300, EXTERNO","ZENERGY - H18MM D300 SZERELŐLEMEZ TARTÓ, KÜLSŐ"]
["31146","ZENERGY - WSPORNIK PŁYT MONTAŻOWYCH H18MM D400",35.5,"1-ZE-01",18.8,6,"OE_SUPPORT","31146","SZT","85389099","27.12.40.0",null,"5901988311469","OE - Support de plaque de montage H18mm P400","OE - Mounting plate bracket H18mm D400","OE- SOPORTE REGULACION PLACAS MONT. 3P/4P, D400","ZENERGY - H18MM D400 SZERELŐLEMEZ TARTÓ"]
["31150","ZENERGY - WYGRODZENIE POZIOME WYŁĄCZNIKÓW D200, W650 FORMA3",184.8,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988311506","OE - Cabine horizontale pour interrupteurs P200, L650 Forme 3","OE - Horizontal fencing for D200, W650 Forma3 circuit breakers","OE- Cercado HORIZ. de interruptores automáticos D200, W650 Forma3","ZENERGY - VÍZSZINTES KERÍTÉS D200, W650 FORMA3 MEGSZAKÍTÓHOZ"]
["31155","ZENERGY - WYGRODZENIE BOCZNE; DOCISK ŻALUZJI DO WSPORNIKA 31055 3P/4P, D400, FORMA2",34,"1-ZE-01",1.4833333333333334,6,"OE_SEPARATION_BUSBAR","31155","SZT","85389099","27.12.40.0",null,"5901988311551","OE - Clôture latérale; Stores pince sur support 31055 3P / 4P, P400, Forma2","OE - Side fence; Shutter pressure to the bracket 31055 3P / 4P, D400, separation Form 2","OE- TRAVESAŃO  MONTAJE EMBARRADO LATERAL PARA SOPORTES 3105X 3P/4P D400 FORMA 2","ZENERGY - OLDALKERÍTÉS; REDŐNYBORÍTÓ A 31055 3P/4P, D400, FORMA2 TÁMASZTÁSHOZ"]
["31158","ZENERGY - WYGRODZENIE SZYN POZIOMYCH POLA NAROŻNEGO D600, 4MOD 2 FORMA - KOMPLETNE (blachy pionowe + poziome)",574.6,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988311582","OE - CLÔTURE HORIZONTALE DE CHAMP D'ANGLE P600, FORME 4MOD 2 - COMPLÈTE (tôles verticales + horizontales)","OE - Horizontal rail fence of corner field D600, 4MOD 2 FORM - COMPLETE (Vertical + Horizontal sheets)","*OE - VALLA DE CARRIL HORIZONTAL DE CAMPO DE ESQUINA D600, 4MOD 2 FORMA - COMPLETO (hojas verticales + horizontales)","ZENERGY - D600 SZAROKTERÜLET VÍZSZINTES SÍNEK KERÍTÉSE, 4MOD 2 FORMA - TELJES (függőleges + vízszintes lapok)"]
["31163","ZENERGY - COKÓŁ H400, PEŁNE OSŁONY BOCZNE, D600",615.6,"1-ZE-01",1.6666666666666666E-2,1,"OE_PLINTHS",null,"SZT","85389099",null,null,"5901988311636","OE - Socle H400, écrans latéraux complets, P600","OE - H400 plinth, Plain side covers, D600","OE- ZOCALO H400, LATERAL (2UDS), D600","ZENERGY - LÁZLET H400, TELJES OLDALBURKOLATOK, D600"]
["31165","ZENERGY - COKÓŁ H400, OSŁONA PRZÓD,TYŁ, W650",483.8,"1-ZE-01",0.01,1,"OE_PLINTHS",null,"SZT","85389099",null,null,"5901988311650","OE - Socle H400, couverture avant et arrière, L650","OE - H400 plinth, front and rear cover, W650","OE- ZOCALO H400, FRONTAL/TRASERO (2UDS) W650","ZENERGY - LÁZLET H400, BURKOLAT ELSŐ, HÁTSÓ, W650"]
["31169","ZENERGY - NIEAKTUALNE (ZAM. 20406)",89.7,"1-ZE-01",null,null,"OE_SUPPORT","31169","SZT","85389099",null,null,"5901988311698","OE - obsolète (Zam. 20406)","OE - obsolete (replaces 20406)","OE- OBSOLETO (REEMPLAZA A 20406)","ZENERGY – ELVÉGZETT (RENDELÉS 20406)"]
["31172","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE 4MOD 2SZT W1300 2 FORMA",236.3,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988311728","OE - Barrières horizontales pour clôtures - Bâches verticales 4MOD 2pcs L1300 2 Form","OE - Horizontal rails fencing - Vertical sheets 4MOD 2pcs W1300 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. 4MOD W1300 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - BFÜGGŐLEGES LAP 4MOD 2DB W1300 2 FORMA"]
["31176","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE 4MOD 2SZT W600 2 FORMA",142.19999999999999,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","31176","SZT","85389099","27.12.40.0",null,"5901988311766","OE - Rails horizontaux pour clôtures - tôle verticale 4MOD 2pcs L600 2 Form","OE - Horizontal rails fencing - Vertical sheets 4MOD 2pcs W600 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. 4MOD W600 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - FÜGGŐLEGES LAP 4MOD 2DB W600 2 FORM"]
["31179","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE 4MOD 2SZT W850 2 FORMA",187,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","31179","SZT","85389099","27.12.40.0",null,"5901988311797","OE - Rails horizontaux pour clôtures - tôle verticale 4MOD 2pcs L850 2 Form","OE - Horizontal rails fencing - Vertical sheets 4MOD 2pcs W850 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. 4MOD W850 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - FÜGGŐLEGES LAP 4MOD 2DB W850 2 FORM"]
["31185","ZENERGY - COKÓŁ H400, OSŁONA PRZÓD,TYŁ, W850",565.9,"1-ZE-01",null,null,"OE_PLINTHS",null,"SZT","85389099",null,null,"5901988311858","OE - Socle H400, couverture avant et arrière, L850","OE - H400 plinth, front and rear cover, W850","OE- ZOCALO H400, FRONTAL/TRASERO (2UDS) W850","ZENERGY - Lábazat H400, BURKOLAT ELSŐ, HÁTSÓ, W850"]
["31189","ZENERGY - NIEAKTUALNE (ZAM. 20408)",93.6,"1-ZE-01",null,null,"OE_SUPPORT","31189","SZT","85389099",null,null,"5901988311896","OE - obsolète (Zam. 20408)","OE - obsolete (replaces 20408)","OE- OBSOLETO (REEMPLAZA A 20408)","ZENERGY – ELVÉGZETT (RENDELÉS 20408)"]
["31191","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE REGULOWANE 5-10MOD 1kpl W1200 2 Forma",432.3,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988311919","OE - Barrières horizontales pour clôtures - Bâches verticales régulier 5-10MOD 1jeu L1200 2 Form","OE - Fencing for Horizontal rails - Vertical adjustable sheets 5-10MOD 1 set W1200 2 Form","OE- Valla para rieles HORIZ.es - láminas ajustables VERT.es 5-10MOD 1 juego W1200 2 Forma","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - ÁLLÍTHATÓ FÜGGŐLEGES LAP 5-10MOD 1 készlet W1200 2 Forma"]
["31194","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE REGULOWANE 5-10MOD 1kpl W400 2 Forma",201.6,"1-ZE-01",5.8333333333333334E-2,1,"OE_SEPARATION_BUSBAR","31194","SZT","85389099","27.12.40.0",null,"5901988311940","OE - Barrières horizontales pour clôtures - Bâches verticales régulier 5-10MOD 1jeu L400 2 Form","OE - Fencing for Horizontal rails - Vertical adjustable sheets 5-10MOD 1 set W400 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. AJUST. ALTURA 5-10MOD  W400 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - ÁLLÍTHATÓ FÜGGŐLEGES LAP 5-10MOD 1 készlet W400 2 Forma"]
["31197","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE REGULOWANE 5-10MOD 1kpl W650 2 Forma",286,"1-ZE-01",1.1833333333333333,6,"OE_SEPARATION_BUSBAR","31197","SZT","85389099","27.12.40.0",null,"5901988311971","OE - Barrières horizontales pour clôtures - Bâches verticales régulier 5-10MOD 1jeu L650 2 Form","OE - Fencing for Horizontal rails - Vertical adjustable sheets 5-10MOD 1 set W650 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. AJUST. ALTURA 5-10MOD  W650 (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - ÁLLÍTHATÓ FÜGGŐLEGES LAP 5-10MOD 1 készlet W650 2 Forma"]
["31201","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE 3MOD 2szt W1200 2 Forma",160.19999999999999,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.12.40.0",null,"5901988312015","OE - Rails horizontaux pour clôtures - tôle verticale 3MOD 2pcs L1000 2 Form","OE - Horizontal rails fencing - 3MOD Vertical sheets 2pcs W1200 2 Form","OE- Cercado de rieles HORIZ.es - Láminas VERT.es 3MOD 2pcs W1200 2 Form","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - FÜGGŐLEGES LAP 3MOD 2 db W1200 2 Form"]
["31204","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE 3MOD 2szt W400 2 Forma",74.599999999999994,"1-ZE-01",8.3333333333333329E-2,4,"OE_SEPARATION_BUSBAR","31204","SZT","85389099","27.12.40.0",null,"5901988312046","OE - Rails horizontaux pour clôtures - tôle verticale 3MOD 2pcs L1000 2 Form","OE - Horizontal rails fencing - 3MOD Vertical sheets 2pcs W400 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. 3M (150MM) W400  (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - FÜGGŐLEGES LAP 3MOD 2 db W400 2 forma"]
["31207","ZENERGY - WYGRODZENIE SZYN POZIOMYCH - BLACHY PIONOWE 3MOD 2szt W650 2 Forma",107.5,"1-ZE-01",0.31666666666666665,4,"OE_SEPARATION_BUSBAR","31207","SZT","8538909900","27.12.40.0",null,"5901988312077","OE - Rails horizontaux pour clôtures - tôle verticale 3MOD 2pcs L1000 2 Form","OE - Horizontal rails fencing - 3MOD Vertical sheets 2pcs W650 2 Form","OE- PROTECC. EMBARRADO HORIZ. TAPAS VERT. 3M (150MM) W650  (2UDS) 2 FORMA","ZENERGY - VÍZSZINTES SÍNEK KERÍTÉSE - FÜGGŐLEGES LAP 3MOD 2 db W650 2 Form"]
["31211","ZENERGY - POKRYWA GÓRNA IP30, W650+400, D230",177.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988312114","OE - Capot supérieur IP30, L650 + 400, P230","OE - Top cover IP30, W650 + 400, D230","OE- TECHO IP30, W650+400, D230","ZENERGY - FELSŐ BURKOLAT IP30, W650+400, D230"]
["31215","ZENERGY - POKRYWA GÓRNA IP30, W650+450, D230",181.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988312152","OE - Capot supérieur IP30, L650 + 450, P230","OE - Top cover IP30, W650 + 450, D230","OE- TECHO IP30, W650+450, D230","ZENERGY - FELSŐ BURKOLAT IP30, W650+450, D230"]
["31219","ZENERGY - POKRYWA GÓRNA IP30, W850+400, D230",196.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988312190","OE - Capot supérieur IP30, L850 + 400, P230","OE - Top cover IP30, W850 + 400, D230","OE- TECHO IP30, W850+400, D230","ZENERGY - FELSŐ BURKOLAT IP30, W850+400, D230"]
["31220","ZENERGY - POKRYWA GÓRNA IP30, W850+450, D230",202,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988312206","OE - Capot supérieur IP30, L850 + 450, P230","OE - Top cover IP30, W850 + 450, D230","OE- TECHO IP30, W850+450, D230","ZENERGY - FELSŐ BURKOLAT IP30, W850+450, D230"]
["31227","ZENERGY - POKRYWA GÓRNA IP30, W150+850+300, D230",202,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988312275","OE - Capot supérieur IP30, L150 + 850 + 300, P230","OE - Top cover IP30, W150 + 850 + 300, D230","OE- TECHO IP30, W150+850+300, D230","ZENERGY - FELSŐ BURKOLAT IP30, W150+850+300, D230"]
["31233","ZENERGY - POKRYWA GÓRNA IP30, W200+650+400, D230",196.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988312336","OE - Capot supérieur IP30, L200 + 650 + 400, P230","OE - Top cover IP30, W200 + 650 + 400, D230","OE- TECHO IP30, W200+650+400, D230","ZENERGY – FELSŐ BURKOLAT IP30, W200+650+400, D230"]
["31260","ZENERGY - POKRYWA GÓRNA IP30, W600, D230",133.9,"1-ZE-01",null,null,"OE_COVERS","31260","SZT","85389099",null,null,"5901988312602","OE - Capot supérieur IP30, L600, P230","OE - Top cover IP30, W600, D230","OE- TECHO IP30, W600, D230","ZENERGY - FELSŐ BURKOLAT IP30, W600, D230"]
["31271","ZENERGY - POKRYWA GÓRNA IP30, W300+400, D230",142.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988312718","OE - Capot supérieur IP30, L300 + 400, P230","OE - Top cover IP30, W300 + 400, D230","OE- TECHO IP30, W300+400, D230","ZENERGY - FELSŐ BURKOLAT IP30, W300+400, D230"]
["31285","ZENERGY - POKRYWA GÓRNA IP30, W850, D230",157.69999999999999,"1-ZE-01",0.01,1,"OE_COVERS","31285","SZT","85389099",null,null,"5901988312855","OE - Capot supérieur IP30, L850, P230","OE - Top cover IP30, W850, D230","OE- TECHO IP30, W850, D230","ZENERGY - FELSŐ BURKOLAT IP30, W850, D230"]
["31295","ZENERGY - POKRYWA GÓRNA IP30, W650+300, D230",167.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988312954","OE - Capot supérieur IP30, L650 + 300, P230","OE - Top cover IP30, W650 + 300, D230","OE- TECHO IP30, W650+300, D230","ZENERGY - FELSŐ BURKOLAT IP30, W650+300, D230"]
["31312","ZENERGY - POKRYWA GÓRNA IP30, W1200, D300",298.10000000000002,"1-ZE-01",null,null,"OE_COVERS","31312","SZT","85389099",null,null,"5901988313128","OE - Capot supérieur IP30, L1200, P300","OE - Top cover IP30, W1200, D300","OE- TECHO IP30, W1200, D300","ZENERGY - FELSŐ BURKOLAT IP30, W1200, D300"]
["31313","ZENERGY - POKRYWA GÓRNA IP30, W1300, D300",315.39999999999998,"1-ZE-01",null,null,"OE_COVERS","31313","SZT","85389099",null,null,"5901988313135","OE - Capot supérieur IP30, L1300, P300","OE - Top cover IP30, W1300, D300","OE- TECHO IP30, W1300, D300","ZENERGY - FELSŐ BURKOLAT IP30, W1300, D300"]
["31318","ZENERGY - POKRYWA GÓRNA IP30, W850+300, D300",287.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988313180","OE - Capot supérieur IP30, L850 + 300, P300","OE - Top cover IP30, W850 + 300, D300","OE- TECHO IP30, W850+300, D300","ZENERGY - FELSŐ BURKOLAT IP30, W850+300, D300"]
["31322","ZENERGY - POKRYWA GÓRNA IP30, W150+650+300, D300",278.60000000000002,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988313227","OE - Capot supérieur IP30, L150 + 650 + 300, P300","OE - Top cover IP30, W150 + 650 + 300, D300","OE- TECHO IP30, W150+650+300, D300","ZENERGY – FELSŐ BURKOLAT IP30, W150+650+300, D300"]
["31330","ZENERGY - POKRYWA GÓRNA IP30, W300, D300",133.9,"1-ZE-01",null,null,"OE_COVERS","31330","SZT","85389099",null,null,"5901988313302","OE - Capot supérieur IP30, L300, P300","OE - Top cover IP30, W300, D300","OE- TECHO IP30, W300, D300","ZENERGY - FELSŐ BURKOLAT IP30, W300, D300"]
["31345","ZENERGY - POKRYWA GÓRNA IP30, W450, D300",160.9,"1-ZE-01",4.1666666666666664E-2,1,"OE_COVERS","31345","SZT","85389099",null,null,"5901988313456","OE - Capot supérieur IP30, L450, P300","OE - Top cover IP30, W450, D300","OE- TECHO IP30, W450, D300","ZENERGY - FELSŐ BURKOLAT IP30, W450, D300"]
["31371","ZENERGY - POKRYWA GÓRNA IP30, W300+400, D300",206.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988313715","OE - Capot supérieur IP30, L300 + 400, P300","OE - Top cover IP30, W300 + 400, D300","OE- TECHO IP30, W300+400, D300","ZENERGY - FELSŐ BURKOLAT IP30, W300+400, D300"]
["31381","ZENERGY - POKRYWA GÓRNA IP30, W650+150, D300",223.6,"1-ZE-01",0.13333333333333333,4,"OE_COVERS",null,"SZT","85389099",null,null,"5901988313814","OE - Capot supérieur IP30, L650 + 150, P300","OE - Top cover IP30, W650 + 150, D300","OE- TECHO IP30, W650+150, D300","ZENERGY - FELSŐ BURKOLAT IP30, W650+150, D300"]
["31385","ZENERGY - POKRYWA GÓRNA IP30, W850, D300",234.4,"1-ZE-01",0.19166666666666668,6,"OE_COVERS","31385","SZT","85389099",null,null,"5901988313852","OE - Capot supérieur IP30, L850, P300","OE - Top cover IP30, W850, D300","OE- TECHO IP30, W850, D300","ZENERGY - FELSŐ BORÍTÓRNS IP30, W850, D300"]
["31395","ZENERGY - POKRYWA GÓRNA IP30, W650+300, D300",251.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988313951","OE - Capot supérieur IP30, L650 + 300, P300","OE - Top cover IP30, W650 + 300, D300","OE- TECHO IP30, W650+300, D300","ZENERGY - FELSŐ BURKOLAT IP30, W650+300, D300"]
["31410","ZENERGY - POKRYWA GÓRNA IP30, W1000, D400",266.8,"1-ZE-01",0.38333333333333336,4,"OE_COVERS","31410","SZT","85389099","27.12.40.0",null,"5901988314101","OE - Capot supérieur IP30, L1000, P400","OE - Top cover IP30, W1000, D400","OE- TECHO IP30, W1000, D400","ZENERGY - FELSŐ BURKOLAT IP30, W1000, D400"]
["31415","ZENERGY - POKRYWA GÓRNA IP30, W650+450, D400",284,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988314156","OE - Capot supérieur IP30, L650 + 450, P400","OE - Top cover IP30, W650 + 450, D400","OE- TECHO IP30, W650+450, D400","ZENERGY - FELSŐ BURKOLAT IP30, W650+450, D400"]
["31419","ZENERGY - POKRYWA GÓRNA IP30, W850+400, D400",310,"1-ZE-01",null,null,"OE_COVERS","31419","SZT","85389099",null,null,"5901988314194","OE - Capot supérieur IP30, L850 + 400, P400","OE - Top cover IP30, W850 + 400, D400","OE- TECHO IP30, W850+400, D400","ZENERGY - FELSŐ BURKOLAT IP30, W850+400, D400"]
["31423","ZENERGY - POKRYWA GÓRNA IP30, W150+650+400, D400",301.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988314217","OE - Capot supérieur IP30, L150 + 650 + 400, P400","OE - Top cover IP30, W150 + 650 + 400, D400","OE- TECHO IP30, W150+650+400, D400","ZENERGY – FELSŐ BURKOLAT IP30, W150+650+400, D400"]
["31432","ZENERGY - POKRYWA GÓRNA IP30, W200+650+300, D400",292.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988314323","OE - Capot supérieur IP30, L200 + 650 + 300, P400","OE - Top cover IP30, W200 + 650 + 300, D400","OE- TECHO IP30, W200+650+300, D400","ZENERGY – FELSŐ BURKOLAT IP30, W200+650+300, D400"]
["31441","ZENERGY - POKRYWA GÓRNA IP30, W400, D400, z przepustem pod kable",285.10000000000002,"1-ZE-01",null,null,"OE_COVERS","31441","SZT","85389099","27.12.40.0",null,"5901988314415","OE - CAPOT SUPÉRIEUR IP30, L400, P400, avec presse-étoupe","OE - Top cover IP30, W400, D400, with a cable gland","OE- TECHO IP30, W400, D400, CON ENTRADA PARA CABLES","ZENERGY - FELSŐ BURKOLAT IP30, W400, D400, kábelbevezetéssel"]
["31445","ZENERGY - POKRYWA GÓRNA IP30, W450, D400",167.4,"1-ZE-01",null,null,"OE_COVERS","31445","SZT","85389099","27.12.40.0",null,"5901988314453","OE - Capot supérieur IP30, L450, P400","OE - Top cover IP30, W450, D400","OE- TECHO IP30, W450, D400","ZENERGY - FELSŐ BURKOLAT IP30, W450, D400"]
["31460","ZENERGY - POKRYWA GÓRNA IP30, W600, D400",194.4,"1-ZE-01",0.18333333333333332,2,"OE_COVERS","31460","SZT","85389099","27.12.40.0",null,"5901988314606","OE - Capot supérieur IP30, L600, P400","OE - Top cover IP30, W600, D400","OE- TECHO IP30, W600, D400","ZENERGY - FELSŐ BURKOLAT IP30, W600, D400"]
["31465","ZENERGY - POKRYWA GÓRNA IP30, W650, D400",203,"1-ZE-01",0.41666666666666669,6,"OE_COVERS","31465","SZT","85389099","27.12.40.0",null,"5901988314651","OE - Capot supérieur IP30, L650, P400","OE - Top cover IP30, W650, D400","OE- TECHO IP30, W650, D400","ZENERGY - FELSŐ BURKOLAT IP30, W650, D400"]
["31479","ZENERGY - POKRYWA GÓRNA IP30, W800, D400, z przepustem pod kable Lewy",406.1,"1-ZE-01",null,null,"OE_COVERS","31479","SZT","85389099","27.12.40.0",null,"5901988314798","OE - CAPOT SUPÉRIEUR IP30, L800, P400, avec presse-étoupe Gauche","OE - Top cover IP30, W800, D400, with a cable gland Left","OE- TECHO IP30, W800, D400, CON ENTRADA PARA CABLES IZQUIERDA","ZENERGY - FELSŐ BURKOLAT IP30, W800, D400, kábelbevezetéssel bal"]
["31482","ZENERGY - POKRYWA GÓRNA IP30, W800, D400, z przepustem pod kable Prawy",406.1,"1-ZE-01",null,null,"OE_COVERS","31482","SZT","85389099","27.12.40.0",null,"5901988314828","OE - CAPOT SUPÉRIEUR IP30, L800, P400, avec presse-étoupe Droit","OE - Top cover IP30, W800, D400, with a cable gland Right","OE- TECHO IP30, W650+150, D400, CON ENTRADA PARA CABLES DERECHA","ZENERGY - FELSŐ BURKOLAT IP30, W800, D400, kábelbevezetéssel Jobb"]
["31487","ZENERGY - POKRYWA GÓRNA IP30, W850, D400, z przepustem pod kable Prawy",432,"1-ZE-01",null,null,"OE_COVERS","31487","SZT","85389099","27.12.40.0",null,"5901988314873","OE - CAPOT SUPÉRIEUR IP30, L850, P400, avec presse-étoupe Droit","OE - Top cover IP30, W850, D400, with a cable gland Right","OE- TECHO IP30, W650+200, D400, CON ENTRADA PARA CABLES DERECHA","ZENERGY - FELSŐ BURKOLAT IP30, W850, D400, kábelbevezetéssel Jobb"]
["31500","ZENERGY - PŁYTA DŁAWICOWA IP55, W450+150, D1000",508.2,null,null,null,"OE_GLAND_PLATES",null,null,"85389099",null,null,"5901988315009"]
["31503","ZENERGY - PŁYTA DŁAWICOWA IP55, W650+200, D1000",669.9,null,null,null,"OE_GLAND_PLATES",null,null,"85389099",null,null,"5901988315030"]
["31506","ZENERGY - PŁYTA DŁAWICOWA IP55, W850+150, D1000",662.2,null,null,null,"OE_GLAND_PLATES",null,null,"85389099",null,null,"5901988315061"]
["31513","ZENERGY - PŁYTA DŁAWICOWA IP55, W450+200, D300",370.7,"1-ZE-01",null,null,"OE_GLAND_PLATES","31513","SZT","85389099","27.12.40.0",null,"5901988315139","OE - Plaque angulaire IP55, L450 + 200, P300","OE - Gland plate IP55, W450 + 200, D300","OE- PLACA PASACABLES IP55, W450 + 200, D300","ZENERGY - GANDING LEMEZ IP55, W450+200, D300"]
["31515","ZENERGY - PŁYTA DŁAWICOWA IP55, W450+200, D400",396,"1-ZE-01",null,null,"OE_GLAND_PLATES","31515","SZT","85389099","27.12.40.0",null,"5901988315153","OE - Plaque angulaire IP55, L450 + 200, P400","OE - Gland plate IP55, W450 + 200, D400","OE- PLACA PASACABLES IP55, W450 + 200, D400","ZENERGY - GANDING LEMEZ IP55, W450+200, D400"]
["31519","ZENERGY - PŁYTA DŁAWICOWA IP55, W450+200, D800",498.3,"1-ZE-01",null,null,"OE_GLAND_PLATES","31519","SZT","85389099","27.12.40.0",null,"5901988315191","OE - plaque presse-étoupe IP55, L450+200, P800","OE - Gland plate IP55, W450 + 200, D800","OE- PLACA PASACABLES IP55, W450 + 200, D800","ZENERGY - GANDING LEMEZ IP55, W450+200, D800"]
["31522","ZENERGY - PŁYTA DŁAWICOWA IP55, W1300, D230",339.9,"1-ZE-01",null,null,"OE_GLAND_PLATES","31522","SZT","85389099","27.12.40.0",null,"5901988315221","OE - Plaque angulaire IP55, L1300, P230","OE - Gland plate IP55, W1300, D230","OE- PLACA PASACABLES IP55, W1300, D230","ZENERGY - GANDING LEMEZ IP55, W1300, D230"]
["31526","ZENERGY - PŁYTA DŁAWICOWA IP55, W600, D230",256.3,"1-ZE-01",null,null,"OE_GLAND_PLATES","31526","SZT","85389099","27.12.40.0",null,"5901988315269","OE - Plaque d'angle IP55, L600, P230","OE - Gland plate IP55, W600, D230","OE- PLACA PASACABLES IP55, W600, D230","ZENERGY - GANDING LEMEZ IP55, W600, D230"]
["31529","ZENERGY - PŁYTA DŁAWICOWA IP55, W850, D230",281.60000000000002,"1-ZE-01",null,null,"OE_GLAND_PLATES","31529","SZT","85389099","27.12.40.0",null,"5901988315290","OE - Plaque angulaire IP55, L850, P230","OE - Gland plate IP55, W850, D230","OE- PLACA PASACABLES IP55, W850, D230","ZENERGY - GANDING LEMEZ IP55, W850, D230"]
["31532","ZENERGY - PŁYTA DŁAWICOWA IP55, W1300, D300",359.7,"1-ZE-01",null,null,"OE_GLAND_PLATES","31532","SZT","85389099",null,null,"5901988315320","OE - Plaque angulaire IP55, L1300, P300","OE - Gland plate IP55, W1300, D300","OE- PLACA PASACABLES IP55, W1300, D300","ZENERGY - GANDING LEMEZ IP55, W1300, D300"]
["31533","ZENERGY - PŁYTA DŁAWICOWA IP55, W300, D300",218.9,"1-ZE-01",null,null,"OE_GLAND_PLATES","31533","SZT","85381000","27.12.40.0",null,"5901988315337","OE - Plaque angulaire IP55, L300, P300","OE - Gland plate IP55, W300, D300","OE- PLACA PASACABLES IP55, W300, D300","ZENERGY - GANDING LEMEZ IP55, W300, D300"]
["31536","ZENERGY - PŁYTA DŁAWICOWA IP55, W600, D300",268.8,"1-ZE-01",3.3333333333333333E-2,2,"OE_GLAND_PLATES","31536","SZT","85389099",null,null,"5901988315368","OE - Plaque angulaire IP55, L600, P300","OE - Gland plate IP55, W600, D300","OE- PLACA PASACABLES IP55, W600, D300","ZENERGY - GANDING LEMEZ IP55, W600, D300"]
["31539","ZENERGY - PŁYTA DŁAWICOWA IP55, W850, D300",299,"1-ZE-01",null,null,"OE_GLAND_PLATES","31539","SZT","85389099",null,null,"5901988315399","OE - Plaque angulaire IP55, L850, P300","OE - Gland plate IP55, W850, D300","OE- PLACA PASACABLES IP55, W850, D300","ZENERGY - GANDING LEMEZ IP55, W850, D300"]
["31543","ZENERGY - PŁYTA DŁAWICOWA IP55, W300, D400",237.4,"1-ZE-01",0.48333333333333334,5,"OE_GLAND_PLATES","31543","SZT","85389099","27.12.40.0",null,"5901988315436","OE - Plaque angulaire IP55, L300, P400","OE - Gland plate IP55, W300, D400","OE- PLACA PASACABLES IP55, W300, D400","ZENERGY - GANDING LEMEZ IP55, W300, D400"]
["31546","ZENERGY - PŁYTA DŁAWICOWA IP55, W600, D400",287.8,"1-ZE-01",8.3333333333333329E-2,4,"OE_GLAND_PLATES","31546","SZT","85389099","27.12.40.0",null,"5901988315467","OE - Plaque angulaire IP55, L600, P400","OE - Gland plate IP55, W600, D400","OE- PLACA PASACABLES IP55, W600, D400","ZENERGY - GANDING LEMEZ IP55, W600, D400"]
["31550","ZENERGY - PŁYTA DŁAWICOWA IP55, W650+150, D230",432.3,"1-ZE-01",null,null,"OE_GLAND_PLATES","31550","SZT","85389099","27.12.40.0",null,"5901988315504","OE - Plaque angulaire IP55, L650 + 150, P230","OE - Gland plate IP55, W650 + 150, D230","OE- PLACA PASACABLES IP55, W650+150, D230","ZENERGY - GANDING LEMEZ IP55, W650+150, D230"]
["31553","ZENERGY - PŁYTA DŁAWICOWA IP55, W650+200, D300",422.4,"1-ZE-01",null,null,"OE_GLAND_PLATES","31553","SZT","85389099",null,null,"5901988315535","OE - Plaque angulaire IP55, L650 + 200, P300","OE - Gland plate IP55, W650 + 200, D300","OE- PLACA PASACABLES IP55, W650+200, D300","ZENERGY - GANDING LEMEZ IP55, W650+200, D300"]
["31556","ZENERGY - PŁYTA DŁAWICOWA IP55, W650+150, D600",565.6,"1-ZE-01",0.16666666666666666,7,"OE_GLAND_PLATES","31556","SZT","85389099","27.12.40.0",null,"5901988315566","OE - Plaque angulaire IP55, L650 + 150, P600","OE - Gland plate IP55, W650 + 150, D600","OE- PLACA PASACABLES IP55, W650+150, D600","ZENERGY - GANDING LEMEZ IP55, W650+150, D600"]
["31557","ZENERGY - PŁYTA DŁAWICOWA IP55, W650+200, D600",583.5,"1-ZE-01",null,null,"OE_GLAND_PLATES","31557","SZT","85389099","27.12.40.0",null,"5901988315573","OE - Plaque angulaire IP55, L650 + 200, P600","OE - Gland plate IP55, W650 + 200, D600","OE- PLACA PASACABLES IP55, W650+200, D600","ZENERGY - GANDING LEMEZ IP55, W650+200, D600"]
["31560","ZENERGY - PŁYTA DŁAWICOWA IP55, W1000, D600",454.7,"1-ZE-01",null,null,"OE_GLAND_PLATES","31560","SZT","85389099","27.12.40.0",null,"5901988315603","OE - Plaque d'angle IP55, L1000, P600","OE - Gland plate IP55, W1000, D600","OE- PLACA PASACABLES IP55, W1000, D600","ZENERGY - GANDING LEMEZ IP55, W1000, D600"]
["31564","ZENERGY - PŁYTA DŁAWICOWA IP55, W400, D600",313.60000000000002,"1-ZE-01",3.3333333333333333E-2,2,"OE_GLAND_PLATES","31564","SZT","85389099","27.12.40.0",null,"5901988315641","OE - Plaque angulaire IP55, L400, P600","OE - Gland plate IP55, W400, D600","OE- PLACA PASACABLES IP55, W400, D600","ZENERGY - GANDING LEMEZ IP55, W400, D600"]
["31567","ZENERGY - PŁYTA DŁAWICOWA IP55, W650, D600",384.2,"1-ZE-01",1.0916666666666666,10,"OE_GLAND_PLATES","31567","SZT","85389099","27.12.40.0",null,"5901988315672","OE - plaque presse-étoupe IP55, L650, P600","OE - Gland plate IP55, W650, D600","OE- PLACA PASACABLES IP55, W650, D600","ZENERGY - GANDING LEMEZ IP55, W650, D600"]
["31570","ZENERGY - PŁYTA DŁAWICOWA IP55, W850+150, D230",419.1,"1-ZE-01",null,null,"OE_GLAND_PLATES","31570","SZT","85389099",null,null,"5901988315702","OE - Plaque angulaire IP55, L850 + 150, P230","OE - Gland plate IP55, W850 + 150, D230","OE- PLACA PASACABLES IP55, W850 + 150, D230","ZENERGY - GANDING LEMEZ IP55, W850+150, D230"]
["31574","ZENERGY - PŁYTA DŁAWICOWA IP55, W850+150, D400",487.2,"1-ZE-01",0.14166666666666666,4,"OE_GLAND_PLATES","31574","SZT","85389099",null,null,"5901988315740","OE - Plaque angulaire IP55, L850 + 150, P400","OE - Gland plate IP55, W850 + 150, D400","OE- PLACA PASACABLES IP55, W850 + 150, D400","ZENERGY - GANDING LEMEZ IP55, W850+150, D400"]
["31578","ZENERGY - PŁYTA DŁAWICOWA IP55, W850+150, D800",620.4,"1-ZE-01",null,null,"OE_GLAND_PLATES","31578","SZT","85389099",null,null,"5901988315788","OE - plaque presse-étoupe IP55, L850+150, P800","OE - Gland plate IP55, W850 + 150, D800","OE- PLACA PASACABLES IP55, W850 + 150, D800","ZENERGY - GANDING LEMEZ IP55, W850+150, D800"]
["31581","ZENERGY - PŁYTA DŁAWICOWA IP55, W1200, D800",506.2,"1-ZE-01",null,null,"OE_GLAND_PLATES","31581","SZT","85389099",null,null,"5901988315818","OE - Plaque angulaire IP55, L1200, P800","OE - Gland plate IP55, W1200, D800","OE- PLACA PASACABLES IP55, W1200, D800","ZENERGY - GANDING LEMEZ IP55, W1200, D800"]
["31582","ZENERGY - PŁYTA DŁAWICOWA IP55, W1300, D800",527.5,"1-ZE-01",null,null,"OE_GLAND_PLATES","31582","SZT","85389099",null,null,"5901988315825","OE - Plaque angulaire IP55, L1300, P800","OE - Gland plate IP55, W1300, D800","OE- PLACA PASACABLES IP55, W1300, D800","ZENERGY - GANDING LEMEZ IP55, W1300, D800"]
["31585","ZENERGY - PŁYTA DŁAWICOWA IP55, W450, D800",324.8,"1-ZE-01",6.6666666666666666E-2,1,"OE_GLAND_PLATES","31585","SZT","85389099",null,null,"5901988315856","OE - Plaque angulaire IP55, L450, P800","OE - Gland plate IP55, W450, D800","OE- PLACA PASACABLES IP55, W450, D800","ZENERGY - GANDING LEMEZ IP55, W450, D800"]
["31589","ZENERGY - PŁYTA DŁAWICOWA IP55, W850, D800",422.2,"1-ZE-01",0.01,1,"OE_GLAND_PLATES","31589","SZT","85389099",null,null,"5901988315894","OE - Plaque angulaire IP55, L850, P800","OE - Gland plate IP55, W850, D800","OE- PLACA PASACABLES IP55, W850, D800","ZENERGY - GANDING LEMEZ IP55, W850, D800"]
["31592","ZENERGY - PŁYTA DŁAWICOWA IP55, W1300, D1000",548.79999999999995,null,null,null,"OE_GLAND_PLATES",null,null,"85389099",null,null,"5901988315924"]
["31595","ZENERGY - PŁYTA DŁAWICOWA IP55, W450, D1000",341,null,null,null,"OE_GLAND_PLATES",null,null,"85389099",null,null,"5901988315955"]
["31599","ZENERGY - PŁYTA DŁAWICOWA IP55, W850, D1000",443.5,null,null,null,"OE_GLAND_PLATES",null,null,"85389099",null,null,"5901988315993"]
["31612","ZENERGY - POKRYWA GÓRNA IP30, W1200, D600",371.5,"1-ZE-01",null,null,"OE_COVERS","31612","SZT","85389099",null,null,"5901988316129","OE - Capot supérieur IP30, L1200, P600","OE - Top cover IP30, W1200, D600","OE- TECHO IP30, W1200, D600","ZENERGY - FELSŐ BURKOLAT IP30, W1200, D600"]
["31616","ZENERGY - POKRYWA GÓRNA IP30, W850+150, D600",327.2,"1-ZE-01",null,null,"OE_COVERS","31610","SZT","85389099",null,null,"5901988316167","OE - Capot supérieur IP30, L850 + 150, P600","OE - Top cover IP30, W850 + 150, D600","OE- TECHO IP30, W850+150, D600","ZENERGY - FELSŐ BURKOLAT IP30, W850+150, D600"]
["31617","ZENERGY - POKRYWA GÓRNA IP30, W850+200, D600",344.5,"1-ZE-01",0.01,1,"OE_COVERS","31617","SZT","85389099",null,null,"5901988316174","OE - Capot supérieur IP30, L850 + 200, P600","OE - Top cover IP30, W850 + 200, D600","OE- TECHO IP30, W850 + 200, D600","ZENERGY - FELSŐ BURKOLAT IP30, W850+200, D600"]
["31620","ZENERGY - POKRYWA GÓRNA IP30, W850+450, D600",394.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988316204","OE - Capot supérieur IP30, L850 + 450, P600","OE - Top cover IP30, W850 + 450, D600","OE- TECHO IP30, W850+450, D600","ZENERGY - FELSŐ BURKOLAT IP30, W850+450, D600"]
["31628","ZENERGY - POKRYWA GÓRNA IP30, W150+850+400, D600",414.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988316280","OE - Capot supérieur IP30, L150 + 850 + 400, P600","OE - Top cover IP30, W150 + 850 + 400, D600","OE- TECHO IP30, W150+850+400, D600","ZENERGY – FELSŐ BURKOLAT IP30, W150+850+400, D600"]
["31633","ZENERGY - POKRYWA GÓRNA IP30, W200+650+400, D600",382.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988316334","OE - Capot supérieur IP30, L200 + 650 + 400, P600","OE - Top cover IP30, W200 + 650 + 400, D600","OE- TECHO IP30, W200+650+400, D600","ZENERGY – FELSŐ BURKOLAT IP30, W200+650+400, D600"]
["31660","ZENERGY - POKRYWA GÓRNA IP30, W600, D600",237.6,"1-ZE-01",8.3333333333333329E-2,2,"OE_COVERS","31660","SZT","85389099","27.12.40.0",null,"5901988316600","OE - Capot supérieur IP30, L600, P600","OE - Top cover IP30, W600, D600","OE- TECHO IP30, W600, D600","ZENERGY - FELSŐ BURKOLAT IP30, W600, D600"]
["31671","ZENERGY - POKRYWA GÓRNA IP30, W300+400, D600",261.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988316716","OE - Capot supérieur IP30, L300 + 400, P600","OE - Top cover IP30, W300 + 400, D600","OE- TECHO IP30, W300+400, D600","ZENERGY - FELSŐ BURKOLAT IP30, W300+400, D600"]
["31680","ZENERGY - POKRYWA GÓRNA IP30, W800, D600",261.39999999999998,"1-ZE-01",0.21666666666666667,4,"OE_COVERS","31680","SZT","85389099","27.12.40.0",null,"5901988316808","OE - Capot supérieur IP30, L800, P600","OE - Top cover IP30, W800, D600","OE- TECHO IP30, W800, D600","ZENERGY - FELSŐ BURKOLAT IP30, W800, D600"]
["31681","ZENERGY - POKRYWA GÓRNA IP30, W650+150, D600",261.39999999999998,"1-ZE-01",0.21666666666666667,2,"OE_COVERS","31680","SZT","85389099","27.12.40.0",null,"5901988316815","OE - Capot supérieur IP30, L650 + 150, P600","OE - Top cover IP30, W650 + 150, D600","OE- TECHO IP30, W650+150, D600","ZENERGY - FELSŐ BURKOLAT IP30, W650+150, D600"]
["31690","ZENERGY - POKRYWA GÓRNA IP30 POLA NAROŻNEGO D800",325.60000000000002,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988316907","OE - COUVERCLE SUPÉRIEUR IP30 BOÎTE D'ANGLE P800","OE - Top cover IP30 CORNER BOX D800","*OE - TAPA SUPERIOR IP30 CAJA DE ESQUINA D800","ZENERGY - FELSŐ BURKOLAT IP30 SAROK DOBOZ D800"]
["31712","OE - ŚRUBA M12X35, DIN 933 BIAŁY OCYNK KL.8.8, 6-KĄT - 100szt.",160.4,"1-ZE-01",null,null,null,null,"P",null,null,null,null,null,null,null,"OE - CSAVAR M12X35, DIN 933 FEHÉR HORGANYOZOTT OSZTÁLY 8.8, 6-SZÖG - 100 db."]
["31715","OE - ŚRUBA M12X50, DIN 933 BIAŁY OCYNK KL.8.8, 6-KĄT - 100szt.",271.10000000000002,"1-ZE-01",null,null,null,null,"P",null,null,null,null,null,null,null,"OE - CSAVAR M12X50, DIN 933 FEHÉR HORGANYOZOTT OSZTÁLY 8.8, 6-SZÖG - 100 db."]
["31718","OE - ŚRUBA M12X70, DIN 933 BIAŁY OCYNK KL.8.8, 6-KĄT - 100szt.",373.7,"1-ZE-01",null,null,null,null,"P",null,null,null,null,null,null,null,"OE - CSAVAR M12X70, DIN 933 FEHÉR HORGANYOZ 8.8 OSZTÁLY, 6 SZÖG - 100 db."]
["31803","ZENERGY - ŚRUBA M6X16 OCYNK SZEŚCIOKANT KL. 8.8 DIN 933 - 100SZT (31925)",30.6,"1-ZE-01",null,null,"OE_SUPPORT",null,"P","85389099","27.12.40.0",null,"5901988318031","OE - Vis M6x16 à six pans creux galvanisé 8.8 DIN 933 - 100pcs (31925)","OE - Bolt M6x16, Galvanized hexagonal, class 8.8 DIN 933 - 100 pieces (31925)","OE- Perno M6x16, hexagonal galvanizado, clase 8.8 DIN 933 - 100 piezas (31925)","ZENERGY - CSAVAR M6X16 HANGANYOZOTT OSZTÁLY. 8,8 DIN 933 – 100 DB (31925)"]
["31810","ZENERGY - POKRYWA GÓRNA IP30, W1000, D800",399.3,"1-ZE-01",4.1666666666666664E-2,1,"OE_COVERS","31810","SZT","85389099",null,null,"5901988318109","OE - Capot supérieur IP30, L1000, P800","OE - Top cover IP30, W1000, D800","OE- TECHO IP30, W1000, D800","ZENERGY - FELSŐ BURKOLAT IP30, W1000, D800"]
["31813","ZENERGY - POKRYWA GÓRNA IP30, W1300, D800",485.1,"1-ZE-01",null,null,"OE_COVERS","31813","SZT","85389099",null,null,"5901988318130","OE - Capot supérieur IP30, L1300, P800","OE - Top cover IP30, W1300, D800","OE- TECHO IP30, W1300, D800","ZENERGY - FELSŐ BURKOLAT IP30, W1300, D800"]
["31815","ZENERGY - POKRYWA GÓRNA IP30, W650+450, D800",429,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988318154","OE - Capot supérieur IP30, L650 + 450, P800","OE - Top cover IP30, W650 + 450, D800","OE- TECHO IP30, W650+450, D800","ZENERGY - FELSŐ BURKOLAT IP30, W650+450, D800"]
["31818","ZENERGY - POKRYWA GÓRNA IP30, W850+300, D800",442.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988318185","OE - Capot supérieur IP30, L850 + 300, P800","OE - Top cover IP30, W850 + 300, D800","OE- TECHO IP30, W850+300, D800","ZENERGY - FELSŐ BURKOLAT IP30, W850+300, D800"]
["31821","ZENERGY - POKRYWA GÓRNA IP30, W150+650+400, D800",457.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988318215","OE - Capot supérieur IP30, L150 + 650 + 400, P800","OE - Top cover IP30, W150 + 650 + 400, D800","OE- TECHO IP30, W150+650+400, D800","ZENERGY – FELSŐ BURKOLAT IP30, W150+650+400, D800"]
["31830","ZENERGY - POKRYWA GÓRNA IP30, W300, D800",201.3,"1-ZE-01",null,null,"OE_COVERS","31830","SZT","85389099",null,null,"5901988318307","OE - Capot supérieur IP30, L300, P800","OE - Top cover IP30, W300, D800","OE- TECHO IP30, W300, D800","ZENERGY - FELSŐ BURKOLAT IP30, W300, D800"]
["31840","ZENERGY - POKRYWA GÓRNA IP30, W400, D800",231,"1-ZE-01",4.1666666666666664E-2,1,"OE_COVERS","31840","SZT","85389099","27.12.40.0",null,"5901988318406","OE - Capot supérieur IP30, L400, P800","OE - Top cover IP30, W400, D800","OE- TECHO IP30, W400, D800","ZENERGY - FELSŐ BURKOLAT IP30, W400, D800"]
["31860","ZENERGY - POKRYWA GÓRNA IP30, W600, D800",287.10000000000002,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","31860","SZT","85389099",null,null,"5901988318604","OE - Capot supérieur IP30, L600, P800","OE - Top cover IP30, W600, D800","OE- TECHO IP30, W600, D800","ZENERGY - FELSŐ BURKOLAT IP30, W600, D800"]
["31866","ZENERGY - POKRYWA GÓRNA IP30, W450+200, D800",300.3,"1-ZE-01",null,null,"OE_COVERS","31865","SZT","85389099",null,null,"5901988318666","OE - Capot supérieur IP30, L450 + 200, P800","OE - Top cover IP30, W450 + 200, D800","OE- TECHO IP30, W450+200, D800","ZENERGY - FELSŐ BURKOLAT IP30, W450+200, D800"]
["31879","ZENERGY - POKRYWA GÓRNA IP30, W800, D800, z przepustem pod kable Lewy",548.9,"1-ZE-01",null,null,"OE_COVERS","31879","SZT","85389099","27.12.40.0",null,"5901988318796","OE - Capot supérieur IP30, L800, P800, avec un conduit pour câbles Droit","OE - Top cover IP30, W800, D800, with a cable gland Left","OE- TECHO IP30, W800, D800, CON PRENSAESTOPAS DERECHA","ZENERGY - FELSŐ BURKOLAT IP30, W800, D800, kábelbemenettel bal"]
["31880","ZENERGY - POKRYWA GÓRNA IP30, W800, D800",343.2,"1-ZE-01",8.3333333333333329E-2,4,"OE_COVERS","31880","SZT","85389099","27.12.40.0",null,"5901988318802","OE - Capot supérieur IP30, L800, P800","OE - Top cover IP30, W800, D800","OE- TECHO IP30, W800, D800","ZENERGY - FELSŐ BURKOLAT IP30, W800, D800"]
["31884","ZENERGY - POKRYWA GÓRNA IP30, W850, D800, z przepustem pod kable Lewy",573.1,"1-ZE-01",null,null,"OE_COVERS","31884","SZT","85389099","27.12.40.0",null,"5901988318840","OE - CAPOT SUPÉRIEUR IP30, L850, P800, avec presse-étoupe Gauche","OE - Top cover IP30, W850, D800, with a conduit for cables Left","OE- TECHO IP30, W850, D800 CON ENTRADA PARA CABLES IZQUIERDA","ZENERGY - FELSŐ BURKOLAT IP30, W850, D800, kábelbemenettel bal"]
["31887","ZENERGY - POKRYWA GÓRNA IP30, W850, D800, z przepustem pod kable Prawy",573.1,"1-ZE-01",null,null,"OE_COVERS","31887","SZT","85389099","27.12.40.0",null,"5901988318871","OE - CAPOT SUPÉRIEUR IP30, L850, P800, avec presse-étoupe Droit","OE - Top cover IP30, W850, D800, with cable entry Right","OE- TECHO IP30, W650+200, D800 CON ENTRADA PARA CABLES DERECHA","ZENERGY - FELSŐ BURKOLAT IP30, W850, D800, kábelbevezetésselJobbra"]
["31900","OE - Wkręty samowiercące, formujące Torx-25 M5x16 - 500 sztuk",198.7,"1-ZE-01",0.5,1,"OE_SUPPORT","31900","P","7318159500",null,null,"5901988319007","OE - Vis autoformeuses Torx-25 M5x16 - 500 pcs","OE - Torx-25 M5x16 self-drilling forming screws - 500 pieces","OE -TORNILLO AUTOROSCANTE TORX-25 M5x16 - 500 UDS","OE - Önfúró, alakító csavarok Torx-25 M5x16 - 500 db"]
["31903","ZENERGY - METALOWA KRATKA WENTYLACYJNA IP54 +  MATA FILTR; OTWÓR:280X450MM",131,"1-ZE-01",0.15833333333333333,4,"OE_VENTILATION",null,"SZT","85389099",null,null,"5901988319038","OE - Grille de ventilation en métal IP54 + passe-filtre; trou: 280x450mm","OE - Metal ventilation grille IP54 + filter mat; opening: 280x450mm","OE- REJILLA VENTIL. MET. IP54 + FILTRO; AGUJERO:280X450MM","ZENERGY - FÉM SZELLŐZŐRÁCS IP54 + SZŰRŐSÉTÉNY; LYUK: 280X450MM"]
["31907","ZENERGY - WKRĘT DO METALU Z ŁBEM STOŻKOWYM Z WGŁ. KRZYŻ. M5X70, OCYNK - 100SZT.",55.2,"1-ZE-01",null,null,"OE_SUPPORT",null,"P","73181595",null,null,"5901988319076","OE - Vis en métal à tête fraisée avec capuchon. traverser. M5x70, galvanisé - 100 pièces","OE - Countersunk metal screw with recess cross. M5x70, Galvanized - 100 pcs.","OE-TORNILLO PARA METAL. M5X70,  - 100UDS","ZENERGY - ELLENFEJES FÉM CSAVAR KERESZT. M5X70, HORGANYOZOTT - 100 DB."]
["31911","ZENERGY - WKRĘTY SAMOFORMUJĄCE M5X8 DIN 7500PE - 500SZT",206.3,"1-ZE-01",null,null,"OE_SUPPORT","31911","P","73181595","25.94.11.0",null,"5901988319113","OE - Vis auto-perforantes M5x8 DIN 7500C - 500pcs","OE - Self-forming screws M5x8 DIN 7500PE - 500pcs","OE- TORNILLOS AUTOROSCANTES M5X8 DIN 7500C - 500UDS","ZENERGY - ÖNFORMÁLÓ CSAVAROK M5X8 DIN 7500PE - 500 DB"]
["31915","ZENERGY - ŚRUBY Z ŁBEM WPUSZCZONYM  Z GNIAZDEM SZEŚCIOKĄTNYM M5X10 DIN 7500M - 1000SZT",263.5,"1-ZE-01",3.3333333333333333E-2,1,"OE_SUPPORT","31915","P","73181595","25.94.11.0",null,"5901988319151","OE - Vis à tête fraisée à six pans creux M5x10 DIN 7500M - 1000 pcs","OE - M5x10 DIN 7500M recessed head screws - 1000pcs","OE- TORNILLO HEXAGONAL M5X10 DIN 7500M - 1000UDS","ZENERGY - ELLÁTÁSÚ FEJŰ CSAVAROK M5X10 DIN 7500M - 1000 DB HEXALJAL"]
["31916","ZENERGY - ŚRUBY Z ŁBEM WPUSZCZONYM  Z GNIAZDEM SZEŚCIOKĄTNYM M5X25 DIN 7500M - 1000SZT",353.2,"1-ZE-01",0.01,1,"OE_SUPPORT","31916","P","73181595","25.94.11.0",null,"5901988319168","OE - Vis à tête fraisée à six pans creux M5x25 DIN 7500M - 1000 pcs","OE - Countersunk screws with hexagon socket M5x25 DIN 7500M - 1000pcs","OE- TORNILLO HEXAGONAL M5X25 DIN 7500M - 1000UDS","ZENERGY - ELLÁTÁSÚ FEJŰ CSAVAROK M5X25 DIN 7500M - 1000 DB HEXALJAL"]
["31919","ZENERGY - ŚRUBA GRZYBKOWA KOŁNIERZOWA M5×6 OCYNK ISO7380 - 100SZT.",23.3,"1-ZE-01",null,null,"OE_SUPPORT",null,"P","73181595","25.94.11.0",null,"5901988319199","OE - Boulon à collerette M5 M6 × 6 galvanisé ISO7380 - 100pcs","OE - M5 × 6 shoulder bolt Galvanized ISO7380 - 100 pcs.","OE- M5 × 6 cuello cabeza de hongo galvanizado ISO7380 - 100 uds.","ZENERGY - KARIMÁS GOMBÁS CSAVAR M5×6 HORGANYOZOTT ISO7380 - 100 DB."]
["31922","ZENERGY - NAKRĘTKA Z KOŁNIERZEM ZĄBKOWANYM M6 DIN6923 - 100SZT.",15.8,"1-ZE-01",null,null,"OE_SUPPORT","31922","P","73181595","25.94.11.0",null,"5901988319229","OE - Ecrou à collerette M6 DIN6923 - 100pcs","OE - Nut with serrated collar M6 DIN6923 - 100pcs","OE- TUERCA CON COLLAR DENTADO  M6 DIN6923 - 100UDS","ZENERGY - ANYA FOGÁZOTT KARIMÁVAL M6 DIN6923 - 100 DB."]
["31926","ZENERGY - NAKRĘTKA Z UCHEM M10 DIN 582 - 100SZT.",866.2,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","73181595","25.94.11.0",null,"5901988319267","OE - Écrou avec oreille M10 DIN 582 - 100pcs","OE - Eye nut M10 DIN 582 - 100pcs","OE- Tuerca de ojo M10 DIN 582 - 100uds","ZENERGY - ANYA FÜLEVEL M10 DIN 582 - 100 DB."]
["31929","OE - Pędzelek z farbą do retuszu RAL 7035",77.900000000000006,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","73181595","25.94.11.0",null,"5901988319298","OE - Spray de retouche RAL 9001","OE - Retouching spray RAL 9001","OE- PINTURA EN SPRAY RAL 9001","OE - Ecset RAL 7035 retusáló festékkel"]
["31933","ZENERGY - WSPORNIK + IZOLATORY NA PLECY 3P M8 30/30 ROZSTAW 100MM",126.6,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"SZT","85389099","27.12.40.0",null,"5901988319335","OE - Support + isolateurs dorsaux 3P M8 30/30 entraxe 100mm","OE - Bracket + insulators for the back 3P M8 30/30, spacing 100mm","OE- SOPORTE + SOPORTE FONDO  3P M8 30/30 SEPARACION 100MM","ZENERGY - KONZOL + HÁTSZIGETELŐK 3P M8 30/30 HELY 100MM"]
["31936","ZENERGY - NAKRĘTKA M12, DIN 934 BIAŁY OCYNK. KL.8.8 - 100szt.",53.8,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH",null,"P","8538909900",null,null,"5901988319366","OE - support PE / N + isolateur M8 30/30","OE - PE / N bracket + insulator M8 30/30","OE- SOPORTE PE / N + SOPORT. PARA BARRA M8 30/30","ZENERGY - ANYA M12, DIN 934 FEHÉR HORGANYOZ. CL.8.8 - 100 db."]
["31939","ZENERGY - ZAŚLEPKI BARYŁKOWE 7.2 DO POPRZECZKI - 1000SZT.",790.6,"1-ZE-01",null,null,"OE_SUPPORT",null,"P","85389099","27.12.40.0",null,"5901988319397","OE - Embouts sphériques - 1000 pcs","OE - Barrel End Caps for the Crossbar - 1000pcs","OE- TAPONES PARA TRAVIESAS - 1000UDS","ZENERGY - 7.2 HORDÓ DUGÓ KERESZTRUDAHOZ - 1000 DB."]
["31940","ZENERGY - METALOWA KRATKA WENTYLACYJNA, BEZ MATY FILTRA; OTWÓR:160X160MM; DO WENTYLATORA:120X120MM; FRONT:196X180MM; GŁĘBOKOŚĆ:15MM",89.9,"1-ZE-01",0.65833333333333333,2,"OE_VENTILATION",null,"SZT","85389099","27.12.40.0",null,"5901988319403","OE - Grille de ventilation en métal, sans tapis filtrant; ouverture: 160x160mm; pour le ventilateur: 120x120mm; Avant: 196x180mm; Profondeur: 15 mm","OE - Metal ventilation grille, without filter mat; opening: 160x160mm; for the fan: 120x120mm; front: 196x180mm; depth: 15mm","OE- Rejilla de ventilación metálica, sin estera filtrante; agujero: 160x160mm; para ventilador: 120x120mm; frente: 196x180mm; profundidad: 15 mm","ZENERGY - FÉM SZELLŐZŐRÁCS, SZŰRŐSÉTÉNY NÉLKÜL; LYUK:160X160MM; VENTILÁTORHOZ:120X120MM; ELSŐ:196X180MM; MÉLYSÉG: 15mm"]
["31943","ZENERGY - ŚRUBA M6X110 DIN933 A2 AISI304 DLA MOSTÓW ALCUBAR H80 (1600A) - 100SZT.",202,"1-ZE-01",4.1666666666666664E-2,4,"OE_SUPPORT","31943","P","73181595","25.94.11.0","230927LK","5901988319434","OE - Vis M6x110 DIN933 A2 AISI304 pour ponts AlCubar H80 (1600A) - 100pcs","OE - Screw M6x110 DIN933 A2 AISI304 for AlCubar H80 (1600A) bridges - 100 pcs","*OE - TORNILLO M6X110 DIN933 A2 AISI304 PARA PUENTE ALCUBAR H80 (1600A) - 100 UDS.","ZENERGY - CSAVAR M6X110 DIN933 A2 AISI304 AlCubar H80 HIDAKHOZ (1600A) - 100 DB."]
["31947","ZENERGY - PRĘT GWINTOWANY M6X1000 INOX A2 AISI304 DLA MOSTÓW ALCUBAR  3200-6300A - 100SZT",948.6,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR","31947","P","73181595","25.94.11.0","231011LK","5901988319472","OE - Tige filetée M6x1000 INOX A2 AISI304 pour ponts AlCubar 3200-6300A - 100pcs","OE - Threaded rod M6x1000 INOX A2 AISI304 for AlCubar 3200-6300A bridges - 100 pcs","OE- VARILLA ROSCADA M6X1000 A2 INOX AISI 304 - 100UDS","ZENERGY - MENETES RÚD M6X1000 INOX A2 AISI304 AlCubarHIDAKHOZ 3200-6300A - 100 DB"]
["31950","ZENERGY - METALOWA KIESZEŃ NA DOKUMENTACJĘ W1000",84.2,"1-ZE-01",0.30833333333333335,1,"OE_SUPPORT",null,"KPL","85389099","27.12.40.0",null,"5901988319502","OE - Pochette en métal pour la documentation L1000","OE - Metal pocket for W1000 documentation","OE- PORTADOCUMENTOS W1000","ZENERGY - FÉM DOKUMENTÁCIÓS ZSEB W1000"]
["31953","ZENERGY - METALOWA KIESZEŃ NA DOKUMENTACJĘ W300",44.9,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099","27.12.40.0",null,"5901988319533","OE - Pochette en métal pour la documentation L300","OE - Metal pocket for W300 documentation","OE- PORTADOCUMENTOS W300","ZENERGY - FÉM DOKUMENTÁCIÓS ZSEB W300"]
["31957","ZENERGY - METALOWA KIESZEŃ NA DOKUMENTACJĘ W650 / PODWÓJNE W1300",66.5,"1-ZE-01",0.35833333333333334,1,"OE_SUPPORT","31957","SZT","85389099","27.12.40.0",null,"5901988319571","OE - Pochette en métal pour la documentation L650","OE - Metal pocket for W650 documentation","OE- PORTADOCUMENTOS W650","ZENERGY - FÉM DOKUMENTÁCIÓS ZSEB W650 / DOUBLE W1300"]
["31960","ZENERGY - ZAWIESZENIE DO ŚCIANY (OBUDOWA WISZĄCA) W1050 (650+400)",210.6,"1-ZE-01",0.01,1,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988319601","OE - Suspension murale (boîtier suspendu) L1050 (650 + 400)","OE - Suspension to the wall (hanging housing) W1050 (650 + 400)","OE- PIEZA FIJACION MURAL (ARMARIO MURAL) W1050 (650+400)","ZENERGY - FALFÜGGESZTÉS (FÜGGŐ HÁZ) W1050 (650+400)"]
["31963","ZENERGY - ZAWIESZENIE DO ŚCIANY (OBUDOWA WISZĄCA) W1250 (850+400)",235.4,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988318543","OE - Suspension murale (boîtier suspendu) W1250 (850 + 400)","OE - Suspension to the wall (hanging housing) W1250 (850 + 400)","OE- PIEZA FIJACION MURAL (ARMARIO MURAL) W1250 (850+400)","ZENERGY - FALFÜGGESZTÉS (FÜGGŐ HÁZ) W1250 (850+400)"]
["31965","ZENERGY - POKRYWA GÓRNA IP30, W650, D1000",377.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0","210120LK","5901988319656","OE - COUVERCLE SUPÉRIEUR IP30, L650, P1000","OE - Top cover IP30, W650, D1000","*OE - CUBIERTA SUPERIOR IP30, W650, D1000","ZENERGY - FELSŐ BURKOLAT IP30, W650, D1000"]
["31969","ZENERGY - ZAWIESZENIE DO ŚCIANY (OBUDOWA WISZĄCA) W950 (650+300)",195.5,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099",null,null,"5901988319656","OE - Suspension murale (murale) W950 (650 + 300)","OE - Suspension to the wall (hanging housing) W950 (650 + 300)","OE- PIEZA FIJACION MURAL (ARMARIO MURAL) W950 (650+300)","ZENERGY - FALFÜGGESZTÉS (FÜGGŐ HÁZ) W950 (650+300)"]
["31973","ZENERGY - ZAWIESZENIE DO ŚCIANY (OBUDOWA WISZĄCA) W300",117.7,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099","27.12.40.0",null,"5901988319731","OE - Suspension murale (murale) L300","OE - Suspension to the wall (hanging housing) W300","OE- PIEZA FIJACION MURAL (ARMARIO MURAL) W300","ZENERGY - FALFÜGG. (FÜGGŐ HÁZ) W300"]
["31978","ZENERGY - ZAWIESZENIE DO ŚCIANY (OBUDOWA WISZĄCA) W800",177.1,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099","27.12.40.0",null,"5901988319786","OE - Suspension murale (murale) L800","OE - Suspension to the wall (hanging housing) W800","OE- PIEZA FIJACION MURAL (ARMARIO MURAL) W800","ZENERGY - FELFÜGGESZTÉSFALRA (FÜGGŐ HÁZRA) W800"]
["31980","ZENERGY OM - PRZEPUST - MEMBRANA KABLOWA PMB35 IP-65",65.5,"1-ZE-09",1.7666666666666666,5,"OM_HORIZONTAL_COVER","ZENNPMB35","SZT","85389099",null,null,"5901988319809","OM - Pénétration - Membrane de câble PMB35 IP-65","OM - Culvert - PMB35 IP-65 cable membrane","OM- Alcantarilla - Membrana de cable PMB35 IP-65","ZENERGY OM - PERSELY - KÁBEL MEMBRÁN PMB35 IP-65"]
["31984","ZENERGY - ŁĄCZNIK SZYNY 1X10X50,  50X60",165.6,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988319847","OE - Connecteur de rail 1x10x50, 50x60","OE - 1x10x50, 50x60 rail connector","OE- UNION BARRAS PLANAS 1X10X50,  50X60","ZENERGY - SÍN CSATLAKOZÓ 1X10X50, 50X60"]
["31987","ZENERGY - ŁĄCZNIK SZYNY 1X10X100,  100X80",371.5,"1-ZE-01",0.31666666666666665,1,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988319878","OE - Connecteur de rail 1x10x100, 100x80","OE - Rail connector 1x10x100, 100x80","OE- UNION BARRAS PLANAS 1X10X100,  100X80","ZENERGY – SÍN CSATLAKOZÓ 1X10X100, 100X80"]
["31991","ZENERGY - METALOWA KRATKA OSŁONA NA TYŁ WENTYLATORA:172X151MM",37,"1-ZE-01",3.3333333333333333E-2,2,"OE_VENTILATION",null,"SZT","85389099","27.12.40.0",null,"5901988319915","OE - COUVERCLE DE VENTILATEUR ARRIÈRE EN GRILLE MÉTALLIQUE : 172X151MM","OE - Metal ventilation grille for vent back:172X151mm","*OE - CUBIERTA DE VENTILADOR TRASERO DE REJILLA METÁLICA: 172X151MM","ZENERGY - FÉM RÁCS BURKOLAT A VENTILÁTOR HÁTSÁHOZ: 172X151MM"]
["31992","ZENERGY - PRĘT GWINTOWANY M6x160 INOX A2 AISI304 dla mostów Miedzianych 120mm - 100SZT",201.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_BUSBARS_ALCUBAR","31992","P","73181595","25.94.11.0","231011LK","5901988319922","OE - Tige filetée M6x160 INOX A2 AISI304 pour ponts120mm - 100pcs","OE - Threaded rod M6x160 INOX A2 AISI304 for busbars 120mm - 100 pcs","OE- VARILLA ROSCADA M6X160 A2 INOX AISI 304 - 100UDS","ZENERGY - MENETES RÚD M6x160 INOX A2 AISI304 rézhídhoz 120mm - 100DB"]
["31995","ZENERGY - ŁĄCZNIK SZYNY 2X10X60,  60X60",189.8,"1-ZE-01",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","74072900",null,null,"5901988319953","OE - Connecteur de rail 2x10x60, 60x60","OE - Rail connector 2x10x60, 60x60","OE- UNION BARRAS PLANAS 2X10X60,  60X60","ZENERGY - SÍN CSATLAKOZÓ 2X10X60, 60X60"]
["31999","ZENERGY - Etykieta samoprzylepna \"Nie stawać na\" średnica 100mm",16.2,"1-ZE-01",null,null,"OE_ACCESSORIES","31999","SZT","85389099",null,"230927LK","5901988319991","Ne pas marcher sur... – Autocollant adhésif 100 mm de diamètre","OE - Self-adhesive label \"Do not stand\" 100mm diameter","*OE - Etiqueta autoadhesiva \"No pisar\" 100 mm de diámetro","ZENERGY - Öntapadós \"Ne lépj rá\" címke átmérője 100mm"]
["32002","ZENERGY OU - SZYNA APARATURY MODUŁOWEJ TS-35, W350, D180, 10 MOD, KOMPLETNA",27.1,"1-ZE-01",null,null,"OE_RAIL_DIN",null,"SZT","85389099",null,null,"5901988320027","OU - Rail d'équipement modulaire TS-35, W350, D180, 10 mod, complet","OU - Modular equipment rail TS-35, W350, D180, 10 mod, complete","OU- CARRIL DIN, W350, D180, 10 MOD, COMPLETO","ZENERGY OU - MODULÁRIS BERENDEZÉS SÍN TS-35, W350, D180, 10 MOD, TELJES"]
["32005","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W400, 10 MOD, REGULOWANA, BEZ WSPORNIKÓW",50.4,"1-ZE-01",null,null,"OE_RAIL_DIN","32005","SZT","8538909900","27.12.40.0",null,"5901988320058","OE - Rail d'appareil modulaire TS-35, L400, 10 mod., Réglable, sans supports","OE - Modular apparatus rail TS-35, W400, 10 mod, adjustable, without supports","OE-CARRIL DIN, W400, 10 MOD. REGUL. PROF.  SIN SOPORT.","ZENERGY - MODULÁRUS BERENDEZÉS SÍN TS-35, W400, 10 MOD, ÁLLÍTHATÓ, KONZER NÉLKÜL"]
["32010","ZENERGY - OSŁONA CZOŁOWA PEŁNA W400, 1M / 250",37.700000000000003,"1-ZE-01",null,null,"01_PLAIN_COVERS","32010","SZT","85389099","27.12.40.0",null,"5901988320102","OE - Couverture avant complète L400, 1M / 250","OE - Plain Front cover W400, 1M / 250","OE- TAPA CIEGA W400, 1M (H 50MM)","ZENERGY - TELJES ELSŐ BURKOLAT W400, 1M / 250"]
["32013","ZENERGY - ZESTAW OŚWIETLENIA ROZDZIELNICY W850, z osłonami czołowymi",433.6,"1-ZE-01",1.6666666666666666E-2,1,"OE_ACCESSORIES",null,"SZT","85389099","27.12.40.0",null,"5901988320133","OE - Kit d'éclairage pour appareillage L850","OE - W850 switchgear lighting kit","OE- Kit de iluminación para aparamenta W850","ZENERGY - W850 KAPCSOLÓVILÁGÍTÁS KÉSZLET, előlapokkal"]
["32014","ZENERGY - ZESTAW OŚWIETLENIA ROZDZIELNICY W1000, z osłonami czołowymi",455.4,"1-ZE-01",null,null,"OE_ACCESSORIES",null,"SZT","85389099",null,null,"5901988320140","OE - KIT D'ÉCLAIRAGE DE TABLEAU L1000, avec capots avant","OE - W1000 Switchboard lighting kit, with Front covers","*OE - W1000 KIT DE ILUMINACIÓN DE TABLERO, con cubiertas frontales","ZENERGY - W1000 KAPCSOLÓ VILÁGÍTÁS KÉSZLET, előlapokkal"]
["32017","ZENERGY - ZESTAW OŚWIETLENIA ROZDZIELNICY W1000, bez osłon czołowych",415.2,"1-ZE-01",null,null,"OE_ACCESSORIES","32017","SZT","85389099",null,null,"5901988320171","OE - KIT D'ÉCLAIRAGE DE TABLEAU L1000, sans façades","OE - W1000 Switchboard lighting kit, without Front covers","*OE - W1000 KIT DE ILUMINACIÓN PARA CUADRO DE CONMUTACIÓN, sin tapas frontales","ZENERGY - W1000 KAPCSOLÓVILÁGÍTÁS KÉSZLET, előlapok nélkül"]
["32020","ZENERGY - OSŁONA CZOŁOWA PEŁNA W400, 2M / 250",41.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","32020","SZT","85389099","27.12.40.0",null,"5901988320201","OE - Couverture avant complète L400, 2M / 250","OE - Plain Front cover W400, 2M / 250","OE- TAPA CIEGA W400, 2M (H 100MM)","ZENERGY - TELJES ELSŐ BURKOLAT W400, 2M / 250"]
["32025","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W400, 2M / 250, 10 MOD",42.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","32025","SZT","85389099",null,null,"5901988320256","OE - Couverture d'appareil modulaire L400, 2M / 250, 10 mod","OE - Modular equipment cover W400, 2M / 250, 10 mod","OE-TAPA MODULAR W400, 2M (H 100MM) 10 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W400, 2M / 250, 10 MOD"]
["32031","ZENERGY - OSŁONA CZOŁOWA W400, 3M / 250, OTW. 92X92",44.7,"1-ZE-01",1.6666666666666666E-2,1,"OE_EQUIPMENT_COVERS","32031","SZT","85389099","27.12.40.0",null,"5901988320317","OE - Cache avant complet L400, 3M / 250, ouvert 92x92","OE - W400, 3M / 250 Front cover, hole 92x92","OE- TAPA CIEGA W400, 3M (H 150MM) CON AGUJERO 92X92","ZENERGY - ELSŐ BURKOLAT W400, 3M / 250, NYITOTT. 92X92"]
["32038","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W400, 3M / 250",52.9,"1-ZE-01",null,null,"01_PERFORATED_COVERS","32038","SZT","85389099","27.12.40.0",null,"5901988320386","OE - Couvercle avant perforé L400, 3M / 250","OE - Perforated Front cover W400, 3M / 250","OE- TAPA FRONTAL VENTILADA W400, 3M (H 150MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W400, 3M / 250"]
["32042","ZENERGY - OSŁONA CZOŁOWA WGŁĘBIONA, W400, 4M / 250",166.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","32042","SZT","85389099",null,null,"5901988320423","OE - Ecran facial encastré, L400, 4M / 250","OE - Recessed front hood, W400, 4M / 250","OE- TAPA FRONTAL EMPOTRADA W400, 4M / 250","ZENERGY - süllyesztett ELSŐ BURKOLAT, W400, 4M / 250"]
["32048","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W400, 4M / 250",57.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS","32048","SZT","85389099","27.12.40.0",null,"5901988320485","OE - Couvercle avant perforé L400, 4M / 250","OE - Perforated Front cover W400, 4M / 250","OE- TAPA FRONTAL VENTILADA W400, 4M (H 200MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W400, 4M / 250"]
["32055","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W400, 5M / 250, 10 MOD",56.3,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","32055","SZT","85389099","27.12.40.0",null,"5901988320553","OE - Couverture d'appareil modulaire L400, 5M / 250, 10 mod","OE - Modular equipment cover W400, 5M / 250, 10 mod","OE-TAPA MODULAR W400, 5M (H 250MM) 10 MOD","ZENERGY - W400 MODULÁRUS BERENDEZÉSBURKOLAT, 5M / 250, 10 MOD"]
["32056","ZENERGY - OSŁONA APARATURY MODUŁOWEJ, OTWÓR PRZESUNIĘTY W400, 5M / 250, 10 MOD",56.3,"1-ZE-01",0.1,1,"02_DIN_RAIL_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988320560","OE - Couvercle modulaire, trou décalé L400, 5M / 250, 10 mod.","OE - Modular equipment cover, offset hole W400, 5M / 250, 10 mod","OE- TAPA MODULAR , agujero DESPLAZADO W400, 5M / 250, 10 mod","ZENERGY - MODULÁRUS BERENDEZÉS BURKOLAT, OFFSET HOLE W400, 5M / 250, 10 MOD"]
["32060","ZENERGY - OSŁONA CZOŁOWA PEŁNA W400, 6M / 250",52.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","32060","SZT","85389099","27.12.40.0",null,"5901988320607","OE - Couverture avant complète L400, 6M / 250","OE - Plain Front cover W400, 6M / 250","OE- TAPA CIEGA W400, 6M (H 300MM)","ZENERGY - TELJES ELSŐ BURKOLAT W400, 6M / 250"]
["32070","ZENERGY - OSŁONA CZOŁOWA PEŁNA W400, 7M / 250",75.7,"1-ZE-01",null,null,"01_PLAIN_COVERS","32070","SZT","85389099","27.12.40.0",null,"5901988320706","OE - Couverture avant complète L400, 7M / 250","OE - Plain Front cover W400, 7M / 250","OE- TAPA CIEGA W400, 7M (H 350MM)","ZENERGY - TELJES ELSŐ BURKOLAT W400, 7M / 250"]
["32079","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W400, 9M / 250",210.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","32079","SZT","85389099",null,null,"5901988320799","OE - Couverture transparente L400, 9M / 250","OE - Transparent Front cover W400, 9M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 9M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W400, 9M / 250"]
["32091","ZENERGY - OSŁONA CZOŁOWA PEŁNA W400, 10M / 250",87.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","32091","SZT","85389099","27.12.40.0",null,"5901988320911","OE - Couverture avant complète L400, 10M / 250","OE - Plain Front cover W400, 10M / 250","OE- TAPA CIEGA W400, 10M (H 500MM)","ZENERGY - TELJES ELSŐ BURKOLAT W400, 10M / 250"]
["32099","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W400, 12M / 250",227.7,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","32099","SZT","85389099",null,null,"5901988320997","OE - Couverture transparente L400, 12M / 250","OE - Transparent Front cover W400, 12M / 250","OE- TAPA FRONTAL TRANSPARENTE W400, 12M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W400, 12M / 250"]
["32105","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W1000, 43 MOD, REGULOWANA, BEZ WSPORNIKÓW",70.3,"1-ZE-01",1.6666666666666666E-2,2,"OE_RAIL_DIN","32105","SZT","85389099","27.12.40.0",null,"5901988321055","OE - Rail d'équipement modulaire TS-35, L1000, 43 mod, réglable, sans supports","OE - Modular apparatus rail TS-35, W1000, 43 mod, adjustable, without supports","OE-CARRIL DIN W1000, 46 MOD.REG. PROF. + 2 SOPORT. 31040","ZENERGY - MODULÁRUS BERENDEZÉS SÍN TS-35, W1000, 43 MOD, ÁLLÍTHATÓ, KONZER NÉLKÜL"]
["32108","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, PROSTA, KORYTKO KABLOWE MONTOWANE Z PRZODU, W1000, 43 MOD, KOMPLETNA",50.8,"1-ZE-01",null,null,"OE_RAIL_DIN","32108","SZT","85389099","27.12.40.0",null,"5901988321086","OE - RAIL D'APPAREIL MODULAIRE TS-35, DROIT, CHEMIN DE CÂBLES MONTÉ À L'AVANT, L1000, 43 MOD, COMPLET","OE - TS-35 MODULAR RAIL, STRAIGHT, FRONT MOUNTED CABLE TRAY, W1000, 43 MOD, COMPLETE","OE- TS-35 CARRIL RECTO, MONTAJE FRONTAL, W1000, 43 MOD","ZENERGY - TS-35 MODULÁRUS BERENDEZÉS SÍN, EGYENES, ELŐRE FELSZERELT KÁBELTÁLCA, W1000, 43 MOD, TELJES"]
["32121","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W1200, 50 MOD, KOMPLETNA",62.6,null,8.3333333333333329E-2,4,"OE_RAIL_DIN",null,null,"",null,null,"5901988321215"]
["32128","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W1000, 2M / 850",72.7,"1-ZE-01",null,null,"01_PERFORATED_COVERS","32128","SZT","85389099",null,null,"5901988321284","OE - Panneau avant perforé L1000, 2M / 850","OE - Perforated Front cover W1000, 2M / 850","OE- TAPA FRONTAL VENTILADA W1000, 2M (H 100MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W1000, 2M / 850"]
["32139","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W1000, 3M / 850",256.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","32139","SZT","85389099",null,null,"5901988321390","OE - capot avant transparent L1000, 3M / 850","OE - Transparent Front cover W1000, 3M / 850","OE- TAPA FRONTAL TRANSPARENTE W1000, 3M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W1000, 3M / 850"]
["32148","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W1000, 4M / 850",97.8,"1-ZE-01",null,null,"01_PERFORATED_COVERS","32148","SZT","85389099",null,null,"5901988321482","OE - Panneau avant perforé L1000, 4M / 850","OE - Perforated Front cover W1000, 4M / 850","OE- TAPA FRONTAL VENTILADA W1000, 4M (H 200MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W1000, 4M / 850"]
["32160","ZENERGY - OSŁONA CZOŁOWA PEŁNA W1000, 6M / 850",96.5,"1-ZE-01",null,null,"01_PLAIN_COVERS","32160","SZT","85389099","27.12.40.0",null,"5901988321604","OE - Couverture avant complète L1000, 6M / 850","OE - Plain Front cover W1000, 6M / 850","OE- TAPA CIEGA W1000, 6M (H 300MM)","ZENERGY - TELJES ELSŐ BURKOLAT W1000, 6M / 850"]
["32180","ZENERGY - OSŁONA CZOŁOWA PEŁNA W1000, 8M / 850",144.1,"1-ZE-01",null,null,"01_PLAIN_COVERS","32180","SZT","85389099",null,null,"5901988321802","OE - Couverture avant complète L1000, 8M / 850","OE - Plain Front cover W1000, 8M / 850","OE- TAPA CIEGA W1000, 8M (H 400MM)","ZENERGY - TELJES ELSŐ BURKOLAT W1000, 8M / 850"]
["32192","ZENERGY - OSŁONA CZOŁOWA PEŁNA W1000, 11M / 850",163.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","32192","SZT","85389099",null,null,"5901988321925","OE - Couverture avant complète L1000, 11M / 850","OE - Full Front cover W1000, 11M / 850","OE- TAPA FRONTAL CIEGA W1000, 11M / 850","ZENERGY - TELJES ELSŐ BURKOLAT W1000, 11M / 850"]
["32193","ZENERGY - OSŁONA CZOŁOWA PEŁNA W1000, 12M / 850",173.8,"1-ZE-01",0.01,1,"01_PLAIN_COVERS","32193","SZT","85389099",null,null,"5901988321932","OE - Couverture avant complète L1000, 12M / 850","OE - Plain Front cover W1000, 12M / 850","OE- TAPA CIEGA W1000, 12M (H 600MM)","ZENERGY - TELJES ELSŐ BURKOLAT W1000, 12M / 850"]
["32202","Zenergy - Zaślepka modułowa RAL7035 jasny szary, długość 2000mm",49.3,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","32202","SZT","39269097",null,null,"5901988322021","OE - Fiche modulaire RAL7035 gris clair, longueur 2000mm","OE - Modular blanking strip RAL7035 light gray, length 2000mm","*OE - Obturador para tapa modular RAL7035 gris claro, longitud 2000mm","Zenergy - Moduláris dugó RAL7035 világosszürke, hossz 2000mm"]
["32411","ZENERGY - POKRYWA GÓRNA IP43, W650+400, D400, otwór na 1 wentylator",430.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988324117","OE - Capot supérieur IP43, L650 + 400, P400, ventilateur","OE - Top cover IP43, W650 + 400, D400, fan","OE- TECHO IP43, W650+400, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W650+400, D400, 1 ventilátor számára nyíló"]
["32418","ZENERGY - POKRYWA GÓRNA IP43, W850+300, D400, otwór na 1 wentylator",449.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988324186","OE - Capot supérieur IP43, L850 + 300, P400, ventilateur","OE - Top cover IP43, W850 + 300, D400, fan","OE- TECHO IP43, W850+300, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W850+300, D400, 1 ventilátor számára nyíló"]
["32427","ZENERGY - POKRYWA GÓRNA IP43, W150+850+300, D400, otwór na 1 wentylator",478.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988324278","OE - Capot supérieur IP43, L150 + 850 + 300, P400, ventilateur","OE - Top cover IP43, W150 + 850 + 300, D400, fan","OE- TECHO IP43, W150+850+300, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W150+850+300, D400, 1 ventilátor számára nyíló"]
["32432","ZENERGY - POKRYWA GÓRNA IP43, W200+650+300, D400, otwór na 1 wentylator",449.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988324322","OE - Capot supérieur IP43, L200 + 650 + 300, P400, ventilateur","OE - Top cover IP43, W200 + 650 + 300, D400, fan","OE- TECHO IP43, W200+650+300, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W200+650+300, D400, 1 ventilátor számára nyíló"]
["32445","ZENERGY - POKRYWA GÓRNA IP43, W450, D400, otwór na 1 wentylator",314.3,"1-ZE-01",null,null,"OE_COVERS","32445","SZT","85389099",null,"230829PW","5901988324452","OE - Capot supérieur IP43, L450, P400, ventilateur","OE - Top cover IP43, W450, D400, fan","OE- TECHO IP43, W450, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W450, D400, 1 ventilátor számára nyíló"]
["32466","ZENERGY - POKRYWA GÓRNA IP43, W450+200, D400, otwór na 1 wentylator",352.1,"1-ZE-01",null,null,"OE_COVERS","31465","SZT","85389099",null,null,"5901988324667","OE - Capot supérieur IP43, L450 + 200, P400, ventilateur","OE - Top cover IP43, W450 + 200, D400, fan","OE- TECHO IP43, W450+200, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W450+200, D400, 1 ventilátor számára nyíló"]
["32471","ZENERGY - POKRYWA GÓRNA IP43, W300+400, D400, otwór na 1 wentylator",361.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988324711","OE - Capot supérieur IP43, L300 + 400, P400, ventilateur","OE - Top cover IP43, W300 + 400, D400, fan","OE- TECHO IP43, W300+400, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W300+400, D400, 1 ventilátor számára nyíló"]
["32481","ZENERGY - POKRYWA GÓRNA IP43, W650+150, D400, otwór na 1 wentylator",382.3,"1-ZE-01",null,null,"OE_COVERS","32481","SZT","85389099",null,"230824PW","5901988324810","OE - Capot supérieur IP43, L650 + 150, P400, ventilateur","OE - Top cover IP43, W650 + 150, D400, fan","OE- TECHO IP43, W650+150, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W650+150, D400, 1 ventilátor számára nyíló"]
["32495","ZENERGY - POKRYWA GÓRNA IP43, W650+300, D400, otwór na 1 wentylator",411.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988324957","OE - Capot supérieur IP43, L650 + 300, P400, ventilateur","OE - Top cover IP43, W650 + 300, D400, fan","OE- TECHO IP43, W650+300, D400, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W650+300, D400, 1 ventilátor számára nyíló"]
["32502","ZENERGY OU - SZYNA APARATURY MODUŁOWEJ TS-35, W400, D180, 13 MOD, KOMPLETNA",27.1,"1-ZE-01",null,null,"OE_RAIL_DIN",null,"SZT","85389099",null,null,"5901988325022","OU - Rail d'équipement modulaire TS-35, L400, D180, 13 mod, complet","OU - Modular equipment rail TS-35, W400, D180, 13 mod, complete","OU- CARRIL DIN, W400, D180, 13 MOD, COMPLETO","ZENERGY OU - MODULÁRIS BERENDEZÉS SÍN TS-35, W400, D180, 13 MOD, TELJES"]
["32505","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W450, 13 MOD, REGULOWANA, BEZ WSPORNIKÓW",52.8,"1-ZE-01",null,null,"OE_RAIL_DIN","32505","SZT","85389099",null,null,"5901988325053","OE - Rail d'équipement modulaire TS-35, L450, 13 mod, réglable, sans supports","OE - Modular apparatus rail TS-35, W450, 13 mod, adjustable, without supports","OE-CARRIL DIN W450, 13 MOD.REG. PROF. + 2 SOPORT. 31040","ZENERGY - MODULÁRUS BERENDEZÉS SÍN TS-35, W450, 13 MOD, ÁLLÍTHATÓ, KONZER NÉLKÜL"]
["32510","ZENERGY - OSŁONA CZOŁOWA PEŁNA W450, 1M / 300",39.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","32510","SZT","85389099","27.12.40.0",null,"5901988325107","OE - Couverture avant complète L450, 1M / 300","OE - Plain Front cover W450, 1M / 300","OM-TAPA CIEGA W450, 1M (H 50MM)","ZENERGY - TELJES ELSŐ BURKOLAT W450, 1M / 300"]
["32528","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W450, 2M / 300",52.9,"1-ZE-01",null,null,"01_PERFORATED_COVERS","32528","SZT","85389099",null,null,"5901988325282","OE - Panneau avant perforé L450, 2M / 300","OE - Perforated Front cover W450, 2M / 300","OE- TAPA FRONTAL VENTILADA W450, 2M (H 100MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W450, 2M / 300"]
["32532","ZENERGY - OSŁONA CZOŁOWA WGŁĘBIONA, W450, 3M / 300",174.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","32532","SZT","85389099",null,null,"5901988325329","OE - Couvercle avant profond de, L450,  3M / 300","OE - Recessed front hood, W450, 3M / 300","OE- TAPA FRONTAL EMPOTRADA W450, 3M / 300","ZENERGY - süllyesztett ELSŐ BURKOLAT, W450, 3M / 300"]
["32535","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W450, 3M / 300, 13 MOD",43.9,"1-ZE-01",1.4416666666666667,5,"02_DIN_RAIL_COVERS","32535","SZT","85389099","27.12.40.0",null,"5901988325350","OE - Couverture d'appareil modulaire L450, 3M / 300, 13 mod","OE - Modular equipment cover W450, 3M / 300, 13 mod","OM-TAPA MODULAR W450, 3M (H 150MM) 13 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W450, 3M / 300, 13 MOD"]
["32540","ZENERGY - OSŁONA CZOŁOWA PEŁNA W450, 4M / 300",47.5,"1-ZE-01",0.55833333333333335,2,"01_PLAIN_COVERS","32540","SZT","85389099","27.12.40.0",null,"5901988325404","OE - Couverture avant complète L450, 4M / 300","OE - Plain Front cover W450, 4M / 300","OM-TAPA CIEGA W450, 4M (H 200MM)","ZENERGY - TELJES ELSŐ BURKOLAT W450, 4M / 300"]
["32546","ZENERGY - OSŁONA APARATURY MODUŁOWEJ, OTWÓR PRZESUNIĘTY W450, 4M / 300, 13 MOD",48.4,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988325466","OE - Couvercle d'appareil modulaire, trou décalé L450, 4M / 300, 13 modulaire","OE - Modular equipment cover, offset hole W450, 4M / 300, 13 mod","OE- TAPA MODULAR  agujero DESPLAZADO W450, 4M / 300, 13 mod","ZENERGY - MODULÁRUS BERENDEZÉS BURKOLAT, OFFSET HOLE W450, 4M / 300, 13 MOD"]
["32550","ZENERGY - OSŁONA CZOŁOWA PEŁNA W450, 5M / 300",52.9,"1-ZE-01",0.33333333333333331,2,"01_PLAIN_COVERS","32550","SZT","85389099","27.12.40.0",null,"5901988325503","OE - Couverture avant complète L450, 5M / 300","OE - Plain Front cover W450, 5M / 300","OM-TAPA CIEGA W450, 5M (H 250MM)","ZENERGY - TELJES ELSŐ BURKOLAT W450, 5M / 300"]
["32555","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W450, 5M / 300, 13 MOD",59.4,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","32555","SZT","85389099","27.12.40.0",null,"5901988325558","OE - Couverture d'appareil modulaire L450, 5M / 300, 13 mod","OE - Modular equipment cover W450, 5M / 300, 13 mod","OM-TAPA MODULAR W450, 5M (H 250MM) 13 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W450, 5M / 300, 13 MOD"]
["32560","ZENERGY - OSŁONA CZOŁOWA PEŁNA W450, 6M / 300",54.9,"1-ZE-01",1.3,6,"01_PLAIN_COVERS","32560","SZT","85389099","27.12.40.0",null,"5901988325602","OE - Couverture avant complète L450, 6M / 300","OE - Plain Front cover W450, 6M / 300","OM-TAPA CIEGA W450, 6M (H 300MM)","ZENERGY - TELJES ELSŐ BURKOLAT W450, 6M / 300"]
["32568","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W450, 6M / 300",67.8,"1-ZE-01",0.15833333333333333,5,"01_PERFORATED_COVERS","32568","SZT","85389099",null,null,"5901988325688","OE - Panneau avant perforé L450, 6M / 300","OE - Perforated Front cover W450, 6M / 300","OE- TAPA FRONTAL VENTILADA W450, 6M (H 300MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W450, 6M / 300"]
["32569","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W450, 8M / 300",215.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","32569","SZT","85389099",null,null,"5901988325695","OE - Couverture, L450, 8M / 300","OE - Transparent Front cover W450, 8M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 8M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W450, 8M / 300"]
["32590","ZENERGY - OSŁONA CZOŁOWA PEŁNA W450, 9M / 300",89,"1-ZE-01",0.3,2,"01_PLAIN_COVERS","32590","SZT","85389099","27.12.40.0",null,"5901988325909","OE - Couverture avant complète L450, 9M / 300","OE - Plain Front cover W450, 9M / 300","OM-TAPA CIEGA W450, 9M (H 450MM)","ZENERGY - TELJES ELSŐ BURKOLAT W450, 9M / 300"]
["32591","ZENERGY - OSŁONA CZOŁOWA PEŁNA W450, 10M / 300",90.9,"1-ZE-01",0.1,1,"01_PLAIN_COVERS","32591","SZT","85389099","27.12.40.0",null,"5901988325916","OE - Couverture avant complète L450, 10M / 300","OE - Plain Front cover W450, 10M / 300","OM-TAPA CIEGA W450, 10M (H 500MM)","ZENERGY - TELJES ELSŐ BURKOLAT W450, 10M / 300"]
["32596","ZENERGY OM-VSD - OSŁONA APARATURY MODUŁOWEJ, UKŁAD PIONOWY W450, 10M / 300, 1X26 MOD",120.8,"1-ZE-01",null,null,"OM_VSD_PLATES","32596","SZT","85389099",null,null,"5901988325961","OM-VSD - Couvercle modulaire pour appareils, vertical L450, 10M / 300, 1x26 modulaire","OM-VSD - Modular apparatus cover, Vertical layout W450, 10M / 300, 1x26 mod","OM-VSD- TAPA MODULAR VERTIC. W450, 10M / 300, 1X26 MOD","ZENERGY OM-VSD - MODULÁRIS BERENDEZÉSBURKOLAT, FÜGGŐLEGES W450, 10M / 300, 1X26 MOD"]
["32599","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W450, 12M / 300",241.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","32599","SZT","85389099",null,null,"5901988325992","OE - Couvercle avant, transparent L450, 12M / 300","OE - Transparent Front cover W450, 12M / 300","OE- TAPA FRONTAL TRANSPARENTE W450, 12M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W450, 12M / 300"]
["32611","ZENERGY - POKRYWA GÓRNA IP43, W650+400, D600, otwór na 1 wentylator",472,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988326111","OE - Capot supérieur IP43, L650 + 400, P600, ventilateur","OE - Top cover IP43, W650 + 400, D600, fan","OE- TECHO IP43, W650+400, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W650+400, D600, 1 ventilátor számára nyíló"]
["32618","ZENERGY - POKRYWA GÓRNA IP43, W850+300, D600, otwór na 1 wentylator",493.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988326180","OE - Capot supérieur IP43, L850 + 300, P600, ventilateur","OE - Top cover IP43, W850 + 300, D600, fan","OE- TECHO IP43, W850+300, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W850+300, D600, 1 ventilátor számára nyíló"]
["32621","ZENERGY - POKRYWA GÓRNA IP43, W150+650+400, D600, otwór na 1 wentylator",504.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988326210","OE - Capot supérieur IP43, L150 + 650 + 400, P600, ventilateur","OE - Top cover IP43, W150 + 650 + 400, D600, fan","OE- TECHO IP43, W150+650+400, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W150+650+400, D600, 1 ventilátor számára nyíló"]
["32622","ZENERGY - POKRYWA GÓRNA IP43, W150+650+300, D600, otwór na 1 wentylator",481.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988326227","OE - Capot supérieur IP43, L150 + 650 + 300, P600, ventilateur","OE - Top cover IP43, W150 + 650 + 300, D600, fan","OE- TECHO IP43, W150+650+300, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W150+650+300, D600, 1 ventilátor számára nyíló"]
["32630","ZENERGY - POKRYWA GÓRNA IP43, W300, D600, otwór na 1 wentylator",304.60000000000002,"1-ZE-01",null,null,"OE_COVERS","31630","SZT","85389099",null,null,"5901988326302","OE - Capot supérieur IP43, L300, P600, ventilateur","OE - Top cover IP43, W300, D600, fan","OE- TECHO IP43, W300, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W300, D600, 1 ventilátor számára nyíló"]
["32640","ZENERGY - POKRYWA GÓRNA IP43, W400, D600, otwór na 1 wentylator",327.2,"1-ZE-01",null,null,"OE_COVERS","32640","SZT","85389099",null,"230831PW","5901988326401","OE - Capot supérieur IP43, L400, P600, ventilateur","OE - Top cover IP43, W400, D600, fan","OE- TECHO IP43, W400, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W400, D600, 1 ventilátor számára nyíló"]
["32666","ZENERGY - POKRYWA GÓRNA IP43, W450+200, D600, otwór na 1 wentylator",382.3,"1-ZE-01",null,null,"OE_COVERS","31665","SZT","85389099",null,null,"5901988326661","OE - Capot supérieur IP43, L450 + 200, P600, ventilateur","OE - Top cover IP43, W450 + 200, D600, fan","OE- TECHO IP43, W450+200, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W450+200, D600, 1 ventilátor számára nyíló"]
["32680","ZENERGY - POKRYWA GÓRNA IP43, W800, D600, otwór na 1 wentylator",414.7,"1-ZE-01",null,null,"OE_COVERS","32680","SZT","85389099",null,"230830PW","5901988326807","OE - Capot supérieur IP43, L800, P600, ventilateur","OE - Top cover IP43, W800, D600, fan","OE- TECHO IP43, W800, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W800, D600, 1 ventilátor számára nyíló"]
["32686","ZENERGY - POKRYWA GÓRNA IP43, W650+200, D600, otwór na 1 wentylator",426.6,"1-ZE-01",null,null,"OE_COVERS","32686","SZT","85389099",null,"230829PW","5901988326869","OE - Capot supérieur IP43, L650 + 200, P600, ventilateur","OE - Top cover IP43, W650 + 200, D600, fan","OE- TECHO IP43, W650+200, D600, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W650+200, D600, 1 ventilátor számára nyíló"]
["32701","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, PROSTA, KORYTKO KABLOWE MONTOWANE Z TYŁU, W650, 24 MOD, KOMPLETNA",42.4,"1-ZE-01",0.01,1,"OE_RAIL_DIN","32701","SZT","85389099","27.12.40.0",null,"5901988327019","OE - Rail d'appareil modulaire TS-35, droit, chemin de câbles monté à l'arrière, L650, 24 mod, complet","OE - TS-35 modular equipment rail, straight, rear mounted cable tray, W650, 24 mod, complete","OE- CARRIL DIN FIJO, RECTO, MONT. CANALETA DETAS, W650, 24 MOD.","ZENERGY - TS-35 MODULÁRUS BERENDEZÉS SÍN, EGYENES, HÁTSÓ SZERELT KÁBELTÁLCA, W650, 24 MOD, TELJES"]
["32704","ZENERGY OU - SZYNA APARATURY MODUŁOWEJ TS-35, W600, D250, 24 MOD, KOMPLETNA",33.700000000000003,"1-ZE-01",null,null,"OE_RAIL_DIN",null,"SZT","85389099","27.12.40.0",null,"5901988327040","OU - Rail d'équipement modulaire TS-35, L600, D250, 24 mod, complet","OU - Modular equipment rail TS-35, W600, D250, 24 mod, complete","OU- CARRIL DIN, W600, D250, 24 MOD, COMPLETO","ZENERGY OU - MODULÁRIS BERENDEZÉS SÍN TS-35, W600, D250, 24 MOD, TELJES"]
["32705","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W650, 24 MOD, REGULOWANA, BEZ WSPORNIKÓW",59.2,"1-ZE-01",null,null,"OE_RAIL_DIN","32705","SZT","85389099","27.12.40.0",null,"5901988327057","OE - Rail d'appareil modulaire TS-35, L650, 24 mod, réglable, sans crochets","OE - Modular apparatus rail TS-35, W650, 24 mod, adjustable, without brackets","OE-CARRIL DIN, W650, 24 MOD. REGUL. PROF.  SIN SOPORT.","ZENERGY - MODULÁRUS BERENDEZÉS SÍN TS-35, W650, 24 MOD, ÁLLÍTHATÓ, KONZER NÉLKÜL"]
["32708","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, PROSTA, KORYTKO KABLOWE MONTOWANE Z PRZODU, W650, 24 MOD, KOMPLETNA",42.4,"1-ZE-01",null,null,"OE_RAIL_DIN","32708","SZT","85389099","27.12.40.0",null,"5901988327088","OE - RAIL D'APPAREIL MODULAIRE TS-35, DROIT, CHEMIN DE CÂBLES MONTÉ À L'AVANT, L650, 24 MOD, COMPLET","OE - TS-35 MODULAR RAIL, STRAIGHT, FRONT MOUNTED CABLE TRAY, W650, 24 MOD, COMPLETE","OE- TS-35 CARRIL RECTO, CABLES DE MONTAJE FRONTAL, W650, 24 MOD","ZENERGY - TS-35 MODULÁRUS BERENDEZÉS SÍN, EGYENES, ELŐRE FELSZERELT KÁBELTÁLCA, W650, 24 MOD, TELJES"]
["32712","IT - OSŁONA CZOŁOWA PERFOROWANA RACK 1U",50.6,null,0.5,2,"01_PERFORATED_COVERS","32712",null,null,null,"240130PW",null,null,null,null,"IT - PERFORÁLT ELSŐ BURKOLAT 1U"]
["32716","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W650, 11M / 500",137.5,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988327163","OE - CACHE AVANT PERFORÉ L650, 11M / 500","OE - Perforated Front cover W650, 11M / 500","*OE - TAPA DELANTERA PERFORADA W650, 11M / 500","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W650, 11M / 500"]
["32720","ZENERGY - OSŁONA CZOŁOWA PEŁNA W650, 2M / 500",40.4,"1-ZE-01",1.8,2,"01_PLAIN_COVERS","32720","SZT","85389099","27.12.40.0",null,"5901988327200","OE - Couverture avant complète L650, 2M / 500","OE - Plain Front cover W650, 2M / 500","OE- TAPA CIEGA W650, 2M (H 100MM) ","ZENERGY - TELJES ELSŐ BURKOLAT W650, 2M / 500"]
["32730","ZENERGY - OSŁONA CZOŁOWA PEŁNA W650, 3M / 500",40.799999999999997,"1-ZE-01",12.9,6,"01_PLAIN_COVERS","32730","SZT","85389099","27.12.40.0",null,"5901988327309","OE - Couverture avant complète L650, 3M / 500","OE - Plain Front cover W650, 3M / 500","OE- TAPA CIEGA W650, 3M (H 150MM) ","ZENERGY - TELJES ELSŐ BURKOLAT W650, 3M / 500"]
["32733","ZENERGY IT - OSŁONA CZOŁOWA RACK 3U",44.4,"1-ZE-01",0.11666666666666667,4,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988327330","IT - Couvercle avant L650, 3U / 500","IT - W650, 3U / 500 Front cover","OE IT- TAPA TROQ. W650, 3U / 500","ZENERGY IT - ELSŐ BURKOLAT 3U"]
["32736","ZENERGY - OSŁONA APARATURY MODUŁOWEJ, OTWÓR PRZESUNIĘTY W650, 3.5M / 500, 24 MOD",52.6,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","32736","SZT","85389099","27.12.40.0",null,"5901988327361","OE - Couverture d'appareil modulaire L650, 3.5M / 500, 24 mod","OE - Modular apparatus cover, offset hole W650, 3.5M / 500, 24 mod","OE- TAPA MODULAR ORIFICIO DESPLAZADO W650, 3.5M / 500, 24 MOD","ZENERGY - MODULÁRUS BERENDEZÉS BURKOLAT, OFFSET HOLE W650, 3,5M / 500, 24 MOD"]
["32738","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W650, 3M / 500",65.599999999999994,"1-ZE-01",0.95833333333333337,1,"01_PERFORATED_COVERS","32738","SZT","8538909900","27.12.40.0",null,"5901988327385","OE - Panneau avant perforé L650, 3M / 500","OE - Perforated Front cover W650, 3M / 500","OE- TAPA FRONTAL VENTILADA W650, 3M (H 150MM) ","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W650,3M/500"]
["32741","ZENERGY - OSŁONA CZOŁOWA W650, 4M / 500, OTW. 92X92",64.8,"1-ZE-01",3.3333333333333333E-2,1,"OE_EQUIPMENT_COVERS","32741","SZT","85389099","27.12.40.0",null,"5901988327415","OE - Cache avant complet L650, 4M / 500, ouvert 92x92","OE - W650, 4M / 500 Front cover, open. 92x92","OE- TAPA CIEGA W650, 4M (H 200MM) CON AGUJERO 92X92","ZENERGY - ELSŐ BURKOLAT W650, 4M / 500, NYITOTT. 92X92"]
["32744","ZENERGY IT - OSŁONA CZOŁOWA W650, 4U / 500, MOD",72.099999999999994,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988327446","IT - Couvercle avant L650, 4U / 500, mod","IT - Front cover W650, 4U / 500, mod","OE IT- TAPA TROQ. W650, 4U / 500, MOD","ZENERGY IT - ELSŐ BURKOLAT W650, 4U / 500, MOD"]
["32748","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W650, 4M / 500",74.099999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","32748","SZT","85389099","27.12.40.0",null,"5901988327484","OE - Panneau avant perforé L650, 4M / 500","OE - Perforated Front cover W650, 4M / 500","OE- TAPA FRONTAL VENTILADA W650, 4M (H 200MM) ","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W650, 4M / 500"]
["32751","ZENERGY - OSŁONA CZOŁOWA W650, 5M / 500, OTW. 92X92",76.7,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","32751","SZT","85389099",null,null,"5901988327514","OE - Cache avant complet L650, 5M / 500, ouvert 92x92","OE - Front cover W650, 5M / 500, open. 92x92","OE- TAPA CIEGA W650, 5M (H 250MM) CON AGUJERO 92X92","ZENERGY - ELSŐ BURKOLAT W650, 5M / 500, NYITOTT. 92X92"]
["32755","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W650, 5M / 500, 24 MOD",68.7,"1-ZE-01",0.5,2,"02_DIN_RAIL_COVERS","32755","SZT","85389099","27.12.40.0",null,"5901988327552","OE - Couverture d'appareil modulaire L650, 5M / 500, 24 mod","OE - Modular equipment cover W650, 5M / 500, 24 mod","OE- TAPA MODULAR W650, 5M (H 250MM) 24 MOD","ZENERGY - W650 MODULÁRIS BERENDEZÉSBURKOLAT, 5M / 500, 24 MOD"]
["32758","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W650, 5M / 500",80.400000000000006,"1-ZE-01",0.24166666666666667,1,"01_PERFORATED_COVERS","32758","SZT","85389099","27.12.40.0",null,"5901988327583","OE - Panneau avant perforé L650, 5M / 500","OE - Perforated Front cover W650, 5M / 500","OE- TAPA FRONTAL VENTILADA W650, 5M (H 250MM) ","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W650, 5M / 500"]
["32761","ZENERGY - OSŁONA CZOŁOWA SIRCO1250 3P, W650, 6M / 500",82.3,"1-ZE-01",5.8333333333333334E-2,1,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988327613","OE - SIRCO1250 3P, L650, 6M / 500 protection avant","OE - Front cover SIRCO1250 3P, W650, 6M / 500","OE- TAPA TROQ.SIRCO1250 3P, W650, 6M/500","ZENERGY - ELSŐ BURKOLAT SIRCO1250 3P, W650, 6M / 500"]
["32762","ZENERGY - OSŁONA CZOŁOWA WGŁĘBIONA, W650, 6M / 500",217.8,"1-ZE-01",0.01,1,"01_PLAIN_COVERS","32762","SZT","85389099",null,null,"5901988327620","OE - Ecran facial encastré, L650, 6M / 500","OE - Recessed Front cover, W650, 6M / 500","OE- TAPA FRONTAL EMPOTRADA W650, 6M / 500","ZENERGY - SÜLYÉTETT ELSŐ BURKOLAT, W650, 6M / 500"]
["32765","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W650, 6M / 500, 24 MOD",88.6,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988327651","OE - COUVERCLE MODULAIRE L650, 6M / 500, 24 MOD","OE - Modular cover W650, 6M / 500, 24 MOD","*OE - CUBIERTA MODULAR W650, 6M / 500, 24 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W650, 6M / 500, 24 MOD"]
["32768","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W650, 6M / 500",84.5,"1-ZE-01",0.35833333333333334,1,"01_PERFORATED_COVERS","32768","SZT","85389099","27.12.40.0",null,"5901988327682","OE - Panneau avant perforé L650, 6M / 500","OE - Perforated Front cover W650, 6M / 500","OE- TAPA FRONTAL VENTILADA W650, 6M (H 300MM) ","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W650, 6M / 500"]
["32773","ZENERGY - OSŁONA CZOŁOWA SOCOMEC D20, W650, 4M / 500",60.6,"1-ZE-01",null,null,"01_PLAIN_COVERS","32773","SZT","85389099",null,null,"5901988327736",0,0,0,"ZENERGY - ELSŐ BURKOLAT SOCOMEC D20, W650, 4M / 500"]
["32777","OE - Osłona czołowa ATL800, W650, 6M / 500, otw. 220x160",88.6,null,null,null,"OE_EQUIPMENT_COVERS","32777",null,null,null,"240228PW",null,"OE - Couverture avant ATL800, W650, 6M / 500, ouverture 220x160","OE - Front cover ATL800, W650, 6M / 500, opening 220x160","OE - Tapa frontal ATL800, W650, 6M / 500, apertura 220x160","OE - Első burkolat ATL800, W650, 6M / 500, nyitható 220x160"]
["32781","ZENERGY - OSŁONA CZOŁOWA SIRCO1600 3P, W650, 10M / 500",121,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988327811","OE - CAPOT AVANT SIRCO1600 3P, L650, 10M / 500","OE - Front cover SIRCO1600 3P, W650, 10M / 500","*OE - TAPA DELANTERA SIRCO1600 3P, W650, 10M / 500","ZENERGY - ELSŐ BURKOLAT SIRCO1600 3P, W650, 10M / 500"]
["32784","ZENERGY IT - OSŁONA CZOŁOWA RACK 10U",92.4,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988327842","IT - CACHE AVANT RACK 9U","IT - Front cover RACK 9U","*IT - TAPA FRONTAL RACK 9U","ZENERGY IT - ELSŐ BURKOLAT 10U"]
["32788","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W650, 8M / 500",117.7,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988327880","OE - CACHE AVANT PERFORÉ L650, 8M / 500","OE - Perforated Front cover W650, 8M / 500","*OE - TAPA DELANTERA PERFORADA W650, 8M / 500","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W650, 8M / 500"]
["32789","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W650, 10M / 500",288.7,"1-ZE-01",0.01,1,"01_TRANSPARENT_COVERS","32789","SZT","85389099","27.12.40.0",null,"5901988327897","OE - Couverture, L650, 10M / 500","OE - Transparent Front cover W650, 10M / 500","OE- TAPA FRONTAL TRANSPARENTE W650, 10M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W650, 10M / 500"]
["32792","ZENERGY - OSŁONA CZOŁOWA PEŁNA W650, 11M / 500",123.2,"1-ZE-01",null,null,"01_PLAIN_COVERS","32792","SZT","85389099","27.12.40.0",null,"5901988327927","OE - Couverture avant complète L650, 11M / 500","OE - Plain Front cover W650, 11M / 500","OE- TAPA CIEGA W650, 11M (H 550MM) ","ZENERGY - TELJES ELSŐ BURKOLAT W650, 11M / 500"]
["32795","ZENERGY OM-VSD - OSŁONA APARATURY MODUŁOWEJ, UKŁAD PIONOWY W650, 9M / 500, 2X24 MOD",144.9,"1-ZE-01",null,null,"OM_VSD_PLATES","32795","SZT","85389099",null,null,"5901988327958","OM-VSD - Couvercle modulaire pour appareils, vertical L650, 9M / 500, modulaire 2x24","OM-VSD - Modular equipment cover, Vertical layout W650, 9M / 500, 2x24 mod","OM-VSD- TAPA MODULAR VERTIC. W650, 9M/500, 2X24 MOD","ZENERGY OM-VSD - MODULÁRIS BERENDEZÉSBURKOLAT, FÜGGŐLEGES W650, 9M / 500, 2X24 MOD"]
["32800","Zenergy - Szyna aparatury modułowej TS-35, W800, 32 mod, kompletna",49.3,"1-ZE-01",0.35833333333333334,2,"OE_RAIL_DIN",null,null,"85389099",null,null,"5901988328009"]
["32809","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W850, 35 MOD, MONTAŻ DO RAMY OSŁON CZOŁOWYCH",68.099999999999994,null,null,null,"OE_RAIL_DIN",null,null,"85389099",null,null,"5901988328092"]
["32813","ZENERGY - POKRYWA GÓRNA IP43, W1300, D800, otwór na 1 wentylator",620.4,"1-ZE-01",null,null,"OE_COVERS","31813","SZT","85389099",null,null,"5901988328139","OE - Capot supérieur IP43, L1300, P800, ventilateur","OE - Top cover IP43, W1300, D800, fan","OE- TECHO IP43, W1300, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W1300, D800, 1 ventilátor számára nyíló"]
["32819","ZENERGY - POKRYWA GÓRNA IP43, W850+400, D800, otwór na 1 wentylator",607.20000000000005,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988328191","OE - Capot supérieur IP43, L850 + 400, P800, ventilateur","OE - Top cover IP43, W850 + 400, D800, fan","OE- TECHO IP43, W850+400, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W850+400, D800, 1 ventilátor számára nyíló"]
["32822","ZENERGY - POKRYWA GÓRNA IP43, W150+650+300, D800, otwór na 1 wentylator",564.29999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988328221","OE - Capot supérieur IP43, L150 + 650 + 300, P800, ventilateur","OE - Top cover IP43, W150 + 650 + 300, D800, fan","OE- TECHO IP43, W150+650+300, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W150+650+300, D800, 1 ventilátor számára nyíló"]
["32827","ZENERGY - POKRYWA GÓRNA IP43, W150+850+300, D800, otwór na 1 wentylator",620.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988328276","OE - Capot supérieur IP43, L150 + 850 + 300, P800, ventilateur","OE - Top cover IP43, W150 + 850 + 300, D800, fan","OE- TECHO IP43, W150+850+300, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W150+850+300, D800, 1 ventilátor számára nyíló"]
["32832","ZENERGY - POKRYWA GÓRNA IP43, W200+650+300, D800, otwór na 1 wentylator",578.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988328320","OE - Capot supérieur IP43, L200 + 650 + 300, P800, ventilateur","OE - Top cover IP43, W200 + 650 + 300, D800, fan","OE- TECHO IP43, W200+650+300, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W200+650+300, D800, 1 ventilátor számára nyíló"]
["32860","ZENERGY - POKRYWA GÓRNA IP43, W600, D800, otwór na 1 wentylator",422.4,"1-ZE-01",null,null,"OE_COVERS","32860","SZT","85389099",null,"230830PW","5901988328603","OE - Capot supérieur IP43, L600, P800, ventilateur","OE - Top cover IP43, W600, D800, fan","OE- TECHO IP43, W600, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W600, D800, 1 ventilátor számára nyíló"]
["32871","ZENERGY - POKRYWA GÓRNA IP43, W300+400, D800, otwór na 1 wentylator",452.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988328719","OE - Capot supérieur IP43, L300 + 400, P800, ventilateur","OE - Top cover IP43, W300 + 400, D800, fan","OE- TECHO IP43, W300+400, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W300+400, D800, 1 ventilátor számára nyíló"]
["32881","ZENERGY - POKRYWA GÓRNA IP43, W650+150, D800, otwór na 1 wentylator",479.6,"1-ZE-01",null,null,"OE_COVERS","32881","SZT","85389099",null,"230829PW","5901988328818","OE - Capot supérieur IP43, L650 + 150, P800, ventilateur","OE - Top cover IP43, W650 + 150, D800, fan","OE- TECHO IP43, W650+150, D800, ADMIRADOR","ZENERGY - FELSŐ BURKOLAT IP43, W650+150, D800, 1 ventilátor számára nyíló"]
["32893","ZENERGY IT - OSŁONA CZOŁOWA RACK 9U, wgłębiona, licznikowa 2TL",99.4,"1-ZE-01",0.15833333333333333,1,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY IT - ELSŐ BURKOLAT 9U, süllyesztett, pult 2TL"]
["32901","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, PROSTA, KORYTKO KABLOWE MONTOWANE Z TYŁU, W850, 35 MOD, KOMPLETNA",48.6,"1-ZE-01",null,null,"OE_RAIL_DIN","32901","SZT","85389099","27.12.40.0",null,"5901988329013","OE - Rail d'appareil modulaire TS-35, droit, chemin de câbles monté à l'arrière, L850, 35 mod, complet","OE - TS-35 modular equipment rail, straight, rear mounted cable tray, W850, 35 mod, complete","OE- CARRIL DIN FIJO, RECTO, MONT. CANALETA DETAS, W850, 35 MOD.","ZENERGY - TS-35 MODULÁRUS BERENDEZÉS SÍN, EGYENES, HÁTSÓ SZERELT KÁBELTÁLCA, W850, 35 MOD, TELJES"]
["32902","ZENERGY OU - SZYNA APARATURY MODUŁOWEJ TS-35, W800, D180, 35 MOD, KOMPLETNA",35.5,"1-ZE-01",null,null,"OE_RAIL_DIN",null,"SZT","85389099","27.12.40.0",null,"5901988329020","OU - Rail d'équipement modulaire TS-35, L800, D180, 35 mod, complet","OU - Modular equipment rail TS-35, W800, D180, 35 mod, complete","OU- CARRIL DIN, W800, D180, 35 MOD, COMPLETO","ZENERGY OU - MODULÁRIS BERENDEZÉS SÍN TS-35, W800, D180, 35 MOD, TELJES"]
["32905","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, W850, 35 MOD, REGULOWANA, BEZ WSPORNIKÓW",68.099999999999994,"1-ZE-01",null,null,"OE_RAIL_DIN","32905","SZT","85389099","27.12.40.0",null,"5901988329051","OE - Rail d'équipement modulaire TS-35, L850, 35 mod, réglable, sans supports","OE - Modular apparatus rail TS-35, W850, 35 mod, adjustable, without brackets","OE- CARRIL DIN, W850, 35 MOD. REGUL. PROF.  SIN SOPORT.","ZENERGY - MODULÁRUS BERENDEZÉS SÍN TS-35, W850, 35 MOD, ÁLLÍTHATÓ, KONZER NÉLKÜL"]
["32908","ZENERGY - SZYNA APARATURY MODUŁOWEJ TS-35, PROSTA, KORYTKO KABLOWE MONTOWANE Z PRZODU, W850, 35 MOD, KOMPLETNA",48.6,"1-ZE-01",null,null,"OE_RAIL_DIN","32908","SZT","85389099","27.12.40.0",null,"5901988329082","OE - RAIL POUR APPAREILS MODULAIRES TS-35, DROIT, CHEMIN DE CÂBLES MONTÉ À L'AVANT, L850, 35 MOD, COMPLET","OE - TS-35 MODULAR RAIL, STRAIGHT, FRONT MOUNTED CABLE TRAY, W850, 35 MOD, COMPLETE","OE- TS-35 CARRIL RECTO, MONTAJE FRONTAL, W850, 35 MOD","ZENERGY - TS-35 MODULÁRUS BERENDEZÉS SÍN, EGYENES, ELŐRE FELSZERELT KÁBELTÁLCA, W850, 35 MOD, TELJES"]
["32914","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W850, 9M / 700",144.1,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988329143","OE - CACHE AVANT PERFORÉ L850, 9M / 700","OE - Perforated Front cover W850, 9M / 700","*OE - TAPA DELANTERA PERFORADA W850, 9M / 700","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W850, 9M / 700"]
["32917","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W850, 12M / 700",167.2,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988329174","OE - CACHE AVANT PERFORÉ L850, 12M / 700","OE - Perforated Front cover W850, 12M / 700","*OE - TAPA DELANTERA PERFORADA W850, 12M / 700","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W850, 12M / 700"]
["32925","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W850, 2M / 700, 35 MOD",55.9,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","32925","SZT","85389099","27.12.40.0",null,"5901988329259","OE - Couverture d'appareil modulaire L850, 2M / 700, 35 mod","OE - Modular equipment cover W850, 2M / 700, 35 mod","OE- TAPA MODULAR W850, 2M (H 100MM) 35 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W850, 2M / 700, 35 MOD"]
["32932","ZENERGY - OSŁONA CZOŁOWA WGŁĘBIONA, W850, 3M / 700",220,"1-ZE-01",null,null,"01_PLAIN_COVERS","32932","SZT","85389099",null,null,"5901988329327","OE - Couvercle avant profond de, L850,  3M / 700","OE - Recessed front hood, W850, 3M / 700","OE- TAPA FRONTAL EMPOTRADA W850, 3M / 700","ZENERGY - SÜLYÉTETT ELSŐ BURKOLAT, W850, 3M / 700"]
["32935","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W850, 3M / 700, 35 MOD",63.6,"1-ZE-01",10.9,4,"02_DIN_RAIL_COVERS","32935","SZT","85389099","27.12.40.0",null,"5901988329358","OE - Couverture d'appareil modulaire L850, 3M / 700, 35 mod","OE - Modular equipment cover W850, 3M / 700, 35 mod","OE- TAPA MODULAR W850, 3M (H 150MM) 35 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W850, 3M / 700, 35 MOD"]
["32941","ZENERGY - OSŁONA CZOŁOWA W850, 4M / 700, OTW. 92X92",71.5,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","32941","SZT","85381000","27.12.40.0",null,"5901988329419","OE - Protection frontale L850, 4M / 700, ouverte 92x92","OE - W850, 4M / 700 Front cover, hole 92x92","OE/OM - TAPA CIEGA W850 4M (H 200MM) CON AGUJERO 92X92","ZENERGY - ELSŐ BURKOLAT W850, 4M / 700, NYITVA. 92X92"]
["32946","ZENERGY - OSŁONA APARATURY MODUŁOWEJ, OTWÓR PRZESUNIĘTY W850, 4M / 700, 35 MOD",71.3,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988329464","OE - Couvercle d'appareil modulaire, trou décalé L850, 4M / 700, 35 mod","OE - Modular equipment cover, offset hole W850, 4M / 700, 35 mod","OE- TAPA MODULAR  AGUJERO desplazado W850, 4M / 700, 35 mod","ZENERGY - MODULÁRUS BERENDEZÉS BURKOLAT, OFFSET HOLE W850, 4M / 700, 35 MOD"]
["32950","ZENERGY - OSŁONA CZOŁOWA PEŁNA W850, 5M / 700",77.7,"1-ZE-01",0.6333333333333333,4,"01_PLAIN_COVERS","32950","SZT","85389099","27.12.40.0",null,"5901988329501","OE - Couverture avant complète L850, 5M / 700","OE - Plain Front cover W850, 5M / 700","OE- TAPA CIEGA W850, 5M (H 250MM)","ZENERGY - TELJES ELSŐ BURKOLAT W850, 5M / 700"]
["32956","ZENERGY - OSŁONA APARATURY MODUŁOWEJ, OTWÓR PRZESUNIĘTY W850, 5M / 700, 35 MOD",79.099999999999994,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988329563","OE - Couvercle d'appareil modulaire, trou décalé L850, 5M / 700, 35 modulaire","OE - Modular equipment cover, offset hole W850, 5M / 700, 35 mod","OE- TAPA MODULAR  AGUJERO DESPLAZADO W850, 5M / 700, 35 mod","ZENERGY - MODULÁRUS BERENDEZÉS BURKOLAT, OFFSET HOLE W850, 5M / 700, 35 MOD"]
["32960","ZENERGY - OSŁONA CZOŁOWA PEŁNA W850, 6M / 700",83.4,"1-ZE-01",1.4,7,"01_PLAIN_COVERS","32960","SZT","85389099","27.12.40.0",null,"5901988329600","OE - Couverture avant complète L850, 6M / 700","OE - Plain Front cover W850, 6M / 700","OE- TAPA CIEGA W850, 6M (H 300MM)","ZENERGY - TELJES ELSŐ BURKOLAT W850, 6M / 700"]
["32966","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W850, 6M / 700, 2x35 MOD",81.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS",null,"SZT","85389099",null,null,"5901988329662","OE - COUVERCLE MODULAIRE L850, 6M / 700, 2x35 MOD","OE - Modular cover W850, 6M / 700, 2x35 MOD","*OE - CUBIERTA MODULAR W850, 6M / 700, 2x35 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W850, 6M / 700, 2x35 MOD"]
["32978","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W850, 7M / 700",127.6,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988329785","OE - CACHE AVANT PERFORÉ L850, 7M / 700","OE - Perforated Front cover W850, 7M / 700","*OE - TAPA DELANTERA PERFORADA W850, 7M / 700","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W850, 7M / 700"]
["32981","ZENERGY - OSŁONA CZOŁOWA SIRCO1600 3P, W850, 10M / 700",135,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988329815","OE - CAPOT AVANT SIRCO1600 3P, L850, 10M / 700","OE - Front cover SIRCO1600 3P, W850, 10M / 700","*OE - TAPA DELANTERA SIRCO1600 3P, W850, 10M / 700","ZENERGY - ŐRFRONT SIRCO1600 3P, W850, 10M / 700"]
["32986","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W850, 9M / 700, 3x35 MOD",124.3,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS",null,"SZT","85389099",null,null,"5901988329860","OE - COUVERCLE MODULAIRE L850, 9M / 700, 3x35 MOD","OE - Modular cover W850, 9M / 700, 3x35 MOD","*OE - TAPA MODULAR W850, 9M / 700, 3x35 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W850, 9M / 700, 3x35 MOD"]
["32990","ZENERGY - OSŁONA CZOŁOWA PEŁNA W850, 9M / 700",128.69999999999999,"1-ZE-01",0.14166666666666666,2,"01_PLAIN_COVERS","32990","SZT","85389099","27.12.40.0",null,"5901988329907","OE - Couverture avant complète L850, 9M / 700","OE - Plain Front cover W850, 9M / 700","OE- TAPA CIEGA W850, 9M (H 450MM)","ZENERGY - TELJES ELSŐ BURKOLAT W850, 9M / 700"]
["32993","ZENERGY - OSŁONA CZOŁOWA PEŁNA W850, 12M / 700",149.6,"1-ZE-01",1.6666666666666666E-2,1,"01_PLAIN_COVERS","32993","SZT","85389099","27.12.40.0",null,"5901988329938","OE - Couverture avant complète L850, 12M / 700","OE - Plain Front cover W850, 12M / 700","OE- TAPA CIEGA W850, 12M (H 600MM)","ZENERGY - TELJES ELSŐ BURKOLAT W850, 12M / 700"]
["32997","ZENERGY OM-VSD - OSŁONA APARATURY MODUŁOWEJ, UKŁAD PIONOWY W850, 11M / 700, 3X29 MOD",178.3,"1-ZE-01",null,null,"OM_VSD_PLATES","32997","SZT","85389099",null,null,"5901988329976","OM-VSD - Couvercle modulaire, vertical L850, 11M / 700, modulaire 3x29","OM-VSD - Modular equipment cover, Vertical layout W850, 11M / 700, 3x29 mod","OM-VSD- TAPA MODULAR VERTIC. W850, 11M/700, 3X29 MOD","ZENERGY OM-VSD - MODULÁRUS BERENDEZÉSBURKOLAT, FÜGGŐLEGES W850, 11M / 700, 3X29 MOD"]
["33013","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W1000, 3M, OCYNK, BEZ WSPORNIKÓW",93.3,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33013","SZT","85389099","27.12.40.0",null,"5901988330132","OE - Plaque de montage complète L1000, 3M, galvanisée, sans supports","OE - Plain Mounting plate W1000, 3M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W1000, 3M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W1000, 3M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33017","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W1000, 8M, OCYNK, BEZ WSPORNIKÓW",210.6,"1-ZE-01",0.01,1,"OE_PLAIN_PLATES","33017","SZT","85389099",null,null,"5901988330170","OE - Plaque de montage complète L1000, 8M, galvanisée, sans supports","OE - Plain Mounting plate W1000, 8M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W1000, 8M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W1000, 8M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33033","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W300, 3M, OCYNK, BEZ WSPORNIKÓW",40.5,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33033","SZT","85389099",null,null,"5901988330330","OE - Plaque de montage complète L300, 3M, galvanisée, sans supports","OE - Plain Mounting plate W300, 3M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W300, 3M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W300, 3M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33036","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W300, 6M, OCYNK, BEZ WSPORNIKÓW",71,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33036","SZT","85389099","27.12.40.0",null,"5901988330361","OE - Plaque de montage complète L300, 6M, galvanisée, sans supports","OE - Plain Mounting plate W300, 6M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W300, 6M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W300, 6M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33037","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W300, 8M, OCYNK, BEZ WSPORNIKÓW",89.1,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33037","SZT","85389099",null,null,"5901988330378","OE - Plaque de montage complète L300, 8M, galvanisée, sans supports","OE - Plain Mounting plate W300, 8M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W300, 8M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W300, 8M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33042","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W400, 2M, OCYNK, BEZ WSPORNIKÓW",40.5,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33042","KPL","85389099","27.12.40.0",null,"5901988330422","OE - Plaque de montage complète L400, 2M, galvanisée, sans supports","OE - Plain Mounting plate W400, 2M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W400, 2M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W400, 2M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33045","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W400, 5M, OCYNK, BEZ WSPORNIKÓW",62.9,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33045","SZT","85389099","27.12.40.0",null,"5901988330453","OE - Plaque de montage complète L400, 5M, galvanisée, sans supports","OE - Plain Mounting plate W400, 5M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W400, 5M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W400, 5M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33048","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W400, 10M, OCYNK, BEZ WSPORNIKÓW",115.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33048","SZT","85389099","27.12.40.0",null,"5901988330484","OE - Plaque de montage complète L400, 10M, galvanisée, sans supports","OE - Plain Mounting plate W400, 10M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W400, 10M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W400, 10M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33055","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W450, 5M, OCYNK, BEZ WSPORNIKÓW",79.099999999999994,"1-ZE-01",1.6666666666666666E-2,1,"OE_PLAIN_PLATES","33055","SZT","85389099",null,null,"5901988330552","OE - Plaque de montage complète L450, 5M, galvanisée, sans supports","OE - Plain Mounting plate W450, 5M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W450, 5M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W450, 5M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33059","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W450, 12M, OCYNK, BEZ WSPORNIKÓW",155.5,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33059","SZT","85389099",null,null,"5901988330590","OE - Plaque de montage complète L450, 12M, galvanisée, sans supports","OE - Plain Mounting plate W450, 12M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W450, 12M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W450, 12M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33064","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W600, 4M, OCYNK, BEZ WSPORNIKÓW",66.900000000000006,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33064","KPL","85389099",null,null,"5901988330644","OE - Plaque de montage complète L600, 4M, galvanisée, sans supports","OE - Plain Mounting plate W600, 4M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W600, 4M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W600, 4M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33067","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W600, 8M, OCYNK, BEZ WSPORNIKÓW",131.80000000000001,"1-ZE-01",5.8333333333333334E-2,2,"OE_PLAIN_PLATES","33067","KPL","85389099",null,null,"5901988330675","OE - Plaque de montage complète L600, 8M, galvanisée, sans supports","OE - Plain Mounting plate W600, 8M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W600, 8M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W600, 8M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33068","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W600, 10M, OCYNK, BEZ WSPORNIKÓW",164.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33068","KPL","85389099",null,null,"5901988330682","OE - Plaque de montage complète L600, 10M, galvanisée, sans supports","OE - Plain Mounting plate W600, 10M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W600, 10M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W600, 10M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33073","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W650, 3M, OCYNK, BEZ WSPORNIKÓW",66.900000000000006,"1-ZE-01",4.1666666666666664E-2,1,"OE_PLAIN_PLATES","33073","SZT","85389099","27.12.40.0",null,"5901988330736","OE - Plaque de montage complète L650, 3M, galvanisée, sans supports","OE - Plain Mounting plate W650, 3M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W650, 3M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W650, 3M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33077","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W650, 8M, OCYNK, BEZ WSPORNIKÓW",152.30000000000001,"1-ZE-01",1.6666666666666666E-2,1,"OE_PLAIN_PLATES","33077","SZT","8538909900","27.12.40.0",null,"5901988330774","OE - Plaque de montage complète L650, 8M, galvanisée, sans supports","OE - Plain Mounting plate W650, 8M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W650, 8M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W650, 8M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33082","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W800, 2M, OCYNK, BEZ WSPORNIKÓW",79.099999999999994,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33082","KPL","85389099",null,null,"5901988330828","OE - Plaque de montage complète L800, 2M, galvanisée, sans supports","OE - Plain Mounting plate W800, 2M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W800, 2M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W800, 2M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33085","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W800, 5M, OCYNK, BEZ WSPORNIKÓW",122,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33085","KPL","85389099",null,null,"5901988330859","OE - Plaque de montage complète L800, 5M, galvanisée, sans supports","OE - Plain Mounting plate W800, 5M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W800, 5M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W800, 5M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33089","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W800, 12M, OCYNK, BEZ WSPORNIKÓW",270,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33089","SZT","85389099",null,null,"5901988330897","OE - Plaque de montage complète L800, 12M, galvanisée, sans supports","OE - Plain Mounting plate W800, 12M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W800, 12M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W800, 12M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33094","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W850, 4M, OCYNK, BEZ WSPORNIKÓW",111.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES","33094","SZT","85389099","27.12.40.0",null,"5901988330941","OE - Plaque de montage complète L850, 4M, galvanisée, sans étriers","OE - Plain Mounting plate W850, 4M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W850, 4M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W850, 4M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33097","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W850, 8M, OCYNK, BEZ WSPORNIKÓW",200.9,"1-ZE-01",0.01,1,"OE_PLAIN_PLATES","33097","SZT","8538909900","27.12.40.0",null,"5901988330972","OE - Plaque de montage complète L850, 8M, galvanisée, sans étriers","OE - Plain Mounting plate W850, 8M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W850, 8M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W850, 8M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33098","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W850, 10M, OCYNK, BEZ WSPORNIKÓW",263.5,"1-ZE-01",4.1666666666666664E-2,2,"OE_PLAIN_PLATES","33098","SZT","85389099","27.12.40.0",null,"5901988330989","OE - Plaque de montage complète L850, 10M, galvanisée, sans supports","OE - Plain Mounting plate W850, 10M, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W850, 10M, SIN SOPORT.","ZENERGY - TÖMÖR SZERELŐLEMEZ W850, 10M, HORGANYOZOTT, KONZER NÉLKÜL"]
["33101","ZENERGY - PRZYŁĄCZE TRANSFEROWE D400, 100 - 250A 4P",524.70000000000005,"1-ZE-01",4.1666666666666664E-2,2,"OE_MCCB_TRANSFER","33101","SZT","85369010","27.33.13.0",null,"5901988331016","OE - Connexion de transfert P400, 100 - 250A 4P","OE - Transfer connector D400, 100 - 250A 4P","OE- CONEXION PREFABRICADA D400, 100 - 250A 4P","ZENERGY - ÁTVITELI CSATLAKOZÁS D400, 100 - 250A 4P"]
["33105","ZENERGY - PRZYŁĄCZE TRANSFEROWE D400, 630 - 1600A 3P, 6M",551.1,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","33105","SZT","85389099",null,null,"5901988331054","OE - Connexion de transfert P400, 630 - 1600A 3P, 6M","OE - Transfer connection D400, 630 - 1600A 3P, 6M","OE- CONEXION PREFABRICADA D400, 630 - 1600A 3P, 6M","ZENERGY - ÁTVITELI CSATLAKOZÁS D400, 630 - 1600A 3P, 6M"]
["33108","ZENERGY - OSŁONA PRZYŁĄCZA TRANSFEROWEGO D400, 1600A 4P,7M",43.7,"1-ZE-01",null,null,"OE_MCCB_TRANSFER",null,"SZT","85389099",null,null,"5901988331085","OE - Couvercle pour port de transfert P400, 1600A 4P, 7M","OE - Cover for transfer connection D400, 1600A 4P, 7M","OE- TAPA CONEXION PREF. D400, 1600A 4P,7M","ZENERGY - ÁTVITELI CSATLAKOZÓ FEDÉL D400, 1600A 4P,7M"]
["33112","ZENERGY - WSPORNIK IZOLATORÓW MOSTU PIONOWEGO NA PLECACH W1300, WZMOCNIONY",0,"1-ZE-01",null,null,"OE_SUPPORT","33112","SZT","85389099",null,null,"5901988331122","OE - Support pour isolants de pont vertical sur le dos L1300, renforcé","OE - Bracket for insulators of the Vertical bridge on the back of the W1300, reinforced","OE- SOPORTE EMB. VERTIC. EN LA PARTE TRASERA DEL W1300, REFORZADO","ZENERGY - FÜGGŐLEGES HÍDSZIGETELŐ TARTÁS A W1300 HÁTLAPÁN, MEGERŐSÍTETT"]
["33116","ZENERGY - WSPORNIK IZOLATORÓW MOSTU PIONOWEGO NA PLECACH W600, WZMOCNIONY",70.400000000000006,"1-ZE-01",8.3333333333333329E-2,1,"OE_SUPPORT","33116","SZT","85389099",null,null,"5901988331160","OE - Support pour isolateurs de ponts verticaux à l'arrière L600, renforcé","OE - Bracket for insulators of the Vertical bridge on the back of the W600, reinforced","OE- SOPORTE EMB. VERTIC. EN LA PARTE TRASERA DEL W600, REFORZADO","ZENERGY – FÜGGŐLEGES HÍDSZIGETELŐ TARTÁS A W600 HÁTLAPÁN, MEGERŐSÍTETT"]
["33119","ZENERGY - WSPORNIK IZOLATORÓW MOSTU PIONOWEGO NA PLECACH W850, WZMOCNIONY",80.8,"1-ZE-01",null,null,"OE_SUPPORT","33119","SZT","85389099",null,null,"5901988331191","OE - Support pour isolateurs de ponts verticaux sur dos L850, renforcé","OE - Bracket for insulators of the Vertical bridge on the back of the W850, reinforced","OE- SOPORTE EMB. VERTIC. EN LA PARTE TRASERA DEL W850, REFORZADO","ZENERGY – FÜGGŐLEGES HÍDSZIGETELŐ TARTÁS A W850 HÁTLAPÁN, MEGERŐSÍTETT"]
["33120","ZENERGY - WSPORNIK IZOLATORÓW MOSTU PIONOWEGO D775, WZMOCNIONY",77.7,null,null,null,"OE_SUPPORT",null,null,"85389099",null,null,"5901988331207"]
["33124","ZENERGY - WSPORNIK UNIWERSALNY D400, 1 RZĄD OTWORÓW 8X9MM / 11X13MM",40.799999999999997,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988331245","OE - support universel P400, 1 rangée de trous 8x9mm / 11x13mm","OE - Universal bracket D400, 1 row of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL D400, 1 FILA DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER D400, 1 SOR LYUK 8X9MM / 11X13MM"]
["33133","ZENERGY - WSPORNIK UNIWERSALNY D300, 2 RZĘDY OTWORÓW 8X9MM / 11X13MM",36.4,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85381000","27.12.40.0",null,"5901988331337","OE - Support universel P300, 2 rangées de trous 8x9mm / 11x13mm","OE - Universal bracket D300, 2 rows of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL D300, ILAS DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER D300, 2 SOR LYUK 8X9MM / 11X13MM"]
["33142","ZENERGY - WSPORNIK UNIWERSALNY W1300, 1 RZĄD OTWORÓW 8X9MM / 11X13MM",70.599999999999994,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099",null,null,"5901988331429","OE - Support universel L1300, 1 rangée de trous 8x9mm / 11x13mm","OE - W1300 universal bracket, 1 row of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W1300, 1 FILA DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W1300, 1 SOR LYUK 8X9MM / 11X13MM"]
["33145","ZENERGY - WSPORNIK UNIWERSALNY W450, 1 RZĄD OTWORÓW 8X9MM / 11X13MM",40.799999999999997,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099",null,null,"5901988331450","OE - Support universel L450, 1 rangée de trous 8x9mm / 11x13mm","OE - W450 universal bracket, 1 row of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W450, 1 FILA DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W450, 1 SOR LYUK 8X9MM / 11X13MM"]
["33148","ZENERGY - WSPORNIK UNIWERSALNY W800, 1 RZĄD OTWORÓW 8X9MM / 11X13MM",44.8,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099",null,null,"5901988331481","OE - Support universel L800, 1 rangée de trous 8x9mm / 11x13mm","OE - W800 universal bracket, 1 row of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W800, 1 FILA DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W800, 1 SOR LYUK 8X9MM / 11X13MM"]
["33152","ZENERGY - WSPORNIK UNIWERSALNY W1300, 2 RZĘDY OTWORÓW 8X9MM / 11X13MM",70.599999999999994,"1-ZE-01",null,null,"OE_SUPPORT",null,"KPL","85389099",null,null,"5901988331528","OE - support universel L1300, 2 rangées de trous 8x9mm / 11x13mm","OE - W1300 universal bracket, 2 rows of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W1300, ILAS DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W1300, 2 SOR LYUK 8X9MM / 11X13MM"]
["33155","ZENERGY - WSPORNIK UNIWERSALNY W450, 2 RZĘDY OTWORÓW 8X9MM / 11X13MM",40.799999999999997,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988331559","OE - Support universel L450, 2 rangées de trous 8x9mm / 11x13mm","OE - W450 universal bracket, 2 rows of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W450, ILAS DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W450, 2 SOR LYUK 8X9MM / 11X13MM"]
["33156","ZENERGY - WSPORNIK UNIWERSALNY W600, 2 RZĘDY OTWORÓW 8X9MM / 11X13MM",42.8,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988331566","OE - Support universel L600, 2 rangées de trous 8x9mm / 11x13mm","OE - W600 universal bracket, 2 rows of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W600, ILAS DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W600, 2 SOR LYUK 8X9MM / 11X13MM"]
["33159","ZENERGY - WSPORNIK UNIWERSALNY W850, 2 RZĘDY OTWORÓW 8X9MM / 11X13MM",48.9,"1-ZE-01",0.18333333333333332,2,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988331597","OE - Support universel L850, 2 rangées de trous 8x9mm / 11x13mm","OE - W850 universal bracket, 2 rows of holes 8x9mm / 11x13mm","OE- SOPORTE UNIVERSAL W850, ILAS DE AGUJEROS 8X9MM ","ZENERGY - UNIVERZÁLIS KONZER W850, 2 SOR LYUK 8X9MM / 11X13MM"]
["33162","ZENERGY - DRABINKA KABLOWA W1300",59.9,"1-ZE-01",null,null,"OE_SUPPORT","33162","SZT","85389099","27.12.40.0",null,"5901988331627","OE - Échelle à câbles L1300","OE - W1300 Cable ladder","OE- SOPORTE FIJACION CABLES W1300","ZENERGY - KÁBELLÉTRA W1300"]
["33166","ZENERGY - DRABINKA KABLOWA W600",31.1,"1-ZE-01",0.31666666666666665,2,"OE_SUPPORT","33166","SZT","85389099","27.12.40.0",null,"5901988331665","OE - Échelle à câbles L600","OE - W600 Cable ladder","OE- SOPORTE FIJACION CABLES W600","ZENERGY - W600 KÁBELLÉTRA"]
["33169","ZENERGY - DRABINKA KABLOWA W850",45.6,"1-ZE-01",1.2,4,"OE_SUPPORT","33169","SZT","85389099","27.12.40.0",null,"5901988331696","OE - Échelle à câble L850","OE - W850 Cable ladder","OE- SOPORTE FIJACION CABLES W850","ZENERGY - KÁBELLÉTRA W850"]
["33173","ZENERGY - DRABINKA KABLOWA D300",29.5,"1-ZE-01",null,null,"OE_SUPPORT","33173","SZT","85389099","27.12.40.0",null,"5901988331733","OE - échelle de câble P300","OE - Cable ladder D300","OE- SOPORTE FIJACION CABLES D300","ZENERGY - KÁBELLÉTRA D300"]
["33178","ZENERGY - DRABINKA KABLOWA W200",26.5,"1-ZE-01",null,null,"OE_SUPPORT","33178","SZT","85389099","27.12.40.0",null,"5901988331788","OE - Échelle à câbles L200","OE - W200 Cable ladder","OE- SOPORTE FIJACION CABLES W200","ZENERGY - KÁBELLÉTRA W200"]
["33182","ZENERGY - DRABINKA KABLOWA NA DRZWI W500 / PODWÓJNE W1000",62.4,"1-ZE-01",0.2,1,"OE_SUPPORT","33182","SZT","85389099","27.12.40.0",null,"5901988331825","OE - Échelle à câbles pour Portes W500 / doubles L1000","OE - W500 / double W1000 Cable ladder","OE- SOPORTE FIJACION CABLES PARA PUERTA  W1300","ZENERGY - KÁBELLÉTRA AJTÓHOZ W500 / DOUBLE W1000"]
["33183","ZENERGY - DRABINKA KABLOWA NA DRZWI W300",55,"1-ZE-01",null,null,"OE_SUPPORT","33183","SZT","85389099",null,null,"5901988331832","OE - Échelle à câbles pour Portes L300","OE - W300 door Cable ladder","OE- SOPORTE FIJACION CABLES PARA PUERTA  W300","ZENERGY - KÁBELLÉTRA AZ AJTÓN W300"]
["33186","ZENERGY - DRABINKA KABLOWA NA DRZWI W600 / PODWÓJNE W1200",64.7,"1-ZE-01",8.3333333333333329E-2,1,"OE_SUPPORT","33186","SZT","85389099","27.12.40.0",null,"5901988331863","OE - Échelle à câbles pour Portes L600 / doubles L1200","OE - W600 / double W1200 Cable ladder","OE- SOPORTE FIJACION CABLES PARA PUERTA  W600","ZENERGY - KÁBELLÉTRA AJTÓHOZ W600 / DOUBLE W1200"]
["33189","ZENERGY - DRABINKA KABLOWA NA DRZWI W850",74.3,"1-ZE-01",null,null,"OE_SUPPORT","33189","SZT","85389099","27.90.33.0",null,"5901988331894","OE - Échelle à câbles pour Portes L850","OE - W850 door Cable ladder","OE- SOPORTE FIJACION CABLES PARA PUERTA  W850","ZENERGY - KÁBELLÉTRA AZ AJTÓN W850"]
["33193","ZENERGY - DRABINKA KABLOWA NA PŁYTĘ MONTAŻOWĄ L=500",67.2,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099","27.12.40.0",null,"5901988331931","OE - Échelle à câbles pour plaque de montage L = 700","OE - Cable ladder for Mounting plate L = 700","OE- SOPORTE FIJACION CABLES PARA PLACA MONTAJE   L=700","ZENERGY - KÁBELLÉTRA SZERELŐLAPHOZ L=500"]
["33195","ZENERGY - DRABINKA KABLOWA NA MASKOWNICĘ W450",45.6,"1-ZE-01",null,null,"OE_SUPPORT","33195","SZT","85389099","27.12.40.0",null,"5901988331955","OE - Échelle à câbles pour la calandre L450","OE - Cable ladder for W450 grill","OE- SOPORTE FIJACION CABLES PARA TAPA W450","ZENERGY - KÁBELLÉTRA W450 BURKOLATHOZ"]
["33204","ZENERGY - PŁYTA MONTAŻOWA LICZNIKOWA 1TL, W400, 12M, OCYNK, MALOWANA",342.4,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","33204","SZT","85389099",null,null,"5901988332044","OE - Plaque de montage pour compteur 1TL, L400, 12M, galvanisée, peinte","OE - Counter Mounting plate 1TL, W400, 12M, Galvanized, painted","OE- PLACA MONTAJE  CONTADOR 1TL, W400, 12M","ZENERGY - KONTROLLALAP 1TL, W400, 12M, HORGANYOZOTT, FESTETT"]
["33210","ZENERGY - POKRYWA GÓRNA IP43/55, W1000, D230",190.1,"1-ZE-01",null,null,"OE_COVERS","31210","SZT","85389099",null,null,"5901988332105","OE - Capot supérieur IP43 / 55, L1000, P230","OE - Top cover IP43 / 55, W1000, D230","OE- TECHO IP43/55, W1000, D230","ZENERGY - FELSŐ BURKOLAT IP43/55, W1000, D230"]
["33213","ZENERGY - POKRYWA GÓRNA IP43/55, W1300, D230",221.4,"1-ZE-01",null,null,"OE_COVERS","31213","SZT","85389099",null,null,"5901988332136","OE - Capot supérieur IP43 / 55, L1300, P230","OE - Top cover IP43 / 55, W1300, D230","OE- TECHO IP43/55, W1300, D230","ZENERGY - FELSŐ BURKOLAT IP43/55, W1300, D230"]
["33215","ZENERGY - POKRYWA GÓRNA IP43/55, W650+450, D230",199.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332150","OE - Capot supérieur IP43 / 55, L650 + 450, P230","OE - Top cover IP43 / 55, W650 + 450, D230","OE- TECHO IP43/55, W650+450, D230","ZENERGY - FELSŐ BORÍTÓA IP43/55, W650+450, D230"]
["33219","ZENERGY - POKRYWA GÓRNA IP43/55, W850+400, D230",214.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332198","OE - Capot supérieur IP43 / 55, L850 + 400, P230","OE - Top cover IP43 / 55, W850 + 400, D230","OE- TECHO IP43/55, W850+400, D230","ZENERGY – FELSŐ BURKOLAT IP43/55, W850+400, D230"]
["33222","ZENERGY - POKRYWA GÓRNA IP43/55, W150+650+300, D230",199.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332228","OE - Capot supérieur IP43 / 55, L150 + 650 + 300, P230","OE - Top cover IP43 / 55, W150 + 650 + 300, D230","OE- TECHO IP43/55, W150+650+300, D230","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+650+300, D230"]
["33232","ZENERGY - POKRYWA GÓRNA IP43/55, W200+650+300, D230",205.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332327","OE - Capot supérieur IP43 / 55, L200 + 650 + 300, P230","OE - Top cover IP43 / 55, W200 + 650 + 300, D230","OE- TECHO IP43/55, W200+650+300, D230","ZENERGY – FELSŐ BURKOLAT IP43/55, W200+650+300, D230"]
["33245","ZENERGY - POKRYWA GÓRNA IP43/55, W450, D230",139.30000000000001,"1-ZE-01",null,null,"OE_COVERS","31245","SZT","85389099",null,null,"5901988332457","OE - Capot supérieur IP43 / 55, L450, P230","OE - Top cover IP43 / 55, W450, D230","OE- TECHO IP43/55, W450, D230","ZENERGY - FELSŐ BURKOLAT IP43/55, W450, D230"]
["33271","ZENERGY - POKRYWA GÓRNA IP43/55, W300+400, D230",162,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332716","OE - Capot supérieur IP43 / 55, L300 + 400, P230","OE - Top cover IP43 / 55, W300 + 400, D230","OE- TECHO IP43/55, W300+400, D230","ZENERGY - FELSŐ BURKOLAT IP43/55, W300+400, D230"]
["33281","ZENERGY - POKRYWA GÓRNA IP43/55, W650+150, D230",171.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332815","OE - Capot supérieur IP43 / 55, L650 + 150, P230","OE - Top cover IP43 / 55, W650 + 150, D230","OE- TECHO IP43/55, W650+150, D230","ZENERGY – FELSŐ BURKOLAT IP43/55, W650+150, D230"]
["33291","ZENERGY - POKRYWA GÓRNA IP43/55, W450+450, D230",181.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332914","OE - Capot supérieur IP43 / 55, L450 + 450, P230","OE - Top cover IP43 / 55, W450 + 450, D230","OE- TECHO IP43/55, W450+450, D230","ZENERGY – FELSŐ BURKOLAT IP43/55, W450+450, D230"]
["33295","ZENERGY - POKRYWA GÓRNA IP43/55, W650+300, D230",186.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988332952","OE - Capot supérieur IP43 / 55, L650 + 300, P230","OE - Top cover IP43 / 55, W650 + 300, D230","OE- TECHO IP43/55, W650+300, D230","ZENERGY – FELSŐ BURKOLAT IP43/55, W650+300, D230"]
["33312","ZENERGY - POKRYWA GÓRNA IP43/55, W1200, D300",341.3,"1-ZE-01",null,null,"OE_COVERS","31312","SZT","85389099",null,null,"5901988333126","OE - Capot supérieur IP43 / 55, L1200, P300","OE - Top cover IP43 / 55, W1200, D300","OE- TECHO IP43/55, W1200, D300","ZENERGY - FELSŐ BURKOLAT IP43/55, W1200, D300"]
["33316","ZENERGY - POKRYWA GÓRNA IP43/55, W850+150, D300",301.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988333164","OE - Capot supérieur IP43 / 55, L850 + 150, P300","OE - Top cover IP43 / 55, W850 + 150, D300","OE- TECHO IP43/55, W850+150, D300","ZENERGY – FELSŐ BURKOLAT IP43/55, W850+150, D300"]
["33321","ZENERGY - POKRYWA GÓRNA IP43/55, W150+650+400, D300",341.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988333218","OE - Capot supérieur IP43 / 55, L150 + 650 + 400, P300","OE - Top cover IP43 / 55, W150 + 650 + 400, D300","OE- TECHO IP43/55, W150+650+400, D300","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+650+400, D300"]
["33328","ZENERGY - POKRYWA GÓRNA IP43/55, W150+850+400, D300",379.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988333287","OE - Capot supérieur IP43 / 55, L150 + 850 + 400, P300","OE - Top cover IP43 / 55, W150 + 850 + 400, D300","OE- TECHO IP43/55, W150+850+400, D300","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+850+400, D300"]
["33340","ZENERGY - POKRYWA GÓRNA IP43/55, W400, D300",182.5,"1-ZE-01",0.01,1,"OE_COVERS","31340","SZT","85389099",null,null,"5901988333409","OE - Capot supérieur IP43 / 55, L400, P300","OE - Top cover IP43 / 55, W400, D300","OE- TECHO IP43/55, W400, D300","ZENERGY - FELSŐ BURKOLAT IP43/55, W400, D300"]
["33365","ZENERGY - POKRYWA GÓRNA IP43/55, W650, D300",232.2,"1-ZE-01",5.8333333333333334E-2,6,"OE_COVERS","31365","SZT","85389099",null,null,"5901988333652","OE - Capot supérieur IP43 / 55, L650, P300","OE - Top cover IP43 / 55, W650, D300","OE- TECHO IP43/55, W650, D300","ZENERGY - FELSŐ BURKOLAT IP43/55, W650, D300"]
["33376","ZENERGY - POKRYWA GÓRNA IP43/55, W300+450, D300",251.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988333768","OE - Capot supérieur IP43 / 55, L300 + 450, P300","OE - Top cover IP43 / 55, W300 + 450, D300","OE- TECHO IP43/55, W300+450, D300","ZENERGY – FELSŐ BURKOLAT IP43/55, W300+450, D300"]
["33380","ZENERGY - POKRYWA GÓRNA IP43/55, W800, D300",261.39999999999998,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","31380","SZT","85389099",null,null,"5901988333805","OE - Capot supérieur IP43 / 55, L800, P300","OE - Top cover IP43 / 55, W800, D300","OE- TECHO IP43/55, W800, D300","ZENERGY - FELSŐ BURKOLAT IP43/55, W800, D300"]
["33391","ZENERGY - POKRYWA GÓRNA IP43/55, W450+450, D300",281.89999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988333911","OE - Capot supérieur IP43 / 55, L450 + 450, P300","OE - Top cover IP43 / 55, W450 + 450, D300","OE- TECHO IP43/55, W450+450, D300","ZENERGY – FELSŐ BURKOLAT IP43/55, W450+450, D300"]
["33410","ZENERGY - POKRYWA GÓRNA IP43/55, W1000, D400",306.7,"1-ZE-01",0.30833333333333335,5,"OE_COVERS","31410","SZT","85389099","27.12.40.0",null,"5901988334109","OE - Capot supérieur IP43 / 55, L1000, P400","OE - Top cover IP43 / 55, W1000, D400","OE- TECHO IP43/55, W1000, D400","ZENERGY - FELSŐ BURKOLAT IP43/55, W1000, D400"]
["33413","ZENERGY - POKRYWA GÓRNA IP43/55, W1300, D400",364,"1-ZE-01",null,null,"OE_COVERS","31413","SZT","85389099","27.12.40.0",null,"5901988334130","OE - Capot supérieur IP43 / 55, L1300, P400","OE - Top cover IP43 / 55, W1300, D400","OE- TECHO IP43/55, W1300, D400","ZENERGY - FELSŐ BURKOLAT IP43/55, W1300, D400"]
["33418","ZENERGY - POKRYWA GÓRNA IP43/55, W850+300, D400",334.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988334185","OE - Capot supérieur IP43 / 55, L850 + 300, P400","OE - Top cover IP43 / 55, W850 + 300, D400","OE- TECHO IP43/55, W850+300, D400","ZENERGY – FELSŐ BURKOLAT IP43/55, W850+300, D400"]
["33422","ZENERGY - POKRYWA GÓRNA IP43/55, W150+650+300, D400",326.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988334222","OE - Capot supérieur IP43 / 55, L150 + 650 + 300, P400","OE - Top cover IP43 / 55, W150 + 650 + 300, D400","OE- TECHO IP43/55, W150+650+300, D400","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+650+300, D400"]
["33430","ZENERGY - POKRYWA GÓRNA IP43/55, W300, D400",171.7,"1-ZE-01",0.8833333333333333,7,"OE_COVERS","31430","SZT","85389099","27.12.40.0",null,"5901988334307","OE - Capot supérieur IP43 / 55, L300, P400","OE - Top cover IP43 / 55, W300, D400","OE- TECHO IP43/55, W300, D400","ZENERGY - FELSŐ BURKOLAT IP43/55, W300, D400"]
["33440","ZENERGY - POKRYWA GÓRNA IP43/55, W400, D400",190.1,"1-ZE-01",0.19166666666666668,5,"OE_COVERS","31440","SZT","85389099","27.12.40.0",null,"5901988334406","OE - Capot supérieur IP43 / 55, L400, P400","OE - Top cover IP43 / 55, W400, D400","OE- TECHO IP43/55, W400, D400","ZENERGY - FELSŐ BURKOLAT IP43/55, W400, D400"]
["33441","ZENERGY - POKRYWA GÓRNA IP43/55, W400, D400, z przepustem pod kable",316.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988334413","OE - CAPOT SUPÉRIEUR IP43/55, L400, P400, avec presse-étoupe","OE - Top cover IP43/55, W400, D400, with cable gland","*OE - CUBIERTA SUPERIOR IP43/55, W400, D400, con prensaestopas","ZENERGY - FELSŐ BURKOLAT IP43/55, W400, D400, kábelbemenettel"]
["33460","ZENERGY - POKRYWA GÓRNA IP43/55, W600, D400",229,"1-ZE-01",0.10833333333333334,8,"OE_COVERS","31460","SZT","85389099","27.12.40.0",null,"5901988334604","OE - Capot supérieur IP43 / 55, L600, P400","OE - Top cover IP43 / 55, W600, D400","OE- TECHO IP43/55, W600, D400","ZENERGY - FELSŐ BURKOLAT IP43/55, W600, D400"]
["33471","ZENERGY - POKRYWA GÓRNA IP43/55, W300+400, D400",247.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988334710","OE - Capot supérieur IP43 / 55, L300 + 400, P400","OE - Top cover IP43 / 55, W300 + 400, D400","OE- TECHO IP43/55, W300+400, D400","ZENERGY – FELSŐ BURKOLAT IP43/55, W300+400, D400"]
["33480","ZENERGY - POKRYWA GÓRNA IP43/55, W800, D400",268.89999999999998,"1-ZE-01",0.45833333333333331,11,"OE_COVERS","31480","SZT","85389099","27.12.40.0",null,"5901988334802","OE - Capot supérieur IP43 / 55, L800, P400","OE - Top cover IP43 / 55, W800, D400","OE- TECHO IP43/55, W800, D400","ZENERGY - FELSŐ BURKOLAT IP43/55, W800, D400"]
["33484","ZENERGY - POKRYWA GÓRNA IP43/55, W850, D400, z przepustem pod kable Lewy",479.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988334840","OE - CAPOT SUPÉRIEUR IP43/55, L850, P400, avec presse-étoupe Gauche","OE - Top cover IP43/55, W850, D400, with cable gland Left","*OE - CUBIERTA SUPERIOR IP43/55, W850, D400, con prensaestopas Izquierda","ZENERGY - FELSŐ BURKOLAT IP43/55, W850, D400, kábelbemenettel bal"]
["33491","ZENERGY - POKRYWA GÓRNA IP43/55, W450+450, D400",287.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988334918","OE - Capot supérieur IP43 / 55, L450 + 450, P400","OE - Top cover IP43 / 55, W450 + 450, D400","OE- TECHO IP43/55, W450+450, D400","ZENERGY – FELSŐ BURKOLAT IP43/55, W450+450, D400"]
["33501","ZENERGY - PŁYTA MONTAŻOWA LICZNIKOWA 3TL, W400, 24M, OCYNK",445,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","33501","SZT","85389099",null,null,"5901988335014","OE - Plaque de connexion 3TL, L400, 24M, galv","OE - Counter Mounting plate 3TL, W400, 24M, galv","OE- PLACA MONTAJE  CONTADOR 3TL, W400, 24M","ZENERGY - 3TL-ES MÉTERES SZERELŐLAP, W400, 24M, HOGAGYZAT"]
["33506","ZENERGY - PŁYTA MONTAŻOWA LICZNIKOWA 4TL, W650, 18M, OCYNK",594,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","33506","SZT","85381000","27.12.40.0",null,"5901988335069","OE - Plaque de connexion 4TL, L650, 18M, galv","OE - Counter Mounting plate 4TL, W650, 18M, galv","OE- PLACA MONTAJE  CONTADOR 4TL, W650, 18M","ZENERGY - KONTROLL SZERELŐLEMEZ 4TL, W650, 18M, HORGANYOZ"]
["33507","ZENERGY - PŁYTA MONTAŻOWA LICZNIKOWA 6TL, W650, 24M, OCYNK",644.79999999999995,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","33507","SZT","85389099",null,null,"5901988335076","OE - Plaque de connexion 6TL, L650, 24M, galv","OE - Counter Mounting plate 6TL, W650, 24M, galv","OE- PLACA MONTAJE  CONTADOR 6TL, W650, 24M","ZENERGY - MÉRŐSZERELŐ LEMEZ 6TL, W650, 24M, HORGANYOZ"]
["33513","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W1000, 3M, OCYNK",254.9,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335137","OE - Plaque de câblage L1000, 3M, galvanisée + supports","OE - Perforated Mounting plate W1000, 3M, galv","OE- PLACA MONTAJE  TROQ. W1000, 3M + SOPORT.","ZENERGY - NYITOTT SZERELŐLEMEZ W1000, 3M, HOGANGOZOTT"]
["33533","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W300, 3M, OCYNK",127.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335335","OE - Plaque de montage L300, 3M, galvanisée + supports","OE - Perforated Mounting plate W300, 3M, galv","OE- PLACA MONTAJE  TROQ. W300, 3M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W300, 3M, HORGANYOZ"]
["33536","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W300, 6M, OCYNK",205.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335366","OE - Plaque de montage pour plaquette L300, 6M, galvanisée + supports","OE - Perforated Mounting plate W300, 6M, galv","OE- PLACA MONTAJE  TROQ. W300, 6M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W300, 6M, HORGANYOZ"]
["33539","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W300, 12M, OCYNK",320.8,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335397","OE - Plaque de montage pour plaquette L300, 12M, galvanisée + supports","OE - Perforated Mounting plate W300, 12M, galv","OE- PLACA MONTAJE  TROQ. W300, 12M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W300, 12M, HORGANYOZ"]
["33544","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W400, 4M, OCYNK",157.69999999999999,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988335441","OE - Plaque de montage pour trou L400, 4M, galvanisée + supports","OE - Perforated Mounting plate W400, 4M, galv","OE- PLACA MONTAJE  TROQ. W400, 4M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W400, 4M, HORGANYOZ"]
["33549","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W400, 12M, OCYNK",345.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988335496","OE - Plaque de montage percée L400, 12M, galvanisée + supports","OE - Perforated Mounting plate W400, 12M, galv","OE- PLACA MONTAJE  TROQ. W400, 12M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W400, 12M, HORGANYOZ"]
["33552","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W450, 2M, OCYNK",127.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335526","OE - Plaque de montage percée L450, 2M, galvanisée + supports","OE - Perforated Mounting plate W450, 2M, galv","OE- PLACA MONTAJE  TROQ. W450, 2M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W450, 2M, HORGANYOZ"]
["33555","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W450, 5M, OCYNK",197.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335557","OE - Plaque de montage pour plaquette L450, 5M, galvanisée + supports","OE - Perforated Mounting plate W450, 5M, galv","OE- PLACA MONTAJE  TROQ. W450, 5M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W450, 5M, HORGANYOZ"]
["33558","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W450, 10M, OCYNK",318.60000000000002,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335588","OE - Plaque de montage Wafer L450, 10M, galvanisée + supports","OE - Perforated Mounting plate W450, 10M, galv","OE- PLACA MONTAJE  TROQ. W450, 10M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W450, 10M, HORGANYOZ"]
["33564","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W600, 4M, OCYNK",205.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335649","OE - Plaque de montage L600, 4M, galvanisée + supports","OE - Perforated Mounting plate W600, 4M, galv","OE- PLACA MONTAJE  TROQ. W600, 4M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W600, 4M, HORGANYOZ"]
["33567","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W600, 8M, OCYNK",322.89999999999998,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335670","OE - Plaque de montage percée L600, 8M, galvanisée + supports","OE - Perforated Mounting plate W600, 8M, galv","OE- PLACA MONTAJE  TROQ. W600, 8M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W600, 8M, HORGANYOZ"]
["33572","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W650, 2M, OCYNK",152.30000000000001,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988335724","OE - Plaque de montage percée L650, 2M, galvanisée + supports","OE - Mounting plate W650, 2M, galv","OE- PLACA MONTAJE  TROQ. W650, 2M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W650, 2M, HORGANYOZ"]
["33576","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W650, 6M, OCYNK",300.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988335762","OE - Plaque de montage pour trou L650, 6M, galvanisée + supports","OE - Mounting plate W650, 6M, galv","OE- PLACA MONTAJE  TROQ. W650, 6M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W650, 6M, HORGANYOZ"]
["33579","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W650, 12M, OCYNK",477.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988335793","OE - Plaque de montage pour trou L650, 12M, galvanisée + supports","OE - Perforated Mounting plate W650, 12M, galv","OE- PLACA MONTAJE  TROQ. W650, 12M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W650, 12M, HORGANYOZ"]
["33582","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W800, 2M, OCYNK",170.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335823","OE - Plaque de montage L800, 2M, galvanisée + supports","OE - Perforated Mounting plate W800, 2M, galv","OE- PLACA MONTAJE  TROQ. W800, 2M + SOPORT.","ZENERGY - NYITOTT SZERELŐLEMEZ W800, 2M, HOGANGOZOTT"]
["33585","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W800, 5M, OCYNK",277.60000000000002,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335854","OE - Plaque de montage percée L800, 5M, galvanisée + supports","OE - Perforated Mounting plate W800, 5M, galv","OE- PLACA MONTAJE  TROQ. W800, 5M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W800, 5M, HORGANYOZ"]
["33588","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W800, 10M, OCYNK",464.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335885","OE - Plaque de montage pour trou L800, 10M, galvanisée + supports","OE - Perforated Mounting plate W800, 10M, galv","OE- PLACA MONTAJE  TROQ. W800, 10M + SOPORT.","ZENERGY - NYITOTT SZERELŐLEMEZ W800, 10M, HOGAGYZAT"]
["33594","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W850, 4M, OCYNK",266.8,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335946","OE - Plaque de montage soudée L850, 4M, galvanisée + supports","OE - Perforated Mounting plate W850, 4M, galv","OE- PLACA MONTAJE  TROQ. W850, 4M + SOPORT.","ZENERGY - NYITOTT FELSZERELŐLEMEZ W850, 4M, HORGANYOZ"]
["33597","ZENERGY - PŁYTA MONTAŻOWA OTWOROWANA W850, 8M, OCYNK",446,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988335977","OE - Plaque de montage soudée L850, 8M, galvanisée + supports","OE - Perforated Mounting plate W850, 8M, galv","OE- PLACA MONTAJE  TROQ. W850, 8M + SOPORT.","ZENERGY - NYITOTT SZERELŐLEMEZ W850, 8M, HORGANYOZ"]
["33600","Zenergy - Przyłącze transferowe W650, 100 - 250A 3P-4P",521.4,"1-ZE-01",5.8333333333333334E-2,1,"OE_MCCB_TRANSFER","33600","SZT","85389099","27.90.44.0",null,"5901988336004","OE - Connexion de transfert L650, 100 - 250A 3P-4P","OE - Transfer connection W650, 100 - 250A 3P-4P","OE- CONEXIÓN DE TRANSFERENCIA W650, 100- 250A 3P-4P","Zenergy - W650 transzfer csatlakozás, 100 - 250A 3P-4P"]
["33605","OE - Przyłącze transferowe W650, 400 - 630A 3P",584.1,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","33605","SZT",null,null,"240731RT","5901988336059","OE - Connexion de transfert L650, 400 - 630A 3P","OE - Transfer connection W650, 400 - 630A 3P","OE- CONEXIÓN DE TRANSFERENCIA W650, 400- 630A 3P","OE - Átviteli csatlakozás W650, 400 - 630A 3P"]
["33608","ZENERGY - POKRYWA GÓRNA IP43/55, W1000, D600, z przepustem pod kable Lewy",595.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336080","OE - CAPOT SUPÉRIEUR IP43/55, L1000, P600, avec presse-étoupe Gauche","OE - Top cover IP43/55, W1000, D600, with cable gland Left","*OE - CUBIERTA SUPERIOR IP43/55, W1000, D600, con prensaestopas Izquierda","ZENERGY - FELSŐ BURKOLAT IP43/55, W1000, D600, kábelbemenettel bal"]
["33609","ZENERGY - POKRYWA GÓRNA IP43/55, W1000, D600, z przepustem pod kable Prawy",595.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336097","OE - CAPOT SUPÉRIEUR IP43/55, L1000, P600, avec presse-étoupe Droit","OE - Top cover IP43/55, W1000, D600, with cable gland Right","*OE - CUBIERTA SUPERIOR IP43/55, W1000, D600, con prensaestopas Derecha","ZENERGY - FELSŐ BURKOLAT IP43/55, W1000, D600, kábelbemenettel jobb"]
["33612","ZENERGY - POKRYWA GÓRNA IP43/55, W1200, D600",415.8,"1-ZE-01",1.6666666666666666E-2,2,"OE_COVERS","31612","SZT","85389099",null,null,"5901988336127","OE - Capot supérieur IP43 / 55, L1200, P600","OE - Top cover IP43 / 55, W1200, D600","OE- TECHO IP43/55, W1200, D600","ZENERGY - FELSŐ BURKOLAT IP43/55, W1200, D600"]
["33617","ZENERGY - POKRYWA GÓRNA IP43/55, W850+200, D600",362.9,"1-ZE-01",null,null,"OE_COVERS","31617","SZT","85389099",null,null,"5901988336172","OE - Capot supérieur IP43/55, L850+200, P600","OE - Top cover IP43 / 55, W850 + 200, D600","OE- TECHO IP43/55, W850 + 200, D600","ZENERGY – FELSŐ BURKOLAT IP43/55, W850+200, D600"]
["33621","ZENERGY - POKRYWA GÓRNA IP43/55, W150+650+400, D600",415.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336219","OE - Capot supérieur IP43 / 55, L150 + 650 + 400, P600","OE - Top cover IP43 / 55, W150 + 650 + 400, D600","OE- TECHO IP43/55, W150+650+400, D600","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+650+400, D600"]
["33628","ZENERGY - POKRYWA GÓRNA IP43/55, W150+850+400, D600",462.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336288","OE - Capot supérieur IP43 / 55, L150 + 850 + 400, P600","OE - Top cover IP43 / 55, W150 + 850 + 400, D600","OE- TECHO IP43/55, W150+850+400, D600","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+850+400, D600"]
["33640","ZENERGY - POKRYWA GÓRNA IP43/55, W400, D600",226.8,"1-ZE-01",3.3333333333333333E-2,2,"OE_COVERS","31640","SZT","85389099","27.12.40.0",null,"5901988336400","OE - Capot supérieur IP43 / 55, L400, P600","OE - Top cover IP43 / 55, W400, D600","OE- TECHO IP43/55, W400, D600","ZENERGY - FELSŐ BURKOLAT IP43/55, W400, D600"]
["33646","ZENERGY - POKRYWA GÓRNA IP43/55, W450, D600, z przepustem kablowym",378,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336462","OE - CAPOT SUPÉRIEUR IP43/55, L450, P600, avec presse-étoupe","OE - Top cover IP43/55, W450, D600, with cable gland","*OE - CUBIERTA SUPERIOR IP43/55, W450, D600, con prensaestopas","ZENERGY - FELSŐ BURKOLAT IP43/55, W450, D600, kábelbemenettel"]
["33665","ZENERGY - POKRYWA GÓRNA IP43/55, W650, D600",268.89999999999998,"1-ZE-01",0.5083333333333333,5,"OE_COVERS","31665","SZT","85389099","27.12.40.0",null,"5901988336653","OE - Capot supérieur IP43 / 55, L650, P600","OE - Top cover IP43 / 55, W650, D600","OE- TECHO IP43/55, W650, D600","ZENERGY - FELSŐ BURKOLAT IP43/55, W650, D600"]
["33666","ZENERGY - POKRYWA GÓRNA IP43/55, W450+200, D600",286.2,"1-ZE-01",null,null,"OE_COVERS","31665","SZT","85389099",null,null,"5901988336660","OE - Capot supérieur IP43 / 55, L450 + 200, P600","OE - Top cover IP43 / 55, W450 + 200, D600","OE- TECHO IP43/55, W450+200, D600","ZENERGY – FELSŐ BURKOLAT IP43/55, W450+200, D600"]
["33679","ZENERGY - POKRYWA GÓRNA IP43/55, W800, D600, z przepustem kablowym Lewy",502.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336790","OE - CAPOT SUPÉRIEUR IP43/55, L800, P600, avec presse-étoupe Gauche","OE - Top cover IP43/55, W800, D600, with cable gland Left","*OE - CUBIERTA SUPERIOR IP43/55, W800, D600, con prensaestopas Izquierda","ZENERGY - FELSŐ BURKOLAT IP43/55, W800, D600, kábelbemenettel bal"]
["33682","ZENERGY - POKRYWA GÓRNA IP43/55, W800, D600, z przepustem kablowym Prawy",502.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336820","OE - CAPOT SUPÉRIEUR IP43/55, L800, P600, avec presse-étoupe Droit","OE - Top cover IP43/55, W800, D600, with cable gland Right","*OE - CUBIERTA SUPERIOR IP43/55, W800, D600, con prensaestopas Derecha","ZENERGY - FELSŐ BURKOLAT IP43/55, W800, D600, kábelbemenettel jobb"]
["33687","ZENERGY - POKRYWA GÓRNA IP43/55, W850, D600, z przepustem kablowym Prawy",547.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988336875","OE - CAPOT SUPÉRIEUR IP43/55, L850, P600, avec presse-étoupe Droit","OE - Top cover IP43/55, W850, D600, with cable gland Right","*OE - CUBIERTA SUPERIOR IP43/55, W850, D600, con prensaestopas Derecha","ZENERGY - FELSŐ BURKOLAT IP43/55, W850, D600, kábelbemenettel jobb"]
["33741","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W400, 1M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",46.5,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337414","OE - Plaque de montage complète L400, 1M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W400, 1M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W400, 1M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W400, 1M, VÍZSZINTES, HORGANYOZOTT, TÁMASZOK NÉLKÜL"]
["33745","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W400, 5M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",79.099999999999994,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337452","OE - Plaque de montage complète L400, 5M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W400, 5M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W400, 5M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐLEMEZ W400, 5M, VÍZSZINTES, HOGANYZOTT, TÁMASZTÁS NÉLKÜL"]
["33748","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W400, 8M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",119.9,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337483","OE - Plaque de montage complète L400, 8M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W400, 8M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W400, 8M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W400, 8M, VÍZSZINTES, HORGANYOZOTT, TÁMASZTÁS NÉLKÜL"]
["33752","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W450, 2M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",58.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337520","OE - Platine de montage, complète L450, 2M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W450, 2M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W450, 2M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W450, 2M, VÍZSZINTES, HOGANYZOTT, TÁMASZTÁS NÉLKÜL"]
["33753","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W450, 3M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",64.8,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337537","OE - Platine de montage, complète L450, 3M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W450, 3M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W450, 3M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W450, 3M, VÍZSZINTES, HOGAGYZAT, TÁMASZTÁS NÉLKÜL"]
["33756","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W450, 6M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",111.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337568","OE - Plaque de montage complète L450, 6M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W450, 6M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W450, 6M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W450, 6M, VÍZSZINTES, HORGANYOZOTT, TÁMASZOK NÉLKÜL"]
["33771","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W650, 1M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",75.099999999999994,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337711","OE - Plaque de montage complète L650, 1M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W650, 1M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W650, 1M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐLEMEZ W650, 1M, VÍZSZINTES, HOGAGYZAT, TÁMASZTÁS NÉLKÜL"]
["33774","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W650, 4M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",105.6,"1-ZE-01",4.1666666666666664E-2,1,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337742","OE - Plaque de montage complète L650, 4M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W650, 4M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W650, 4M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W650, 4M, VÍZSZINTES, HORGANYOZOTT, TÁMASZOK NÉLKÜL"]
["33777","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W650, 7M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",170.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337773","OE - Plaque de montage complète L650, 7M, horizontale, galvanisée, sans supports","OE - Plain Mounting plate W650, 7M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W650, 7M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W650, 7M, VÍZSZINTES, HOGANYZOTT, TÁMASZOK NÉLKÜL"]
["33781","ZENERGY IT - PÓŁKA RUCHOMA 19\",1U, O GŁ. 650MM, OBCIĄŻENIE <40KG MOCOWANA W CZTERECH PUNKTACH, SZAFY W650",316.39999999999998,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337810","IT - Tablette mobile 19 \", 1U, profondeur principale 650 mm, charge <40 kg fixée en quatre points, armoire L650","IT - 19 1U movable shelf, 650mm deep, load <40kg, mounted in four points, W650 cabinets","Zenergy IT - Estante móvil de 19 \", 1U, 650 mm de profundidad, carga <40 kg, montado en cuatro puntos, gabinetes W650","ZENERGY IT - MOZGÓPOLC 19\", 1U, MÉLYSÉG 650MM, TERHELÉS <40KG, NÉGY PONTBA SZERELHETŐ, W650-ES SZEKRÉNYEK"]
["33792","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W850, 2M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",103.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337926","OE - Plaque de montage complète L850, 2M, horizontale, galvanisée, sans étriers","OE - Plain Mounting plate W850, 2M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W850, 2M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W850, 2M, VÍZSZINTES, HOGANYZOTT, TÁMASZOK NÉLKÜL"]
["33797","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W850, 7M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",221.4,"1-ZE-01",0.10833333333333334,4,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337971","OE - Plaque de montage complète L850, 7M, horizontale, galvanisée, sans étriers","OE - Plain Mounting plate W850, 7M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W850, 7M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐ LEMEZ W850, 7M, VÍZSZINTES, HORGANYOZOTT, TÁMASZOK NÉLKÜL"]
["33798","ZENERGY - PŁYTA MONTAŻOWA PEŁNA W850, 8M, POZIOMA, OCYNK, BEZ WSPORNIKÓW",245.2,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988337988","OE - Plaque de montage complète L850, 8M, horizontale, galvanisée, sans étriers","OE - Plain Mounting plate W850, 8M, Horizontal, Galvanized, without brackets","OE- PLACA MONTAJE  PARCIAL CIEGA W850, 8M, HORIZ. SIN SOPORT.","ZENERGY - TELJES RÖGZÍTŐLEMEZ W850, 8M, VÍZSZINTES, HORGANYOZOTT, TÁMASZOK NÉLKÜL"]
["33809","ZENERGY - POKRYWA GÓRNA IP43/55, W1000, D800, z przepustem pod kable Prawy",709.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338091","OE - CAPOT SUPÉRIEUR IP43/55, L1000, P800, avec presse-étoupe Droit","OE - Top cover IP43/55, W1000, D800, with cable gland Right","*OE - CUBIERTA SUPERIOR IP43/55, W1000, D800, con prensaestopas Derecha","ZENERGY - FELSŐ BURKOLAT IP43/55, W1000, D800, kábelbemenettel jobb"]
["33813","ZENERGY - POKRYWA GÓRNA IP43/55, W1300, D800",503.8,"1-ZE-01",null,null,"OE_COVERS","31813","SZT","85389099",null,null,"5901988338138","OE - Capot supérieur IP43 / 55, L1300, P800","OE - Top cover IP43 / 55, W1300, D800","OE- TECHO IP43/55, W1300, D800","ZENERGY - FELSŐ BURKOLAT IP43/55, W1300, D800"]
["33817","ZENERGY - POKRYWA GÓRNA IP43/55, W850+200, D800",440,"1-ZE-01",null,null,"OE_COVERS","31817","SZT","85389099",null,null,"5901988338176","OE - Capot supérieur IP43/55, L850+200, P800","OE - Top cover IP43 / 55, W850 + 200, D800","OE- TECHO IP43/55, W850 + 200, D800","ZENERGY – FELSŐ BURKOLAT IP43/55, W850+200, D800"]
["33820","ZENERGY - POKRYWA GÓRNA IP43/55, W850+450, D800",503.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338206","OE - Capot supérieur IP43 / 55, L850 + 450, P800","OE - Top cover IP43 / 55, W850 + 450, D800","OE- TECHO IP43/55, W850+450, D800","ZENERGY – FELSŐ BURKOLAT IP43/55, W850+450, D800"]
["33828","ZENERGY - POKRYWA GÓRNA IP43/55, W150+850+400, D800",533.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338282","OE - Capot supérieur IP43 / 55, L150 + 850 + 400, P800","OE - Top cover IP43 / 55, W150 + 850 + 400, D800","OE- TECHO IP43/55, W150+850+400, D800","ZENERGY – FELSŐ BURKOLAT IP43/55, W150+850+400, D800"]
["33833","ZENERGY - POKRYWA GÓRNA IP43/55, W200+650+400, D800",490.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338336","OE - Capot supérieur IP43 / 55, L200 + 650 + 400, P800","OE - Top cover IP43 / 55, W200 + 650 + 400, D800","OE- TECHO IP43/55, W200+650+400, D800","ZENERGY – FELSŐ BURKOLAT IP43/55, W200+650+400, D800"]
["33845","ZENERGY - POKRYWA GÓRNA IP43/55, W450, D800",264,"1-ZE-01",8.3333333333333329E-2,1,"OE_COVERS","31845","SZT","85389099",null,null,"5901988338459","OE - Capot supérieur IP43 / 55, L450, P800","OE - Top cover IP43 / 55, W450, D800","OE- TECHO IP43/55, W450, D800","ZENERGY - FELSŐ BURKOLAT IP43/55, W450, D800"]
["33846","ZENERGY - POKRYWA GÓRNA IP43/55, W450, D800, z przepustem pod kable",435.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338466","OE - CAPOT SUPÉRIEUR IP43/55, L450, P800, avec presse-étoupe","OE - Top cover IP43/55, W450, D800, with cable gland","*OE - CUBIERTA SUPERIOR IP43/55, W450, D800, con prensaestopas","ZENERGY - FELSŐ BURKOLAT IP43/55, W450, D800, kábelbemenettel"]
["33865","ZENERGY - POKRYWA GÓRNA IP43/55, W650, D800",320.10000000000002,"1-ZE-01",9.166666666666666E-2,2,"OE_COVERS","31865","SZT","85389099","27.12.40.0",null,"5901988338657","OE - Capot supérieur IP43 / 55, L650, P800","OE - Top cover IP43 / 55, W650, D800","OE- TECHO IP43/55, W650, D800","ZENERGY - FELSŐ BURKOLAT IP43/55, W650, D800"]
["33879","ZENERGY - POKRYWA GÓRNA IP43/55, W800, D800, z przepustem pod kable Lewy",609.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338794","OE - CAPOT SUPÉRIEUR IP43/55, L800, P800, avec presse-étoupe Gauche","OE - Top cover IP43/55, W800, D800, with cable gland Left","*OE - CUBIERTA SUPERIOR IP43/55, W800, D800, con prensaestopas Izquierda","ZENERGY - FELSŐ BURKOLAT IP43/55, W800, D800, perselyekkelezt a bal kábelek alatt"]
["33882","ZENERGY - POKRYWA GÓRNA IP43/55, W800, D800, z przepustem pod kable Prawy",609.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988338824","OE - CAPOT SUPÉRIEUR IP43/55, L800, P800, avec presse-étoupe Droit","OE - Top cover IP43/55, W800, D800, with cable gland Right","*OE - CUBIERTA SUPERIOR IP43/55, W800, D800, con prensaestopas Derecha","ZENERGY - FELSŐ BURKOLAT IP43/55, W800, D800, kábelbemenettel jobb"]
["33886","ZENERGY - POKRYWA GÓRNA IP43/55, W650+200, D800",378.4,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","31885","SZT","85389099",null,null,"5901988338862","OE - Capot supérieur IP43 / 55, L650 + 200, P800","OE - Top cover IP43 / 55, W650 + 200, D800","OE- TECHO IP43/55, W650+200, D800","ZENERGY – FELSŐ BURKOLAT IP43/55, W650+200, D800"]
["34000","ZENERGY -",48.2,"1-ZE-01",null,null,null,null,"SZT","85389099","27.12.40.0",null,null,null,null,null,"ZENERGY -"]
["34003","ZENERGY - ADAPTER DLA ANALIZATORÓW ZATABLICOWYCH 92X92MM, ORAZ DIN DO PŁYT 3M 4M 5M",115.5,"1-ZE-01",null,null,"OE_MCCB_PLATES","34003","SZT","85389099",null,null,"5901988340032","OE - Adaptateur pour analyseurs de panneau de 92x92mm et DIN pour cartes 3M 4M 5M","OE - Adapter for 92x92mm backplane analyzers, and DIN for 3M 4M 5M plates","OE- ADAPTADOR PARA ANALIZ. BACKPLANE 92X92MM, Y DIN PARA PLACAS 3M 4M 5M","ZENERGY - ADAPTER 92X92MM-ES LEMEZELEMZŐKHEZ ÉS DIN 3M 4M 5M-ES LEMEZEKHEZ"]
["34004","OE - Adapter dla Analizatorów zatablicowych 92x92mm, oraz DIN do płyt ACB",115,"1-ZE-01",null,null,"OE_ACB_PLATES","34004","SZT",null,null,"230321LK","5901988340049","OE - Adaptateur pour analyseurs de panneau de 92x92mm et DIN pour cartes ACB","OE - Adapter for 92x92mm backplane analyzers, and DIN for ACB plates","OE- ADAPTADOR PARA ANALIZ. BACKPLANE 92X92MM, Y DIN PARA PLACAS ACB","OE - Adapter 92x92 mm-es tábla mögötti analizátorokhoz és DIN az ACB kártyákhoz"]
["34021","ZENERGY - OSŁONA CZOŁOWA DLA MCCB 3P Z ANALIZATOREM, WYKONANIE SPECJALNE, W650, 4M / 500, POZIOMO",70,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340216","OE - Couvercle frontal pour MCCB 3P avec analyseur, modèle spécial, L650, 4M / 500, horizontal","OE - Front cover for MCCB 3P with analyzer, special version, W650, 4M / 500, Horizontal","ZEN- TAPA TROQ. PARA CAJA MOLD. 3P + ANALIZ. DE REDES, TROQUEL ESPECIAL, W650, 4M / 500, HORIZ.","ZENERGY - ELSŐ BURKOLAT MCCB 3P-HOZ ELEMZŐVEL, SPECIÁLIS VÁLTOZAT, W650, 4M / 500, VÍZSZINTES"]
["34025","ZENERGY - OSŁONA CZOŁOWA DLA MCCB 4P Z ANALIZATOREM, WYKONANIE SPECJALNE, W650, 4M / 500, POZIOMO",70,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340254","OE - Couvercle frontal pour MCCB 4P avec analyseur, modèle spécial, L650, 4M / 500, horizontal","OE - Front cover for MCCB 4P with analyzer, special version, W650, 4M / 500, Horizontal","ZEN- TAPA TROQ. PARA CAJA MOLD. 4P + ANALIZ. DE REDES, TROQUEL ESPECIAL, W650, 4M / 500, HORIZ.","ZENERGY - ELSŐ BURKOLAT MCCB 4P-HOZ ELEMZŐVEL, SPECIÁLIS VÁLTOZAT, W650, 4M / 500, VÍZSZINTES"]
["34030","ZENERGY - OSŁONA CZOŁOWA DLA MCCB 3P Z ANALIZATOREM, WYKONANIE SPECJALNE, W850, 3M / 700, POZIOMO",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340308","OE - Couvercle frontal pour MCCB 3P avec analyseur, modèle spécial, L850, 3M / 700, horizontal","OE - Front cover for MCCB 3P with analyzer, special version, W850, 3M / 700, Horizontal","ZEN- TAPA TROQ. PARA CAJA MOLD. 3P + ANALIZ. DE REDES, TROQUEL ESPECIAL, W850, 3M / 700, HORIZ.","ZENERGY - ELSŐ BURKOLAT MCCB 3P-HOZ ELEMZŐVEL, SPECIÁLIS VÁLTOZAT, W850, 3M / 700, VÍZSZINTES"]
["34035","ZENERGY - OSŁONA CZOŁOWA DLA MCCB 4P Z ANALIZATOREM, WYKONANIE SPECJALNE, W850, 4M / 700, POZIOMO",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340353","OE - Couvercle frontal pour MCCB 4P avec analyseur, modèle spécial, L850, 4M / 700, horizontal","OE - Front cover for MCCB 4P with analyzer, special version, W850, 4M / 700, Horizontal","ZEN- TAPA TROQ. PARA CAJA MOLD. 4P + ANALIZ. DE REDES, TROQUEL ESPECIAL, W850, 4M / 700, HORIZ.","ZENERGY - ELSŐ BURKOLAT MCCB 4P-HOZ ELEMZŐVEL, SPECIÁLIS VÁLTOZAT, W850, 4M / 700, VÍZSZINTES"]
["34038","ZENERGY - OSŁONA CZOŁOWA DLA MCCB 4P Z ANALIZATOREM, WYKONANIE SPECJALNE, W850, 7M / 700, POZIOMO",141.9,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340384","OE - Couvercle frontal pour MCCB 4P avec analyseur, modèle spécial, L850, 7M / 700, horizontal","OE - Front cover for MCCB 4P with analyzer, special version, W850, 7M / 700, Horizontal","ZEN- TAPA TROQ. PARA CAJA MOLD. 4P + ANALIZ. DE REDES, TROQUEL ESPECIAL, W850, 7M / 700, HORIZ.","ZENERGY - ELSŐ BURKOLAT MCCB 4P-HOZ ELEMZŐVEL, SPECIÁLIS VÁLTOZAT, W850, 7M / 700, VÍZSZINTES"]
["34043","ZENERGY - OSŁONA CZOŁOWA DLA NSX400-630 4P I ANALIZATORA 92X92MM, W650, 5M / 500, POZIOMO, DŹWIGNIA",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","35766","SZT","85389099",null,null,"5901988340438","OE - Flasque avant pour analyseur NSX400-630 4P et 92x92mm, L650, 5M / 500, horizontal, à levier","OE - Front cover for NSX400-630 4P and 92x92mm, W650, 5M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA ANALIZADOR NSX400-630 4P  Y 92X92MM, W650, 5M/500, HORIZ.","ZENERGY - ELSŐ BURKOLAT NSX400-630 4P ÉS 92X92MM ELEMZŐHOZ, W650, 5M / 500, VÍZSZINTES, KAR"]
["34048","ZENERGY - NIEAKTUALNE (OSŁONA CZOŁOWA OCHRONNIKA PRZEPIĘCIOWEGO B+C Z ZABEZPIECZENIEM BEZPIECZNIKOWYM 250A W650, 4M / 500)",67.3,"1-ZE-01",null,null,"03_SWITCHES_COVERS","34048","SZT","85389099",null,null,"5901988340483","OE - capot avant du parasurtenseur B + C avec protection de fusible 250A L650, 4M / 500","OE - Front cover of surge arrester B + C with fuse 250A W650, 4M / 500","OE- TAPA TROQ. DE SOBRETENSIONES B+C CON FUSIBLE 250A W650, 3M/500","ZENERGY - ELVÉGZŐ (B+C TÚLLÉVÉDŐ ELSŐ BURKOLAT BIZTOSÍTOTTÉKVÉDELEMEL 250A W650, 4M / 500)"]
["34049","ZENERGY - NIEAKTUALNE (OSŁONA CZOŁOWA OCHRONNIKA PRZEPIĘCIOWEGO B+C Z ZABEZPIECZENIEM BEZPIECZNIKOWYM 630A W650, 5M / 500)",82.3,"1-ZE-01",null,null,"03_SWITCHES_COVERS","34049","SZT","85389099",null,null,"5901988340490","OE - capot avant du parasurtenseur B + C avec protection de fusible 630A L650, 5M / 500","OE - Front cover of surge arrester B + C with fuse 630A W650, 5M / 500","OE- TAPA TROQ. DE SOBRETENSIONES B+C CON FUSIBLE 630A W650, 3M/500","ZENERGY - ELVÉGZŐ (B+C TÚLÁLLÍTÁSVÉDELEM ELSŐ BURKOLAT BIZTOSÍTÉKVÉDELEMVEL 630A W650, 5M / 500)"]
["34052","ZENERGY - OSŁONA CZOŁOWA DLA UCB160-250 3P I ANALIZATORA 92X92MM, W650, 3M / 500, POZIOMO, DŹWIGNIA",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","34052","SZT","85389099",null,null,"5901988340520","OE - Couvercle frontal pour analyseur UCB160-250 3P et 92x92mm, L650, 3M / 500, horizontal, à levier","OE - Front cover for UCB160-250 3P and analyzer 92x92mm, W650, 3M / 500, Horizontal, Lever","OE- TAPA TROQ. PARA UCB160-250 3P,  Y ANALIZ. 92X92MM, W650, 3M/500, HORIZ. ","ZENERGY - ELSŐ BURKOLAT UCB160-250 3P ÉS 92X92MM ELEMZŐHOZ, W650, 3M / 500, VÍZSZINTES, KAR"]
["34055","ZENERGY - OSŁONA CZOŁOWA DLA UCB400 4P I ANALIZATORA 92X92MM, W650, 5M / 500, POZIOMO, DŹWIGNIA",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","34055","SZT","85389099",null,null,"5901988340551","OE - Flasque avant pour UCB400 4P et 92x92mm, L650, analyseur 5M / 500, horizontal, à levier","OE - Front cover for UCB400 4P and 92x92mm, W650, 5M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UCB400 4P  Y ANALIZADOR DE REDES 92X92MM, W650, 5M/500, HORIZ. ","ZENERGY - ELSŐ BURKOLAT UCB400 4P ÉS 92X92MM ELEMZŐHOZ, W650, 5M / 500, VÍZSZINTES, KAR"]
["34061","ZENERGY - OSŁONA CZOŁOWA DLA UPB100-250 4P I ANALIZATORA 92X92MM, W650, 4M / 500, POZIOMO, DŹWIGNIA",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","34061","SZT","85389099",null,null,"5901988340612","OE - Couvercle frontal pour analyseur UPB100-250 4P et 92x92mm, L650, 4M / 500, horizontal, à levier","OE - Front cover for UPB100-250 4P and 92x92mm, W650, 4M / 500 analyzer, Horizontal, Lever","OE- TAPA TROQ. UPB100-250 4P  Y ANALIZADOR DE REDES 92X92MM, W650, 4M/500, HORIZ. ","ZENERGY - ELSŐ BURKOLAT UPB100-250 4P ÉS 92X92MM ELEMZŐHOZ, W650, 4M / 500, VÍZSZINTES, KAR"]
["34070","ZENERGY - OSŁONA CZOŁOWA DLA NSX100-250 3P I ANALIZATORA 92X92MM, W850, 3M / 700, POZIOMO, DŹWIGNIA",79,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340704","OE - Couvercle frontal pour analyseur NSX100-250 3P et 92x92mm, L850, 3M / 700, horizontal, à levier","OE - Front cover for NSX100-250 3P and 92x92mm, W850, 3M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ.NSX100-250 3P y 92x92mm, W850, 3M/700, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT NSX100-250 3P ÉS 92X92MM ELEMZŐHOZ, W850, 3M / 700, VÍZSZINTES, KAR"]
["34074","ZENERGY - ADAPTER DLA ANALIZATORÓW ZATABLICOWYCH 92X92MM, 4M / 500",127.6,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340742","OE - Adaptateur universel pour appareils de mesure + capot avant L650, 4M / 500","OE - Adapter for 92x92mm, 4M / 500 backplane analyzers","OE- Adaptador para analizadores backplane de 92x92mm, 4M/500","ZENERGY - ADAPTER BEÉPÍTETT ELEMZŐKHOZ 92X92MM, 4M / 500"]
["34081","ZENERGY - OSŁONA CZOŁOWA DLA UCB100 4P I ANALIZATORA 92X92MM, W850, 4M / 700, POZIOMO, DŹWIGNIA",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340810","OE - Couvercle frontal pour analyseur UCB100 4P et 92x92mm, L850, 4M / 700, horizontal, à levier","OE - Front cover for UCB100 4P and 92x92mm, W850, 4M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ.UCB100 4P y 92x92mm, W850, 4M/700, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT UCB100 4P ÉS 92X92MM ELEMZŐHOZ, W850, 4M / 700, VÍZSZINTES, KAR"]
["34084","ZENERGY - OSŁONA CZOŁOWA DLA UCB400 3P I ANALIZATORA 92X92MM, W850, 4M / 700, POZIOMO, DŹWIGNIA",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","34084","SZT","85389099",null,null,"5901988340841","OE - Flasque avant pour analyseur UCB400 3P et 92x92mm, L850, 4M / 700, horizontal, à levier","OE - Front cover for UCB400 3P and 92x92mm, W850, 4M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UCB400 3P Y 92X92MM, W850, 4M/700, HORIZ. ","ZENERGY - ELSŐ BURKOLAT UCB400 3P ÉS 92X92MM ELEMZŐHOZ, W850, 4M / 700, VÍZSZINTES, KAR"]
["34085","ZENERGY - OSŁONA CZOŁOWA DLA UCB400 4P I ANALIZATORA 92X92MM, W850, 5M / 700, POZIOMO, DŹWIGNIA",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","34085","SZT","85389099",null,null,"5901988340858","OE - Flasque avant pour UCB400 4P et 92x92mm, L850, analyseur 5M / 700, horizontal, à levier","OE - Front cover for UCB400 4P and 92x92mm, W850, 5M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. PARA UCB400 4P Y ANALIZ. 92X92MM, W850, 5M/700, HORIZ. ","ZENERGY - ELSŐ BURKOLAT UCB400 4P ÉS 92X92MM ELEMZŐHOZ, W850, 5M / 700, VÍZSZINTES, KAR"]
["34088","ZENERGY - OSŁONA CZOŁOWA DLA UCB1000-1250 3P I ANALIZATORA 92X92MM, W850, 6M / 700, POZIOMO, DŹWIGNIA",100.4,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340889","OE - Couvercle frontal pour analyseur UCB1000-1250 3P et 92x92mm, L850, 6M / 700, horizontal, à levier","OE - Front cover for UCB1000-1250 3P and 92x92mm, W850, 6M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. UCB1000-1250 3P y analizador 92x92mm, W850, 6M/700, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT UCB1000-1250 3P ÉS 92X92MM ELEMZŐHOZ, W850, 6M / 700, VÍZSZINTES, KAR"]
["34091","ZENERGY - OSŁONA CZOŁOWA DLA UPB100-250 4P I ANALIZATORA 92X92MM, W850, 4M / 700, POZIOMO, DŹWIGNIA",85,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988340919","OE - Couvercle frontal pour analyseur UPB100-250 4P et 92x92mm, L850, 4M / 700, horizontal, à levier","OE - Front cover for UPB100-250 4P and 92x92mm, W850, 4M / 700 analyzer, Horizontal, Lever","OE- TAPA TROQ. UPB100-250 4P y 92x92mm, W850, 4M/700, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT UPB100-250 4P ÉS 92X92MM ELEMZŐHOZ, W850, 4M / 700, VÍZSZINTES, KAR"]
["34101","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W1000, 4M, POZIOMO",236.5,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341015","OE - Couvercle avant INS250 3 / 4P, L400, 5M / 250, verticalement","OE - INS / INV100-250, W1000, 4M Mounting plate, Horizontal","OE- INS / INV100-250, W1000, PLACA MONTAJE de 4M, HORIZ.","ZENERGY - SZERELŐLEMEZ INS/INV100-250, W1000, 4M, VÍZSZINTES"]
["34104","ZENERGY - PŁYTA MONTAŻOWA INS/INV1600, W1000, 8M, PIONOWO",348.7,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341046","OE - plaque de montage INS / INV1600, L1000, 8M, verticale","OE - INS / INV1600, W1000, 8M Mounting plate, Vertical","OE- INS / INV1600, W1000, PLACA MONTAJE 8M, VERT.","ZENERGY – SZERELŐLAP INS/INV1600, W1000, 8M, FÜGGŐLEGES"]
["34109","ZENERGY - PŁYTA MONTAŻOWA 2X INS/INV320-630 RZR, W1000, 9M, POZIOMO",363,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341091","OE - plaque de montage 2x INS / INV320-630 RZR, L1000, 9M, horizontal","OE - Mounting plate 2x INS / INV320-630 RZR, W1000, 9M, Horizontal","OE- PLACA MONTAJE 2x INS / INV320-630 RZR, W1000, 9M, HORIZ.","ZENERGY - SZERELŐLEMEZ 2X INS/INV320-630 RZR, W1000, 9M, VÍZSZINTES"]
["34112","ZENERGY - OSŁONA CZOŁOWA INS/INV100-250, W1000, 4M / 850, POZIOMO",95.4,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341121","OE - capot avant INS / INV100-250, L1000, 4M / 850, horizontal","OE - INS / INV100-250, W1000, 4M / 850 Front cover, Horizontal","OE- TAPA TROQ. INS / INV100-250, W1000, 4M / 850 TAPA TROQ., HORIZ.","ZENERGY - ELSŐ BURKOLAT INS/INV100-250, W1000, 4M / 850, VÍZSZINTES"]
["34116","ZENERGY - OSŁONA CZOŁOWA INS/INV1600, W1000, 6M / 850, PIONOWO",113.3,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341169","OE - capot avant INS / INV1600, L1000, 6M / 850, vertical","OE - INS / INV1600, W1000, 6M / 850 front visor, Vertical","OE- TAPA TROQ. INS / INV1600, W1000, 6M / 850, VERT.","ZENERGY - ELSŐ BURKOLAT INS/INV1600, W1000, 6M / 850, FÜGGŐLEGES"]
["34119","ZENERGY - OSŁONA CZOŁOWA 2X INS/INV100-250 RZR, W1000, 6M / 850, POZIOMO, DŹWIGNIA",113.3,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341190","OE - capot avant 2x INS / INV100-250 RZR, L1000, 6M / 850, horizontal, levier","OE - Front cover 2x INS / INV100-250 RZR, W1000, 6M / 850, Horizontal, Lever","OE- TAPA TROQ. 2x INS/INV100-250 RZR, W1000, 6M/850, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT 2X INS/INV100-250 RZR, W1000, 6M / 850, VÍZSZINTES, KAR"]
["34124","ZENERGY - PŁYTA MONTAŻOWA NSX100-250 3/4P, W1000, 3M, PIONOWO, DŹWIGNIA",216.7,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341244","OE - Plaque de montage INS250 3 / 4P, L650, 3M, horizontale + supports","OE - Mounting plate NSX100-250 3 / 4P, W1000, 3M, Vertical, Lever","OE- PLACA MONTAJE NSX100-250 3/4P, W1000, 3M, VERT. MANETA","ZENERGY - SZERELŐLÁM NSX100-250 3/4P, W1000, 3M, FÜGGŐLEGES, KAR"]
["34128","ZENERGY - PŁYTA MONTAŻOWA NSX100-250 4P, W1000, 4M, POZIOMO, DŹWIGNIA",236.5,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341282","OE - Plaque de montage NSX100-250 4P, L1000, 4M, horizontale, levier","OE - Mounting plate NSX100-250 4P, W1000, 4M, Horizontal, Lever","OE- PLACA MONTAJE NSX100-250 4P, W1000, 4M, HORIZ. MANETA","ZENERGY - SZERELŐLAP NSX100-250 4P, W1000, 4M, VÍZSZINTES, KAR"]
["34134","ZENERGY - OSŁONA CZOŁOWA NSX100-250 3/4P, W1000, 5M / 850, PIONOWO, SILNIK, OBROTOWY",103.6,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341343","OE - Couvercle avant 2x INS630 RZR, L650, 10M / 500, horizontal, levier","OE - NSX100-250 3 / 4P Front Shield, W1000, 5M / 850, Vertical, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3 / 4P Protector frontal, W1000, 5M / 850, VERT., Motor, Giratorio","ZENERGY - ELSŐ BURKOLAT NSX100-250 3/4P, W1000, 5M / 850, FÜGGŐLEGES, MOTOROS, FORGÓ"]
["34138","ZENERGY - OSŁONA CZOŁOWA NSX100-250 3P, W1000, 3M / 850, POZIOMO, SILNIK, OBROTOWY",85.7,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341381","OE - capot avant NSX100-250 3P, L1000, 3M / 850, horizontal, moteur, rotatif","OE - NSX100-250 3P Front Hood, W1000, 3M / 850, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3P , W1000, 3M / 850, HORIZ. Motor, Giratorio","ZENERGY - ELSŐ BURKOLAT NSX100-250 3P, W1000, 3M / 850, VÍZSZINTES, MOTOROS, FORGÓ"]
["34142","ZENERGY - OSŁONA CZOŁOWA NSX100-250 4P, W1000, 4M / 850, POZIOMO, SILNIK, OBROTOWY",95.4,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341428","OE - Plaque de montage INS1600 3 / 4P, L650, 8M, verticale / horizontale + étriers","OE - NSX100-250 4P, W1000, 4M / 850 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 4P, W1000, 4M / 850, HORIZ. Motor, Giratorio","ZENERGY - ELSŐ BURKOLAT NSX100-250 4P, W1000, 4M / 850, VÍZSZINTES, MOTOROS, FORGÓ"]
["34145","ZENERGY - OSŁONA CZOŁOWA 2X NSX100-250 3/4P SZR, W1000, 7M / 850, BLOKADA PŁYTOWA, PIONOWO, SILNIK",137.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","34145","SZT","85389099",null,null,"5901988341459","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L1000, 7M / 850, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W1000, 7M / 850, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W1000, 7M/850, VERT. MOTOR","ZENERGY - ELSŐ BURKOLAT 2X NSX100-250 3/4P SZR, W1000, 7M / 850, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34150","ZENERGY - PŁYTA MONTAŻOWA NSX400-630 3P, W1000, 4M, POZIOMO, DŹWIGNIA",238.7,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341503","OE - Couvercle avant IN2500 3 / 4P, L650, 8M / 500, horizontal","OE - Mounting plate NSX400-630 3P, W1000, 4M, Horizontal, Lever","OE- PLACA MONTAJE NSX400-630 3P, W1000, 4M, HORIZ. MANETA","ZENERGY - SZERELŐLAP NSX400-630 3P, W1000, 4M, VÍZSZINTES, KAR"]
["34151","ZENERGY - PŁYTA MONTAŻOWA NSX400-630 4P, W1000, 5M, POZIOMO, DŹWIGNIA",249.7,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988341510","OE - Plaque de montage NSX400-630 4P, L1000, 5M, horizontale, levier","OE - Mounting plate NSX400-630 4P, W1000, 5M, Horizontal, Lever","OE- PLACA MONTAJE NSX400-630 4P, W1000, 5M, HORIZ. MANETA","ZENERGY - SZERELŐLAP NSX400-630 4P, W1000, 5M, VÍZSZINTES, KAR"]
["34156","ZENERGY - OSŁONA CZOŁOWA 1X NSX400-630 3/4P, W1000, 9M / 850, PIONOWO, DŹWIGNIA",171.6,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341565","OE - CAPOT AVANT 1X NSX400-630 3/4P, L1000, 9M/850, VERTICAL, LEVIER","OE - Front cover 1X NSX400-630 3/4P, W1000, 9M / 850, Vertical, Lever","*OE - CUBIERTA DELANTERA 1X NSX400-630 3/4P, W1000, 9M / 850, VERTICAL, PALANCA","ZENERGY - ELSŐ BURKOLAT 1X NSX400-630 3/4P, W1000, 9M / 850, FÜGGŐLEGES, KAR"]
["34160","ZENERGY - OSŁONA CZOŁOWA NSX400-630 3/4P, W1000, 9M / 850, PIONOWO, SILNIK, OBROTOWY",171.6,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341602","OE - Plaque de montage NS3200-INS2500, L650, 8M, verticalement + supports","OE - Front cover NSX400-630 3 / 4P, W1000, 9M / 850, Vertical, Motor, Rotary","OE- TAPA TROQ. NSX400-630 3/4P, W1000, 9M/850, VERT., Motor, Giratorio","ZENERGY - ELSŐ BURKOLAT NSX400-630 3/4P, W1000, 9M / 850, FÜGGŐLEGES, MOTOROS, FORGÓ"]
["34163","ZENERGY - OSŁONA CZOŁOWA NSX400-630 3P, W1000, 4M / 850, POZIOMO, SILNIK, OBROTOWY",95.4,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341633","OE - capot avant NSX400-630 3P, L1000, 4M / 850, horizontal, moteur, rotatif","OE - NSX400-630 3P, W1000, 4M / 850 Front Shield, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 3P, W1000, 4M / 850, HORIZ. Motor, Giratorio","ZENERGY - ELSŐ BURKOLAT NSX400-630 3P, W1000, 4M / 850, VÍZSZINTES, MOTOROS, FORGÓ"]
["34166","ZENERGY - OSŁONA CZOŁOWA NSX400-630 4P, W1000, 5M / 850, POZIOMO, DŹWIGNIA",103.5,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988341664","OE - capot avant NSX400-630 4P, L1000, 5M / 850, horizontal, levier","OE - NSX400-630 4P Front Shield, W1000, 5M / 850, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 4P TAPA TROQ., W1000, 5M / 850, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT NSX400-630 4P, W1000, 5M / 850, VÍZSZINTES, KAR"]
["34170","ZENERGY - OSŁONA CZOŁOWA 2X NSX400-630 3/4P SZR, W1000, 9M / 850, BLOKADA PŁYTOWA, PIONOWO, SILNIK",171.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","34170","SZT","85389099",null,null,"5901988341701","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L1000, 9M / 850, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W1000, 9M / 850, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX400-630 3/4P SZR, W1000, 9M/850, VERT. MOTOR","ZENERGY - ELSŐ BURKOLAT 2X NSX400-630 3/4P SZR, W1000, 9M / 850, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34279","Zenergy - Płyta montażowa NW40b-NW63, W1200, wysuwny, bez wsporników",343.9,"1-ZE-01",null,null,"OE_ACB_PLATES","34279","SZT","85389099",null,null,"5901988342791","OE - plaque de montage NW40b-NW63, L1200, debrochable, sans supports","OE - Mounting plate NW40b-NW63, W1200, withdrawable, without brackets","OE- PLACA MONTAJE NW40B-NW63, W1200, EXTRAÍBLE, SIN SOPORTES","Zenergy - Szerelőlap NW40b-NW63, W1200, kihúzható, konzolok nélkül"]
["34400","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W400, 3M, PIONOWO",112.2,"1-ZE-01",null,null,"OE_MCCB_PLATES","34400","SZT","85381000","27.12.40.0",null,"5901988344009","OE - Couvercle avant NS1600 3P, L400, 8M / 250, verticalement, de manière permanente","OE - INS / INV100-250, W400, 3M Mounting plate, Vertical","OE- PLACA MONTAJE INS / INV100-250, W400, 3M, VERT.","ZENERGY - SZERELŐLAP INS/INV100-250, W400, 3M, FÜGGŐLEGES"]
["34401","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W400, 4M, POZIOMO",132,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988344016","OE - Plaque de montage NS1600 3P, L400, 6M, verticalement, de façon permanente + supports","OE - INS / INV100-250, W400, 4M Mounting plate, Horizontal","OE- PLACA MONTAJE INS / INV100-250, W400, 4M, HORIZ.","ZENERGY - SZERELŐLEMEZ INS/INV100-250, W400, 4M, VÍZSZINTES"]
["34410","ZENERGY - PODPORA PŁYTY MONTAŻOWEJ DLA VIGI, W400",51.6,"1-ZE-01",null,null,"OE_MCCB_PLATES","34410","SZT","85389099","27.12.40.0",null,"5901988344108","OE - Support pour plaque de montage pour Vigi, L400","OE - Mounting plate support for Vigi, W400","OE- SOPORTE DE PLACA MONTAJE PARA VIGI, W400","ZENERGY - A SZERELŐLAP TARTÁSA VIGA, W400-HOZ"]
["34414","ZENERGY - OSŁONA CZOŁOWA INS/INV320-630, W400, 5M / 250, POZIOMO",68.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","34414","SZT","85389099",null,null,"5901988344146","OE - Couvercle avant NS1600 3 / 4P, L650, 8M / 500, entraînement par moteur, permanent","OE - INS / INV320-630 Front cover, W400, 5M / 250, Horizontal","OE- TAPA TROQ. INS / INV320-630, W400, 5M / 250 , HORIZ.","ZENERGY - ELSŐ BURKOLAT INS/INV320-630, W400, 5M / 250, VÍZSZINTES"]
["34426","ZENERGY - PŁYTA MONTAŻOWA NSX100-250 3/4P, W400, 3M, PIONOWO, WTYKOWY, WYSUWNY",104.3,"1-ZE-01",null,null,"OE_MCCB_PLATES","34426","SZT","85381000","27.12.40.0",null,"5901988344269","OE - Couvercle avant NT16 3 / 4P, L650, 8M / 500, en permanence","OE - Mounting plate NSX100-250 3 / 4P, W400, 3M, Vertical, plug-in, withdrawable","OE- PLACA MONTAJE NSX100-250 3/4P, W400, 3M, VERT. ENCHUFABLE, EXTRAÍBLE","ZENERGY - RÖGZÍTŐLAP NSX100-250 3/4P, W400, 3M, FÜGGŐLEGES, DUGULÓ, KIHAJTÓ"]
["34449","ZENERGY - PŁYTA MONTAŻOWA NSX400-630 3/4P, W400, 6M, PIONOWO, DŹWIGNIA",159.5,"1-ZE-01",1.6666666666666666E-2,2,"OE_MCCB_PLATES","34449","SZT","85381000","27.12.40.0",null,"5901988344498","OE - Plaque de montage NSX400-630 3 / 4P, L400, 6M, verticale, levier","OE - Mounting plate NSX400-630 3 / 4P, W400, 6M, Vertical, Lever","OE- PLACA MONTAJE NSX400-630 3/4P, W400, 6M, VERT.","ZENERGY - SZERELŐLAP NSX400-630 3/4P, W400, 6M, FÜGGŐLEGES, KAR"]
["34475","ZENERGY - PŁYTA MONTAŻOWA NS1600 3P, W400, 6M, PIONOWO, NA STAŁE, BEZ WSPORNIKÓW",173.7,"1-ZE-01",8.3333333333333329E-2,1,"OE_ACB_PLATES","34475","SZT","85389099","27.12.40.0",null,"5901988344757","OE - plaque de montage NS1600 3P, L400, 6M, verticale, permanente, sans supports","OE - Mounting plate NS1600 3P, W400, 6M, Vertical, fixed, without brackets","OE- PLACA MONTAJE NS1600 3P, W400, 6M, VERT. FIJA, SIN SOPORTES","ZENERGY - SZERELŐLAP NS1600 3P, W400, 6M, FÜGGŐLEGES, RÖGZÍTETT, KONZER NÉLKÜL"]
["34484","ZENERGY - OSŁONA CZOŁOWA NS1600 3P, W400, 8M / 250, PIONOWO, SILNIK, NA STAŁE",105.8,"1-ZE-01",null,null,"OE_ACB_COVERS","34484","SZT","85389099",null,null,"5901988344849","OE - capot avant NS1600 3P, L400, 8M / 250, vertical, moteur, permanent","OE - NS1600 3P Front Hood, W400, 8M / 250, Vertical, Motor, Fixed","OE- TAPA TROQ. NS1600 3P, W400, 8M / 250, VERT. MOTOR, FIJO","ZENERGY - ELSŐ BURKOLAT NS1600 3P, W400, 8M / 250, FÜGGŐLEGES, MOTOROS, RÖGZÍTETT"]
["34500","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W450, 3M, PIONOWO",127.6,"1-ZE-01",3.3333333333333333E-2,2,"OE_MCCB_PLATES","34500","SZT","85381000","27.12.40.0",null,"5901988345006","OE - Couvercle avant NSX250 3P, L400, 5M / 250, à la verticale, à levier","OE - INS / INV100-250, W450, 3M Mounting plate, Vertical","OE- PLACA MONTAJE INS/ INV100-250, W450, 3M, VERT.","ZENERGY – SZERELŐLAP INS/INV100-250, W450, 3M, FÜGGŐLEGES"]
["34501","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W450, 4M, POZIOMO",144.1,"1-ZE-01",null,null,"OE_MCCB_PLATES","34528","SZT","85381000","27.12.40.0",null,"5901988345013","OE - Couvercle avant NSX250 4P, L400, 5M / 250, à la verticale, à levier","OE - INS / INV100-250, W450, 4M Mounting plate, Horizontal","OE- PLACA MONTAJE INS/ INV100-250, W450, 4M, HORIZ.","ZENERGY - SZERELŐLEMEZ INS/INV100-250, W450, 4M, VÍZSZINTES"]
["34510","ZENERGY - PODPORA PŁYTY MONTAŻOWEJ DLA VIGI, W450",57.3,"1-ZE-01",null,null,"OE_MCCB_PLATES","34510","SZT","85389099","27.12.40.0",null,"5901988345105","OE - Support pour plaque de montage pour Vigi, L450","OE - Mounting plate support for Vigi, W450","OE- SOPORTE DE PLACA MONTAJE PARA VIGI, W450","ZENERGY - SZERELŐLAP TARTÓ VIGA, W450-hez"]
["34514","ZENERGY - OSŁONA CZOŁOWA INS/INV320-630, W450, 5M / 300, POZIOMO",72.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","34514","SZT","85389099",null,null,"5901988345143","OE - capot avant INS / INV320-630, L450, 5M / 300, horizontal","OE - INS / INV320-630, W450, 5M / 300 Front cover, Horizontal","OE- TAPA TROQ. INS/INV320-630, W450, 5M/300, HORIZ.","ZENERGY - ELSŐ BURKOLAT INS/INV320-630, W450, 5M / 300, VÍZSZINTES"]
["34526","ZENERGY - PŁYTA MONTAŻOWA NSX100-250 3/4P, W450, 3M, PIONOWO, WTYKOWY, WYSUWNY",118.8,"1-ZE-01",null,null,"OE_MCCB_PLATES","34526","SZT","85381000","27.12.40.0",null,"5901988345266","OE - plaque de montage NSX100-250 3 / 4P, L450, 3M, verticale, enfichable, dĂ©brochable","OE - Mounting plate NSX100-250 3 / 4P, W450, 3M, Vertical, plug-in, withdrawable","OE- PLACA MONTAJE NSX100-250 3 / 4P, W450, 3M, VERT. ENCHUFABLE, EXTRAÍBLE","ZENERGY - SZERELŐLÁM NSX100-250 3/4P, W450, 3M, FÜGGŐLEGES, DUGALOM, KIHAJTÓ"]
["34530","ZENERGY - PŁYTA MONTAŻOWA 2X NSX100-250 3/4P SZR, W450, BLOKADA PŁYTOWA, POZIOMO, SILNIK",118.8,"1-ZE-01",null,null,"OE_MCCB_PLATES","34530","SZT","85381000","27.12.40.0",null,"5901988345303","OE - plaque de montage 2x NSX100-250 SZR 3 / 4P, L450, verrouillage de plaque, horizontal, moteur","OE - Mounting plate 2x NSX100-250 3 / 4P SZR, W450, plate lock, Horizontal, Motor","OE- PLACA MONTAJE 2X NSX100-250 3/4P SZR, W450, , HORIZ., MOTOR","ZENERGY - SZERELŐLEMEZ 2X NSX100-250 3/4P SZR, W450, LEMEZZÁR, VÍZSZINTES, MOTOR"]
["34536","ZENERGY - OSŁONA CZOŁOWA 1x NSX100-250 4P, W450, 5M / 300, PIONOWO, SILNIK, OBROTOWY",74.099999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","34536","SZT","85389099",null,null,"5901988345365","OE - Capot avant 1x NSX100-250 4P, L450, 5M / 300, vertical, moteur, rotatif","OE - 1x NSX100-250 4P Front Hood, W450, 5M / 300, Vertical, Motor, Rotary","OE- 1X NSX100-250 4P COFRE DELANTERO, W450, 5M / 300, VERT. MOTOR","ZENERGY - ELSŐ BURKOLAT 1x NSX100-250 4P, W450, 5M / 300, FÜGGŐLEGES, MOTOROS, FORGÓ"]
["34541","ZENERGY - OSŁONA CZOŁOWA NSX100-250 4P, W450, 4M / 300, POZIOMO, DŹWIGNIA",62,"1-ZE-01",0.18333333333333332,2,"OE_MCCB_COVERS","34541","SZT","85389099",null,null,"5901988345419","OE - capot avant NSX100-250 4P, L450, 4M / 300, horizontal, levier","OE - NSX100-250 4P Front Hood, W450, 4M / 300, Horizontal, Lever","OE- NSX100-250 4P  W450, 4M / 300, HORIZ.","ZENERGY - ELSŐ BURKOLAT NSX100-250 4P, W450, 4M / 300, VÍZSZINTES, KAR"]
["34542","ZENERGY - OSŁONA CZOŁOWA NSX100-250 4P, W450, 4M / 300, POZIOMO, SILNIK, OBROTOWY",62,"1-ZE-01",null,null,"OE_MCCB_COVERS","34542","SZT","85389099",null,null,"5901988345426","OE - capot avant NSX100-250 4P, L450, 4M / 300, horizontal, moteur, rotatif","OE - NSX100-250 4P Front Hood, W450, 4M / 300, Horizontal, Motor, Rotary","OE- NSX100-250 4P  W450, 4M / 300, HORIZ. MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX100-250 4P, W450, 4M / 300, VÍZSZINTES, MOTOROS, FORGÓ"]
["34550","ZENERGY - PŁYTA MONTAŻOWA NSX400-630 3P, W450, 4M, POZIOMO, DŹWIGNIA",118.8,"1-ZE-01",null,null,"OE_MCCB_PLATES","34550","SZT","85381000","27.12.40.0",null,"5901988345501","OE - Couvercle avant NSX630 3P, L400, 9M / 250, vertical, levier","OE - Mounting plate NSX400-630 3P, W450, 4M, Horizontal, Lever","OE- PLACA MONTAJE NSX400-630 3P, W450, 4M, HORIZ.","ZENERGY - SZERELŐLÁM NSX400-630 3P, W450, 4M, VÍZSZINTES, KAR"]
["34557","ZENERGY - OSŁONA CZOŁOWA NSX400-630 3/4P, W450, 9M / 300, PIONOWO, SILNIK, OBROTOWY, WYSUWNY",113.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","34557","SZT","85389099",null,null,"5901988345570","OE - capot avant NSX400-630 3 / 4P, L450, 9M / 300, vertical, moteur, rotatif, dĂ©brochable","OE - Front cover NSX400-630 3 / 4P, W450, 9M / 300, Vertical, Motor, rotatable, withdrawable","OE- TAPA TROQ. NSX400-630 3 / 4P, W450, 9M / 300, VERT. MOTOR, EXTRAÍBLE","ZENERGY - ELSŐ BURKOLAT NSX400-630 3/4P, W450, 9M / 300, FÜGGŐLEGES, MOTOROS, FORGATHATÓ, CSÚSZTÓ"]
["34572","ZENERGY - PŁYTA MONTAŻOWA SIRCO1250 3P, W450, 4M, PIONOWO, BEZ WSPORNIKÓW",105.6,null,0.01,1,"OE_MCCB_PLATES",null,null,"85389099",null,null,"5901988345723"]
["34578","ZENERGY - PŁYTA MONTAŻOWA NT16, W450, NA STAŁE, BEZ WSPORNIKÓW",109.9,"1-ZE-01",null,null,"OE_ACB_PLATES","34578","SZT","85389099","27.12.40.0",null,"5901988345785","OE - plaque de montage NT16, L450, en permanence, sans Ă©triers","OE - NT16, W450 Mounting plate, permanently, without brackets","OE- PLACA MONTAJE NT16, W450, FIJA, SIN SOPORTES","ZENERGY - SZERELŐLAP NT16, W450, RÖGZÍTETT, KONZER NÉLKÜL"]
["34585","ZENERGY - OSŁONA CZOŁOWA NS1600 3/4P, W450, 8M / 300, PIONOWO, NAPĘD OBROTOWY, NA STAŁE",113.9,"1-ZE-01",null,null,"OE_ACB_COVERS","34585","SZT","85389099","27.12.40.0",null,"5901988345853","OE - capot avant NS1600 3 / 4P, L450, 8M / 300, vertical, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W450, 8M / 300, Vertical, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P W450, 8M / 300, VERT. ACCIONAMIENTO , FIJO","ZENERGY - ELSŐ BURKOLAT NS1600 3/4P, W450, 8M / 300, FÜGGŐLEGES, FORGÓHAJTÁS, RÖGZÍTETT"]
["34610","ZENERGY - OSŁONA CZOŁOWA PEŁNA W600, 1M / 450",44,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988346102","OE - Couverture avant complète L600, 1M / 450","OE - Plain Front cover W600, 1M / 450","OE- TAPA FRONTAL CIEGA  W600, 1M (H 50MM)","ZENERGY - TELJES ELSŐ BURKOLAT W600, 1M / 450"]
["34625","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W600, 2M / 450, 21 MOD",48.8,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS",null,"SZT","85389099",null,null,"5901988346256","OE - Couvercle pour appareil modulaire L600, 2M / 450, 21 mod","OE - Modular equipment cover W600, 2M / 450, 21 mod","OE-TAPA MODULAR W600, 2M (H 100MM) 21 MOD","ZENERGY - W600 MODULÁRIS BERENDEZÉS BURKOLAT, 2M / 450, 21 MOD"]
["34628","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W600, 2M / 450",57,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988346287","OE - Panneau avant perforé L600, 2M / 450","OE - Perforated Front cover W600, 2M / 450","OE- TAPA FRONTAL VENTILADA W600, 2M (H 100MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W600, 2M / 450"]
["34639","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W600, 3M / 450",200.1,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS",null,"SZT","85389099",null,null,"5901988346393","OE - Couvercle transparent L600, 3M / 450","OE - Transparent Front cover W600, 3M / 450","OE- TAPA FRONTAL TRANSPARENTE W600, 3M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W600, 3M / 450"]
["34641","ZENERGY - OSŁONA CZOŁOWA W600, 4M / 450, OTW. 92X92",60.2,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988346416","OE - Cache avant complet L600, 4M / 450, ouvert 92x92","OE - W600, 4M / 450 Front cover, open. 92x92","OE- TAPA FRONTAL CIEGA  W600, 4M (H 200MM) CON AGUJERO 92X92","ZENERGY - ELSŐ BURKOLAT W600, 4M / 450, NYITOTT. 92X92"]
["34650","ZENERGY - OSŁONA CZOŁOWA PEŁNA W600, 5M / 450",67,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988346508","OE - Couverture avant complète L600, 5M / 450","OE - Plain Front cover W600, 5M / 450","OE- TAPA FRONTAL CIEGA  W600, 5M (H 250MM)","ZENERGY - TELJES ELSŐ BURKOLAT W600, 5M / 450"]
["34658","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W600, 5M / 450",80,"1-ZE-01",null,null,"01_PERFORATED_COVERS",null,"SZT","85389099",null,null,"5901988346584","OE - Panneau avant perforé L600, 5M / 450","OE - Perforated Front cover W600, 5M / 450","OE- TAPA FRONTAL VENTILADA W600, 5M (H 250MM)","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W600, 5M / 450"]
["34669","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W600, 8M / 450",265.7,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS",null,"SZT","85389099",null,null,"5901988346690","OE - Couvercle transparent L600, 8M / 450","OE - Transparent Front cover W600, 8M / 450","OE- TAPA FRONTAL TRANSPARENTE W600, 8M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W600, 8M / 450"]
["34680","ZENERGY - OSŁONA CZOŁOWA PEŁNA W600, 8M / 450",105.2,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988346805","OE - Couverture avant complète L600, 8M / 450","OE - Plain Front cover W600, 8M / 450","OE- TAPA FRONTAL CIEGA  W600, 8M (H 400MM)","ZENERGY - TELJES ELSŐ BURKOLAT W600, 8M / 450"]
["34691","ZENERGY - OSŁONA CZOŁOWA PEŁNA W600, 10M / 450",121,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988346911","OE - Couverture avant complète L600, 10M / 450","OE - Plain Front cover W600, 10M / 450","OE- TAPA FRONTAL CIEGA  W600, 10M (H 500MM)","ZENERGY - TELJES ELSŐ BURKOLAT W600, 10M / 450"]
["34692","ZENERGY - OSŁONA CZOŁOWA PEŁNA W600, 11M / 450",124.3,"1-ZE-01",null,null,"01_PLAIN_COVERS",null,"SZT","85389099",null,null,"5901988346928","OE - Couverture avant complète L600, 11M / 450","OE - Plain Front cover W600, 11M / 450","OE- TAPA FRONTAL CIEGA  W600, 11M (H 550MM)","ZENERGY - TELJES ELSŐ BURKOLAT W600, 11M / 450"]
["34699","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W600, 12M / 450",316.3,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS",null,"SZT","85389099",null,null,"5901988346997","OE - Couvercle transparent L600, 12M / 450","OE - Transparent Front cover W600, 12M / 450","OE- TAPA FRONTAL TRANSPARENTE W600, 12M ","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W600, 12M / 450"]
["34702","ZENERGY - PŁYTA MONTAŻOWA INS/INV320-630, 2X INS/INV320-630 RZR, W650, 4M, PIONOWO",174.9,"1-ZE-01",0.01,1,"OE_MCCB_PLATES","34702","SZT","85381000","27.12.40.0",null,"5901988347024","OE - plaque de montage INS / INV320-630, 2x INS/INV320-630 RZR, L650, 4M, verticale","OE - Mounting plate INS / INV320-630, 2x INS / INV320-630 RZR, W650, 4M, Vertical","OE- PLACA MONTAJE INS/INV320-630, 2X INS/INV320-630 RZR, W650, 4M, VERT.","ZENERGY - SZERELŐLEMEZ INS/INV320-630, 2X INS/INV320-630 RZR, W650, 4M, FÜGGŐLEGES"]
["34706","ZENERGY - PŁYTA MONTAŻOWA 2X INS/INV100-250 RZR, W650, 3M, PIONOWO",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_PLATES","34706","SZT","85381000","27.12.40.0",null,"5901988347062","OE - plaque de montage 2x INS / INV100-250 RZR, L650, 3M, vertical","OE - Mounting plate 2x INS / INV100-250 RZR, W650, 3M, Vertical","OE- PLACA MONTAJE 2X INS / INV100-250 RZR, W650, 3M, VERT.","ZENERGY - SZERELŐLEMEZ 2X INS/INV100-250 RZR, W650, 3M, FÜGGŐLEGES"]
["34710","ZENERGY - PODPORA PŁYTY MONTAŻOWEJ DLA VIGI, W650",64.599999999999994,"1-ZE-01",null,null,"OE_MCCB_PLATES","34710","SZT","85389099","27.12.40.0",null,"5901988347109","OE - Support de plaque de montage pour Vigi, L650","OE - Mounting plate support for Vigi, W650","OE- SOPORTE DE PLACA MONTAJE PARA VIGI, W650","ZENERGY - SZERELŐLAP TARTÓ VIGA, W650-hez"]
["34714","ZENERGY - OSŁONA CZOŁOWA INS/INV320-630, W650, 5M / 500, POZIOMO",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","34714","SZT","85389099","27.12.40.0",null,"5901988347147","OE - capot avant INS / INV320-630, L650, 5M / 500, horizontal","OE - INS / INV320-630, W650, 5M / 500 Front cover, Horizontal","OE- TAPA TROQ. INS/INV320-630, W650, 5M/500, HORIZ.","ZENERGY - ELSŐ BURKOLAT INS/INV320-630, W650, 5M / 500, VÍZSZINTES"]
["34718","ZENERGY - OSŁONA CZOŁOWA 2X INS/INV100-250 RZR, W650, 5M / 500, PIONOWO, DŹWIGNIA",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","34718","SZT","85389099","27.12.40.0",null,"5901988347185","OE - capot avant 2x INS / INV100-250 RZR, L650, 5M / 500, vertical, levier","OE - Front cover 2x INS / INV100-250 RZR, W650, 5M / 500, Vertical, Lever","OE- TAPA TROQ. 2X INS / INV100-250 RZR, W650, 5M / 500, VERT.","ZENERGY - ELSŐ BURKOLAT 2X INS/INV100-250 RZR, W650, 5M / 500, FÜGGŐLEGES, KAR"]
["34721","ZENERGY - OSŁONA CZOŁOWA 2X INS/INV320-630 RZR, W650, 10M / 500, POZIOMO",150.69999999999999,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988347215","OE - capot avant 2x INS / INV320-630 RZR, L650, 10M / 500, horizontal","OE - Front cover 2x INS / INV320-630 RZR, W650, 10M / 500, Horizontal","OE- TAPA TROQ. 2x INS / INV320-630 RZR, W650, 10M / 500, HORIZ.","ZENERGY - ELSŐ BURKOLAT 2X INS/INV320-630 RZR, W650, 10M / 500, VÍZSZINTES"]
["34722","ZENERGY - PŁYTA MONTAŻOWA 5/4x NSXm100-160 3/4P, W650, 3M, PIONOWO, DŹWIGNIA",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_PLATES","34722","SZT","85389099","27.12.40.0",null,"5901988347222","OE - PLAQUE DE MONTAGE 5/4x NSXm100-160 3/4P, L650, 3M, VERTICAL, LEVIER","OE - Mounting plate 5 / 4x NSXm100-160 3 / 4P, W650, 3M, Vertical, Lever","OE- PLACA MONTAJE 5/4X NSXM100-160 3/4P, W650, 3M, VERT.","ZENERGY - SZERELŐLÁM 5/4x NSXm100-160 3/4P, W650, 3M, FÜGGŐLEGES, KAR"]
["34726","ZENERGY - PŁYTA MONTAŻOWA 4/3X NSX100-250 3/4P, W650, 3M, PIONOWO, WTYKOWY, WYSUWNY",146.30000000000001,"1-ZE-01",0.01,1,"OE_MCCB_PLATES","34726","SZT","85381000","27.12.40.0",null,"5901988347260","OE - plaque de montage 4 / 3x NSX100-250 3 / 4P, L650, 3M, verticale, enfichable, dĂ©brochable","OE - Mounting plate 4 / 3x NSX100-250 3 / 4P, W650, 3M, Vertical, plug-in, withdrawable","OE- PLACA MONTAJE 4 / 3X NSX100-250 3 / 4P, W650, 3M, VERT. ENCHUFABLE, EXTRAÍBLE","ZENERGY - RÖGZÍTŐLEMEZ 4/3X NSX100-250 3/4P, W650, 3M, FÜGGŐLEGES, DUGALOM, KIHAJTÓ"]
["34729","ZENERGY - PŁYTA MONTAŻOWA 2X: NSX100-250 3/4P, NSX400-630 3/4P SZR, W650, BLOKADA PŁYTOWA, PIONOWO, SILNIK",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_PLATES","34729","SZT","85381000","27.12.40.0",null,"5901988347291","OE - plaque de montage 2x NSX100-250, NSX400-630 SZR 3 / 4P, L650, verrouillage de plaque, vertical, moteur","OE - Mounting plate 2x NSX100-250 3 / 4P, NSX400-630 3 / 4P SZR, W650, plate lock, Vertical, Motor","OE- PLACA MONTAJE 2X NSX100-250 3/4P, NSX400-630 3/4P SZR, W650, , VERT. MOTOR","ZENERGY - SZERELŐLEMEZ 2X: NSX100-250 3/4P, NSX400-630 3/4P SZR, W650, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34735","ZENERGY - OSŁONA CZOŁOWA 4/3X NSX100-250 VIGI 3/4P, W650, 7M / 500, PIONOWO, DŹWIGNIA",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","34735","SZT","85389099","27.12.40.0",null,"5901988347352","OE - capot avant 4 / 3x NSX100-250 VIGI 3 / 4P, L650, 7M / 500, vertical, levier","OE - Front cover 4 / 3x NSX100-250 VIGI 3 / 4P, W650, 7M / 500, Vertical, Lever","OE- TAPA TROQ. 4 / 3X NSX100-250 VIGI 3 / 4P, W650, 7M / 500, VERT.","ZENERGY - ELSŐ BURKOLAT 4/3X NSX100-250 VIGI 3/4P, W650, 7M / 500, FÜGGŐLEGES, KAR"]
["34738","ZENERGY - OSŁONA CZOŁOWA NSX100-250 3P, W650, 3M / 500, POZIOMO, SILNIK, OBROTOWY",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","34738","SZT","85389099","27.12.40.0",null,"5901988347383","OE - capot avant NSX100-250 3P, L650, 3M / 500, horizontal, moteur, rotatif","OE - NSX100-250 3P Front Hood, W650, 3M / 500, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3P  W650, 3M / 500, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX100-250 3P, W650, 3M / 500, VÍZSZINTES, MOTOROS, FORGÓ"]
["34742","ZENERGY - OSŁONA CZOŁOWA NSX100-250 4P, W650, 4M / 500, POZIOMO, SILNIK, OBROTOWY",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","34742","SZT","85389099","27.12.40.0",null,"5901988347420","OE - capot avant NSX100-250 4P, L650, 4M / 500, horizontal, moteur, rotatif","OE - NSX100-250 4P, W650, 4M / 500 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 4P, W650, 4M / 500, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX100-250 4P, W650, 4M / 500, VÍZSZINTES, MOTOROS, FORGÓ"]
["34746","ZENERGY - OSŁONA CZOŁOWA 2X NSX100-250 3/4P SZR, W650, 8M / 500, BLOKADA PŁYTOWA, POZIOMO, SILNIK",138.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","34746","SZT","85389099","27.12.40.0",null,"5901988347468","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L650, 8M / 500, verrou de plaque, horizontal, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W650, 8M / 500, plate lock, Horizontal, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W650, 8M/500,  HORIZ., MOTOR","ZENERGY - ELSŐ BURKOLAT 2X NSX100-250 3/4P SZR, W650, 8M / 500, LEMEZZÁR, VÍZSZINTES, MOTOR"]
["34751","ZENERGY - PŁYTA MONTAŻOWA NSX400-630 4P, W650, 5M, POZIOMO, DŹWIGNIA",189.2,"1-ZE-01",null,null,"OE_MCCB_PLATES","34751","SZT","85381000","27.12.40.0",null,"5901988347512","OE - Plaque de montage NSX400-630 4P, L650, 5M, horizontale, levier","OE - Mounting plate NSX400-630 4P, W650, 5M, Horizontal, Lever","OE- PLACA MONTAJE NSX400-630 4P, W650, 5M, HORIZ.","ZENERGY - SZERELŐLAP NSX400-630 4P, W650, 5M, VÍZSZINTES, KAR"]
["34752","produkt wycofany (patrz ref.ZENE34729)",156.1,"1-ZE-01",null,null,null,null,"SZT","85381000","27.12.40.0",null,null,null,null,null,"megszűnt termék (lásd a ZENE34729 hivatkozást)"]
["34756","ZENERGY - OSŁONA CZOŁOWA 1X NSX400-630 3/4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","34756","SZT","85389099",null,null,"5901988347567","OE - capot avant 1x NSX400-630 3 / 4P, L650, 9M / 500, vertical, levier","OE - 1x NSX400-630 3 / 4P Front cover, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. 1X NSX400-630 3/4P, W650, 9M/500, VERT.","ZENERGY - ELSŐ BURKOLAT 1X NSX400-630 3/4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["34760","ZENERGY - OSŁONA CZOŁOWA 2X NSX400-630 3/4P, W650, 9M / 500, PIONOWO, SILNIK, OBROTOWY",144.1,"1-ZE-01",1.6666666666666666E-2,1,"OE_MCCB_COVERS","34760","SZT","85389099","27.12.40.0",null,"5901988347604","OE - capot avant 2x NSX400-630 3 / 4P, L650, 9M / 500, vertical, moteur, rotatif","OE - Front cover 2x NSX400-630 3 / 4P, W650, 9M / 500, Vertical, Motor, rotary","OE- TAPA TROQ. 2X NSX400-630 3/4P, W650, 9M/500, VERT. MOTOR, ROTATIVO","ZENERGY - ELSŐ BURKOLAT 2X NSX400-630 3/4P, W650, 9M / 500, FÜGGŐLEGES, MOTOROS, FORGÓ"]
["34763","ZENERGY - OSŁONA CZOŁOWA NSX400-630 3P, W650, 4M / 500, POZIOMO, SILNIK, OBROTOWY",74.5,"1-ZE-01",1.6666666666666666E-2,1,"OE_MCCB_COVERS","34763","SZT","85389099","27.12.40.0",null,"5901988347635","OE - capot avant NSX400-630 3P, L650, 4M / 500, horizontal, moteur, rotatif","OE - NSX400-630 3P, W650, 4M / 500 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 3P, W650, 4M / 500, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX400-630 3P, W650, 4M / 500, VÍZSZINTES, MOTOROS, FORGÓ"]
["34766","ZENERGY - OSŁONA CZOŁOWA NSX400-630 4P, W650, 5M / 500, POZIOMO, DŹWIGNIA",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","34766","SZT","85389099","27.12.40.0",null,"5901988347666","OE - capot avant NSX400-630 4P, L650, 5M / 500, horizontal, levier","OE - NSX400-630 4P Front Hood, W650, 5M / 500, Horizontal, Lever","OE-TAPA TROQ.  NSX400-630 4P  W650, 5M / 500, HORIZ.","ZENERGY - ELSŐ BURKOLAT NSX400-630 4P, W650, 5M / 500, VÍZSZINTES, KAR"]
["34770","ZENERGY - OSŁONA CZOŁOWA 2X NSX400-630 3/4P SZR, W650, 9M / 500, BLOKADA PŁYTOWA, PIONOWO, SILNIK",144.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","34770","SZT","85389099","27.12.40.0",null,"5901988347703","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L650, 9M / 500, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W650, 9M / 500, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX400-630 3/4P SZR, W650, 9M/500,  VERT. MOTOR","ZENERGY - ELSŐ BURKOLAT 2X NSX400-630 3/4P SZR, W650, 9M / 500, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34773","ZENERGY - OSŁONA CZOŁOWA UA/BA, W650, 4M / 500, POZIOMO, DŹWIGNIA",73.099999999999994,"1-ZE-01",0.01,1,"OE_EQUIPMENT_COVERS","34773","SZT","85389099",null,null,"5901988347734","OE - Capot avant UA/BA, L650, 4M / 500","OE - Front visor UA / BA, W650, 4M / 500","OE- TAPA TROQ. UA/BA, W650, 4M/500","ZENERGY - ELSŐ BURKOLAT UA/BA, W650, 4M / 500, VÍZSZINTES, KAR"]
["34776","ZENERGY - PŁYTA MONTAŻOWA NS1600, W650, 7M, POZIOMO, NA STAŁE",286.39999999999998,"1-ZE-01",null,null,"OE_ACB_PLATES","34776","SZT","85389099","27.12.40.0",null,"5901988347765","OE - plaque de montage NS1600, L650, 7M, horizontale, permanente","OE - Mounting plate NS1600, W650, 7M, Horizontal, fixed","OE- PLACA MONTAJE NS1600, W650, 7M, HORIZ., FIJA","ZENERGY - SZERELŐLAP NS1600, W650, 7M, VÍZSZINTES, RÖGZÍTETT"]
["34777","ZENERGY - PŁYTA MONTAŻOWA NS1600/NT16, W650, WYSUWNY, BEZ WSPORNIKÓW",211.6,"1-ZE-01",0.1,1,"OE_ACB_PLATES","34777","SZT","85389099","27.12.40.0",null,"5901988347772","OE - plaque de montage NS1600 / NT16, L650, dĂ©brochable, sans supports","OE - Mounting plate NS1600 / NT16, W650, withdrawable, without brackets","OE- PLACA MONTAJE NS1600 / NT16, W650, EXTRAÍBLE, SIN SOPORTES","ZENERGY - SZERELŐLAP NS1600/NT16, W650, CSÚSZTÓ, KONZER NÉLKÜL"]
["34780","ZENERGY - PŁYTA MONTAŻOWA NW40, W650, NA STAŁE, BEZ WSPORNIKÓW",315.10000000000002,"1-ZE-01",null,null,"OE_ACB_PLATES","34780","SZT","85389099","27.12.40.0",null,"5901988347802","OE - plaque de montage NW40, L650, en permanence, sans Ă©triers","OE - Mounting plate NW40, W650, permanently, without brackets","OE- PLACA MONTAJE NW40, W650, FIJA, SIN SOPORTES","ZENERGY - SZERELŐLAP NW40, W650, RÖGZÍTETT, KONZER NÉLKÜL"]
["34786","ZENERGY - OSŁONA CZOŁOWA NS1600 3/4P, W650, 7M / 500, POZIOMO, DŹWIGNIA, NA STAŁE",134.6,"1-ZE-01",0.01,1,"OE_ACB_COVERS","34786","SZT","85389099","27.12.40.0",null,"5901988347864","OE - capot avant NS1600 3 / 4P, L650, 7M / 500, horizontal, levier, en permanence","OE - NS1600 3 / 4P front visor, W650, 7M / 500, Horizontal, Lever, fixed","OE- TAPA TROQ. NS1600 3 / 4P, W650, 7M / 500, HORIZ., FIJA","ZENERGY - ELSŐ BURKOLAT NS1600 3/4P, W650, 7M / 500, VÍZSZINTES, KAROS, RÖGZÍTETT"]
["34789","ZENERGY - OSŁONA CZOŁOWA NS1600/NT16 3/4P, W650, 7M / 500, WYSUWNY",153,"1-ZE-01",8.3333333333333329E-2,1,"OE_ACB_COVERS","34789","SZT","85389099","27.12.40.0",null,"5901988347895","OE - Face avant NS1600/NT16 3/4P, L650, 7M / 500, coulissant","OE - Front cover NS1600 / NT16 3 / 4P, W650, 7M / 500, withdrawable","OE- TAPA TROQ. NS1600/NT16 3/4P, W650, 7M/500, EXTRAÍBLE","ZENERGY - ELSŐ BURKOLAT NS1600/NT16 3/4P, W650, 7M / 500, CSÚSZTÓ"]
["34792","ZENERGY - OSŁONA CZOŁOWA NW40 3/4P, W650, 8M / 500, PIONOWO, NA STAŁE",240.4,"1-ZE-01",0.15,2,"OE_ACB_COVERS","34792","SZT","85389099","27.12.40.0",null,"5901988347925","OE - capot avant NW40 3 / 4P, L650, 8M / 500, vertical, permanent","OE - NW40 3 / 4P, W650, 8M / 500 front visor, Vertical, fixed","OE- TAPA TROQ. NW40 3/4P, W650, 8M/500, VERT. FIJA","ZENERGY - ELSŐ BURKOLAT NW40 3/4P, W650, 8M / 500, FÜGGŐLEGES, RÖGZÍTETT"]
["34825","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W800, 2M / 650, 32 MOD",53.6,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","34825","SZT","85389099",null,null,"5901988348250","OE - Couverture d'appareil modulaire L800, 2M / 650, 32 mod","OE - Modular equipment cover W800, 2M / 650, 32 mod","OE- TAPA MODULAR W800, 2M / 650, 32 MOD","ZENERGY - W800 MODULÁRIS BERENDEZÉS BURKOLAT, 2M / 650, 32 MOD"]
["34835","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W800, 3M / 650, 32 MOD",61.2,"1-ZE-01",0.14166666666666666,1,"02_DIN_RAIL_COVERS","34835","SZT","85389099",null,null,"5901988348359","OE - Couvercle pour appareil modulaire L800, 3M / 650, 32 mod","OE - Modular equipment cover W800, 3M / 650, 32 mod","OE- TAPA MODULAR W800, 3M / 650, 32 MOD","ZENERGY - MODULÁRUS BERENDEZÉSBURKOLAT W800, 3M / 650, 32 MOD"]
["34838","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W800, 3M / 650",71.099999999999994,"1-ZE-01",null,null,"01_PERFORATED_COVERS","34838","SZT","85389099",null,null,"5901988348380","OE - Panneau avant perforé L800, 3M / 650","OE - Perforated Front cover W800, 3M / 650","OE- TAPA TROQ.  W800, 3M / 650","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W800, 3M / 650"]
["34845","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W800, 4M / 650, 32 MOD",68.5,"1-ZE-01",0.20833333333333334,1,"02_DIN_RAIL_COVERS","34845","SZT","85389099",null,null,"5901988348458","OE - Couvercle pour appareil modulaire L800, 4M / 650, 32 mod","OE - Modular equipment cover W800, 4M / 650, 32 mod","OE- TAPA MODULAR W800, 4M / 650, 32 MOD","ZENERGY - W800 MODULÁRUS BERENDEZÉSBURKOLAT, 4M / 650, 32 MOD"]
["34858","ZENERGY - OSŁONA CZOŁOWA PERFOROWANA W800, 5M / 650",91.3,"1-ZE-01",null,null,"01_PERFORATED_COVERS","34858","SZT","85389099",null,null,"5901988348588","OE - Panneau avant perforé L800, 5M / 650","OE - Perforated Front cover W800, 5M / 650","OE- TAPA TROQ.  W800, 5M / 650","ZENERGY - PERFORÁLT ELSŐ BURKOLAT W800, 5M / 650"]
["34865","ZENERGY - OSŁONA APARATURY MODUŁOWEJ W800, 6M / 650, 32 MOD",81.2,"1-ZE-01",null,null,"02_DIN_RAIL_COVERS","34865","SZT","85389099",null,null,"5901988348656","OE - Couverture d'appareil modulaire L800, 6M / 650, 32 mod","OE - Modular equipment cover W800, 6M / 650, 32 mod","OE- TAPA MODULAR W800, 6M / 650, 32 MOD","ZENERGY - W800 MODULÁRUS BERENDEZÉSBURKOLAT, 6M / 650, 32 MOD"]
["34870","ZENERGY - OSŁONA CZOŁOWA PEŁNA W800, 7M / 650",108.9,"1-ZE-01",null,null,"01_PLAIN_COVERS","34870","SZT","85389099",null,null,"5901988348700","OE - Couverture avant complète L800, 7M / 650","OE - Plain Front cover W800, 7M / 650","OE- TAPA TROQ. CIEGA W800, 7M / 650","ZENERGY - TELJES ELSŐ BURKOLAT W800, 7M / 650"]
["34889","ZENERGY - OSŁONA CZOŁOWA PRZEŹROCZYSTA W800, 10M / 650",333.5,"1-ZE-01",null,null,"01_TRANSPARENT_COVERS","34889","SZT","85389099",null,null,"5901988348892","OE - Couverture transparente L800, 10M / 650","OE - Transparent Front cover W800, 10M / 650","OE- TAPA TROQ. TRANSP. W800, 10M / 650","ZENERGY - ÁTLÁTSZÓ ELSŐ BURKOLAT W800, 10M / 650"]
["34893","ZENERGY - OSŁONA CZOŁOWA PEŁNA W800, 12M / 650",143,"1-ZE-01",null,null,"01_PLAIN_COVERS","34893","SZT","85389099",null,"230622RT","5901988148935","OE - Couverture avant complète L800, 12M / 650","OE - Plain Front cover W800, 12M / 650","OE- TAPA TROQ. CIEGA W800, 12M / 650","ZENERGY - TELJES ELSŐ BURKOLAT W800, 12M / 650"]
["34900","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W850, 3M, PIONOWO",180.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","34900","SZT","85381000","27.12.40.0",null,"5901988349004","OE - Couvercle avant 1x NSX630 3 / 4P, L850, 9M / 700, vertical, levier","OE - INS / INV100-250, W850, 3M Mounting plate, Vertical","OE- PLACA MONTAJE INS / INV100-250, W850, 3M, VERT.","ZENERGY – SZERELŐLAP INS/INV100-250, W850, 3M, FÜGGŐLEGES"]
["34901","ZENERGY - PŁYTA MONTAŻOWA INS/INV100-250, W850, 4M, POZIOMO",189.2,"1-ZE-01",null,null,"OE_MCCB_PLATES","34928","SZT","85381000","27.12.40.0",null,"5901988349011","OE - plaque de montage INS / INV100-250, L850, 3M, horizontale","OE - INS / INV100-250, W850, 4M Mounting plate, Horizontal","OE- PLACA MONTAJE INS / INV100-250, W850, 4M, HORIZ.","ZENERGY - SZERELŐLEMEZ INS/INV100-250, W850, 4M, VÍZSZINTES"]
["34904","ZENERGY - PŁYTA MONTAŻOWA INS/INV1600, W850, 8M, PIONOWO",292.60000000000002,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988349042","OE - plaque de montage INS / INV1600, L850, 8M, verticale","OE - INS / INV1600, W850, 8M Mounting plate, Vertical","OE- PLACA MONTAJE INS / INV1600, W850, 8M, VERT.","ZENERGY – SZERELŐLAP INS/INV1600, W850, 8M, FÜGGŐLEGES"]
["34907","ZENERGY - PŁYTA MONTAŻOWA 2X INS/INV100-250 RZR, W850, 6M, POZIOMO",218.9,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85381000","27.12.40.0",null,"5901988349073","OE - Couvercle avant NSX630 3P, L850, 4M / 700, horizontal, levier","OE - Mounting plate 2x INS / INV100-250 RZR, W850, 6M, Horizontal","OE- PLACA MONTAJE 2x INS / INV100-250 RZR, W850, 6M, HORIZ.","ZENERGY - SZERELŐLEMEZ 2X INS/INV100-250 RZR, W850, 6M, VÍZSZINTES"]
["34912","ZENERGY - OSŁONA CZOŁOWA INS/INV100-250, W850, 4M / 700, POZIOMO",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","34912","SZT","85389099","27.12.40.0",null,"5901988349127","OE - capot avant INS / INV100-250, L850, 4M / 700, horizontal","OE - INS / INV100-250, W850, 4M / 700 Front cover, Horizontal","OE- TAPA TROQ. INS / INV100-250, W850, 4M / 700,  HORIZ.","ZENERGY - ELSŐ BURKOLAT INS/INV100-250, W850, 4M / 700, VÍZSZINTES"]
["34916","ZENERGY - OSŁONA CZOŁOWA INS/INV1600, W850, 6M / 700, PIONOWO",106.9,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988349165","OE - capot avant INS / INV1600, L850, 6M / 700, vertical","OE - INS / INV1600, W850, 6M / 700 front visor, Vertical","OE- TAPA TROQ. INS / INV1600, W850, 6M / 700, VERT.","ZENERGY - ELSŐ BURKOLAT INS/INV1600, W850, 6M / 700, FÜGGŐLEGES"]
["34919","ZENERGY - OSŁONA CZOŁOWA 2X INS/INV100-250 RZR, W850, 6M / 700, POZIOMO, DŹWIGNIA",106.9,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988349196","OE - capot avant 2x INS / INV100-250 RZR, L850, 6M / 700, horizontal, levier","OE - Front cover 2x INS / INV100-250 RZR, W850, 6M / 700, Horizontal, Lever","OE- TAPA TROQ. 2x INS / INV100-250 RZR, W850, 6M / 700, HORIZ. MANETA","ZENERGY - ELSŐ BURKOLAT 2X INS/INV100-250 RZR, W850, 6M / 700, VÍZSZINTES, KAR"]
["34926","ZENERGY - PŁYTA MONTAŻOWA 6/4X NSX100-250 3/4P, W850, 3M, PIONOWO, WTYKOWY, WYSUWNY",180.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","34926","SZT","85381000","27.12.40.0",null,"5901988349264","OE - plaque de montage 6 / 4x NSX100-250 3 / 4P, L850, 3M, verticale, enfichable, dĂ©brochable","OE - Mounting plate 6 / 4x NSX100-250 3 / 4P, W850, 3M, Vertical, plug-in, draw-out","OE- PLACA MONTAJE 6 / 4X NSX100-250 3 / 4P, W850, 3M, VERT. ENCHUFABLE, EXTRAÍBLE","ZENERGY - RÖGZÍTŐLEMEZ 6/4X NSX100-250 3/4P, W850, 3M, FÜGGŐLEGES, DUGALOM, KIHAJTÓ"]
["34929","ZENERGY - PŁYTA MONTAŻOWA 2X NSX100-250 3/4P, NSX400-630 3/4P SZR, W850, BLOKADA PŁYTOWA, PIONOWO, SILNIK",180.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","34929","SZT","85381000","27.12.40.0",null,"5901988349295","OE - plaque de montage 2x NSX100-250, NSX400-630 SZR 3 / 4P, L850, verrouillage de plaque, vertical, moteur","OE - Mounting plate 2x NSX100-250 3 / 4P SZR, W850, plate lock, Vertical, Motor","OE- PLACA MONTAJE 2X NSX100-250 3/4P SZR, W850, , VERT. MOTOR","ZENERGY - SZERELŐLEMEZ 2X NSX100-250 3/4P, NSX400-630 3/4P SZR, W850, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34930","ZENERGY - PŁYTA MONTAŻOWA 2X NSX100-250 3/4P SZR, W850, BLOKADA PŁYTOWA, POZIOMO, SILNIK",180.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","34930","SZT","85381000","27.12.40.0",null,"5901988349301","OE - Couvercle avant INS630 3 / 4P, L850, 5M / 700, horizontal","OE - Mounting plate 2x NSX100-250 3 / 4P SZR, W850, plate lock, Horizontal, Motor","OE- PLACA MONTAJE 2X NSX100-250 3/4P SZR, W850, , HORIZ., MOTOR","ZENERGY - SZERELŐLEMEZ 2X NSX100-250 3/4P SZR, W850, LEMEZZÁR, VÍZSZINTES, MOTOR"]
["34935","ZENERGY - OSŁONA CZOŁOWA 6/4X NSX100-250 VIGI 3/4P, W850, 7M / 700, PIONOWO, DŹWIGNIA",133.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","34935","SZT","85389099","27.12.40.0",null,"5901988349356","OE - capot avant 6 / 4x NSX100-250 VIGI 3 / 4P, L850, 7M / 700, vertical, levier","OE - Front cover 6 / 4x NSX100-250 VIGI 3 / 4P, W850, 7M / 700, Vertical, Lever","OE- TAPA TROQ. 6 / 4X NSX100-250 VIGI 3 / 4P, W850, 7M / 700, VERT.","ZENERGY - ELSŐ BURKOLAT 6/4X NSX100-250 VIGI 3/4P, W850, 7M / 700, FÜGGŐLEGES, KAR"]
["34938","ZENERGY - OSŁONA CZOŁOWA NSX100-250 3P, W850, 3M / 700, POZIOMO, SILNIK, OBROTOWY",79,"1-ZE-01",null,null,"OE_MCCB_COVERS","34938","SZT","85389099",null,null,"5901988349387","OE - capot avant NSX100-250 3P, L850, 3M / 700, horizontal, moteur, rotatif","OE - NSX100-250 3P Front Hood, W850, 3M / 700, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 3P  W850, 3M / 700, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX100-250 3P, W850, 3M / 700, VÍZSZINTES, MOTOROS, FORGÓ"]
["34942","ZENERGY - OSŁONA CZOŁOWA NSX100-250 4P, W850, 4M / 700, POZIOMO, SILNIK, OBROTOWY",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","34942","SZT","85389099",null,null,"5901988349424","OE - capot avant NSX100-250 4P, L850, 4M / 700, horizontal, moteur, rotatif","OE - NSX100-250 4P, W850, 4M / 700 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX100-250 4P, W850, 4M / 700 COFRE DELANTERO, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX100-250 4P, W850, 4M / 700, VÍZSZINTES, MOTOROS, FORGÓ"]
["34945","ZENERGY - OSŁONA CZOŁOWA 2X NSX100-250 3/4P SZR, W850, 7M / 700, BLOKADA PŁYTOWA, PIONOWO, SILNIK",133.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","34945","SZT","85389099",null,null,"5901988349455","OE - capot avant 2x NSX100-250 SZR 3 / 4P, L850, 7M / 700, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX100-250 3 / 4P SZR, W850, 7M / 700, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX100-250 3/4P SZR, W850, 7M/700, VERT. MOTOR","ZENERGY - ELSŐ BURKOLAT 2X NSX100-250 3/4P SZR, W850, 7M / 700, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34951","ZENERGY - PŁYTA MONTAŻOWA NSX400-630 4P, W850, 5M, POZIOMO, DŹWIGNIA",209,"1-ZE-01",0.15,4,"OE_MCCB_PLATES","34951","SZT","85381000","27.12.40.0",null,"5901988349516","OE - Plaque de montage NSX400-630 4P, L850, 5M, horizontale, levier","OE - Mounting plate NSX400-630 4P, W850, 5M, Horizontal, Lever","OE- PLACA MONTAJE  UPB/UPD400-630, UCB/UCD400 4P, W850, 5M, HORIZ.","ZENERGY - SZERELŐLAP NSX400-630 4P, W850, 5M, VÍZSZINTES, KAR"]
["34959","ZENERGY - OSŁONA CZOŁOWA 3X NSX400-630 3/4P, W850, 9M / 700, PIONOWO, DŹWIGNIA",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","34959","SZT","85389099",null,null,"5901988349592","OE - capot avant 3x NSX400-630 3 / 4P, L850, 9M / 700, vertical, levier","OE - Front cover 3x NSX400-630 3 / 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. 3X NSX400-630 3/4P, W850, 9M/700, VERT.","ZENERGY - ELSŐ BURKOLAT 3X NSX400-630 3/4P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["34963","ZENERGY - OSŁONA CZOŁOWA NSX400-630 3P, W850, 4M / 700, POZIOMO, SILNIK, OBROTOWY",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","34963","SZT","85389099",null,null,"5901988349639","OE - capot avant NSX400-630 3P, L850, 4M / 700, horizontal, moteur, rotatif","OE - NSX400-630 3P, W850, 4M / 700 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 3P, W850, 4M / 700, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX400-630 3P, W850, 4M / 700, VÍZSZINTES, MOTOROS, FORGÓ"]
["34964","ZENERGY - OSŁONA CZOŁOWA NSX400-630 VIGI 3P, W850, 4M / 700, POZIOMO, DŹWIGNIA",86.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","34964","SZT","85389099",null,null,"5901988349646","OE - capot avant NSX400-630 VIGI 3P, L850, 4M / 700, horizontal, levier","OE - Front cover NSX400-630 VIGI 3P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. NSX400-630 VIGI 3P, W850, 4M/700, HORIZ.","ZENERGY - ELSŐ BURKOLAT NSX400-630 VIGI 3P, W850, 4M / 700, VÍZSZINTES, KAR"]
["34967","ZENERGY - OSŁONA CZOŁOWA NSX400-630 4P, W850, 5M / 700, POZIOMO, SILNIK, OBROTOWY",97.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","34967","SZT","85389099",null,null,"5901988349677","OE - capot avant NSX400-630 4P, L850, 5M / 700, horizontal, moteur, rotatif","OE - NSX400-630 4P, W850, 5M / 700 Front Hood, Horizontal, Motor, Rotary","OE- TAPA TROQ. NSX400-630 4P, W850, 5M / 700, HORIZ., MOTOR, ","ZENERGY - ELSŐ BURKOLAT NSX400-630 4P, W850, 5M / 700, VÍZSZINTES, MOTOROS, FORGÓ"]
["34970","ZENERGY - OSŁONA CZOŁOWA 2X NSX400-630 3/4P SZR, W850, 9M / 700, BLOKADA PŁYTOWA, PIONOWO, SILNIK",155.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","34970","SZT","85389099",null,null,"5901988349707","OE - capot avant 2x NSX400-630 SZR 3 / 4P, L850, 9M / 700, verrouillage de plaque, vertical, moteur","OE - Front cover 2x NSX400-630 3 / 4P SZR, W850, 9M / 700, plate lock, Vertical, Motor","OE- TAPA TROQ. 2X NSX400-630 3/4P SZR, W850, 9M/700, VERT. MOTOR","ZENERGY - ELSŐ BURKOLAT 2X NSX400-630 3/4P SZR, W850, 9M / 700, LEMEZZÁR, FÜGGŐLEGES, MOTOR"]
["34976","ZENERGY - PŁYTA MONTAŻOWA NS1600, W850, 7M, POZIOMO, NA STAŁE",317.39999999999998,"1-ZE-01",null,null,"OE_ACB_PLATES","34976","SZT","85389099","27.12.40.0",null,"5901988349769","OE - plaque de montage NS1600, L850, 7M, horizontale, permanente","OE - Mounting plate NS1600, W850, 7M, Horizontal, fixed","OE- PLACA MONTAJE NS1600, W850, 7M, HORIZ., FIJA","ZENERGY - SZERELŐLAP NS1600, W850, 7M, VÍZSZINTES, RÖGZÍTETT"]
["34979","ZENERGY - PŁYTA MONTAŻOWA NW40, W850, WYSUWNY, BEZ WSPORNIKÓW",330.1,"1-ZE-01",null,null,"OE_ACB_PLATES","34979","SZT","85389099","27.12.40.0",null,"5901988349790","OE - plaque de montage NW40, L850, debrochable, sans supports","OE - Mounting plate NW40, W850, withdrawable, without brackets","OE- PLACA MONTAJE NW40, W850, EXTRAÍBLE, SIN SOPORTES","ZENERGY - RÖGZÍTŐLEMEZ NW40, W850, TOSZTÓ, KONZER NÉLKÜL"]
["34985","ZENERGY - OSŁONA CZOŁOWA NS1600 3/4P, W850, 8M / 700, PIONOWO, NAPĘD OBROTOWY, NA STAŁE",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","34985","SZT","85389099",null,null,"5901988349851","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, vertical, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W850, 8M / 700, Vertical, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P, W850, 8M / 700, VERT. ACCIONAMIENTO , FIJO","ZENERGY - ELSŐ BURKOLAT NS1600 3/4P, W850, 8M / 700, FÜGGŐLEGES, FORGÓHAJTÁS, RÖGZÍTETT"]
["34988","ZENERGY - OSŁONA CZOŁOWA NS1600 3/4P, W850, 8M / 700, POZIOMO, NAPĘD OBROTOWY, NA STAŁE",165.6,"1-ZE-01",null,null,"OE_ACB_COVERS","34988","SZT","85389099",null,null,"5901988349882","OE - capot avant NS1600 3 / 4P, L850, 8M / 700, horizontal, entraĂ®nement rotatif, permanent","OE - NS1600 3 / 4P Front cover, W850, 8M / 700, Horizontal, Rotary Drive, Fixed","OE- TAPA TROQ. NS1600 3 / 4P, W850, 8M / 700, HORIZ. FIJO","ZENERGY - ELSŐ BURKOLAT NS1600 3/4P, W850, 8M / 700, VÍZSZINTES, FORGÓHAJTÁS, RÖGZÍTETT"]
["34991","ZENERGY - OSŁONA CZOŁOWA NW40 3/4P, W850, 9M / 700, PIONOWO, WYSUWNY",294.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","34991","SZT","85389099",null,null,"5901988349912","OE - capot avant NW40 3 / 4P, L850, 9M / 700, vertical, dĂ©brochable","OE - NW40 3 / 4P, W850, 9M / 700 Front cover, Vertical, withdrawable","OE- TAPA TROQ. NW40 3/4P, W850, 9M/700, VERT. EXTRAÍBLE","ZENERGY - ELSŐ BURKOLAT NW40 3/4P, W850, 9M / 700, FÜGGŐLEGES, CSÚSZTÓ"]
["34992","ZENERGY - OSŁONA CZOŁOWA NW40 3/4P, W850, 8M / 700, PIONOWO, NA STAŁE",299,"1-ZE-01",3.3333333333333333E-2,1,"OE_ACB_COVERS","34992","SZT","85389099",null,null,"5901988349929","OE - capot avant NW40 3 / 4P, L850, 8M / 700, vertical, permanent","OE - NW40 3 / 4P, W850, 8M / 700 front visor, Vertical, fixed","OE- TAPA TROQ. NW40 3/4P, W850, 8M/700, VERT. FIJO","ZENERGY - ELSŐ BURKOLAT NW40 3/4P, W850, 8M / 700, FÜGGŐLEGES, RÖGZÍTETT"]
["35100","ZENERGY - WSPORNIK DLA UCHWYTU KABLOWEGO TYPU UKR1/UKR2 80MM, W400",48.6,"1-ZE-01",null,null,"OE_SUPPORT","35100","SZT","85389099",null,null,"5901988351007","OE - Support pour serre-câble type UKR1/UKR2 80mm, L400","OE - Bracket for the cable clamp UKR1 / UKR2 80mm, W400","OE- SOPORTE PARA CABLES TIPO UKR1/UKR2 80MM, W400","ZENERGY - TÁMOGATÁS UKR1/UKR2 80MM, W400 TÍPUSÚ KÁBELKERETHEZ"]
["35103","ZENERGY - WSPORNIK DLA UCHWYTU KABLOWEGO TYPU UKR1/UKR2 80MM, W650",74.3,"1-ZE-01",0.3,2,"OE_SUPPORT","35103","SZT","85389099",null,null,"5901988351038","OE - Support pour serre-câble type UKR1/UKR2 80mm, L650","OE - Bracket for the cable clip type UKR1 / UKR2 80mm, W650","OE- SOPORTE PARA CABLES TIPO UKR1/UKR2 80MM, W650","ZENERGY - TÁMOGATÁS UKR1/UKR2 80MM, W650 TÍPUSÚ KÁBELKERETHEZ"]
["35107","ZENERGY - WSPORNIK DLA UCHWYTU KABLOWEGO TYPU UKR1/UKR2 80MM, W1200",103.2,"1-ZE-01",null,null,"OE_SUPPORT","35107","SZT","85389099",null,null,"5901988351076","OE - Support pour serre-câble type UKR1/UKR2 80mm, L1200","OE - Bracket for the cable clip type UKR1 / UKR2 80mm, W1200_double posts","OE- SOPORTE PARA CABLES TIPO UKR1/UKR2 80MM, W1200","ZENERGY - TÁMOGATÁS UKR1/UKR2 80MM, W1200 TÍPUSÚ KÁBELKONCOLORHOZ"]
["35210","ZENERGY - POŁĄCZENIE POZIOME MCCB Z MOSTEM 3P 160A-250A FLEX 20X3",202.4,"1-ZE-01",0.01,1,"OE_MCCB_TRANSFER","35210","SZT","85389099",null,null,"5901988352103","OE - Connexion horizontale du MCCB avec un pont 3P 250A","OE - Horizontal MCCB connection with 3P 160A-250A Flex 20x3 bridge","OE- CONEXION HORIZ. MCCB CON EMBARRADO 3P 250A","ZENERGY - VÍZSZINTES CSATLAKOZÁS MCCB BRIDGE 3P 160A-250A FLEX 20X3"]
["35214","ZENERGY - POŁĄCZENIE POZIOME MCCB Z MOSTEM 4P 400A-630A FLEX 24X8",452.1,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","35214","SZT","85389099","27.12.40.0",null,"5901988352141","OE - Connexion horizontale MCCB avec pont 4P 400A-630A Flex 24x8","OE - Horizontal MCCB connection with 4P 400A-630A Flex 24x8 bridge","OE- CONEXIÓN HORIZ. MCCB CON EMB. 4P 400A-630A FLEX 24X8","ZENERGY - VÍZSZINTES CSATLAKOZÁS MCCB BRIDGE 4P 400A-630A FLEX 24X8"]
["35217","ZENERGY - POŁĄCZENIE POZIOME MCCB Z TRANSFEREM 3P 400A-630A FLEX 24X8",451,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","35217","SZT","85389099",null,null,"5901988352172","OE - Connexion horizontale MCCB avec transfert 4P 250A","OE - Horizontal MCCB connection with 3P 400A-630A Flex 24x8 transfer","OE- CONEXION HORIZ. MCCB CON CONEXION PREF. 4P 250A","ZENERGY - VÍZSZINTES CSATLAKOZÁS MCCB TRANSFER 3P 400A-630A FLEX 24X8"]
["35220","ZENERGY - POŁĄCZENIE POZIOME MCCB Z TRANSFEREM 4P 400A-630A FLEX 24X8",601.70000000000005,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","35220","SZT","85389099","27.12.40.0",null,"5901988352202","OE - Connexion horizontale du MCCB avec un pont 3P 800A","OE - MCCB Horizontal connection with transfer 4P 400A-630A Flex 24x8","OE- CONEXION HORIZ. MCCB CON EMBARRADO 3P 800A","ZENERGY - VÍZSZINTES CSATLAKOZÁS MCCB TRANSFER 4P 400A-630A FLEX 24X8"]
["35221","ZENERGY - POŁĄCZENIE POZIOME MCCB Z TRANSFEREM 4P 630A IP-55 FLEX 32X8",693,"1-ZE-01",0.01,1,"OE_MCCB_TRANSFER",null,"SZT","85389099",null,null,"5901988352219","OE - Connexion horizontale du MCCB au pont 3P 1250A","OE - Horizontal MCCB connection with transfer 4P 630A IP-55 Flex 32x8","OE- CONEXION HORIZ. MCCB CON EMBARRADO 3P 1250A","ZENERGY - VÍZSZINTES CSATLAKOZÁS MCCB TRANSFER 4P 630A IP-55 FLEX 32X8"]
["35224","ZENERGY - POŁĄCZENIE POZIOME MCCB Z MOSTEM 4P 800A-1000A CU 50X10",610.5,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","35224","SZT","85389099",null,null,"5901988352240","OE - Connexion horizontale MCCB avec pont 4P 800A-1000A Cu 50x10","OE - Horizontal MCCB connection with bridge 4P 800A-1000A Cu 50x10","OE- CONEXIÓN HORIZ. MCCB CON EMB. 4P 800A-1000A CU 50X10","ZENERGY - VÍZSZINTES CSATLAKOZÁS MCCB BRIDGE 4P 800A-1000A CU 50X10"]
["35228","ZENERGY - POŁĄCZENIE POZIOME MCCB Z TRANSFEREM 4P 800A-1000A CU 50X10",746.9,"1-ZE-01",null,null,"OE_MCCB_TRANSFER","35228","SZT","85389099",null,null,"5901988352288","OE - Connexion horizontale MCCB avec transfert 4P 1250A","OE - MCCB Horizontal connection with transfer 4P 800A-1000A Cu 50x10","OE- CONEXION HORIZ. MCCB CON CONEXION PREF. 4P 1250A","ZENERGY – VÍZSZINTES CSATLAKOZÁS MCCB TRANSFER 4P 800A-1000A CU 50X10"]
["35737","ZENERGY - OSŁONA CZOŁOWA NSX100-250 3P, W650, 3M / 500, POZIOMO, DŹWIGNIA+POMIAR",67.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","35737","SZT","85389099",null,null,"5901988357375","OE - capot avant NSX100-250 3P, L650, 3M / 500, horizontal, levier + mesure","OE - Front cover NSX100-250 3P, W650, 3M / 500, Horizontal, Lever + measurement","OE- TAPA TROQ. NSX100-250 3P, W650, 3M/500, HORIZ. + MEDIDA","ZENERGY - ELSŐ BURKOLAT NSX100-250 3P, W650, 3M / 500, VÍZSZINTES, KAR + MÉRÉS"]
["35741","ZENERGY - OSŁONA CZOŁOWA NSX100-250 4P, W650, 4M / 500, POZIOMO, DŹWIGNIA+POMIAR",74.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","35741","SZT","85389099",null,null,"5901988357412","OE - capot avant NSX100-250 4P, L650, 4M / 500, horizontal, levier + mesure","OE - Front cover NSX100-250 4P, W650, 4M / 500, Horizontal, Lever + measurement","OE- TAPA TROQ. NSX100-250 4P, W650, 4M/500, HORIZ. + MEDIDA","ZENERGY - ELSŐ BURKOLAT NSX100-250 4P, W650, 4M / 500, VÍZSZINTES, KAR + MÉRÉS"]
["35766","ZENERGY - OSŁONA CZOŁOWA NSX400-630 4P, W650, 5M / 500, POZIOMO, DŹWIGNIA+POMIAR",81.400000000000006,"1-ZE-01",null,null,"OE_MCCB_COVERS","35766","SZT","85389099",null,null,"5901988357665","OE - capot avant NSX400-630 4P, L650, 5M / 500, horizontal, levier + mesure","OE - Front cover NSX400-630 4P, W650, 5M / 500, Horizontal, Lever + measurement","OE- TAPA TROQ. NSX400-630 4P, W650, 5M/500, HORIZ. + MEDIDA","ZENERGY - ELSŐ BURKOLAT NSX400-630 4P, W650, 5M / 500, VÍZSZINTES, KAR+MÉRÉS"]
["35786","ZENERGY - OSŁONA CZOŁOWA DLA NSB I ANALIZATORA 92X92MM W650, 7M / 500",139.19999999999999,"1-ZE-01",null,null,"OE_ACB_COVERS","35786","SZT","85389099",null,null,"5901988357863","OE - capot avant pour analyseur NSb et 92x92mm L650, 7M / 500","OE - Front cover for NSb and 92x92mm W650, 7M / 500 analyzer","OE- TAPA TROQ. PARA ANALIZADOR NSB Y 92X92MM W650, 7M/500","ZENERGY - ELSŐ BURKOLAT NSB-HOZ ÉS ELEMZŐHEZ 92X92MM W650, 7M / 500"]
["36002","ZENERGY - ZAŚLEPKA ROZŁĄCZNIKA LISTWOWEGO EFEN 250-630A",59.1,"1-ZE-01",2.0333333333333332,5,"OE_COVERS","36002","SZT","85389099","27.12.40.0",null,"5901988360023","OE - Interrupteur de store déconnecteur EFEN 250-630A","OE - End cap for switch disconnector EFEN 250-630A","OE- OBTURADOR BASE FUSIBLES 250-630A","ZENERGY - SAPKA CSÍKOS KAPCSOLÓKAPCSOLÓHOZ EFEN 250-630A"]
["36003","ZENERGY - ZAŚLEPKA ROZŁĄCZNIKA SKRZYNKOWEGO EFEN 160A",36.700000000000003,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36003","SZT","85389099","27.12.40.0",null,"5901988360030","OE - Embout pour sectionneur à commutateur EFEN 160A","OE - End cap for EFEN 160A box switch box","OE- OBTURADOR BASE FUSIBLES 160A","ZENERGY - EFEN 160A DOBOZ KAPCSOLÓ"]
["36006","ZENERGY - ZAŚLEPKA ROZŁĄCZNIKA LISTWOWEGO EFEN 100A, ROZSTAW SZYN 60MM",24.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988360061","OE - Sectionneur sectionneur EFEN 100A, espacement des rails 100 mm","OE - End cap EFEN 100A rail switch disconnector, 100mm spacing","OE- OBTURADOR BASE FUSIBLES 100A, SEPARACION BARRAS 100MM","ZENERGY - SAPKA EFEN 100A SZALAK KAPCSOLÓHOZ, RÚD távköz 60mm"]
["36010","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK LISTWOWY EFEN 250-630, ROZSTAW 185MM + 1 IZOLATOR + WSPORNIKI",412.2,"1-ZE-01",0.76666666666666672,10,"OE_INSULATOR_D400","36010","SZT","85389099","27.12.40.0",null,"5901988360108","OE - Plaque de montage sectionneur de bande EFEN 250-630, espacement de 185mm + 1 isolant + supports","OE - Mounting plate switch disconnector EFEN 250-630, 185mm spacing + 1 insulator + brackets","OE- PLACA MONTAJE  BASE PORTAFUSIBLES250-630, 185MM + 1 IZOLATOR + SOPORT","ZENERGY - RÖGZÍTŐLEMEZ SZÍV KAPCSOLÓ EFEN 250-630, HELY 185MM + 1 SZIGETELŐ + TARTÓK"]
["36013","ZENERGY - ZAŚLEPKA ROZŁĄCZNIKA SKRZYNKOWEGO HYUN 160A 3P",36.700000000000003,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988360139","OE - Embout pour sectionneur HYUN 160A 3P","OE - End cap for box switch disconnector HYUN 160A 3P","OE- OBTURADOR BASE FUSIBLES HYUN 160A 3P","ZENERGY – HYUN 160A 3P DOBOZ KAPCSOLÓ"]
["36016","ZENERGY - ZAŚLEPKA UCB 100 4P",31.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","36016","SZT","85389099","27.12.40.0",null,"5901988360160","OE - Embout UCB 100 4P","OE - End cap UCB 100 4P","OE- OBTURADOR UCB 100 4P","ZENERGY - CAP UCB 100 4P"]
["36020","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN 100A, MONTAŻ NA SZYNACH, ROZSTAW 60MM + 2 IZOLATORY, BEZ WSPORNIKÓW (ZAMIENNIK REF. ZENE36040)",321.39999999999998,"1-ZE-01",null,null,"OE_INSULATOR_D400",null,"SZT","85469010",null,null,"5901988360207","OE - Plaque de montage, déconnecteur EFEN 100A, montage sur rail + 2 isolateurs + consoles","OE - Mounting plate EFEN 100A switch disconnector, mounting on rails, spacing 60mm + 2 insulators, without brackets (replacement ref. ZENE36040)","OE- PLACA MONTAJE EFEN 100A interruptor seccionador, montaje sobre carriles, paso 60mm + 2 aisladores, sin soportes (recambio ref. ZENE36040)","ZENERGY - SZERELŐLEMEZ EFEN 100A DOBOZ KAPCSOLÓ, SÍNRE SZERELÉS, HELY 60MM + 2 SZIGETELŐ, KONZOLOK NÉLKÜL (CSERE REF. ZENE36040)"]
["36025","ZENERGY - ZAŚLEPKA HGM 100 3P",31.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","36025","SZT","85389099",null,null,"5901988360252","OE - Embout HGM 100 3P","OE - HGM 100 3P End cap","OE- OBTURADOR HGM 100 3P","ZENERGY - DUGÓ HGM 100 3P"]
["36026","ZENERGY - ZAŚLEPKA HGM 125 3P",31.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","36026","SZT","85389099",null,null,"5901988360269","OE - Embout HGM 125 3P","OE - HGM 125 3P End cap","OE- OBTURADOR HGM 125 3P","ZENERGY - DUGÓ HGM 125 3P"]
["36029","ZENERGY - ZAŚLEPKA HGM 630-800 3P",37.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","36029","SZT","85389099",null,null,"5901988360290","OE - Embout HGM 630-800 3P","OE - HGM 630-800 3P End cap","OE- OBTURADOR HGM 630-800 3P","ZENERGY - DUGÓ HGM 630-800 3P"]
["36035","ZENERGY - ZAŚLEPKA HGM 100 4P",31.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","36025","SZT","85389099","27.12.40.0",null,"5901988360351","OE - Embout HGM 100 4P","OE - HGM 100 4P End cap","OE- OBTURADOR HGM 100 4P","ZENERGY - DUGÓ HGM 100 4P"]
["36039","ZENERGY - ZAŚLEPKA HGM 630-800 4P",37.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","36029","SZT","85389099","27.12.40.0",null,"5901988360399","OE - Embout HGM 630-800 4P","OE - HGM 630-800 4P End cap","OE- OBTURADOR HGM 630-800 4P","ZENERGY - DUGÓ HGM 630-800 4P"]
["36042","ZENERGY - WSPORNIK PRAWY DLA PŁYTA MONTAŻOWA ROZŁĄCZNIK LISTWOWY EFEN 250-630",0,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988360429","OE - Support DROIT pour plaque de montage déconnecteur à bande EFEN 250-630","OE - RIGHT bracket for Mounting plate switch disconnector EFEN 250-630","OE- Soporte DERECHO para PLACA MONTAJE de interruptor-seccionador EDEN 250-630","ZENERGY - JOBB KONZER SZERELŐLEMEZ SZÍV KAPCSOLÓDÓHOZ EFEN 250-630"]
["36060","ZENERGY - ZAŚLEPKA HGP 100-160 3P",31.5,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988360603","OE - Embout HGP 100-160 3P","OE - End cap HGP 100-160 3P","*OE - Tapa final HGP 100-160 3P","ZENERGY - DUGÓ HGP 100-160 3P"]
["36065","ZENERGY - ZAŚLEPKA HGP 100-160 4P",31.7,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988360658","OE - Embout HGP 100-160 4P","OE - End cap HGP 100-160 4P","*OE - Tapa final HGP 100-160 4P","ZENERGY - DUGÓ HGP 100-160 4P"]
["36068","ZENERGY - ZAŚLEPKA HGP 800 4P",37.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","36068","SZT","85389099",null,null,"5901988360689","OE - Embout HGP 800 4P","OE - End cap HGP 800 4P","*OE - Tapa final HGP 800 4P","ZENERGY - DUGÓ HGP 800 4P"]
["36113","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK LISTWOWY EFEN 250-630 DLA ALCUBAR H150R, ROZSTAW 185MM + IZOLATORY + WSPORNIKI",409.9,"1-ZE-01",0.11666666666666667,2,"OE_INSULATOR_D400","36113","SZT","85389099",null,null,"5901988361136","OE - Plaque de montage EFEN 250-630 interrupteur-sectionneur pour AlCubar H150R, espacement 185MM + isolateurs + supports","OE - Mounting plate EFEN 250-630 switch disconnector for AlCubar H150R, spacing 185mm + insulators + brackets","*OE - Placa de montaje EFEN 250-630 interruptor seccionador para AlCubar H150R paso 185MM + aisladores + soportes","ZENERGY - RÖGZÍTŐLEMEZ SZALAG KAPCSOLÓ EFEN 250-630 ALCUBA H150R-HOZ, HELY 185MM + SZIGETELŐK + KONZEREK"]
["36114","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK LISTWOWY EFEN 250-630 DLA ALCUBAR H150R, ROZSTAW 185MM + IZOLATORY + WSPORNIKI, DLA ŁĄCZNIKA SZYN",409.9,"1-ZE-01",0.4,4,"OE_INSULATOR_D400","36114","SZT","85389099",null,null,"5901988361143","OE - Plaque de montage EFEN 250-630 interrupteur-sectionneur pour AlCubar H150R, espacement 185MM + isolateurs + supports, pour connecteur de jeu de barres","OE - Mounting plate EFEN 250-630 switch disconnector for AlCubar H150R, spacing 185mm + insulators + brackets, for busbar connector","*OE - Placa de montaje EFEN 250-630 interruptor seccionador para AlCubar H150R paso 185MM + aisladores + soportes, para conector de barras","ZENERGY - RÖGZÍTŐLEMEZ SZÍV KAPCSOLÓ EFEN 250-630 ALCUBA H150R-HOZ, HELY 185MM + SZIGETELŐK + TARTÓK, BUSZ CSATLAKOZÁSHOZ"]
["36117","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK LISTWOWY EFEN 250-630 DLA ALCUBAR H100R (środek pola), ROZSTAW 185MM + IZOLATORY + WSPORNIK/KĄTOWNIK",409.9,"1-ZE-01",null,null,"OE_INSULATOR_D400","36117","SZT","85389099",null,null,"5901988361174","OE - Plaque de montage, sectionneur de bande EFEN 250-630 pour AlCubar H100R (centre), espacement 185 mm + isolateurs + support/carré","OE - Mounting plate for switch disconnector EFEN 250-630 for AlCubar H100R (field center), spacing 185mm + insulators + bracket / angle","OE- PLACA MONTAJE PARA SECCIONADOR EFN 250-630 PARA ALCUBAR H100R ","ZENERGY - RÖGZÍTŐLEMEZ CSALAK KAPCSOLÓ EFEN 250-630 ALCUBA H100R-HOZ (mező középső), HELY 185MM + SZIGETELŐK + KONZER/SZÖG KONZER"]
["36140","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN 400-630A, W1000, PIONOWO + WSPORNIKI",275.39999999999998,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES",null,"SZT","85389099",null,null,"5901988361402","OE - Plaque de montage, sectionneur de boîte EFEN 400-630A, L1000, verticalement + supports","OE - Mounting plate EFEN 400-630A, W1000 switch-disconnector, Vertical + brackets","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 400-630A, W1000, VERT. + SOPORT.","ZENERGY - SZERELŐLEMEZ DOBOZ KAPCSOLÓKAPCSOLÓ EFEN 400-630A, W1000, FÜGGŐLEGES + KONZEREK"]
["36170","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 4X EFEN 250A, W1000, 9M / 850, PIONOWO",142.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36170","SZT","85389099",null,null,"5901988361709","OE - Déconnecteur 4x EFEN 250, L1000, 9M, verticalement","OE - Cover, switch box 4x EFEN 250, W1000, 9M, Vertical","OE- TAPA BASE PORTAFUSIBLES  4X250, W1000, 9M, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 4X EFEN 250A, W1000, 9M / 850, FÜGGŐLEGES"]
["36420","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN, SILAS; SCHN LV4 160A, W400, PIONOWO",90.2,"1-ZE-01",0.11666666666666667,1,"OE_EQUIPMENT_PLATES","36420","SZT","85389099",null,null,"5901988364205","OE - plaque de montage EFEN 160A, L400, interrupteur-sectionneur vertical","OE - Mounting plate EFEN NT-IN, SILAS switch disconnector; SCHN LV4 160A, W400, Vertical","OE- PLACA MONTAJE EFEN NT-IN, CAJA DE INTERRUPTORES SILAS; SCHN LV4 160A, W400, VERT.","ZENERGY - SZERELŐLEMEZ EFEN NT-IN DOBOZ KAPCSOLÓ, SILAS; SCHN LV4 160A, W400, FÜGGŐLEGES"]
["36520","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN, SILAS; SCHN LV4 160A, W450, PIONOWO",104.8,"1-ZE-01",6.6666666666666666E-2,4,"OE_EQUIPMENT_PLATES","36520","SZT","85389099",null,null,"5901988365202","OE - Sectionneur de boîte de montage de plaque EFEN 160A, L450, vertical","OE - Mounting plate EFEN NT-IN, SILAS; SCHN LV4 160A, W450, Vertical","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 160A, W450, VERT.","ZENERGY - SZERELŐLEMEZ EFEN NT-IN DOBOZ KAPCSOLÓ, SILAS; SCHN LV4 160A, W450, FÜGGŐLEGES"]
["36540","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN 400A, W450, PIONOWO",166.3,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","36540","SZT","85389099",null,null,"5901988365400","OE - Sectionneur de boîte à plaques de montage EFEN 400A, L450, verticalement","OE - Mounting plate EFEN NT-IN 400A, W450 switch disconnector, Vertical","OE- PLACA MONTAJE EFEN NT-IN 400A, W450 SECCIONADOR, VERT.","ZENERGY - SZERELŐLEMEZ DOBOZ KAPCSOLÓ EFEN NT-IN 400A, W450, FÜGGŐLEGES"]
["36550","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 2X EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, PIONOWO",57.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36550","SZT","85389099",null,null,"5901988365509","OE - Déconnecteur 2x EFEN 100, L450, 6M, verticalement","OE - Cover box switch box 2x EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, Vertical","OE- CAJA TAPA CAJA INTERRUPTOR 2X EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 2X EFEN NT-IN; SCHN LV4 100A, W450, 6M / 300, FÜGGŐLEGES"]
["36565","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 2X EFEN SILAS; SCHN LV4 160A, W450, 6M / 300, PIONOWO",54.6,"1-ZE-01",0.05,1,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988365653","OE - SHIELD BOX DISCONNECT 2X EFEN SILAS ; SCHN LV4 160A, L450, 6M/300, VERTICALE","OE - Fuse disconnector cover 2X EFEN SILAS; SCHN LV4 160A, W450, 6M / 300, Vertical","*OE - CAJA DE ESCUDO DESCONECTAR 2X EFEN SILAS; SCHN LV4 160A, W450, 6M/300, VERTICAL","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 2X EFEN SILAS; SCHN LV4 160A, W450, 6M / 300, FÜGGŐLEGES"]
["36610","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN; SCHN LV4 100A, W650, PIONOWO",136.1,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","36610","SZT","85389099","27.12.40.0",null,"5901988366100","OE - Sectionneur de boîte à plaques de montage EFEN 100A, L650, verticalement","OE - Mounting plate EFEN NT-IN switch disconnector; SCHN LV4 100A, W650, Vertical","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 100A, W650, VERT.","ZENERGY - SZERELŐLAP EFEN NT-IN DOBOZ KAPCSOLÓ; SCHN LV4 100A, W650, FÜGGŐLEGES"]
["36631","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN 250A + OCHRONNIK, W650, 5M, POZIOMO",191.2,"1-ZE-01",3.3333333333333333E-2,4,"OE_EQUIPMENT_PLATES","36631","SZT","85389099",null,null,"5901988366315","OE - Plaque de montage, interrupteur-sectionneur EFEN 250A + protecteur, L650, 5M, horizontal","OE - Mounting plate EFEN NT-IN 250A switch disconnector + arrester, W650, 5M, Horizontal","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 250A + PROTECC. W650, 5M, HORIZ.","ZENERGY - SZERELŐLÁMEFEN NT-IN DOBOZ KAPCSOLÓ 250A + VÉDŐ, W650, 5M, VÍZSZINTES"]
["36640","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN 2X400A -1X630A, W650, PIONOWO",218.2,"1-ZE-01",1.6666666666666666E-2,2,"OE_EQUIPMENT_PLATES","36640","SZT","8538909900","27.12.40.0",null,"5901988366407","OE - Plaque de montage, déconnecteur EFEN 400-630A, L650, verticalement + étriers","OE - Mounting plate EFEN NT-IN switch disconnector 2x400A -1x630A, W650, Vertical","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 400-630A, W650, VERT. + SOPORT.","ZENERGY - SZERELŐLEMEZ EFEN NT-IN DOBOZ KAPCSOLÓ 2X400A -1X630A, W650, FÜGGŐLEGES"]
["36661","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN 160A + ochronnik, W650, 3M / 500, POZIOMO",69.900000000000006,"1-ZE-01",0.11666666666666667,2,"OE_EQUIPMENT_COVERS","36661","SZT","85389099","27.12.40.0",null,"5901988366612","OE - Couvercle de disjoncteur EFEN NT-IN 160A + protecteur, L650, 3M / 500, horizontal","OE - Cover EFEN NT-IN 160A switch disconnector + arrester, W650, 3M / 500, Horizontal","OE- TAPA EFEN NT-IN 160A SECCIONADOR + DESCARGADOR, W650, 3M/500, HORIZ.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ EFEN NT-IN 160A + védő, W650, 3M / 500, VÍZSZINTES"]
["36670","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 2x EFEN NT-IN 250A, W650, 9M / 500, PIONOWO",109.1,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36670","SZT","85389099",null,null,"5901988366704","OE - Sectionneur de protection 2x EFEN 250, L650, 9M, verticalement","OE - Cover box switch box 2x EFEN NT-IN 250A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2X250, W650, 9M, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 2x EFEN NT-IN 250A, W650, 9M / 500, FÜGGŐLEGES"]
["36675","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 2x EFEN SILAS; SCHN LV4 250A, W650, 9M / 500, PIONOWO",109.1,"1-ZE-01",0.1,1,"OE_EQUIPMENT_COVERS","36675","SZT","85389099",null,null,"5901988366759","OE - Boîte de dérivation 2x EFEN SILAS 250, L650, 9M, à la verticale","OE - Cover, switch box 2x EFEN SILAS; SCHN LV4 250A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2XSILAS 250, W650, 9M, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 2x EFEN SILAS; SCHN LV4 250A, W650, 9M / 500, FÜGGŐLEGES"]
["36680","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 2x EFEN NT-IN 400A, W650, 9M / 500, PIONOWO",109.1,"1-ZE-01",0.01,1,"OE_EQUIPMENT_COVERS","36680","SZT","8538909900",null,null,"5901988366803","OE - Déconnecteur 2x EFEN 400, L650, 9M, verticalement","OE - Cover box switch box 2x EFEN NT-IN 400A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  2X400, W650, 9M, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 2x EFEN NT-IN 400A, W650, 9M / 500, FÜGGŐLEGES"]
["36683","ZENERGY - OSŁONA ROZŁĄCZNIK LISTWOWY 9X EFEN 160, W650, 11M / 500, ROZSTAW SZYN 100MM",116.6,"1-ZE-01",0.10833333333333334,4,"OE_EQUIPMENT_COVERS","36683","SZT","85389099","27.12.40.0",null,"5901988366834","OE - Interrupteur-cache-contacteur 9x EFEN 160, L650, 11M, écartement de voie 100mm","OE - Cover rail switch disconnector 9x EFEN 160, W650, 11M / 500, bar spacing 100mm","OE- TAPA BASE FUSIBLES 9X160, W650, 11M, SEPARACION BARRAS  100MM","ZENERGY - FEDŐSZALAK KAPCSOLÓ 9X EFEN 160, W650, 11M / 500, RÁDHELY 100MM"]
["36690","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 1x EFEN NT-IN 630A, W650, 9M / 500, PIONOWO",116.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36690","SZT","85389099",null,null,"5901988366902","OE - Déconnecteur 1x EFEN 630, L650, 9M, verticalement","OE - Cover, switch box 1x EFEN NT-IN 630A, W650, 9M / 500, Vertical","OE- TAPA BASE PORTAFUSIBLES  1X630, W650, 9M, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 1x EFEN NT-IN 630A, W650, 9M / 500, FÜGGŐLEGES"]
["36739","ZENERGY - OSŁONA CZOŁOWA HAGER P160 3P 160A, W650, 3M / 500, POZIOMO, DŹWIGNIA",64.3,null,0.18333333333333332,2,"OE_MCCB_COVERS",null,null,"85389099",null,null,"5901988367398"]
["36910","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN; SCHN LV4 100A, W850, PIONOWO",165.2,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","36910","SZT","85389099",null,null,"5901988369101","OE - Sectionneur de boîtier de plaque de montage EFEN 100A, L850, verticalement","OE - Mounting plate EFEN NT-IN switch disconnector; SCHN LV4 100A, W850, Vertical","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 100A, W850, VERT.","ZENERGY - SZERELŐLAP EFEN NT-IN DOBOZ KAPCSOLÓ; SCHN LV4 100A, W850, FÜGGŐLEGES"]
["36930","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY 3X EFEN NT-IN 250A, W850, PIONOWO",197.6,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","36930","SZT","85389099",null,null,"5901988369309","OE - Sectionneur de boîte de montage de plaque EFEN 250A, L850, vertical","OE - Mounting plate 3x EFEN NT-IN 250A, W850 switch disconnector, Vertical","OE- PLACA MONTAJE  BASE PORTAFUSIBLES 250A, W850, VERT.","ZENERGY - SZERELŐLEMEZ DOBOZ KAPCSOLÓDÓ 3X EFEN NT-IN 250A, W850, FÜGGŐLEGES"]
["36936","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY 3X EFEN SILAS, SCHN LV4: 250A-630A, W850, PIONOWO",207.4,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","36936","SZT","85389099",null,null,"5901988369361","OE - plaque de montage pour disjoncteur EFEN SILAS ; SCHN LV4 250A-630A, L850, vertical","OE - Mounting plate EFEN SILAS switch disconnector; SCHN LV4 250A-630A, W850, Vertical","OE- PLACA MONTAJE EFEN SILAS INTERRUPTOR-SECCIONADOR; SCHN LV4 250A-630A, W850, VERT.","ZENERGY - SZERELŐLEMEZ DOBOZ KAPCSOLÓDÓ 3X EFEN SILAS, SCHN LV4: 250A-630A, W850, FÜGGŐLEGES"]
["36941","ZENERGY - OSŁONA CZOŁOWA HAGER P160 4P 160A, W850, 4M / 500, POZIOMO, DŹWIGNIA",79.8,null,0.21666666666666667,4,"OE_EQUIPMENT_COVERS",null,null,"85389099",null,null,"5901988369415"]
["36942","ZENERGY - PŁYTA MONTAŻOWA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN, SILAS; SCHN LV4 630A, W850, 6M, POZIOMO",235.4,"1-ZE-01",null,null,"OE_EQUIPMENT_PLATES","36942","SZT","85389099","27.90.12.0",null,"5901988369422","OE - Plaque de montage pour déconnecteur EFEN SILAS box ; SCHN LV4 630A, L850, 6M, horizontal","OE - Mounting plate EFEN NT-IN switch disconnector; SILAS; SCHN LV4 630A, W850, 6M, Horizontal","OE- PLACA MONTAJE EFEN NT-IN CAJA DE CONEXIONES; SILAS; SCHN LV4 630A, W850, 6M, HORIZ.","ZENERGY - SZERELŐLEMEZ EFEN NT-IN DOBOZ KAPCSOLÓ, SILAS; SCHN LV4 630A, W850, 6M, VÍZSZINTES"]
["36951","ZENERGY - OSŁONA CZOŁOWA HAGER P160 3/4P 160A, W850, 5M / 500, PIONOWO, DŹWIGNIA",90,null,0.40833333333333333,4,"OE_EQUIPMENT_COVERS",null,null,"85389099",null,null,"5901988369514"]
["36962","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY EFEN SILAS; SCHN LV4 160A + ochronnik, W850, 3M / 700, POZIOMO",75.3,"1-ZE-01",3.3333333333333333E-2,2,"OE_EQUIPMENT_COVERS","36962","SZT","8538909900",null,null,"5901988369620","OE - Couvercle interrupteur-sectionneur EFEN SILAS ; SCHN LV4 160A + protecteur, L850, 3M / 700, horizontalement","OE - Cover EFEN SILAS switch box; SCHN LV4 160A + arrester, W850, 3M / 700, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 160A + LIMITADOR SOBRET. W850, 3M/700, HORIZ.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ EFEN SILAS; SCHN LV4 160A + levezető, W850, 3M / 700, VÍZSZINTES"]
["36972","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY EFEN SILAS; SCHN LV4 250A + ochronnik, W850, 5M / 700, POZIOMO",91.6,"1-ZE-01",8.3333333333333329E-2,2,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988369729","OE - Couvercle interrupteur-sectionneur EFEN SILAS ; SCHN LV4 250A + protecteur, L850, 5M / 700, horizontalement","OE - Cover EFEN SILAS switch box; SCHN LV4 250A + arrester, W850, 5M / 700, Horizontal","OE- Tapa caja interruptores EFEN SILAS; SCHN LV4 250A + pararrayos, W850, 5M/700, HORIZ.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ EFEN SILAS; SCHN LV4 250A + levezető, W850, 5M / 700, VÍZSZINTES"]
["36981","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY EFEN NT-IN 400A + ochronnik, W850, 5M / 700, POZIOMO",91.6,"1-ZE-01",5.8333333333333334E-2,2,"OE_EQUIPMENT_COVERS",null,"SZT","85389099",null,null,"5901988369811","OE - Couvercle interrupteur-sectionneur EFEN 400 + protecteur, L850, 5M, horizontalement","OE - Cover EFEN NT-IN 400A switch disconnector + arrester, W850, 5M / 700, Horizontal","OE- Tapa EFEN NT-IN 400A interruptor seccionador + descargador, W850, 5M/700, HORIZ.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ EFEN NT-IN 400A + védő, W850, 5M / 700, VÍZSZINTES"]
["36985","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY 3x EFEN SILAS; SCHN LV4 400A, W850, 9M / 700, PIONOWO",129.6,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36985","SZT","85389099",null,null,"5901988369859","OE - Couvercle interrupteur-sectionneur 3x EFEN SILAS ; SCHN LV4 400A, L850, 9M / 700, vertical","OE - Cover box switch disconnector 3x EFEN SILAS; SCHN LV4 400A, W850, 9M / 700, Vertical","OE- CAJA TAPA SECCIONADOR 3X FEEN SILAS; SCHN LV4 400A, W850, 9M / 700, VERT.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ 3x EFEN SILAS; SCHN LV4 400A, W850, 9M / 700, FÜGGŐLEGES"]
["36994","ZENERGY - OSŁONA ROZŁĄCZNIK SKRZYNKOWY EFEN SILAS; SCHN LV4 630A + ochronnik, W850, 6M / 700, POZIOMO",97.3,"1-ZE-01",null,null,"OE_EQUIPMENT_COVERS","36994","SZT","85389099",null,null,"5901988369941","OE - Couvercle interrupteur-sectionneur EFEN SILAS ; SCHN LV4 630A, L850, 6M / 700, horizontalement","OE - Cover EFEN SILAS switch box; SCHN LV4 630A, W850, 6M / 700, Horizontal","OE- TAPA CAJA INTERRUPTORES EFEN SILAS; SCHN LV4 630A, W850, 6M / 700, HORIZ.","ZENERGY - FEDŐDOBOZ KAPCSOLÓ EFEN SILAS; SCHN LV4 630A + levezető, W850, 6M / 700, VÍZSZINTES"]
["37011","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY PRZÓD,TYŁ, W1100",267.8,"1-ZE-01",3.3333333333333333E-2,1,"OE_PLINTHS","30011","SZT","85389099",null,null,"5901988370114","OE - socle H100, capots avant et arrière complets, W1100","OE - H100 plinth, full covers front, rear, W1100","OE- ZOCALO H100, CIEGO, FRONTAL/TRASERO (2UDS) W1100","ZENERGY - LÁZAT H100, TELJES BURKOLATOK ELSŐ, HÁTSÓ, W1100"]
["37012","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY PRZÓD,TYŁ, W1200",276.5,"1-ZE-01",0.2,2,"OE_PLINTHS","30012","SZT","85389099",null,null,"5901988370121","OE - Socle H100, protection intégrale avant, arrière, L1200","OE - H100 plinth, Plain covers front, rear, W1200","OE- ZOCALO H100, CIEGO, FRONTAL/TRASERO (2UDS) W1200","ZENERGY - LÁZAT H100, TELJES BURKOLATOK ELSŐ, HÁTSÓ, W1200"]
["37040","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY PRZÓD,TYŁ, W400",189,"1-ZE-01",0.76666666666666672,4,"OE_PLINTHS","30040","SZT","85389099","27.12.40.0",null,"5901988370404","OE - Socle H100, protection intégrale avant, arrière, L400","OE - H100 plinth, Plain covers front, rear, W400","OE- ZOCALO  H100, CIEGO, FRONTAL/TRASERO W400","ZENERGY - LÁZAT H100, TELJES BURKOLATOK ELSŐ, HÁTSÓ, W400"]
["37080","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY PRZÓD,TYŁ, W800",220.3,"1-ZE-01",1.2416666666666667,7,"OE_PLINTHS","30080","SZT","85389099","27.12.40.0",null,"5901988370800","OE - Socle H100, protection intégrale avant, arrière, L800","OE - H100 plinth, Plain covers front, rear, W800","OE- ZOCALO  H100, CIEGO, FRONTAL/TRASERO W800","ZENERGY - LÁZAT H100, TELJES BURKOLATOK ELSŐ, HÁTSÓ, W800"]
["37095","ZENERGY - COKÓŁ H100, PEŁNE OSŁONY PRZÓD,TYŁ, W950",248.4,"1-ZE-01",0.29166666666666669,1,"OE_PLINTHS",null,null,"85389099",null,null,"5901988370954"]
["37130","ZENERGY - COKÓŁ H200, PEŁNE OSŁONY PRZÓD,TYŁ, W300",195.5,"1-ZE-01",null,null,"OE_PLINTHS","30130","SZT","85389099",null,null,"5901988371302","OE - Socle H200, protection intégrale avant, arrière, L300","OE - H200 plinth, full covers front, rear, W300","OE- ZOCALO H200, CIEGO, FRONTAL/TRASERO (2UDS) W300","ZENERGY - LÁZAT H200, TELJES BURKOLATOK ELSŐ, HÁTSÓ, W300"]
["37165","ZENERGY - COKÓŁ H200, PEŁNE OSŁONY PRZÓD,TYŁ, W650",303.5,"1-ZE-01",0.05,1,"OE_PLINTHS","30165","SZT","85389099",null,null,"5901988371654","OE - Socle H200, protection intégrale avant, arrière, L650","OE - H200 plinth, full covers front, rear, W650","OE- ZOCALO H200, GIEGO, FRONTAL/TRASERO (2UDS) W650","ZENERGY - LÁZLET H200, TELJES BURKOLATOK ELSŐ, HÁTSÓ, W650"]
["37431","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD100-250 3/4P, W400, 3M, PIONOWO",105.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","37431","SZT","85389099","27.12.40.0",null,"5901988374310","OE - UCB/UCD100-250 3/4P, L400, plaque de montage 3M, vertical","OE - Mounting plate UCB / UCD100-250 3 / 4P, W400, 3M, Vertical","OE- PLACA MONTAJE  UCB/UCD100-250 3/4P, W400, 3M, VERTIC.","ZENERGY - SZERELŐLEMEZ UCB/UCD100-250 3/4P, W400, 3M, FÜGGŐLEGES"]
["37462","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD630-800 3/4P, W400, 6M, PIONOWO",147.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","37462","SZT","85389099","27.12.40.0",null,"5901988374624","OE - Plaque de montage UCB / UPB 800 3 / 4P, L400, 6M, verticalement + étriers","OE - Mounting plate UCB / UCD630-800 3 / 4P, W400, 6M, Vertical","OE- PLACA MONTAJE  UCB/UPB 800 3/4P, W400, 6M (300MM)  VERT. ","ZENERGY – SZERELŐLEMEZ UCB/UCD630-800 3/4P, W400, 6M, FÜGGŐLEGES"]
["37540","ZENERGY - PŁYTA MONTAŻOWA UPB/UPD100-250 3/4P, HGP250 3/4P W450, 4M, PIONOWO",133.1,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988375409","OE - Plaque de montage UCB / UPB 100-250 3 / 4P, L450, 4M, verticalement + étriers","OE - Mounting plate UPB / UPD100-250 3 / 4P, W450, 4M, Vertical","OE- PLACA MONT. UPB100-250 3/4P, HGP250 3/4P W450, 4M (200MM) VERT.","ZENERGY - SZERELŐLEMEZ UPB/UPD100-250 3/4P, HGP250 3/4P W450, 4M, FÜGGŐLEGES"]
["37554","ZENERGY - PŁYTA MONTAŻOWA UAN06-40 3/4P, A/B, W450, NA STAŁE, BEZ WSPORNIKÓW",158.69999999999999,"1-ZE-01",null,null,"OE_ACB_PLATES",null,"SZT","85389099",null,null,"5901988375546","OE - PLAQUE DE MONTAGE UAN06-40 3/4P, A/B, L450, FIXE, SANS SUPPORTS","OE - Mounting plate UAN06-40 3/4P, A/B, W450, FIXED, WITHOUT BRACKETS","*OE - PLACA DE MONTAJE UAN06-40 3/4P, A/B, W450, FIJA, SIN SOPORTES","ZENERGY - SZERELŐLAP UAN06-40 3/4P, A/B, W450, RÖGZÍTETT, KONZER NÉLKÜL"]
["37574","ZENERGY - PŁYTA MONTAŻOWA UCB1600 3P, W450, 7M, PIONOWO",174.9,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988375744","OE - UCB1600 3P, L450, plaque de montage 7M, verticale","OE - Mounting plate UCB1600 3P, W450, 7M, Vertical","OE- PLACA MONTAJE UCB1600 3P, W450, 7M, VERT.","ZENERGY - SZERELŐLAP UCB1600 3P, W450, 7M, FÜGGŐLEGES"]
["37740","ZENERGY - PŁYTA MONTAŻOWA UPB/UPD100-250 3/4P, HGP250 3/4P, W650, 4M, PIONOWO",163.9,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988377403","OE - Plaque de montage UCB / UPB 100-250 3 / 4P, L650, 4M, verticalement + étriers","OE - Mounting plate UPB / UPD100-250 3 / 4P, W650, 4M, Vertical","OE- PLACA MONT. UPB100-250 3/4P, HGP250 3/4P, W650, 4M (200MM) VERT.","ZENERGY - SZERELŐLEMEZ UPB/UPD100-250 3/4P, HGP250 3/4P, W650, 4M, FÜGGŐLEGES"]
["37749","ZENERGY - PŁYTA MONTAŻOWA UPB/UPD400-630 3P, W650, 4M, WTYKOWY, POZIOMO",163.9,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988377496","OE - UPB/UPD400-630 3P, L650, plaque de montage 4M, enfichable, horizontale","OE - Mounting plate UPB / UPD400-630 3P, W650, 4M, plug-in, Horizontal","OE- PLACA MONTAJE UPB / UPD400-630 3P, W650, 4M, enchufable, HORIZ.","ZENERGY - SZERELŐLÁM UPB/UPD400-630 3P, W650, 4M, DUGALHATÓ, VÍZSZINTES"]
["37762","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD630-800 3/4P, W650, 6M, PIONOWO",191.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","37762","SZT","85389099","27.12.40.0",null,"5901988377625","OE - Plaque de montage UCB 630-800 3 / 4P, L650, 6M, verticalement + supports","OE - Mounting plate UCB / UCD630-800 3 / 4P, W650, 6M, Vertical","OE- PLACA MONTAJE  UCB 630-800 3/4P, W650, 6M (300MM)  VERT. ","ZENERGY - SZERELŐLEMEZ UCB/UCD630-800 3/4P, W650, 6M, FÜGGŐLEGES"]
["37768","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD1000-1250 3P, W650, 6M, POZIOMO",191.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","37768","SZT","8538909900","27.12.40.0",null,"5901988377687","OE - Plaque de montage UCB 1000-1250 3P, L650, 6M, horizontale + supports","OE - Mounting plate UCB / UCD1000-1250 3P, W650, 6M, Horizontal","OE- PLACA MONTAJE  UCB 1000-1250 3P, W650, 6M (300MM)  HORIZ. ","ZENERGY - SZERELŐLEMEZ UCB/UCD1000-1250 3P, W650, 6M, VÍZSZINTES"]
["37769","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD630-800 3P, W650, 6M, WTYKOWY, POZIOMO",162.80000000000001,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988377694","OE - UCB/UCD630-800 3P, L650, plaque de montage 6M, enfichable, horizontale","OE - Mounting plate UCB / UCD630-800 3P, W650, 6M, plug-in, Horizontal","OE- PLACA MONTAJE UCB / UCD630-800 3P, W650, 6M, enchufable, HORIZ.","ZENERGY - RÖGZÍTŐLEMEZ UCB/UCD630-800 3P, W650, 6M, DUGALHATÓ, VÍZSZINTES"]
["37777","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD630-800 4P, W650, 7M, POZIOMO",205.7,"1-ZE-01",null,null,"OE_MCCB_PLATES","37777","SZT","85389099","27.12.40.0",null,"5901988377779","OE - Plaque de montage UCB 800 4P, L650, 7M, horizontale + supports","OE - Mounting plate UCB / UCD630-800 4P, W650, 7M, Horizontal","OE- PLACA MONTAJE  UCB 800 4P, W650, 7M (350MM) HORIZ. ","ZENERGY - SZERELŐLEMEZ UCB/UCD630-800 4P, W650, 7M, VÍZSZINTES"]
["37935","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD/UPB/UPD100-250 3P, HGP250 3P W850, 3M, POZIOMO",169.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","37935","SZT","85389099","27.12.40.0",null,"5901988379353","OE - UCB/UCD/UPB/UPB/UPD100-250 3P, L850, plaque de montage 3M, horizontal","OE - Mounting plate UCB / UCD / UPB / UPD100-250 3P, W850, 3M, Horizontal","OE- PLACA MONT. UPB100-250 3P, HGP250 3P W850, 3M (150MM), HORIZ.","ZENERGY - SZERELŐLEMEZ UCB/UCD/UPB/UPD100-250 3P, HGP250 3P W850, 3M, VÍZSZINTES"]
["37949","ZENERGY - PŁYTA MONTAŻOWA UPB/UPD400-630 3P, W850, 4M, WTYKOWY, POZIOMO",177.1,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988379490","OE - UPB/UPD400-630 3P, L850, plaque de montage 4M, enfichable, horizontale","OE - Mounting plate UPB / UPD400-630 3P, W850, 4M, plug-in, Horizontal","OE- PLACA MONTAJE UPB / UPD400-630 3P, W850, 4M, enchufable, HORIZ.","ZENERGY - RÖGZÍTŐLEMEZ UPB/UPD400-630 3P, W850, 4M, DUGALHATÓ, VÍZSZINTES"]
["37961","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD400, UPB/UPD400-630, W850, 6M, PIONOWO",204.6,"1-ZE-01",null,null,"OE_MCCB_PLATES","37961","SZT","85389099","27.12.40.0",null,"5901988379612","OE - UCB/UCD400, UPB/UPD400-630, L850, plaque de montage 6M, verticale","OE - Mounting plate UCB / UCD400, UPB / UPD400-630, W850, 6M, Vertical","OE- PLACA MONTAJE  UCB / UCD400, UPB / UPD400-630, W850, 6M, VERTIC.","ZENERGY - SZERELŐLEMEZ UCB/UCD400, UPB/UPD400-630, W850, 6M, FÜGGŐLEGES"]
["37967","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD630-800 3P, W850, 6M, POZIOMO",204.6,"1-ZE-01",null,null,"OE_MCCB_PLATES","37967","SZT","85389099","27.12.40.0",null,"5901988379674","OE - Plaque de montage UCB / UPB 800 3P, L850, 6M, horizontale + supports","OE - Mounting plate UCB / UCD630-800 3P, W850, 6M, Horizontal","OE- PLACA MONTAJE  UCB/UPB 800 3P, W850, 6M (300MM)  HORIZ. ","ZENERGY - SZERELŐLEMEZ UCB/UCD630-800 3P, W850, 6M, VÍZSZINTES"]
["37973","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD1000-1250 / HGM1600, W850, 7M, PIONOWO",224.4,"1-ZE-01",0.1,1,"OE_MCCB_PLATES","37973","SZT","85389099","27.12.40.0",null,"5901988379735","OE - Plaque de montage UCB 1000-1250/  HGM1600, L850, 7M, verticalement","OE - Mounting plate UCB/UCD1000-1250 / HGM1600, W850, 7M, Vertical","OE- PLACA MONTAJE  UCB 1000-1250 3/4P, W850, 7M (350MM) VERT. ","ZENERGY - SZERELŐLEMEZ UCB/UCD1000-1250 / HGM1600, W850, 7M, FÜGGŐLEGES"]
["37978","ZENERGY - PŁYTA MONTAŻOWA UCB/UCD1000-1250 4P, W850, 7M, POZIOMO",224.4,"1-ZE-01",null,null,"OE_MCCB_PLATES","37978","SZT","85389099","27.12.40.0",null,"5901988379780","OE - UCB/UCD1000-1250 4P, L850, plaque de montage 7M, horizontale","OE - Mounting plate UCB / UCD1000-1250 4P, W850, 7M, Horizontal","OE- PLACA MONTAJE  UCB 1000-1250 4P, W850, 7M (350MM) HORIZ. ","ZENERGY - SZERELŐLEMEZ UCB/UCD1000-1250 4P, W850, 7M, VÍZSZINTES"]
["38035","ZENERGY OM - OSŁONA CZOŁOWA UPB 100-250 3P; HGP250 3P, W1000, 3M / 900, POZIOMO, DŹWIGNIA",81.400000000000006,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988380359","OM - Couvercle avant UPB 100-250 3P, L1000, 3M / 900, horizontal, levier","OM - Front visor UPB 100-250 3P, W1000, 3M / 900, Horizontal, Lever","OM- TAPA TROQ. UPB 100-250 3P; HGP250 3P, W1000, 3M (150MM) HORIZ. ","ZENERGY OM - ELSŐ BURKOLAT UPB 100-250 3P; HGP250 3P, W1000, 3M / 900, VÍZSZINTES, KAR"]
["38050","ZENERGY OM - OSŁONA CZOŁOWA UPB 100-250 3/4P; HGP250 3/4P, W1000, 5M / 900, PIONOWO, DŹWIGNIA",90.4,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988380502","OM - Couvercle avant UPB 100-250 3 / 4P, L1000, 5M / 900, vertical, levier","OM - Front visor UPB 100-250 3 / 4P, W1000, 5M / 900, Vertical, Lever","OM- TAPA TROQ. UPB 100-250 3/4P; HGP250 3/4P, W1000, 5M (250MM) VERT.","ZENERGY OM - ELSŐ BURKOLAT UPB 100-250 3/4P; HGP250 3/4P, W1000, 5M / 900, FÜGGŐLEGES, KAR"]
["38091","ZENERGY OM - OSŁONA CZOŁOWA UPB 400-630 3/4P, W1000, 9M / 900, PIONOWO, DŹWIGNIA",143,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988380915","OM - Couvercle avant UPB 400-630 3 / 4P, L1000, 9M / 900, vertical, levier","OM - Front visor UPB 400-630 3 / 4P, W1000, 9M / 900, Vertical, Lever","OM- TAPA TROQ. UPB 400-630 3/4P, W1000, 9M (450MM)  VERT.","ZENERGY OM - ELSŐ BURKOLAT UPB 400-630 3/4P, W1000, 9M / 900, FÜGGŐLEGES, KAR"]
["38145","ZENERGY OM - OSŁONA CZOŁOWA UCB 160-250 4P, W1000, 4M / 900, POZIOMO, DŹWIGNIA",86.9,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988381455","OM - Capot avant UCB 160-250 4P, L1000, 4M / 900, horizontal, effet de levier","OM - Front cover UCB 160-250 4P, W1000, 4M / 900, Horizontal, Lever","OM- TAPA TROQ. UCB 160-250 4P, W1000, 4M (200MM)  HORIZ.","ZENERGY OM - ELSŐ BURKOLAT UCB 160-250 4P, W1000, 4M / 900, VÍZSZINTES, KAR"]
["38150","ZENERGY OM - OSŁONA CZOŁOWA UCB 160-250 3/4P, W1000, 5M / 900, PIONOWO, DŹWIGNIA",94.4,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988381509","OM - Capot avant UCB 160-250 3 / 4P, L1000, 5M / 900, vertical, levier","OM - Front cover UCB 160-250 3 / 4P, W1000, 5M / 900, Vertical, Lever","OM- TAPA TROQ. UCB 160-250 3/4P, W1000, 5M (250MM)  VERT.","ZENERGY OM - ELSŐ BURKOLAT UCB 160-250 3/4P, W1000, 5M / 900, FÜGGŐLEGES, KAROS"]
["38177","ZENERGY OM - OSŁONA CZOŁOWA UCB 630-800 4P, W1000, 7M / 900, POZIOMO, DŹWIGNIA",126.5,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988381776","OM - Capot avant UCB 630-800 4P, L1000, 7M / 900, horizontal, levier","OM - Front cover UCB 630-800 4P, W1000, 7M / 900, Horizontal, Lever","OM- TAPA TROQ. UCB 630-800 4P, W1000, 7M (350MM)  HORIZ.","ZENERGY OM - ELSŐ BURKOLAT UCB 630-800 4P, W1000, 7M / 900, VÍZSZINTES, KAR"]
["38192","ZENERGY OM - OSŁONA CZOŁOWA UCB 630-800 3P, W1000, 9M / 900, PIONOWO, DŹWIGNIA",148.5,"1-ZE-09",null,null,"OE_MCCB_COVERS",null,"SZT","85381000","27.12.40.0",null,"5901988381929","OM - Capot avant UCB 630-800 3P, L1000, 9M / 900, vertical, levier","OM - Front cover UCB 630-800 3P, W1000, 9M / 900, Vertical, Lever","OM- TAPA TROQ. UCB 630-800 3P, W1000, 9M (450MM)  VERT.","ZENERGY OM - ELSŐ BURKOLAT UCB 630-800 3P, W1000, 9M / 900, FÜGGŐLEGES, KAR"]
["38260","ZENERGY - OSŁONA CZOŁOWA HGP/UPB 100-250 3/4P DŁUGA OSŁONA ZACISKÓW, W400, 6M / 250, PIONOWO, DŹWIGNIA",60,null,null,null,"OE_MCCB_COVERS",null,null,"",null,null,"5901988382605"]
["38291","ZENERGY - OSŁONA CZOŁOWA UPB 400-630 3/4P, W400, 9M / 250, PIONOWO, DŹWIGNIA",93.8,"1-ZE-01",0.01,1,"OE_MCCB_COVERS","38291","SZT","85389099",null,null,"5901988382919","OE - Panneau avant UPB 400-630 3 / 4P, L400, 9M / 250, vertical, levier","OE - Front visor UPB 400-630 3 / 4P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. UPB 400-630 3/4P, W400, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UPB 400-630 3/4P, W400, 9M / 250, FÜGGŐLEGES, KAR"]
["38334","ZENERGY - OSŁONA CZOŁOWA UCB 100 3P, W400, 3M / 250, POZIOMO, DŹWIGNIA",49.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","38334","SZT","85389099",null,null,"5901988383343","OE - Capot avant UCB 100 3P, L400, 3M / 250, horizontal, levier","OE - Front cover UCB 100 3P, W400, 3M / 250, Horizontal, Lever","OE- TAPA TROQ. UCB 100 3P, W400, 3M (150MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 100 3P, W400, 3M / 250, VÍZSZINTES, KAR"]
["38345","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 4P, W400, 4M / 250, POZIOMO, DŹWIGNIA",52.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","38345","SZT","85389099",null,null,"5901988383459","OE - Capot avant UCB 160-250 4P, L400, 4M / 250, horizontal, levier","OE - Front cover UCB 160-250 4P, W400, 4M / 250, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 4P, W400, 4M (200MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 4P, W400, 4M / 250, VÍZSZINTES, KAR"]
["38351","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 4P, W400, 5M / 250, PIONOWO, DŹWIGNIA",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85371098","27.12.31.0",null,"5901988383510","OE - Couvercle avant UCB 160-250 4P, L400, 5M / 250, vertical, levier","OE - Front cover UCB 160-250 4P, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 160-250 4P, W400, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 4P, W400, 5M / 250, FÜGGŐLEGES, KAR"]
["38391","ZENERGY - OSŁONA CZOŁOWA UCB 400 4P, W400, 9M / 250, PIONOWO, DŹWIGNIA",98.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","38391","SZT","85371098","27.12.31.0",null,"5901988383916","OE - Couvercle avant UCB 400 4P, L400, 9M / 250, vertical, levier","OE - Front visor UCB 400 4P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. UCB 400 4P, W400, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 400 4P, W400, 9M / 250, FÜGGŐLEGES, KAR"]
["38450","ZENERGY - OSŁONA CZOŁOWA UPB:100-250 3/4P; HGP250 3/4P, W450, 5M / 300, PIONOWO, DŹWIGNIA",65.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","38450","SZT","85389099","27.12.40.0",null,"5901988384500","OE - Couvercle avant HGP 250, UPB 100-250 3 / 4P, L450, 5M / 300, vertical, levier","OE - Front visor HGP 250, UPB 100-250 3 / 4P, W450, 5M / 300, Vertical, Lever","ZEN- TAPA TROQ. HGP250 3/4P, W450, 5M (250MM) VERT.","ZENERGY - ELSŐ BURKOLAT UPB:100-250 3/4P; HGP250 3/4P, W450, 5M / 300, FÜGGŐLEGES, KAR"]
["38522","ZENERGY - OSŁONA CZOŁOWA UCB 1000-1250 3P, W450, 12M / 300, PIONOWO, DŹWIGNIA",115.5,"1-ZE-01",0.01,1,"OE_MCCB_COVERS","38522","SZT","85389099","27.12.40.0",null,"5901988385224","OE - Capot avant UCB 1000-1250 3P, L450, 12M / 300, vertical, levier","OE - Front cover UCB 1000-1250 3P, W450, 12M / 300, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 3P, W450, 12M (600MM) VERT.","ZENERGY - ELSŐ BURKOLAT UCB 1000-1250 3P, W450, 12M / 300, FÜGGŐLEGES, KAR"]
["38544","ZENERGY - OSŁONA CZOŁOWA UCB 100 4P, W450, 4M / 300, POZIOMO, DŹWIGNIA",58.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38544","SZT","85389099","27.12.40.0",null,"5901988385446","OE - Capot avant UCB 100 4P, L450, 4M / 300, horizontal, levier","OE - Front cover UCB 100 4P, W450, 4M / 300, Horizontal, Lever","OM- TAPA TROQ. UCB 100 4P, W450, 4M (200MM) HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 100 4P, W450, 4M / 300, VÍZSZINTES, KAR"]
["38545","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 4P, W450, 4M / 300, POZIOMO, DŹWIGNIA",58.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38545","SZT","85389099","27.12.40.0",null,"5901988385453","OE - Capot avant UCB 160-250 4P, L450, 4M / 300, horizontal, effet de levier","OE - Front cover UCB 160-250 4P, W450, 4M / 300, Horizontal, Lever","OM- TAPA TROQ. UCB 160-250 4P, W450, 4M (200MM) HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 4P, W450, 4M / 300, VÍZSZINTES, KAR"]
["38551","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 4P, W450, 5M / 300, PIONOWO, DŹWIGNIA",65.5,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988385514","OE - Capot avant UCB 160-250 4P, L450, 5M / 300, vertical, levier","OE - Front cover UCB 160-250 4P, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. UCB 160-250 4P, W450, 5M (250MM) VERT.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 4P, W450, 5M / 300, FÜGGŐLEGES, KAR"]
["38592","ZENERGY - OSŁONA CZOŁOWA UCB 630-800 3P, W450, 9M / 300, PIONOWO, DŹWIGNIA",106.2,"1-ZE-01",null,null,"OE_MCCB_COVERS","38592","SZT","85389099","27.12.40.0",null,"5901988385927","OE - Capot avant UCB 630-800 3P, L450, 9M / 300, vertical, levier","OE - Front cover UCB 630-800 3P, W450, 9M / 300, Vertical, Lever","OM- TAPA TROQ. UCB 630-800 3P, W450, 9M (450MM) VERT.","ZENERGY - ELSŐ BURKOLAT UCB 630-800 3P, W450, 9M / 300, FÜGGŐLEGES, KAR"]
["38642","ZENERGY - OSŁONA CZOŁOWA UAB 100 3/4P, W650, 4M / 500, PIONOWO, DŹWIGNIA",76.5,"1-ZE-01",null,null,"OE_ACB_COVERS","38642","SZT","85389099","27.12.40.0","230622RT","5901988386429","OE - Couvercle avant UAB 100 3 / 4P, L650, 4M / 500, vertical, levier","OE - Front visor UAB 100 3 / 4P, W650, 4M / 500, Vertical, Lever","OE- TAPA TROQ. UAB 100 3/4P, W650, 4M / 500, VERT.","ZENERGY - ELSŐ BURKOLAT UAB 100 3/4P, W650, 4M / 500, FÜGGŐLEGES, KAR"]
["38647","OE - Osłona czołowa HGP250 4P, W650, 4M / 500, poziomo, silnik",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","38647","SZT",null,null,"240506PW",null,"OE - Panneau avant HGP250 4P, W650, 4M / 500, horizontal, moteur","OE - Front cover HGP250 4P, W650, 4M / 500, horizontal, motor","OE - Tapa frontal HGP250 4P, W650, 4M / 500, horizontal, motor","OE - Első burkolat HGP250 4P, W650, 4M / 500, vízszintes, motor"]
["38653","OE - Osłona czołowa HGP250 4P, W650, 5M / 500, pionowo, silnik",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38653","SZT",null,null,"240515PW","5901988386535","OE - Panneau avant HGP250 4P, W650, 5M / 500, vertical, moteur","OE - Front cover HGP250 4P, W650, 5M / 500, vertical, motor","OE - Tapa frontal HGP250 4P, W650, 5M / 500, vertical, motor","OE - Első burkolat HGP250 4P, W650, 5M / 500, függőleges, motor"]
["38690","ZENERGY - OSŁONA CZOŁOWA 1x UPB 400-630 3/4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",125.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","38690","SZT","85389099","27.12.40.0",null,"5901988386900","OE - Panneau avant 1x UPB 400-630 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 1x UPB 400-630 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. 1X UPB 400-630 3/4P, W650, 9M/500, VERTIC. ","ZENERGY - ELSŐ BURKOLAT 1x UPB 400-630 3/4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["38706","ZENERGY - OSŁONA CZOŁOWA UCB 1000-1250 3/4P, W650, 12M / 500, PIONOWO, SILNIK",135.30000000000001,"1-ZE-01",0.01,1,"OE_MCCB_COVERS","38706","SZT","85389099","27.12.40.0",null,"5901988387068","OE - Capot avant UCB 1000-1250 3 / 4P, L650, 10M / 500, verticalement, moteur","OE - Front cover UCB 1000-1250 3 / 4P, W650, 12M / 500, Vertical, engine","OE- TAPA TROQ. UCB 1000-1250 3/4P, W650, 10M (500MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 1000-1250 3/4P, W650, 12M / 500, FÜGGŐLEGES, MOTOR"]
["38709","ZENERGY - OSŁONA CZOŁOWA UAN 06-32 3/4P, A, W650, 10M / 500, WYSUWNY",157.6,"1-ZE-01",4.1666666666666664E-2,1,"OE_ACB_COVERS","38709","SZT","85389099","27.12.40.0",null,"5901988387099","OE - Couvercle avant UAN 06-32 3 / 4P, A, L650, 10M / 500, débrochable","OE - Front cover UAN 06-32 3 / 4P, A, W650, 10M / 500, withdrawable","OE- TAPA TROQ. UAN TIPO A 06-32 3/4P, W650, 10M (500MM)  EXTR.","ZENERGY - ELSŐ BURKOLAT UAN 06-32 3/4P, A, W650, 10M / 500, CSÚSZTÓ"]
["38712","ZENERGY - OSŁONA CZOŁOWA UAN 06-32 3/4P, A, W650, 10M / 500, WYSUWNY + ANALIZATOR",157.6,"1-ZE-01",0.01,1,"OE_ACB_COVERS",null,"SZT","8538909900",null,null,"5901988387129","OE - CAPOT AVANT UAN 06-32 3/4P, A, L650, 10M/500, RETRAIT + ANALYSEUR","OE - Front cover UAN 06-32 3/4P, A, W650, 10M / 500, withdrawal + analyzer","*OE - TAPA FRONTAL UAN 06-32 3/4P, A, W650, 10M/500, EXTRACCIÓN + ANALIZADOR","ZENERGY - ELSŐ BURKOLAT UAN 06-32 3/4P, A, W650, 10M / 500, KIVEZETÉS + ELEMZŐ"]
["38723","ZENERGY - OSŁONA CZOŁOWA UCB 1000-1250 4P, W650, 12M / 500, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988387235","OE - Capot avant UCB 1000-1250 4P, L650, 12M / 500, vertical, levier","OE - Front cover UCB 1000-1250 4P, W650, 12M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 1000-1250 4P, W650, 12M (600MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 1000-1250 4P, W650, 12M / 500, FÜGGŐLEGES, KAROS"]
["38745","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 4P, W650, 4M / 500, POZIOMO, DŹWIGNIA",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","38745","SZT","85389099","27.12.40.0",null,"5901988387457","OE - Capot avant UCB 160-250 4P, L650, 4M / 500, horizontal, effet de levier","OE - Front cover UCB 160-250 4P, W650, 4M / 500, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 4P, W650, 4M (200MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 4P, W650, 4M / 500, VÍZSZINTES, KAR"]
["38750","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 3/4P, W650, 5M / 500, PIONOWO, DŹWIGNIA",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38750","SZT","85389099","27.12.40.0",null,"5901988387501","OE - Couvercle avant UCB 160-250 3 / 4P, L650, 5M / 500, vertical, levier","OE - Front cover UCB 160-250 3 / 4P, W650, 5M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 160-250 3/4P, W650, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 3/4P, W650, 5M / 500, FÜGGŐLEGES, KAROS"]
["38769","ZENERGY - OSŁONA CZOŁOWA UCB 630-800 3P, W650, 6M / 500, POZIOMO, SILNIK",82.7,"1-ZE-01",null,null,"OE_MCCB_COVERS","38769","SZT","85389099","27.12.40.0",null,"5901988387693","OE - Capot avant UCB 630-800 3P, L650, 6M / 500, horizontal, moteur","OE - Front cover UCB 630-800 3P, W650, 6M / 500, Horizontal, Engine","OE- TAPA TROQ. UCB 630-800 3P, W650, 6M (300MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 630-800 3P, W650, 6M / 500, VÍZSZINTES, MOTOR"]
["38779","ZENERGY - OSŁONA CZOŁOWA UCB 630-800 4P, W650, 7M / 500, POZIOMO, SILNIK",108.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","38779","SZT","85389099","27.12.40.0",null,"5901988387792","OE - Capot avant UCB 630-800 4P, L650, 7M / 500, horizontal, moteur","OE - Front cover UCB 630-800 4P, W650, 7M / 500, Horizontal, Engine","OE- TAPA TROQ. UCB 630-800 4P, W650, 7M (350MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 630-800 4P, W650, 7M / 500, VÍZSZINTES, MOTOR"]
["38791","ZENERGY - OSŁONA CZOŁOWA 2x UCB 400 3/4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",0.01,1,"OE_MCCB_COVERS","38791","SZT","85389099","27.12.40.0",null,"5901988387914","OE - Couvercle avant 2x UCB 400 3 / 4P, L650, 9M / 500, vertical, levier","OE - Front cover 2x UCB 400 3 / 4P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 400 3/4P, W650, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT 2x UCB 400 3/4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["38792","ZENERGY - OSŁONA CZOŁOWA UCB 630-800 3P, W650, 9M / 500, PIONOWO, DŹWIGNIA",135.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","38792","SZT","85389099","27.12.40.0",null,"5901988387921","OE - Capot avant UCB 630-800 3P, L650, 9M / 500, vertical, levier","OE - Front cover UCB 630-800 3P, W650, 9M / 500, Vertical, Lever","OE- TAPA TROQ. UCB 630-800 3P, W650, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 630-800 3P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["38795","ZENERGY - OSŁONA CZOŁOWA UAN 08-40 3/4P, B, W650, 9M / 500, NA STAŁE",157.6,"1-ZE-01",0.24166666666666667,4,"OE_ACB_COVERS","38795","SZT","85389099","27.12.40.0",null,"5901988387952","OE - Couvercle avant UAN 08-40 3 / 4P, B, L650, 9M / 500, fixe","OE - Front cover UAN 08-40 3 / 4P, B, W650, 9M / 500, permanent","OE- TAPA TROQ. UAN 08-40 3/4P, B, W650, 9M (450MM)  FIJO","ZENERGY - ELSŐ BURKOLAT UAN 08-40 3/4P, B, W650, 9M / 500, ÁLLANDÓ"]
["38845","ZENERGY - OSŁONA CZOŁOWA UPB:100-250 4P; HGP250 4P, W850, 4M / 700, POZIOMO, DŹWIGNIA",85,"1-ZE-01",null,null,"OE_MCCB_COVERS","38845","SZT","85389099","27.12.40.0",null,"5901988388454","OE - Capot avant HGP 250, UPB 100-250 4P, L850, 4M / 700, horizontal, levier","OE - Front visor HGP 250, UPB 100-250 4P, W850, 4M / 700, Horizontal, Lever","ZEN- TAPA TROQ. HGP250 4P, W850, 4M (200MM) HORIZ. ","ZENERGY - ELSŐ BURKOLAT UPB:100-250 4P; HGP250 4P, W850, 4M / 700, VÍZSZINTES, KAR"]
["38856","ZENERGY - OSŁONA CZOŁOWA UPB 400-630 4P, W850, 5M / 700, POZIOMO, DŹWIGNIA",87.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","38856","SZT","85389099","27.12.40.0",null,"5901988388560","OE - Capot avant UPB 400-630 4P, L850, 5M / 700, horizontal, levier","OE - Front cover UPB 400-630 4P, W850, 5M / 700, Horizontal, Lever","OE- TAPA TROQ. UPB 400-630 4P, W850, 5M (250MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UPB 400-630 4P, W850, 5M / 700, VÍZSZINTES, KAR"]
["38909","ZENERGY - OSŁONA CZOŁOWA UAN 06-32 3/4P, A, W850, 10M / 700, WYSUWNY",176,"1-ZE-01",null,null,"OE_ACB_COVERS","38909","SZT","85389099","27.12.40.0",null,"5901988389093","OE - Couvercle avant UAN 06-32 3 / 4P,A, L850, 10M / 700, débrochable","OE - Front cover UAN 06-32 3 / 4P, W850, 10M / 700, Removable","OE- TAPA TROQ. UAN A 06-32 3/4P, W850, 10M (500MM)  EXTR.","ZENERGY - ELSŐ BURKOLAT UAN 06-32 3/4P, A, W850, 10M / 700, CSÚSZTÓ"]
["38921","ZENERGY - OSŁONA CZOŁOWA 2X UCB 1000-1250 4P, W850, 12M / 700, PIONOWO, DŹWIGNIA",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38920","SZT","85389099","27.12.40.0",null,"5901988389215","OE - Capot avant 2x UCB 1000-1250 4P, L850, 12M / 700, vertical, levier","OE - Front cover 2x UCB 1000-1250 4P, W850, 12M / 700, Vertical, Lever","OE- TAPA TROQ. 2X UCB 1000-1250 4P, W850, 12M (600MM)  VERT.","ZENERGY - ELSŐ BURKOLAT 2X UCB 1000-1250 4P, W850, 12M / 700, FÜGGŐLEGES, KAR"]
["38924","ZENERGY - OSŁONA CZOŁOWA UCB 1600 3P, W850, 12M / 700, PIONOWO, DŹWIGNIA",168.3,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988389246","OE - Couvercle avant UCB 1600 3P, L850, 12M / 700, vertical, levier","OE - Front cover for UCB 1600 3P, W850, 12M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 1600 3P, W850, 12M (600MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 1600 3P, W850, 12M / 700, FÜGGŐLEGES, KAR"]
["38944","ZENERGY - OSŁONA CZOŁOWA UCB 100 4P, W850, 4M / 700, POZIOMO, DŹWIGNIA",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38944","SZT","85389099","27.12.40.0",null,"5901988389444","OE - Capot avant UCB 100 4P, L850, 4M / 700, horizontal, levier","OE - Front cover UCB 100 4P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 100 4P, W850, 4M (200MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 100 4P, W850, 4M / 700, VÍZSZINTES, KAR"]
["38945","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 4P, W850, 4M / 700, POZIOMO, DŹWIGNIA",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","38945","SZT","85389099","27.12.40.0",null,"5901988389451","OE - Capot avant UCB 160-250 4P, L850, 4M / 700, horizontal, effet de levier","OE - Front cover UCB 160-250 4P, W850, 4M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 160-250 4P, W850, 4M (200MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 4P, W850, 4M / 700, VÍZSZINTES, KAR"]
["38950","ZENERGY - OSŁONA CZOŁOWA UCB 160-250 3/4P, W850, 5M / 700, PIONOWO, DŹWIGNIA",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","38950","SZT","85389099","27.12.40.0",null,"5901988389505","OE - Couvercle avant UCB 160-250 3 / 4P, L850, 5M / 700, vertical, levier","OE - Front cover UCB 160-250 3 / 4P, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 160-250 3/4P, W850, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 160-250 3/4P, W850, 5M / 700, FÜGGŐLEGES, KAROS"]
["38977","ZENERGY - OSŁONA CZOŁOWA UCB 630-800 4P, W850, 7M / 700, POZIOMO, DŹWIGNIA",125.4,"1-ZE-01",null,null,"OE_MCCB_COVERS","38977","SZT","85389099","27.12.40.0",null,"5901988389772","OE - Capot avant UCB 630-800 4P, L850, 7M / 700, horizontal, levier","OE - Front cover UCB 630-800 4P, W850, 7M / 700, Horizontal, Lever","OE- TAPA TROQ. UCB 630-800 4P, W850, 7M (350MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT UCB 630-800 4P, W850, 7M / 700, VÍZSZINTES, KAR"]
["38991","ZENERGY - OSŁONA CZOŁOWA UCB 400 3/4P, W850, 9M / 700, PIONOWO, DŹWIGNIA",146.30000000000001,"1-ZE-01",null,null,"OE_MCCB_COVERS","38991","SZT","85389099","27.12.40.0",null,"5901988389918","OE - Couvercle avant UCB 400 3 / 4P, L850, 9M / 700, vertical, levier","OE - Front cover UCB 400 3 / 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. UCB 400 3/4P, W850, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT UCB 400 3/4P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["38994","ZENERGY - OSŁONA CZOŁOWA UAN 06-20 3/4P, A, W850, 9M / 700, NA STAŁE",166.8,"1-ZE-01",6.6666666666666666E-2,4,"OE_ACB_COVERS","38994","SZT","85389099","27.12.40.0",null,"5901988389949","OE - Couvercle avant UAN 06-20 3 / 4P, A, L850, 9M / 700, permanent","OE - Front cover UAN 06-20 3 / 4P, A, W850, 9M / 700, permanent","OE- TAPA TROQ. UAN 06-20 3/4P, A, W850, 9M (450MM)  FIJO","ZENERGY - ELSŐ BURKOLAT UAN 06-20 3/4P, A, W850, 9M / 700, ÁLLANDÓ"]
["39044","ZENERGY - PŁYTA MONTAŻOWA HGP:400-630 3P POZIOMO, W1000, 4M, BEZ WSPORNIKÓW",194.7,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988390440","OE - PLAQUE DE MONTAGE HGP:400-630 3P HORIZONTAL, L1000, 4M, SANS SUPPORTS","OE - Mounting plate HGP:400-630 3P Horizontal, W1000, 4M, WITHOUT BRACKETS","OE- PLACA MONT. HGP400-630 3P HORIZ. W1000, 4M, ","ZENERGY - SZERELŐLEMEZ HGP:400-630 3P VÍZSZINTES, W1000, 4M, KONZER NÉLKÜL"]
["39046","ZENERGY - PŁYTA MONTAŻOWA UPB:100-250; HGP250 PIONOWO / HGM, UCB:160-250 4P, 400 3P; UPB:100-250, 400-630 3P; HGP250 POZIOMO, W1000, 4M, BEZ WSPORNIKÓW",194.7,"1-ZE-01",null,null,"OE_MCCB_PLATES",null,"SZT","85389099",null,null,"5901988390464","OE - plaque de montage HGP:250, UPB: 100-250 verticalement / HGM, UCB: 160-250 4P, 400 3P; HGP:250, UPB: 100-250, 400-630 3P horizontal, L1000, 4M, sans supports","OE - Mounting plate UPB: 100-250 Vertical / HGM, UCB: 160-250 4P, 400 3P; UPB: 100-250, 400-630 3P Horizontal, W1000, 4M, without brackets","OE- PLACA MONT. HGP250 VERT. / HGM160-250 4P, 400 3P;  HGP250 HORIZ. W1000","ZENERGY - SZERELŐLAP UPB:100-250; HGP250 VERTICAL / HGM, UCB:160-250 4P, 400 3P; UPB: 100-250, 400-630 3P; HGP250 HORIZONTAL, W1000, 4M, TÁMOGATÁS NÉLKÜL"]
["39070","Zenergy - izolator wsporczy 3x 10mm / 70mm Poliamid PA66GF25",39.200000000000003,"1-ZE-01",87.216666666666669,7,"OE_INSULATOR_WIDTH","39070","SZT","85469010","27.33.14.0","230404LK","5901988390709","Zenergy - support isolateur 3x 10mm / 70mm Polyamide PA66GF25","Zenergy - support insulator 3x 10mm / 70mm Polyamide PA66GF25","*OE - aislador soporte 3x 10mm / 70mm Poliamida PA66GF25","Zenergy - oszlop szigetelő 3x 10mm / 70mm poliamid PA66GF25"]
["39100","OE - Wspornik izolatora na plecach W1000, regulowana wysokość",194.9,"1-ZE-01",1.6666666666666666E-2,1,"OE_INSULATOR_WIDTH","39100","SZT","85389099",null,"231013LK","5901988398507","OE - Support d'isolant à l'arrière W1000","OE - Insulator support on back W1000","OE - Soporte aislante en la parte posterior W1000","OE - W1000 hátszigetelő támaszték, állítható magasságú"]
["39120","OE - Wspornik izolatora na plecach W1200, most poziomy",216,null,0.71666666666666667,4,"OE_INSULATOR_WIDTH",null,null,"85469010",null,null,"5901988391201"]
["39200","ZENERGY - IZOLATOR WSPORCZY ROZSTAW 60MM SZYN 30X10MM 3P",61.2,"1-ZE-01",8.0083333333333329,1,"OE_INSULATOR_WIDTH","39200","SZT","85472000","27.33.14.0","230404LK","5901988392000","OE - Entretoise de support espacement 60mm rails 30x10mm 3P","OE - Supporting insulator 60mm spacing 30x10mm 3P","OE- SOPORTE AUX. SEPARACION 60MM BARRA 30X10MM 3P","ZENERGY - OSZTÓSZIGETELŐ 60MM BUSZHELY 30X10MM 3P"]
["39203","Zenergy - Uchwyt kablowy UK-4675 średnica kabla 46-75mm",33.299999999999997,"1-ZE-01",null,null,"OE_SUPPORT","39203","SZT","85389099",null,null,"5901988392031","OE - Serre-câble UK-4675, diamètre de câble 46-75 mm","OE - UK-4675 cable holder, cable diameter 46-75mm","OE- SOPORTE PARA CABLES UK-4675, DIÁMETRO DEL CABLE 46-75 MM","Zenergy - UK-4675 kábeltartó, kábel átmérője 46-75mm"]
["39221","ZENERGY MCC - STAŁY STYK STEROWANIA",8.9,"1-ZE-01",14.216666666666667,2,"OE_MCC","39221","SZT","85389099",null,null,"5901988392215","MCC - CONTACT DE COMMANDE FIXE","MCC - FIXED CONTROL CONTACT","MCC - CONTACTO DE CONTROL FIJO","ZENERGY MCC – ÁLLANDÓ VEZÉRLÉS KAPCSOLAT"]
["39225","ZENERGY MCC - SZCZĘKA ODPŁYWOWA 250A - CZARNA",34.5,"1-ZE-01",null,null,"OE_MCC","39225","KPL","85389099",null,null,"5901988392253","MCC - JOINT DE DRAIN 250A - NOIR","MCC - DRAIN JAW 250A - BLACK","MCC - BOQUILLA DE DRENAJE 250A - NEGRO","ZENERGY MCC - CSERÉLŐPOFÁK 250A - FEKETE"]
["39228","ZENERGY MCC - SZCZĘKA ZASILAJĄCA 800A - CZERWONA",91.4,"1-ZE-01",null,null,"OE_MCC","39228","SZT","85389099",null,null,"5901988392284","MCC - POWER JAW 800A - ROUGE","MCC - POWER JAW JAW 800A - RED","MCC - POWER JAW JAW 800A - ROJO","ZENERGY MCC - POWER JAWS 800A - PIROS"]
["39229","ZENERGY MCC - SZCZĘKA ODPŁYWOWA 800A - CZARNA",91.4,"1-ZE-01",3.2583333333333333,2,"OE_MCC","39229","SZT","85389099",null,"200914PK","5901988392291","MCC - JOINT DE DRAIN 800A - NOIR","MCC - DRAIN JOINT 800A - BLACK","MCC - JUNTA DE DRENAJE 800A - NEGRO","ZENERGY MCC - NYERŐ POFA 800A - FEKETE"]
["39232","ZENERGY - IZOLATOR WSPORCZY ALCUBAR 630A, 27 X 27 MM -  KPL. 2 ELEMENTY",30.8,"1-ZE-01",65.900000000000006,4,"OE_INSULATORS",null,"KPL","8547200090","27.33.14.0",null,"5901988392321","OE - Isolant de soutien AlCubar 630A, 27 x 27 mm - kpl. 2 éléments","OE - AlCubar post insulator 630A, 27 x 27 mm - set 2 pieces","OE- SOPORTE DE REFUERZO ALCUB 630A, 27 X 27 MM - 2 ELEMENTOS","ZENERGY - OSZTÓSZIGETELŐ ALCUBAR 630A, 27 X 27 MM - SZETT. 2 ELEM"]
["39236","ZENERGY - PŁYTA MONTAŻOWA HGM, UCB:100-250 PIONOWO / HGM, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P POZIOMO, W400, 3M, BEZ WSPORNIKÓW",98,"1-ZE-01",null,null,"OE_MCCB_PLATES","39236","SZT","85389099","27.12.40.0",null,"5901988392369","OE - Plaque de montage HGM, UCB: 100-250 verticalement / HGM, UCB: 100, 160-250 3P, HGP:250 3P, UPB: 100-250 3P horizontal, L400, 3M, sans supports","OE - Mounting plate HGM, UCB: 100-250 Vertical / HGM, UCB: 100, 160-250 3P, HGP:250, UPB: 100-250 3P Horizontal, W400, 3M, without brackets","OE- PLACA MONT. HGM100-250 VERT. / HGM100, 160-250 3P;  HGP250 3P HORIZ. W400","ZENERGY - SZERELŐLEMEZ HGM, UCB:100-250 FÜGGŐLEGES / HGM, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P VÍZSZINTES, W400, 3M, KONZER NÉLKÜL"]
["39254","ZENERGY - PŁYTA MONTAŻOWA HGP:400-630 3/4P PIONOWO / HGP:400-630 4P POZIOMO, W400, 5M, BEZ WSPORNIKÓW",116.6,"1-ZE-01",null,null,"OE_MCCB_PLATES","39254","SZT","85389099",null,null,"5901988392543","OE - PLAQUE DE MONTAGE HGP:400-630 3/4P VERTICALEMENT / HGP:400-630 4P HORIZONTALEMENT, L400, 5M, SANS SUPPORTS","OE - Mounting plate HGP:400-630 3/4P VerticalLY / HGP:400-630 4P HorizontalLY, W400, 5M, WITHOUT BRACKETS","OE- PLACA MONT. HGP400-630 3/4P VERT. / HGP400-630 4P HORIZ. W400, 5M, ","ZENERGY - SZERELŐLEMEZ HGP:400-630 3/4P FÜGGŐLEGES / HGP:400-630 4P VÍZSZINTES, W400, 5M, KONZER NÉLKÜL"]
["39266","ZENERGY - PŁYTA MONTAŻOWA HGP800 3/4P; HGM, UCB:630-800 3P PIONOWO, W400, 6M, BEZ WSPORNIKÓW",122.1,"1-ZE-01",null,null,"OE_MCCB_PLATES","39266","SZT","85389099",null,null,"5901988392666","OE - Plaque de montage HGP800 3/4P, HGM, UCB: 630-800 3P verticalement, L400, 6M, sans supports","OE - Mounting plate HGP800 3/4P, HGM, UCB: 630-800 3P Vertical, W400, 6M, without brackets","OE- PLACA MONTAJE  HGM 630-800 3P VERT. W400, 6M   ","ZENERGY - SZERELŐLAP HGP800 3/4P; HGM, UCB: 630-800 3P FÜGGŐLEGES, W400, 6M, TARTÓK NÉLKÜL"]
["39350","ZENERGY - OSŁONA CZOŁOWA HGM 100 3/4P, W400, 5M / 250, PIONOWO, DŹWIGNIA",56.1,"1-ZE-01",null,null,"OE_MCCB_COVERS","39350","SZT","85381000","27.12.40.0",null,"5901988393502","OE - Couvercle avant HGM 100 3 / 4P, L400, 5M / 250, vertical, levier","OE - HGM 100 3 / 4P front visor, W400, 5M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 100 3/4P, W400, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT HGM 100 3/4P, W400, 5M / 250, FÜGGŐLEGES, KAR"]
["39394","ZENERGY - OSŁONA CZOŁOWA HGM 630-800 3P, W400, 9M / 250, PIONOWO, DŹWIGNIA",93.8,"1-ZE-01",1.6666666666666666E-2,1,"OE_MCCB_COVERS","39394","SZT","85389099",null,null,"5901988393946","OE - Couvercle avant HGM 630-800 3P, L400, 9M / 250, vertical, levier","OE - Front Cover HGM 630-800 3P, W400, 9M / 250, Vertical, Lever","OE- TAPA TROQ. HGM 630-800 3P, W400, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT HGM 630-800 3P, W400, 9M / 250, FÜGGŐLEGES, KAR"]
["39401","ALCUBAR / CU - WSPORNIK IZOLATORA, D400, MOST PIONOWY Z BOKU",106.4,"1-ZE-01",4.95,8,"OE_INSULATOR_DEPTH","39401","SZT","85469010",null,"230628LK","5901988394011","OE - Support d'isolateur, P400, pont vertical sur le côté","OE - Insulator support, D400, Vertical bridge on the side","OE - Soporte aislante, D400 PARA EMB. VERTICAL LATERAL","AlCubar / CU - SZIGETELŐ KONZER, D400, OLDALSÓ FÜGGŐLEGES HÍD"]
["39402","ALCUBAR / CU - WSPORNIK IZOLATORA, DOIZOLOWANIE SZYN",106.4,"1-ZE-01",1.6166666666666667,6,"OE_INSULATOR_DEPTH","39402","SZT","85469010",null,"230628LK","5901988201180","OE - Support d'isolateur, isolation des rails horizontaux","OE - Insulator support, additional insulation of Horizontal busbars","OE - Soporte aislante, REFUERZO EMB. HORIZ. ","AlCubar / CU - SZIGETELŐTÁMASZTÁS, BUSZSZIGETELÉS"]
["39408","ZENERGY - IZOLATOR WSPORCZY H40X8MM; ŚREDNICA 31-40MM; UN=1200VAC",15.2,"1-ZE-01",null,null,"OE_INSULATORS","39408","SZT","85469010",null,null,"5901988394080","OE - Isolant de soutien H40x8mm; diamètre 31-40mm; Un = 1200VAC","OE - Post insulator H40x8mm; diameter 31-40mm; Un = 1200VAC","OE- SOPORTE AUX. H40X8MM; DIAMETRO 31-40MM; UN=1200VAC","ZENERGY - OSZTÓSZIGETELŐ H40X8MM; ÁTMÉRŐ 31-40MM; UN=1200VAC"]
["39450","OE - Wspornik izolatora na plecach W450, regulowana wysokość",134.4,"1-ZE-01",0.3,1,"OE_INSULATOR_WIDTH","39450","SZT","85469010",null,"230821RT","5901988394509","OE - Support d'isolant à l'arrière W450","OE - Insulator support on back W450","OE - Soporte aislante en la parte posterior W450","OE - W450 hátszigetelő támaszték, állítható magasságú"]
["39456","ZENERGY - PŁYTA MONTAŻOWA HGM, UCB:400; UPB:400-630 PIONOWO, W450, 5M, BEZ WSPORNIKÓW",134.19999999999999,"1-ZE-01",null,null,"OE_MCCB_PLATES","37561","SZT","85389099",null,null,"5901988394561","OE - plaque de montage HGM, UCB: 400; UPB: 400-630 verticalement, L450, 5M, sans supports","OE - Mounting plate HGM, UCB: 400; UPB: 400-630 Vertically, W450, 5M, without brackets","OE- PLACA MONTAJE  HGM 400; UPB:400-630 VERT. W450, 5M  ","ZENERGY - HGM SZERELŐLAP, UCB:400; UPB:400-630 FÜGGŐLEGES, W450, 5M, TARTÓK NÉLKÜL"]
["39524","ZENERGY - OSŁONA CZOŁOWA HGM 1600 3P, W450, 12M / 300, PIONOWO, DŹWIGNIA",115.5,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988395247","OE - CAPOT AVANT HGM 1600 3P, L450, 12M / 300, VERTICAL, LEVIER","OE - Front Cover HGM 1600 3P, W450, 12M / 300, Vertical, Lever","*OE - TAPA DELANTERA HGM 1600 3P, W450, 12M / 300, VERTICAL, PALANCA","ZENERGY - ELSŐ BURKOLAT HGM 1600 3P, W450, 12M / 300, FÜGGŐLEGES, KAR"]
["39550","ZENERGY - OSŁONA CZOŁOWA HGM 100 3/4P, W450, 5M / 300, PIONOWO, DŹWIGNIA",63.6,"1-ZE-01",null,null,"03_SWITCHES_COVERS","39550","SZT","85389099","27.12.40.0",null,"5901988395506","OE - Couvercle avant HGM 100 3 / 4P, L450, 5M / 300, vertical, levier","OE - HGM 100 3 / 4P front visor, W450, 5M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 100 3/4P, W450, 5M (250MM) VERT.","ZENERGY - ELSŐ BURKOLAT HGM 100 3/4P, W450, 5M / 300, FÜGGŐLEGES, KAR"]
["39593","ZENERGY - OSŁONA CZOŁOWA HGM 400 3/4P, W450, 9M / 300, PIONOWO, DŹWIGNIA",108.1,"1-ZE-01",0.20833333333333334,4,"03_SWITCHES_COVERS","39593","SZT","85389099","27.12.40.0",null,"5901988395933","OE - Couvercle avant HGM 400 3 / 4P, L450, 9M / 300, vertical, levier","OE - HGM 400 3 / 4P front visor, W450, 9M / 300, Vertical, Lever","OM- TAPA TROQ. HGM 400 3/4P, W450, 9M (450MM) VERT.","ZENERGY- ELSŐ BURKOLAT HGM 400 3/4P, W450, 9M / 300, FÜGGŐLEGES, KAR"]
["39600","OE - Wspornik izolatora, D600, most poziomy",151.19999999999999,"1-ZE-01",null,null,"OE_INSULATOR_WIDTH","39600","SZT","85469010",null,"230807LK","5901988396008","OE - Support d'isolateur, D600, pont horizontal","OE - Insulator support, D600, horizontal busduct","OE - Soporte aislante, D600 PARA EMB. HORIZ.","OE - Szigetelő tartó, D600, vízszintes híd"]
["39601","OE - Wspornik izolatora wzmocniony, D600/D1000, most poziomy",272.2,null,0.95833333333333337,4,"OE_INSULATOR_DEPTH",null,null,"",null,null,"5901988396015"]
["39646","ZENERGY - PŁYTA MONTAŻOWA UPB:100-250; HGP250 PIONOWO / HGM, UCB:160-250 4P, 400 3P; UPB:100-250, 400-630 3P; HGP250 POZIOMO, W650, 4M, BEZ WSPORNIKÓW",163.9,"1-ZE-01",4.1666666666666664E-2,1,"OE_MCCB_PLATES","39646","SZT","85381000","27.12.40.0",null,"5901988396466","OE - plaque de montage HGP:250, UPB: 100-250 verticalement / HGM, UCB: 160-250 4P, 400 3P, HGP:250, UPB: 100-250, 400-630 3P horizontal, L650, 4M, sans supports","OE - Mounting plate HGP:250, UPB: 100-250 Vertical / HGM, UCB: 160-250 4P, 400 3P, HGP:250, UPB: 100-250, 400-630 3P Horizontal, W650, 4M, without brackets","OE- PLACA MONT. HGP250 VERT. / HGM160-250 4P, 400 3P;  HGP250 HORIZ. W650","ZENERGY - SZERELŐLAP UPB:100-250; HGP250 VERTICAL / HGM, UCB:160-250 4P, 400 3P; UPB: 100-250, 400-630 3P; HGP250 VÍZSZINTES, W650, 4M, KONZER NÉLKÜL"]
["39654","ZENERGY - PŁYTA MONTAŻOWA HGP:400-630 3/4P PIONOWO / HGP:400-630 4P POZIOMO, W650, 5M, BEZ WSPORNIKÓW",178.2,"1-ZE-01",6.6666666666666666E-2,5,"OE_MCCB_PLATES","39654","SZT","8538909900",null,null,"5901988396541","OE - PLAQUE DE MONTAGE HGP:400-630 3/4P VERTICALEMENT / HGP:400-630 4P HORIZONTALEMENT, L650, 5M, SANS SUPPORTS","OE - Mounting plate HGP:400-630 3/4P VerticalLY / HGP:400-630 4P HorizontalLY, W650, 5M, WITHOUT BRACKETS","OE- PLACA MONT. HGP400-630 3/4P VERT. / HGP400-630 4P HORIZ. W650, 5M, ","ZENERGY - SZERELŐLEMEZ HGP:400-630 3/4P FÜGGŐLEGES / HGP:400-630 4P VÍZSZINTES, W650, 5M, KONZER NÉLKÜL"]
["39701","ZENERGY - OSŁONA CZOŁOWA HGM 100 3/4P + ANALIZATOR 92X92mm, W650, 3M / 500, POZIOMO",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988397012","OE - CAPOT AVANT HGM 100 3/4P + ANALYSEUR 92X92mm, L650, 3M / 500, HORIZONTAL","OE - Front Cover HGM 100 3/4P + analyzer 92X92mm, W650, 3M / 500, Horizontal","ZEN- TAPA TROQ. HGM 100 3/4P + ANALIZ. DE REDES 92X92mm, W650, 3M / 500, HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 100 3/4P + ELEMZŐ 92X92mm, W650, 3M / 500, VÍZSZINTES"]
["39704","ZENERGY - OSŁONA CZOŁOWA HGM 160-250 3P + ANALIZATOR 92X92mm, W650, 3M / 500, POZIOMO",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS","39704","SZT","85389099",null,null,"5901988397043","OE - CAPOT AVANT HGM 160-250 3P + ANALYSEUR 92X92mm, L650, 3M / 500, HORIZONTAL","OE - Front Cover HGM 160-250 3P + analyzer 92X92mm, W650, 3M / 500, Horizontal","ZEN- TAPA TROQ. HGM 160-250 3P + ANALIZ. DE REDES 92X92mm, W650, 3M / 500, HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 160-250 3P + ELEMZŐ 92X92mm, W650, 3M / 500, VÍZSZINTES"]
["39722","ZENERGY - OSŁONA CZOŁOWA HGM 1000-1250 3P, W650, 12M / 500, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",8.3333333333333329E-2,2,"OE_MCCB_COVERS","39722","SZT","85389099","27.12.40.0",null,"5901988397227","OE - COUVERCLE HGM 1000-1250 3P, L650, 12M/500, VERTICAL, LEVIER","OE - Cover HGM 1000-1250 3P, W650, 12M / 500, Vertical, Lever","*OE - CUBIERTA HGM 1000-1250 3P, W650, 12M / 500, VERTICAL, PALANCA","ZENERGY - ELSŐ BURKOLAT HGM 1000-1250 3P, W650, 12M / 500, FÜGGŐLEGES, KAR"]
["39735","produkt wycofany (ZENERGY - OSŁONA CZOŁOWA HGM 100 3P, W650, 3M / 500, POZIOMO, DŹWIGNIA)",55.7,"1-ZE-01",null,null,null,null,"SZT","85389099","27.12.40.0",null,null,null,null,null,"kivont termék (ZENERGY - ELSŐ BURKOLAT HGM 100 3P, W650, 3M / 500, VÍZSZINTES, KAR)"]
["39738","OE - Osłona czołowa HGM 125 3P, W650, 3M / 500, poziomo, silnik",62.5,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT",null,null,null,null,"OE - Panneau avant HGM 125 3P, W650, 3M / 500, horizontale, moteur","OE - Front cover HGM 125 3P, W650, 3M / 500, horizontal, motor","OE - Tapa frontal HGM 125 3P, W650, 3M / 500, horizontal, motor","OE - Első burkolat HGM 125 3P, W650, 3M / 500, vízszintes, motor"]
["39738",null,62.5]
["39743","OE - Osłona czołowa HGM 160-250 4P NRST, W650, 4M / 500, poziomo, silnik",70,"1-ZE-01",null,null,"OE_MCCB_COVERS","39743","SZT",null,null,"240506PW",null,"OE - Protection frontale HGM 160-250 4P NRST, W650, 4M / 500, horizontale, moteur","OE - Front cover HGM 160-250 4P NRST, W650, 4M / 500, horizontal, motor","OE - Tapa frontal HGM 160-250 4P NRST, W650, 4M / 500, horizontal, motor","OE - Első burkolat HGM 160-250 4P NRST, W650, 4M / 500, vízszintes, motor"]
["39747","ZENERGY - OSŁONA CZOŁOWA HGM 160-250 4P NRST, W650, 4M / 500, POZIOMO, DŹWIGNIA",71.2,"1-ZE-01",0.2,1,"03_SWITCHES_COVERS","39747","SZT","85389099","27.12.40.0",null,"5901988397470","OE - Couvercle avant HGM 160-250 4P, L650, 4M / 500, horizontal, levier","OE - Front Cover HGM 160-250 4P, W650, 4M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 160-250 4P, W650, 4M (200MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 160-250 4P NRST, W650, 4M / 500, VÍZSZINTES, KAROS"]
["39751","ZENERGY - OSŁONA CZOŁOWA HGM 125 3/4P, W650, 5M / 500, PIONOWO, DŹWIGNIA",77.7,"1-ZE-01",null,null,"03_SWITCHES_COVERS","39751","SZT","85389099","27.12.40.0",null,"5901988397517","OE - Couvercle avant HGM 125 3 / 4P, L650, 5M / 500, vertical, levier","OE - HGM 125 3 / 4P front visor, W650, 5M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 125 3/4P, W650, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT HGM 125 3/4P, W650, 5M / 500, FÜGGŐLEGES, KAR"]
["39755","OE - Osłona czołowa HGM 160-250 3/4P, W650, 5M / 500, pionowo, silnik",76.3,"1-ZE-01",null,null,"OE_MCCB_COVERS","39755","SZT",null,null,"240506PW",null,"OE - Protection frontale HGM 160-250 3/4P, W650, 5M / 500, vertical, moteur","OE - Front cover HGM 160-250 3/4P, W650, 5M / 500, vertical, motor","OE - Tapa frontal HGM 160-250 3/4P, W650, 5M / 500, vertical, motor","OE - Első burkolat HGM 160-250 3/4P, W650, 5M / 500, függőleges, motor"]
["39779","ZENERGY - OSŁONA CZOŁOWA HGM 630-800 4P NRST, W650, 7M / 500, POZIOMO, DŹWIGNIA",103.8,"1-ZE-01",null,null,"03_SWITCHES_COVERS","39779","SZT","85389099","27.12.40.0",null,"5901988397791","OE - Couvercle avant HGM 630-800 4P, L650, 7M / 500, horizontal, levier","OE - Front Cover HGM 630-800 4P, W650, 7M / 500, Horizontal, Lever","ZEN- TAPA TROQ. HGM 630-800 4P, W650, 7M (350MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 630-800 4P NRST, W650, 7M / 500, VÍZSZINTES, KAR"]
["39795","ZENERGY - OSŁONA CZOŁOWA HGM 630-800 4P, W650, 9M / 500, PIONOWO, DŹWIGNIA",137.80000000000001,"1-ZE-01",null,null,"03_SWITCHES_COVERS","39795","SZT","85389099","27.12.40.0",null,"5901988397951","OE - Couvercle avant HGM 630-800 4P, L650, 9M / 500, vertical, levier","OE - Front Cover HGM 630-800 4P, W650, 9M / 500, Vertical, Lever","ZEN- TAPA TROQ. HGM 630-800 4P, W650, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT HGM 630-800 4P, W650, 9M / 500, FÜGGŐLEGES, KAR"]
["39836","ZENERGY - PŁYTA MONTAŻOWA HGM, UCB:100-250 PIONOWO / HGM, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P POZIOMO, W850, 3M, BEZ WSPORNIKÓW",163.9,"1-ZE-01",null,null,"OE_MCCB_PLATES","39836","SZT","85381000","27.12.40.0",null,"5901988398361","OE - Plaque de montage HGM, UCB: 100-250 verticalement / HGM, UCB: 100, 160-250 3P, HGP:250 3P, UPB: 100-250 3P horizontal, L850, 3M, sans supports","OE - Mounting plate HGM, UCB: 100-250 Vertical / HGM, UCB: 100, 160-250 3P, HGP:250 3P, UPB: 100-250 3P Horizontal, W850, 3M, without brackets","OE- PLACA MONT. HGM100-250 VERT. / HGM100, 160-250 3P;  HGP250 3P HORIZ. W850","ZENERGY - SZERELŐLEMEZ HGM, UCB:100-250 FÜGGŐLEGES / HGM, UCB:100, 160-250 3P; UPB:100-250 3P; HGP250 3P VÍZSZINTES, W850, 3M, KONZER NÉLKÜL"]
["39851","OE - Wspornik izolatora W850, regulowana głębokość",173.6,"1-ZE-01",0.375,4,"OE_INSULATOR_WIDTH","39851","SZT","85469010",null,"230821RT","5901988398514","OE - Support d'isolateur W850 pour jeux de barres verticaux","OE - Insulator support W850 for vertical busbars","OE - Soporte aislador W850 para barras verticales","OE - W850 szigetelőtartó, állítható mélység"]
["39866","ZENERGY - PŁYTA MONTAŻOWA HGP800 3/4P; HGM, UCB:630-800 PIONOWO / HGP800 3P; HGM, UCB:630-800 3P POZIOMO, W850, 6M, BEZ WSPORNIKÓW",205.7,"1-ZE-01",null,null,"OE_MCCB_PLATES","39866","SZT","85381000","27.12.40.0",null,"5901988398668","OE - Plaque de montage HGP800 3/4P; HGM, UCB:630-800 verticalement / HGP800 3P; HGM, UCB:630-800 3P horizontal, L850, 6M, sans supports","OE - Mounting plate HGP800 3/4P; HGM, UCB:630-800 Vertical / HGP800 3P; HGM, UCB:630-800 3P Horizontal, W850, 6M, without brackets","OE- PLACA MONTAJE  HGM 630-800 VERT. HGM,UCB:630-800 3P HORIZ. W850, 6M  ","ZENERGY - SZERELŐLAP HGP800 3/4P; HGM, UCB:630-800 FÜGGŐLEGES / HGP800 3P; HGM, UCB:630-800 3P VÍZSZINTES, W850, 6M, TARTÓK NÉLKÜL"]
["39903","ZENERGY - OSŁONA CZOŁOWA HGM 125 4P + ANALIZATOR 92X92mm, W850, 3M / 700, POZIOMO",70.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988399030","OE - CAPOT AVANT HGM 125 4P + ANALYSEUR 92X92mm, L850, 3M / 700, HORIZONTAL","OE - Front Cover HGM 125 4P + analyzer 92X92mm, W850, 3M / 700, Horizontal","*OE - TAPA FRONTAL HGM 125 4P + ANALIZADOR 92X92mm, W850, 3M / 700, HORIZONTAL","ZENERGY - ELSŐ BURKOLAT HGM 125 4P + ELEMZŐ 92X92mm, W850, 3M / 700, VÍZSZINTES"]
["39906","ZENERGY - OSŁONA CZOŁOWA HGM 400 3P + ANALIZATOR 92X92mm, W850, 4M / 700, POZIOMO",81.3,"1-ZE-01",null,null,"OE_MCCB_COVERS",null,"SZT","85389099",null,null,"5901988399061","OE - CAPOT AVANT HGM 400 3P + ANALYSEUR 92X92mm, L850, 4M / 700, HORIZONTAL","OE - Front Cover HGM 400 3P + analyzer 92X92mm, W850, 4M / 700, Horizontal","*OE - TAPA FRONTAL HGM 400 3P + ANALIZADOR 92X92mm, W850, 4M / 700, HORIZONTAL","ZENERGY - ELSŐ BURKOLAT HGM 400 3P + ELEMZŐ 92X92mm, W850, 4M / 700, VÍZSZINTES"]
["39922","ZENERGY - OSŁONA CZOŁOWA HGM 1000-1250 3P, W850, 12M / 700, PIONOWO, DŹWIGNIA",168.3,"1-ZE-01",0.01,1,"OE_MCCB_COVERS","39922","SZT","85389099",null,null,"5901988399221","OE - CAPOT AVANT HGM 1000-1250 3P, L850, 12M / 700, VERTICAL, LEVIER","OE - Front Cover HGM 1000-1250 3P, W850, 12M / 700, Vertical, Lever","*OE - TAPA DELANTERA HGM 1000-1250 3P, W850, 12M / 700, VERTICAL, PALANCA","ZENERGY - ELSŐ BURKOLAT HGM 1000-1250 3P, W850, 12M / 700, FÜGGŐLEGES, KAR"]
["39936","ZENERGY - OSŁONA CZOŁOWA HGM 125 3P, W850, 3M / 700, POZIOMO, DŹWIGNIA",70.599999999999994,"1-ZE-01",null,null,"OE_MCCB_COVERS","39936","SZT","85389099",null,null,"5901988399368","OE - Couvercle avant HGM 125 3P, L850, 3M / 700, horizontal, levier","OE - HGM 125 3P front visor, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 125 3P, W850, 3M (150MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 125 3P, W850, 3M / 700, VÍZSZINTES, KAR"]
["39946","ZENERGY - OSŁONA CZOŁOWA HGM 125 4P NRST, W850, 3M / 700, POZIOMO, DŹWIGNIA",71.900000000000006,"1-ZE-01",null,null,"03_SWITCHES_COVERS","39946","SZT","85389099","27.12.40.0",null,"5901988399467","OE - Couvercle avant HGM 125 4P, L850, 3M / 700, horizontal, levier","OE - HGM 125 4P Front cover, W850, 3M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 125 4P, W850, 3M (150MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 125 4P NRST, W850, 3M / 700, VÍZSZINTES, KAR"]
["39950","ZENERGY - OSŁONA CZOŁOWA HGM 100 3/4P, W850, 5M / 700, PIONOWO, DŹWIGNIA",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","39950","SZT","85381000","27.12.40.0",null,"5901988399504","OE - Couvercle avant HGM 100 3 / 4P, L850, 5M / 700, vertical, levier","OE - HGM 100 3 / 4P front visor, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 100 3/4P, W850, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT HGM 100 3/4P, W850, 5M / 700, FÜGGŐLEGES, KAR"]
["39951","ZENERGY - OSŁONA CZOŁOWA HGM 125 3/4P, W850, 5M / 700, PIONOWO, DŹWIGNIA",91.6,"1-ZE-01",null,null,"OE_MCCB_COVERS","39951","SZT","85381000","27.12.40.0",null,"5901988399511","OE - Couvercle avant HGM 125 3 / 4P, L850, 5M / 700, vertical, levier","OE - HGM 125 3 / 4P front visor, W850, 5M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 125 3/4P, W850, 5M (250MM)  VERT.","ZENERGY - ELSŐ BURKOLAT HGM 125 3/4P, W850, 5M / 700, FÜGGŐLEGES, KAR"]
["39969","ZENERGY - OSŁONA CZOŁOWA HGM 630-800 3P, W850, 6M / 700, POZIOMO, DŹWIGNIA",95.8,"1-ZE-01",null,null,"OE_MCCB_COVERS","39969","SZT","85389099",null,null,"5901988399696","OE - Couvercle avant HGM 630-800 3P, L850, 6M / 700, horizontal, levier","OE - Front Cover HGM 630-800 3P, W850, 6M / 700, Horizontal, Lever","OE- TAPA TROQ. HGM 630-800 3P, W850, 6M (300MM)  HORIZ.","ZENERGY - ELSŐ BURKOLAT HGM 630-800 3P, W850, 6M / 700, VÍZSZINTES, KAR"]
["39995","ZENERGY - OSŁONA CZOŁOWA 2X HGM 630-800 4P, W850, 9M / 700, PIONOWO, DŹWIGNIA",152.9,"1-ZE-01",null,null,"OE_MCCB_COVERS","39995","SZT","85381000","27.12.40.0",null,"5901988399955","OE - Couvercle avant HGM 630-800 4P, L850, 9M / 700, vertical, levier","OE - Front Cover HGM 630-800 4P, W850, 9M / 700, Vertical, Lever","OE- TAPA TROQ. HGM 630-800 4P, W850, 9M (450MM)  VERT.","ZENERGY - ELSŐ BURKOLAT 2X HGM 630-800 4P, W850, 9M / 700, FÜGGŐLEGES, KAR"]
["40140","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1200 W400",267.8,"1-ZE-01",0.01,1,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988401405","OE - Cadre des panneaux avant articulés H1200 L400","OE - Frame of hinged Front covers H1200 W400","OE- MARCO PIVOTANTE H1200 W400","ZENERGY - SZÁNTOS ELSŐ BURKOLAT KERET H1200 W400"]
["40146","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1200 W450 DO PLOMBOWANIA",303.60000000000002,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988401467","OE - H1200 L450 cache-charnière pour sceller","OE - H1200 W450 hinged Front covers frame for sealing","OE- MARCO PIVOTANTE H1200 W450 ","ZENERGY - ZSÁNLÓS ELSŐ FEDŐKERET H1200 W450 TÖMÍTÉSHEZ"]
["40185","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1200 W850",366.1,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988401856","OE - H1200 L850 cadre de panneau de charnière avant","OE - Frame of hinged Front covers H1200 W850","OE- MARCO PIVOTANTE H1200 W850","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H1200 W850"]
["40212","ZENERGY - DRZWI WENTYLOWANE IP30, H1200 X W1200, PODWÓJNE",2081.1999999999998,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988402129","OE - portes ventilées double IP30, H1200 x L1200","OE - Ventilated doors IP30, H1200 x W1200, double","OE- PUERTA VENTIL. IP30, H1200 x W1200, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1200 X W1200, DUPLÉS"]
["40213","ZENERGY - DRZWI WENTYLOWANE IP30, H1200 X W1300, PODWÓJNE",2098.4,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988402136","OE - portes ventilées double IP30, H1200 x L1300","OE - Ventilated doors IP30, H1200 x W1300, double","OE- PUERTA VENTIL. IP30, H1200 x W1300, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1200 X W1300, DUPLÉS"]
["40245","ZENERGY - DRZWI WENTYLOWANE IP30, H1200 X W450",898.6,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988402457","OE - Portes ventilées IP30, H1200 x L450","OE - Ventilated door IP30, H1200 x W450","OE- PUERTA VENTIL. IP30, H1200 x W450","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1200 X W450"]
["40280","ZENERGY - DRZWI WENTYLOWANE IP30, H1200 X W800",1152.4000000000001,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988402808","OE - Portes ventilées IP30, H1200 x L800","OE - Ventilated door IP30, H1200 x W800","OE- PUERTA VENTIL. IP30, H1200 x W800","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1200 X W800"]
["40312","ZENERGY - DRZWI PEŁNE IP30, H1200 X W1200, PODWÓJNE",1996.9,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988403126","OE - Portes pleine IP30, H1200 x L1200, double","OE - Plain door IP30, H1200 x W1200, double","OE- PUERTA OPACA IP30, H1200 x W1200, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H1200 X W1200, DUPLA"]
["40340","ZENERGY - DRZWI PEŁNE IP30, H1200 X W400",814.3,"1-ZE-01",0.01,1,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988403409","OE - Portes pleine IP30, H1200 x L400","OE - Plain door IP30, H1200 x W400","OE- PUERTA OPACA IP30, H1200 x W400","ZENERGY - TÖMÖR AJTÓ IP30, H1200 X W400"]
["40365","ZENERGY - DRZWI PEŁNE IP30, H1200 X W650",997.9,"1-ZE-01",1.6666666666666666E-2,2,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988403652","OE - Portes pleine IP30, H1200 x L650","OE - Plain door IP30, H1200 x W650","OE- PUERTA OPACA IP30, H1200 x W650","ZENERGY - TÖMÖR AJTÓ IP30, H1200 X W650"]
["40412","ZENERGY - DRZWI WENTYLOWANE IP43, H1200 X W1200, PODWÓJNE",2225.9,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988404123","OE - Portes ventilées IP43, H1200 x L1200, double","OE - Ventilated door IP43, H1200 x W1200, double","OE- PUERTA VENTIL. IP43, H1200 x W1200, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1200 X W1200, DUPLÉS"]
["40440","ZENERGY - DRZWI WENTYLOWANE IP43, H1200 X W400",920.2,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988404406","OE - Portes ventilées IP43, H1200 x L400","OE - Ventilated door IP43, H1200 x W400","OE- PUERTA VENTIL. IP43, H1200 x W400","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1200 X W400"]
["40445","ZENERGY - DRZWI WENTYLOWANE IP43, H1200 X W450",1179.4000000000001,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988404451","OE - Portes ventilées IP43, H1200 x L450","OE - Ventilated door IP43, H1200 x W450","OE- PUERTA VENTIL. IP43, H1200 x W450","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1200 X W450"]
["40480","ZENERGY - DRZWI WENTYLOWANE IP43, H1200 X W800",1228,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988404802","OE - Portes ventilées IP43, H1200 x L800","OE - Ventilated door IP43, H1200 x W800","OE- PUERTA VENTIL. IP43, H1200 x W800","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1200 X W800"]
["40510","ZENERGY - DRZWI PEŁNE IP55, H1200 X W1000",1338.1,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988405106","OE - Portes pleine IP55, H1200 x L1000","OE - Plain door IP55, H1200 x W1000","OE- PUERTA OPACA IP55, H1200 x W1000","ZENERGY - TÖMÖR AJTÓ IP55, H1200 X W1000"]
["40530","ZENERGY - DRZWI PEŁNE IP55, H1200 X W300",800.3,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988405304","OE - Portes pleine IP55, H1200 x L300","OE - Plain door IP55, H1200 x W300","OE- PUERTA OPACA IP55, H1200 x W300","ZENERGY - TÖMÖR AJTÓ IP55, H1200 X W300"]
["40560","ZENERGY - DRZWI PEŁNE IP55, H1200 X W600",1036.8,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988405601","OE - Portes pleine IP55, H1200 x L600","OE - Plain door IP55, H1200 x W600","OE- PUERTA OPACA IP55, H1200 x W600","ZENERGY - TÖMÖR AJTÓ IP55, H1200 X W600"]
["40585","ZENERGY - DRZWI PEŁNE IP55, H1200 X W850",1222.5999999999999,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988405854","OE - Portes pleine IP55, H1200 x L850","OE - Plain door IP55, H1200 x W850","OE- PUERTA OPACA IP55, H1200 x W850","ZENERGY - TÖMÖR AJTÓ IP55, H1200 X W850"]
["40613","ZENERGY - DRZWI PRZESZKLONE IP55, H1200 X W1300, PODWÓJNE",2556.4,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988406134","OE - Portes vitrée IP55, H1200 x L1300, double","OE - Glazed door IP55, H1200 x W1300, double","OE- PUERTA TRANSPARENTE IP55, H1200 x W1300, DOBLE","ZENERGY - ÜVEGAJTÓK IP55, H1200 X W1300, DUPLA"]
["40660","ZENERGY - DRZWI PRZESZKLONE IP55, H1200 X W600",1234.4000000000001,"1-ZE-01",1.6666666666666666E-2,1,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988406608","OE - Portes vitrée IP55, H1200 x L600","OE - Glazed door IP55, H1200 x W600","OE- PUERTA TRANSPARENTE IP55, H1200 x W600","ZENERGY - ÜVEZETETT AJTÓK IP55, H1200 X W600"]
["40665","ZENERGY - DRZWI PRZESZKLONE IP55, H1200 X W650",1277.5999999999999,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988406653","OE - Portes vitrée IP55, H1200 x L650","OE - Glazed door IP55, H1200 x W650","OE- PUERTA TRANSPARENTE IP55, H1200 x W650","ZENERGY - ÜVEZETETT AJTÓK IP55, H1200 X W650"]
["40695","ZENERGY - DRZWI PRZESZKLONE IP55, H1200 X W950",1575.7,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988406950","OE - Portes vitrée IP55, H1200 x L950","OE - Glazed door IP55, H1200 x W950","OE- PUERTA TRANSPARENTE IP55, H1200 x W950","ZENERGY - ÜVEZETETT AJTÓK IP55, H1200 X W950"]
["40913","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1200 X W1300 + WSPORNIKI,  ( 1100 X 1200 )",1047.5999999999999,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988409135","OE - Plaque de montage complète H1200 x L1300 + supports, (1100 x 1200)","OE - Plain Mounting plate H1200 x W1300 + brackets, (1100 x 1200)","OE- PLACA MONTAJE  TOTAL CIEGA H1200 x W1300 + SOPORT. (1100 X 1200)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1200 X W1300 + KONZEREK, (1100 X 1200)"]
["40960","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1200 X W600 + WSPORNIKI,  ( 1050 X 500 )",549.70000000000005,"1-ZE-01",8.3333333333333329E-2,2,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988409609","OE - Plaque de montage complète H1200 x L600 + supports, (1050 x 500)","OE - Plain Mounting plate H1200 x W600 + brackets, (1050 x 500)","OE- PLACA MONTAJE  TOTAL CIEGA H1200 x W600 + SOPORT. (1050 X 500)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1200 X W600 + KONZEREK, (1050 X 500)"]
["40985","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1200 X W850 + WSPORNIKI,  ( 1050 X 750 )",723.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988409852","OE - Plaque de montage complète H1200 x L850 + supports, (1050 x 750)","OE - Plain Mounting plate H1200 x W850 + brackets, (1050 x 750)","OE- PLACA MONTAJE  TOTAL CIEGA H1200 x W850 + SOPORT. (1050 X 750)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H1200 X W850 + KONZEREK, (1050 X 750)"]
["40995","ZENERGY - PEŁNY ŁĄCZNIK PŁYT MONTAŻOWYCH H1200,  ( 1100 X 98 )",180.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988409951","OE - Connecteur complet pour plaques de montage H1200, (1100 x 98)","OE - Plain Mounting plate connector H1200, (1100 x 98)","OE- UNION PLACA MONTAJE  TOTAL H1200, ( 1100 X 98 )","ZENERGY - SZERELŐLEMEZEK TELJES CSATLAKOZÓJA H1200, (1100 X 98)"]
["41110","ZENERGY - DRZWI PRZESZKLONE IP30, H1200 X W1000",1493.6,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988411107","OE - Portes vitrées IP30, H1200 x L1000","OE - Glazed door IP30, H1200 x W1000","OE- PUERTA TRANSP. IP30, H1200 x W1000","ZENERGY - ÜVEGAJTÓK IP30, H1200 X W1000"]
["41140","ZENERGY - DRZWI PRZESZKLONE IP30, H1200 X W400",893.2,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988411404","OE - Portes vitrées IP30, H1200 x L400","OE - Glazed door IP30, H1200 x W400","OE- PUERTA TRANSP. IP30, H1200 x W400","ZENERGY - ÜVEZETETT AJTÓK IP30, H1200 X W400"]
["41145","ZENERGY - DRZWI PRZESZKLONE IP30, H1200 X W450",937.4,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988411459","OE - Portes vitrées IP30, H1200 x L450","OE - Glazed door IP30, H1200 x W450","OE- PUERTA TRANSP. IP30, H1200 x W450","ZENERGY - ÜVEZETETT AJTÓK IP30, H1200 X W450"]
["41185","ZENERGY - DRZWI PRZESZKLONE IP30, H1200 X W850",1347.8,"1-ZE-01",null,null,"OE_DOORS_1200",null,"SZT","85389099",null,null,"5901988411855","OE - Portes vitrées IP30, H1200 x L850","OE - Glazed door IP30, H1200 x W850","OE- PUERTA TRANSP. IP30, H1200 x W850","ZENERGY - ÜVEZETETT AJTÓK IP30, H1200 X W850"]
["41211","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1200 X W850+200",686.9,"1-ZE-01",0.01,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988412111","OE - Couverture arrière complète IP30, H1200 x L650 + 400","OE - Rear Plain cover IP30, H1200 x W850 + 200","OE- FONDO ATORNILLADO LISO IP30, H1200 x W650+400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1200 X W850+200"]
["41240","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1200 X W400",366.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988412401","OE - Couverture arrière complète IP30, H1200 x L400","OE - Plain rear cover IP30, H1200 x W400","OE- FONDO ATORNILLADO LISO IP30, H1200 x W400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1200 X W400"]
["41265","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1200 X W650",500,"1-ZE-01",0.01,1,"OE_COVERS","41265","SZT","85389099",null,null,"5901988412654","OE - Couverture arrière complète IP30, H1200 x L650","OE - Plain rear cover IP30, H1200 x W650","OE- FONDO ATORNILLADO LISO IP30, H1200 x W650","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1200 X W650"]
["41310","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1200 X W1000",694.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988413101","OE - Couvercle ventilé IP30, H1200 x L1000","OE - Rear ventilated cover IP30, H1200 x W1000","OE- FONDO ATORNILLADO VENTIL. IP30, H1200 x W1000","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1200 X W1000"]
["41313","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1200 X W1300",1086.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988413132","OE - Hotte d'aération arrière IP30, H1200 x L1300","OE - Rear ventilated cover IP30, H1200 x W1300","OE- FONDO ATORNILLADO VENTIL. IP30, H1200 x W1300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1200 X W1300"]
["41345","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1200 X W450",453.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988413453","OE - Couverture arrière ventilée IP30, H1200 x L450","OE - Rear ventilated cover IP30, H1200 x W450","OE- FONDO ATORNILLADO VENTIL. IP30, H1200 x W450","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1200 X W450"]
["41360","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1200 X W600",537.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988413606","OE - Couverture arrière ventilée IP30, H1200 x L600","OE - Rear ventilated cover IP30, H1200 x W600","OE- FONDO ATORNILLADO VENTIL. IP30, H1200 x W600","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1200 X W600"]
["41385","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1200 X W850",651.20000000000005,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988413859","OE - Hotte d'aération arrière IP30, H1200 x L850","OE - Rear ventilated cover IP30, H1200 x W850","OE- FONDO ATORNILLADO VENTIL. IP30, H1200 x W850","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1200 X W850"]
["41412","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1200 X W1200",1182.5999999999999,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988414122","OE - Coque arrière ventilée IP43, H1200 x L1200","OE - Rear ventilated cover IP43, H1200 x W1200","OE- FONDO ATORNILLADO VENTIL.IP43, H1200 x W1200","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1200 X W1200"]
["41440","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1200 X W400",499,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988414405","OE - Coque arrière ventilée IP43, H1200 x L400","OE - Rear ventilated cover IP43, H1200 x W400","OE- FONDO ATORNILLADO VENTIL.IP43, H1200 x W400","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1200 X W400"]
["41465","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1200 X W650",636.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988414658","OE - Hotte d'aération arrière IP43, H1200 x L650","OE - Rear ventilated cover IP43, H1200 x W650","OE- FONDO ATORNILLADO VENTIL.IP43, H1200 x W650","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1200 X W650"]
["41510","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1200 X W1000",735.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988415105","OE - Couverture arrière complète IP55, H1200 x L1000","OE - Plain rear cover IP55, H1200 x W1000","OE- FONDO ATORNILLADO LISO IP55, H1200 x W1000","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1200 X W1000"]
["41513","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1200 X W1300",1144.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988415136","OE - Couverture arrière complète IP55, H1200 x L1300","OE - Plain rear cover IP55, H1200 x W1300","OE- FONDO ATORNILLADO LISO IP55, H1200 x W1300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1200 X W1300"]
["41545","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1200 X W450",453.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988415457","OE - Couverture arrière complète IP55, H1200 x L450","OE - Plain rear cover IP55, H1200 x W450","OE- FONDO ATORNILLADO LISO IP55, H1200 x W450","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1200 X W450"]
["41560","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1200 X W600",543.20000000000005,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988415600","OE - Couverture arrière complète IP55, H1200 x L600","OE - Plain rear cover IP55, H1200 x W600","OE- FONDO ATORNILLADO LISO IP55, H1200 x W600","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1200 X W600"]
["41585","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1200 X W850",665.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988415853","OE - Couverture arrière complète IP55, H1200 x L850","OE - Plain rear cover IP55, H1200 x W850","OE- FONDO ATORNILLADO LISO IP55, H1200 x W850","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1200 X W850"]
["41685","OE - Pokrywa górna IP30, W850, D600, wentylator 3500 m3/h",869.4,"1-ZE-01",null,null,"OE_COVERS","41685","SZT",null,null,null,null,"OE - Capot supérieur IP30, L850, P600, ventilateur 3500 m3/h","OE - Top cover IP30, W850, D600, ventilator 3500 m3/h","OE- TECHO IP30, W850, D600, fan 3500 m3/h","OE - Felső burkolat IP30, W850, D600, ventilátor 3500 m3/h"]
["41885","ZENERGY - POKRYWA GÓRNA IP43, W850, D800, wentylator 350mm, 3500m3/h",946,"1-ZE-01",9.166666666666666E-2,4,"OE_COVERS","41885","SZT","85389099",null,null,"5901988316853","OE - Capot supérieur IP30, L850, P800, ventilateur 3500 m3/h","OE - Top cover IP30, W850, D800, ventilator 3500 m3/h","OE- TECHO IP30, W850, D800, fan 3500 m3/h","ZENERGY - FELSŐ BURKOLAT IP43, W850, D800, 350 mm-es ventilátor, 3500 m3/h"]
["41930","Zenergy - Pokrywa górna IP30, W300, D1000",214.5,"1-ZE-01",null,null,"OE_COVERS","41930","SZT","85389099",null,"210326LK","5901988419301","OE - Capot supérieur IP30, L300, P1000","OE - Top cover IP30, W300, D1000","OE- TECHO IP30, W300, D1000","Zenergy - Felső burkolat IP30, W300, D1000"]
["41960","Zenergy - Pokrywa górna IP30, W600, D1000",359.7,"1-ZE-01",null,null,"OE_COVERS","41960","SZT","85389099",null,"210326LK","5901988419608","OE - Capot supérieur IP30, L600, P1000","OE - Top cover IP30, W600, D1000","OE- TECHO IP30, W600, D1000","Zenergy - Felső burkolat IP30, W600, D1000"]
["42040","ZENERGY - RAMA, H1200 X D230 X W400",671.8,"1-ZE-01",0.01,1,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988420406","OE - Cradle, H1200 x P230 x L400","OE - Frame, H1200 x D230 x W400","OE- ESTRUCTURA, H1200 x D230 x W400","ZENERGY - KERET, H1200 X D230 X W400"]
["42065","ZENERGY - RAMA, H1200 X D230 X W650",731.2,"1-ZE-01",0.01,1,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988420659","OE - Cradle, H1200 x P230 x L650","OE - Frame, H1200 x D230 x W650","OE- ESTRUCTURA, H1200 x D230 x W650","ZENERGY - KERET, H1200 X D230 X W650"]
["42080","ZENERGY - RAMA, H1200 X D230 X W800",786.5,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988420802","OE - Cradle, H1200 x P230 x L800","OE - Frame, H1200 x D230 x W800","OE- ESTRUCTURA, H1200 x D230 x W800","ZENERGY - KERET, H1200 X D230 X W800"]
["42086","ZENERGY - RAMA, H1200 X D230 X W850, 650+200",1074.7,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988420864","OE - Cradle, H1200 x P230 x L850, 650 + 200","OE - Frame, H1200 x D230 x W850, 650 + 200","OE- ESTRUCTURA, H1200 x D230 x W850, 650+200","ZENERGY – KERET, H1200 X D230 X W850, 650+200"]
["42110","ZENERGY - RAMA, H1200 X D230 X W1100, 150+650+300",1347.5,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988421106","OE - Cadre, H1200 x P230 x L1100, 150 + 650 + 300","OE - Frame, H1200 x D230 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1200 x D230 x W1100, 150+650+300","ZENERGY – KERET, H1200 X D230 X W1100, 150+650+300"]
["42121","ZENERGY - RAMA, H1200 X D230 X W1200, 150+650+400",1379.4,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988421212","OE - Cadre, H1200 x P230 x L1200, 150 + 650 + 400","OE - Frame, H1200 x D230 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1200 x D230 x W1200, 150+650+400","ZENERGY – KERET, H1200 X D230 X W1200, 150+650+400"]
["42131","ZENERGY - RAMA, H1200 X D230 X W1300, 650+650",1193.5,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988421311","OE - Cadre, H1200 x P230 x L1300, 650 + 650","OE - Frame, H1200 x D230 x W1300, 650 + 650","OE- ESTRUCTURA, H1200 x D230 x W1300, 650+650","ZENERGY – KERET, H1200 X D230 X W1300, 650+650"]
["42411","ZENERGY - POKRYWA GÓRNA IP43, W1000, D400, otwory na 3 wentylatory",463.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP43, W1000, D400, nyílások 3 ventilátornak"]
["42414","ZENERGY - POKRYWA GÓRNA IP43, W1200, D400, otwory na 3 wentylatory",504.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP43, W1200, D400, nyílások 3 ventilátornak"]
["42415","ZENERGY - POKRYWA GÓRNA IP43, W1300, D400, otwory na 3 wentylatory",526.29999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP43, W1300, D400, nyílások 3 ventilátornak"]
["42481","ZENERGY - POKRYWA GÓRNA IP43, W650+150, D400, otwory na 2 wentylatory",401.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP43, W650+150, D400, lyukak 2 ventilátornak"]
["42610","ZENERGY - POKRYWA GÓRNA IP43, W1000, D600, otwory na 2 wentylatory",484.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP43, W1000, D600, lyukak 2 ventilátornak"]
["42614","ZENERGY - POKRYWA GÓRNA IP43, W1200, D600, otwory na 3 wentylatory",554.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP43, W1200, D600, nyílások 3 ventilátornak"]
["42680","ZENERGY - POKRYWA GÓRNA IP43, W800, D600, otwory na 2 wentylatory",435.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP43, W800, D600, lyukak 2 ventilátornak"]
["42686","ZENERGY - POKRYWA GÓRNA IP43, W650+200, D600, otwory na 2 wentylatory",448,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP43, W650+200, D600, furatok 2 ventilátornak"]
["42813","ZENERGY - POKRYWA GÓRNA IP43, W1300, D800, otwory na 2 wentylatory",639.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP43, W1300, D800, nyílások 2 ventilátornak"]
["42865","ZENERGY - POKRYWA GÓRNA IP43, W650, D800, otwory na 2 wentylatory",450.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP43, W650, D800, lyukak 2 ventilátornak"]
["42880","ZENERGY - POKRYWA GÓRNA IP43, W800, D800, otwory na 2 wentylatory",494.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP43, W800, D800, lyukak 2 ventilátornak"]
["42886","ZENERGY - POKRYWA GÓRNA IP43, W650+200, D800, otwory na 2 wentylatory",510.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP43, W650+200, D800, furatok 2 ventilátornak"]
["43060","ZENERGY - RAMA, H1200 X D300 X W600",762.3,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988430603","OE - Cadre, H1200 x P300 x L600","OE - Frame, H1200 x D300 x W600","OE- ESTRUCTURA, H1200 x D300 x W600","ZENERGY - KERET, H1200 X D300 X W600"]
["43085","ZENERGY - RAMA, H1200 X D300 X W850",831.6,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988430856","OE - Cradle, H1200 x P300 x L850","OE - Frame, H1200 x D300 x W850","OE- ESTRUCTURA, H1200 x D300 x W850","ZENERGY - KERET, H1200 X D300 X W850"]
["43100","ZENERGY - RAMA, H1200 X D300 X W1000",888.8,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988431006","OE - Cradle, H1200 x P300 x P1000","OE - Frame, H1200 x D300 x W1000","OE- ESTRUCTURA, H1200 x D300 x W1000","ZENERGY - KERET, H1200 X D300 X W1000"]
["43120","ZENERGY - RAMA, H1200 X D300 X W1200",954.8,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988431204","OE - Cradle, H1200 x P300 x L1200","OE - Frame, H1200 x D300 x W1200","OE- ESTRUCTURA, H1200 x D300 x W1200","ZENERGY - KERET, H1200 X D300 X W1200"]
["43130","ZENERGY - RAMA, H1200 X D300 X W1300",973.5,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988431303","OE - Cradle, H1200 x P300 x L1300","OE - Frame, H1200 x D300 x W1300","OE- ESTRUCTURA, H1200 x D300 x W1300","ZENERGY - KERET, H1200 X D300 X W1300"]
["43170","ZENERGY - RAMA, H1200 X D300 X W1700, 850+850",1342,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988431709","OE - Cadre, H1200 x P300 x L1700, 850 + 850","OE - Frame, H1200 x D300 x W1700, 850 + 850","OE- ESTRUCTURA, H1200 x D300 x W1700, 850+850","ZENERGY – KERET, H1200 X D300 X W1700, 850+850"]
["43410","ZENERGY - POKRYWA GÓRNA IP30, W1000, D400, otwór na 1 wentylator",391.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1000, D400, 1 ventilátor számára nyíló"]
["43430","ZENERGY - POKRYWA GÓRNA IP30, W300, D400, otwór na 1 wentylator",266.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W300, D400, 1 ventilátor számára nyíló"]
["43460","ZENERGY - POKRYWA GÓRNA IP30, W600, D400, otwór na 1 wentylator",319.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W600, D400, 1 ventilátor számára nyíló"]
["43481","ZENERGY - POKRYWA GÓRNA IP30, W650+150, D400, otwór na 1 wentylator",355.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W650+150, D400, 1 ventilátor számára nyíló"]
["43610","ZENERGY - POKRYWA GÓRNA IP30, W1000, D600, otwór na 1 wentylator",428.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1000, D600, 1 ventilátor számára nyíló"]
["43640","ZENERGY - POKRYWA GÓRNA IP30, W400, D600, otwór na 1 wentylator",304.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W400, D600, 1 ventilátor számára nyíló"]
["43665","ZENERGY - POKRYWA GÓRNA IP30, W650, D600, otwór na 1 wentylator",355.5,"1-ZE-01",0.65833333333333333,2,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W650, D600, 1 ventilátor számára nyíló"]
["43681","ZENERGY - POKRYWA GÓRNA IP30, W650+150, D600, otwór na 1 wentylator",385.7,"1-ZE-01",0.25833333333333336,2,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W650+150, D600, 1 ventilátor számára nyíló"]
["43685","ZENERGY - POKRYWA GÓRNA IP30, W850, D600, otwór na 1 wentylator",396.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W850, D600, 1 ventilátor számára nyíló"]
["43812","ZENERGY - POKRYWA GÓRNA IP30, W1200, D800, otwór na 1 wentylator",542.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1200, D800, 1 ventilátor számára nyíló"]
["43840","ZENERGY - POKRYWA GÓRNA IP30, W400, D800, otwór na 1 wentylator",334.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W400, D800, 1 ventilátor számára nyíló"]
["43866","ZENERGY - POKRYWA GÓRNA IP30, W450+200, D800, otwór na 1 wentylator",398.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W450+200, D800, 1 ventilátor számára nyíló"]
["43885","ZENERGY - POKRYWA GÓRNA IP30, W850, D800, otwór na 1 wentylator",452,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W850, D800, 1 ventilátor számára nyíló"]
["44040","ZENERGY - RAMA, H1200 X D400 X W400",745.2,"1-ZE-01",0.01,1,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988440404","OE - Cradle, H1200 x P400 x P400","OE - Frame, H1200 x D400 x W400","OE- ESTRUCTURA, H1200 x D400 x W400","ZENERGY - KERET, H1200 X D400 X W400"]
["44060","ZENERGY - RAMA, H1200 X D400 X W600",791.6,"1-ZE-01",1.6666666666666666E-2,1,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988440602","OE - Cadre, H1200 x P400 x L600","OE - Frame, H1200 x D400 x W600","OE- ESTRUCTURA, H1200 x D400 x W600","ZENERGY - KERET, H1200 X D400 X W600"]
["44086","ZENERGY - RAMA, H1200 X D400 X W850 650+200",1177,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988440862","OE - Cradle, H1200 x P400 x L850 650 + 200","OE - Frame, H1200 x D400 x W850 650 + 200","OE- ESTRUCTURA, H1200 x D400 x W850 650+200","ZENERGY – KERET, H1200 X D400 X W850 650+200"]
["44095","ZENERGY - RAMA, H1200 X D400 X W950, 650+300",1216.5999999999999,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988440954","OE - Cradle, H1200 x P400 x L950, 650 + 300","OE - Frame, H1200 x D400 x W950, 650 + 300","OE- ESTRUCTURA, H1200 x D400 x W950, 650+300","ZENERGY – KERET, H1200 X D400 X W950, 650+300"]
["44110","ZENERGY - RAMA, H1200 X D400 X W1100, 150+650+300",1467.4,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988441104","OE - Cadre, H1200 x P400 x L1100, 150 + 650 + 300","OE - Frame, H1200 x D400 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1200 x D400 x W1100, 150+650+300","ZENERGY – KERET, H1200 X D400 X W1100, 150+650+300"]
["44125","ZENERGY - RAMA, H1200 X D400 X W1250, 850+400",1303.5,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988441258","OE - Cadre, H1200 x P400 x L1250, 850 + 400","OE - Frame, H1200 x D400 x W1250, 850 + 400","OE- ESTRUCTURA, H1200 x D400 x W1250, 850+400","ZENERGY – KERET, H1200 X D400 X W1250, 850+400"]
["44150","ZENERGY - RAMA, H1200 X D400 X W1500 650+850",1353,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988441500","OE - Cadre, H1200 x P400 x P1500 650 + 850","OE - Frame, H1200 x D400 x W1500 650 + 850","OE- ESTRUCTURA, H1200 x D400 x W1500 650+850","ZENERGY – KERET, H1200 X D400 X W1500 650+850"]
["44410","ZENERGY - POKRYWA GÓRNA IP30, W1000, D400, otwory na 2 wentylatory",411.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1000, D400, lyukak 2 ventilátornak"]
["44414","ZENERGY - POKRYWA GÓRNA IP30, W1200, D400, otwory na 3 wentylatory",469.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1200, D400, nyílások 3 ventilátornak"]
["44480","ZENERGY - POKRYWA GÓRNA IP30, W800, D400, otwory na 2 wentylatory",373.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W800, D400, lyukak 2 ventilátornak"]
["44486","ZENERGY - POKRYWA GÓRNA IP30, W650+200, D400, otwory na 2 wentylatory",382.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP30, W650+200, D400, furatok 2 ventilátornak"]
["44610","ZENERGY - POKRYWA GÓRNA IP30, W1000, D600, otwory na 2 wentylatory",450.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1000, D600, nyílások 2 ventilátornak"]
["44613","ZENERGY - POKRYWA GÓRNA IP30, W1300, D600, otwory na 2 wentylatory",514.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W1300, D600, lyukak 2 ventilátornak"]
["44680","ZENERGY - POKRYWA GÓRNA IP30, W800, D600, otwory na 2 wentylatory",405,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W800, D600, lyukak 2 ventilátornak"]
["44686","ZENERGY - POKRYWA GÓRNA IP30, W650+200, D600, otwory na 2 wentylatory",416.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W650+200, D600, lyukak 2 ventilátornak"]
["44812","ZENERGY - POKRYWA GÓRNA IP30, W1200, D800, otwory na 2 wentylatory",569.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ FEDÉL IP30, W1200, D800, lyukak 2 ventilátornak"]
["44865","ZENERGY - POKRYWA GÓRNA IP30, W650, D800, otwory na 2 wentylatory",418.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W650, D800, lyukak 2 ventilátornak"]
["44885","ZENERGY - POKRYWA GÓRNA IP30, W850, D800, otwory na 2 wentylatory",474.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - FELSŐ BURKOLAT IP30, W850, D800, lyukak 2 ventilátornak"]
["45340","ZENERGY - DRZWI PRZEDZIAŁU KABLOWEGO IP30, H1200 X W400",277.2,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988453404","OE - Portes du compartiment à câbles IP30, H1200 x L400","OE - Cable compartment door IP30, H1200 x W400","OE- PUERTA PARA MOD. CABLES IP30, H1200 x W400","ZENERGY - KÁBELREKESZ AJTÓ IP30, H1200 X W400"]
["46030","ZENERGY - RAMA, H1200 X D600 X W300",992.2,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988460303","OE - Cradle, H1200 x P600 x L300","OE - Frame, H1200 x D600 x W300","OE- ESTRUCTURA, H1200 x D600 x W300","ZENERGY - KERET, H1200 X D600 X W300"]
["46060","ZENERGY - RAMA, H1200 X D600 X W600",1096.2,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988460600","OE - Cadre, H1200 x P600 x L600","OE - Frame, H1200 x D600 x W600","OE- ESTRUCTURA, H1200 x D600 x W600","ZENERGY - KERET, H1200 X D600 X W600"]
["46085","ZENERGY - RAMA, H1200 X D600 X W850",1216.0999999999999,"1-ZE-01",null,null,"OE_FRAME_1200","46085","SZT","85389099",null,null,"5901988460853","OE - Cradle, H1200 x P600 x L850","OE - Frame, H1200 x D600 x W850","OE- ESTRUCTURA, H1200 x D600 x W850","ZENERGY - KERET, H1200 X D600 X W850"]
["46105","ZENERGY - RAMA, H1200 X D600 X W1050, 650+400",1692.9,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988461058","OE - Cadre, H1200 x P600 x L1050, 650 + 400","OE - Frame, H1200 x D600 x W1050, 650 + 400","OE- ESTRUCTURA, H1200 x D600 x W1050, 650+400","ZENERGY – KERET, H1200 X D600 X W1050, 650+400"]
["46120","ZENERGY - RAMA, H1200 X D600 X W1200",1394.8,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988461201","OE - Cadre, H1200 x P600 x L1200","OE - Frame, H1200 x D600 x W1200","OE- ESTRUCTURA, H1200 x D600 x W1200","ZENERGY - KERET, H1200 X D600 X W1200"]
["46131","ZENERGY - RAMA, H1200 X D600 X W1300, 650+650",1784.2,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988461317","OE - Cadre, H1200 x P600 x L1300, 650 + 650","OE - Frame, H1200 x D600 x W1300, 650 + 650","OE- ESTRUCTURA, H1200 x D600 x W1300, 650+650","ZENERGY – KERET, H1200 X D600 X W1300, 650+650"]
["48030","ZENERGY - RAMA, H1200 X D800 X W300",1079.7,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988480301","OE - Cradle, H1200 x P800 x L300","OE - Frame, H1200 x D800 x W300","OE- ESTRUCTURA, H1200 x D800 x W300","ZENERGY - KERET, H1200 X D800 X W300"]
["48040","ZENERGY - RAMA, H1200 X D800 X W400",1146.9000000000001,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988480400","OE - Cradle, H1200 x P800 x L400","OE - Frame, H1200 x D800 x W400","OE- ESTRUCTURA, H1200 x D800 x W400","ZENERGY - KERET, H1200 X D800 X W400"]
["48065","ZENERGY - RAMA, H1200 X D800 X W650",1248.8,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988480653","OE - Cradle, H1200 x P800 x L650","OE - Frame, H1200 x D800 x W650","OE- ESTRUCTURA, H1200 x D800 x W650","ZENERGY - KERET, H1200 X D800 X W650"]
["48085","ZENERGY - RAMA, H1200 X D800 X W850",1349.6,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988480851","OE - Cradle, H1200 x P800 x L850","OE - Frame, H1200 x D800 x W850","OE- ESTRUCTURA, H1200 x D800 x W850","ZENERGY - KERET, H1200 X D800 X W850"]
["48105","ZENERGY - RAMA, H1200 X D800 X W1050, 650+400",1844.6,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988481056","OE - Cadre, H1200 x P800 x L1050, 650 + 400","OE - Frame, H1200 x D800 x W1050, 650 + 400","OE- ESTRUCTURA, H1200 x D800 x W1050, 650+400","ZENERGY – KERET, H1200 X D800 X W1050, 650+400"]
["48120","ZENERGY - RAMA, H1200 X D800 X W1200",1518.7,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988481209","OE - Cradle, H1200 x P800 x L1200","OE - Frame, H1200 x D800 x W1200","OE- ESTRUCTURA, H1200 x D800 x W1200","ZENERGY - KERET, H1200 X D800 X W1200"]
["48130","ZENERGY - RAMA, H1200 X D800 X W1300",1553.4,"1-ZE-01",null,null,"OE_FRAME_1200",null,"SZT","85389099",null,null,"5901988481308","OE - Cradle, H1200 x P800 x L1300","OE - Frame, H1200 x D800 x W1300","OE- ESTRUCTURA, H1200 x D800 x W1300","ZENERGY - KERET, H1200 X D800 X W1300"]
["49223","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1200 X D230",568.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988492236","OE - Hottes de ventilation latérales IP30, H1200 x P230","OE - IP30, H1200 x D230 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1200 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1200 X D230"]
["49260","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1200 X D600",630.70000000000005,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988492601","OE - Hottes de ventilation latérales IP30, H1200 x P600","OE - IP30, H1200 x D600 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1200 x D600 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1200 X D600"]
["49280","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1200 X D800",663.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988492809","OE - Hottes de ventilation latérales IP30, H1200 x P800","OE - IP30, H1200 x D800 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1200 x D800 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1200 X D800"]
["49325","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H1200 X D230",197.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988493257","OE - Capots latéraux solides, plats, vissés IP30, H1200 x P230","OE - Side panels Plain, flat, screwed on, IP30, H1200 x D230","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H1200 x D230 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H1200 X D230"]
["49340","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H1200 X D400",543.20000000000005,"1-ZE-01",3.3333333333333333E-2,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988493400","OE - Couvercles latéraux complets IP30, H1200 x P400","OE - Plain side covers IP30, H1200 x D400","OE- PAREDES LATERALES LISO IP30, H1200 x D400  (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H1200 X D400"]
["49361","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1200 X D600",279.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988493615","OE - Couvercles latéraux complets, fixes IP30, H1200 x P600","OE - Plain, fixed side covers IP30, H1200 x D600","OE- PAREDES LATERALES LISO FIJO IP30, H1200 x D600 (2UDS)","ZENERGY – TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H1200 X D600"]
["49381","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1200 X D800",330,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988493813","OE - Couvercles latéraux complets, fixes IP30, H1400 x P800","OE - Plain side covers, fixed IP30, H1200 x D800","OE- PAREDES LATERALES LISO FIJO IP30, H1400 x D800 (2UDS)","ZENERGY – OLDALBURKOLATOK, TELJES, RÖGZÍTETT, IP30, H1200 X D800"]
["49440","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1200 X D400",672.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988494407","OE - Hottes de ventilation latérales IP43, H1200 x P400","OE - IP43, H1200 x D400 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1200 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H1200 X D400"]
["49523","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1200 X D230",564.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988495237","OE - Couvercles latéraux complets IP55, H1200 x P230","OE - Plain side covers IP55, H1200 x D230","OE- PAREDES LATERALES LISO IP55, H1200 x D230 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1200 X D230"]
["49560","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1200 X D600",657.7,"1-ZE-01",0.01,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988495602","OE - Capots latéraux, intégralement IP55, H1200 x P600","OE - Plain side covers IP55, H1200 x D600","OE- PAREDES LATERALES LISO IP55, H1200 x D600 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1200 X D600"]
["50111","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1400 W1000 DO PLOMBOWANIA",453.2,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988501112","OE - H1400 L1000 cadre de cadre à charnière avant pour sceller","OE - Frame of Front covers on hinges H1400 W1000 for sealing","OE- MARCO PIVOTANTE H1400 W1000 ","ZENERGY - ZSÁNLÓS ELSŐ FEDŐKERET H1400 W1000 TÖMÍTÉSHEZ"]
["50141","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1400 W400 DO PLOMBOWANIA",303.60000000000002,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988501419","OE - H1400 L400 Cadre de panneau avant articulé pour sceller","OE - The frame of Front covers on hinges H1400 W400 for sealing","OE- MARCO PIVOTANTE H1400 W400 ","ZENERGY - ZSÁNLÓS ELSŐ FEDŐKERET H1400 W400 TÖMÍTÉSHEZ"]
["50165","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1400 W650",329.4,"1-ZE-01",0.2,1,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988501655","OE - H1400 L650 cadre de panneau avant articulé","OE - Hinged Front covers frame H1400 W650","OE- MARCO PIVOTANTE H1400 W650","ZENERGY - SZÁNTOS ELSŐ BURKOLAT KERET H1400 W650"]
["50185","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1400 W850",384.5,"1-ZE-01",1.6666666666666666E-2,1,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988501853","OE - H1400 L850 cadre de panneau avant articulé","OE - The frame of the hinged Front covers H1400 W850","OE- MARCO PIVOTANTE H1400 W850","ZENERGY - SZÁNTOS ELSŐ BURKOLAT KERET H1400 W850"]
["50212","ZENERGY - DRZWI WENTYLOWANE IP30, H1400 X W1200, PODWÓJNE",2180.5,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988502126","OE - Portes ventilée double IP14, H1400 x L1200","OE - Ventilated door IP30, H1400 x W1200, double","OE- PUERTA VENTIL. IP30, H1400 x W1200, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1400 X W1200, DUPLÉS"]
["50240","ZENERGY - DRZWI WENTYLOWANE IP30, H1400 X W400",897.5,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988502409","OE - Portes ventilées IP30, H1400 x L400","OE - Ventilated door IP30, H1400 x W400","OE- PUERTA VENTIL. IP30, H1400 x W400","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1400 X W400"]
["50265","ZENERGY - DRZWI WENTYLOWANE IP30, H1400 X W650",1089.7,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988502652","OE - Portes ventilées IP30, H1400 x L650","OE - Ventilated door IP30, H1400 x W650","OE- PUERTA VENTIL. IP30, H1400 x W650","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1400 X W650"]
["50295","ZENERGY - DRZWI WENTYLOWANE IP30, H1400 X W950",1294.9000000000001,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988502959","OE - Portes ventilées IP30, H1400 x L950","OE - Ventilated door IP30, H1400 x W950","OE- PUERTA VENTIL. IP30, H1400 x W950","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1400 X W950"]
["50310","ZENERGY - DRZWI PEŁNE IP30, H1400 X W1000",1317.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988503109","OE - Portes pleine IP30, H1400 x L1000","OE - Plain door IP30, H1400 x W1000","OE- PUERTA OPACA IP30, H1400 x W1000","ZENERGY - TÖMÖR AJTÓ IP30, H1400 X W1000"]
["50313","ZENERGY - DRZWI PEŁNE IP30, H1400 X W1300, PODWÓJNE",2110.3000000000002,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988503130","OE - Portes pleine IP30, H1400 x L1300, double","OE - Plain door IP30, H1400 x W1300, double","OE- PUERTA OPACA IP30, H1400 x W1300, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H1400 X W1300, DUPLA"]
["50340","ZENERGY - DRZWI PEŁNE IP30, H1400 X W400",853.2,"1-ZE-01",1.6666666666666666E-2,2,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988503406","OE - Portes pleine IP30, H1400 x L400","OE - Plain door IP30, H1400 x W400","OE- PUERTA OPACA IP30, H1400 x W400","ZENERGY - TÖMÖR AJTÓ IP30, H1400 X W400"]
["50371","ZENERGY - SŁUPEK OCYNK, H1400, RAMA ZEWNĘTRZNA",52.7,"1-ZE-01",5.8333333333333334E-2,1,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988503710","OE - poteau galvanisé, H1400, cadre externe","OE - Galvanized post, H1400, external frame","OE- PERFIL GALVANIZADO, H1400, PARA MARCO LATERAL EXTERIOR","ZENERGY - HORGANYOZOTT OSZT, H1400, KÜLSŐ KERET"]
["50374","ZENERGY - SŁUPEK INOX, H1400, RAMA WEWNETRZNA",121,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988503741","OE - Poteau INOX, H1400, cadre interne","OE - INOX post, H1400, internal frame","OE- PERFIL INOX, H1400, PARA MARCO LATERAL INTERIOR","ZENERGY – SZÓUPEK INOX, H1400, BELSŐ KERET"]
["50410","ZENERGY - DRZWI WENTYLOWANE IP43, H1400 X W1000",1446.1,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988504106","OE - Portes ventilées IP43, H1400 x L1000","OE - Ventilated door IP43, H1400 x W1000","OE- PUERTA VENTIL. IP43, H1400 x W1000","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1400 X W1000"]
["50414","ZENERGY - DRZWI WENTYLOWANE IP43, H1400 X W1050",1517.4,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988504144","OE - Portes ventilées IP43, H1400 x L1050","OE - Ventilated door IP43, H1400 x W1050","OE- PUERTA VENTIL. IP43, H1400 x W1050","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1400 X W1050"]
["50445","ZENERGY - DRZWI WENTYLOWANE IP43, H1400 X W450",1234.4000000000001,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988504458","OE - Portes ventilées IP43, H1400 x L450","OE - Ventilated door IP43, H1400 x W450","OE- PUERTA VENTIL. IP43, H1400 x W450","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1400 X W450"]
["50460","ZENERGY - DRZWI WENTYLOWANE IP43, H1400 X W600",1137.2,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988504601","OE - Portes ventilées IP43, H1400 x L600","OE - Ventilated door IP43, H1400 x W600","OE- PUERTA VENTIL. IP43, H1400 x W600","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1400 X W600"]
["50485","ZENERGY - DRZWI WENTYLOWANE IP43, H1400 X W850",1326.2,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988504854","OE - Portes ventilées IP43, H1400 x L850","OE - Ventilated door IP43, H1400 x W850","OE- PUERTA VENTIL. IP43, H1400 x W850","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1400 X W850"]
["50512","ZENERGY - DRZWI PEŁNE IP55, H1400 X W1200, PODWÓJNE",2028.2,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988505127","OE - Portes pleine IP55, H1400 x L1200, double","OE - Plain door IP55, H1400 x W1200, double","OE- PUERTA OPACA IP55, H1400 x W1200, DOBLE","ZENERGY - TÖMÖR AJTÓ IP55, H1400 X W1200, DUPLÉS"]
["50530","ZENERGY - DRZWI PEŁNE IP55, H1400 X W300",838.1,"1-ZE-01",0.2,5,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988505301","OE - Portes pleine IP55, H1400 x L300","OE - Plain door IP55, H1400 x W300","OE- PUERTA OPACA IP55, H1400 x W300","ZENERGY - TÖMÖR AJTÓ IP55, H1400 X W300"]
["50565","ZENERGY - DRZWI PEŁNE IP55, H1400 X W650",1122.0999999999999,"1-ZE-01",0.20833333333333334,2,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988505653","OE - Portes pleine IP55, H1400 x L650","OE - Plain door IP55, H1400 x W650","OE- PUERTA OPACA IP55, H1400 x W650","ZENERGY - TÖMÖR AJTÓ IP55, H1400 X W650"]
["50610","ZENERGY - DRZWI PRZESZKLONE IP55, H1400 X W1000",1738.8,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988506100","OE - Portes vitrée IP55, H1400 x L1000","OE - Glazed door IP55, H1400 x W1000","OE- PUERTA TRANSPARENTE IP55, H1400 x W1000","ZENERGY - ÜVEGAJTÓK IP55, H1400 X W1000"]
["50640","ZENERGY - DRZWI PRZESZKLONE IP55, H1400 X W400",1039,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988506407","OE - Portes vitrée IP55, H1400 x L400","OE - Glazed door IP55, H1400 x W400","OE- PUERTA TRANSPARENTE IP55, H1400 x W400","ZENERGY - ÜVEZETETT AJTÓK IP55, H1400 X W400"]
["50665","ZENERGY - DRZWI PRZESZKLONE IP55, H1400 X W650",1338.1,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988506650","OE - Portes vitrée IP55, H1400 x L650","OE - Glazed door IP55, H1400 x W650","OE- PUERTA TRANSPARENTE IP55, H1400 x W650","ZENERGY - ÜVEZETETT AJTÓK IP55, H1400 X W650"]
["50680","ZENERGY - DRZWI PRZESZKLONE IP55, H1400 X W800",1509.8,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988506803","OE - Portes vitrée IP55, H1400 x L800","OE - Glazed door IP55, H1400 x W800","OE- PUERTA TRANSPARENTE IP55, H1400 x W800","ZENERGY - ÜVEZETETT AJTÓK IP55, H1400 X W800"]
["50742","ZENERGY - SŁUPEK OCYNK, H1400, RAMA WEWNĘTRZNA, PODWÓJNA",69.7,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988507428","OE - poteau galvanisé, H1400, cadre interne, double","OE - Galvanized post, H1400, double inner frame","OE- PERFIL GALVANIZADO, H1400,  PARA MARCO LATERAL INTERIOR, DOBLE","ZENERGY - horganyzott oszlop, H1400, BELSŐ KERET, DUPLÁS"]
["50885","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 7X EFEN 160-630, H1400 X W850, 20+4M",594,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988508852","OE - Cadre pivotant d'interrupteurs-sectionneurs 7x EFEN 160-630, H1400 x L850, 20 + 4M","OE - Hinged frame for switch disconnectors 7x EFEN 160-630, H1400 x W850, 20 + 4M","OE- ESTRUCTURA PARA REGLETAS SECC. 7X160-630, H1400 x W850, 20+4M","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 7X EFEN 160-630, H1400 X W850, 20+4M"]
["50913","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1400 X W1300 + WSPORNIKI,  ( 1250 X 1200 )",1006.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988509132","OE - Plaque de montage complète H1400 x L1300 + supports, (1250 x 1200)","OE - Plain Mounting plate H1400 x W1300 + brackets, (1250 x 1200)","OE- PLACA MONTAJE  TOTAL CIEGA H1400 x W1300 + SOPORT. (1250 X 1200)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1400 X W1300 + KONZEREK, (1250 X 1200)"]
["50945","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1400 X W450 + WSPORNIKI,  ( 1250 X 350 )",409.3,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988509453","OE - Plaque de montage complète H1400 x L450 + supports, (1250 x 350)","OE - Plain Mounting plate H1400 x W450 + brackets, (1250 x 350)","OE- PLACA MONTAJE  TOTAL CIEGA H1400 x W450 + SOPORT. (1250 X 350)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H1400 X W450 + KONZEREK, (1250 X 350)"]
["50985","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1400 X W850 + WSPORNIKI,  ( 1250 X 750 )",694.4,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988509859","OE - Plaque de montage complète H1400 x L850 + supports, (1250 x 750)","OE - Plain Mounting plate H1400 x W850 + brackets, (1250 x 750)","OE- PLACA MONTAJE  TOTAL CIEGA H1400 x W850 + SOPORT. (1250 X 750)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1400 X W850 + KONZEREK, (1250 X 750)"]
["51112","ZENERGY - DRZWI PRZESZKLONE IP30, H1400 X W1200, PODWÓJNE",2378.1999999999998,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988511128","OE - Portes vitrées IP30, H1400 x L1200, double vitrage","OE - Glazed door IP30, H1400 x W1200, double","OE- PUERTA TRANSP. IP30, H1400 x W1200, doble","ZENERGY - ÜVEGAJTÓK IP30, H1400 X W1200, DUPLA"]
["51113","ZENERGY - DRZWI PRZESZKLONE IP30, H1400 X W1300, PODWÓJNE",2410.6,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988511135","OE - Portes vitrées IP30, H1400 x L1300, double vitrage","OE - Glazed door IP30, H1400 x W1300, double","OE- PUERTA TRANSP. IP30, H1400 x W1300, doble","ZENERGY - ÜVEGAJTÓK IP30, H1400 X W1300, DUPLA"]
["51160","ZENERGY - DRZWI PRZESZKLONE IP30, H1400 X W600",1163.2,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988511609","OE - Portes vitrées IP30, H1400 x L600","OE - Glazed door IP30, H1400 x W600","OE- PUERTA TRANSP. IP30, H1400 x W600","ZENERGY - ÜVEZETETT AJTÓK IP30, H1400 X W600"]
["51185","ZENERGY - DRZWI PRZESZKLONE IP30, H1400 X W850",1410.5,"1-ZE-01",null,null,"OE_DOORS_1400",null,"SZT","85389099",null,null,"5901988511852","OE - Portes vitrées IP30, H1400 x L850","OE - Glazed door IP30, H1400 x W850","OE- PUERTA TRANSP. IP30, H1400 x W850","ZENERGY - ÜVEZETETT AJTÓK IP30, H1400 X W850"]
["51212","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1400 X W1200",1001.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988512125","OE - Couverture arrière complète IP30, H1400 x L1200","OE - Plain rear cover IP30, H1400 x W1200","OE- FONDO ATORNILLADO LISO IP30, H1400 x W1200","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1400 X W1200"]
["51240","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1400 X W400",384.5,"1-ZE-01",1.6666666666666666E-2,2,"OE_COVERS",null,"SZT","85389099",null,null,"5901988512408","OE - Couverture arrière complète IP30, H1400 x L400","OE - Plain rear cover IP30, H1400 x W400","OE- FONDO ATORNILLADO LISO IP30, H1400 x W400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1400 X W400"]
["51265","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1400 X W650",523.79999999999995,"1-ZE-01",0.3,5,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988512651","OE - Couverture arrière complète IP30, H1400 x L650","OE - Plain rear cover IP30, H1400 x W650","OE- FONDO ATORNILLADO LISO IP30, H1400 x W650","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1400 X W650"]
["51310","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1400 X W1000",726.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988513108","OE - Hotte d'aération arrière IP30, H1400 x L1000","OE - Rear ventilated cover IP30, H1400 x W1000","OE- FONDO ATORNILLADO VENTIL. IP30, H1400 x W1000","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1400 X W1000"]
["51313","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1400 X W1300",1138.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988513139","OE - Couvercle ventilé IP30, H1400 x L1300","OE - Rear ventilated cover IP30, H1400 x W1300","OE- FONDO ATORNILLADO VENTIL. IP30, H1400 x W1300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1400 X W1300"]
["51330","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1400 X W300",338,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988513306","OE - Hotte d'aération arrière IP30, H1400 x L300","OE - Rear ventilated cover IP30, H1400 x W300","OE- FONDO ATORNILLADO VENTIL. IP30, H1400 x W300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1400 X W300"]
["51380","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1400 X W800",659.9,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988513801","OE - Hotte d'aération arrière IP30, H1400 x L800","OE - Rear ventilated cover IP30, H1400 x W800","OE- FONDO ATORNILLADO VENTIL. IP30, H1400 x W800","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1400 X W800"]
["51395","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1400 X W650+300",738.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988513955","OE - Couverture arrière ventilée IP30, H1400 x L650 + 300","OE - Rear ventilated cover IP30, H1400 x W650 + 300","OE- FONDO ATORNILLADO VENTIL. IP30, H1400 x W650+300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1400 X W650+300"]
["51413","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1400 X W1300",1289.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988514136","OE - Coque arrière ventilée IP43, H1400 x L1300","OE - Rear ventilated cover IP43, H1400 x W1300","OE- FONDO ATORNILLADO VENTIL.IP43, H1400 x W1300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1400 X W1300"]
["51445","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1400 X W450",546.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988514457","OE - Coque arrière ventilée IP43, H1400 x L450","OE - Rear ventilated cover IP43, H1400 x W450","OE- FONDO ATORNILLADO VENTIL.IP43, H1400 x W450","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1400 X W450"]
["51480","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1400 X W800",738.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988514808","OE - Couverture arrière ventilée IP43, H1400 x L800","OE - Rear ventilated cover IP43, H1400 x W800","OE- FONDO ATORNILLADO VENTIL.IP43, H1400 x W800","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1400 X W800"]
["51511","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1400 X W850+200",841.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988515119","OE - Couverture arrière complète IP55, H1400 x L650 + 400","OE - Plain rear cover IP55, H1400 x W850 + 200","OE- FONDO ATORNILLADO LISO IP55, H1400 x W650+400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1400 X W850+200"]
["51530","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1400 X W300",335.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988515300","OE - Couverture arrière complète IP55, H1400 x L300","OE - Plain rear cover IP55, H1400 x W300","OE- FONDO ATORNILLADO LISO IP55, H1400 x W300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1400 X W300"]
["51540","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1400 X W400",452.5,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988515409","OE - Couverture arrière complète IP55, H1400 x L400","OE - Plain rear cover IP55, H1400 x W400","OE- FONDO ATORNILLADO LISO IP55, H1400 x W400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1400 X W400"]
["51565","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1400 X W650",599.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988515652","OE - Couverture arrière complète IP55, H1400 x L650","OE - Plain rear cover IP55, H1400 x W650","OE- FONDO ATORNILLADO LISO IP55, H1400 x W650","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1400 X W650"]
["51595","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1400 X W650+300",748.4,"1-ZE-01",0.19166666666666668,4,"OE_COVERS",null,"SZT","85389099",null,null,"5901988515959","OE - Couverture arrière complète IP55, H1400 x L650 + 300","OE - Plain rear cover IP55, H1400 x W650 + 300","OE- FONDO ATORNILLADO LISO IP55, H1400 x W650+300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1400 X W650+300"]
["52045","ZENERGY - RAMA, H1400 X D230 X W450",711.7,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988520458","OE - Cradle, H1400 x P230 x L450","OE - Frame, H1400 x D230 x W450","OE- ESTRUCTURA, H1400 x D230 x W450","ZENERGY - KERET, H1400 X D230 X W450"]
["52080","ZENERGY - RAMA, H1400 X D230 X W800",862.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988520809","OE - Cradle, H1400 x P230 x L800","OE - Frame, H1400 x D230 x W800","OE- ESTRUCTURA, H1400 x D230 x W800","ZENERGY - KERET, H1400 X D230 X W800"]
["52095","ZENERGY - RAMA, H1400 X D230 X W950, 650+300",1135.2,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988520953","OE - Cradle, H1400 x P230 x L950, 650 + 300","OE - Frame, H1400 x D230 x W950, 650 + 300","OE- ESTRUCTURA, H1400 x D230 x W950, 650+300","ZENERGY – KERET, H1400 X D230 X W950, 650+300"]
["52110","ZENERGY - RAMA, H1400 X D230 X W1100, 150+650+300",1355.2,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988521103","OE - Cadre, H1400 x P230 x L1100, 150 + 650 + 300","OE - Frame, H1400 x D230 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1400 x D230 x W1100, 150+650+300","ZENERGY – KERET, H1400 X D230 X W1100, 150+650+300"]
["52121","ZENERGY - RAMA, H1400 X D230 X W1200, 150+650+400",1395.9,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988521219","OE - Cradle, H1400 x P230 x L1200, 150 + 650 + 400","OE - Frame, H1400 x D230 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1400 x D230 x W1200, 150+650+400","ZENERGY – KERET, H1400 X D230 X W1200, 150+650+400"]
["52125","ZENERGY - RAMA, H1400 X D230 X W1250, 850+400",1256.2,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988521257","OE - Cradle, H1400 x P230 x L1250, 850 + 400","OE - Frame, H1400 x D230 x W1250, 850 + 400","OE- ESTRUCTURA, H1400 x D230 x W1250, 850+400","ZENERGY – KERET, H1400 X D230 X W1250, 850+400"]
["52150","ZENERGY - RAMA, H1400 X D230 X W1500, 650+850",1357.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988521509","OE - Cadre, H1400 x P230 x L1500, 650 + 850","OE - Frame, H1400 x D230 x W1500, 650 + 850","OE- ESTRUCTURA, H1400 x D230 x W1500, 650+850","ZENERGY – KERET, H1400 X D230 X W1500, 650+850"]
["53040","ZENERGY - RAMA, H1400 X D300 X W400",730.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988530402","OE - Cradle, H1400 x P300 x L400","OE - Frame, H1400 x D300 x W400","OE- ESTRUCTURA, H1400 x D300 x W400","ZENERGY - KERET, H1400 X D300 X W400"]
["53080","ZENERGY - RAMA, H1400 X D300 X W800",903.1,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988530808","OE - Cradle, H1400 x P300 x L800","OE - Frame, H1400 x D300 x W800","OE- ESTRUCTURA, H1400 x D300 x W800","ZENERGY - KERET, H1400 X D300 X W800"]
["53086","ZENERGY - RAMA, H1400 X D300 X W850, 650+200",1081.3,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988530860","OE - Cradle, H1400 x P300 x L850, 650 + 200","OE - Frame, H1400 x D300 x W850, 650 + 200","OE- ESTRUCTURA, H1400 x D300 x W850, 650+200","ZENERGY – KERET, H1400 X D300 X W850, 650+200"]
["53110","ZENERGY - RAMA, H1400 X D300 X W1100, 150+650+300",1445.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988531102","OE - Cradle, H1400 x P300 x L1100, 150 + 650 + 300","OE - Frame, H1400 x D300 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1400 x D300 x W1100, 150+650+300","ZENERGY – KERET, H1400 X D300 X W1100, 150+650+300"]
["53125","ZENERGY - RAMA, H1400 X D300 X W1250, 850+400",1326.6,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988531256","OE - Cradle, H1400 x P300 x L1250, 850 + 400","OE - Frame, H1400 x D300 x W1250, 850 + 400","OE- ESTRUCTURA, H1400 x D300 x W1250, 850+400","ZENERGY – KERET, H1400 X D300 X W1250, 850+400"]
["53150","ZENERGY - RAMA, H1400 X D300 X W1500, 650+850",1427.8,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988531508","OE - Cradle, H1400 x P300 x L1500, 650 + 850","OE - Frame, H1400 x D300 x W1500, 650 + 850","OE- ESTRUCTURA, H1400 x D300 x W1500, 650+850","ZENERGY – KERET, H1400 X D300 X W1500, 650+850"]
["53170","ZENERGY - RAMA, H1400 X D300 X W1700, 850+850",1508.1,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988531706","OE - Cadre, H1400 x P300 x L1700, 850 + 850","OE - Frame, H1400 x D300 x W1700, 850 + 850","OE- ESTRUCTURA, H1400 x D300 x W1700, 850+850","ZENERGY – KERET, H1400 X D300 X W1700, 850+850"]
["54045","ZENERGY - RAMA, H1400 X D400 X W450",794.2,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988540456","OE - Cradle, H1400 x P400 x P450","OE - Frame, H1400 x D400 x W450","OE- ESTRUCTURA, H1400 x D400 x W450","ZENERGY - KERET, H1400 X D400 X W450"]
["54080","ZENERGY - RAMA, H1400 X D400 X W800",928.8,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988540807","OE - Cradle, H1400 x P400 x P800","OE - Frame, H1400 x D400 x W800","OE- ESTRUCTURA, H1400 x D400 x W800","ZENERGY - KERET, H1400 X D400 X W800"]
["54095","ZENERGY - RAMA, H1400 X D400 X W950, 650+300",1230.0999999999999,"1-ZE-01",0.19166666666666668,5,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988540951","OE - Cadre, H1400 x P400 x L950, 650 + 300","OE - Frame, H1400 x D400 x W950, 650 + 300","OE- ESTRUCTURA, H1400 x D400 x W950, 650+300","ZENERGY – KERET, H1400 X D400 X W950, 650+300"]
["54110","ZENERGY - RAMA, H1400 X D400 X W1100, 150+650+300",1514.7,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988541101","OE - Cadre, H1400 x P400 x L1100, 150 + 650 + 300","OE - Frame, H1400 x D400 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1400 x D400 x W1100, 150+650+300","ZENERGY – KERET, H1400 X D400 X W1100, 150+650+300"]
["54121","ZENERGY - RAMA, H1400 X D400 X W1200, 150+650+400",1555.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988541217","OE - Cadre, H1400 x P400 x L1200, 150 + 650 + 400","OE - Frame, H1400 x D400 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1400 x D400 x W1200, 150+650+400","ZENERGY – KERET, H1400 X D400 X W1200, 150+650+400"]
["54131","ZENERGY - RAMA, H1400 X D400 X W1300, 650+650",1395.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988541316","OE - Cradle, H1400 x P400 x L1300, 650 + 650","OE - Frame, H1400 x D400 x W1300, 650 + 650","OE- ESTRUCTURA, H1400 x D400 x W1300, 650+650","ZENERGY – KERET, H1400 X D400 X W1300, 650+650"]
["54170","ZENERGY - RAMA, H1400 X D400 X W1700, 850+850",1556.5,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988541705","OE - Cadre, H1400 x P400 x L1700, 850 + 850","OE - Frame, H1400 x D400 x W1700, 850 + 850","OE- ESTRUCTURA, H1400 x D400 x W1700, 850+850","ZENERGY – KERET, H1400 X D400 X W1700, 850+850"]
["55330","ZENERGY - DRZWI PRZEDZIAŁU KABLOWEGO IP30, H1400 X W300",280.5,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988553302","OE - Portes d'entrée de câble IP30, H1400 x L300","OE - Cable compartment door IP30, H1400 x W300","OE- PUERTA PARA MOD. CABLES IP30, H1400 x W300","ZENERGY - KÁBELREKESZ AJTÓ IP30, H1400 X W300"]
["56040","ZENERGY - RAMA, H1400 X D600 X W400",1095.5999999999999,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988560409","OE - Cradle, H1400 x P600 x L400","OE - Frame, H1400 x D600 x W400","OE- ESTRUCTURA, H1400 x D600 x W400","ZENERGY - KERET, H1400 X D600 X W400"]
["56080","ZENERGY - RAMA, H1400 X D600 X W800",1268.3,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988560805","OE - Cradle, H1400 x P600 x L800","OE - Frame, H1400 x D600 x W800","OE- ESTRUCTURA, H1400 x D600 x W800","ZENERGY - KERET, H1400 X D600 X W800"]
["56086","ZENERGY - RAMA, H1400 X D600 X W850, 650+200",1629.1,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988560867","OE - Cradle, H1400 x P600 x L850, 650 + 200","OE - Frame, H1400 x D600 x W850, 650 + 200","OE- ESTRUCTURA, H1400 x D600 x W850, 650+200","ZENERGY – KERET, H1400 X D600 X W850, 650+200"]
["56105","ZENERGY - RAMA, H1400 X D600 X W1050, 650+400",1775.4,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988561055","OE - Cadre, H1400 x P600 x L1050, 650 + 400","OE - Frame, H1400 x D600 x W1050, 650 + 400","OE- ESTRUCTURA, H1400 x D600 x W1050, 650+400","ZENERGY – KERET, H1400 X D600 X W1050, 650+400"]
["56121","ZENERGY - RAMA, H1400 X D600 X W1200, 150+650+400",2198.9,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988561215","OE - Cadre, H1400 x P600 x L1200, 150 + 650 + 400","OE - Frame, H1400 x D600 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1400 x D600 x W1200, 150+650+400","ZENERGY – KERET, H1400 X D600 X W1200, 150+650+400"]
["56131","ZENERGY - RAMA, H1400 X D600 X W1300, 650+650",1903,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988561314","OE - Cadre, H1400 x P600 x L1300, 650 + 650","OE - Frame, H1400 x D600 x W1300, 650 + 650","OE- ESTRUCTURA, H1400 x D600 x W1300, 650+650","ZENERGY – KERET, H1400 X D600 X W1300, 650+650"]
["58030","ZENERGY - RAMA, H1400 X D800 X W300",1154.7,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988580308","OE - Cradle, H1400 x P800 x L300","OE - Frame, H1400 x D800 x W300","OE- ESTRUCTURA, H1400 x D800 x W300","ZENERGY - KERET, H1400 X D800 X W300"]
["58040","ZENERGY - RAMA, H1400 X D800 X W400",1199.5,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988580407","OE - Cradle, H1400 x P800 x L400","OE - Frame, H1400 x D800 x W400","OE- ESTRUCTURA, H1400 x D800 x W400","ZENERGY - KERET, H1400 X D800 X W400"]
["58065","ZENERGY - RAMA, H1400 X D800 X W650",1309.3,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988580650","OE - Cradle, H1400 x P800 x L650","OE - Frame, H1400 x D800 x W650","OE- ESTRUCTURA, H1400 x D800 x W650","ZENERGY - KERET, H1400 X D800 X W650"]
["58100","ZENERGY - RAMA, H1400 X D800 X W1000",1462.7,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988581008","OE - Cradle, H1400 x P800 x L1000","OE - Frame, H1400 x D800 x W1000","OE- ESTRUCTURA, H1400 x D800 x W1000","ZENERGY - KERET, H1400 X D800 X W1000"]
["58110","ZENERGY - RAMA, H1400 X D800 X W1100, 150+650+300",2363.1999999999998,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988581107","OE - Cadre, H1400 x P800 x L1100, 150 + 650 + 300","OE - Frame, H1400 x D800 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1400 x D800 x W1100, 150+650+300","ZENERGY – KERET, H1400 X D800 X W1100, 150+650+300"]
["58121","ZENERGY - RAMA, H1400 X D800 X W1200, 150+650+400",2404.6,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988581213","OE - Cadre, H1400 x P800 x L1200, 150 + 650 + 400","OE - Frame, H1400 x D800 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1400 x D800 x W1200, 150+650+400","ZENERGY – KERET, H1400 X D800 X W1200, 150+650+400"]
["58150","ZENERGY - RAMA, H1400 X D800 X W1500, 650+850",2116.8000000000002,"1-ZE-01",null,null,"OE_FRAME_1400",null,"SZT","85389099",null,null,"5901988581503","OE - Cadre, H1400 x P800 x L1500, 650 + 850","OE - Frame, H1400 x D800 x W1500, 650 + 850","OE- ESTRUCTURA, H1400 x D800 x W1500, 650+850","ZENERGY – KERET, H1400 X D800 X W1500, 650+850"]
["59224","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP30, H1400 X D230",289.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988592240","OE - Ventilateurs latéraux ventilés fixes IP30, H1400 x P230","OE - Ventilated, fixed side covers IP30, H1400 x D230","OE- PAREDES LATERALES VENTIL. FIJO IP30, H1400 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP30, H1400 X D230"]
["59225","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1400 X D230",289.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988592257","OE - Évents d'aération, ventilés, plats, vissés IP30, H1400 x P230","OE - Side panels ventilated, flat, screwed on, IP30, H1400 x D230","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1400 x D230 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1400 X D230"]
["59232","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1400 X D300",310,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988592325","OE - Écrans latéraux ventilés, plats et vissés IP30, H1400 x P300","OE - Side panels ventilated, flat, screwed on, IP30, H1400 x D300","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1400 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1400 X D300"]
["59242","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1400 X D400",331.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988592424","OE - Évents latéraux, ventilés, plats et vissés IP30, H1400 x P400","OE - Side panels ventilated, flat, screwed on, IP30, H1400 x D400","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1400 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1400 X D400"]
["59280","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1400 X D800",695.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988592806","OE - Hottes de ventilation latérales IP30, H1400 x P800","OE - IP30, H1400 x D800 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1400 x D800 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1400 X D800"]
["59323","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H1400 X D230",527,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988593230","OE - Couvercles latéraux complets IP30, H1400 x P230","OE - Plain side covers IP30, H1400 x D230","OE- PAREDES LATERALES LISO IP30, H1400 x D230 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H1400 X D230"]
["59327","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1400 X D230",119.8,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988593278","OE - Panneau de séparation, vertical, galvanisé, H1400 x P230","OE - Vertical partition, Galvanized, H1400 x D230","OE- Tabique VERT., galvanizado, H1400 x D230","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1400 X D230"]
["59335","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1400 X D300",131,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988593353","OE - Panneau de séparation, vertical, galvanisé, H1400 x P300","OE - Vertical partition, Galvanized, H1400 x D300","OE- Tabique VERT., galvanizado, H1400 x D300","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1400 X D300"]
["59342","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H1400 X D400",262.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988593421","OE - Capots latéraux solides, plats, vissés IP30, H1400 x P400","OE - Side panels Plain, flat, screwed on, IP30, H1400 x D400","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H1400 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H1400 X D400"]
["59345","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1400 X D400",142.19999999999999,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988593452","OE - Panneau de séparation, vertical, galvanisé, H1400 x P400","OE - Vertical partition, Galvanized, H1400 x D400","OE- Tabique VERT., galvanizado, H1400 x D400","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1400 X D400"]
["59361","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1400 X D600",306.7,"1-ZE-01",0.16666666666666666,5,"OE_COVERS",null,"SZT","85389099",null,null,"5901988593612","OE - Couvercles latéraux complets, fixes IP30, H1400 x P600","OE - Plain, fixed side covers IP30, H1400 x D600","OE- PAREDES LATERALES LISO FIJO IP30, H1400 x D600 (2UDS)","ZENERGY – OLDALBURKOLATOK, TELJES, RÖGZÍTETT, IP30, H1400 X D600"]
["59380","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H1400 X D800",672.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988593803","OE - Couvercles latéraux complets IP30, H1400 x P800","OE - Plain side covers IP30, H1400 x D800","OE- PAREDES LATERALES LISO IP30, H1400 x D800 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H1400 X D800"]
["59423","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1400 X D230",523.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988594237","OE - Hottes de ventilation latérales IP43, H1400 x P230","OE - IP43, H1400 x D230 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1400 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H1400 X D230"]
["59430","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1400 X D300",682.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988594305","OE - Hottes de ventilation latérales IP43, H1400 x P300","OE - IP43, H1400 x D300 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1400 x D300 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H1400 X D300"]
["59440","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1400 X D400",706.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988594404","OE - Hottes de ventilation latérales IP43, H1400 x P400","OE - IP43, H1400 x D400 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1400 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H1400 X D400"]
["59461","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1400 X D600",436.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988594619","OE - Ventilateurs latéraux ventilés fixes IP43, H1400 x P600","OE - Ventilated, fixed side covers IP43, H1400 x D600","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1400 x D600 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H1400 X D600"]
["59482","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP43, H1400 X D800",464.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988594824","OE - Couvercles latéraux ventilés, plats, à visser IP43, H1400 x P800","OE - Side panels ventilated, flat, screwed on, IP43, H1400 x D800","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP43, H1400 x D800 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP43, H1400 X D800"]
["59523","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1400 X D230",591.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988595234","OE - Couvercles latéraux complets IP55, H1400 x P230","OE - Plain side covers IP55, H1400 x D230","OE- PAREDES LATERALES LISO IP55, H1400 x D230 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1400 X D230"]
["59560","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1400 X D600",689,"1-ZE-01",0.01,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988595609","OE - Capots latéraux complets IP55, H1400 x P600","OE - Plain side covers IP55, H1400 x D600","OE- PAREDES LATERALES LISO IP55, H1400 x D600 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1400 X D600"]
["60111","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1600 W1000 DO PLOMBOWANIA",474.1,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988601119","OE - Cadres H1600 L1000 Cadre articulé avant pour sceller","OE - Frame of Front covers on hinges H1600 W1000 for sealing","OE- MARCO PIVOTANTE H1600 W1000 ","ZENERGY - csuklós ELSŐ BURKOLAT H1600 W1000 TÖMÍTÉSHEZ"]
["60146","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1600 W450 DO PLOMBOWANIA",332.2,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988601461","OE - H1600 L450 cadre de panneau avant articulé pour sceller","OE - Frame of Front covers on hinges H1600 W450 for sealing","OE- MARCO PIVOTANTE H1600 W450 ","ZENERGY - ZSÁNLÓS ELSŐ FEDŐKERET H1600 W450 TÖMÍTÉSHEZ"]
["60170","ZENERGY IT - DWA WSPORNIKI PIONOWE MODUŁU \"U\" 19-CALI NA WKRĘTY SAMOFORMUJĄCE, SZAFY H1600 W650",401.8,"1-ZE-01",null,null,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988601706","IT - Deux supports verticaux pour le module en forme de U \"19\" pour vis autoformeuses, armoires H1600 L650","IT - Two 19-inch U  Vertical supports for self-forming screws, H1600 W650 cabinets ","OE IT- DOS SOPORT. VERT. MOD. \"U\" 19\" ARMARIO H1600 W650","ZENERGY IT - KÉT FÜGGŐLEGES TARTÁS A 19 hüvelykes \"U\" MODULHOZ ÖNFORMÁLÓ CSAVARKKAL, H1600 W650 SZEKRÉNYEK"]
["60210","ZENERGY - DRZWI WENTYLOWANE IP30, H1600 X W1000",1423.4,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988602109","OE - Portes ventilées IP30, H1600 x L1000","OE - Ventilated door IP30, H1600 x W1000","OE- PUERTA VENTIL. IP30, H1600 x W1000","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1600 X W1000"]
["60214","ZENERGY - DRZWI WENTYLOWANE IP30, H1600 X W1050",1494.7,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988602147","OE - Portes ventilées IP30, H1600 x L1050","OE - Ventilated door IP30, H1600 x W1050","OE- PUERTA VENTIL. IP30, H1600 x W1050","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1600 X W1050"]
["60245","ZENERGY - DRZWI WENTYLOWANE IP30, H1600 X W450",983.9,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988602451","OE - Portes ventilées IP30, H1600 x L450","OE - Ventilated door IP30, H1600 x W450","OE- PUERTA VENTIL. IP30, H1600 x W450","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1600 X W450"]
["60260","ZENERGY - DRZWI WENTYLOWANE IP30, H1600 X W600",1104.8,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988602604","OE - Portes ventilées IP30, H1600 x L600","OE - Ventilated door IP30, H1600 x W600","OE- PUERTA VENTIL. IP30, H1600 x W600","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1600 X W600"]
["60285","ZENERGY - DRZWI WENTYLOWANE IP30, H1600 X W850",1301.4000000000001,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988602857","OE - Portes ventilées IP30, H1600 x L850","OE - Ventilated door IP30, H1600 x W850","OE- PUERTA VENTIL. IP30, H1600 x W850","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1600 X W850"]
["60311","ZENERGY - DRZWI PEŁNE IP30, H1600 X W1000, PODWÓJNE",1792.8,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,null,null,null,null,"ZENERGY - TÖMÖR AJTÓ IP30, H1600 X W1000, DUPLÉS"]
["60330","ZENERGY - DRZWI PEŁNE IP30, H1600 X W300",810,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988603304","OE - Portes pleine IP30, H1600 x L300","OE - Plain door IP30, H1600 x W300","OE- PUERTA OPACA IP30, H1600 x W300","ZENERGY - TÖMÖR AJTÓ IP30, H1600 X W300"]
["60360","ZENERGY - DRZWI PEŁNE IP30, H1600 X W600",1032.5,"1-ZE-01",5.8333333333333334E-2,1,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988603601","OE - Portes pleine IP30, H1600 x L600","OE - Plain door IP30, H1600 x W600","OE- PUERTA OPACA IP30, H1600 x W600","ZENERGY - TÖMÖR AJTÓ IP30, H1600 X W600"]
["60373","ZENERGY - SŁUPEK INOX, H1600, RAMA ZEWNĘTRZNA",127.4,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988603731","OE - Poteau INOX, H1600, cadre externe","OE - INOX post, H1600, external frame","OE- PERFIL INOX, H1600, PARA MARCO LATERAL EXTERIOR","ZENERGY - INOX POST, H1600, KÜLSŐ KERET"]
["60385","ZENERGY - DRZWI PEŁNE IP30, H1600 X W850",1232.3,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099","27.12.40.0",null,"5901988603854","OE - Portes pleine IP30, H1600 x L850","OE - Plain door IP30, H1600 x W850","OE- PUERTA OPACA IP30, H1600 x W850","ZENERGY - TELJES AJTÓ IP30, H1600 X W850"]
["60412","ZENERGY - DRZWI WENTYLOWANE IP43, H1600 X W1200, PODWÓJNE",2437.6,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988604127","OE - Portes ventilées doubles IP16, H1600 x L1200","OE - Ventilated door IP43, H1600 x W1200, double","OE- PUERTA VENTIL. IP43, H1600 x W1200, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1600 X W1200, DUPLÉS"]
["60413","ZENERGY - DRZWI WENTYLOWANE IP43, H1600 X W1300, PODWÓJNE",2448.4,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988604134","OE - Portes ventilées IP43, H1600 x L1300, double","OE - Ventilated door IP43, H1600 x W1300, double","OE- PUERTA VENTIL. IP43, H1600 x W1300, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1600 X W1300, DUPLÉS"]
["60440","ZENERGY - DRZWI WENTYLOWANE IP43, H1600 X W400",1006.6,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988604400","OE - Portes ventilées IP43, H1600 x L400","OE - Ventilated door IP43, H1600 x W400","OE- PUERTA VENTIL. IP43, H1600 x W400","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1600 X W400"]
["60465","ZENERGY - DRZWI WENTYLOWANE IP43, H1600 X W650",1219.3,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988604653","OE - Portes ventilées IP43, H1600 x L650","OE - Ventilated door IP43, H1600 x W650","OE- PUERTA VENTIL. IP43, H1600 x W650","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1600 X W650"]
["60512","ZENERGY - DRZWI PEŁNE IP55, H1600 X W1200, PODWÓJNE",2111.4,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988605124","OE - Portes pleine IP55, H1600 x L1200, double","OE - Plain door IP55, H1600 x W1200, double","OE- PUERTA OPACA IP55, H1600 x W1200, DOBLE","ZENERGY - TELJES AJTÓ IP55, H1600 X W1200, DUPLÉS"]
["60514","ZENERGY - DRZWI PEŁNE IP55, H1600 X W1050",1539,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988605148","OE - Portes pleine IP55, H1600 x L1050","OE - Plain door IP55, H1600 x W1050","OE- PUERTA OPACA IP55, H1600 x W1050","ZENERGY - TÖMÖR AJTÓ IP55, H1600 X W1050"]
["60560","ZENERGY - DRZWI PEŁNE IP55, H1600 X W600",1135.0999999999999,"1-ZE-01",3.3333333333333333E-2,1,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988605605","OE - Portes pleine IP55, H1600 x L600","OE - Plain door IP55, H1600 x W600","OE- PUERTA OPACA IP55, H1600 x W600","ZENERGY - TÖMÖR AJTÓ IP55, H1600 X W600"]
["60585","ZENERGY - DRZWI PEŁNE IP55, H1600 X W850",1339.2,"1-ZE-01",0.01,1,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988605858","OE - Portes pleine IP55, H1600 x L850","OE - Plain door IP55, H1600 x W850","OE- PUERTA OPACA IP55, H1600 x W850","ZENERGY - TÖMÖR AJTÓ IP55, H1600 X W850"]
["60612","ZENERGY - DRZWI PRZESZKLONE IP55, H1600 X W1200, PODWÓJNE",2762.6,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988606121","OE - Portes vitrée IP55, H1600 x L1200, double","OE - Glazed door IP55, H1600 x W1200, double","OE- PUERTA TRANSPARENTE IP55, H1600 x W1200, DOBLE","ZENERGY - ÜVEGAJTÓK IP55, H1600 X W1200, DUPLA"]
["60613","ZENERGY - DRZWI PRZESZKLONE IP55, H1600 X W1300, PODWÓJNE",2798.3,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988606138","OE - Portes vitrée IP55, H1600 x L1300, double","OE - Glazed door IP55, H1600 x W1300, double","OE- PUERTA TRANSPARENTE IP55, H1600 x W1300, DOBLE","ZENERGY - ÜVEGAJTÓK IP55, H1600 X W1300, DUPLA"]
["60660","ZENERGY - DRZWI PRZESZKLONE IP55, H1600 X W600",1351.1,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988606602","OE - Portes vitrée IP55, H1600 x L600","OE - Glazed door IP55, H1600 x W600","OE- PUERTA TRANSPARENTE IP55, H1600 x W600","ZENERGY - ÜVEZETETT AJTÓK IP55, H1600 X W600"]
["60695","ZENERGY - DRZWI PRZESZKLONE IP55, H1600 X W950",1728,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988606954","OE - Portes vitrée IP55, H1600 x L950","OE - Glazed door IP55, H1600 x W950","OE- PUERTA TRANSPARENTE IP55, H1600 x W950","ZENERGY - ÜVEGAJTÓK IP55, H1600 X W950"]
["60745","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 3X EFEN 160-630, H1600 X W450, 19+9M, ANALIZATORY 3X 96X96MM",598.4,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988607456","OE - Cadre pivotant composé de 3 interrupteurs-sectionneurs EFEN 160-630 à lamelles, H1600 x L450, 19 + 9M, 3 analyseurs, 96x96 mm","OE - Hinged frame for 3x EFEN 160-630, H1600 x W450, 19 + 9M slat switch disconnectors, analyzers 3x 96x96mm","OE- ESTRUCTURA PARA REGLETAS SECC. 3X160-630, H1600 x W450, 19+9M, ANA","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 3X EFEN 160-630, H1600 X W450, 19+9M, ELEMZŐK 3X 96X96MM"]
["60766","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 5X EFEN 160-630, H1600 X W650, 19+9M, ANALIZATORY 5X 96X96MM DO PLOMBOWANIA",694.1,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988607661","OE - Cadre pivotant d'interrupteurs-sectionneurs 5x EFEN 160-630, H1600 x L650, 19 + 9M, analyseurs 5x de 96x96mm pour l'étanchéité","OE - Hinged frame for 5x EFEN 160-630, H1600 x W650, 19 + 9M slat switch disconnectors, analyzers 5x 96x96mm for sealing","OE- ESTRUCTURA PARA REGLETAS SECC.  5X160-630, H1600 x W650, 19+9M, AN","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 5X EFEN 160-630, H1600 X W650, 19+9M, ELEMZŐK 5X 96X96MM TÖMÍTÉSHEZ"]
["60846","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 3X EFEN 160-630, H1600 X W450, 22+6M DO PLOMBOWANIA",502.7,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988608460","OE - Cadre pivotant composé de 3 sectionneurs EFEN 160-630 à interrupteur à lattes, H1600 x L450, 22 + 6M pour l'étanchéité","OE - Hinged frame for 3x EFEN 160-630, H1600 x W450, 22 + 6M slat switch disconnectors for sealing","OE- ESTRUCTURA PARA REGLETAS SECC. 3X160-630, H1600 x W450, 22+6M ","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 3X EFEN 160-630, H1600 X W450, 22+6M TÖMÍTÉSRE"]
["60885","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 7X EFEN 160-630, H1600 X W850, 22+6M",651.20000000000005,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988608859","OE - Cadre pivotant d'interrupteurs-sectionneurs 7x EFEN 160-630, H1600 x L850, 22 + 6M","OE - Hinged frame for switch disconnectors 7x EFEN 160-630, H1600 x W850, 22 + 6M","OE- ESTRUCTURA PARA REGLETAS SECC. 7X160-630, H1600 x W850, 22+6M","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 7X EFEN 160-630, H1600 X W850, 22+6M"]
["60912","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1600 X W1200 + WSPORNIKI,  ( 1450 X 1100 )",1067,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988609122","OE - Plaque de montage complète H1600 x L1200 + supports, (1450 x 1100)","OE - Plain Mounting plate H1600 x W1200 + brackets, (1450 x 1100)","OE- PLACA MONTAJE  TOTAL CIEGA H1600 x W1200 + SOPORT. (1450 X 1100)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1600 X W1200 + KONZEREK, (1450 X 1100)"]
["60913","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1600 X W1300 + WSPORNIKI,  ( 1450 X 1200 )",1147,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988609139","OE - Plaque de montage complète H1600 x L1300 + supports, (1450 x 1200)","OE - Plain Mounting plate H1600 x W1300 + brackets, (1450 x 1200)","OE- PLACA MONTAJE  TOTAL CIEGA H1600 x W1300 + SOPORT. (1450 X 1200)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H1600 X W1300 + KONZEREK, (1450 X 1200)"]
["60945","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1600 X W450 + WSPORNIKI,  ( 1450 X 350 )",467.6,"1-ZE-01",null,null,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988609450","OE - Plaque de montage complète H1600 x L450 + supports, (1450 x 350)","OE - Plain Mounting plate H1600 x W450 + brackets, (1450 x 350)","OE- PLACA MONTAJE  TOTAL CIEGA H1600 x W450 + SOPORT. (1450 X 350)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H1600 X W450 + KONZEREK, (1450 X 350)"]
["60985","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1600 X W850 + WSPORNIKI,  ( 1450 X 750 )",791.6,"1-ZE-01",0.01,1,"OE_PLAIN_PLATES",null,"SZT","85389099",null,null,"5901988609856","OE - Plaque de montage complète H1600 x L850 + supports, (1450 x 750)","OE - Plain Mounting plate H1600 x W850 + brackets, (1450 x 750)","OE- PLACA MONTAJE  TOTAL CIEGA H1600 x W850 + SOPORT. (1450 X 750)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1600 X W850 + KONZEREK, (1450 X 750)"]
["61112","ZENERGY - DRZWI PRZESZKLONE IP30, H1600 X W1200, PODWÓJNE",2486.1999999999998,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988611125","OE - Portes vitrées IP30, H1600 x L1200, double vitrage","OE - Glazed door IP30, H1600 x W1200, double","OE- PUERTA TRANSP. IP30, H1600 x W1200, doble","ZENERGY - ÜVEGAJTÓK IP30, H1600 X W1200, DUPLA"]
["61145","ZENERGY - DRZWI PRZESZKLONE IP30, H1600 X W450",1024.9000000000001,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988611453","OE - Portes vitrées IP30, H1600 x L450","OE - Glazed door IP30, H1600 x W450","OE- PUERTA TRANSP. IP30, H1600 x W450","ZENERGY - ÜVEZETETT AJTÓK IP30, H1600 X W450"]
["61185","ZENERGY - DRZWI PRZESZKLONE IP30, H1600 X W850",1475.3,"1-ZE-01",null,null,"OE_DOORS_1600",null,"SZT","85389099",null,null,"5901988611859","OE - Portes vitrées IP30, H1600 x L850","OE - Glazed door IP30, H1600 x W850","OE- PUERTA TRANSP. IP30, H1600 x W850","ZENERGY - ÜVEGAJTÓK IP30, H1600 X W850"]
["61212","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1600 X W1200",1047.5999999999999,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988612122","OE - Couverture arrière complète IP30, H1600 x L1200","OE - Plain rear cover IP30, H1600 x W1200","OE- FONDO ATORNILLADO LISO IP30, H1600 x W1200","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1600 X W1200"]
["61245","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1600 X W450",421.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988612450","OE - Couverture arrière complète IP30, H1600 x L450","OE - Plain rear cover IP30, H1600 x W450","OE- FONDO ATORNILLADO LISO IP30, H1600 x W450","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1600 X W450"]
["61260","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1600 X W600",518.4,"1-ZE-01",5.8333333333333334E-2,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988612603","OE - Couverture arrière complète IP30, H1600 x L600","OE - Plain rear cover IP30, H1600 x W600","OE- FONDO ATORNILLADO LISO IP30, H1600 x W600","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1600 X W600"]
["61285","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1600 X W850",642.6,"1-ZE-01",0.01,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988612856","OE - Couverture arrière complète IP30, H1600 x L850","OE - Plain rear cover IP30, H1600 x W850","OE- FONDO ATORNILLADO LISO IP30, H1600 x W850","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1600 X W850"]
["61312","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1600 X W1200",1142.5999999999999,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988613129","OE - Hotte d'aération arrière IP30, H1600 x L1200","OE - Rear ventilated cover IP30, H1600 x W1200","OE- FONDO ATORNILLADO VENTIL. IP30, H1600 x W1200","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1600 X W1200"]
["61340","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1600 X W400",473,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988613402","OE - Hotte d'aération arrière IP30, H1600 x L400","OE - Rear ventilated cover IP30, H1600 x W400","OE- FONDO ATORNILLADO VENTIL. IP30, H1600 x W400","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1600 X W400"]
["61365","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1600 X W650",618.79999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988613655","OE - Hotte d'aération arrière IP30, H1600 x L650","OE - Rear ventilated cover IP30, H1600 x W650","OE- FONDO ATORNILLADO VENTIL. IP30, H1600 x W650","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1600 X W650"]
["61410","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1600 X W1000",852.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988614102","OE - Couvercle ventilé IP43, H1600 x L1000","OE - Rear ventilated cover IP43, H1600 x W1000","OE- FONDO ATORNILLADO VENTIL.IP43, H1600 x W1000","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1600 X W1000"]
["61413","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1600 X W1300",1347.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988614133","OE - Coque arrière ventilée IP43, H1600 x L1300","OE - Rear ventilated cover IP43, H1600 x W1300","OE- FONDO ATORNILLADO VENTIL.IP43, H1600 x W1300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1600 X W1300"]
["61430","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1600 X W300",421.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988614300","OE - Coque arrière ventilée IP43, H1600 x L300","OE - Rear ventilated cover IP43, H1600 x W300","OE- FONDO ATORNILLADO VENTIL.IP43, H1600 x W300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1600 X W300"]
["61460","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1600 X W600",661,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988614607","OE - Coque arrière ventilée IP43, H1600 x L600","OE - Rear ventilated cover IP43, H1600 x W600","OE- FONDO ATORNILLADO VENTIL.IP43, H1600 x W600","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1600 X W600"]
["61485","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1600 X W850",799.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988614850","OE - Coque arrière ventilée IP43, H1600 x L850","OE - Rear ventilated cover IP43, H1600 x W850","OE- FONDO ATORNILLADO VENTIL.IP43, H1600 x W850","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1600 X W850"]
["61512","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1600 X W1200",899.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988615123","OE - Couverture arrière complète IP55, H1600 x L1200","OE - Plain rear cover IP55, H1600 x W1200","OE- FONDO ATORNILLADO LISO IP55, H1600 x W1200","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1600 X W1200"]
["61540","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1600 X W400",473,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988615406","OE - Couverture arrière complète IP55, H1600 x L400","OE - Plain rear cover IP55, H1600 x W400","OE- FONDO ATORNILLADO LISO IP55, H1600 x W400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1600 X W400"]
["61565","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1600 X W650",626.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988615659","OE - Couverture arrière complète IP55, H1600 x L650","OE - Plain rear cover IP55, H1600 x W650","OE- FONDO ATORNILLADO LISO IP55, H1600 x W650","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1600 X W650"]
["62030","ZENERGY - RAMA, H1600 X D230 X W300",675.4,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988620301","OE - Cradle, H1600 x P230 x L300","OE - Frame, H1600 x D230 x W300","OE- ESTRUCTURA, H1600 x D230 x W300","ZENERGY - KERET, H1600 X D230 X W300"]
["62060","ZENERGY - RAMA, H1600 X D230 X W600",805.2,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988620608","OE - Cradle, H1600 x P230 x L600","OE - Frame, H1600 x D230 x W600","OE- ESTRUCTURA, H1600 x D230 x W600","ZENERGY - KERET, H1600 X D230 X W600"]
["62065","ZENERGY - RAMA, H1600 X D230 X W650",826.1,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988620653","OE - Cradle, H1600 x P230 x L650","OE - Frame, H1600 x D230 x W650","OE- ESTRUCTURA, H1600 x D230 x W650","ZENERGY - KERET, H1600 X D230 X W650"]
["62085","ZENERGY - RAMA, H1600 X D230 X W850",913,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988620851","OE - Cradle, H1600 x P230 x L850","OE - Frame, H1600 x D230 x W850","OE- ESTRUCTURA, H1600 x D230 x W850","ZENERGY - KERET, H1600 X D230 X W850"]
["62100","ZENERGY - RAMA, H1600 X D230 X W1000",977.9,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988621001","OE - Cradle, H1600 x P230 x L1000","OE - Frame, H1600 x D230 x W1000","OE- ESTRUCTURA, H1600 x D230 x W1000","ZENERGY - KERET, H1600 X D230 X W1000"]
["62120","ZENERGY - RAMA, H1600 X D230 X W1200",1063.7,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988621209","OE - Cradle, H1600 x P230 x L1200","OE - Frame, H1600 x D230 x W1200","OE- ESTRUCTURA, H1600 x D230 x W1200","ZENERGY - KERET, H1600 X D230 X W1200"]
["62150","ZENERGY - RAMA, H1600 X D230 X W1500, 650+850",1401.4,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988621506","OE - Cradle, H1600 x P230 x L1500, 650 + 850","OE - Frame, H1600 x D230 x W1500, 650 + 850","OE- ESTRUCTURA, H1600 x D230 x W1500, 650+850","ZENERGY – KERET, H1600 X D230 X W1500, 650+850"]
["62209","ZENERGY ON - ROZDZIELNICA NATYNKOWA H550 X W600 3X24MOD IP30, 9H MOD, BEZ DRZWI",555.4,"1-ZE-03",0.6,7,"ON_ENCLOSURES","62209","SZT","85381000","27.12.40.0",null,"5901988622091","ON - Appareillage en saillie 3x24MOD IP30, MOD 9H, Portes pleine H550 x L600","ON - H550 x W600 3x24MOD IP30, 9H MOD surface-mounted distribution board, without door","*ON - Cuadro de distribución de superficie H550 x W600 3x24MOD IP30, 9H MOD, sin puertas","ZENERGY ON - FELÜLETRE SZERELT KAPCSOLÓTÁBLA H550 X W600 3X24MOD IP30, 9H MOD, AJTÓ NÉLKÜL"]
["62218","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1000 X W600 6X24MOD IP30, 18H MOD, BEZ DZWI",842.7,"1-ZE-03",0.55000000000000004,10,"ON_ENCLOSURES","62218","SZT","85381000","27.12.40.0",null,"5901988622183","ON - Appareillage pour montage en saillie 6x24MOD IP30, MOD 18H, Portes pleine H1000 x L600","ON - H1000 x W600 6x24MOD IP30, 18H MOD, surface mounted distribution box, without door","*ON - Cuadro de distribución de superficie H1000 x W600 6x24MOD IP30, 18H MOD, sin puerta","ZENERGY ON - FELÜLETRE SZERELŐ KAPCSOLÓTÁBLA H1000 X W600 6X24MOD IP30, 18H MOD, AJTÓ NÉLKÜL"]
["62227","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1450 X W600 9X24MOD IP30, 27H MOD, BEZ DRZWI",1217.9000000000001,"1-ZE-03",0.01,1,"ON_ENCLOSURES","62227","SZT","85381000","27.12.40.0",null,"5901988622275","ON - tableau de distribution monté en saillie 9x24MOD IP30, MOD 27H, Portes pleine H1450 x L600","ON - H1450 x W600 9x24MOD IP30, 27H MOD surface-mounted distribution board, without door","*ON - Cuadro de distribución de superficie H1450 x W600 9x24MOD IP30, 27H MOD, sin puertas","ZENERGY ON - FELÜLETRE SZERELT KAPCSOLÓTÁBLA H1450 X W600 9X24MOD IP30, 27H MOD, AJTÓ NÉLKÜL"]
["62230","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1600 X W600 10X24MOD IP30, 30H MOD, BEZ DRZWI",1426.8,"1-ZE-03",null,null,"ON_ENCLOSURES","62230","SZT","85381000","27.12.40.0",null,"5901988622305","ON - 10x24MOD IP30, Appareillage à montage en surface 30H MOD, Portes pleine H1600 x L600","ON - H1600 x W600 10x24MOD IP30, 30H MOD surface-mounted distribution board, without door","*ON - Cuadro de distribución de superficie H1600 x W600 10x24MOD IP30, 30H MOD, sin puertas","ZENERGY ON - FELÜLETRE SZERELT KAPCSOLÓTÁBLA H1600 X W600 10X24MOD IP30, 30H MOD, AJTÓ NÉLKÜL"]
["62309","ZENERGY ON - ROZDZIELNICA NATYNKOWA H550 X W800 x D205 3X35MOD IP30, 9H MOD, BEZ DRZWI",706,"1-ZE-03",null,null,"ON_ENCLOSURES","62309","SZT","85381000",null,null,"5901988623098","ON - Appareillage en saillie 3x35MOD IP30, MOD 9H, Portes pleine H550 x L800","ON - H550 x W800 x D205 surface-mounted distribution board 3x35MOD IP30, 9H MOD, without door","*ON- Cuadro de distribución de superficie H550 x W800 x D205 3x35MOD IP30, 9H MOD, sin puerta","ZENERGY ON - FELÜLETRE SZERELŐ KAPCSOLÓTÁBLA H550 X W800 x D205 3X35MOD IP30, 9H MOD, AJTÓ NÉLKÜL"]
["62318","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1000 X W800 x D205 6X35MOD IP30, 18H MOD, BEZ DZWI",1101.3,"1-ZE-03",1.6666666666666666E-2,2,"ON_ENCLOSURES","62318","SZT","85381000",null,null,"5901988623180","ON - Appareillage pour montage en saillie 6x35MOD IP30, MOD 18H, Portes pleine H1000 x L800","ON - Surface mounted distribution box H1000 x W800 x D205 6x35MOD IP30, 18H MOD, without door","*ON- Caja de distribución de superficie H1000 x W800 x D205 6x35MOD IP30, 18H MOD, sin puerta","ZENERGY ON - FELÜLETRE SZERELT KAPCSOLÓTÁBLA H1000 X W800 x D205 6X35MOD IP30, 18H MOD, AJTÓ NÉLKÜL"]
["62330","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1600 X W800 x D205 10X35MOD IP30, 30H MOD, BEZ DRZWI",1864.5,"1-ZE-03",0.05,4,"ON_ENCLOSURES","62330","SZT","85381000",null,null,"5901988623302","ON - 10x35MOD IP30, Appareillage à montage en surface 30H MOD, Portes pleine H1600 x L800","ON - Surface mounted distribution box H1600 x W800 x D205 10x35MOD IP30, 30H MOD, without door","*ON- Caja de distribución de superficie H1600 x W800 x D205 10x35MOD IP30, 30H MOD, sin puerta","ZENERGY ON - FELÜLETRE SZERELŐ KAPCSOLÓTÁBLA H1600 X W800 x D205 10X35MOD IP30, 30H MOD, AJTÓ NÉLKÜL"]
["63045","ZENERGY - RAMA, H1600 X D300 X W450",784.3,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988630454","OE - Cradle, H1600 x P300 x L450","OE - Frame, H1600 x D300 x W450","OE- ESTRUCTURA, H1600 x D300 x W450","ZENERGY - KERET, H1600 X D300 X W450"]
["63081","ZENERGY - RAMA, H1600 X D300 X W800, 650+150",1124.2,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988630812","OE - Cradle, H1600 x P300 x L800, 650 + 150","OE - Frame, H1600 x D300 x W800, 650 + 150","OE- ESTRUCTURA, H1600 x D300 x W800, 650+150","ZENERGY – KERET, H1600 X D300 X W800, 650+150"]
["63095","ZENERGY - RAMA, H1600 X D300 X W950, 650+300",1254,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988630959","OE - Cradle, H1600 x P300 x L950, 650 + 300","OE - Frame, H1600 x D300 x W950, 650 + 300","OE- ESTRUCTURA, H1600 x D300 x W950, 650+300","ZENERGY – KERET, H1600 X D300 X W950, 650+300"]
["63110","ZENERGY - RAMA, H1600 X D300 X W1100, 150+650+300",1511.4,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988631109","OE - Cradle, H1600 x P300 x L1100, 150 + 650 + 300","OE - Frame, H1600 x D300 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1600 x D300 x W1100, 150+650+300","ZENERGY – KERET, H1600 X D300 X W1100, 150+650+300"]
["63115","ZENERGY - RAMA, H1600 X D300 X W1150, 850+300",1335.4,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988631154","OE - Cradle, H1600 x P300 x L1150, 850 + 300","OE - Frame, H1600 x D300 x W1150, 850 + 300","OE- ESTRUCTURA, H1600 x D300 x W1150, 850+300","ZENERGY – KERET, H1600 X D300 X W1150, 850+300"]
["63125","ZENERGY - RAMA, H1600 X D300 X W1250, 850+400",1376.1,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988631253","OE - Cradle, H1600 x P300 x L1250, 850 + 400","OE - Frame, H1600 x D300 x W1250, 850 + 400","OE- ESTRUCTURA, H1600 x D300 x W1250, 850+400","ZENERGY – KERET, H1600 X D300 X W1250, 850+400"]
["63170","ZENERGY - RAMA, H1600 X D300 X W1700, 850+850",1557.6,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988631703","OE - Cradle, H1600 x P300 x L1700, 850 + 850","OE - Frame, H1600 x D300 x W1700, 850 + 850","OE- ESTRUCTURA, H1600 x D300 x W1700, 850+850","ZENERGY – KERET, H1600 X D300 X W1700, 850+850"]
["64045","ZENERGY - RAMA, H1600 X D400 X W450",814.3,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988640453","OE - Cradle, H1600 x P400 x L450","OE - Frame, H1600 x D400 x W450","OE- ESTRUCTURA, H1600 x D400 x W450","ZENERGY - KERET, H1600 X D400 X W450"]
["64080","ZENERGY - RAMA, H1600 X D400 X W800",962.3,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988640804","OE - Cradle, H1600 x P400 x L800","OE - Frame, H1600 x D400 x W800","OE- ESTRUCTURA, H1600 x D400 x W800","ZENERGY - KERET, H1600 X D400 X W800"]
["64095","ZENERGY - RAMA, H1600 X D400 X W950, 650+300",1305.7,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988640958","OE - Cradle, H1600 x P400 x L950, 650 + 300","OE - Frame, H1600 x D400 x W950, 650 + 300","OE- ESTRUCTURA, H1600 x D400 x W950, 650+300","ZENERGY – KERET, H1600 X D400 X W950, 650+300"]
["64110","ZENERGY - RAMA, H1600 X D400 X W1100, 150+650+300",1586.2,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988641108","OE - Cadre, H1600 x P400 x L1100, 150 + 650 + 300","OE - Frame, H1600 x D400 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1600 x D400 x W1100, 150+650+300","ZENERGY – KERET, H1600 X D400 X W1100, 150+650+300"]
["64120","ZENERGY - RAMA, H1600 X D400 X W1200",1152.8,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988641207","OE - Cradle, H1600 x P400 x L1200","OE - Frame, H1600 x D400 x W1200","OE- ESTRUCTURA, H1600 x D400 x W1200","ZENERGY - KERET, H1600 X D400 X W1200"]
["64121","ZENERGY - RAMA, H1600 X D400 X W1200, 150+650+400",1625.8,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988641214","OE - Cadre, H1600 x P400 x L1200, 150 + 650 + 400","OE - Frame, H1600 x D400 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1600 x D400 x W1200, 150+650+400","ZENERGY – KERET, H1600 X D400 X W1200, 150+650+400"]
["64131","ZENERGY - RAMA, H1600 X D400 X W1300, 650+650",1474,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988641313","OE - Cradle, H1600 x P400 x L1300, 650 + 650","OE - Frame, H1600 x D400 x W1300, 650 + 650","OE- ESTRUCTURA, H1600 x D400 x W1300, 650+650","ZENERGY – KERET, H1600 X D400 X W1300, 650+650"]
["65330","ZENERGY - DRZWI PRZEDZIAŁU KABLOWEGO IP30, H1600 X W300",292.60000000000002,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988653309","OE - Portes d'entrée de câble IP30, H1600 x L300","OE - Cable compartment door IP30, H1600 x W300","OE- PUERTA PARA MOD. CABLES IP30, H1600 x W300","ZENERGY - KÁBELREKESZ AJTÓ IP30, H1600 X W300"]
["66040","ZENERGY - RAMA, H1600 X D600 X W400",1153.9000000000001,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988660406","OE - Cradle, H1600 x P600 x L400","OE - Frame, H1600 x D600 x W400","OE- ESTRUCTURA, H1600 x D600 x W400","ZENERGY - KERET, H1600 X D600 X W400"]
["66065","ZENERGY - RAMA, H1600 X D600 X W650",1238.8,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988660659","OE - Cradle, H1600 x P600 x L650","OE - Frame, H1600 x D600 x W650","OE- ESTRUCTURA, H1600 x D600 x W650","ZENERGY - KERET, H1600 X D600 X W650"]
["66086","ZENERGY - RAMA, H1600 X D600 X W850, 650+200",1717.1,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988660864","OE - Cradle, H1600 x P600 x L850, 650 + 200","OE - Frame, H1600 x D600 x W850, 650 + 200","OE- ESTRUCTURA, H1600 x D600 x W850, 650+200","ZENERGY – KERET, H1600 X D600 X W850, 650+200"]
["66105","ZENERGY - RAMA, H1600 X D600 X W1050, 650+400",1864.5,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988661052","OE - Cradle, H1600 x P600 x L1050, 650 + 400","OE - Frame, H1600 x D600 x W1050, 650 + 400","OE- ESTRUCTURA, H1600 x D600 x W1050, 650+400","ZENERGY – KERET, H1600 X D600 X W1050, 650+400"]
["66115","ZENERGY - RAMA, H1600 X D600 X W1150, 850+300",1904.1,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988661151","OE - Cradle, H1600 x P600 x L1150, 850 + 300","OE - Frame, H1600 x D600 x W1150, 850 + 300","OE- ESTRUCTURA, H1600 x D600 x W1150, 850+300","ZENERGY – KERET, H1600 X D600 X W1150, 850+300"]
["66120","ZENERGY - RAMA, H1600 X D600 X W1200",1499.3,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988661205","OE - Cradle, H1600 x P600 x L1200","OE - Frame, H1600 x D600 x W1200","OE- ESTRUCTURA, H1600 x D600 x W1200","ZENERGY - KERET, H1600 X D600 X W1200"]
["66130","ZENERGY - RAMA, H1600 X D600 X W1300",1542.2,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988661304","OE - Cradle, H1600 x P600 x L1300","OE - Frame, H1600 x D600 x W1300","OE- ESTRUCTURA, H1600 x D600 x W1300","ZENERGY - KERET, H1600 X D600 X W1300"]
["68030","ZENERGY - RAMA, H1600 X D800 X W300",1220.8,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988680305","OE - Cradle, H1600 x P800 x L300","OE - Frame, H1600 x D800 x W300","OE- ESTRUCTURA, H1600 x D800 x W300","ZENERGY - KERET, H1600 X D800 X W300"]
["68060","ZENERGY - RAMA, H1600 X D800 X W600",1351.8,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988680602","OE - Cradle, H1600 x P800 x L600","OE - Frame, H1600 x D800 x W600","OE- ESTRUCTURA, H1600 x D800 x W600","ZENERGY - KERET, H1600 X D800 X W600"]
["68081","ZENERGY - RAMA, H1600 X D800 X W800, 650+150",1878.2,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988680817","OE - Cradle, H1600 x P800 x L800, 650 + 150","OE - Frame, H1600 x D800 x W800, 650 + 150","OE- ESTRUCTURA, H1600 x D800 x W800, 650+150","ZENERGY – KERET, H1600 X D800 X W800, 650+150"]
["68100","ZENERGY - RAMA, H1600 X D800 X W1000",1527.7,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988681005","OE - Cradle, H1600 x P800 x L1000","OE - Frame, H1600 x D800 x W1000","OE- ESTRUCTURA, H1600 x D800 x W1000","ZENERGY - KERET, H1600 X D800 X W1000"]
["68115","ZENERGY - RAMA, H1600 X D800 X W1150, 850+300",2072,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988681159","OE - Cradle, H1600 x P800 x L1150, 850 + 300","OE - Frame, H1600 x D800 x W1150, 850 + 300","OE- ESTRUCTURA, H1600 x D800 x W1150, 850+300","ZENERGY – KERET, H1600 X D800 X W1150, 850+300"]
["68120","ZENERGY - RAMA, H1600 X D800 X W1200",1616.2,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988681203","OE - Cradle, H1600 x P800 x L1200","OE - Frame, H1600 x D800 x W1200","OE- ESTRUCTURA, H1600 x D800 x W1200","ZENERGY - KERET, H1600 X D800 X W1200"]
["68130","ZENERGY - RAMA, H1600 X D800 X W1300",1659.8,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988681302","OE - Cradle, H1600 x P800 x L1300","OE - Frame, H1600 x D800 x W1300","OE- ESTRUCTURA, H1600 x D800 x W1300","ZENERGY - KERET, H1600 X D800 X W1300"]
["68170","ZENERGY - RAMA, H1600 X D800 X W1700, 850+850",2298.1999999999998,"1-ZE-01",null,null,"OE_FRAME_1600",null,"SZT","85389099",null,null,"5901988681708","OE - Cadre, H1600 x P800 x L1700, 850 + 850","OE - Frame, H1600 x D800 x W1700, 850 + 850","OE- ESTRUCTURA, H1600 x D800 x W1700, 850+850","ZENERGY – KERET, H1600 X D800 X W1700, 850+850"]
["69230","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1600 X D300",643.70000000000005,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988692308","OE - Hottes de ventilation latérales IP30, H1600 x P300","OE - IP30, H1600 x D300 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1600 x D300 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1600 X D300"]
["69240","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1600 X D400",665.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988692407","OE - Hottes de ventilation latérales IP30, H1600 x P400","OE - IP30, H1600 x D400 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1600 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1600 X D400"]
["69260","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H1600 X D600",690.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988692605","OE - Housses suspendues latérales IP30, H1600 x P600","OE - IP30, H1600 x D600 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H1600 x D600 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H1600 X D600"]
["69262","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1600 X D600",384.5,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988692629","OE - Écrans latéraux ventilés, plats et vissés IP30, H1600 x P600","OE - Side panels ventilated, flat, screwed on, IP30, H1600 x D600","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1600 x D600 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1600 X D600"]
["69325","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H1600 X D230",246.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988693251","OE - Capots latéraux solides, plats, vissés IP30, H1600 x P230","OE - Side panels Plain, flat, screwed on, IP30, H1600 x D230","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H1600 x D230 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H1600 X D230"]
["69327","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1600 X D230",133.30000000000001,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988693275","OE - Panneau de séparation, vertical, galvanisé, H1600 x P230","OE - Vertical partition, Galvanized, H1600 x D230","OE- Tabique VERT., galvanizado, H1600 x D230","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1600 X D230"]
["69332","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H1600 X D300",267.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988693329","OE - Capots latéraux solides, plats, vissés IP30, H1600 x P300","OE - Side panels Plain, flat, screwed on IP30, H1600 x D300","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H1600 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H1600 X D300"]
["69341","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1600 X D400",289.39999999999998,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988693411","OE - Couvercles latéraux complets, fixes IP30, H1600 x P400","OE - Plain, fixed side covers IP30, H1600 x D400","OE- PAREDES LATERALES LISO FIJO IP30, H1600 x D400  (2UDS)","ZENERGY – TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H1600 X D400"]
["69361","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1600 X D600",335.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988693619","OE - Couvercles latéraux complets, fixes IP30, H1600 x P600","OE - Plain, fixed side covers IP30, H1600 x D600","OE- PAREDES LATERALES LISO FIJO IP30, H1600 x D600 (2UDS)","ZENERGY - TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H1600 X D600"]
["69380","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H1600 X D800",702.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988693800","OE - Couvercles latéraux complets IP30, H1600 x P800","OE - Plain side covers IP30, H1600 x D800","OE- PAREDES LATERALES LISO IP30, H1600 x D800 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H1600 X D800"]
["69385","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1600 X D800",227.4,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","69385","SZT","85389099",null,null,"5901988693855","OE - Panneau de séparation, vertical, galvanisé, H1600 x P800","OE - Vertical partition, Galvanized, H1600 x D800","OE- TABIQUE VERTIC. GALV. H1600XD800","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1600 X D800"]
["69430","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1600 X D300",778.7,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988694302","OE - Hottes de ventilation latérales IP43, H1600 x P300","OE - IP43, H1600 x D300 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1600 x D300 (2UDS)","ZENERGY – SZELLŐZTETT OLDALBURKOLATOK IP43, H1600 X D300"]
["69440","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1600 X D400",804.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988694401","OE - Hottes de ventilation latérales IP43, H1600 x P400","OE - IP43, H1600 x D400 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1600 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H1600 X D400"]
["69441","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1600 X D400",469.8,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988694418","OE - Ventilateurs latéraux ventilés fixes IP43, H1600 x P400","OE - Ventilated, fixed side covers IP43, H1600 x D400","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1600 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H1600 X D400"]
["69461","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1600 X D600",511.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988694616","OE - Ventilateurs latéraux ventilés fixes IP43, H1600 x P600","OE - Ventilated, fixed side covers IP43, H1600 x D600","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1600 x D600 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H1600 X D600"]
["69481","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1600 X D800",545.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988694814","OE - Évents latéraux, ventilés, fixes IP43, H1600 x P800","OE - Ventilated, fixed side covers IP43, H1600 x D800","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1600 x D800 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H1600 X D800"]
["69540","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1600 X D400",725.8,"1-ZE-01",1.6666666666666666E-2,2,"OE_COVERS",null,"SZT","85389099",null,null,"5901988695408","OE - Capots latéraux complets IP55, H1600 x P400","OE - Plain side covers IP55, H1600 x D400","OE- PAREDES LATERALES LISO IP55, H1600 x D400  (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1600 X D400"]
["70110","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1800 W1000",461.2,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","70110","SZT","85389099",null,null,"5901988701109","OE - H1800 L1000 cadre cadre à charnière avant","OE - H1800 W1000 hinged Front covers frame","OE- MARCO PIVOTANTE H1800 W1000","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H1800 W1000"]
["70145","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1800 W450",319.7,"1-ZE-01",3.3333333333333333E-2,1,"OE_FRAME_INTERNAL","70145","SZT","85389099","27.12.40.0",null,"5901988701451","OE - H1800 L450 cadre de panneau avant articulé","OE - The frame of the hinged Front covers H1800 W450","OE- MARCO PIVOTANTE H1800 W450","ZENERGY - SZÁNTOS ELSŐ BURKOLAT H1800 W450"]
["70166","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1800 W650 DO PLOMBOWANIA",381.2,"1-ZE-01",4.1666666666666664E-2,1,"OE_FRAME_INTERNAL","70165","SZT","85389099",null,null,"5901988701666","OE - H1800 L650 cadre de panneau avant articulé pour sceller","OE - Frame of Front covers on hinges H1800 W650 for sealing","OE- MARCO PIVOTANTE H1800 W650 ","ZENERGY - csuklós ELSŐ BURKOLAT KERET H1800 W650 TÖMÍTÉSHEZ"]
["70185","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1800 W850",419,"1-ZE-01",8.3333333333333329E-2,4,"OE_FRAME_INTERNAL","70185","SZT","85389099",null,null,"5901988701857","OE - H1800 L850 cadre de panneau avant articulé","OE - H1800 W850 hinged Front covers frame","OE- MARCO PIVOTANTE H1800 W850","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H1800 W850"]
["70186","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H1800 W850 DO PLOMBOWANIA",442.8,"1-ZE-01",6.6666666666666666E-2,2,"OE_FRAME_INTERNAL","70185","SZT","85389099",null,null,"5901988701864","OE - H1800 L850 cadre de panneau avant articulé pour sceller","OE - Frame of Front covers on hinges H1800 W850 for sealing","OE- MARCO PIVOTANTE H1800 W850 ","ZENERGY - csuklós ELSŐ BURKOLAT KERET H1800 W850 TÖMÍTÉSHEZ"]
["70213","ZENERGY - DRZWI WENTYLOWANE IP30, H1800 X W1300, PODWÓJNE",2397.6,"1-ZE-01",null,null,"OE_DOORS_1800",null,"SZT","85389099",null,null,"5901988702137","OE - Portes ventilées double IP30, H1800 x L1300","OE - Ventilated doors IP30, H1800 x W1300, double","OE- PUERTA VENTIL. IP30, H1800 x W1300, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1800 X W1300, DUPLÉS"]
["70240","ZENERGY - DRZWI WENTYLOWANE IP30, H1800 X W400",978.5,"1-ZE-01",null,null,"OE_DOORS_1800","70340","SZT","85389099",null,null,"5901988702403","OE - Portes ventilées IP30, H1800 x L400","OE - Ventilated door IP30, H1800 x W400","OE- PUERTA VENTIL. IP30, H1800 x W400","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1800 X W400"]
["70285","ZENERGY - DRZWI WENTYLOWANE IP30, H1800 X W850",1358.6,"1-ZE-01",null,null,"OE_DOORS_1800","70385","SZT","85389099",null,null,"5901988702854","OE - Portes ventilées IP30, H1800 x L850","OE - Ventilated door IP30, H1800 x W850","OE- PUERTA VENTIL. IP30, H1800 x W850","ZENERGY - SZELLŐZTETT AJTÓK IP30, H1800 X W850"]
["70312","ZENERGY - DRZWI PEŁNE IP30, H1800 X W1200, PODWÓJNE",2238.8000000000002,"1-ZE-01",1.6666666666666666E-2,1,"OE_DOORS_1800","70312","SZT","85389099",null,null,"5901988703127","OE - Portes pleine IP30, H1800 x L1200, double","OE - Plain door IP30, H1800 x W1200, double","OE- PUERTA OPACA IP30, H1800 x W1200, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H1800 X W1200, DUPLA"]
["70340","ZENERGY - DRZWI PEŁNE IP30, H1800 X W400",911.5,"1-ZE-01",3.3333333333333333E-2,1,"OE_DOORS_1800","70340","SZT","85389099","27.12.40.0",null,"5901988703400","OE - Portes pleine IP30, H1800 x L400","OE - Plain door IP30, H1800 x W400","OE- PUERTA OPACA IP30, H1800 x W400","ZENERGY - TÖMÖR AJTÓ IP30, H1800 X W400"]
["70365","ZENERGY - DRZWI PEŁNE IP30, H1800 X W650",1118.9000000000001,"1-ZE-01",0.11666666666666667,4,"OE_DOORS_1800","70365","SZT","85389099","27.12.40.0",null,"5901988703653","OE - Portes pleine IP30, H1800 x L650","OE - Plain door IP30, H1800 x W650","OE- PUERTA OPACA IP30, H1800 x W650","ZENERGY - TELJES AJTÓ IP30, H1800 X W650"]
["70373","ZENERGY - SŁUPEK INOX, H1800, RAMA ZEWNĘTRZNA",142.6,"1-ZE-01",8.3333333333333329E-2,1,"OE_FRAME_1800","70371","SZT","85389099",null,null,"5901988703738","OE - Poteau INOX, H1800, cadre externe","OE - INOX post, H1800, external frame","OE- PERFIL INOX, H1800, PARA MARCO LATERAL EXTERIOR","ZENERGY - INOX POST, H1800, KÜLSŐ KERET"]
["70374","ZENERGY - SŁUPEK INOX, H1800, RAMA WEWNETRZNA",155.1,"1-ZE-01",null,null,"OE_FRAME_1800","70372","SZT","85389099",null,null,"5901988703745","OE - Poteau INOX, H1800, cadre interne","OE - INOX post, H1800, internal frame","OE- PERFIL INOX, H1800, PARA MARCO LATERAL INTERIOR","ZENERGY - INOX POSTA, H1800, BELSŐ KERET"]
["70395","ZENERGY - DRZWI PEŁNE IP30, H1800 X W950",1366.2,"1-ZE-01",null,null,"OE_DOORS_1800","70395","SZT","85389099",null,null,"5901988703950","OE - Portes pleine IP30, H1800 x L950","OE - Plain door IP30, H1800 x W950","OE- PUERTA OPACA IP30, H1800 x W950","ZENERGY - TELJES AJTÓ IP30, H1800 X W950"]
["70414","ZENERGY - DRZWI WENTYLOWANE IP43, H1800 X W1050",1655.6,"1-ZE-01",null,null,"OE_DOORS_1800",null,"SZT","85389099",null,null,"5901988704148","OE - Portes ventilées IP43, H1800 x L1050","OE - Ventilated door IP43, H1800 x W1050","OE- PUERTA VENTIL. IP43, H1800 x W1050","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1800 X W1050"]
["70445","ZENERGY - DRZWI WENTYLOWANE IP43, H1800 X W450",1347.8,"1-ZE-01",null,null,"OE_DOORS_1800","70345","SZT","85389099",null,null,"5901988704452","OE - Portes ventilées IP43, H1800 x L450","OE - Ventilated door IP43, H1800 x W450","OE- PUERTA VENTIL. IP43, H1800 x W450","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1800 X W450"]
["70480","ZENERGY - DRZWI WENTYLOWANE IP43, H1800 X W800",1401.8,"1-ZE-01",null,null,"OE_DOORS_1800","70380","SZT","85389099",null,null,"5901988704803","OE - Portes ventilées IP43, H1800 x L800","OE - Ventilated door IP43, H1800 x W800","OE- PUERTA VENTIL. IP43, H1800 x W800","ZENERGY - SZELLŐZTETT AJTÓK IP43, H1800 X W800"]
["70512","ZENERGY - DRZWI PEŁNE IP55, H1800 X W1200, PODWÓJNE",2492.6,"1-ZE-01",1.6666666666666666E-2,1,"OE_DOORS_1800","70312","SZT","85389099",null,null,"5901988705121","OE - Portes pleine IP55, H1800 x L1200, double","OE - Plain door IP55, H1800 x W1200, double","OE- PUERTA OPACA IP55, H1800 x W1200, DOBLE","ZENERGY - TELJES AJTÓ IP55, H1800 X W1200, DUPLÉS"]
["70530","ZENERGY - DRZWI PEŁNE IP55, H1800 X W300",958,"1-ZE-01",null,null,"OE_DOORS_1800","70330","SZT","85389099",null,null,"5901988705305","OE - Portes pleine IP55, H1800 x L300","OE - Plain door IP55, H1800 x W300","OE- PUERTA OPACA IP55, H1800 x W300","ZENERGY - TÖMÖR AJTÓ IP55, H1800 X W300"]
["70560","ZENERGY - DRZWI PEŁNE IP55, H1800 X W600",1238.8,"1-ZE-01",5.8333333333333334E-2,4,"OE_DOORS_1800","70360","SZT","85389099",null,null,"5901988705602","OE - Portes pleine IP55, H1800 x L600","OE - Plain door IP55, H1800 x W600","OE- PUERTA OPACA IP55, H1800 x W600","ZENERGY - TÖMÖR AJTÓ IP55, H1800 X W600"]
["70565","ZENERGY - DRZWI PEŁNE IP55, H1800 X W650",1277.5999999999999,"1-ZE-01",null,null,"OE_DOORS_1800","70365","SZT","85389099","27.12.40.0",null,"5901988705657","OE - Portes pleine IP55, H1800 x L650","OE - Plain door IP55, H1800 x W650","OE- PUERTA OPACA IP55, H1800 x W650","ZENERGY - TÖMÖR AJTÓ IP55, H1800 X W650"]
["70595","ZENERGY - DRZWI PEŁNE IP55, H1800 X W950",1519.6,"1-ZE-01",null,null,"OE_DOORS_1800","70395","SZT","85389099",null,null,"5901988705954","OE - Portes pleine IP55, H1800 x L950","OE - Plain door IP55, H1800 x W950","OE- PUERTA OPACA IP55, H1800 x W950","ZENERGY - TÖMÖR AJTÓ IP55, H1800 X W950"]
["70640","ZENERGY - DRZWI PRZESZKLONE IP55, H1800 X W400",1184.8,"1-ZE-01",null,null,"OE_DOORS_1800","71140","SZT","85389099",null,null,"5901988706401","OE - Portes vitrée IP55, H1800 x L400","OE - Glazed door IP55, H1800 x W400","OE- PUERTA TRANSPARENTE IP55, H1800 x W400","ZENERGY - ÜVEZETETT AJTÓK IP55, H1800 X W400"]
["70665","ZENERGY - DRZWI PRZESZKLONE IP55, H1800 X W650",1527.1,"1-ZE-01",null,null,"OE_DOORS_1800","71165","SZT","85389099",null,null,"5901988706654","OE - Portes vitrée IP55, H1800 x L650","OE - Glazed door IP55, H1800 x W650","OE- PUERTA TRANSPARENTE IP55, H1800 x W650","ZENERGY - ÜVEZETETT AJTÓK IP55, H1800 X W650"]
["70695","ZENERGY - DRZWI PRZESZKLONE IP55, H1800 X W950",1883.5,"1-ZE-01",null,null,"OE_DOORS_1800","70695","SZT","85389099",null,null,"5901988706951","OE - Portes vitrée IP55, H1800 x L950","OE - Glazed door IP55, H1800 x W950","OE- PUERTA TRANSPARENTE IP55, H1800 x W950","ZENERGY - ÜVEZETETT AJTÓK IP55, H1800 X W950"]
["70746","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 3X EFEN 160-630, H1800 X W450, 23+13M, ANALIZATORY 3X 96X96MM DO PLOMBOWANIA",610.5,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","70746","SZT","85389099",null,null,"5901988707460","OE - Cadre pivotant composé de 3 interrupteurs-sectionneurs EFEN 160-630 à lamelles, H1800 x L450, 23 + 13M, 3 analyseurs pour l'étanchéité","OE - Hinged frame for 3x EFEN 160-630, H1800 x W450, 23 + 13M slat switch disconnectors, 3x 96x96mm analyzers for sealing","OE- ESTR. PARA REGLETAS SECC. 3X160-630, H1800 x W450, 23+13M, ANALIZ.","ZENERGY - 3X EFEN SZALAK KAPCSOLÓ DÖNTÉSŰ KERETE 160-630, H1800 X W450, 23+13M, 3X 96X96MM ELEMZŐK ZÁRTHOZ"]
["70765","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 5X EFEN 160-630, H1800 X W650, 23+13M, ANALIZATORY 5X 96X96MM",678.7,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","70765","SZT","85389099",null,null,"5901988707651","OE - Cadre pivotant d'interrupteurs-sectionneurs 5x EFEN 160-630, H1800 x L650, 23 + 13M, analyseurs 5x 96x96mm","OE - Hinged frame for 5x EFEN 160-630, H1800 x W650, 23 + 13M rail disconnectors, analyzers 5x 96x96mm","OE- ESTR. PARA REGLETAS SECC. 5X160-630, H1800 x W650, 23+13M, ANALIZ.","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 5X EFEN 160-630, H1800 X W650, 23+13M, ELEMZŐK 5X 96X96MM"]
["70865","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 5X EFEN 160-630, H1800 X W650, 23+9M",559.4,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","70865","SZT","85389099",null,null,"5901988708658","OE - Cadre pivotant d'interrupteurs-sectionneurs 5x EFEN 160-630, H1800 x L650, 23 + 9M","OE - Hinged frame for switch disconnectors 5x EFEN 160-630, H1800 x W650, 23 + 9M","OE- ESTR. PARA REGLETAS SECC. 5X160-630, H1800 x W650, 23+9M","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 5X EFEN 160-630, H1800 X W650, 23+9M"]
["70866","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 5X EFEN 160-630, H1800 X W650, 23+9M DO PLOMBOWANIA",583,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","70865","SZT","85389099",null,null,"5901988708665","OE - Cadre pivotant d'interrupteurs-sectionneurs 5x EFEN 160-630, H1800 x L650, 23 + 9M pour l'étanchéité","OE - Hinged frame for switch disconnectors 5x EFEN 160-630, H1800 x W650, 23 + 9M for sealing","OE- ESTR. PARA REGLETAS SECC. 5X160-630, H1800 x W650, 23+9M ","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 5X EFEN 160-630, H1800 X W650, 23+9M TÖMÍTÉSRE"]
["70910","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1800 X W1000 + WSPORNIKI,  ( 1650 X 900 )",1027.0999999999999,"1-ZE-01",null,null,"OE_PLAIN_PLATES","70910","SZT","85389099","27.12.40.0",null,"5901988709105","OE - Plaque de montage complète, supports H1800 x L1000 +, (1650 x 900)","OE - Plain Mounting plate H1800 x W1000 + brackets, (1650 x 900)","OE- PLACA MONTAJE  TOTAL CIEGA H1800 x W1000 + SOPORT. (1650 X 900)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1800 X W1000 + KONZEREK, (1650 X 900)"]
["70940","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1800 X W400 + WSPORNIKI,  ( 1650 X 300 )",492.5,"1-ZE-01",null,null,"OE_PLAIN_PLATES","70940","SZT","85389099",null,null,"5901988709402","OE - Plaque de montage complète H1800 x L400 + supports, (1650 x 300)","OE - Plain Mounting plate H1800 x W400 + brackets, (1650 x 300)","OE- PLACA MONTAJE  TOTAL CIEGA H1800 x W400 + SOPORT. (1650 X 300)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1800 X W400 + KONZEREK, (1650 X 300)"]
["70965","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H1800 X W650 + WSPORNIKI,  ( 1650 X 550 )",715,"1-ZE-01",null,null,"OE_PLAIN_PLATES","70965","SZT","85389099","27.12.40.0",null,"5901988709655","OE - Plaque de montage complète H1800 x L650 + supports, (1650 x 550)","OE - Plain Mounting plate H1800 x W650 + brackets, (1650 x 550)","OE- PLACA MONTAJE  TOTAL CIEGA H1800 x W650 + SOPORT. (1650 X 550)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H1800 X W650 + KONZEREK, (1650 X 550)"]
["70995","ZENERGY - PEŁNY ŁĄCZNIK PŁYT MONTAŻOWYCH H1800,  ( 1650 X 98 )",222.5,"1-ZE-01",0.19166666666666668,6,"OE_PLAIN_PLATES",null,"SZT","85389099","27.12.40.0",null,"5901988709952","OE - Connecteur complet pour plaques de montage H1800, (1650 x 98)","OE - Plain Mounting plate connector H1800, (1650 x 98)","OE- UNION PLACA MONTAJE  TOTAL H1800, ( 1650 X 98 )","ZENERGY - SZERELŐLEMEZEK TELJES CSATLAKOZÓJA H1800, (1650 X 98)"]
["71140","ZENERGY - DRZWI PRZESZKLONE IP30, H1800 X W400",1020.6,"1-ZE-01",null,null,"OE_DOORS_1800","71140","SZT","85389099",null,null,"5901988711405","OE - Portes vitrées IP30, H1800 x L400","OE - Glazed door IP30, H1800 x W400","OE- PUERTA TRANSP. DOBLE IP30, H1800XW400","ZENERGY - ÜVEZETETT AJTÓK IP30, H1800 X W400"]
["71165","ZENERGY - DRZWI PRZESZKLONE IP30, H1800 X W650",1315.4,"1-ZE-01",null,null,"OE_DOORS_1800","71165","SZT","85389099",null,null,"5901988711658","OE - Portes vitrées IP30, H1800 x L650","OE - Glazed door IP30, H1800 x W650","OE- PUERTA TRANSP. DOBLE IP30, H1800XW650","ZENERGY - ÜVEGAJTÓK IP30, H1800 X W650"]
["71180","ZENERGY - DRZWI PRZESZKLONE IP30, H1800 X W800",1481.8,"1-ZE-01",null,null,"OE_DOORS_1800","71180","SZT","85389099",null,null,"5901988711801","OE - Portes vitrées IP30, H1800 x L800","OE - Glazed door IP30, H1800 x W800","OE- PUERTA TRANSP. DOBLE IP30, H1800XW800","ZENERGY - ÜVEGAJTÓK IP30, H1800 X W800"]
["71211","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1800 X W850+200",841.3,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988712112","OE - Couverture arrière complète IP30, H1800 x L650 + 400","OE - Plain rear cover IP30, H1800 x W850 + 200","OE- FONDO ATORNILLADO LISO IP30, H1800 x W650+400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1800 X W850+200"]
["71230","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1800 X W300",292.7,"1-ZE-01",null,null,"OE_COVERS","71230","SZT","85389099",null,null,"5901988712303","OE - Couverture arrière complète IP30, H1800 x L300","OE - Plain rear cover IP30, H1800 x W300","OE- FONDO ATORNILLADO LISO IP30, H1800 x W300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1800 X W300"]
["71265","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1800 X W650",570.20000000000005,"1-ZE-01",5.8333333333333334E-2,2,"OE_COVERS","71265","SZT","85389099","27.12.40.0",null,"5901988712655","OE - Couverture arrière complète IP30, H1800 x L650","OE - Plain rear cover IP30, H1800 x W650","OE- FONDO ATORNILLADO LISO IP30, H1800 x W650","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1800 X W650"]
["71295","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H1800 X W650+300",740.9,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988712952","OE - Couverture arrière complète IP30, H1800 x L650 + 300","OE - Plain rear cover IP30, H1800 x W650 + 300","OE- FONDO ATORNILLADO LISO IP30, H1800 x W650+300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H1800 X W650+300"]
["71312","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1800 X W1200",1191.2,"1-ZE-01",null,null,"OE_COVERS","71312","SZT","85389099",null,null,"5901988713126","OE - Couvercle ventilé IP30, H1800 x L1200","OE - Rear ventilated cover IP30, H1800 x W1200","OE- FONDO ATORNILLADO VENTIL. IP30, H1800 x W1200","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1800 X W1200"]
["71345","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1800 X W450",518.4,"1-ZE-01",null,null,"OE_COVERS","71345","SZT","85389099","27.12.40.0",null,"5901988713454","OE - Hotte d'aération arrière IP30, H1800 x L450","OE - Rear ventilated cover IP30, H1800 x W450","OE- FONDO ATORNILLADO VENTIL. IP30, H1800 x W450","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1800 X W450"]
["71380","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1800 X W800",719.3,"1-ZE-01",null,null,"OE_COVERS","71380","SZT","85389099",null,null,"5901988713805","OE - Couvercle ventilé IP30, H1800 x L800","OE - Rear ventilated cover IP30, H1800 x W800","OE- FONDO ATORNILLADO VENTIL. IP30, H1800 x W800","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1800 X W800"]
["71385","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H1800 X W850",745.2,"1-ZE-01",null,null,"OE_COVERS","71385","SZT","85389099",null,null,"5901988713850","OE - Couvercle ventilé IP30, H1800 x L850","OE - Rear ventilated cover IP30, H1800 x W850","OE- FONDO ATORNILLADO VENTIL. IP30, H1800 x W850","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H1800 X W850"]
["71411","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1800 X W850+200",1083.2,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988714116","OE - Hotte d'aération arrière IP43, H1800 x L650 + 400","OE - Rear ventilated cover IP43, H1800 x W850 + 200","OE- FONDO ATORNILLADO VENTIL.IP43, H1800 x W650+400","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1800 X W850+200"]
["71430","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1800 X W300",460.1,"1-ZE-01",null,null,"OE_COVERS","71330","SZT","85389099",null,null,"5901988714307","OE - Hotte d'aération arrière IP43, H1800 x L300","OE - Rear ventilated cover IP43, H1800 x W300","OE- FONDO ATORNILLADO VENTIL.IP43, H1800 x W300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1800 X W300"]
["71460","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H1800 X W600",721.4,"1-ZE-01",null,null,"OE_COVERS","71360","SZT","85389099",null,null,"5901988714604","OE - Couvercle ventilé IP43, H1800 x L600","OE - Rear ventilated cover IP43, H1800 x W600","OE- FONDO ATORNILLADO VENTIL.IP43, H1800 x W600","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H1800 X W600"]
["71510","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1800 X W1000",878,"1-ZE-01",null,null,"OE_COVERS","71210","SZT","85389099",null,null,"5901988715106","OE - Couverture arrière complète IP55, H1800 x L1000","OE - Plain rear cover IP55, H1800 x W1000","OE- FONDO ATORNILLADO LISO IP55, H1800 x W1000","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1800 X W1000"]
["71513","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1800 X W1300",1368.4,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988715137","OE - Couverture arrière complète IP55, H1800 x L1300","OE - Plain rear cover IP55, H1800 x W1300","OE- FONDO ATORNILLADO LISO IP55, H1800 x W1300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1800 X W1300"]
["71560","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1800 X W600",649.1,"1-ZE-01",5.8333333333333334E-2,4,"OE_COVERS","71260","SZT","85389099",null,null,"5901988715601","OE - Couverture arrière complète IP55, H1800 x L600","OE - Plain rear cover IP55, H1800 x W600","OE- FONDO ATORNILLADO LISO IP55, H1800 x W600","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1800 X W600"]
["71585","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1800 X W850",794.9,"1-ZE-01",null,null,"OE_COVERS","71285","SZT","85389099","27.12.40.0",null,"5901988715854","OE - Couverture arrière complète IP55, H1800 x L850","OE - Plain rear cover IP55, H1800 x W850","OE- FONDO ATORNILLADO LISO IP55, H1800 x W850","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1800 X W850"]
["71595","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H1800 X W650+300",852.1,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099",null,null,"5901988715953","OE - Couverture arrière complète IP55, H1800 x L650 + 300","OE - Plain rear cover IP55, H1800 x W650 + 300","OE- FONDO ATORNILLADO LISO IP55, H1800 x W650+300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H1800 X W650+300"]
["72045","ZENERGY - RAMA, H1800 X D230 X W450",745.2,"1-ZE-01",null,null,"OE_FRAME_1800","72045","SZT","85389099",null,null,"5901988720452","OE - Cradle, H1800 x P230 x L450","OE - Frame, H1800 x D230 x W450","OE- ESTRUCTURA, H1800 x D230 x W450","ZENERGY - KERET, H1800 X D230 X W450"]
["72080","ZENERGY - RAMA, H1800 X D230 X W800",909.7,"1-ZE-01",null,null,"OE_FRAME_1800","72080","SZT","85389099",null,null,"5901988720803","OE - Cradle, H1800 x P230 x L800","OE - Frame, H1800 x D230 x W800","OE- ESTRUCTURA, H1800 x D230 x W800","ZENERGY - KERET, H1800 X D230 X W800"]
["72095","ZENERGY - RAMA, H1800 X D230 X W950, 650+300",1208.9000000000001,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988720957","OE - Cradle, H1800 x P230 x L950, 650 + 300","OE - Frame, H1800 x D230 x W950, 650 + 300","OE- ESTRUCTURA, H1800 x D230 x W950, 650+300","ZENERGY – KERET, H1800 X D230 X W950, 650+300"]
["72110","ZENERGY - RAMA, H1800 X D230 X W1100, 150+650+300",1453.1,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988721107","OE - Cradle, H1800 x P230 x L1100, 150 + 650 + 300","OE - Frame, H1800 x D230 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1800 x D230 x W1100, 150+650+300","ZENERGY – KERET, H1800 X D230 X W1100, 150+650+300"]
["72125","ZENERGY - RAMA, H1800 X D230 X W1250, 850+400",1331,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988721251","OE - Cradle, H1800 x P230 x L1250, 850 + 400","OE - Frame, H1800 x D230 x W1250, 850 + 400","OE- ESTRUCTURA, H1800 x D230 x W1250, 850+400","ZENERGY – KERET, H1800 X D230 X W1250, 850+400"]
["72133","ZENERGY - RAMA, H1800 X D230 X W1300, 850+450",1034,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988721336","OE - Cradle, H1800 x P230 x L1300, 850 + 450","OE - Frame, H1800 x D230 x W1300, 850 + 450","OE- ESTRUCTURA, H1800 x D230 x W1300, 850+450","ZENERGY – KERET, H1800 X D230 X W1300, 850+450"]
["72170","ZENERGY - RAMA, H1800 X D230 X W1700, 850+850",1512.5,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988721701","OE - Cadre, H1800 x P230 x L1700, 850 + 850","OE - Frame, H1800 x D230 x W1700, 850 + 850","OE- ESTRUCTURA, H1800 x D230 x W1700, 850+850","ZENERGY – KERET, H1800 X D230 X W1700, 850+850"]
["73030","ZENERGY - RAMA, H1800 X D300 X W300",740.3,"1-ZE-01",null,null,"OE_FRAME_1800","73030","SZT","85389099",null,null,"5901988730307","OE - Cradle, H1800 x P300 x L300","OE - Frame, H1800 x D300 x W300","OE- ESTRUCTURA, H1800 x D300 x W300","ZENERGY - KERET, H1800 X D300 X W300"]
["73060","ZENERGY - RAMA, H1800 X D300 X W600",854.3,"1-ZE-01",0.01,1,"OE_FRAME_1800","73060","SZT","85389099",null,null,"5901988730604","OE - Cradle, H1800 x P300 x L600","OE - Frame, H1800 x D300 x W600","OE- ESTRUCTURA, H1800 x D300 x W600","ZENERGY - KERET, H1800 X D300 X W600"]
["73081","ZENERGY - RAMA, H1800 X D300 X W800, 650+150",1156.0999999999999,"1-ZE-01",null,null,"OE_FRAME_1800","73081","SZT","85389099",null,null,"5901988730819","OE - Cradle, H1800 x P300 x L800, 650 + 150","OE - Frame, H1800 x D300 x W800, 650 + 150","OE- ESTRUCTURA, H1800 x D300 x W800, 650+150","ZENERGY – KERET, H1800 X D300 X W800, 650+150"]
["73100","ZENERGY - RAMA, H1800 X D300 X W1000",1023.8,"1-ZE-01",null,null,"OE_FRAME_1800","73100","SZT","85389099",null,null,"5901988731007","OE - Cradle, H1800 x P300 x L1000","OE - Frame, H1800 x D300 x W1000","OE- ESTRUCTURA, H1800 x D300 x W1000","ZENERGY - KERET, H1800 X D300 X W1000"]
["73115","ZENERGY - RAMA, H1800 X D300 X W1150, 850+300",1368.4,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988731151","OE - Cadre, H1800 x P300 x L1150, 850 + 300","OE - Frame, H1800 x D300 x W1150, 850 + 300","OE- ESTRUCTURA, H1800 x D300 x W1150, 850+300","ZENERGY – KERET, H1800 X D300 X W1150, 850+300"]
["73130","ZENERGY - RAMA, H1800 X D300 X W1300",1171.5,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988731304","OE - Cradle, H1800 x P300 x L1300","OE - Frame, H1800 x D300 x W1300","OE- ESTRUCTURA, H1800 x D300 x W1300","ZENERGY - KERET, H1800 X D300 X W1300"]
["73150","ZENERGY - RAMA, H1800 X D300 X W1500, 650+850",1510.3,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988731502","OE - Cadre, H1800 x P300 x L1500, 650 + 850","OE - Frame, H1800 x D300 x W1500, 650 + 850","OE- ESTRUCTURA, H1800 x D300 x W1500, 650+850","ZENERGY – KERET, H1800 X D300 X W1500, 650+850"]
["74030","ZENERGY - RAMA, H1800 X D400 X W300",773.3,"1-ZE-01",null,null,"OE_FRAME_1800","74030","SZT","85389099",null,null,"5901988740306","OE - Cradle, H1800 x P400 x L300","OE - Frame, H1800 x D400 x W300","OE- ESTRUCTURA, H1800 x D400 x W300","ZENERGY - KERET, H1800 X D400 X W300"]
["74045","ZENERGY - RAMA, H1800 X D400 X W450",837,"1-ZE-01",null,null,"OE_FRAME_1800","74045","SZT","85389099",null,null,"5901988740450","OE - Cradle, H1800 x P400 x L450","OE - Frame, H1800 x D400 x W450","OE- ESTRUCTURA, H1800 x D400 x W450","ZENERGY - KERET, H1800 X D400 X W450"]
["74080","ZENERGY - RAMA, H1800 X D400 X W800",986,"1-ZE-01",0.05,4,"OE_FRAME_1800","74080","SZT","85389099",null,null,"5901988740801","OE - Cradle, H1800 x P400 x L800","OE - Frame, H1800 x D400 x W800","OE- ESTRUCTURA, H1800 x D400 x W800","ZENERGY - KERET, H1800 X D400 X W800"]
["74095","ZENERGY - RAMA, H1800 X D400 X W950, 650+300",1342,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988740955","OE - Cadre, H1800 x P400 x L950, 650 + 300","OE - Frame, H1800 x D400 x W950, 650 + 300","OE- ESTRUCTURA, H1800 x D400 x W950, 650+300","ZENERGY – KERET, H1800 X D400 X W950, 650+300"]
["74110","ZENERGY - RAMA, H1800 X D400 X W1100, 150+650+300",1632.4,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988741105","OE - Cadre, H1800 x P400 x L1100, 150 + 650 + 300","OE - Frame, H1800 x D400 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1800 x D400 x W1100, 150+650+300","ZENERGY - KERET, H1800 X D400 X W1100, 150+650+300"]
["74121","ZENERGY - RAMA, H1800 X D400 X W1200, 150+650+400",1673.1,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988741211","OE - Cadre, H1800 x P400 x L1200, 150 + 650 + 400","OE - Frame, H1800 x D400 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H1800 x D400 x W1200, 150+650+400","ZENERGY – KERET, H1800 X D400 X W1200, 150+650+400"]
["74133","ZENERGY - RAMA, H1800 X D400 X W1300, 850+450",1562,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988741334","OE - Cradle, H1800 x P400 x L1300, 850 + 450","OE - Frame, H1800 x D400 x W1300, 850 + 450","OE- ESTRUCTURA, H1800 x D400 x W1300, 850+450","ZENERGY – KERET, H1800 X D400 X W1300, 850+450"]
["74170","ZENERGY - RAMA, H1800 X D400 X W1700, 850+850",1614.6,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988741709","OE - Cadre, H1800 x P400 x L1700, 850 + 850","OE - Frame, H1800 x D400 x W1700, 850 + 850","OE- ESTRUCTURA, H1800 x D400 x W1700, 850+850","ZENERGY - KERET, H1800 XD400 X W1700, 850+850"]
["75385","ZENERGY - DRZWI PRZEDZIAŁU KABLOWEGO IP30, H1800 X W850",357.5,"1-ZE-01",null,null,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988753856","OE - PORTE DU COMPARTIMENT CÂBLES IP30, H1800 X L850","OE - Cable compartment door IP30, H1800 x W850","*OE - PUERTA DEL COMPARTIMIENTO DE CABLES IP30, H1800 x W850","ZENERGY - KÁBELREKESZ AJTÓ IP30, H1800 X W850"]
["76030","ZENERGY - RAMA, H1800 X D600 X W300",1149.5,"1-ZE-01",null,null,"OE_FRAME_1800","76030","SZT","85389099",null,null,"5901988760304","OE - Cradle, H1800 x P600 x L300","OE - Frame, H1800 x D600 x W300","OE- ESTRUCTURA, H1800 x D600 x W300","ZENERGY - KERET, H1800 X D600 X W300"]
["76060","ZENERGY - RAMA, H1800 X D600 X W600",1256,"1-ZE-01",0.01,1,"OE_FRAME_1800","76060","SZT","85389099",null,null,"5901988760601","OE - Cadre, H1800 x P600 x L600","OE - Frame, H1800 x D600 x W600","OE- ESTRUCTURA, H1800 x D600 x W600","ZENERGY - KERET, H1800 X D600 X W600"]
["76081","ZENERGY - RAMA, H1800 X D600 X W800, 650+150",1738.8,"1-ZE-01",0.01,1,"OE_FRAME_1800","76081","SZT","85389099",null,null,"5901988760816","OE - Cadre, H1800 x P600 x L800, 650 + 150","OE - Frame, H1800 x D600 x W800, 650 + 150","OE- ESTRUCTURA, H1800 x D600 x W800, 650+150","ZENERGY – KERET, H1800 X D600 X W800, 650+150"]
["76095","ZENERGY - RAMA, H1800 X D600 X W950, 650+300",1882.1,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988760953","OE - Cadre, H1800 x P600 x L950, 650 + 300","OE - Frame, H1800 x D600 x W950, 650 + 300","OE- ESTRUCTURA, H1800 x D600 x W950, 650+300","ZENERGY – KERET, H1800 X D600 X W950, 650+300"]
["76110","ZENERGY - RAMA, H1800 X D600 X W1100, 150+650+300",2354,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988761103","OE - Cadre, H1800 x P600 x L1100, 150 + 650 + 300","OE - Frame, H1800 x D600 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1800 x D600 x W1100, 150+650+300","ZENERGY – KERET, H1800 X D600 X W1100, 150+650+300"]
["76125","ZENERGY - RAMA, H1800 X D600 X W1250, 850+400",2003.1,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988761257","OE - Cadre, H1800 x P600 x L1250, 850 + 400","OE - Frame, H1800 x D600 x W1250, 850 + 400","OE- ESTRUCTURA, H1800 x D600 x W1250, 850+400","ZENERGY – KERET, H1800 X D600 X W1250, 850+400"]
["76133","ZENERGY - RAMA, H1800 X D600 X W1300, 850+450",1538.9,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988761332","OE - Cadre, H1800 x P600 x L1300, 850 + 450","OE - Frame, H1800 x D600 x W1300, 850 + 450","OE- ESTRUCTURA, H1800 x D600 x W1300, 850+450","ZENERGY – KERET, H1800 X D600 X W1300, 850+450"]
["76160","ZENERGY - RAMA, H1800 X D600 X W1600, 800+800",2074.6,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988761608","OE - Cadre, H1800 x P600 x L1600, 800 + 800","OE - Frame, H1800 x D600 x W1600, 800 + 800","OE- ESTRUCTURA, H1800 x D600 x W1600, 800+800","ZENERGY – KERET, H1800 X D600 X W1600, 800+800"]
["76170","ZENERGY - RAMA, H1800 X D600 X W1700, 850+850",2146,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988761707","OE - Cadre, H1800 x P600 x L1700, 850 + 850","OE - Frame, H1800 x D600 x W1700, 850 + 850","OE- ESTRUCTURA, H1800 x D600 x W1700, 850+850","ZENERGY – KERET, H1800 X D600 X W1700, 850+850"]
["78045","ZENERGY - RAMA, H1800 X D800 X W450",1329.4,"1-ZE-01",null,null,"OE_FRAME_1800","78045","SZT","85389099",null,null,"5901988780456","OE - Cradle, H1800 x P800 x L450","OE - Frame, H1800 x D800 x W450","OE- ESTRUCTURA, H1800 x D800 x W450","ZENERGY - KERET, H1800 X D800 X W450"]
["78081","ZENERGY - RAMA, H1800 X D800 X W800, 650+150",1942.1,"1-ZE-01",null,null,"OE_FRAME_1800","78081","SZT","85389099",null,null,"5901988780814","OE - Cadre, H1800 x P800 x L800, 650 + 150","OE - Frame, H1800 x D800 x W800, 650 + 150","OE- ESTRUCTURA, H1800 x D800 x W800, 650+150","ZENERGY – KERET, H1800 X D800 X W800, 650+150"]
["78095","ZENERGY - RAMA, H1800 X D800 X W950, 650+300",2055.1999999999998,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988780951","OE - Cradle, H1800 x P800 x L950, 650 + 300","OE - Frame, H1800 x D800 x W950, 650 + 300","OE- ESTRUCTURA, H1800 x D800 x W950, 650+300","ZENERGY – KERET, H1800 X D800 X W950, 650+300"]
["78110","ZENERGY - RAMA, H1800 X D800 X W1100, 150+650+300",2581.6,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988781101","OE - Cadre, H1800 x P800 x L1100, 150 + 650 + 300","OE - Frame, H1800 x D800 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H1800 x D800 x W1100, 150+650+300","ZENERGY – KERET, H1800 X D800 X W1100, 150+650+300"]
["78130","ZENERGY - RAMA, H1800 X D800 X W1300",1703.5,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988781309","OE - Cradle, H1800 x P800 x L1300","OE - Frame, H1800 x D800 x W1300","OE- ESTRUCTURA, H1800 x D800 x W1300","ZENERGY - KERET, H1800 X D800 X W1300"]
["78150","ZENERGY - RAMA, H1800 X D800 X W1500, 650+850",2281.4,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988781507","OE - Cadre, H1800 x P800 x L1500, 650 + 850","OE - Frame, H1800 x D800 x W1500, 650 + 850","OE- ESTRUCTURA, H1800 x D800 x W1500, 650+850","ZENERGY – KERET, H1800 X D800 X W1500, 650+850"]
["78160","ZENERGY - RAMA, H1800 X D800 X W1600, 800+800",2251.1999999999998,"1-ZE-01",null,null,"OE_FRAME_1800",null,"SZT","85389099",null,null,"5901988781606","OE - Cradle, H1800 x P800 x L1600, 800 + 800","OE - Frame, H1800 x D800 x W1600, 800 + 800","OE- ESTRUCTURA, H1800 x D800 x W1600, 800+800","ZENERGY – KERET, H1800 X D800 X W1600, 800+800"]
["79224","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP30, H1800 X D230",343.4,"1-ZE-01",null,null,"OE_COVERS","79324","SZT","85389099",null,null,"5901988792244","OE - Évents latéraux, ventilés, fixes IP30, H1800 x P230","OE - Ventilated, fixed side covers IP30, H1800 x D230","OE- PAREDES LATERALES VENTIL. FIJO IP30, H1800 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP30, H1800 X D230"]
["79231","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP30, H1800 X D300",366.1,"1-ZE-01",null,null,"OE_COVERS","79331","SZT","85389099",null,null,"5901988792312","OE - Évents latéraux, ventilés, fixes IP30, H1800 x P300","OE - Ventilated, fixed side covers IP30, H1800 x D300","OE- PAREDES LATERALES VENTIL. FIJO IP30, H1800 x D300 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP30, H1800 X D300"]
["79242","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1800 X D400",387.7,"1-ZE-01",null,null,"OE_COVERS","79342","SZT","85389099",null,null,"5901988792428","OE - Couvercles latéraux ventilés, plats, à visser IP30, H1800 x P400","OE - Side panels ventilated, flat, screwed on, IP30, H1800 x D400","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1800 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1800 X D400"]
["79262","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1800 X D600",412.6,"1-ZE-01",null,null,"OE_COVERS","79362","SZT","85389099",null,null,"5901988792626","OE - Orifices latéraux, ventilés, plats et vissés IP30, H1800 x P600","OE - Side panels ventilated, flat, screwed on, IP30, H1800 x D600","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1800 x D600 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1800 X D600"]
["79282","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H1800 X D800",446.6,"1-ZE-01",null,null,"OE_COVERS","79382","SZT","85389099",null,null,"5901988792824","OE - Évents latéraux, ventilés, plats, vissés IP30, H1800 x P800","OE - Side panels ventilated, flat, screwed on, IP30, H1800 x D800","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H1800 x D800 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H1800 X D800"]
["79327","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1800 X D230",146.69999999999999,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988793272","OE - Panneau de séparation, vertical, galvanisé, H1800 x P230","OE - Vertical partition, Galvanized, H1800 x D230","OE- Tabique VERT., galvanizado, H1800 x D230","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1800 X D230"]
["79332","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H1800 X D300",292.7,"1-ZE-01",null,null,"OE_COVERS","79332","SZT","85389099",null,null,"5901988793326","OE - Capots latéraux solides, plats, vissés IP30, H1800 x P300","OE - Plain, flat, screwed side covers IP30, H1800 x D300","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H1800 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H1800 X D300"]
["79335","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H1800 X D300",159,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR",null,"SZT","85389099",null,null,"5901988793357","OE - Panneau de séparation, vertical, galvanisé, H1800 x P300","OE - Vertical partition, Galvanized, H1800 x D300","OE- Tabique VERT., galvanizado, H1800 x D300","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H1800 X D300"]
["79342","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H1800 X D400",314.3,"1-ZE-01",null,null,"OE_COVERS","79342","SZT","85389099",null,null,"5901988793425","OE - Capots latéraux solides, plats, vissés IP30, H1800 x P400","OE - Side panels Plain, flat, screwed on, IP30, H1800 x D400","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H1800 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H1800 X D400"]
["79361","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1800 X D600",365,"1-ZE-01",null,null,"OE_COVERS","79361","SZT","85389099",null,null,"5901988793616","OE - Couvercles latéraux complets, fixes IP30, H1800 x P600","OE - Plain side covers, fixed IP30, H1800 x D600","OE- PAREDES LATERALES LISO FIJO IP30, H1800 x D600 (2UDS)","ZENERGY – TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H1800 X D600"]
["79381","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H1800 X D800",420.2,"1-ZE-01",null,null,"OE_COVERS","79381","SZT","85389099",null,null,"5901988793814","OE - Couvercles latéraux complets, fixes IP30, H1800 x P800","OE - Plain, fixed side covers IP30, H1800 x D800","OE- PAREDES LATERALES LISO FIJO IP30, H1800 x D800 (2UDS)","ZENERGY – TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H1800 X D800"]
["79423","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H1800 X D230",596.20000000000005,"1-ZE-01",null,null,"OE_COVERS","79223","SZT","85389099",null,null,"5901988794231","OE - Hottes de ventilation latérales IP43, H1800 x P230","OE - IP43, H1800 x D230 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H1800 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H1800 X D230"]
["79431","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1800 X D300",457.9,"1-ZE-01",null,null,"OE_COVERS","79431","SZT","85389099",null,null,"5901988794316","OE - Évents latéraux, ventilés, fixes IP43, H1800 x P300","OE - Ventilated, fixed side covers IP43, H1800 x D300","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1800 x D300 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H1800 X D300"]
["79441","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1800 X D400",484.9,"1-ZE-01",null,null,"OE_COVERS","79441","SZT","85389099",null,null,"5901988794415","OE - Évents latéraux, ventilés, fixes IP43, H1800 x P400","OE - Ventilated, fixed side covers IP43, H1800 x D400","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1800 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H1800 X D400"]
["79461","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H1800 X D600",524.9,"1-ZE-01",null,null,"OE_COVERS","79461","SZT","85389099",null,null,"5901988794613","OE - Ventilateurs latéraux ventilés fixes IP43, H1800 x P600","OE - Ventilated, fixed side covers IP43, H1800 x D600","OE- PAREDES LATERALES VENTIL. FIJO IP43, H1800 x D600 (2UDS)","ZENERGY - OLDALBURKOLAT MINILÁLT, ÁLLANDÓ IP43, H1800 X D600"]
["79462","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP43, H1800 X D600",524.9,"1-ZE-01",null,null,"OE_COVERS","79362","SZT","85389099",null,null,"5901988794620","OE - Grilles d'aération latérales, ventilées, plates, vissées IP43, H1800 x P600","OE - Side panels ventilated, flat, screwed on, IP43, H1800 x D600","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP43, H1800 x D600 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP43, H1800 X D600"]
["79523","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1800 X D230",675,"1-ZE-01",null,null,"OE_COVERS","79323","SZT","85389099",null,null,"5901988795238","OE - Couvercles latéraux complets IP55, H1800 x P230","OE - Plain side covers IP55, H1800 x D230","OE- PAREDES LATERALES LISO IP55, H1800 x D230 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1800 X D230"]
["79560","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H1800 X D600",787.3,"1-ZE-01",3.3333333333333333E-2,1,"OE_COVERS","79360","SZT","85389099",null,null,"5901988795603","OE - Capots latéraux complets IP55, H1800 x P600","OE - Plain side covers IP55, H1800 x D600","OE- PAREDES LATERALES LISO IP55, H1800 x D600 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H1800 X D600"]
["80002","OM - Fantom Zamykanie drzwi przy ramie",0,"1-ZE-10",null,null,"OM_FANTOM_PRODUCTS","80002","SZT","8538909900",null,null,"5901988800024","OE - Fantôme fermant la porte sur le cadre","OE - Fantom Closing the door on the frame","OM- Fantasma CIERRE DE LA PUERTA EN EL MARCO ARMARIOS MURALES","OM - Phantom Az ajtó bezárása a keretnél"]
["80005","OE - Fantom mocowanie wygrodzenia szyn pionowych w ramie",0,"1-ZE-10",null,null,"OE_FANTOM_PRODUCTS","80005","SZT","8538909900",null,null,"5901988800055","OE - fixation de la cloison des rails verticaux dans le cadre - Fantom","OE - Fantom fixing the partition of the Vertical rails in the frame","OE - Fantasma SOPORTE PARA TAPA FRONTAL EMBARRADO REF. 31071/31072","OE - A függőleges sínes kerítés fantom szerelése a keretben"]
["80110","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2000 W1000",437.4,"1-ZE-01",0.01,1,"OE_FRAME_INTERNAL","80110","SZT","85389099","27.12.40.0",null,"5901988801106","OE - Cadre de charnière avant à charnière H2000 L1000","OE - Frame of hinged Front covers H2000 W1000","OE- MARCO PIVOTANTE H2000 W1000","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H2000 W1000"]
["80141","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2000 W400 DO PLOMBOWANIA",339.9,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","80140","SZT","85389099","27.12.40.0",null,"5901988801410","OE - Cadre avant articulé H2000 L400 pour sceller","OE - Frame of Front covers on hinges H2000 W400 for sealing","OE- MARCO PIVOTANTE H2000 W400 ","ZENERGY - ZSÁNLÓS ELSŐ FEDŐKERET H2000 W400 TÖMÍTÉSHEZ"]
["80160","OE - Rama osłon czołowych na zawiasach H2000 W600",341,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","80160","SZT",null,null,"230823PW",null,"OE - Cadre de charnière avant à charnière H2000 L600","OE - Frame of hinged Front covers H2000 W600","OE- MARCO PIVOTANTE H2000 W600","OE - Csuklós első burkolatok kerete H2000 W600"]
["80165","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2000 W650",340.2,"1-ZE-01",2.2916666666666665,7,"OE_FRAME_INTERNAL","80165","SZT","85389099","27.12.40.0",null,"5901988801656","OE - Cadre de charnière avant à charnière H2000 L650","OE - Frame of hinged Front covers H2000 W650","OE- MARCO PIVOTANTE H2000 W650","ZENERGY - SZÁNTOS ELSŐ BURKOLAT KERET H2000 W650"]
["80180","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2000 W800",411.5,"1-ZE-01",6.6666666666666666E-2,1,"OE_FRAME_INTERNAL","80180","SZT","85389099","27.12.40.0",null,"5901988801809","OE - Cadre de hayon avant articulé H2000 L800","OE - Frame of hinged Front covers H2000 W800","OE- MARCO PIVOTANTE H2000 W800","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H2000 W800"]
["80185","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2000 W850",428.8,"1-ZE-01",0.5,6,"OE_FRAME_INTERNAL","80185","SZT","85389099","27.12.40.0",null,"5901988801854","OE - Cadre de charnière avant à charnière H2000 L850","OE - Frame of hinged Front covers H2000 W850","OE- MARCO PIVOTANTE H2000 W850","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H2000 W850"]
["80212","ZENERGY - DRZWI WENTYLOWANE IP30, H2000 X W1200, PODWÓJNE",2189.1999999999998,"1-ZE-01",null,null,"OE_DOORS_2000","80312","SZT","85389099",null,null,"5901988802127","OE - Portes ventilées IP30, H2000 x L1200, double","OE - Ventilated doors IP30, H2000 x W1200, double","OE- PUERTA VENTIL. IP30, H2000 x W1200, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2000 X W1200, DUPLÉS"]
["80230","ZENERGY - DRZWI WENTYLOWANE IP30, H2000 X W300",762.5,"1-ZE-01",6.6666666666666666E-2,2,"OE_DOORS_2000","80330","SZT","85389099",null,null,"5901988802301","OE - Portes ventilées IP30, H2000 x L300","OE - Ventilated door IP30, H2000 x W300","OE- PUERTA VENTIL. IP30, H2000 x W300","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2000 X W300"]
["80265","ZENERGY - DRZWI WENTYLOWANE IP30, H2000 X W650",1015.2,"1-ZE-01",0.89166666666666672,8,"OE_DOORS_2000","80365","SZT","85389099",null,null,"5901988802653","OE - Portes ventilées IP30, H2000 x L650","OE - Ventilated door IP30, H2000 x W650","OE- PUERTA VENTIL. IP30, H2000 x W650","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2000 X W650"]
["80295","ZENERGY - DRZWI WENTYLOWANE IP30, H2000 X W950",1298.2,"1-ZE-01",null,null,"OE_DOORS_2000","80395","SZT","85389099",null,null,"5901988802950","OE - Portes ventilées IP30, H2000 x L950","OE - Ventilated door IP30, H2000 x W950","OE- PUERTA VENTIL. IP30, H2000 x W950","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2000 X W950"]
["80312","ZENERGY - DRZWI PEŁNE IP30, H2000 X W1200, PODWÓJNE",2099.5,"1-ZE-01",0.19166666666666668,6,"OE_DOORS_2000","80312","SZT","85389099","27.12.40.0",null,"5901988803124","OE - Portes pleine IP30, H2000 x L1200, double","OE - Plain door IP30, H2000 x W1200, double","OE- PUERTA OPACA IP30, H2000 x W1200, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H2000 X W1200, DUPLA"]
["80313","ZENERGY - DRZWI PEŁNE IP30, H2000 X W1300, PODWÓJNE",2117.9,"1-ZE-01",null,null,"OE_DOORS_2000","80313","SZT","85389099","27.12.40.0",null,"5901988803131","OE - Portes pleine IP30, H2000 x L1300, double","OE - Plain door IP30, H2000 x W1300, double","OE- PUERTA OPACA IP30, H2000 x W1300, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H2000 X W1300, DUPLA"]
["80340","ZENERGY - DRZWI PEŁNE IP30, H2000 X W400",777.6,"1-ZE-01",0.21666666666666667,5,"OE_DOORS_2000","80340","SZT","85389099","27.12.40.0",null,"5901988803407","OE - Portes pleine IP30, H2000 x L400","OE - Plain door IP30, H2000 x W400","OE- PUERTA OPACA IP30, H2000 x W400","ZENERGY - TÖMÖR AJTÓ IP30, H2000 X W400"]
["80371","ZENERGY - SŁUPEK OCYNK, H2000, RAMA ZEWNĘTRZNA",74.099999999999994,"1-ZE-01",3.6166666666666667,7,"OE_FRAME_2000","80371","SZT","85389099","27.12.40.0",null,"5901988803711","OE - Poteau galvanisé, H2000, cadre externe","OE - Galvanized post, H2000, Outer frame","OE- PERFIL GALVANIZADO, H2000, PARA MARCO LATERAL EXTERIOR","ZENERGY - HORGANYOZOTT OSZTA, H2000, KÜLSŐ KERET"]
["80374","ZENERGY - SŁUPEK INOX, H2000, RAMA WEWNETRZNA",166.3,"1-ZE-01",null,null,"OE_FRAME_2000","80372","SZT","85389099","27.12.40.0",null,"5901988803742","OE - Poteau INOX, H2000, cadre interne","OE - INOX post, H2000, internal frame","OE- PERFIL INOX, H2000, PARA MARCO LATERAL INTERIOR","ZENERGY - INOX POSTA, H2000, BELSŐ KERET"]
["80380","ZENERGY - DRZWI PEŁNE IP30, H2000 X W800",1147,"1-ZE-01",0.73333333333333328,6,"OE_DOORS_2000","80380","SZT","85389099","27.12.40.0",null,"5901988803803","OE - Portes pleine IP30, H2000 x L800","OE - Plain door IP30, H2000 x W800","OE- PUERTA OPACA IP30, H2000 x W800","ZENERGY - TÖMÖR AJTÓ IP30, H2000 X W800"]
["80410","ZENERGY - DRZWI WENTYLOWANE IP43, H2000 X W1000",1531.4,"1-ZE-01",null,null,"OE_DOORS_2000","80310","SZT","85389099",null,null,"5901988804107","OE - Portes ventilées IP43, H2000 x L1000","OE - Ventilated door IP43, H2000 x W1000","OE- PUERTA VENTIL. IP43, H2000 x W1000","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2000 X W1000"]
["80430","ZENERGY - DRZWI WENTYLOWANE IP43, H2000 X W300",887.8,"1-ZE-01",null,null,"OE_DOORS_2000","80330","SZT","85389099",null,null,"5901988804305","OE - Portes ventilées IP43, H2000 x L300","OE - Ventilated door IP43, H2000 x W300","OE- PUERTA VENTIL. IP43, H2000 x W300","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2000 X W300"]
["80460","ZENERGY - DRZWI WENTYLOWANE IP43, H2000 X W600",1142.5999999999999,"1-ZE-01",null,null,"OE_DOORS_2000","80360","SZT","85389099",null,null,"5901988804602","OE - Portes ventilées IP43, H2000 x L600","OE - Ventilated door IP43, H2000 x W600","OE- PUERTA VENTIL. IP43, H2000 x W600","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2000 X W600"]
["80465","ZENERGY - DRZWI WENTYLOWANE IP43, H2000 X W650",1170.7,"1-ZE-01",4.1666666666666664E-2,4,"OE_DOORS_2000","80365","SZT","85389099","27.12.40.0",null,"5901988804657","OE - Portes ventilées IP43, H2000 x L650","OE - Ventilated door IP43, H2000 x W650","OE- PUERTA VENTIL. IP43, H2000 x W650","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2000 X W650"]
["80495","ZENERGY - DRZWI WENTYLOWANE IP43, H2000 X W950",1454.8,"1-ZE-01",null,null,"OE_DOORS_2000","80395","SZT","85389099",null,null,"5901988804954","OE - Portes ventilées IP43, H2000 x L950","OE - Ventilated door IP43, H2000 x W950","OE- PUERTA VENTIL. IP43, H2000 x W950","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2000 X W950"]
["80513","ZENERGY - DRZWI PEŁNE IP55, H2000 X W1300, PODWÓJNE",2514.1999999999998,"1-ZE-01",null,null,"OE_DOORS_2000","80313","SZT","85389099","27.12.40.0",null,"5901988805135","OE - Portes pleine IP55, H2000 x L1300, double","OE - Plain door IP55, H2000 x W1300, double","OE- PUERTA OPACA IP55, H2000 x W1300, DOBLE","ZENERGY - TÖMÖR AJTÓK IP55, H2000 X W1300, DUPLA"]
["80540","ZENERGY - DRZWI PEŁNE IP55, H2000 X W400",940.7,"1-ZE-01",0.16666666666666666,6,"OE_DOORS_2000","80340","SZT","85389099","27.12.40.0",null,"5901988805401","OE - Portes pleine IP55, H2000 x L400","OE - Plain door IP55, H2000 x W400","OE- PUERTA OPACA IP55, H2000 x W400","ZENERGY - TÖMÖR AJTÓ IP55, H2000 X W400"]
["80565","ZENERGY - DRZWI PEŁNE IP55, H2000 X W650",1198.8,"1-ZE-01",0.76666666666666672,12,"OE_DOORS_2000","80365","SZT","85389099","27.12.40.0",null,"5901988805654","OE - Portes pleine IP55, H2000 x L650","OE - Plain door IP55, H2000 x W650","OE- PUERTA OPACA IP55, H2000 x W650","ZENERGY - TÖMÖR AJTÓ IP55, H2000 X W650"]
["80610","ZENERGY - DRZWI PRZESZKLONE IP55, H2000 X W1000",2102.8000000000002,"1-ZE-01",0.01,1,"OE_DOORS_2000","81110","SZT","85389099","27.12.40.0",null,"5901988806101","OE - Portes vitrée IP55, H2000 x L1000","OE - Glazed door IP55, H2000 x W1000","OE- PUERTA TRANSPARENTE IP55, H2000 x W1000","ZENERGY - ÜVEGAJTÓK IP55, H2000 X W1000"]
["80614","ZENERGY - DRZWI PRZESZKLONE IP55, H2000 X W1050",2233.4,"1-ZE-01",null,null,"OE_DOORS_2000","81114","SZT","85389099",null,null,"5901988806149","OE - Portes vitrée IP55, H2000 x L1050","OE - Glazed door IP55, H2000 x W1050","OE- PUERTA TRANSPARENTE IP55, H2000 x W1050","ZENERGY - ÜVEGAJTÓK IP55, H2000 X W1050"]
["80660","ZENERGY - DRZWI PRZESZKLONE IP55, H2000 X W600",1297.0999999999999,"1-ZE-01",null,null,"OE_DOORS_2000","81160","SZT","85389099","27.12.40.0",null,"5901988806606","OE - Portes vitrée IP55, H2000 x L600","OE - Glazed door IP55, H2000 x W600","OE- PUERTA TRANSPARENTE IP55, H2000 x W600","ZENERGY - ÜVEZETETT AJTÓK IP55, H2000 X W600"]
["80665","ZENERGY - DRZWI PRZESZKLONE IP55, H2000 X W650",1618.9,"1-ZE-01",5.8333333333333334E-2,2,"OE_DOORS_2000","81165","SZT","85389099","27.12.40.0",null,"5901988806651","OE - Portes vitrée IP55, H2000 x L650","OE - Glazed door IP55, H2000 x W650","OE- PUERTA TRANSPARENTE IP55, H2000 x W650","ZENERGY- ÜVEZETETT AJTÓK IP55, H2000 X W650"]
["80695","ZENERGY - DRZWI PRZESZKLONE IP55, H2000 X W950",1996.9,"1-ZE-01",null,null,"OE_DOORS_2000","81195","SZT","85389099",null,null,"5901988806958","OE - Portes vitrée IP55, H2000 x L950","OE - Glazed door IP55, H2000 x W950","OE- PUERTA TRANSPARENTE IP55, H2000 x W950","ZENERGY - ÜVEZETETT AJTÓK IP55, H2000 X W950"]
["80746","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 3X EFEN 160-630, H2000 X W450, 23+11M, ANALIZATORY 3X 96X96MM DO PLOMBOWANIA",694.1,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","80745","SZT","85389099",null,null,"5901988807467","OE - Cadre pivotant composé de 3 interrupteurs-sectionneurs EFEN 160-630, H2000 x L450, 23 + 11M, 3 analyseurs pour l'étanchéité","OE - Hinged frame for 3x EFEN 160-630, H2000 x W450, 23 + 11M slat switch disconnectors, 3x 96x96mm analyzers for sealing","OE- ESTR. PARA REGLETAS SECC. 3X160-630, H2000 x W450, 23+11M, ANALIZ.","ZENERGY - SZALAGOS KAPCSOLÓK DÖNTÉSE KERET 3X EFEN 160-630, H2000"]
["80785","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 7X EFEN 160-630, H2000 X W850, 23+11M, ANALIZATORY 7X 96X96MM",887.8,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","80785","SZT","85389099",null,null,"5901988807856","OE - Cadre pivotant d'interrupteurs-sectionneurs 7x EFEN 160-630, H2000 x L850, 23 + 11M, analyseurs 7x 96x96mm","OE - Hinged frame for switch disconnectors 7x EFEN 160-630, H2000 x W850, 23 + 11M, analyzers 7x 96x96mm","OE- ESTR. PARA REGLETAS SECC. 7X160-630, H2000 x W850, 23+11M, ANALIZ.","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 7X EFEN 160-630, H2000 X W850, 23+11M, ELEMZŐK 7X 96X96MM"]
["80846","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 3X EFEN 160-630, H2000 X W450, 23+13M DO PLOMBOWANIA",587.5,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","80845","SZT","85389099",null,null,"5901988808464","OE - Cadre pivotant composé de 3 interrupteurs-sectionneurs EFEN 160-630, H2000 x L450, 23 + 13M pour l'étanchéité","OE - Hinged frame for 3x EFEN 160-630, H2000 x W450, 23 + 13M slat switch disconnectors for sealing","OE- ESTR. PARA REGLETAS SECC. 3X160-630, H2000 x W450, 23+13M ","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 3X EFEN 160-630, H2000 X W450, 23+13M TÖMÍTÉSRE"]
["80886","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 7X EFEN 160-630, H2000 X W850, 23+13M DO PLOMBOWANIA",777.6,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","80885","SZT","85389099","27.12.40.0",null,"5901988808860","OE - Cadre pivotant d'interrupteurs-sectionneurs 7x EFEN 160-630, H2000 x L850, 23 + 13M pour l'étanchéité","OE - Hinged frame for switch disconnectors 7x EFEN 160-630, H2000 x W850, 23 + 13M for sealing","OE- ESTR. PARA REGLETAS SECC. 7X160-630, H2000 x W850, 23+13M ","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 7X EFEN 160-630, H2000 X W850, 23+13M TÖMÍTÉSRE"]
["80912","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W1200 + WSPORNIKI,  ( 1850 X 1100 )",1256,"1-ZE-01",0.10833333333333334,6,"OE_PLAIN_PLATES","80912","SZT","85389099","27.12.40.0",null,"5901988809126","OE - Plaque de montage complète H2000 x L1200 + supports, (1850 x 1100)","OE - Plain Mounting plate H2000 x W1200 + brackets, (1850 x 1100)","OE- PLACA MONTAJE  TOTAL CIEGA H2000 x W1200 + SOPORT. (1850 X 1100)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H2000 X W1200 + KONZEREK, (1850 X 1100)"]
["80913","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W1300 + WSPORNIKI,  ( 1850 X 1200 )",1350,"1-ZE-01",null,null,"OE_PLAIN_PLATES","80913","SZT","85389099","27.12.40.0",null,"5901988809133","OE - Plaque de montage complète H2000 x L1300 + supports, (1850 x 1200)","OE - Plain Mounting plate H2000 x W1300 + brackets, (1850 x 1200)","OE- PLACA MONTAJE  TOTAL CIEGA H2000 x W1300 + SOPORT. (1850 X 1200)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H2000 X W1300 + KONZEREK, (1850 X 1200)"]
["80940","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W400 + WSPORNIKI,  ( 1850 X 300 )",513,"1-ZE-01",1.6666666666666666E-2,2,"OE_PLAIN_PLATES","80940","SZT","85389099","27.12.40.0",null,"5901988809409","OE - Plaque de montage complète H2000 x L400 + supports, (1850 x 300)","OE - Plain Mounting plate H2000 x W400 + brackets, (1850 x 300)","OE- PLACA MONTAJE  TOTAL CIEGA H2000 x W400 + SOPORT. (1850 X 300)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H2000 X W400 + KONZEREK, (1850 X 300)"]
["80980","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W800 + WSPORNIKI,  ( 1850 X 700 )",882.4,"1-ZE-01",0.15833333333333333,7,"OE_PLAIN_PLATES","80980","SZT","85389099","27.12.40.0",null,"5901988809805","OE - Plaque de montage complète H2000 x L800 + supports, (1850 x 700)","OE - Plain Mounting plate H2000 x W800 + brackets, (1850 x 700)","OE- PLACA MONTAJE  TOTAL CIEGA H2000 x W800 + SOPORT. (1850 X 700)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H2000 X W800 + KONZEREK, (1850 X 700)"]
["80995","ZENERGY - PEŁNY ŁĄCZNIK PŁYT MONTAŻOWYCH H2000,  ( 1850 X 98 )",231.1,"1-ZE-01",0.24166666666666667,2,"OE_PLAIN_PLATES","80995","SZT","85389099","27.12.40.0",null,"5901988809959","OE - Connecteur complet pour plaques de montage H2000, (1850 x 98)","OE - Plain Mounting plate connector H2000, (1850 x 98)","OE- UNION PLACA MONTAJE  TOTAL H2000, ( 1850 X 98 )","ZENERGY - SZERELŐLEMEZEK TELJES CSATLAKOZÓJA H2000, (1850 X 98)"]
["81112","ZENERGY - DRZWI PRZESZKLONE IP30, H2000 X W1200, PODWÓJNE",2653.6,"1-ZE-01",null,null,"OE_DOORS_2000","81112","SZT","85389099",null,null,"5901988811129","OE - Portes vitrées IP30, H2000 x L1200, double vitrage","OE - Glazed door IP30, H2000 x W1200, double","OE- PUERTA TRANSP. DOBLE IP30, H2000XW1200","ZENERGY - ÜVEGAJTÓK IP30, H2000 X W1200, DUPLA"]
["81120","ZENERGY - RAMA, H2000 X D1000 X W1200",1841.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988811204","OE - Cadre, H2000 x P1000 x L1200","OE - Frame, H2000 x D1000 x H1200","*OE - Marco, H2000 x D1000 x W1200","ZENERGY - KERET, H2000 X D1000 X W1200"]
["81160","ZENERGY - DRZWI PRZESZKLONE IP30, H2000 X W600",1167.5,"1-ZE-01",null,null,"OE_DOORS_2000","81160","SZT","85389099",null,null,"5901988811600","OE - Portes vitrées IP30, H2000 x L600","OE - Glazed door IP30, H2000 x W600","OE- PUERTA TRANSP. DOBLE IP30, H2000XW600","ZENERGY - ÜVEZETETT AJTÓK IP30, H2000 X W600"]
["81185","ZENERGY - DRZWI PRZESZKLONE IP30, H2000 X W850",1705.3,"1-ZE-01",null,null,"OE_DOORS_2000","81185","SZT","85389099",null,null,"5901988811853","OE - Portes vitrées IP30, H2000 x L850","OE - Glazed door IP30, H2000 x W850","OE- PUERTA TRANSP. DOBLE IP30, H2000XW850","ZENERGY - ÜVEZETETT AJTÓK IP30, H2000 X W850"]
["81195","ZENERGY - DRZWI PRZESZKLONE IP30, H2000 X W950",1797.1,"1-ZE-01",null,null,"OE_DOORS_2000","81195","SZT","85389099",null,null,"5901988811952","OE - Portes vitrées IP30, H2000 x L950","OE - Glazed door IP30, H2000 x W950","OE- PUERTA TRANSP. DOBLE IP30, H2000XW950","ZENERGY - ÜVEZETETT AJTÓK IP30, H2000 X W950"]
["81212","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W1200",1034.5999999999999,"1-ZE-01",0.2,4,"OE_COVERS","81212","SZT","85389099","27.12.40.0",null,"5901988812126","OE - Couverture arrière complète IP30, H2000 x L1200","OE - Plain rear cover IP30, H2000 x W1200","OE- FONDO ATORNILLADO LISO IP30, H2000 x W1200","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2000 X W1200"]
["81240","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W400",396.4,"1-ZE-01",0.24166666666666667,4,"OE_COVERS","81240","SZT","85389099","27.12.40.0",null,"5901988812409","OE - Couverture arrière complète IP30, H2000 x L400","OE - Plain rear cover IP30, H2000 x W400","OE- FONDO ATORNILLADO LISO IP30, H2000 x W400","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2000 X W400"]
["81280","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W800",612.4,"1-ZE-01",0.73333333333333328,4,"OE_COVERS","81280","SZT","85389099","27.12.40.0",null,"5901988812805","OE - Couverture arrière complète IP30, H2000 x L800","OE - Plain rear cover IP30, H2000 x W800","OE- FONDO ATORNILLADO LISO IP30, H2000 x W800","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2000 X W800"]
["81310","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2000 X W1000",752.8,"1-ZE-01",5.8333333333333334E-2,2,"OE_COVERS","81310","SZT","85389099","27.12.40.0",null,"5901988813109","OE - Coque arrière ventilée IP30, H2000 x L1000","OE - Rear ventilated cover IP30, H2000 x W1000","OE- FONDO ATORNILLADO VENTIL. IP30, H2000 x W1000","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2000 X W1000"]
["81330","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2000 X W300",347.8,"1-ZE-01",0.14166666666666666,4,"OE_COVERS","81330","SZT","85389099","27.12.40.0",null,"5901988813307","OE - Hotte d'aération arrière IP30, H2000 x L300","OE - Rear ventilated cover IP30, H2000 x W300","OE- FONDO ATORNILLADO VENTIL. IP30, H2000 x W300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2000 X W300"]
["81350","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30 POLA NAROŻNEGO D400, H2000 X W500",517.29999999999995,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988813505","OE - Hotte de ventilation arrière IP30, angle en coin P400, H2000 x L500","OE - Rear ventilated cover IP30 of the corner section D400, H2000 x W500","OE- FONDO ATORNILLADO VENTILADO IP30 de la sección de la esquina D400, H2000 x W500","ZENERGY - SZELLŐZTETETT HÁTSÓ BURKOLAT IP30 SAROKTERÜLET D400, H2000 X W500"]
["81370","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30 POLA NAROŻNEGO D600, H2000 X W700",642.6,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988813703","OE - Caisson d'angle IP30 avec couvercle arrière ventilé P600, H2000 x L700","OE - Rear ventilated cover, IP30 of the corner section D600, H2000 x W700","OE- FONDO ATORNILLADO VENTILADO, IP30 de la sección de la esquina D600, H2000 x W700","ZENERGY - SZELLŐZTETETT HÁTSÓ BURKOLAT IP30 SAROKTERÜLET D600, H2000 X W700"]
["81380","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2000 X W800",682.6,"1-ZE-01",0.56666666666666665,6,"OE_COVERS","81380","SZT","85389099","27.12.40.0",null,"5901988813802","OE - Hotte d'aération arrière IP30, H2000 x L800","OE - Rear ventilated cover IP30, H2000 x W800","OE- FONDO ATORNILLADO VENTIL. IP30, H2000 x W800","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2000 X W800"]
["81390","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30 POLA NAROŻNEGO D800, H2000 X W900",762.3,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988813901","OE - COUVERCLE ARRIÈRE VENTILÉ IP30 CORNER FIELD P800, H2000 x L900","OE - Rear ventilated cover IP30 corner field D800, H2000 x W900","*OE - CUBIERTA TRASERA VENTILADA IP30 CAMPO DE ESQUINA D800, H2000 x W900","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30 SAROKTERÜLET D800, H2000 X W900"]
["81411","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2000 X W850+200",1080,"1-ZE-01",null,null,"OE_COVERS","81211","SZT","85389099",null,null,"5901988814113","OE - Coque arrière ventilée IP43, H2000 x L650 + 400","OE - Rear ventilated cover IP43, H2000 x W850 + 200","OE- FONDO ATORNILLADO VENTIL.IP43, H2000 x W650+400","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2000 X W850+200"]
["81440","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2000 X W400",591.79999999999995,"1-ZE-01",null,null,"OE_COVERS","81240","SZT","85389099","27.12.40.0",null,"5901988814403","OE - Hotte d'aération arrière IP43, H2000 x L400","OE - Rear ventilated cover IP43, H2000 x W400","OE- FONDO ATORNILLADO VENTIL.IP43, H2000 x W400","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2000 X W400"]
["81465","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2000 X W650",758.2,"1-ZE-01",5.8333333333333334E-2,4,"OE_COVERS","81465","SZT","85389099","27.12.40.0",null,"5901988814656","OE - Coque arrière ventilée IP43, H2000 x L650","OE - Rear ventilated cover IP43, H2000 x W650","OE- FONDO ATORNILLADO VENTIL.IP43, H2000 x W650","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2000 X W650"]
["81510","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2000 X W1000",874.8,"1-ZE-01",0.40833333333333333,5,"OE_COVERS","81210","SZT","85389099","27.12.40.0",null,"5901988815103","OE - Couverture arrière complète IP55, H2000 x L1000","OE - Plain rear cover IP55, H2000 x W1000","OE- FONDO ATORNILLADO LISO IP55, H2000 x W1000","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2000 X W1000"]
["81513","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2000 X W1300",1363,"1-ZE-01",null,null,"OE_COVERS",null,"SZT","85389099","27.12.40.0",null,"5901988815134","OE - Couverture arrière complète IP55, H2000 x L1300","OE - Plain rear cover IP55, H2000 x W1300","OE- FONDO ATORNILLADO LISO IP55, H2000 x W1300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2000 X W1300"]
["81545","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2000 X W450",541.1,"1-ZE-01",6.6666666666666666E-2,5,"OE_COVERS","81245","SZT","85389099","27.12.40.0",null,"5901988815455","OE - Couverture arrière complète IP55, H2000 x L450","OE - Plain rear cover IP55, H2000 x W450","OE- FONDO ATORNILLADO LISO IP55, H2000 x W450","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2000 X W450"]
["81565","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2000 X W650",680.4,"1-ZE-01",0.71666666666666667,11,"OE_COVERS","81265","SZT","85389099","27.12.40.0",null,"5901988815653","OE - Couverture arrière complète IP55, H2000 x L650","OE - Plain rear cover IP55, H2000 x W650","OE- FONDO ATORNILLADO LISO IP55, H2000 x W650","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2000 X W650"]
["81595","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2000 X W650+300",850,"1-ZE-01",null,null,"OE_COVERS","81295","SZT","85389099",null,null,"5901988815950","OE - Couverture arrière complète IP55, H2000 x L650 + 300","OE - Plain rear cover IP55, H2000 x W650 + 300","OE- FONDO ATORNILLADO LISO IP55, H2000 x W650+300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2000 X W650+300"]
["82045","ZENERGY - RAMA, H2000 X D230 X W450",778.8,"1-ZE-01",null,null,"OE_FRAME_2000","82045","SZT","85389099",null,null,"5901988820459","OE - Cradle, H2000 x P230 x L450","OE - Frame, H2000 x D230 x W450","OE- ESTRUCTURA, H2000 x D230 x W450","ZENERGY - KERET, H2000 X D230 X W450"]
["82067","ZENERGY - RAMA, H2000 X D230 X W650, 450+200",1059.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988820671","OE - Cadre, H2000 x P230 x L650, 450 + 200","OE - Frame, H2000 x D230 x W650, 450 + 200","OE- ESTRUCTURA, H2000 x D230 x W650, 450+200","ZENERGY – KERET, H2000 X D230 X W650, 450+200"]
["82085","ZENERGY - RAMA, H2000 X D230 X W850",931,"1-ZE-01",0.01,1,"OE_FRAME_2000","82085","SZT","85389099",null,null,"5901988820855","OE - Cradle, H2000 x P230 x L850","OE - Frame, H2000 x D230 x W850","OE- ESTRUCTURA, H2000 x D230 x W850","ZENERGY - KERET, H2000 X D230 X W850"]
["82100","ZENERGY - RAMA, H2000 X D230 X W1000",1010.9,"1-ZE-01",null,null,"OE_FRAME_2000","82100","SZT","85389099",null,null,"5901988821005","OE - Cradle, H2000 x P230 x L1000","OE - Frame, H2000 x D230 x W1000","OE- ESTRUCTURA, H2000 x D230 x W1000","ZENERGY - KERET, H2000 X D230 X W1000"]
["82107","ZENERGY - RAMA, H2000 X D230 X W1050, 850+200",1201.2,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821074","OE - Cadre, H2000 x P230 x L1050, 850 + 200","OE - Frame, H2000 x D230 x W1050, 850 + 200","OE- ESTRUCTURA, H2000 x D230 x W1050, 850+200","ZENERGY – KERET, H2000 X D230 X W1050, 850+200"]
["82115","ZENERGY - RAMA, H2000 X D230 X W1150, 850+300",1317.8,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821159","OE - Cadre, H2000 x P230 x L1150, 850 + 300","OE - Frame, H2000 x D230 x W1150, 850 + 300","OE- ESTRUCTURA, H2000 x D230 x W1150, 850+300","ZENERGY – KERET, H2000 X D230 X W1150, 850+300"]
["82117","ZENERGY - RAMA, H2000 X D230 X W1150, 200+650+300",1515.8,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821173","OE - Cadre, H2000 x P230 x L1150, 200 + 650 + 300","OE - Frame, H2000 x D230 x W1150, 200 + 650 + 300","OE- ESTRUCTURA, H2000 x D230 x W1150, 200+650+300","ZENERGY – KERET, H2000 X D230 X W1150, 200+650+300"]
["82122","ZENERGY - RAMA, H2000 X D230 X W1200, 150+450+450+150",1731.4,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821227","OE - Cadre, H2000 x P230 x L1200, 150 + 450 + 450 + 150","OE - Frame, H2000 x D230 x W1200, 150 + 450 + 450 + 150","OE- ESTRUCTURA, H2000 x D230 x W1200, 150+450+450+150","ZENERGY - KERET, H2000 X D230 X W1200, 150+450+450+150"]
["82127","ZENERGY - RAMA, H2000 X D230 X W1250, 200+650+400",1538.9,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821272","OE - Cadre, H2000 x P230 x L1250, 200 + 650 + 400","OE - Frame, H2000 x D230 x W1250, 200 + 650 + 400","OE- ESTRUCTURA, H2000 x D230 x W1250, 200+650+400","ZENERGY – KERET, H2000 X D230 X W1250, 200+650+400"]
["82132","ZENERGY - RAMA, H2000 X D230 X W1300, 650+200+450",1584,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821326","OE - Cadre, H2000 x P230 x L1300, 650 + 200 + 450","OE - Frame, H2000 x D230 x W1300, 650 + 200 + 450","OE- ESTRUCTURA, H2000 x D230 x W1300, 650+200+450","ZENERGY – KERET, H2000 X D230 X W1300, 650+200+450"]
["82145","ZENERGY - RAMA, H2000 X D230 X W1450, 650+150+650",1633.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821456","OE - Cadre, H2000 x P230 x P1450, 650 + 150 + 650","OE - Frame, H2000 x D230 x W1450, 650 + 150 + 650","OE- ESTRUCTURA, H2000 x D230 x W1450, 650+150+650","ZENERGY – KERET, H2000 X D230 X W1450, 650+150+650"]
["82152","ZENERGY - RAMA, H2000 X D230 X W1500, 200+650+650",1637.9,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821524","OE - Cadre, H2000 x P230 x L1500, 200 + 650 + 650","OE - Frame, H2000 x D230 x W1500, 200 + 650 + 650","OE- ESTRUCTURA, H2000 x D230 x W1500, 200+650+650","ZENERGY – KERET, H2000 X D230 X W1500, 200+650+650"]
["82162","ZENERGY - RAMA, H2000 X D230 X W1600, 150+650+800",1692.9,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821623","OE - Cadre, H2000 x P230 x L1600, 150 + 650 + 800","OE - Frame, H2000 x D230 x W1600, 150 + 650 + 800","OE- ESTRUCTURA, H2000 x D230 x W1600, 150+650+800","ZENERGY – KERET, H2000 X D230 X W1600, 150+650+800"]
["82166","ZENERGY - RAMA, H2000 X D230 X W1650, 1000+650",1515.8,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821661","OE - Cadre, H2000 x P230 x L1650, 1000 + 650","OE - Frame, H2000 x D230 x W1650, 1000 + 650","OE- ESTRUCTURA, H2000 x D230 x W1650, 1000+650","ZENERGY - KERET, MA, H2000 X D230 X W1650, 1000+650"]
["82169","ZENERGY - RAMA, H2000 X D230 X W1650, 200+650+800",1697.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821692","OE - Cadre, H2000 x P230 x L1650, 200 + 650 + 800","OE - Frame, H2000 x D230 x W1650, 200 + 650 + 800","OE- ESTRUCTURA, H2000 x D230 x W1650, 200+650+800","ZENERGY – KERET, H2000 X D230 X W1650, 200+650+800"]
["82172","ZENERGY - RAMA, H2000 X D230 X W1700, 650+650+400",1794.1,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821722","OE - Cadre, H2000 x P230 x L1700, 650 + 650 + 400","OE - Frame, H2000 x D230 x W1700, 650 + 650 + 400","OE- ESTRUCTURA, H2000 x D230 x W1700, 650+650+400","ZENERGY – KERET, H2000 X D230 X W1700, 650+650+400"]
["82197","ZENERGY - RAMA, H2000 X D230 X W2000, 850+300+850",1855.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988821975","OE - Cadre, H2000 x P230 x L2000, 850 + 300 + 850","OE - Frame, H2000 x D230 x W2000, 850 + 300 + 850","OE- ESTRUCTURA, H2000 x D230 x W2000, 850+300+850","ZENERGY – KERET, H2000 X D230 X W2000, 850+300+850"]
["83060","ZENERGY - RAMA, H2000 X D300 X W600",873.7,"1-ZE-01",0.01,1,"OE_FRAME_2000","83060","SZT","85389099",null,null,"5901988830601","OE - Cadre, H2000 x P300 x P600","OE - Frame, H2000 x D300 x W600","OE- ESTRUCTURA, H2000 x D300 x W600","ZENERGY - KERET, H2000 X D300 X W600"]
["83067","ZENERGY - RAMA, H2000 X D300 X W650, 450+200",1131.9000000000001,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988830670","OE - Cadre, H2000 x P300 x L650, 450 + 200","OE - Frame, H2000 x D300 x W650, 450 + 200","OE- ESTRUCTURA, H2000 x D300 x W650, 450+200","ZENERGY – KERET, H2000 X D300 X W650, 450+200"]
["83086","ZENERGY - RAMA, H2000 X D300 X W850, 650+200",1194.5999999999999,"1-ZE-01",null,null,"OE_FRAME_2000","83086","SZT","85389099",null,null,"5901988830861","OE - Cadre, H2000 x P300 x P850, 650 + 200","OE - Frame, H2000 x D300 x W850, 650 + 200","OE- ESTRUCTURA, H2000 x D300 x W850, 650+200","ZENERGY – KERET, H2000 X D300 X W850, 650+200"]
["83096","ZENERGY - RAMA, H2000 X D300 X W950, 400+400+150",1580.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988830960","OE - Cadre, H2000 x P300 x L950, 400 + 400 + 150","OE - Frame, H2000 x D300 x W950, 400 + 400 + 150","OE- ESTRUCTURA, H2000 x D300 x W950, 400+400+150","ZENERGY – KERET, H2000 X D300 X W950, 400+400+150"]
["83100","ZENERGY - RAMA, H2000 X D300 X W1000",1040,"1-ZE-01",3.3333333333333333E-2,4,"OE_FRAME_2000","83100","KPL","85389099",null,null,"5901988831004","OE - Cradle, H2000 x P300 x L1000","OE - Frame, H2000 x D300 x W1000","OE- ESTRUCTURA, H2000 x D300 x W1000","ZENERGY - KERET, H2000 X D300 X W1000"]
["83107","ZENERGY - RAMA, H2000 X D300 X W1050, 850+200",1273.8,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831073","OE - Cadre, H2000 x P300 x P1050, 850 + 200","OE - Frame, H2000 x D300 x W1050, 850 + 200","OE- ESTRUCTURA, H2000 x D300 x W1050, 850+200","ZENERGY – KERET, H2000 X D300 X W1050, 850+200"]
["83115","ZENERGY - RAMA, H2000 X D300 X W1150, 850+300",1400.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831158","OE - Cadre, H2000 x P300 x P1150, 850 + 300","OE - Frame, H2000 x D300 x W1150, 850 + 300","OE- ESTRUCTURA, H2000 x D300 x W1150, 850+300","ZENERGY – KERET, H2000 X D300 X W1150, 850+300"]
["83122","ZENERGY - RAMA, H2000 X D300 X W1200, 150+450+450+150",1862.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831226","OE - Cadre, H2000 x P300 x P1200, 150 + 450 + 450 + 150","OE - Frame, H2000 x D300 x W1200, 150 + 450 + 450 + 150","OE- ESTRUCTURA, H2000 x D300 x W1200, 150+450+450+150","ZENERGY – KERET, H2000 X D300 X W1200, 150+450+450+150"]
["83126","ZENERGY - RAMA, H2000 X D300 X W1250, 650+200+400",1645.6,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831264","OE - Cadre, H2000 x P300 x P1250, 650 + 200 + 400","OE - Frame, H2000 x D300 x W1250, 650 + 200 + 400","OE- ESTRUCTURA, H2000 x D300 x W1250, 650+200+400","ZENERGY – KERET, H2000 X D300 X W1250, 650+200+400"]
["83131","ZENERGY - RAMA, H2000 X D300 X W1300, 650+650",1486.1,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831318","OE - Cadre, H2000 x P300 x P1300, 650 + 650","OE - Frame, H2000 x D300 x W1300, 650 + 650","OE- ESTRUCTURA, H2000 x D300 x W1300, 650+650","ZENERGY - KERET, H2000 X D300 X W1300, 650+650"]
["83145","ZENERGY - RAMA, H2000 X D300 X W1450, 650+150+650",1740.2,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831455","OE - Cadre, H2000 x P300 x P1450, 650 + 150 + 650","OE - Frame, H2000 x D300 x W1450, 650 + 150 + 650","OE- ESTRUCTURA, H2000 x D300 x W1450, 650+150+650","ZENERGY – KERET, H2000 X D300 X W1450, 650+150+650"]
["83151","ZENERGY - RAMA, H2000 X D300 X W1500, 650+200+650",1745.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831516","OE - Cadre, H2000 x P300 x P1500, 650 + 200 + 650","OE - Frame, H2000 x D300 x W1500, 650 + 200 + 650","OE- ESTRUCTURA, H2000 x D300 x W1500, 650+200+650","ZENERGY – KERET, H2000 X D300 X W1500, 650+200+650"]
["83152","ZENERGY - RAMA, H2000 X D300 X W1500, 200+650+650",1745.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831523","OE - Cadre, H2000 x P300 x P1500, 200 + 650 + 650","OE - Frame, H2000 x D300 x W1500, 200 + 650 + 650","OE- ESTRUCTURA, H2000 x D300 x W1500, 200+650+650","ZENERGY – KERET, H2000 X D300 X W1500, 200+650+650"]
["83162","ZENERGY - RAMA, H2000 X D300 X W1600, 150+650+800",1800.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831622","OE - Cadre, H2000 x P300 x P1600, 150 + 650 + 800","OE - Frame, H2000 x D300 x W1600, 150 + 650 + 800","OE- ESTRUCTURA, H2000 x D300 x W1600, 150+650+800","ZENERGY – KERET, H2000 X D300 X W1600, 150+650+800"]
["83166","ZENERGY - RAMA, H2000 X D300 X W1650, 1000+650",1598.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831660","OE - Cadre, H2000 x P300 x P1650, 1000 + 650","OE - Frame, H2000 x D300 x W1650, 1000 + 650","OE- ESTRUCTURA, H2000 x D300 x W1650, 1000+650","ZENERGY – KERET, H2000 X D300 X W1650, 1000+650"]
["83172","ZENERGY - RAMA, H2000 X D300 X W1700, 650+650+400",1910.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831721","OE - Cadre, H2000 x P300 x P1700, 650 + 650 + 400","OE - Frame, H2000 x D300 x W1700, 650 + 650 + 400","OE- ESTRUCTURA, H2000 x D300 x W1700, 650+650+400","ZENERGY – KERET, H2000 X D300 X W1700, 650+650+400"]
["83187","ZENERGY - RAMA, H2000 X D300 X W1850, 1000+850",1662.1,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988831875","OE - Cadre, H2000 x P300 x L1850, 1000 + 850","OE - Frame, H2000 x D300 x W1850, 1000 + 850","OE- ESTRUCTURA, H2000 x D300 x W1850, 1000+850","ZENERGY – KERET, H2000 X D300 X W1850, 1000+850"]
["84040","ZENERGY - RAMA, H2000 X D400 X W400",777.6,"1-ZE-01",8.3333333333333329E-2,5,"OE_FRAME_2000","84040","SZT","85389099","27.12.40.0",null,"5901988840402","OE - Cradle, H2000 x P400 x P400","OE - Frame, H2000 x D400 x W400","OE- ESTRUCTURA, H2000 x D400 x W400","ZENERGY - KERET, H2000 X D400 X W400"]
["84065","ZENERGY - RAMA, H2000 X D400 X W650",874.8,"1-ZE-01",0.29166666666666669,12,"OE_FRAME_2000","84065","SZT","85389099","27.12.40.0",null,"5901988840655","OE - Cradle, H2000 x P400 x P650","OE - Frame, H2000 x D400 x W650","OE- ESTRUCTURA, H2000 x D400 x W650","ZENERGY - KERET, H2000 X D400 X W650"]
["84076","ZENERGY - RAMA, H2000 X D400 X W750, 450+300",1236.5999999999999,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988840761","OE - CADRE, H2000 x P400 x L750, 450+300","OE - Frame, H2000 x D400 x H750, 450+300","*OE - MARCO, H2000 x D400 x W750, 450+300","ZENERGY – KERET, H2000 X D400 X W750, 450+300"]
["84085","ZENERGY - RAMA, H2000 X D400 X W850",951.5,"1-ZE-01",0.29166666666666669,10,"OE_FRAME_2000","84085","SZT","8538909900","27.12.40.0",null,"5901988840853","OE - Cradle, H2000 x P400 x P850","OE - Frame, H2000 x D400 x W850","OE- ESTRUCTURA, H2000 x D400 x W850","ZENERGY - KERET, H2000 X D400 X W850"]
["84091","ZENERGY - RAMA, H2000 X D400 X W900, 450+450",1421.9,"1-ZE-01",1.6666666666666666E-2,2,"OE_FRAME_2000",null,null,"85389099",null,null,"5901988840914"]
["84097","ZENERGY - RAMA, H2000 X D400 X W950, 800+150",1303.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988840976","OE - CADRE, H2000 x P400 x L950, 800+150","OE - Frame, H2000 x D400 x H950, 800+150","*OE - MARCO, H2000 x D400 x W950, 800+150","ZENERGY – KERET, H2000 X D400 X W950, 800+150"]
["84107","ZENERGY - RAMA, H2000 X D400 X W1050, 850+200",1249.5999999999999,"1-ZE-01",null,null,"OE_FRAME_2000","84107","SZT","85389099","27.12.40.0",null,"5901988841072","OE - Cadre, H2000 x P400 x P1050, 850 + 200","OE - Frame, H2000 x D400 x W1050, 850 + 200","OE- ESTRUCTURA, H2000 x D400 x W1050, 850+200","ZENERGY – KERET, H2000 X D400 X W1050, 850+200"]
["84111","ZENERGY - RAMA, H2000 X D400 X W1100, 650+450",1306.8,"1-ZE-01",0.01,1,"OE_FRAME_2000","84111","SZT","85389099","27.12.40.0",null,"5901988841119","OE - Cadre, H2000 x P400 x P1100, 650 + 450","OE - Frame, H2000 x D400 x W1100, 650 + 450","OE- ESTRUCTURA, H2000 x D400 x W1100, 650+450","ZENERGY – KERET, H2000 X D400 X W1100, 650+450"]
["84121","ZENERGY - RAMA, H2000 X D400 X W1200, 150+650+400",1567.1,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099","27.12.40.0",null,"5901988841218","OE - Cadre, H2000 x P400 x P1200, 150 + 650 + 400","OE - Frame, H2000 x D400 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H2000 x D400 x W1200, 150+650+400","ZENERGY – KERET, H2000 X D400 X W1200, 150+650+400"]
["84125","ZENERGY - RAMA, H2000 X D400 X W1250, 850+400",1360.8,"1-ZE-01",8.3333333333333329E-2,4,"OE_FRAME_2000","84125","SZT","85389099",null,null,"5901988841256","OE - Cadre, H2000 x P400 x P1250, 850 + 400","OE - Frame, H2000 x D400 x W1250, 850 + 400","OE- ESTRUCTURA, H2000 x D400 x W1250, 850+400","ZENERGY – KERET, H2000 X D400 X W1250, 850+400"]
["84128","ZENERGY - RAMA, H2000 X D400 X W1250, 650+150+450",1606,"1-ZE-01",0.01,1,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841287","OE - CADRE, H2000 x P400 x L1250, 650+150+450","OE - Frame, H2000 x D400 x H1250, 650+150+450","*OE - MARCO, H2000 x D400 x W1250, 650+150+450","ZENERGY – KERET, H2000 X D400 X W1250, 650+150+450"]
["84129","OE - Rama, H2000 x D400 x W1200, słupek 74mm",1199,"1-ZE-01",null,null,"OE_FRAME_2000","84129","SZT",null,null,"240801RT","5901988841294","OE - Cadre, H2000 x P400 x P1200, poteau de cadre 74mm","OE - Frame, H2000 x D400 x W1200, frame post 74mm","OE- ESTRUCTURA, H2000 x D400 x W1200, poste del marco 74mm","OE – keret, H2000 x D400 x 1200, oszlop 74 mm"]
["84132","ZENERGY - RAMA, H2000 X D400 X W1300, 650+200+450",1642.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841324","OE - Cadre, H2000 x P400 x P1300, 650 + 200 + 450","OE - Frame, H2000 x D400 x W1300, 650 + 200 + 450","OE- ESTRUCTURA, H2000 x D400 x W1300, 650+200+450","ZENERGY – KERET, H2000 X D400 X W1300, 650+200+450"]
["84144","ZENERGY - RAMA, H2000 X D400 X W1450, 850+150+450",0,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841447","OE - CADRE, H2000 x P400 x L1450, 850+150+450","OE - Frame, H2000 x D400 x H1450, 850+150+450","*OE - MARCO, H2000 x D400 x W1450, 850+150+450","ZENERGY – KERET, H2000 X D400 X W1450, 850+150+450"]
["84150","ZENERGY - RAMA, H2000 X D400 X W1500, 650+850",1451.5,"1-ZE-01",null,null,"OE_FRAME_2000","84150","SZT","85389099",null,null,"5901988841508","OE - Cadre, H2000 x P400 x P1500, 650 + 850","OE - Frame, H2000 x D400 x W1500, 650 + 850","OE- ESTRUCTURA, H2000 x D400 x W1500, 650+850","ZENERGY – KERET, H2000 X D400 X W1500, 650+850"]
["84160","ZENERGY - RAMA, H2000 X D400 X W1600, 800+800",1424.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841607","OE - Cadre, H2000 x P400 x L1600, 800 + 800","OE - Frame, H2000 x D400 x W1600, 800 + 800","OE- ESTRUCTURA, H2000 x D400 x W1600, 800+800","ZENERGY – KERET, H2000 X D400 X W1600, 800+800"]
["84165","ZENERGY - RAMA, H2000 X D400 X W1650, 650+150+850",1761.1,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841652","OE - Cadre, H2000 x P400 x P1650, 650 + 150 + 850","OE - Frame, H2000 x D400 x W1650, 650 + 150 + 850","OE- ESTRUCTURA, H2000 x D400 x W1650, 650+150+850","ZENERGY – KERET, H2000 X D400 X W1650, 650+150+850"]
["84170","ZENERGY - RAMA, H2000 X D400 X W1700, 850+850",1552.1,"1-ZE-01",null,null,"OE_FRAME_2000","84170","SZT","85389099",null,null,"5901988841706","OE - Cadre, H2000 x P400 x P1700, 850 + 850","OE - Frame, H2000 x D400 x W1700, 850 + 850","OE- ESTRUCTURA, H2000 x D400 x W1700, 850+850","ZENERGY – KERET, H2000 X D400 X W1700, 850+850"]
["84173","ZENERGY - RAMA, H2000 X D400 X W1700, 850+200+650",1765.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841737","OE - Cadre, H2000 x P400 x P1700, 850 + 200 + 650","OE - Frame, H2000 x D400 x W1700, 850 + 200 + 650","OE- ESTRUCTURA, H2000 x D400 x W1700, 850+200+650","ZENERGY – KERET, H2000 X D400 X W1700, 850+200+650"]
["84181","ZENERGY - RAMA, H2000 X D400 X W1800, 650+150+850+150",2036.1,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988841812","OE - Cadre, H2000 x P400 x L1800, 650 + 150 + 850 + 150","OE - Frame, H2000 x D400 x W1800, 650 + 150 + 850 + 150","OE- ESTRUCTURA, H2000 x D400 x W1800, 650+150+850+150","ZENERGY – KERET, H2000 X D400 X W1800, 650+150+850+150"]
["85145","OE - Rama osłon czołowych na zawiasach H2000 W450",309.10000000000002,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","85145","SZT",null,null,"230524LK","5901988851453","OE - Cadre de charnière avant à charnière H2000 L450","OE - Frame of hinged Front covers H2000 W450","OE- MARCO PIVOTANTE H2000 W450","OE - Csuklós első burkolatok kerete H2000 W450"]
["85340","ZENERGY - DRZWI PRZEDZIAŁU KABLOWEGO IP30, H2000 X W400",316.39999999999998,"1-ZE-01",5.8333333333333334E-2,4,"OE_FRAME_INTERNAL","85340","SZT","85389099",null,null,"5901988853402","OE - Portes du compartiment à câbles IP30, H2000 x L400","OE - Cable compartment door IP30, H2000 x W400","OE- PUERTA PARA MOD. CABLES IP30, H2000 x W400","ZENERGY - KÁBELREKESZ AJTÓ IP30, H2000 X W400"]
["86040","ZENERGY - RAMA, H2000 X D600 X W400",991.4,"1-ZE-01",3.3333333333333333E-2,2,"OE_FRAME_2000","86040","SZT","85389099","27.12.40.0",null,"5901988860400","OE - Cadre, H2000 x P600 x L400","OE - Frame, H2000 x D600 x W400","OE- ESTRUCTURA, H2000 x D600 x W400","ZENERGY - KERET, H2000 X D600 X W400"]
["86062","ZENERGY - RAMA, H2000 X D600 X W600, 400+200",1548.8,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988860622","OE - CADRE, H2000 X P600 X L600, 400+200","OE - Frame, H2000 x D600 x H600, 400+200","*OE - MARCO, H2000 x D600 x W600, 400+200","ZENERGY – KERET, H2000 X D600 X W600, 400+200"]
["86070","ZENERGY - RAMA, H2000 X D600 X W700 SASIL",1272.7,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988860707","OE - Cradle, H2000 x P600 x L650 Sasil","OE - Frame, H2000 x D600 x W700 Sasil","OE- ESTRUCTURA, H2000 x D600 x W700 Sasil","ZENERGY - KERET, H2000 X D600 X W700 SASIL"]
["86080","ZENERGY - RAMA, H2000 X D600 X W800",1351.1,"1-ZE-01",0.13333333333333333,7,"OE_FRAME_2000","86080","SZT","85389099","27.12.40.0",null,"5901988860806","OE - Cadre, H2000 x P600 x L800","OE - Frame, H2000 x D600 x W800","OE- ESTRUCTURA, H2000 x D600 x W800","ZENERGY - KERET, H2000 X D600 X W800"]
["86085","ZENERGY - RAMA, H2000 X D600 X W850",1304.5999999999999,"1-ZE-01",0.30833333333333335,11,"OE_FRAME_2000","86085","SZT","85389099","27.12.40.0",null,"5901988860851","OE - Cadre, H2000 x P600 x L850","OE - Frame, H2000 x D600 x W850","OE- ESTRUCTURA, H2000 x D600 x W850","ZENERGY - KERET, H2000 X D600 X W850"]
["86086","ZENERGY - RAMA, H2000 X D600 X W850, 650+200",1651.3,"1-ZE-01",null,null,"OE_FRAME_2000","86086","SZT","85389099","27.12.40.0",null,"5901988860868","OE - Cadre, H2000 x P600 x L850, 650 + 200","OE - Frame, H2000 x D600 x W850, 650 + 200","OE- ESTRUCTURA, H2000 x D600 x W850, 650+200","ZENERGY – KERET, H2000 X D600 X W850, 650+200"]
["86096","ZENERGY - RAMA, H2000 X D600 X W950, 400+400+150",2184.6,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988860967","OE - Cadre, H2000 x P600 x L950, 400 + 400 + 150","OE - Frame, H2000 x D600 x W950, 400 + 400 + 150","OE- ESTRUCTURA, H2000 x D600 x W950, 400+400+150","ZENERGY – KERET, H2000 X D600 X W950, 400+400+150"]
["86102","ZENERGY - RAMA, H2000 X D600 X W1000, 850+150",1742,"1-ZE-01",1.6666666666666666E-2,2,"OE_FRAME_2000","86102","SZT","85389099",null,null,"5901988861025","OE - Cadre, H2000 x P600 x L1000, 850 + 150","OE - Frame, H2000 x D600 x W1000, 850 + 150","OE- ESTRUCTURA, H2000 x D600 x W1000, 850+150","ZENERGY – KERET, H2000 X D600 X W1000, 850+150"]
["86106","ZENERGY - RAMA, H2000 X D600 X W1050, 200+650+200",2125.1999999999998,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861063","OE - Cadre, H2000 x P600 x L1050, 200 + 650 + 200","OE - Frame, H2000 x D600 x W1050, 200 + 650 + 200","OE- ESTRUCTURA, H2000 x D600 x W1050, 200+650+200","ZENERGY – KERET, H2000 X D600 X W1050, 200+650+200"]
["86111","ZENERGY - RAMA, H2000 X D600 X W1100, 650+450",1796,"1-ZE-01",1.6666666666666666E-2,1,"OE_FRAME_2000","86111","SZT","85389099",null,null,"5901988861117","OE - Cadre, H2000 x P600 x L1100, 650 + 450","OE - Frame, H2000 x D600 x W1100, 650 + 450","OE- ESTRUCTURA, H2000 x D600 x W1100, 650+450","ZENERGY – KERET, H2000 X D600 X W1100, 650+450"]
["86117","ZENERGY - RAMA, H2000 X D600 X W1150, 200+650+300",2227.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861179","OE - Cadre, H2000 x P600 x L1150, 200 + 650 + 300","OE - Frame, H2000 x D600 x W1150, 200 + 650 + 300","OE- ESTRUCTURA, H2000 x D600 x W1150, 200+650+300","ZENERGY – KERET, H2000 X D600 X W1150, 200+650+300"]
["86122","ZENERGY - RAMA, H2000 X D600 X W1200, 150+450+450+150",2624.6,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861223","OE - Cadre, H2000 x P600 x L1200, 150 + 450 + 450 + 150","OE - Frame, H2000 x D600 x W1200, 150 + 450 + 450 + 150","OE- ESTRUCTURA, H2000 x D600 x W1200, 150+450+450+150","ZENERGY – KERET, H2000 X D600 X W1200, 150+450+450+150"]
["86125","ZENERGY - RAMA, H2000 X D600 X W1250, 850+400",1856.5,"1-ZE-01",null,null,"OE_FRAME_2000","86125","SZT","85389099",null,null,"5901988861254","OE - Cadre, H2000 x P600 x L1250, 850 + 400","OE - Frame, H2000 x D600 x W1250, 850 + 400","OE- ESTRUCTURA, H2000 x D600 x W1250, 850+400","ZENERGY – KERET, H2000 X D600 X W1250, 850+400"]
["86126","ZENERGY - RAMA, H2000 X D600 X W1250, 650+200+400",2251.6999999999998,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861261","OE - Cadre, H2000 x P600 x L1250, 650 + 200 + 400","OE - Frame, H2000 x D600 x W1250, 650 + 200 + 400","OE- ESTRUCTURA, H2000 x D600 x W1250, 650+200+400","ZENERGY – KERET, H2000 X D600 X W1250, 650+200+400"]
["86129","OE - Rama, H2000 x D600 x W1200, słupek 74mm",1496,"1-ZE-01",null,null,"OE_FRAME_2000","86129","SZT",null,null,"240801RT","5901988861292","OE - Cadre, H2000 x P600 x L1200, poteau de cadre 74mm","OE - Frame, H2000 x D600 x W1200, frame post 74mm","OE- ESTRUCTURA, H2000 x D600 x W1200, poste del marco 74mm","OE - keret, H2000 x D600 x W1200, oszlop 74 mm"]
["86133","ZENERGY - RAMA, H2000 X D600 X W1300, 850+450",1904,"1-ZE-01",0.05,2,"OE_FRAME_2000","86133","SZT","85389099",null,null,"5901988861339","OE - Cadre, H2000 x P600 x L1300, 850 + 450","OE - Frame, H2000 x D600 x W1300, 850 + 450","OE- ESTRUCTURA, H2000 x D600 x W1300, 850+450","ZENERGY – KERET, H2000 X D600 X W1300, 850+450"]
["86144","ZENERGY - RAMA, H2000 X D600 X W1450, 850+150+450",2333.9,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861445","OE - CADRE, H2000 X P600 x L1450, 850+150+450","OE - Frame, H2000 x D600 x H1450, 850+150+450","*OE - MARCO, H2000 x D600 x W1450, 850+150+450","ZENERGY – KERET, H2000 X D600 X W1450, 850+150+450"]
["86147","ZENERGY - RAMA, H2000 X D600 X W1450, 150+650+650",2308,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861476","OE - Cadre, H2000 x P600 x L1450, 150 + 650 + 650","OE - Frame, H2000 x D600 x W1450, 150 + 650 + 650","OE- ESTRUCTURA, H2000 x D600 x W1450, 150+650+650","ZENERGY – KERET, H2000 X D600 X W1450, 150+650+650"]
["86151","ZENERGY - RAMA, H2000 X D600 X W1500, 650+200+650",2312.3000000000002,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861513","OE - Cadre, H2000 x P600 x L1500, 650 + 200 + 650","OE - Frame, H2000 x D600 x W1500, 650 + 200 + 650","OE- ESTRUCTURA, H2000 x D600 x W1500, 650+200+650","ZENERGY – KERET, H2000 X D600 X W1500, 650+200+650"]
["86160","ZENERGY - RAMA, H2000 X D600 X W1600, 800+800",1606,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861605","OE - Cadre, H2000 x P600 x L1600, 800 + 800","OE - Frame, H2000 x D600 x W1600, 800 + 800","OE- ESTRUCTURA, H2000 x D600 x W1600, 800+800","ZENERGY – KERET, H2000 X D600 X W1600, 800+800"]
["86161","ZENERGY - RAMA, H2000 X D600 X W1600, 1200+400",1963.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861612","OE - Cadre, H2000 x P600 x L1600, 1200 + 400","OE - Frame, H2000 x D600 x W1600, 1200 + 400","OE- ESTRUCTURA, H2000 x D600 x W1600, 1200+400","ZENERGY – KERET, H2000 X D600 X W1600, 1200+400"]
["86166","ZENERGY - RAMA, H2000 X D600 X W1650, 1000+650",2055.9,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861667","OE - Cadre, H2000 x P600 x L1650, 1000 + 650","OE - Frame, H2000 x D600 x W1650, 1000 + 650","OE- ESTRUCTURA, H2000 x D600 x W1650, 1000+650","ZENERGY – KERET, H2000 X D600 X W1650, 1000+650"]
["86170","ZENERGY - RAMA, H2000 X D600 X W1700, 850+850",2075.6999999999998,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861704","OE - Cadre, H2000 x P600 x L1700, 850 + 850","OE - Frame, H2000 x D600 x W1700, 850 + 850","OE- ESTRUCTURA, H2000 x D600 x W1700, 850+850","ZENERGY – KERET, H2000 X D600 X W1700, 850+850"]
["86174","ZENERGY - RAMA, H2000 X D600 X W1700, 650+200+650+200",2798.4,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861742","OE - Cadre, H2000 x P600 x L1700, 650 + 200 + 650 + 200","OE - Frame, H2000 x D600 x W1700, 650 + 200 + 650 + 200","OE- ESTRUCTURA, H2000 x D600 x W1700, 650+200+650+200","ZENERGY – KERET, H2000 X D600 X W1700, 650+200+650+200"]
["86187","ZENERGY - RAMA, H2000 X D600 X W1850, 1000+850",2120.8000000000002,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988861872","OE - Cadre, H2000 x P600 x L1850, 1000 + 850","OE - Frame, H2000 x D600 x W1850, 1000 + 850","OE- ESTRUCTURA, H2000 x D600 x W1850, 1000+850","ZENERGY – KERET, H2000 X D600 X W1850, 1000+850"]
["86221","ZENERGY - RAMA, H2000 X D600 X W1200, 400+400+400",2410.6,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988862213","OE - CADRE, H2000 X P600 X L1200, 400+400+400","OE - Frame, H2000 x D600 x H1200, 400+400+400","*OE - MARCO, H2000 x D600 x W1200, 400+400+400","ZENERGY – KERET, H2000 X D600 X W1200, 400+400+400"]
["88060","OE - Rama, H2000 x D800 x W600",1243.4000000000001,"1-ZE-01",9.166666666666666E-2,4,"OE_FRAME_2000","88060","SZT",null,null,null,"5901988880606","OE - Cadre, H2000 x P800 x L600","OE - Frame, H2000 x D800 x W600","OE- ESTRUCTURA, H2000 x D800 x W600","OE – keret, H2000 x D800 x H600"]
["88065","ZENERGY - RAMA, H2000 X D800 X W650",1340.9,"1-ZE-01",0.13333333333333333,6,"OE_FRAME_2000","88065","SZT","85389099","27.12.40.0",null,"5901988880651","OE - Cradle, H2000 x P800 x L650","OE - Frame, H2000 x D800 x W650","OE- ESTRUCTURA, H2000 x D800 x W650","ZENERGY - KERET, H2000 X D800 X W650"]
["88067","ZENERGY - RAMA, H2000 X D800 X W650, 450+200",1799.8,"1-ZE-01",null,null,"OE_FRAME_2000","88067","SZT","85389099",null,null,"5901988880675","OE - Cadre, H2000 x P800 x L650, 450 + 200","OE - Frame, H2000 x D800 x W650, 450 + 200","OE- ESTRUCTURA, H2000 x D800 x W650, 450+200","ZENERGY – KERET, H2000 X D800 X W650, 450+200"]
["88080","ZENERGY - RAMA, H2000 X D800 X W800",1406.9,"1-ZE-01",0.1,5,"OE_FRAME_2000","88080","SZT","85389099",null,null,"5901988880804","OE - Cradle, H2000 x P800 x L800","OE - Frame, H2000 x D800 x W800","OE- ESTRUCTURA, H2000 x D800 x W800","ZENERGY - KERET, H2000 X D800 X W800"]
["88086","ZENERGY - RAMA, H2000 X D800 X W850, 650+200",1832.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_FRAME_2000","88086","SZT","85389099","27.12.40.0",null,"5901988880866","OE - Cadre, H2000 x P800 x L850, 650 + 200","OE - Frame, H2000 x D800 x W850, 650 + 200","OE- ESTRUCTURA, H2000 x D800 x W850, 650+200","ZENERGY – KERET, H2000 X D800 X W850, 650+200"]
["88102","ZENERGY - RAMA, H2000 X D800 X W1000, 850+150",1925,"1-ZE-01",0.01,1,"OE_FRAME_2000","88102","SZT","85389099",null,null,"5901988881023","OE - Cadre, H2000 x P800 x L1000, 850 + 150","OE - Frame, H2000 x D800 x W1000, 850 + 150","OE- ESTRUCTURA, H2000 x D800 x W1000, 850+150","ZENERGY – KERET, H2000 X D800 X W1000, 850+150"]
["88107","ZENERGY - RAMA, H2000 X D800 X W1050, 850+200",1914,"1-ZE-01",null,null,"OE_FRAME_2000","88107","SZT","85389099",null,null,"5901988881078","OE - Cadre, H2000 x P800 x L1050, 850 + 200","OE - Frame, H2000 x D800 x W1050, 850 + 200","OE- ESTRUCTURA, H2000 x D800 x W1050, 850+200","ZENERGY – KERET, H2000 X D800 X W1050, 850+200"]
["88115","ZENERGY - RAMA, H2000 X D800 X W1150, 850+300",1998.7,"1-ZE-01",5.8333333333333334E-2,2,"OE_FRAME_2000","88115","SZT","85389099",null,null,"5901988881153","OE - Cadre, H2000 x P800 x L1150, 850 + 300","OE - Frame, H2000 x D800 x W1150, 850 + 300","OE- ESTRUCTURA, H2000 x D800 x W1150, 850+300","ZENERGY – KERET, H2000 X D800 X W1150, 850+300"]
["88122","ZENERGY - RAMA, H2000 X D800 X W1200, 150+450+450+150",2925.4,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881221","OE - Cadre, H2000 x P800 x L1200, 150 + 450 + 450 + 150","OE - Frame, H2000 x D800 x W1200, 150 + 450 + 450 + 150","OE- ESTRUCTURA, H2000 x D800 x W1200, 150+450+450+150","ZENERGY - KERET, H2000 X D800 X W1200, 150+450+450+150"]
["88126","ZENERGY - RAMA, H2000 X D800 X W1250, 650+200+400",2495.4,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881269","OE - Cadre, H2000 x P800 x L1250, 650 + 200 + 400","OE - Frame, H2000 x D800 x W1250, 650 + 200 + 400","OE- ESTRUCTURA, H2000 x D800 x W1250, 650+200+400","ZENERGY – KERET, H2000 X D800 X W1250, 650+200+400"]
["88127","ZENERGY - RAMA, H2000 X D800 X W1250, 200+650+400",2495.4,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881276","OE - Cadre, H2000 x P800 x L1250, 200 + 650 + 400","OE - Frame, H2000 x D800 x W1250, 200 + 650 + 400","OE- ESTRUCTURA, H2000 x D800 x W1250, 200+650+400","ZENERGY – KERET, H2000 X D800 X W1250, 200+650+400"]
["88130","ZENERGY - RAMA, H2000 X D800 X W1300",1626.9,"1-ZE-01",null,null,"OE_FRAME_2000","88130","SZT","85389099",null,null,"5901988881306","OE - Cradle, H2000 x P800 x L1300","OE - Frame, H2000 x D800 x W1300","OE- ESTRUCTURA, H2000 x D800 x W1300","ZENERGY - KERET, H2000 X D800 X W1300"]
["88133","ZENERGY - RAMA, H2000 X D800 X W1300, 850+450",2125.8000000000002,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881337","OE - Cadre, H2000 x P800 x L1300, 850 + 450","OE - Frame, H2000 x D800 x W1300, 850 + 450","OE- ESTRUCTURA, H2000 x D800 x W1300, 850+450","ZENERGY – KERET, H2000 X D800 X W1300, 850+450"]
["88147","ZENERGY - RAMA, H2000 X D800 X W1450, 150+650+650",2548.6999999999998,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881474","OE - Cadre, H2000 x P800 x L1450, 150 + 650 + 650","OE - Frame, H2000 x D800 x W1450, 150 + 650 + 650","OE- ESTRUCTURA, H2000 x D800 x W1450, 150+650+650","ZENERGY – KERET, H2000 X D800 X W1450, 150+650+650"]
["88152","ZENERGY - RAMA, H2000 X D800 X W1500, 200+650+650",2554.1999999999998,"1-ZE-01",0.01,1,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881528","OE - Cadre, H2000 x P800 x L1500, 200 + 650 + 650","OE - Frame, H2000 x D800 x W1500, 200 + 650 + 650","OE- ESTRUCTURA, H2000 x D800 x W1500, 200+650+650","ZENERGY – KERET, H2000 X D800 X W1500, 200+650+650"]
["88163","ZENERGY - RAMA, H2000 X D800 X W1600, 650+300+650",2685.8,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881634","OE - Cadre, H2000 x P800 x L1600, 650 + 300 + 650","OE - Frame, H2000 x D800 x W1600, 650 + 300 + 650","OE- ESTRUCTURA, H2000 x D800 x W1600, 650+300+650","ZENERGY – KERET, H2000 X D800 X W1600, 650+300+650"]
["88169","ZENERGY - RAMA, H2000 X D800 X W1650, 200+650+800",2662.2,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881696","OE - Cadre, H2000 x P800 x L1650, 200 + 650 + 800","OE - Frame, H2000 x D800 x W1650, 200 + 650 + 800","OE- ESTRUCTURA, H2000 x D800 x W1650, 200+650+800","ZENERGY – KERET, H2000 X D800 X W1650, 200+650+800"]
["88172","ZENERGY - RAMA, H2000 X D800 X W1700, 650+650+400",2727.2,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881726","OE - Cadre, H2000 x P800 x L1700, 650 + 650 + 400","OE - Frame, H2000 x D800 x W1700, 650 + 650 + 400","OE- ESTRUCTURA, H2000 x D800 x W1700, 650+650+400","ZENERGY – KERET, H2000 X D800 X W1700, 650+650+400"]
["88173","ZENERGY - RAMA, H2000 X D800 X W1700, 850+200+650",2683.5,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881733","OE - Cadre, H2000 x P800 x L1700, 850 + 200 + 650","OE - Frame, H2000 x D800 x W1700, 850 + 200 + 650","OE- ESTRUCTURA, H2000 x D800 x W1700, 850+200+650","ZENERGY – KERET, H2000 X D800 X W1700, 850+200+650"]
["88197","ZENERGY - RAMA, H2000 X D800 X W2000, 850+300+850",2793.3,"1-ZE-01",null,null,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988881979","OE - Cadre, H2000 x P800 x L2000, 850 + 300 + 850","OE - Frame, H2000 x D800 x W2000, 850 + 300 + 850","OE- ESTRUCTURA, H2000 x D800 x W2000, 850+300+850","ZENERGY – KERET, H2000 X D800 X W2000, 850+300+850"]
["89224","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP30, H2000 X D230",245.2,"1-ZE-01",null,null,"OE_COVERS","89224","SZT","85389099","27.12.40.0",null,"5901988892241","OE - Ventilateurs latéraux ventilés fixes IP30, H2000 x P230","OE - Ventilated, fixed side covers IP30, H2000 x D230","OE- PAREDES LATERALES VENTIL. FIJO IP30, H2000 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP30, H2000 X D230"]
["89232","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H2000 X D300",644.79999999999995,"1-ZE-01",null,null,"OE_COVERS","89232","SZT","85389099",null,null,"5901988892326","OE - Évents latéraux, ventilés, plats et vissés IP30, H2000 x P300","OE - Side panels ventilated, flat, screwed on, IP30, H2000 x D300","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H2000 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H2000 X D300"]
["89242","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H2000 X D400",682.6,"1-ZE-01",null,null,"OE_COVERS","89242","SZT","85389099",null,null,"5901988892425","OE - Couvercles latéraux ventilés, plats, vissés IP30, H2000 x P400","OE - Side panels ventilated, flat, screwed on, IP30, H2000 x D400","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H2000 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H2000 X D400"]
["89280","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP30, H2000 X D800",933.9,"1-ZE-01",0.10833333333333334,5,"OE_COVERS","89280","SZT","85389099","27.12.40.0",null,"5901988892807","OE - Hottes de ventilation latérales IP30, H2000 x P800","OE - IP30, H2000 x D800 Ventilated side covers","OE- PAREDES LATERALES VENTIL. IP30, H2000 x D800 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP30, H2000 X D800"]
["89310","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D1000",1059.3,"1-ZE-01",0.01,1,"OE_COVERS",null,"SZT","85389099",null,null,"5901988893101","OE - COUVERCLES LATÉRAUX COMPLETS IP30, H2000 x P1000","OE - Plain side covers IP30, H2000 x D1000","*OE - TAPAS LATERALES COMPLETAS IP30, H2000 x D1000","ZENERGY – TELJES OLDALBURKOLATOK IP30, H2000 X D1000"]
["89325","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H2000 X D230",301.3,"1-ZE-01",null,null,"OE_COVERS","89325","SZT","85389099",null,null,"5901988893255","OE - Capots latéraux solides, plats, vissés IP30, H2000 x P230","OE - Side panels Plain, flat, screwed on, IP30, H2000 x D230","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H2000 x D230 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H2000 X D230"]
["89327","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H2000 X D230",98.2,"1-ZE-01",1.6666666666666666E-2,1,"OE_SEPARATION_BUSBAR","89327","SZT","85389099",null,null,"5901988893279","OE - Panneau de séparation, vertical, galvanisé, H2000 x P230","OE - Vertical partition, Galvanized, H2000 x D230","OE- TABIQUE VERTIC. GALV. H2000XD230","ZENERGY – FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H2000 X D230"]
["89332","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H2000 X D300",330.5,"1-ZE-01",null,null,"OE_COVERS","89332","SZT","85389099",null,null,"5901988893323","OE - Caches latéraux, pleins, plats, vissés IP30, H2000 x P300","OE - Plain, flat, screwed side covers, IP30, H2000 x D300","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H2000 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H2000 X D300"]
["89341","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H2000 X D400",339.1,"1-ZE-01",1.6666666666666666E-2,1,"OE_COVERS","89341","SZT","85389099",null,null,"5901988893415","OE - Couvercles latéraux complets, fixes IP30, H2000 x P400","OE - Plain, fixed side covers IP30, H2000 x D400","OE- PAREDES LATERALES LISO FIJO IP30, H2000 x D400  (2UDS)","ZENERGY – TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H2000 X D400"]
["89361","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H2000 X D600",392,"1-ZE-01",0.16666666666666666,5,"OE_COVERS","89361","SZT","85389099",null,null,"5901988893613","OE - Couvercles latéraux complets, fixes IP30, H2000 x P600","OE - Plain, fixed side covers IP30, H2000 x D600","OE- PAREDES LATERALES LISO FIJO IP30, H2000 x D600 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, RÖGZÍTETT, IP30, H2000 X D600"]
["89380","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D800",869,"1-ZE-01",0.31666666666666665,8,"OE_COVERS","89380","SZT","85389099","27.12.40.0",null,"5901988893804","OE - Couvercles latéraux complets IP30, H2000 x P800","OE - Plain side covers IP30, H2000 x D800","OE- PANELES LATERALES LISOS ATORNILLADOS IP30, H2000 x D800 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H2000 X D800"]
["89423","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H2000 X D230",520.6,"1-ZE-01",null,null,"OE_COVERS","89223","SZT","85389099",null,null,"5901988894238","OE - Hottes de ventilation latérales IP43, H2000 x P230","OE - IP43, H2000 x D230 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H2000 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H2000 X D230"]
["89430","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H2000 X D300",846.7,"1-ZE-01",null,null,"OE_COVERS","89230","SZT","85389099",null,null,"5901988894306","OE - Hottes de ventilation latérales IP43, H2000 x P300","OE - IP43, H2000 x D300 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H2000 x D300 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H2000 X D300"]
["89440","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H2000 X D400",910.4,"1-ZE-01",null,null,"OE_COVERS","89240","SZT","85389099",null,null,"5901988894405","OE - Hottes de ventilation latérales IP43, H2000 x P400","OE - IP43, H2000 x D400 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H2000 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H2000 X D400"]
["89441","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H2000 X D400",517.29999999999995,"1-ZE-01",null,null,"OE_COVERS","89241","SZT","85389099",null,null,"5901988894412","OE - Ventilateurs latéraux ventilés fixes IP43, H2000 x P400","OE - Ventilated, fixed side covers IP43, H2000 x D400","OE- PAREDES LATERALES VENTIL. FIJO IP43, H2000 x D400  (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H2000 X D400"]
["89461","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP43, H2000 X D600",561.6,"1-ZE-01",null,null,"OE_COVERS","89261","SZT","85389099",null,null,"5901988894610","OE - Ventilateurs latéraux ventilés fixes IP43, H2000 x P600","OE - Ventilated, fixed side covers IP43, H2000 x D600","OE- PAREDES LATERALES VENTIL. FIJO IP43, H2000 x D600 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP43, H2000 X D600"]
["89523","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H2000 X D230",538.9,"1-ZE-01",null,null,"OE_COVERS","89323","SZT","85389099","27.12.40.0",null,"5901988895235","OE - Couvercles latéraux complets IP55, H2000 x P230","OE - Plain side covers IP55, H2000 x D230","OE- PAREDES LATERALES LISO IP55, H2000 x D230 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H2000 X D230"]
["89540","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H2000 X D400",821.9,"1-ZE-01",1.0083333333333333,12,"OE_COVERS","89340","SZT","85389099","27.12.40.0",null,"5901988895402","OE - Capots latéraux, intégralement IP55, H2000 x P400","OE - Plain side covers IP55, H2000 x D400","OE- PAREDES LATERALES LISO IP55, H2000 x D400  (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H2000 X D400"]
["90110","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2200 W1000",544.29999999999995,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","90110","SZT","85389099",null,null,"5901988901103","OE - H2200 L1000 cadre cadre à charnière avant","OE - Frame of hinged Front covers H2200 W1000","OE- MARCO PIVOTANTE H2200 W1000","ZENERGY - CSATORNÁS ELSŐ BURKOLAT H2200 W1000"]
["90141","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2200 W400 DO PLOMBOWANIA",384.2,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","90140","SZT","85389099",null,null,"5901988901417","OE - H2200 L400 Cadre de panneau avant articulé pour sceller","OE - Frame of Front covers on hinges H2200 W400 for sealing","OE- MARCO PIVOTANTE H2200 W400 ","ZENERGY - csuklós ELSŐ BURKOLAT H2200 W400 TÖMÍTÉSHEZ"]
["90156","Zenergy - Rama osłonowa, pełna, na zawiasach H2200 W550/W1200",744.8,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","90156","SZT","85389099",null,null,"5901988901561","OE - Cadre de recouvrement, plein, articulé H2200 L550 / L1200","OE - Cover frame, Plain, hinged H2200 W550 / W1200","OE- MARCO DE CUBIERTA, COMPLETO, CON BISAGRAS H2200 W550 / W1200","Zenergy - Takarókeret, tömör, csuklós H2200 W550/W1200"]
["90166","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2200 W650 DO PLOMBOWANIA",448,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","90165","SZT","85389099",null,null,"5901988901660","OE - H2200 L650 cadre de panneau avant articulé pour sceller","OE - Frame of hinged Front covers H2200 W650 for sealing","OE- MARCO PIVOTANTE H2200 W650 ","ZENERGY - csuklós ELSŐ BURKOLAT KERET H2200 W650 TÖMÍTÉSHEZ"]
["90170","ZENERGY IT - DWA WSPORNIKI PIONOWE MODUŁU \"U\" 19-CALI NA WKRĘTY SAMOFORMUJĄCE, SZAFY H2200 W650",454.7,"1-ZE-01",0.18333333333333332,1,"OE_SUPPORT",null,"SZT","85389099",null,null,"5901988901707","IT - Deux supports verticaux pour le module en forme de U \"19\" pour vis autoformeuses, armoires H2200 L650","IT - Two 19-inch U  Vertical supports for self-forming screws, H2200 W650 cabinets ","OE IT- DOS SOPORT. VERT. MOD. \"U\" 19\" ARMARIO H2200 W650","ZENERGY IT - KÉT FÜGGŐLEGES TARTÁS A 19 hüvelykes \"U\" MODULHOZ ÖNFORMÁLÓ CSAVARKKAL, H2200 W650 SZEKRÉNYEK"]
["90185","ZENERGY - RAMA OSŁON CZOŁOWYCH NA ZAWIASACH H2200 W850",493.9,"1-ZE-01",0.30833333333333335,7,"OE_FRAME_INTERNAL","90185","SZT","85389099","27.12.40.0",null,"5901988901851","OE - H2200 L850 cadre à charnière avant","OE - Frame of hinged Front covers H2200 W850","OE- MARCO PIVOTANTE H2200 W850","ZENERGY - SZÁNTOS ELSŐ BURKOLAT KERET H2200 W850"]
["90212","ZENERGY - DRZWI WENTYLOWANE IP30, H2200 W1200, PODWÓJNE",2628.7,"1-ZE-01",null,null,"OE_DOORS_2200","90312","SZT","85389099","27.12.40.0",null,"5901988902124","OE - IP30, H2200 L1200 portes ventilées, doubles","OE - Ventilated doors IP30, H2200 W1200, double","OE- PUERTA VENTIL. IP30, H2200 W1200, DOBLE","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2200 W1200, DUPLÉS"]
["90230","ZENERGY - DRZWI WENTYLOWANE IP30, H2200 W300",970.9,"1-ZE-01",null,null,"OE_DOORS_2200","90330","SZT","85389099",null,null,"5901988902308","OE - portes ventilées IP30, H2200 L300","OE - Ventilated door IP30, H2200 W300","OE- PUERTA VENTIL. IP30, H2200 W300","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2200 W300"]
["90260","ZENERGY - DRZWI WENTYLOWANE IP30, H2200 W600",1250.5999999999999,"1-ZE-01",null,null,"OE_DOORS_2200","90360","SZT","85389099",null,null,"5901988902605","OE - portes ventilées IP30, H2200 L600","OE - Ventilated door IP30, H2200 W600","OE- PUERTA VENTIL. IP30, H2200 W600","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2200 W600"]
["90295","ZENERGY - DRZWI WENTYLOWANE IP30, H2200 W950",1558.4,"1-ZE-01",null,null,"OE_DOORS_2200","90395","SZT","85389099",null,null,"5901988902957","OE - portes ventilées IP30, H2200 W950","OE - Ventilated door IP30, H2200 W950","OE- PUERTA VENTIL. IP30, H2200 W950","ZENERGY - SZELLŐZTETT AJTÓK IP30, H2200 W950"]
["90312","ZENERGY - DRZWI PEŁNE IP30, H2200 W1200, PODWÓJNE",2520.6999999999998,"1-ZE-01",0.16666666666666666,4,"OE_DOORS_2200","90312","SZT","85389099",null,null,"5901988903121","OE - Portes pleine IP30, H2200 L1200, double","OE - Plain door IP30, H2200 W1200, double","OE- PUERTA OPACA IP30, H2200 W1200, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H2200 W1200, DUPLA"]
["90313","ZENERGY - DRZWI PEŁNE IP30, H2200 W1300, PODWÓJNE",2541.1999999999998,"1-ZE-01",0.01,1,"OE_DOORS_2200","90313","SZT","85389099",null,null,"5901988903138","OE - Portes pleine IP30, H2200 L1300, double","OE - Plain doors IP30, H2200 W1300, double","OE- PUERTA OPACA IP30, H2200 W1300, DOBLE","ZENERGY - TÖMÖR AJTÓK IP30, H2200 W1300, DUPLA"]
["90340","ZENERGY - DRZWI PEŁNE IP30, H2200 W400",989.3,"1-ZE-01",null,null,"OE_DOORS_2200","90340","SZT","85389099",null,null,"5901988903404","OE - Portes pleine IP30, H2200 L400","OE - Plain door IP30, H2200 W400","OE- PUERTA OPACA IP30, H2200 W400","ZENERGY - TELJES AJTÓ IP30, H2200 W400"]
["90365","ZENERGY - DRZWI PEŁNE IP30, H2200 W650",1213.9000000000001,"1-ZE-01",0.15833333333333333,5,"OE_DOORS_2200","90365","SZT","85389099","27.12.40.0",null,"5901988903657","OE - Portes pleine IP30, H2200 L650","OE - Plain door IP30, H2200 W650","OE- PUERTA OPACA IP30, H2200 W650","ZENERGY - TELJES AJTÓ IP30, H2200 W650"]
["90373","ZENERGY - SŁUPEK INOX, H2200, RAMA ZEWNĘTRZNA",171.4,"1-ZE-01",1.3583333333333334,5,"OE_FRAME_2200","90371","SZT","85389099","27.12.40.0",null,"5901988903732","OE - Poteau INOX, H2200, cadre externe","OE - INOX post, H2200, external frame","OE- PERFIL INOX, H2200, PARA MARCO LATERAL EXTERIOR","ZENERGY - INOX POST, H2200, KÜLSŐ KERET"]
["90376","ZENERGY - SŁUPEK WEWNĘTRZNY, H2200, POLE NAROŻNE + 2SZT. ELEMENT ŁĄCZĄCY",92.6,"1-ZE-01",1.6666666666666666E-2,1,"OE_FRAME_2000",null,"SZT","85389099",null,null,"5901988903763","OE - Poteau intérieur, H2200, boîte d'angle + 2 éléments de raccordement","OE - Internal post, H2200, corner field + 2 pcs. connecting element","OE- Poste interno, H2200, campo de esquina + 2 uds. elemento de conexión","ZENERGY - BELSŐ POSTA, H2200, SAROK DOBOZ + 2 DB. CSATLAKOZÓ ELEM"]
["90380","ZENERGY - DRZWI PEŁNE IP30, H2200 W800",1351.1,"1-ZE-01",4.1666666666666664E-2,2,"OE_DOORS_2200","90380","SZT","85389099","27.12.40.0",null,"5901988903800","OE - Portes pleine IP30, H2200 L800","OE - Plain doors IP30, H2200 W800","OE- PUERTA OPACA IP30, H2200 W800","ZENERGY - TELJES AJTÓ IP30, H2200 W800"]
["90410","ZENERGY - DRZWI WENTYLOWANE IP43, H2200 W1000",1837,"1-ZE-01",null,null,"OE_DOORS_2200","90310","SZT","85389099",null,null,"5901988904104","OE - Portes ventilées IP43, H2200 L1000","OE - Ventilated door IP43, H2200 W1000","OE- PUERTA VENTIL. IP43, H2200 W1000","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2200 W1000"]
["90430","ZENERGY - DRZWI WENTYLOWANE IP43, H2200 W300",1065.9000000000001,"1-ZE-01",null,null,"OE_DOORS_2200","90330","SZT","85389099",null,null,"5901988904302","OE - Portes ventilées IP43, H2200 L300","OE - Ventilated door IP43, H2200 W300","OE- PUERTA VENTIL. IP43, H2200 W300","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2200 W300"]
["90440","ZENERGY - DRZWI WENTYLOWANE IP43, H2200 W400",1162.7,"1-ZE-01",null,null,"OE_DOORS_2200","90340","SZT","85389099",null,null,"5901988904401","OE - Portes ventilées IP43, H2200 L400","OE - Ventilated door IP43, H2200 W400","OE- PUERTA VENTIL. IP43, H2200 W400","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2200 W400"]
["90465","ZENERGY - DRZWI WENTYLOWANE IP43, H2200 W650",1379.2,"1-ZE-01",0.01,1,"OE_DOORS_2200","90365","SZT","85389099",null,null,"5901988904654","OE - Portes ventilées IP43, H2200 L650","OE - Ventilated door IP43, H2200 W650","OE- PUERTA VENTIL. IP43, H2200 W650","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2200 W650"]
["90495","ZENERGY - DRZWI WENTYLOWANE IP43, H2200 W950",1714,"1-ZE-01",null,null,"OE_DOORS_2200","90395","SZT","85389099",null,null,"5901988904951","OE - Portes ventilées IP43, H2200 W950","OE - Ventilated door IP43, H2200 W950","OE- PUERTA VENTIL. IP43, H2200 W950","ZENERGY - SZELLŐZTETT AJTÓK IP43, H2200 W950"]
["90514","ZENERGY - DRZWI PEŁNE IP55, H2200 W1050",1853.5,"1-ZE-01",null,null,"OE_DOORS_2200","90314","SZT","85389099",null,null,"5901988905149","OE - Portes pleine IP55, H2200 L1050","OE - Plain door IP55, H2200 W1050","OE- PUERTA OPACA IP55, H2200 W1050","ZENERGY - TÖMÖR AJTÓ IP55, H2200 W1050"]
["90545","ZENERGY - DRZWI PEŁNE IP55, H2200 W450",1142.5999999999999,"1-ZE-01",9.166666666666666E-2,1,"OE_DOORS_2200","90345","SZT","85389099",null,null,"5901988905453","OE - Portes pleine IP55, H2200 L450","OE - Plain door IP55, H2200 W450","OE- PUERTA OPACA IP55, H2200 W450","ZENERGY - TÖMÖR AJTÓ IP55, H2200 W450"]
["90580","ZENERGY - DRZWI PEŁNE IP55, H2200 W800",1468.8,"1-ZE-01",null,null,"OE_DOORS_2200","90380","SZT","85389099",null,null,"5901988905804","OE - Portes pleine IP55, H2200 L800","OE - Plain doors IP55, H2200 W800","OE- PUERTA OPACA IP55, H2200 W800","ZENERGY - TÖMÖR AJTÓ IP55, H2200 W800"]
["90612","ZENERGY - DRZWI PRZESZKLONE IP55, H2200 X W1200, PODWÓJNE",3476,"1-ZE-01",null,null,"OE_DOORS_2200","91112","SZT","85389099",null,null,"5901988906122","OE - Portes vitrée IP55, H2200 L1200, double","OE - Glazed door IP55, H2200 x W1200, double","OE- PUERTA TRANSPARENTE IP55, H2200 W1200, DOBLE","ZENERGY - ÜVEGAJTÓK IP55, H2200 X W1200, DUPLA"]
["90640","ZENERGY - DRZWI PRZESZKLONE IP55, H2200 X W400",1367.3,"1-ZE-01",null,null,"OE_DOORS_2200","91140","SZT","85389099",null,null,"5901988906405","OE - Portes vitrée IP55, H2200 L400","OE - Glazed door IP55, H2200 x W400","OE- PUERTA TRANSPARENTE IP55, H2200 W400","ZENERGY - ÜVEZETETT AJTÓK IP55, H2200 X W400"]
["90645","ZENERGY - DRZWI PRZESZKLONE IP55, H2200 X W450",1314.5,"1-ZE-01",null,null,"OE_DOORS_2200","91145","SZT","85389099",null,null,"5901988906450","OE - Portes vitrée IP55, H2200 L450","OE - Glazed door IP55, H2200 x W450","OE- PUERTA TRANSPARENTE IP55, H2200 W450","ZENERGY - ÜVEZETETT AJTÓK IP55, H2200 X W450"]
["90680","ZENERGY - DRZWI PRZESZKLONE IP55, H2200 X W800",1786.3,"1-ZE-01",1.6666666666666666E-2,1,"OE_DOORS_2200","91180","SZT","85389099",null,null,"5901988906801","OE - Portes vitrée IP55, H2200 L800","OE - Glazed door IP55, H2200 x W800","OE- PUERTA TRANSPARENTE IP55, H2200 W800","ZENERGY - ÜVEZETETT AJTÓK IP55, H2200 X W800"]
["90742","ZENERGY - SŁUPEK OCYNK, H2200, RAMA WEWNĘTRZNA, PODWÓJNA",109.2,"1-ZE-01",8.3333333333333329E-2,1,"OE_FRAME_2200","90742","SZT","85389099",null,null,"5901988907426","OE - poteau galvanisé, H2200, cadre interne, double","OE - Galvanized post, H2200, double inner frame","OE- PERFIL GALVANIZADO, H2200,  PARA MARCO LATERAL INTERIOR, DOBLE","ZENERGY - HORGANYOZOTT OSZTA, H2200, BELSŐ KERET, DUPLÁS"]
["90765","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 5X EFEN 160-630, H2200 W650, 23+15M, ANALIZATORY 5X 96X96MM",831,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","90765","SZT","85389099",null,null,"5901988907655","OE - Cadre pivotant d'interrupteurs-sectionneurs 5x EFEN 160-630, H2200 L650, 23 + 15M, analyseurs 5x 96x96mm","OE - Hinged frame for rail disconnectors 5x EFEN 160-630, H2200 W650, 23 + 15M, analyzers 5x 96x96mm","OE- ESTRUCTURA PARA REGLETAS SECC. 5x160-630, H2200 W650, 23+15M","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 5X EFEN 160-630, H2200 W650, 23+15M, ELEMZŐK 5X 96X96MM"]
["90786","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 7X EFEN 160-630, H2200 W850, 23+13M, ANALIZATORY 7X 96X96MM DO PLOMBOWANIA",947.5,"1-ZE-01",null,null,"OE_FRAME_INTERNAL","90785","SZT","85389099",null,null,"5901988907860","OE - Cadre pivotant d'interrupteurs-sectionneurs 7x EFEN 160-630, H2200 L850, 23 + 13M, analyseurs 7x 96x96mm pour l'étanchéité","OE - Hinged frame for switch disconnectors 7x EFEN 160-630, H2200 W850, 23 + 13M, 7x 96x96mm analyzers for sealing","OE- ESTRUCTURA PARA REGLETAS SECC. 7x160-630, H2200 W850, 23+13M","ZENERGY - CSATLAKOZÓK DÖNTÉSŰ KERET 7X EFEN 160-630, H2200 W850, 23+13M, ELEMZŐK 7X 96X96MM TÖMÍTÉSRE"]
["90865","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 5X EFEN 160-630, H2200 W650, 23+17M",698.9,"1-ZE-01",0.16666666666666666,5,"OE_FRAME_INTERNAL","90865","SZT","85389099",null,null,"5901988908652","OE - Cadre pivotant d'interrupteurs-sectionneurs 5X EFEN à lamelles 160-630, H2200 L650, 23 + 17M","OE - Hinged frame for switch disconnectors 5x EFEN 160-630, H2200 W650, 23 + 17M","OE- ESTRUCTURA PARA REGLETAS SECC. 5x160-630, H2200 W650, 23+17M","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 5X EFEN 160-630, H2200 W650, 23+17M"]
["90885","ZENERGY - RAMA UCHYLNA ROZŁĄCZNIKÓW LISTWOWYCH 7X EFEN 160-630, H2200 W850, 23+17M",797.4,"1-ZE-01",0.05,2,"OE_FRAME_INTERNAL","90885","SZT","85389099",null,null,"5901988908850","OE - Cadre pivotant d'interrupteurs-sectionneurs 7x EFEN 160-630, H2200 L850, 23 + 17M","OE - Hinged frame for switch disconnectors 7x EFEN 160-630, H2200 W850, 23 + 17M","OE- ESTRUCTURA PARA REGLETAS SECC. 7x160-630, H2200 W850, 23+17M","ZENERGY - CSATLAKOZÓK DÖNTÉSE KERET 7X EFEN 160-630, H2200 W850, 23+17M"]
["90912","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2200 X W1200 + WSPORNIKI,  ( 2050 X 1100 )",1359.7,"1-ZE-01",null,null,"OE_PLAIN_PLATES","90912","SZT","85389099",null,null,"5901988909123","OE - Plaque de montage complète H2200 x L1200 + supports, (2050 x 1100)","OE - Plain Mounting plate H2200 x W1200 + brackets, (2050 x 1100)","OE- PLACA MONTAJE  TOTAL CIEGA H2200 x W1200 + SOPORT. ( 2050 X 1100)","ZENERGY - TELJES RÖGZÍTŐ LEMEZ H2200 X W1200 + KONZEREK, (2050 X 1100)"]
["90913","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2200 X W1300 + WSPORNIKI,  ( 2050 X 1200 )",1461.2,"1-ZE-01",0.01,1,"OE_PLAIN_PLATES","90913","SZT","85389099",null,null,"5901988909130","OE - Plaque de montage complète H2200 x L1300 + supports, (2050 x 1200)","OE - Plain Mounting plate H2200 x W1300 + brackets, (2050 x 1200)","OE- PLACA MONTAJE  TOTAL CIEGA H2200 x W1300 + SOPORT. ( 2050 X 1200)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H2200 X W1300 + KONZEREK, (2050 X 1200)"]
["90945","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2200 X W450 + WSPORNIKI,  ( 2050 X 350 )",595.1,"1-ZE-01",null,null,"OE_PLAIN_PLATES","90945","SZT","85389099",null,null,"5901988909451","OE - Plaque de montage complète H2200 x L450 + supports, (2050 x 350)","OE - Plain Mounting plate H2200 x W450 + brackets, (2050 x 350)","OE- PLACA MONTAJE  TOTAL CIEGA H2200 x W450 + SOPORT. ( 2050 X 350)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H2200 X W450 + KONZEREK, (2050 X 350)"]
["90980","ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2200 X W800 + WSPORNIKI,  ( 2050 X 700 )",954.7,"1-ZE-01",null,null,"OE_PLAIN_PLATES","90980","SZT","85389099",null,null,"5901988909802","OE - Plaque de montage complète H2200 x L800 + supports, (2050 x 700)","OE - Plain Mounting plate H2200 x W800 + brackets, (2050 x 700)","OE- PLACA MONTAJE  TOTAL CIEGA H2200 x W800 + SOPORT. ( 2050 X 700)","ZENERGY - TELJES RÖGZÍTŐLEMEZ H2200 X W800 + KONZEREK, (2050 X 700)"]
["91045","ZENERGY - RAMA, H2200 X D1000 X W450",1555.7,"1-ZE-01",null,null,"OE_FRAME_2200","91045","SZT","85389099",null,null,"5901988910457","OE - Cadre, H2200 x P1000 x L450","OE - Frame, H2200 x D1000 x W450","OE- ESTRUCTURA H2200XD1000XW450","ZENERGY - KERET, H2200 X D1000 X W450"]
["91061","OE - Rama, H2200 x D1000 x W600, 450+150",1904,"1-ZE-01",null,null,"OE_FRAME_2200","91061","SZT",null,null,"230322PW",null,"OE - Cadre, H2200 x P1000 x L600, 450 + 150","OE - Frame, H2200 x D1000 x W600, 450 + 150","OE- ESTRUCTURA H2200XD1000XW600, 450 + 150","OE – keret, H2200 x D1000 x W600, 450+150"]
["91082","ZENERGY - RAMA, H2250 X D1000 X W800, IT 47U",1738.2,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988910822","OE - CADRE, H2250 x P1000 x L800, IT 47U","OE - Frame, H2250 x D1000 x H800, IT 47U","*OE - MARCO, H2250 x D1000 x W800, IT 47U","ZENERGY - KERET, H2250 X D1000 X W800, IT 47U"]
["91100","ZENERGY - RAMA, H2200 X D1000 X W1000",1841.3,"1-ZE-01",null,null,"OE_FRAME_2200","91100","SZT","85389099",null,null,"5901988911003","OE - Cadre, H2200 x P1000 x L1200","OE - Frame, H2200 x D1000 x W1000","OE- ESTRUCTURA H2200XD1000XW1000","ZENERGY - KERET, H2200 X D1000 X W1000"]
["91113","ZENERGY - DRZWI PRZESZKLONE IP30, H2200 X W1300, PODWÓJNE",3170.2,"1-ZE-01",null,null,"OE_DOORS_2200","91113","SZT","85389099",null,null,"5901988911133","OE - Portes vitrées IP30, H2200 x L1300, double vitrage","OE - Glazed door IP30, H2200 x W1300, double","OE- PUERTA TRANSP. DOBLE IP30, H2200XW1300, DOBLE","ZENERGY - ÜVEGAJTÓK IP30, H2200 X W1300, DUPLA"]
["91120","ZENERGY - RAMA, H2200 X D1000 X W1200",1870.4,"1-ZE-01",0.15833333333333333,4,"OE_FRAME_2200","91120","SZT","85389099",null,null,"5901988911201","OE - Cadre, H2200 x P1000 x L1200","OE - Frame, H2200 x D1000 x W1200","OE- ESTRUCTURA H2200XD1000XW1200","ZENERGY - KERET, H2200 X D1000 X W1200"]
["91140","ZENERGY - DRZWI PRZESZKLONE IP30, H2200 X W400",1127.5,"1-ZE-01",null,null,"OE_DOORS_2200","91140","SZT","85389099",null,null,"5901988911409","OE - Portes vitrées IP30, H2200 x L400","OE - Glazed door IP30, H2200 x W400","OE- PUERTA TRANSP. DOBLE IP30, H2200XW400","ZENERGY - ÜVEZETETT AJTÓK IP30, H2200 X W400"]
["91165","ZENERGY - DRZWI PRZESZKLONE IP30, H2200 X W650",1452,"1-ZE-01",null,null,"OE_DOORS_2200","91165","SZT","85389099",null,null,"5901988911652","OE - Portes vitrées IP30, H2200 x L650","OE - Glazed door IP30, H2200 x W650","OE- PUERTA TRANSP. DOBLE IP30, H2200XW650","ZENERGY - ÜVEGAJTÓK IP30, H2200 X W650"]
["91195","ZENERGY - DRZWI PRZESZKLONE IP30, H2200 X W950",1889.8,"1-ZE-01",null,null,"OE_DOORS_2200","91195","SZT","85389099",null,null,"5901988911959","OE - Portes vitrées IP30, H2200 x L950","OE - Glazed door IP30, H2200 x W950","OE- PUERTA TRANSP. DOBLE IP30, H2200XW950","ZENERGY - ÜVEGAJTÓK IP30, H2200 X W950"]
["91210","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2200 X W1000",808.9,"1-ZE-01",null,null,"OE_COVERS","91210","SZT","85389099","27.12.40.0",null,"5901988912109","OE - Couverture arrière complète IP30, H2200 x L1000","OE - Plain rear cover IP30, H2200 x W1000","OE- FONDO ATORNILLADO LISO IP30, H2200 x W1000","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2200 X W1000"]
["91230","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2200 X W300",317.5,"1-ZE-01",0.01,1,"OE_COVERS","91230","SZT","85389099","27.12.40.0",null,"5901988912307","OE - Couverture arrière complète IP30, H2200 x L300","OE - Plain rear cover IP30, H2200 x W300","OE- FONDO ATORNILLADO LISO IP30, H2200 x W300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2200 X W300"]
["91260","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2200 X W600",598.4,"1-ZE-01",null,null,"OE_COVERS","91260","SZT","85389099","27.12.40.0",null,"5901988912604","OE - Couverture arrière complète IP30, H2200 x L600","OE - Plain rear cover IP30, H2200 x W600","OE- FONDO ATORNILLADO LISO IP30, H2200 x W600","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2200 X W600"]
["91285","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2200 X W850",726.8,"1-ZE-01",9.166666666666666E-2,4,"OE_COVERS","91285","SZT","85389099","27.12.40.0",null,"5901988912857","OE - Couverture arrière complète IP30, H2200 x L850","OE - Plain rear cover IP30, H2200 x W850","OE- FONDO ATORNILLADO LISO IP30, H2200 x W850","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2200 X W850"]
["91295","ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2200 X W650+300",1248.5,"1-ZE-01",null,null,"OE_COVERS","91295","SZT","85389099","27.12.40.0",null,"5901988912956","OE - Couverture arrière complète IP30, H2200 x L650 + 300","OE - Plain rear cover IP30, H2200 x W650 + 300","OE- FONDO ATORNILLADO LISO IP30, H2200 x W650+300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP30, H2200 X W650+300"]
["91312","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2200 X W1200",1293.8,"1-ZE-01",0.15833333333333333,4,"OE_COVERS","91312","SZT","85389099","27.12.40.0",null,"5901988913120","OE - Couverture arrière ventilée IP30, H2200 x L1200","OE - Rear ventilated cover IP30, H2200 x W1200","OE- FONDO ATORNILLADO VENTIL. IP30, H2200 x W1200","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2200 X W1200"]
["91340","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2200 X W400",535.70000000000005,"1-ZE-01",3.3333333333333333E-2,1,"OE_COVERS","91340","SZT","85389099","27.12.40.0",null,"5901988913403","OE - Hotte d'aération arrière IP30, H2200 x L400","OE - Rear ventilated cover IP30, H2200 x W400","OE- FONDO ATORNILLADO VENTIL. IP30, H2200 x W400","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2200 X W400"]
["91360","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2200 X W600",665.3,"1-ZE-01",0.15833333333333333,2,"OE_COVERS","91360","SZT","85389099","27.12.40.0",null,"5901988913601","OE - Couverture arrière ventilée IP30, H2200 x L600","OE - Rear ventilated cover IP30, H2200 x W600","OE- FONDO ATORNILLADO VENTIL. IP30, H2200 x W600","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2200 X W600"]
["91380","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP30, H2200 X W800",781.9,"1-ZE-01",5.8333333333333334E-2,4,"OE_COVERS","91380","SZT","8538909900","27.12.40.0",null,"5901988913809","OE - Hotte d'aération arrière IP30, H2200 x L800","OE - Rear ventilated cover IP30, H2200 x W800","OE- FONDO ATORNILLADO VENTIL. IP30, H2200 x W800","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP30, H2200 X W800"]
["91410","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2200 X W1000",1026.3,"1-ZE-01",null,null,"OE_COVERS","91310","SZT","85389099",null,null,"5901988914103","OE - Coque arrière ventilée IP43, H2200 x L1000","OE - Rear ventilated cover IP43, H2200 x W1000","OE- FONDO ATORNILLADO VENTIL.IP43, H2200 x W1000","ZENERGY - SZELLŐZTETETT HÁTSÓ BURKOLAT IP43, H2200 X W1000"]
["91413","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2200 X W1300",1625.8,"1-ZE-01",null,null,"OE_COVERS","91313","SZT","85389099",null,null,"5901988914134","OE - Coque arrière ventilée IP43, H2200 x L1300","OE - Rear ventilated cover IP43, H2200 x W1300","OE- FONDO ATORNILLADO VENTIL.IP43, H2200 x W1300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2200 X W1300"]
["91460","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2200 X W600",797.5,"1-ZE-01",null,null,"OE_COVERS","91360","SZT","85389099",null,null,"5901988914608","OE - Coque arrière ventilée IP43, H2200 x L600","OE - Rear ventilated cover IP43, H2200 x W600","OE- FONDO ATORNILLADO VENTIL.IP43, H2200 x W600","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2200 X W600"]
["91465","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2200 X W650",825.1,"1-ZE-01",0.01,1,"OE_COVERS","91365","SZT","85389099",null,null,"5901988914653","OE - Coque arrière ventilée IP43, H2200 x L650","OE - Rear ventilated cover IP43, H2200 x W650","OE- FONDO ATORNILLADO VENTIL.IP43, H2200 x W650","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2200 X W650"]
["91495","ZENERGY - OSŁONA TYLNA WENTYLOWANA IP43, H2200 X W650+300",1058.4000000000001,"1-ZE-01",null,null,"OE_COVERS","91395","SZT","85389099",null,null,"5901988914950","OE - Coque arrière ventilée IP43, H2200 x L650 + 300","OE - Rear ventilated cover IP43, H2200 x W650 + 300","OE- FONDO ATORNILLADO VENTIL.IP43, H2200 x W650+300","ZENERGY - SZELLŐZTETT HÁTSÓ BURKOLAT IP43, H2200 X W650+300"]
["91513","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2200 X W1300",1511.4,"1-ZE-01",null,null,"OE_COVERS","91213","SZT","85389099",null,null,"5901988915131","OE - Couverture arrière complète IP55, H2200 x L1300","OE - Plain rear cover IP55, H2200 x W1300","OE- FONDO ATORNILLADO LISO IP55, H2200 x W1300","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2200 X W1300"]
["91545","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2200 X W450",588.6,"1-ZE-01",9.166666666666666E-2,2,"OE_COVERS","91245","SZT","85389099",null,null,"5901988915452","OE - Couverture arrière complète IP55, H2200 x L450","OE - Plain rear cover IP55, H2200 x W450","OE- FONDO ATORNILLADO LISO IP55, H2200 x W450","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2200 X W450"]
["91580","ZENERGY - OSŁONA TYLNA PEŁNA IP55, H2200 X W800",831.6,"1-ZE-01",3.3333333333333333E-2,1,"OE_COVERS","91280","SZT","85389099",null,null,"5901988915803","OE - Couverture arrière complète IP55, H2200 x L800","OE - Plain rear cover IP55, H2200 x W800","OE- FONDO ATORNILLADO LISO IP55, H2200 x W800","ZENERGY - TELJES HÁTSÓ BURKOLAT IP55, H2200 X W800"]
["92040","ZENERGY - RAMA, H2200 X D230 X W400",819.8,"1-ZE-01",null,null,"OE_FRAME_2200","92040","SZT","85389099",null,null,"5901988920401","OE - Cradle, H2200 x P230 x L400","OE - Frame, H2200 x D230 x W400","OE- ESTRUCTURA, H2200 x D230 x W400","ZENERGY - KERET, H2200 X D230 X W400"]
["92065","ZENERGY - RAMA, H2200 X D230 X W650",929.6,"1-ZE-01",null,null,"OE_FRAME_2200","92065","SZT","85389099",null,null,"5901988920654","OE - Cradle, H2200 x P230 x L650","OE - Frame, H2200 x D230 x W650","OE- ESTRUCTURA, H2200 x D230 x W650","ZENERGY - KERET, H2200 X D230 X W650"]
["92080","ZENERGY - RAMA, H2200 X D230 X W800",995.7,"1-ZE-01",null,null,"OE_FRAME_2200","92080","SZT","85389099",null,null,"5901988920807","OE - Cradle, H2200 x P230 x L800","OE - Frame, H2200 x D230 x W800","OE- ESTRUCTURA, H2200 x D230 x W800","ZENERGY - KERET, H2200 X D230 X W800"]
["92086","ZENERGY - RAMA, H2200 X D230 X W850, 650+200",1215.2,"1-ZE-01",null,null,"OE_FRAME_2200","92086","SZT","85389099",null,null,"5901988920869","OE - Cradle, H2200 x P230 x L850, 650 + 200","OE - Frame, H2200 x D230 x W850, 650 + 200","OE- ESTRUCTURA, H2200 x D230 x W850, 650+200","ZENERGY – KERET, H2200 X D230 X W850, 650+200"]
["92105","ZENERGY - RAMA, H2200 X D230 X W1050, 650+400",1374.2,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988921057","OE - Cradle, H2200 x P230 x L1050, 650 + 400","OE - Frame, H2200 x D230 x W1050, 650 + 400","OE- ESTRUCTURA, H2200 x D230 x W1050, 650+400","ZENERGY – KERET, H2200 X D230 X W1050, 650+400"]
["92120","ZENERGY - RAMA, H2200 X D230 X W1200",1171.5,"1-ZE-01",null,null,"OE_FRAME_2200","92120","SZT","85389099",null,null,"5901988921200","OE - Cradle, H2200 x P230 x L1200","OE - Frame, H2200 x D230 x W1200","OE- ESTRUCTURA, H2200 x D230 x W1200","ZENERGY - KERET, H2200 X D230 X W1200"]
["92130","ZENERGY - RAMA, H2200 X D230 X W1300",1215.2,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988921309","OE - Cradle, H2200 x P230 x L1300","OE - Frame, H2200 x D230 x W1300","OE- ESTRUCTURA, H2200 x D230 x W1300","ZENERGY - KERET, H2200 X D230 X W1300"]
["92150","ZENERGY - RAMA, H2200 X D230 X W1500, 650+850",1559,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988921507","OE - Cadre, H2200 x P230 x L1500, 650 + 850","OE - Frame, H2200 x D230 x W1500, 650 + 850","OE- ESTRUCTURA, H2200 x D230 x W1500, 650+850","ZENERGY – KERET, H2200 X D230 X W1500, 650+850"]
["92164","ZENERGY - RAMA, H2200 X D230 X W1600, 650+150+650+150",1971.2,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988921644","OE - Cadre, H2200 x P230 x L1600, 650 + 150 + 650 + 150","OE - Frame, H2200 x D230 x W1600, 650 + 150 + 650 + 150","OE- ESTRUCTURA, H2200 x D230 x W1600, 650+150+650+150","ZENERGY – KERET, H2200 X D230 X W1600, 650+150+650+150"]
["92187","ZENERGY - RAMA, H2200 X D230 X W1850, 1000+850",1685.6,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988921873","OE - Cadre, H2200 x P230 x L1850, 1000 + 850","OE - Frame, H2200 x D230 x W1850, 1000 + 850","OE- ESTRUCTURA, H2200 x D230 x W1850, 1000+850","ZENERGY – KERET, H2200 X D230 X W1850, 1000+850"]
["93030","ZENERGY - RAMA, H2200 X D300 X W300",815.4,"1-ZE-01",null,null,"OE_FRAME_2200","93030","SZT","85389099",null,null,"5901988930301","OE - Cadre, H2200 x P300 x P300","OE - Frame, H2200 x D300 x W300","OE- ESTRUCTURA, H2200 x D300 x W300","ZENERGY - KERET, H2200 X D300 X W300"]
["93060","ZENERGY - RAMA, H2200 X D300 X W600",947.5,"1-ZE-01",null,null,"OE_FRAME_2200","93060","SZT","85389099",null,null,"5901988930608","OE - Cadre, H2200 x P300 x L600","OE - Frame, H2200 x D300 x W600","OE- ESTRUCTURA, H2200 x D300 x W600","ZENERGY - KERET, H2200 X D300 X W600"]
["93081","ZENERGY - RAMA, H2200 X D300 X W800, 650+150",1270.0999999999999,"1-ZE-01",null,null,"OE_FRAME_2200","93081","SZT","85389099",null,null,"5901988930813","OE - Cadre, H2200 x P300 x L800, 650 + 150","OE - Frame, H2200 x D300 x W800, 650 + 150","OE- ESTRUCTURA, H2200 x D300 x W800, 650+150","ZENERGY – KERET, H2200 X D300 X W800, 650+150"]
["93100","ZENERGY - RAMA, H2200 X D300 X W1000",1123.4000000000001,"1-ZE-01",null,null,"OE_FRAME_2200","93100","SZT","85389099",null,null,"5901988931001","OE - Cadre, H2200 x P300 x P1000","OE - Frame, H2200 x D300 x W1000","OE- ESTRUCTURA, H2200 x D300 x W1000","ZENERGY - KERET, H2200 X D300 X W1000"]
["93111","ZENERGY - RAMA, H2200 X D300 X W1100, 650+450",1454.9,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988931117","OE - Cadre, H2200 x P300 x L1100, 650 + 450","OE - Frame, H2200 x D300 x W1100, 650 + 450","OE- ESTRUCTURA, H2200 x D300 x W1100, 650+450","ZENERGY – KERET, H2200 X D300 X W1100, 650+450"]
["93120","ZENERGY - RAMA, H2200 X D300 X W1200",1211.8,"1-ZE-01",null,null,"OE_FRAME_2200","93120","SZT","85389099",null,null,"5901988931209","OE - Cadre, H2200 x P300 x L1200","OE - Frame, H2200 x D300 x W1200","OE- ESTRUCTURA, H2200 x D300 x W1200","ZENERGY - KERET, H2200 X D300 X W1200"]
["93150","ZENERGY - RAMA, H2200 X D300 X W1500, 650+850",1619.5,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988931506","OE - Cadre, H2200 x P300 x L1500, 650 + 850","OE - Frame, H2200 x D300 x W1500, 650 + 850","OE- ESTRUCTURA, H2200 x D300 x W1500, 650+850","ZENERGY – KERET, H2200 X D300 X W1500, 650+850"]
["93163","ZENERGY - RAMA, H2200 X D300 X W1600, 650+300+650",1962.2,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988931636","OE - Cadre, H2200 x P300 x L1600, 650 + 300 + 650","OE - Frame, H2200 x D300 x W1600, 650 + 300 + 650","OE- ESTRUCTURA, H2200 x D300 x W1600, 650+300+650","ZENERGY – KERET, H2200 X D300 X W1600, 650+300+650"]
["93164","ZENERGY - RAMA, H2200 X D300 X W1600, 650+150+650+150",2072,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988931643","OE - Cadre, H2200 x P300 x L1600, 650 + 150 + 650 + 150","OE - Frame, H2200 x D300 x W1600, 650 + 150 + 650 + 150","OE- ESTRUCTURA, H2200 x D300 x W1600, 650+150+650+150","ZENERGY – KERET, H2200 X D300 X W1600, 650+150+650+150"]
["94040","ZENERGY - RAMA, H2200 X D400 X W400",922.9,"1-ZE-01",3.3333333333333333E-2,2,"OE_FRAME_2200","94040","SZT","85389099",null,null,"5901988940409","OE - Cadre, H2200 x P400 x P400","OE - Frame, H2200 x D400 x W400","OE- ESTRUCTURA, H2200 x D400 x W400","ZENERGY - KERET, H2200 X D400 X W400"]
["94061","ZENERGY - RAMA, H2200 X D400 X W600, 450+150",1367.5,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988940614","OE - CADRE, H2200 X P400 X L600, 450+150","OE - Frame, H2200 x D400 x H600, 450+150","*OE - MARCO, H2200 x D400 x W600, 450+150","ZENERGY – KERET, H2200 X D400 X W600, 450+150"]
["94081","ZENERGY - RAMA, H2200 X D400 X W800 650+150",1435.8,"1-ZE-01",0.01,1,"OE_FRAME_2200","94081","SZT","85389099","27.12.40.0",null,"5901988940812","OE - Cadre, H2200 x P400 x P800 650 + 150","OE - Frame, H2200 x D400 x W800 650 + 150","OE- ESTRUCTURA, H2200 x D400 x W800 650+150","ZENERGY – KERET, H2200 X D400 X W800 650+150"]
["94095","ZENERGY - RAMA, H2200 X D400 X W950, 650+300",1486.2,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988940959","OE - Cadre, H2200 x P400 x L950, 650 + 300","OE - Frame, H2200 x D400 x W950, 650 + 300","OE- ESTRUCTURA, H2200 x D400 x W950, 650+300","ZENERGY – KERET, H2200 X D400 X W950, 650+300"]
["94111","ZENERGY - RAMA, H2200 X D400 X W1100, 650+450",1546.7,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988941116","OE - Cadre, H2200 x P400 x L1100, 650 + 450","OE - Frame, H2200 x D400 x W1100, 650 + 450","OE- ESTRUCTURA, H2200 x D400 x W1100, 650+450","ZENERGY – KERET, H2200 X D400 X W1100, 650+450"]
["94121","ZENERGY - RAMA, H2200 X D400 X W1200, 150+650+400",1863.7,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988941215","OE - Cadre, H2200 x P400 x L1200, 150 + 650 + 400","OE - Frame, H2200 x D400 x W1200, 150 + 650 + 400","OE- ESTRUCTURA, H2200 x D400 x W1200, 150+650+400","ZENERGY – KERET, H2200 X D400 X W1200, 150+650+400"]
["94129","OE - Rama, H2200 x D400 x W1200, słupek 74mm",1355.2,"1-ZE-01",null,null,"OE_FRAME_2200","94129","SZT",null,null,"240801RT","5901988941291","OE - Cadre, H2200 x P400 x L1200, poteau de cadre 74mm","OE - Frame, H2200 x D400 x W1200, frame post 74mm","OE- ESTRUCTURA, H2200 x D400 x W1200, poste del marco 74mm","OE - keret, H2200 x D400 x 1200, oszlop 74 mm"]
["94130","ZENERGY - RAMA, H2200 X D400 X W1300",1311.5,"1-ZE-01",0.01,1,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988941307","OE - Cadre, H2200 x P400 x L1300","OE - Frame, H2200 x D400 x W1300","OE- ESTRUCTURA, H2200 x D400 x W1300","ZENERGY - KERET, H2200 X D400 X W1300"]
["94145","ZENERGY - RAMA, H2200 X D400 X W1450, 650+150+650",1964.5,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988941451","OE - Cadre, H2200 x P400 x P1450, 650 + 150 + 650","OE - Frame, H2200 x D400 x W1450, 650 + 150 + 650","OE- ESTRUCTURA, H2200 x D400 x W1450, 650+150+650","ZENERGY – KERET, H2200 X D400 X W1450, 650+150+650"]
["94160","ZENERGY - RAMA, H2200 X D400 X W1600, 800+800",1678.9,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988941604","OE - Cadre, H2200 x P400 x L1600, 800 + 800","OE - Frame, H2200 x D400 x W1600, 800 + 800","OE- ESTRUCTURA, H2200 x D400 x W1600, 800+800","ZENERGY – KERET, H2200 X D400 X W1600, 800+800"]
["94671","ZENERGY - RAMA, H2200 X D400/D600 POLE NAROŻNE, KOMPLETNE",3441.8,"1-ZE-01",null,null,"OE_FRAME_2200","94671","KPL","85389099",null,null,"5901988946715","OE - Cadre, boîte d'angle H2200 x P600/P400, complète","OE - Frame, H2200 x D600 / D400 corner area, complete","OE- ESTRUCTURA H2200XD600 / D400 ESQUINA, COMPLETO","ZENERGY - KERET, H2200 X D400/D600 SAROKTERÜLET, TELJES"]
["95345","ZENERGY - DRZWI PRZEDZIAŁU KABLOWEGO IP30, H2200 X W450",370.7,"1-ZE-01",0.01,1,"OE_FRAME_INTERNAL",null,"SZT","85389099",null,null,"5901988953454","OE - PORTE DU COMPARTIMENT CÂBLES IP30, H2200 X L450","OE - Cable compartment door IP30, H2200 x W450","*OE - PUERTA DEL COMPARTIMIENTO DE CABLES IP30, H2200 x W450","ZENERGY - KÁBELREKESZ AJTÓ IP30, H2200 X W450"]
["96060","ZENERGY - RAMA, H2200 X D600 X W600",1348.5,"1-ZE-01",null,null,"OE_FRAME_2200","96060","SZT","85389099",null,null,"5901988960605","OE - Cadre, H2200 x P600 x L600","OE - Frame, H2200 x D600 x W600","OE- ESTRUCTURA, H2200 x D600 x W600","ZENERGY - KERET, H2200 X D600 X W600"]
["96071","ZENERGY - RAMA, H2200 X D600 POLE NAROŻNE, KOMPLETNE",3441.8,"1-ZE-01",null,null,"OE_FRAME_2200","96071","KPL","85389099",null,null,"5901988960711","OE - Cadre, boîte d'angle H2200 x P600, complète","OE - Frame, H2200 x D600 corner area, complete","OE- ESTRUCTURA ÁREA DE ESQUINA H2200XD600, COMPLETO","ZENERGY - KERET, H2200 X D600 SAROKTERÜLET, TELJES"]
["96085","ZENERGY - RAMA, H2200 X D600 X W850",1462.7,"1-ZE-01",4.1666666666666664E-2,4,"OE_FRAME_2200","96085","SZT","8538909900",null,null,"5901988960858","OE - Cadre, H2200 x P600 x L850","OE - Frame, H2200 x D600 x W850","OE- ESTRUCTURA, H2200 x D600 x W850","ZENERGY - KERET, H2200 X D600 X W850"]
["96086","ZENERGY - RAMA, H2200 X D600 X W850, 650+200",1869.3,"1-ZE-01",null,null,"OE_FRAME_2200","96086","SZT","85389099",null,null,"5901988960865","OE - Cadre, H2200 x P600 x L850, 650 + 200","OE - Frame, H2200 x D600 x W850, 650 + 200","OE- ESTRUCTURA, H2200 x D600 x W850, 650+200","ZENERGY – KERET, H2200 X D600 X W850, 650+200"]
["96097","ZENERGY - RAMA, H2200 X D600 X W950, 800+150",1917.4,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT",null,null,null,null,null,null,null,"ZENERGY – KERET, H2200 X D600 X W950, 800+150"]
["96110","ZENERGY - RAMA, H2200 X D600 X W1100, 150+650+300",2408,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961107","OE - Cadre, H2200 x P600 x L1100, 150 + 650 + 300","OE - Frame, H2200 x D600 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H2200 x D600 x W1100, 150+650+300","ZENERGY – KERET, H2200 X D600 X W1100, 150+650+300"]
["96114","ZENERGY - RAMA, H2200 X D600 X W1100, (450+200)+450",2391.1999999999998,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961145","OE - Cadre, H2200 x P600 x L1100, (450 + 200) +450","OE - Frame, H2200 x D600 x W1100, (450 + 200) +450","OE- ESTRUCTURA, H2200 x D600 x W1100, (450+200)+450","ZENERGY - KERET, H2200 X D600 X W1100, (450+200)+450"]
["96120","ZENERGY - RAMA, H2200 X D600 X W1200",1624,"1-ZE-01",null,null,"OE_FRAME_2200","96120","SZT","85389099",null,null,"5901988961206","OE - Cadre, H2200 x P600 x L1200","OE - Frame, H2200 x D600 x W1200","OE- ESTRUCTURA, H2200 x D600 x W1200","ZENERGY - KERET, H2200 X D600 X W1200"]
["96130","ZENERGY - RAMA, H2200 X D600 X W1300",1669.9,"1-ZE-01",null,null,"OE_FRAME_2200","96130","SZT","85389099",null,null,"5901988961305","OE - Cadre, H2200 x P600 x L1300","OE - Frame, H2200 x D600 x W1300","OE- ESTRUCTURA, H2200 x D600 x W1300","ZENERGY - KERET, H2200 X D600 X W1300"]
["96141","ZENERGY - RAMA, H2200 X D600 X W1400, 400+850+150",2515.5,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961411","OE - Cadre, H2200 x P600 x L1400, 400 + 850 + 150","OE - Frame, H2200 x D600 x W1400, 400 + 850 + 150","OE- ESTRUCTURA, H2200 x D600 x W1400, 400+850+150","ZENERGY – KERET, H2200 X D600 X W1400, 400+850+150"]
["96149","ZENERGY - RAMA, H2200 X D600 X W1450, 400+850+200",2686.9,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961497","OE - CADRE, H2200 X P600 x L1450, 400+850+200","OE - Frame, H2200 x D600 x H1450, 400+850+200","*OE - MARCO, H2200 x D600 x W1450, 400+850+200","ZENERGY – KERET, H2200 X D600 X W1450, 400+850+200"]
["96150","ZENERGY - RAMA, H2200 X D600 X W1500, 650+850",2149.3000000000002,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961503","OE - Cadre, H2200 x P600 x L1500, 650 + 850","OE - Frame, H2200 x D600 x W1500, 650 + 850","OE- ESTRUCTURA, H2200 x D600 x W1500, 650+850","ZENERGY – KERET, H2200 X D600 X W1500, 650+850"]
["96160","ZENERGY - RAMA, H2200 X D600 X W1600, 800+800",2117.9,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961602","OE - Cadre, H2200 x P600 x L1600, 800 + 800","OE - Frame, H2200 x D600 x W1600, 800 + 800","OE- ESTRUCTURA, H2200 x D600 x W1600, 800+800","ZENERGY – KERET, H2200 X D600 X W1600, 800+800"]
["96165","ZENERGY - RAMA, H2200 X D600 X W1650, 650+150+850",2401.3000000000002,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988961657","OE - CADRE, H2200 X P600 x L1650, 650+150+850","OE - Frame, H2200 x D600 x H1650, 650+150+850","*OE - MARCO, H2200 x D600 x W1650, 650+150+850","ZENERGY – KERET, H2200 X D600 X W1650, 650+150+850"]
["98030","ZENERGY - RAMA, H2200 X D800 X W300",1307,"1-ZE-01",null,null,"OE_FRAME_2200","98030","SZT","85389099",null,null,"5901988980306","OE - Cadre, H2200 x P800 x L300","OE - Frame, H2200 x D800 x W300","OE- ESTRUCTURA, H2200 x D800 x W300","ZENERGY - KERET, H2200 X D800 X W300"]
["98060","ZENERGY - RAMA, H2200 X D800 X W600",1444.8,"1-ZE-01",0.15833333333333333,2,"OE_FRAME_2200","98060","SZT","85389099",null,null,"5901988980603","OE - Cadre, H2200 x P800 x L600","OE - Frame, H2200 x D800 x W600","OE- ESTRUCTURA, H2200 x D800 x W600","ZENERGY - KERET, H2200 X D800 X W600"]
["98071","Zenergy - Rama, H2200 X D800 Pole narożne, Kompletne",3954.7,"1-ZE-01",0.01,1,"OE_FRAME_2200","98071","KPL","85389099",null,null,"5901988980719","OE - Cadre, boîte d'angle H2200 x P800, complète","OE - Frame, H2200 x D800 corner field, complete","OE- ESTRUCTURA CAMPO DE ESQUINA H2200XD800, COMPLETO","Zenergy - Keret, H2200 X D800 Sarokdoboz, Komplett"]
["98080","ZENERGY - RAMA, H2200 X D800 X W800",1536.6,"1-ZE-01",null,null,"OE_FRAME_2200","98080","SZT","85389099",null,null,"5901988980801","OE - Cadre, H2200 x P800 x L800","OE - Frame, H2200 x D800 x W800","OE- ESTRUCTURA, H2200 x D800 x W800","ZENERGY - KERET, H2200 X D800 X W800"]
["98085","ZENERGY - RAMA, H2200 X D800 X W850",1560.2,"1-ZE-01",1.6666666666666666E-2,1,"OE_FRAME_2200","98085","SZT","85389099",null,null,"5901988980856","OE - Cadre, H2200 x P800 x L850","OE - Frame, H2200 x D800 x W850","OE- ESTRUCTURA, H2200 x D800 x W850","ZENERGY - KERET, H2200 X D800 X W850"]
["98086","ZENERGY - RAMA, H2200 X D800 X W850, 650+200",2014.9,"1-ZE-01",9.166666666666666E-2,6,"OE_FRAME_2200","98086","SZT","85389099",null,null,"5901988980863","OE - Cadre, H2200 x P800 x L850, 650 + 200","OE - Frame, H2200 x D800 x W850, 650 + 200","OE- ESTRUCTURA, H2200 x D800 x W850, 650+200","ZENERGY – KERET, H2200 X D800 X W850, 650+200"]
["98100","ZENERGY - RAMA, H2200 X D800 X W1000",1628.5,"1-ZE-01",null,null,"OE_FRAME_2200","98100","SZT","85389099",null,null,"5901988981006","OE - Cadre, H2200 x P800 x L1000","OE - Frame, H2200 x D800 x W1000","OE- ESTRUCTURA, H2200 x D800 x W1000","ZENERGY - KERET, H2200 X D800 X W1000"]
["98110","ZENERGY - RAMA, H2200 X D800 X W1100, 150+650+300",2574.9,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988981105","OE - Cadre, H2200 x P800 x L1100, 150 + 650 + 300","OE - Frame, H2200 x D800 x W1100, 150 + 650 + 300","OE- ESTRUCTURA, H2200 x D800 x W1100, 150+650+300","ZENERGY – KERET, H2200 X D800 X W1100, 150+650+300"]
["98120","ZENERGY - RAMA, H2200 X D800 X W1200",1720.3,"1-ZE-01",null,null,"OE_FRAME_2200","98120","SZT","85389099",null,null,"5901988981204","OE - Cadre, H2200 x P800 x L1200","OE - Frame, H2200 x D800 x W1200","OE- ESTRUCTURA, H2200 x D800 x W1200","ZENERGY - KERET, H2200 X D800 X W1200"]
["98125","ZENERGY - RAMA, H2200 X D800 X W1250, 850+400",2159.4,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988981259","OE - Cadre, H2200 x P800 x L1250, 850 + 400","OE - Frame, H2200 x D800 x W1250, 850 + 400","OE- ESTRUCTURA, H2200 x D800 x W1250, 850+400","ZENERGY – KERET, H2200 X D800 X W1250, 850+400"]
["98129","OE - Rama, H2200 x D800 x W1200, słupek 74mm",1771.8,"1-ZE-01",null,null,"OE_FRAME_2200","98129","SZT",null,null,"240801RT","5901988981297","OE - Cadre, H2200 x P800 x L1200, poteau de cadre 74mm","OE - Frame, H2200 x D800 x W1200, frame post 74mm","OE- ESTRUCTURA, H2200 x D800 x W1200, poste del marco 74mm","OE - Keret, H2200 x D800 x W1200, oszlop 74 mm"]
["98160","ZENERGY - RAMA, H2200 X D800 X W1600, 800+800",2235.5,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988981600","OE - Cadre, H2200 x P800 x L1600, 800 + 800","OE - Frame, H2200 x D800 x W1600, 800 + 800","OE- ESTRUCTURA, H2200 x D800 x W1600, 800+800","ZENERGY – KERET, H2200 X D800 X W1600, 800+800"]
["98163","ZENERGY - RAMA, H2200 X D800 X W1600, 650+300+650",2745.1,"1-ZE-01",null,null,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988981631","OE - Cadre, H2200 x P800 x L1600, 650 + 300 + 650","OE - Frame, H2200 x D800 x W1600, 650 + 300 + 650","OE- ESTRUCTURA, H2200 x D800 x W1600, 650+300+650","ZENERGY – KERET, H2200 X D800 X W1600, 650+300+650"]
["98173","ZENERGY - RAMA, H2200 X D800 X W1700, 850+200+650",2772,"1-ZE-01",1.6666666666666666E-2,1,"OE_FRAME_2200",null,"SZT","85389099",null,null,"5901988981730","OE - CADRE, H2200 X P800 x L1700, 850+200+650","OE - Frame, H2200 x D800 x H1700, 850+200+650","*OE - MARCO, H2200 x D800 x W1700, 850+200+650","ZENERGY – KERET, H2200 X D800 X W1700, 850+200+650"]
["99224","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, STAŁE IP30, H2200 X D230",407,"1-ZE-01",null,null,"OE_COVERS","99224","SZT","85389099",null,null,"5901988992248","OE - Évents latéraux, ventilés, fixes IP30, H2200 x P230","OE - Ventilated, fixed side covers IP30, H2200 x D230","OE- PAREDES LATERALES VENTIL. FIJO IP30, H2200 x D230 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK, RÖGZÍTETT IP30, H2200 X D230"]
["99232","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H2200 X D300",431.2,"1-ZE-01",null,null,"OE_COVERS","99232","SZT","85389099",null,null,"5901988992323","OE - Couvercles latéraux ventilés, plats, à visser IP30, H2200 x P300","OE - Side panels ventilated, flat, screwed on, IP30, H2200 x D300","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H2200 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H2200 X D300"]
["99242","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H2200 X D400",456.5,"1-ZE-01",null,null,"OE_COVERS","99242","SZT","85389099",null,null,"5901988992422","OE - Orifices latéraux, ventilés, plats et vissés IP30, H2200 x P400","OE - Side panels ventilated, flat, screwed on, IP30, H2200 x D400","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H2200 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H2200 X D400"]
["99262","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP30, H2200 X D600",484,"1-ZE-01",null,null,"OE_COVERS","99262","SZT","85389099",null,null,"5901988992620","OE - Écrans latéraux ventilés, plats et vissés IP30, H2200 x P600","OE - Side panels ventilated, flat, screwed on, IP30, H2200 x D600","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP30, H2200 x D600 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP30, H2200 X D600"]
["99324","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H2200 X D230",228.8,"1-ZE-01",null,null,"OE_COVERS","99324","SZT","85389099",null,null,"5901988993245","OE - Couvercles latéraux complets, fixes IP30, H2200 x P230","OE - Plain, fixed side covers IP30, H2200 x D230","OE- PAREDES LATERALES LISO FIJO IP30, H2200 x D230 (2UDS)","ZENERGY - TELJES OLDALSÓ BURKOLATOK, RÖGZÍTETT IP30, H2200 X D230"]
["99330","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2200 D300",752.4,"1-ZE-01",null,null,"OE_COVERS","99330","SZT","85389099",null,null,"5901988993306","OE - Couvercles latéraux complets IP30, H2200 P300","OE - Plain side covers IP30, H2200 D300","OE- PAREDES LATERALES LISO IP30, H2200 D300 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H2200 D300"]
["99331","ZENERGY - OSŁONY BOCZNE PEŁNE, STAŁE IP30, H2200 X D300",358.6,"1-ZE-01",1.6666666666666666E-2,2,"OE_COVERS","99331","SZT","85389099",null,null,"5901988993313","OE - Couvercles latéraux complets, fixes IP30, H2200 x P300","OE - Plain, fixed side covers IP30, H2200 x D300","OE- PAREDES LATERALES LISO FIJO IP30, H2200 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, RÖGZÍTETT, IP30, H2200 X D300"]
["99340","ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2200 D400",764.6,"1-ZE-01",0.05,2,"OE_COVERS","99340","SZT","85389099","27.12.40.0",null,"5901988993405","OE - Capots latéraux complets IP30, H2200 P400","OE - Plain side covers IP30, H2200 D400","OE- PAREDES LATERALES LISO IP30, H2200 D400  (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP30, H2200 D400"]
["99345","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H2200 X D400",198.2,"1-ZE-01",0.01,1,"OE_SEPARATION_BUSBAR","99345","SZT","85389099",null,null,"5901988993450","OE - Panneau de séparation, vertical, galvanisé, H2200 x P400","OE - Vertical partition, Galvanized, H2200 x D400","OE- TABIQUE VERTIC. GALV. H2200XD400","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H2200 X D400"]
["99365","ZENERGY - PRZEGRODA ODDZIELAJĄCA PIONOWA, OCYNK,  H2200 X D600",227.4,"1-ZE-01",null,null,"OE_SEPARATION_BUSBAR","99365","SZT","85389099",null,null,"5901988993658","OE - Panneau de séparation, vertical, galvanisé, H2200 x P600","OE - Vertical partition, Galvanized, H2200 x D600","OE- TABIQUE VERTIC. GALV. H2200XD600","ZENERGY - FÜGGŐLEGES VÁLASZVÁLASZTÁS, HORGANYOZOTT, H2200 X D600"]
["99382","ZENERGY - OSŁONY BOCZNE PEŁNE, PŁASKIE, PRZYKRĘCANE IP30, H2200 X D800",704,"1-ZE-01",null,null,"OE_COVERS","99382","SZT","85389099",null,null,"5901988993825","OE - Capots latéraux solides, plats, vissés IP30, H2200 x P800","OE - Side panels Plain, flat, screwed on, IP30, H2200 x D800","OE- PAREDES LATERALES LISO PLANO ATORNILLADO IP30, H2200 x D800 (2UDS)","ZENERGY - OLDALBURKOLATOK, TELJES, LAPOS, CSAVAROS IP30, H2200 X D800"]
["99425","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP43, H2200 X D230",508.2,"1-ZE-01",null,null,"OE_COVERS","99225","SZT","85389099",null,null,"5901988994259","OE - Couvercles latéraux, ventilés, plats, vissés IP43, H2200 x P230","OE - Side panels ventilated, flat, screwed on, IP43, H2200 x D230","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP43, H2200 x D230 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP43, H2200 X D230"]
["99432","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP43, H2200 X D300",558.79999999999995,"1-ZE-01",null,null,"OE_COVERS","99232","SZT","85389099",null,null,"5901988994327","OE - Orifices latéraux, ventilés, plats et vissés IP43, H2200 x P300","OE - Side panels ventilated, flat, screwed on, IP43, H2200 x D300","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP43, H2200 x D300 (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP43, H2200 X D300"]
["99442","ZENERGY - OSŁONY BOCZNE WENTYLOWANE, PŁASKIE, PRZYKRĘCANE IP43, H2200 X D400",612.70000000000005,"1-ZE-01",null,null,"OE_COVERS","99242","SZT","85389099",null,null,"5901988994426","OE - Caches latéraux ventilés, plats, à visser, IP43, H2200 x P400","OE - Side panels ventilated, flat, screwed on, IP43, H2200 x D400","OE- PAREDES LATERALES VENTIL. PLANO ATORNILLADO IP43, H2200 x D400  (2UDS)","ZENERGY - OLDALBURKOLATOK, SZELLŐZTETT, LAPOS, CSAVAROS IP43, H2200 X D400"]
["99460","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H2200 D600",999,"1-ZE-01",0.01,1,"OE_COVERS","99260","SZT","85389099",null,null,"5901988994600","OE - Hottes de ventilation latérales IP43, H2200 P600","OE - IP43, H2200 D600 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H2200 D600 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H2200 D600"]
["99480","ZENERGY - OSŁONY BOCZNE WENTYLOWANE IP43, H2200 D800",1085.7,"1-ZE-01",null,null,"OE_COVERS","99480","SZT","85389099",null,null,"5901988994808","OE - Hottes de ventilation latérales IP43, H2200 P800","OE - IP43, H2200 D800 Ventilated side covers","OE- PAREDES LATERALES VENTIL.IP43, H2200 D800 (2UDS)","ZENERGY - SZELLŐZTETT OLDALBURKOLATOK IP43, H2200 D800"]
["99510","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H2200 D1000",959.2,"1-ZE-01",0.01,1,"OE_COVERS","99310","SZT","85389099",null,null,"5901988995102","OE - Couvercles latéraux complets IP55, H2200 P1000","OE - Plain side covers IP55, H2200 D1000","OE- PAREDES LATERALES LISO IP55, H2200 D1000","ZENERGY - TELJES OLDALBURKOLATOK IP55, H2200 D1000"]
["99580","ZENERGY - OSŁONY BOCZNE PEŁNE IP55, H2200 D800",1134.0999999999999,"1-ZE-01",0.01,1,"OE_COVERS","99380","SZT","85389099",null,null,"5901988995805","OE - Couvercles latéraux complets IP55, H2200 P800","OE - Plain side covers IP55, H2200 D800","OE- PAREDES LATERALES LISO IP55, H2200 D800 (2UDS)","ZENERGY - TELJES OLDALBURKOLATOK IP55, H2200 D800"]
["191065661","PÓŁKA 19\" WYSUWNA GŁĘBOKOŚĆ 660MM",162.4,"1-ZE-01",null,null,null,null,"SZT",null,null,null,null,null,null,null,"19\" TOSZTÓPOLC, MÉLYSÉG 660MM"]
["03061R","ZENERGY - POPRZECZKA RAMY W600 450+150",81.900000000000006,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,null,"OE - Barre transversale L600 450 + 150","OE - Crossbar for the frame W600 450 + 150","OE- TRAVIESA W600 450+150","ZENERGY - KERESZTTEREM W600 450+150"]
["03066L","ZENERGY - POPRZECZKA RAMY W650 150+500",84.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,null,"OE - Crossbar L650 150 + 500","OE - Crossbar for the frame W650 150 + 500","OE- TRAVIESA W650 150+500","ZENERGY - KERESZTTEREM W650 150+500"]
["03067R","ZENERGY - POPRZECZKA RAMY W650 450+200",84.7,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030674","OE - cadre L650 450 + 200 cadre","OE - Crossbar for the W650 450 + 200 frame","OE- TRAVIESA W650 450+200","ZENERGY - KERESZTTEREM W650 450+200"]
["03081L","ZENERGY - POPRZECZKA RAMY W800 150+650",98.4,"1-ZE-10",0.85833333333333328,4,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988930813","OE - Barre transversale L800 150 + 650","OE - Crossbar for the frame W800 150 + 650","OE- TRAVIESA W800 150+650","ZENERGY - KERESZTTEREM W800 150+650"]
["03086R","ZENERGY - POPRZECZKA RAMY W850 650+200",99.5,"1-ZE-10",1,1,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988030865","OE - Crossbar L850 650 + 200","OE - Crossbar for the W850 650 + 200 frame","OE- TRAVIESA W850 650+200","ZENERGY - KERESZTTEREM W850 650+200"]
["03097L","ZENERGY - POPRZECZKA RAMY W950 150+800",115.6,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"OE - W950 150+800 TRAVERSE DE CADRE","OE - W950 150+800 Frame crossmember","*OE - W950 150+800 TRAVESAÑO DE MARCO","ZENERGY - KERESZTTEREM W950 150+800"]
["03102L","ZENERGY - POPRZECZKA RAMY W1000 150+850",118.8,"1-ZE-10",0.38333333333333336,2,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,null,"OE - Bordure de cadre L1000 150 + 850","OE - Crossbar for the W1000 150 + 850 frame","OE- TRAVIESA W1000 150+850","ZENERGY - KERESZTTEREM W1000 150+850"]
["03105R","produkt wycofany (ZENERGY - POPRZECZKA RAMY W1050 650+400)",136.6,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099","27.12.40.0",null,"5901988031053","produit invalidé OE - Bordure de cadre L1050 650 + 400","product cancelled OE - Crossbar for the W1050 650 + 400 frame","OE- TRAVIESA W1050 650+400","kivont termék (ZENERGY - FRAME CROSS-BAR W1050 650+400)"]
["03110R","produkt wycofany (ZENERGY - POPRZECZKA RAMY W1100 150+650+300)",131,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"produit invalidé OE - Crossbar W1100 150 + 650 + 300","product cancelled OE - Crossbar for the frame W1100 150 + 650 + 300","OE- TRAVIESA W1100 150+650+300","kivont termék (ZENERGY - FRAME CROSS-BAR W1100 150+650+300)"]
["03115R","produkt wycofany (ZENERGY - POPRZECZKA RAMY W1150 850+300)",146.69999999999999,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"produit invalidé OE - Barre transversale W1150 850 + 300","product cancelled OE - Crossbar for the frame W1150 850 + 300","OE- TRAVIESA W1150 850+300","kivont termék (ZENERGY - FRAME CROSS-BAR W1150 850+300)"]
["03120L","ZENERGY - POPRZECZKA RAMY W1200, PODWÓJNE DRZWI, DOLNA",150.1,"1-ZE-10",0.15,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"OE - Traverse L1200, double porte, bas","OE - Crossbar for W1200 frame, double door, bottom","OE- TRAVIESA W1200, PARA PUERTA DOBLE, ABAJO","ZENERGY - W1200 KERET KERESZTREÁD, KÉT AJTÓS, ALSÓ"]
["03120R","ZENERGY - POPRZECZKA RAMY W1200, PODWÓJNE DRZWI, GÓRNA",150.1,"1-ZE-10",0.15,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"OE - Crossbar L1200, Portes double, haut","OE - Crossbar for W1200 frame, double door, top","OE- TRAVIESA W1200, PARA PUERTA DOBLE, ARRIBA","ZENERGY - W1200 KERET KERESZT RÚD, DULA AJTÓS, FELSŐ"]
["03123R","produkt wycofany (ZENERGY - POPRZECZKA RAMY W1200 650+150+400)",141.1,"1-ZE-10",null,null,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"produit invalidé OE - Barre transversale L1200 650 + 150 + 400","product cancelled OE - Crossbar of the frame W1200 650 + 150 + 400","OE- TRAVIESA W1200 650+150+400","kivont termék (ZENERGY - POFRAME BAR W1200 650+150+400)"]
["03130R","ZENERGY - POPRZECZKA RAMY W1300, PODWÓJNE DRZWI, GÓRNA",159.80000000000001,"1-ZE-10",1.6666666666666666E-2,1,"OE_SKD_PARTS",null,"SZT","85389099",null,null,null,"OE - Crossbar L1300, double porte, haut","OE - Crossbar for W1300 frame, double door, top","OE- TRAVIESA W1300, PARA PUERTA DOBLE, ARRIBA","ZENERGY - W1300 KERET KERESZT RÚD, DULA AJTÓ, FELSŐ"]
["10027.0600","AlCubar - Profil anodowany H27, 277mm2, 1 rowek Cu 8mm, 630A dt 55C - 600mm",78.400000000000006,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10027.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C - 600mm","AlCubar - Aluminum anodized busbar profile Al-Cu H27, 360 mm2, 1 Copper row, 8 mm, 630A dt 39C, 800A dt 57C - 600mm","*AlCubar - Perfil H27 anodizado, 277mm2, 1 ranura Cu 8mm, 630A dt 55C - 600mm","AlCubar - Eloxált profil H27, 277mm2, 1 Cu horony 8mm, 630A dt 55C - 600mm"]
["10027.1400","AlCubar - Profil anodowany H27, 277mm2, 1 rowek Cu 8mm, 630A dt 55C - 1400mm",183,"1-ZE-08",0.2,1,"OE_BUSBARS_ALCUBAR",null,"SZT","7604299000",null,null,null,null,null,null,"AlCubar - Eloxált profil H27, 277mm2, 1 Cu horony 8mm, 630A dt 55C - 1400mm"]
["10051.0600","AlCubar - Profil anodowany H50, 480mm2, 1 rowek Cu, 1000A dt 55C - 600mm",116.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10051.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé H50, 480 mm2, 1 gorge Cu, 1000A dt 55C - 600mm","AlCubar - Aluminum anodized busbar profile Al-Cu H50 480 mm2, 1 copper groove, 1000A dt 55C - 600mm","*AlCubar - Perfil anodizado H50, 480mm2, 1 ranura Cu, 1000A dt 55C - 600mm","AlCubar - H50 eloxált profil, 480mm2, 1 Cu horony, 1000A dt 55C - 600mm"]
["10051.1750","AlCubar - Profil anodowany H50, 480mm2, 1 rowek Cu, 1000A dt 55C - 1750mm",344,null,0.11666666666666667,1,"OE_BUSBARS_ALCUBAR",null,null,"76042990",null,null,"5901988900199"]
["10075.0600","AlCubar - Profil anodowany H75, 1100 mm2, 2 rowki Cu, 1600A dt 55C - 600mm",209.1,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10075.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé AlCubar H75, 1100 mm2, 2 rainures en Cu, 1600A dt 55C - 600mm","ALCubar - Aluminum anodized busbar profile Al-Cu  H75, 1100 mm2, 2 Copper rows, 1600A dt 55C - 600mm","*AlCubar - Perfil anodizado H75, 1100 mm2, 2 ranuras Cu, 1600A dt 55C - 600mm","AlCubar - H75 eloxált profil, 1100 mm2, 2 Cu horony, 1600A dt 55C - 600mm"]
["10075.0975","AlCubar - Profil anodowany H75, 1100 mm2, 2 rowki Cu, 1600A dt 55C - 975mm",278.10000000000002,null,null,null,"OE_BUSBARS_ALCUBAR",null,null,"7604299000",null,null,"5901988900205"]
["10075.1750","AlCubar - Profil anodowany H75, 1100 mm2, 2 rowki Cu, 1600A dt 55C - 1750mm",609.79999999999995,"1-ZE-08",0.54166666666666663,5,"OE_BUSBARS_ALCUBAR","10075.1750","SZT","7604299000",null,"231026PW","5901988100759","AlCubar - Profilé anodisé AlCubar H75, 1100 mm2, 2 rainures en Cu, 1600A dt 55C - 1750mm","ALCubar - Aluminum anodized busbar profile Al-Cu  H75, 1100 mm2, 2 Copper rows, 1600A dt 55C - 1750mm","*AlCubar - Perfil anodizado H75, 1100 mm2, 2 ranuras Cu, 1600A dt 55C - 1750mm","AlCubar - H75 eloxált profil, 1100 mm2, 2 Cu horony, 1600A dt 55C - 1750mm"]
["10075.1950","AlCubar - Profil anodowany H75, 1100 mm2, 2 rowki Cu, 1600A dt 55C - 1950mm",679.5,"1-ZE-08",0.11666666666666667,1,"OE_BUSBARS_ALCUBAR","10075.1950","SZT","7604299000",null,"231026PW","5901988100759","AlCubar - Profilé anodisé AlCubar H75, 1100 mm2, 2 rainures en Cu, 1600A dt 55C - 1950mm","ALCubar - Aluminum anodized busbar profile Al-Cu  H75, 1100 mm2, 2 Copper rows, 1600A dt 55C - 1950mm","*AlCubar - Perfil anodizado H75, 1100 mm2, 2 ranuras Cu, 1600A dt 55C - 1950mm","AlCubar - H75 eloxált profil, 1100 mm2, 2 Cu horony, 1600A dt 55C - 1950mm"]
["10100.0600","AlCubar - Profil anodowany H100R, 2490mm2, 2 rowki Cu, 8mm/12mm, 2500A dt 55C - 600mm",356.4,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10100.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé AlCubar H100R, 2490mm2, 2 rainures en Cu, 8 mm et 12 mm, 2500A dt 50C - 600mm","AlCubar - Aluminum anodized busbar profile Al-Cu H100R, 2490mm2, 2 Copper rows, 8 mm & 12 mm, 2500A dt 50C - 600mm","*AlCubar - Perfil anodizado H100R, 2490mm2, 2 ranuras Cu, 8mm/12mm, 2500A dt 55C - 600mm","AlCubar - Eloxált profil H100R, 2490mm2, 2 Cu horony, 8mm/12mm, 2500A dt 55C - 600mm"]
["10100.1700","AlCubar - Profil anodowany H100R, 2490mm2, 2 rowki Cu, 8mm/12mm, 2500A dt 55C - 1700mm",908.8,null,null,null,"OE_BUSBARS_ALCUBAR",null,null,"76042990",null,null,"5909831261442"]
["10102.0600","AlCubar - Profil anodowany H100, 2500 mm2, 2 rowki Cu, 2500A dt 53C - 600mm",360.7,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10102.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 53C - 600mm","AlCubar - Aluminum anodized busbar profile Al-Cu H100, 2500 mm2, 2 copper grooves, 2500A dt 53C - 600mm","*AlCubar - Perfil anodizado H100, 2500 mm2, 2 ranuras Cu, 2500A dt 53C - 600mm","AlCubar - Eloxált profil H100, 2500 mm2, 2 Cu horony, 2500A dt 53C - 600mm"]
["10102.0975","AlCubar - Profil anodowany H100, 2500 mm2, 2 rowki Cu 8mm, 2500A dt 53C - 975mm",527.6,null,null,null,"OE_BUSBARS_ALCUBAR",null,null,"7604299000",null,null,"5901988900212"]
["10102.1750","AlCubar - Profil anodowany H100, 2500 mm2, 2 rowki Cu 8mm, 2500A dt 53C - 1750mm",1052.0999999999999,"1-ZE-08",0.34166666666666667,2,"OE_BUSBARS_ALCUBAR","10102.1750","SZT","7604299000","24.42.22.0","231121PW","5901988900045","AlCubar - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 53C - 1750mm","AlCubar - Aluminum anodized busbar profile Al-Cu H100, 2500 mm2, 2 copper grooves, 2500A dt 53C - 1750mm","*AlCubar - Perfil anodizado H100, 2500 mm2, 2 ranuras Cu, 2500A dt 53C - 1750mm","AlCubar - Eloxált profil H100, 2500 mm2, 2 Cu horony 8mm, 2500A dt 53C - 1750mm"]
["10102.1950","AlCubar - Profil anodowany H100, 2500 mm2, 2 rowki Cu 8mm, 2500A dt 53C - 1950mm",1172.4000000000001,"1-ZE-08",0.1,1,"OE_BUSBARS_ALCUBAR","10102.1950","SZT","7604299000","24.42.22.0","231121PW","5901988900076","AlCubar - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 53C - 1950mm","AlCubar - Aluminum anodized busbar profile Al-Cu H100, 2500 mm2, 2 copper grooves, 2500A dt 53C - 1950mm","*AlCubar - Perfil anodizado H100, 2500 mm2, 2 ranuras Cu, 2500A dt 53C - 1950mm","AlCubar - Eloxált profil H100, 2500 mm2, 2 Cu horony 8mm, 2500A dt 53C - 1950mm"]
["10106P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H400 X W600 2X24MOD IP40, 6H MOD + DRZWI PEŁNE",547.6,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988472986"]
["10109P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H550 X W600 3X24MOD IP40, 9H MOD + DRZWI PEŁNE",650.20000000000005,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988472993"]
["10112P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H700 X W600 4X24MOD IP40, 12H MOD + DRZWI PEŁNE",744.1,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988473006"]
["10115P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H850 X W600 5X24MOD IP40, 15H MOD + DRZWI PEŁNE",887.8,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988473013"]
["10118P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1000 X W600 6X24MOD IP40, 18H MOD + DRZWI PEŁNE",1040,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988473020"]
["10121P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1150 X W600 7X24MOD IP40, 21H MOD + DRZWI PEŁNE",1197.7,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988473037"]
["10124P","ZENERGY PT - ROZDZIELNICA PODTYNKOWA H1300 X W600 8X24MOD IP40, 24H MOD + DRZWI PEŁNE",1347.8,"1-ZE-03",0.01,1,"PT_ENCLOSURES",null,null,"85381000",null,null,"5901988473044"]
["10150.0600","AlCubar - Profil anodowany H150R, 3727mm2, 3 rowki Cu, 8mm i 12mm, 3400A dt 55C - 600mm",547.20000000000005,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10150.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé AlCubar H150R, 3727mm2, 3 rainures en Cu, 8 mm et 12 mm, 3400A dt 55C - 600mm","Aluminum anodized busbar profile Al-Cu AlCubar H150R, 3727mm2, 3 Copper rows, 8 mm & 12 mm, 3400A dt 55C - 600mm","*AlCubar - Perfil anodizado H150R, 3727mm2, 3 ranuras Cu, 8mm y 12mm, 3400A dt 55C - 600mm","AlCubar - Eloxált profil H150R, 3727mm2, 3 Cu horony, 8mm és 12mm, 3400A dt 55C - 600mm"]
["10154.0600","AlCubar - Profil anodowany H150, 3427mm2, 4 rowki Cu 8mm, 3200A dt 55C - 600mm",481.1,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10154.0600","SZT",null,null,"231205RT",null,"AlCubar - Profilé anodisé AlCubar H150, 3427mm2, 4 rainures en Cu, 8 mm.  3200A dt 55C - 600mm","Aluminum anodized busbar profile Al-Cu AlCubar H150, 3427mm2, 4 Copper rows, 8 mm, 3200A dt 55C - 600mm","ALCUB- PERFIL ALCUBAR H150, 4CU 3200A L=1000MM - 600mm","AlCubar - Eloxált profil H150, 3427mm2, 4 Cu horony 8mm, 3200A dt 55C - 600mm"]
["10154.1750","AlCubar - Profil anodowany H150, 3427mm2, 4 rowki Cu 8mm, 3200A dt 55C - 1750mm",1403.3,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10154.1750","SZT","7604299000",null,"231121PW","5901988900083","AlCubar - Profilé anodisé AlCubar H150, 3427mm2, 4 rainures en Cu, 8 mm.  3200A dt 55C - 1750mm","Aluminum anodized busbar profile Al-Cu AlCubar H150, 3427mm2, 4 Copper rows, 8 mm, 3200A dt 55C - 1750mm","ALCUB- PERFIL ALCUBAR H150, 4CU 3200A L=1000MM - 1750mm","AlCubar - Eloxált profil H150, 3427mm2, 4 Cu horony 8mm, 3200A dt 55C - 1750mm"]
["10154.1950","AlCubar - Profil anodowany H150, 3427mm2, 4 rowki Cu 8mm, 3200A dt 55C - 1950mm",1563.8,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","10154.1950","SZT",null,null,"240813LK","5901988900083","AlCubar - Profilé anodisé AlCubar H150, 3427mm2, 4 rainures en Cu, 8 mm.  3200A dt 55C - 1950mm","Aluminum anodized busbar profile Al-Cu AlCubar H150, 3427mm2, 4 Copper rows, 8 mm, 3200A dt 55C - 1950mm","ALCUB- PERFIL ALCUBAR H150, 4CU 3200A L=1000MM - 1950mm","AlCubar - Eloxált profil H150, 3427mm2, 4 Cu horony 8mm, 3200A dt 55C - 1950mm"]
["120404CP","ZENERGY - OBUDOWA H1200, W400, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA, DRZWI POJEDYNCZE  IP55",6334.9,null,null,null,"OE_CABINETS",null,null,"",null,null,""]
["120404P","ZENERGY - OBUDOWA H1200, W400, D400,  PŁYTA MONTAŻOWA,  IP55",3906.1,"1-ZE-01",0.01,1,"OE_CABINETS",null,null,"",null,null,""]
["180504CP","ZENERGY - OBUDOWA H1800, W500, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",4900,"1-ZE-01",0.01,1,"OE_CABINETS",null,null,"",null,null,""]
["180604C2P","ZENERGY - OBUDOWA H1800, W600, D400, COKÓŁ H200,  PŁYTA MONTAŻOWA,  IP55",5342.6,"1-ZE-01",0.01,1,"OE_CABINETS",null,null,"",null,null,""]
["180804CP","ZENERGY - OBUDOWA H1800, W800, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",5038.1000000000004,"1-ZE-01",3.3333333333333333E-2,2,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H1800, W800, D400, LÁZAT H100, SZERELŐLEMEZ, IP55"]
["20021.0950","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C 950MM",234,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C 950mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C 950mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 6 mm, 630A dt 39C, 800A dt 57C 950mm","AlCubar - ANODIZÁLT PROFIL ALCUBAR H27, 360 MM2, 1 CU BARNA, 6 MM, 630A DT 39C, 800A DT 57C 950MM"]
["20021.0980","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C 980MM",242,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C 980mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C 980mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 6 mm, 630A dt 39C, 800A dt 57C 980mm","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU BARNA, 6 MM, 630A DT 39C, 800A DT 57C 980MM"]
["20021.1030","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C 1030MM",254,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C 1030mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C 1030mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 6 mm, 630A dt 39C, 800A dt 57C 1030mm","AlCubar - ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 6 MM, 630A DT 39C, 800A DT 57C 1030MM"]
["20021.1260","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C 1260MM",312,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C 1260mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C 1260mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 6 mm, 630A dt 39C, 800A dt 57C 1260mm","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 6 MM, 630A DT 39C, 800A DT 57C 1260MM"]
["20021.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C 1750MM",432,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C 1750mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C 1750mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 6 mm, 630A dt 39C, 800A dt 57C 1750mm","AlCubar - ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 6 MM, 630A DT 39C, 800A DT 57C 1750MM"]
["20021.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 6 MM, 630A DT 39C, 800A DT 57C 2200MM",542,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 6 mm, 630A dt 39C, 800A dt 57C 2200mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 6 mm, 630A dt 39C, 800A dt 57C 2200mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 6 mm, 630A dt 39C, 800A dt 57C 2200mm","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 6 MM, 630A DT 39C, 800A DT 57C 2200MM"]
["20022.0475","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 475MM",117.2,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 475mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 475mm","ALCUBAR-PERFIL AL-CU H27  1CU 8MM, 630A L=0.475METRO","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 475MM"]
["20022.0660","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 660MM",162.80000000000001,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 660MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 660mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 660MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU BARNA, 8 MM, 630A DT 39C, 800A DT 57C 660MM"]
["20022.0855","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 855MM",210,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 855MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 855mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 855MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 855MM"]
["20022.0877","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 877MM",216,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 877MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 877mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 877MM","AlCubar - ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 877MM"]
["20022.1000","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1000MM",246,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20022.1000","SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 1000mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 1000mm","ALCUB-PERFIL AL-CU H27  1CU 8MM, 630A UNIDAD L=1METRO","AlCubar - ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU BARNA, 8 MM, 630A DT 39C, 800A DT 57C 1000MM"]
["20022.1005","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1005MM",248,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1005MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1005mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1005MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1005MM"]
["20022.1048","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1048MM",258,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1048MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1048mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1048MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1048MM"]
["20022.1200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1200MM",296,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 1200mm","AlCu - Anodised AlCubar H27 profile, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 1200mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 8 mm, 630A dt 39C, 800A dt 57C 1200mm","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU BARNA, 8 MM, 630A DT 39C, 800A DT 57C 1200MM"]
["20022.1400","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1400MM",346,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 1400mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 1400mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 8 mm, 630A dt 39C, 800A dt 57C 1400mm","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1400MM"]
["20022.1470","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1470MM",362,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1470MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1470mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1470MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1470MM"]
["20022.1498","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1498MM",370,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1498MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1498mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1498MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1498MM"]
["20022.1500","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1500MM",370,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1500MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1500mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1500MM","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1500MM"]
["20022.1550","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1550MM",382,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1550MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1550mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1550MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1550MM"]
["20022.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1750MM",432,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20022.1750","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 1750mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 1750mm","ALCUB-PERFIL AL-CU H27  1CU 8MM, 630A L=1750mm","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1750MM"]
["20022.1777","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1777MM",438,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1777MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1777mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1777MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1777MM"]
["20022.1927","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1927MM",476,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1927MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1927mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1927MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1927MM"]
["20022.1948","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1948MM",480,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 1948MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 1948mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 1948MM","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1948MM"]
["20022.1950","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 1950MM",482,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20022.1950","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 1950mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 1950mm","ALCUB-PERFIL AL-CU H27  1CU 8MM, 630A L=1950mm","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 1950MM"]
["20022.2000","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2000MM",494,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 2000mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 2000mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 8 mm, 630A dt 39C, 800A dt 57C 2000mm","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2000MM"]
["20022.2077","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2077MM",512,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 2077MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 2077mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 2077MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2077MM"]
["20022.2125","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2125MM",524,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 2125MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 2125mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 2125MM","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2125MM"]
["20022.2155","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2155MM",532,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 2155MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 2155mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 2155MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2155MM"]
["20022.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2200MM",542,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 2200mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 2200mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 8 mm, 630A dt 39C, 800A dt 57C 2200mm","AlCubar – ANODIZÁLT PROFILOS AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2200MM"]
["20022.2305","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2305MM",568,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 2305MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 2305mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 2305MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2305MM"]
["20022.2398","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2398MM",592,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H27 ANODISÉ, 360 MM2, 1 RAINURE CU, 8 MM, 630A DT 39C, 800A DT 57C 2398MM","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 CU groove, 8 mm, 630A dt 39C, 800A dt 57C 2398mm","*AlCu - PERFIL ANODIZADO ALCUBAR H27, 360 MM2, 1 CU RANURA, 8 MM, 630A DT 39C, 800A DT 57C 2398MM","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2398MM"]
["20022.2500","ALCUBAR - PROFIL ANODOWANY ALCUBAR H27, 360 MM2, 1 ROWEK CU, 8 MM, 630A DT 39C, 800A DT 57C 2500MM",618,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H27, 360 mm2, 1 rainure Cu, 8 mm, 630A dt 39C, 800A dt 57C 2500mm","AlCu - AlCubar Anodized profile H27, 360 mm2, 1 Cu groove, 8 mm, 630A dt 39C, 800A dt 57C 2500mm","Perfil AlCubar anodizado H27, 360 mm2, 1 ranura Cu, 8 mm, 630A dt 39C, 800A dt 57C 2500mm","AlCubar – ANODIZÁLT PROFIL AlCubar H27, 360 MM2, 1 CU HORVÁNY, 8 MM, 630A DT 39C, 800A DT 57C 2500MM"]
["20030.0645","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 645MM",250,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20030.0645","SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H50R, 2 rainures en cuivre, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C - 645mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 645mm","ALCUB- PERFIL AL-CU H50R, 2CU, 8 MM, 1000A L=645mm","AlCubar - ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 645MM"]
["20030.0750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 750MM",290,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 750MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 750mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 750MM","AlCubar - ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 750MM"]
["20030.0845","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 845MM",328,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20030.0845","SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H50R, 2 rainures en cuivre, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C - 845mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 845mm","ALCUB- PERFIL AL-CU H50R,  2 CU, 8 MM, 1000A L=845mm","AlCubar - ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 845MM"]
["20030.0894","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 894MM",346,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 894MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 894mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 894MM","AlCubar – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 894MM"]
["20030.1048","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1048MM",406,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1048MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1048mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1048MM","AlCubar – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1048MM"]
["20030.1100","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1100MM",426,"1-ZE-08",0.13333333333333333,1,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1100MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1100mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1100MM","AlCubar – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1100MM"]
["20030.1175","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1175MM",456,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1175MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1175mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1175MM","AlCubar – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1175MM"]
["20030.1180","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1180MM",458,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1180MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1180mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1180MM","AlCubar – ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1180MM"]
["20030.1200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1200MM",466,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1200MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1200mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1200MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1200MM"]
["20030.1344","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1344MM",522,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1344MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1344mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1344MM","ALKUBÁR – ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1344MM"]
["20030.1380","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1380MM",534,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1380MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1380mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1380MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1380MM"]
["20030.1425","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1425MM",552,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1425MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1425mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1425MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1425MM"]
["20030.1470","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1470MM",570,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H50R, 2 rainures en cuivre, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C - 1470mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1470mm","Perfil AlCubar H50R anodizado, 2 canales Cu, 8 mm y 12 mm, 1000A dt 39C, 1250A dt 58C - 1470mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1470MM"]
["20030.1480","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1480MM",574,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1480MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1480mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1480MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1480MM"]
["20030.1494","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1494MM",580,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1494MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1494mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1494MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1494MM"]
["20030.1498","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1498MM",580,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1498MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1498mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1498MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1498MM"]
["20030.1600","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1600MM",620,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1600MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1600mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1600MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1600mm"]
["20030.1620","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1620MM",628,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1620MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1620mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1620MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1620MM"]
["20030.1648","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1648MM",640,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1648MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1648mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1648MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1648MM"]
["20030.1694","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1694MM",656,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1694MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1694mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1694MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1694MM"]
["20030.1700","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1700MM",660,"1-ZE-08",0.51666666666666672,2,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H50R, 2 rainures en cuivre, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C - 1700mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1700mm","Perfil AlCubar H50R anodizado, 2 canales Cu, 8 mm y 12 mm, 1000A dt 39C, 1250A dt 58C - 1700mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1700MM"]
["20030.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1750MM",678,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20030.1750","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50R, 2 rainures en Cu, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C 1750mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1750mm","ALCUB- PERFIL AL-CU H50R, 2 CU, 8 MM, 1000A L=1750mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1750MM"]
["20030.1770","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1770MM",686,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1770MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1770mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1770MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1770MM"]
["20030.1794","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1794MM",696,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1794MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1794mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1794MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1794MM"]
["20030.1825","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1825MM",708,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1825MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1825mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1825MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1825MM"]
["20030.1944","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1944MM",754,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1944MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1944mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1944MM","ALKUBÁR – ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1944MM"]
["20030.1948","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1948MM",756,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1948MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1948mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1948MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1948MM"]
["20030.1950","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1950MM",756,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20030.1950","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50R, 2 rainures Cu, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C 1950mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1950mm","ALCUB- PERFIL AL-CU H50R,  2 CU, 8 MM, 1000A L=1950mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1950MM"]
["20030.1975","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 1975MM",766,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 1975MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 1975mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 1975MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 1975MM"]
["20030.2000","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2000MM",776,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50R, 2 rainures en Cu, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C 2000mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2000mm","Perfil AlCubar H50R anodizado, 2 canales Cu, 8 mm y 12 mm, 1000A dt 39C, 1250A dt 58C - 2000mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2000MM"]
["20030.2094","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2094MM",812,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2094MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2094mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2094MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2094MM"]
["20030.2142","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2142MM",830,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2142MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2142mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2142MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2142MM"]
["20030.2195","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2195MM",852,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2195MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2195mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2195MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2195MM"]
["20030.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2200MM",852,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50R, 2 rainures en Cu, 8 mm et 12 mm, 1000A dt 39C, 1250A dt 58C 2200mm","AlCu - AlCubar Anodized profile H50R, 2 Cu grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2200mm","Perfil AlCubar H50R anodizado, 2 canales Cu, 8 mm y 12 mm, 1000A dt 39C, 1250A dt 58C - 2200mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2200MM"]
["20030.2300","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2300MM",892,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2300MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2300mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2300MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2300MM"]
["20030.2345","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2345MM",910,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2345MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2345mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2345MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2345MM"]
["20030.2398","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2398MM",930,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2398MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2398mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2398MM","ALKUBÁR – ANODIZÁLT PROFIL ALCUBAR H50R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2398MM"]
["20030.2500","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2500MM",970,"1-ZE-08",3.3333333333333333E-2,2,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2500MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2500mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2500MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2500MM"]
["20030.2525","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2525MM",980,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2525MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2525mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2525MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2525MM"]
["20030.2550","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50R, 2 ROWKI CU, 8 MM I 12 MM, 1000A DT 39C, 1250A DT 58C - 2550MM",988,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 1000A DT 39C, 1250A DT 58C - 2550MM","AlCu - AlCubar Anodized profile H50R, 2 CU grooves, 8 mm and 12 mm, 1000A dt 39C, 1250A dt 58C - 2550mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50R, 2 CU RANURAS, 8 MM Y 12 MM, 1000A DT 39C, 1250A DT 58C - 2550MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H50R, 2 CU BAROVE, 8 MM ÉS 12 MM, 1000A DT 39C, 1250A DT 58C - 2550MM"]
["20031.0575","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 1 ROWEK CU, 1000A DT 40C, 1250A DT 58C - 575MM",113.7,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT",null,null,null,null,null,null,null,"ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H50, 670 MM2, 1 CU HORVÁNY, 1000A DT 40C, 1250A DT 58C - 575MM"]
["20031.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 1 ROWEK CU, 1000A DT 40C, 1250A DT 58C - 1750MM",640,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50, 670 mm2, 1 gorge Cu, 1000A dt 40C, 1250A dt 58C 1750mm","AlCu - AlCubar Anodized profile H50, 670 mm2, 1 Cu groove, 1000A dt 40C, 1250A dt 58C - 1750mm","Perfil AlCubar H50 anodizado, 670 mm2, 1 ranura Cu, 1000A dt 40C, 1250A dt 58C - 1750mm","ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H50, 670 MM2, 1 CU GROOVE, 1000A DT 40C, 1250A DT 58C - 1750MM"]
["20031.1950","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 1 ROWEK CU, 1000A DT 40C, 1250A DT 58C - 1950MM",712,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50, 670 mm2, 1 gorge Cu, 1000A dt 40C, 1250A dt 58C 1950mm","AlCu - Anodized profile AlCubar H50, 670 mm2, 1 Cu groove, 1000A dt 40C, 1250A dt 58C - 1950mm","Perfil AlCubar H50 anodizado, 670 mm2, 1 ranura Cu, 1000A dt 40C, 1250A dt 58C - 1950mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H50, 670 MM2, 1 CU HORVÁNY, 1000A DT 40C, 1250A DT 58C - 1950MM"]
["20032.1700","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 2 ROWKI CU, 1000A DT 40C, 1250A DT 58C - 1700MM",712,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50 ANODISÉ, 670 MM2, 2 RAINURES CU, 1000A DT 40C, 1250A DT 58C - 1700MM","AlCu - AlCubar Anodized profile H50, 670 mm2, 2 CU grooves, 1000A dt 40C, 1250A dt 58C - 1700mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50, 670 MM2, 2 CU RANURAS, 1000A DT 40C, 1250A DT 58C - 1700MM","ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H50, 670 MM2, 2 CU HORVÁZAT, 1000A DT 40C, 1250A DT 58C - 1700MM"]
["20032.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 2 ROWKI CU, 1000A DT 40C, 1250A DT 58C - 1750MM",734,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20032.1750","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50, 670 mm2, 2 rainures Cu, 1000A dt 40C, 1250A dt 58C 1750mm","AlCu - AlCubar Anodized profile H50, 670 mm2, 2 Cu grooves, 1000A dt 40C, 1250A dt 58C - 1750mm","ALCUB- PERFIL AL-CU H50, 2 CU, 8MM, 1000A,  L- 1750mm","ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H50, 670 MM2, 2 CU VONÁZAT, 1000A DT 40C, 1250A DT 58C - 1750MM"]
["20032.2000","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 2 ROWKI CU, 1000A DT 40C, 1250A DT 58C - 2000mm",838,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H50 ANODISÉ, 670 MM2, 2 RAINURES CU, 1000A DT 40C, 1250A DT 58C - 2000mm","AlCu - AlCubar Anodized profile H50, 670 mm2, 2 CU grooves, 1000A dt 40C, 1250A dt 58C - 2000mm","*AlCu - PERFIL ANODIZADO ALCUBAR H50, 670 MM2, 2 CU RANURAS, 1000A DT 40C, 1250A DT 58C - 2000mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H50, 670 MM2, 2 CU BAROVE, 1000A DT 40C, 1250A DT 58C - 2000mm"]
["20032.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H50, 670 MM2, 2 ROWKI CU, 1000A DT 40C, 1250A DT 58C - 2200MM",922,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H50, 670 mm2, 2 rainures en Cu, 1000A dt 40C, 1250A dt 58C 2200mm","AlCu - AlCubar Anodized profile H50, 670 mm2, 2 Cu grooves, 1000A dt 40C, 1250A dt 58C - 2200mm","Perfil AlCubar H50 anodizado, 670 mm2, 2 canales Cu, 1000A dt 40C, 1250A dt 58C - 2200mm","ALKUBÁR – ANODIZÁLT PROFILOS ALKUBÁR H50, 670 MM2, 2 CU HORVÁNY, 1000A DT 40C, 1250A DT 58C - 2200MM"]
["20042.0540","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 540MM",282,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 540MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 540mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 540MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 540MM"]
["20042.0645","AlCubar - Profil anodowany AlCubar H80, 1280 mm2, 2 rowki Cu, 1600A dt 47C, 2000A dt 69C - 645mm",338,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20042.0645","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C 1750mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 0645mm","ALCUB- PERFIL  AL-CU H80, 2 CU, 8MM, 1600A L=645mm","AlCubar - AlCubar H80 eloxált profil, 1280 mm2, 2 Cu horony, 1600A dt 47C, 2000A dt 69C - 645mm"]
["20042.0958","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 958MM",500,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C - 958mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 958mm","Perfil anodizado AlCubar H80, 1280 mm2, 2 canales Cu, 1600A dt 47C, 2000A dt 69C - 958mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 958MM"]
["20042.1198","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 1198MM",626,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 1198MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 1198mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 1198MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 1198MM"]
["20042.1700","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 1700MM",888,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 1700MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 1700mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 1700MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 1700MM"]
["20042.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 1750MM",914,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20042.1750","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C 1750mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 1750mm","ALCUB- PERFIL  AL-CU H80, 2 CU, 8MM, 1600A  L=1750mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 1750MM"]
["20042.1777","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 1777MM",928,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 1777MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 1777mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 1777MM","ALKUBÁR – ANODIZÁLT PROFILOS ALKUBÁR H80, 1280 MM2, 2 CU HORVÁZAT, 1600A DT 47C, 2000A DT 69C – 1777MM"]
["20042.1940","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 1940MM",1014,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 1940MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 1940mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 1940MM","ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 1940MM"]
["20042.1950","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 1950MM",1018,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C 1950mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 1950mm","Perfil anodizado AlCubar H80, 1280 mm2, 2 canales Cu, 1600A dt 47C, 2000A dt 69C - 1950mm","ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 1950MM"]
["20042.2140","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 2140MM",1118,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 2140MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 2140mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 2140MM","ALKUBÁR – ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2,2 CU HORVÁT, 1600A DT 47C, 2000A DT 69C - 2140MM"]
["20042.2180","AlCu - Profil anodowany AlCubar H80, 1280 mm2, 2 rowki Cu, 1600A dt 47C, 2000A dt 69C - 2180mm",1044,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT",null,null,null,null,"AlCu - profil anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C - 2180mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 2180mm","Perfil anodizado AlCubar H80, 1280 mm2, 2 ranuras Cu, 1600A dt 47C, 2000A dt 69C - 2180mm","AlCu - AlCubar H80 eloxált profil, 1280 mm2, 2 Cu horony, 1600A dt 47C, 2000A dt 69C - 2180mm"]
["20042.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 2200MM",1150,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C 2200mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 2200mm","Perfil anodizado AlCubar H80, 1280 mm2, 2 canales Cu, 1600A dt 47C, 2000A dt 69C - 2200mm","ALKUBÁR – ANODIZÁLT PROFILOS ALKUBÁR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C - 2200MM"]
["20042.2398","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 2398MM",1254,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 2398MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 2398mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 2398MM","ALKUBÁR – ANODIZÁLT PROFILOS ALKUBÁR H80, 1280 MM2, 2 CU HORVÁZAT, 1600A DT 47C, 2000A DT 69C - 2398MM"]
["20042.2500","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 2500MM",1306,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H80, 1280 mm2, 2 rainures Cu, 1600A dt 47C, 2000A dt 69C - 2500mm","AlCu - Anodized profile AlCubar H80, 1280 mm2, 2 Cu grooves, 1600A dt 47C, 2000A dt 69C - 2500mm","Perfil anodizado AlCubar H80, 1280 mm2, 2 canales Cu, 1600A dt 47C, 2000A dt 69C - 2500mm","ALKUBÁR - ANODIZÁLT PROFILOS ALKUBÁR H80, 1280 MM2, 2 CU HORVÁZAT, 1600A DT 47C, 2000A DT 69C - 2500MM"]
["20042.2588","ALCUBAR - PROFIL ANODOWANY ALCUBAR H80, 1280 MM2, 2 ROWKI CU, 1600A DT 47C, 2000A DT 69C - 2588MM",1352,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H80 ANODISÉ, 1280 MM2, 2 RAINURES CU, 1600A DT 47C, 2000A DT 69C - 2588MM","AlCu - AlCubar Anodized profile H80, 1280 mm2, 2 CU grooves, 1600A dt 47C, 2000A dt 69C - 2588mm","*AlCu - PERFIL ANODIZADO ALCUBAR H80, 1280 MM2, 2 CU RANURAS, 1600A DT 47C, 2000A DT 69C - 2588MM","ALKUBÁR – ANODIZÁLT PROFIL ALCUBAR H80, 1280 MM2, 2 CU VONÁZAT, 1600A DT 47C, 2000A DT 69C – 2588MM"]
["20050.0645","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 645MM",618,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20050.0645","SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H100R, 2 rainures en cuivre, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 645mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 645mm","ALCUB- PERFIL AL-CU H100R  2 CU, 8 MM, 2500A L=645mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 645MM"]
["20050.0730","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 730MM",698,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 730MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 730mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 730MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 730MM"]
["20050.0780","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 780MM",746,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 780MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 780mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 780MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU HORVÁNY, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 780MM"]
["20050.0845","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 845MM",808,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20050.0845","SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H100R, 2 rainures en cuivre, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 845mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 845mm","ALCUB- PERFIL AL-CU H100R  2 CU, 8 MM, 2500A L=845mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 845MM"]
["20050.0980","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 980MM",938,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 980MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 980mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 980MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU HORVÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 980MM"]
["20050.0990","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 990MM",948,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H100R, 2 rainures en cuivre, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 990mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 990mm","Perfil AlCubar H100R anodizado, 2 canales Cu, 8 mm y 12 mm, 2050A dt 50C, 2500A dt 67C - 990mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 990MM"]
["20050.1005","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1005MM",962,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1005MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1005mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1005MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HORVÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1005MM"]
["20050.1130","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1130MM",1082,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1130MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1130mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1130MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1130MM"]
["20050.1280","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1280MM",1224,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1280MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1280mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1280MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU VONÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1280MM"]
["20050.1330","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1330MM",1272,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1330MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1330mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1330MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1330MM"]
["20050.1388","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1388MM",1328,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1388MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1388mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1388MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1388MM"]
["20050.1480","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1480MM",1416,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1480MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1480mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1480MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1480MM"]
["20050.1530","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1530MM",1464,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1530MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1530mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1530MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU HORVÁNY, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1530MM"]
["20050.1590","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1590MM",1522,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1590MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1590mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1590MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1590MM"]
["20050.1600","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1600MM",1530,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1600MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1600mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1600MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU VANÁZ, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1600MM"]
["20050.1625","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1625MM",1554,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1625MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1625mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1625MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1625MM"]
["20050.1648","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1648MM",1576,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1648MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1648mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1648MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1648MM"]
["20050.1700","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1700MM",1626,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1700MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1700mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1700MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100R, 2 CU-HARÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1700MM"]
["20050.1766","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1766MM",1690,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1766MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1766mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1766MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1766MM"]
["20050.1800","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1800MM",1722,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1800MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1800mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1800MM","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1800MM"]
["20050.1980","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 1980MM",1894,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 1980MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 1980mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 1980MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 1980MM"]
["20050.2000","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 2000MM",1914,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H100R, 2 rainures en Cu, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 2000mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 2000mm","Perfil AlCubar H100R anodizado, 2 canales Cu, 8 mm y 12 mm, 2050A dt 50C, 2500A dt 67C - 2000mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU VONÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 2000MM"]
["20050.2040","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 2040MM",1952,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H100R, 2 rainures en Cu, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 2040mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 2040mm","Perfil AlCubar H100R anodizado, 2 canales Cu, 8 mm y 12 mm, 2050A dt 50C, 2500A dt 67C - 2040mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU-HOROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 2040MM"]
["20050.2180","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 2180MM",2086,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H100R, 2 rainures en cuivre, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 2180mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 2180mm","Perfil AlCubar H100R anodizado, 2 canales Cu, 8 mm y 12 mm, 2050A dt 50C, 2500A dt 67C - 2180mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU VANÁZ, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 2180MM"]
["20050.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 2200MM",2104,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H100R, 2 rainures en Cu, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 2200mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 2200mm","Perfil AlCubar H100R anodizado, 2 canales Cu, 8 mm y 12 mm, 2050A dt 50C, 2500A dt 67C - 2200mm","ALKUBÁR – ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU VANÁZ, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 2200MM"]
["20050.2300","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 2300MM",2200,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100R ANODISÉ, 2 RAINURES CU, 8 MM ET 12 MM, 2050A DT 50C, 2500A DT 67C - 2300MM","AlCu - AlCubar Anodized profile H100R, 2 CU grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 2300mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100R, 2 CU RANURAS, 8 MM Y 12 MM, 2050A DT 50C, 2500A DT 67C - 2300MM","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU BAROVE, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 2300MM"]
["20050.2500","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100R, 2 ROWKI CU, 8 MM I 12 MM, 2050A DT 50C, 2500A DT 67C - 2500MM",2392,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H100R, 2 rainures en cuivre, 8 mm et 12 mm, 2050A dt 50C, 2500A dt 67C - 2500mm","AlCu - AlCubar Anodized profile H100R, 2 Cu grooves, 8 mm and 12 mm, 2050A dt 50C, 2500A dt 67C - 2500mm","Perfil AlCubar H100R anodizado, 2 canales Cu, 8 mm y 12 mm, 2050A dt 50C, 2500A dt 67C - 2500mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100R, 2 CU VONÁZAT, 8 MM ÉS 12 MM, 2050A DT 50C, 2500A DT 67C - 2500MM"]
["20052.0645","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 645MM",648,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20052.0645","SZT","76042990","24.42.22.0",null,"5901988200527","AlCu - profil anodisé AlCubar H100, 2500 mm2, 2 rainures Cu, 2500A dt 55C - longueur 645mm","AlCu - Anodized profile AlCubar H100, 2500 mm2, 2 Cu grooves, 2500A dt 55C - length 645mm","ALCUB- PERFIL  ALCUB- H100, 2 CU, 8MM, 2500A L=645mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 645MM"]
["20052.1495","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 1495MM",1508,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20052.1495","SZT","76042990","24.42.22.0",null,null,"AlCu - profil anodisé AlCubar H100, 2500 mm2, 2 rainures Cu, 2500A dt 55C - longueur 1495mm (W650+W850)","AlCu - Anodized profile AlCubar H100, 2500 mm2, 2 Cu grooves, 2500A dt 55C - length 1495mm (W650 + W850)","ALCUB- PERFIL  ALCUB- H100, 2 CU, 2500A, L=1495mm (W650 + W850)","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 1495MM"]
["20052.1700","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 1700MM",1708,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100 ANODISÉ, 2500 MM2, 2 RAINURES CU, 2500A DT 55C - LONGUEUR 1700MM","AlCu - AlCubar Anodized profile H100, 2500 mm2, 2 CU grooves, 2500A dt 55C - LENGTH 1700mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100, 2500 MM2, 2 CU RANURAS, 2500A DT 55C - LONGITUD 1700MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 1700MM"]
["20052.1750","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 1750MM",1758,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR","20052.1750","SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 55C - longueur de 1750mm","AlCu - Anodized profile AlCubar H100, 2500 mm2, 2 Cu grooves, 2500A dt 55C - length 1750mm","ALCUB- PERFIL  ALCUB- H100, 2 CU, 2500A, L=1750mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU BAROVE, 2500A DT 55C - HOSSZ 1750 mm"]
["20052.1800","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 1800MM",1808,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100 ANODISÉ, 2500 MM2, 2 RAINURES CU, 2500A DT 55C - LONGUEUR 1800MM","AlCu - AlCubar Anodized profile H100, 2500 mm2, 2 CU grooves, 2500A dt 55C - LENGTH 1800mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100, 2500 MM2, 2 CU RANURAS, 2500A DT 55C - LONGITUD 1800MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 1800MM"]
["20052.1825","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 1825MM",1834,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures Cu, 2500A dt 55C - longueur 1825mm","AlCu - Anodized profile AlCubar H100, 2500 mm2, 2 Cu grooves, 2500A dt 55C - length 1825mm","Perfil anodizado AlCubar H100, 2500 mm2, 2 canales Cu, 2500A dt 55C - longitud 1825mm","ALKUBÁR - ANODIZÁLT PROFILOS ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 1825MM"]
["20052.2200","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 2200MM",2210,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - Profilé anodisé AlCubar H100, 2500 mm2, 2 rainures en Cu, 2500A dt 55C - Longueur de 2200mm","AlCu - Anodized profile AlCubar H100, 2500 mm2, 2 Cu grooves, 2500A dt 55C - length 2200mm","Perfil anodizado AlCubar H100, 2500 mm2, 2 canales Cu, 2500A dt 55C - longitud 2200mm","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 2200MM"]
["20052.2500","ALCUBAR - PROFIL ANODOWANY ALCUBAR H100, 2500 MM2, 2 ROWKI CU, 2500A DT 55C - DŁUGOŚĆ 2500MM",2512,"1-ZE-08",null,null,"OE_BUSBARS_ALCUBAR",null,"SZT","76042990","24.42.22.0",null,null,"AlCu - PROFIL ALCUBAR H100 ANODISÉ, 2500 MM2, 2 RAINURES CU, 2500A DT 55C - LONGUEUR 2500MM","AlCu - AlCubar Anodized profile H100, 2500 mm2, 2 CU grooves, 2500A dt 55C - LENGTH 2500mm","*AlCu - PERFIL ANODIZADO ALCUBAR H100, 2500 MM2, 2 CU RANURAS, 2500A DT 55C - LONGITUD 2500MM","ALKUBÁR - ANODIZÁLT PROFIL ALCUBAR H100, 2500 MM2, 2 CU VONÁZAT, 2500A DT 55C - HOSSZ 2500 mm"]
["200604CP","ZENERGY - OBUDOWA H2000, W600, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",5554.4,"1-ZE-08",0.01,1,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H2000, W600, D400, LÁZAT H100, SZERELŐLEMEZ, IP55"]
["2006060CP","ZENERGY - OBUDOWA H2000, W600, D600, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",6118.2,"1-ZE-08",1.6666666666666666E-2,1,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H2000, W600, D600, LÁZAT H100, SZERELŐLEMEZ, IP55"]
["200804CP","ZENERGY - OBUDOWA H2000, W800, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",6073.5,"1-ZE-08",0.01,1,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H2000, W800, D400, LÁZAT H100, SZERELŐLEMEZ, IP55"]
["200805CP","ZENERGY - OBUDOWA H2000, W800, D500, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",6566.8,"1-ZE-08",null,null,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H2000, W800, D500, PLINTH H100, SZERELŐLEMEZ, IP55"]
["200806CP","ZENERGY - OBUDOWA H2000, W800, D600, COKÓŁ H100,  PŁYTA MONTAŻOWA,  IP55",6749.6,"1-ZE-08",null,null,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H2000, W800, D600, LÁZAT H100, SZERELŐLEMEZ, IP55"]
["201004CP","ZENERGY - OBUDOWA H2000, W1000, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA, DRZWI POJEDYNCZE  IP55",6219.7,null,9.166666666666666E-2,4,"OE_CABINETS",null,null,"",null,null,"5901988024833"]
["201004CP2D","ZENERGY - OBUDOWA H2000, W1000, D400, COKÓŁ H100,  PŁYTA MONTAŻOWA, DRZWI PODWÓJNE  IP55",6572.2,"1-ZE-01",0.05,4,"OE_CABINETS",null,null,"",null,null,"5901988024840"]
["201006CP","ZENERGY - OBUDOWA H2000, W1000, D600, COKÓŁ H100,  PŁYTA MONTAŻOWA, DRZWI POJEDYNCZE IP55",6878.5,null,3.3333333333333333E-2,2,"OE_CABINETS",null,null,"",null,null,"5901988028831"]
["201006CP2D","ZENERGY - OBUDOWA H2000, W1000, D600, COKÓŁ H100,  PŁYTA MONTAŻOWA, DRZWI PODWÓJNE  IP55",7027.1,"1-ZE-01",0.01,1,"OE_CABINETS",null,null,"",null,null,"5901988024611"]
["201204CP2D","Zenergy - Obudowa H2000, W1200, D400, cokół H100,  płyta montażowa, drzwi podwójne  IP55",7527.8,"1-ZE-01",4.1666666666666664E-2,4,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"Zenergy - H2000, W1200, D400 ház, H100 lábazat, szerelőlap, IP55 dupla ajtó"]
["201206CP2D","ZENERGY - OBUDOWA H2000, W1200, D600, COKÓŁ H100,  PŁYTA MONTAŻOWA, DRZWI PODWÓJNE  IP55",7818.8,"1-ZE-01",0.01,1,"OE_CABINETS",null,"SZT",null,null,null,null,null,null,null,"ZENERGY - HÁZ H2000, W1200, D600, LÁZALOK H100, SZERELŐLEMEZ, DUPA AJTÓ IP55"]
["20129.0500","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, ROZSTAW 50,61MM, POLIWĘGLAN 15X240X500MM",85.9,"1-ZE-08",0.45833333333333331,5,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.33.14.0",null,null,null,null,null,"ALKUBÁR - ALCUBAR H27 HÍDBURKOLAT, TÉR 50,61MM, POLIKARBONÁT 15X240X500MM"]
["20129.0660","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, ROZSTAW 50,61MM, POLIWĘGLAN 15X240X660MM",115.5,"1-ZE-08",2.35,5,"OE_SEPARATION_BUSBAR","20129.0660","SZT","85389099","27.33.14.0",null,null,"AlCu - Couvercle de pont AlCubar H27, polycarbonate de 40x240mmx660mm","AlCu - AlCubar H27 bridge cover, distance 50.61mm, polycarbonate 15x240x660mm","ALCUB- TAPA PUENTE ALCUB- H27, POLICARBONATO 15X240X660MM","ALKUBÁR - ALCUBAR H27 HÍDBURKOLAT, TÉR 50,61MM, POLIKARBONÁT 15X240X660MM"]
["20129.1000","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, ROZSTAW 50,61MM, POLIWĘGLAN 15X240X1000MM",171.7,"1-ZE-08",0.1,1,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.33.14.0",null,null,null,null,null,"ALKUBÁR - ALCUBAR H27 HÍDBURKOLAT, TÉR 50,61MM, POLIKARBONÁT 15X240X1000MM"]
["20129.1500","ALCUBAR - OSŁONA MOSTU ALCUBAR H27, ROZSTAW 50,61MM, POLIWĘGLAN 15X240X1500MM",257.60000000000002,"1-ZE-08",0.1,1,"OE_SEPARATION_BUSBAR",null,"SZT","85389099","27.33.14.0",null,null,null,null,null,"ALKUBÁR - ALCUBAR H27 HÍDBURKOLAT, TÉR 50,61MM, POLIKARBONÁT 15X240X1500MM"]
["21076N","ZENERGY OM - SZYNA NEUTRALNA N W600, L=470 MM, 20 ZACISKÓW 16MM2 + 1 X M6",98.9,"1-ZE-09",3.3333333333333333E-2,1,"OM_ACCESSORIES",null,null,"85389099",null,null,"5901988473129"]
["22076N","ZENERGY OM - SZYNA NEUTRALNA N W600, L=470 MM, 40 ZACISKÓW 16MM2 + 1xM6",118.6,"1-ZE-09",3.3333333333333333E-2,1,"OM_ACCESSORIES",null,null,"85389099",null,null,"5901988473136"]
["31588.1","ZENERGY - Płyta dławicowa IP55, W800, D775, ocynk",364,"1-ZE-01",4.1666666666666664E-2,1,"OE_GLAND_PLATES",null,null,"85389099",null,null,""]
["62206P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H400 X W600 2X24MOD IP40, 6H MOD + DRZWI PEŁNE",586.4,"1-ZE-03",0.01,1,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473051"]
["62209P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H550 X W600 3X24MOD IP40, 9H MOD + DRZWI PEŁNE",688,"1-ZE-03",0.01,1,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473068"]
["62212P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H700 X W600 4X24MOD IP40, 12H MOD + DRZWI PEŁNE",784.1,"1-ZE-03",0.01,1,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473075"]
["62215P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H850 X W600 5X24MOD IP40, 15H MOD + DRZWI PEŁNE",915.8,"1-ZE-03",0.01,1,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473082"]
["62218P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1000 X W600 6X24MOD IP40, 18H MOD + DRZWI PEŁNE",1060.5999999999999,"1-ZE-03",0.01,1,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473099"]
["62221P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1150 X W600 7X24MOD IP40, 21H MOD + DRZWI PEŁNE",1206.4000000000001,"1-ZE-03",0.01,1,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473105"]
["62224P","ZENERGY ON - ROZDZIELNICA NATYNKOWA H1300 X W600 8X24MOD IP40, 24H MOD + DRZWI PEŁNE",1417,"1-ZE-03",null,null,"ON_ENCLOSURES",null,null,"85381000",null,null,"5901988473112"]
["APZEN1T2G-T2","AUTOMATYKA APZEN 1T2G BEZ UPS M221 TERM. HMISTU 5,7\" KOL.",16678.400000000001,null,null,null,null,null,null,"",null,null,"1234567234205"]
["APZEN2T1G1S1Z-T2","AUTOMATYKA APZEN 2T1G1S1Z BEZ UPS M221 TERM. HMISTU 5,7\" KOL.",27797,null,null,null,null,null,null,"",null,null,"2011767430526"]
["APZEN2T1G1S-T2","AUTOMATYKA APZEN 2T1G1S BEZ UPS M221 TERM HMISTU 5,7\" KOL.",22238.3,null,null,null,null,null,null,"",null,null,"2011767430557"]
["APZEN2T1G1S-T3","AUTOMATYKA APZEN-1T1G1S  BEZ UPS TM221 TERM. M2I 4\" - WYCOFANY",11070,null,null,null,null,null,null,"",null,null,""]
["APZEN2T1G1Z-T2","AUTOMATYKA APZEN 2T1G1Z BEZ UPS M221 TERM. HMISTU 5,7\" KOL.",22238.3,null,null,null,null,null,null,"",null,null,"2011767430533"]
["APZEN2T1G2S-T2","AUTOMATYKA APZEN 2T1G2S Z UPS M221 TERM. HMIGTO 7,5\" KOL.",32317.9,null,null,null,null,null,null,"",null,null,"2011767430540"]
["APZEN2T1G-S1","AUTOMATYKA APZEN 2T1G BEZ UPS TWIDO SYNOPTYKA TERM. SERWIS - WYCOFANY",8526.6,null,null,null,null,null,null,"",null,null,""]
["APZEN2T1G-T2","AUTOMATYKA APZEN 2T1G BEZ UPS M221 TERM. HMISTU 5,7\" KOL.",16678.400000000001,null,null,null,null,null,null,"",null,null,"2011767430564"]
["APZEN2T1G-T3","AUTOMATYKA APZEN 2T1G BEZ UPS M221 TERM. M2I 4\" - WYCOFANY",11070,null,null,null,null,null,null,"",null,null,""]
["APZEN2T1S1G-T1","AUTOMATYKA APZEN 2T1S1G BEZ UPS M221 PRZYCISKI LAMPKI",20878.599999999999,null,null,null,null,null,null,"",null,null,"2011767430496"]
["APZEN2T1S-S1","AUTOMATYKA APZEN 2T1S BEZ UPS TWIDO  SYNOPTYKA TERM. SERWIS - WYCOFANY",8526.6,null,null,null,null,null,null,"",null,null,""]
["APZEN2T1S-S2","AUTOMATYKA APZEN 2T1S BEZ UPS TWIDO  SYNOPTYKA  TERM. SERWIS  STYKI - WYCOFANY",8629.2000000000007,null,null,null,null,null,null,"",null,null,""]
["APZEN2T1S-T1","AUTOMATYKA APZEN 2T1S BEZ UPS M221 PRZYCISKI LAMPKI",15658.9,null,null,null,null,null,null,"",null,null,"2011767430519"]
["APZEN2T1S-T2","AUTOMATYKA APZEN 2T1S BEZ UPS M221 TERM. HMISTU 5,7\" KOL.",16678.400000000001,null,null,null,null,null,null,"",null,null,"2011767430571"]
["APZEN2T1S-T3","AUTOMATYKA APZEN 2T1S BEZ UPS M221 TERM. M2I 4\" - WYCOFANY",11070,null,null,null,null,null,null,"",null,null,""]
["APZEN2T-T1","AUTOMATYKA APZEN 2T BEZ UPS M221 PRZYCISKI LAMPKI",10439.299999999999,null,null,null,null,null,null,"",null,null,"2011767430502"]
["APZEN2T-T2","AUTOMATYKA APZEN 2T BEZ UPS M221 TERM HMISTU 3,5\"",10443.6,null,null,null,null,null,null,"",null,null,"2011767430588"]
["APZEN2T-T3","AUTOMATYKA APZEN 2T BEZ UPS M221 TERM. M2I 4\" - WYCOFANY",5745.6,null,null,null,null,null,null,"",null,null,""]
["MALCU4000P","AlCubar - Obudowa mostu szynowego H200, 4000A 260x465mm",1728,null,null,null,null,null,null,"7604299000",null,null,""]
["MALCUSUP500","AlCubar - Wspornik mostu szynowego 500mm",116.6,"1-ZE-08",null,null,null,null,null,"73181595",null,null,""]
["OU0151010P","OBUDOWA UNIWERSALNA OU H150 X W1000 X D100, PUSTA, DRZWI PEŁNE, IP41",202.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H150 X W1000 X D100, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU0151210P","OBUDOWA UNIWERSALNA OU H150 X W1200 X D100, PUSTA, DRZWI PEŁNE, IP41",207.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H150 X W1200 X D100, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU02003015P","OBUDOWA UNIWERSALNA OU H200 X W300 X D150, PUSTA, DRZWI PEŁNE, IP41",205.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H200 X W300 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU02004018P","OBUDOWA UNIWERSALNA OU H200 X W400 X D180, PUSTA, DRZWI PEŁNE, IP41",370.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H200 X W400 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU02405030P","OBUDOWA UNIWERSALNA OU H240 X W500 X D300, PUSTA, DRZWI PEŁNE, IP41",229,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H240 X W500 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU02503030P","OBUDOWA UNIWERSALNA OU H250 X W300 X D300, PUSTA, DRZWI PEŁNE, IP41",218,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H250 X W300 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03002015P","OBUDOWA UNIWERSALNA OU H300 X W200 X D150, PUSTA, DRZWI PEŁNE, IP41",199.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W200 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03002515P","OBUDOWA UNIWERSALNA OU H300 X W250 X D150, PUSTA, DRZWI PEŁNE, IP41",204.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W250 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03002530P","OBUDOWA UNIWERSALNA OU H300 X W250 X D300, PUSTA, DRZWI PEŁNE, IP41",211.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W250 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03003020P","OBUDOWA UNIWERSALNA OU H300 X W300 X D200, PUSTA, DRZWI PEŁNE, IP41",212.4,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W300 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03004020P","OBUDOWA UNIWERSALNA OU H300 X W400 X D200, PUSTA, DRZWI PEŁNE, IP41",217.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W400 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03004025P","OBUDOWA UNIWERSALNA OU H300 X W400 X D250, PUSTA, DRZWI PEŁNE, IP41",221.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W400 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03005020P","OBUDOWA UNIWERSALNA OU H300 X W500 X D200, PUSTA, DRZWI PEŁNE, IP41",221.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W500 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03005030P","OBUDOWA UNIWERSALNA OU H300 X W500 X D300, PUSTA, DRZWI PEŁNE, IP41",231.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H300 X W500 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU03503515P","OBUDOWA UNIWERSALNA OU H350 X W350 X D150, PUSTA, DRZWI PEŁNE, IP41",215.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H350 X W350 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04003020P","OBUDOWA UNIWERSALNA OU H400 X W300 X D200, PUSTA, DRZWI PEŁNE, IP41",217.9,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W300 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04003023P","OBUDOWA UNIWERSALNA OU H400 X W300 X D230, PUSTA, DRZWI PEŁNE, IP41",220.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W300 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04003025P","OBUDOWA UNIWERSALNA OU H400 X W300 X D250, PUSTA, DRZWI PEŁNE, IP41",221.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W300 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04003030P","OBUDOWA UNIWERSALNA OU H400 X W300 X D300, PUSTA, DRZWI PEŁNE, IP41",224.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W300 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04003520P","OBUDOWA UNIWERSALNA OU H400 X W350 X D200, PUSTA, DRZWI PEŁNE, IP41",221.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W350 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04004018P","OBUDOWA UNIWERSALNA OU H400 X W400 X D180, PUSTA, DRZWI PEŁNE, IP41",221.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W400 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04004020P","OBUDOWA UNIWERSALNA OU H400 X W400 X D200, PUSTA, DRZWI PEŁNE, IP41",224.8,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W400 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04004023P","OBUDOWA UNIWERSALNA OU H400 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",226.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04004030P","OBUDOWA UNIWERSALNA OU H400 X W400 X D300, PUSTA, DRZWI PEŁNE, IP41",233.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W400 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04004035P","OBUDOWA UNIWERSALNA OU H400 X W400 X D350, PUSTA, DRZWI PEŁNE, IP41",237.4,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W400 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04006020P","OBUDOWA UNIWERSALNA OU H400 X W600 X D200, PUSTA, DRZWI PEŁNE, IP41",237.4,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W600 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04006023P","OBUDOWA UNIWERSALNA OU H400 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",245.7,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04006025P","OBUDOWA UNIWERSALNA OU H400 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",255.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04006040P","OBUDOWA UNIWERSALNA OU H400 X W600 X D400, PUSTA, DRZWI PEŁNE, IP41",294.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W600 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04008023P","OBUDOWA UNIWERSALNA OU H400 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",299.60000000000002,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU04008025P","OBUDOWA UNIWERSALNA OU H400 X W800 X D250, PUSTA, DRZWI PEŁNE, IP41",303.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H400 X W800 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05002015P","OBUDOWA UNIWERSALNA OU H500 X W200 X D150, PUSTA, DRZWI PEŁNE, IP41",212.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W200 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05003025P","OBUDOWA UNIWERSALNA OU H500 X W300 X D250, PUSTA, DRZWI PEŁNE, IP41",223.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W300 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05003030P","OBUDOWA UNIWERSALNA OU H500 X W300 X D300, PUSTA, DRZWI PEŁNE, IP41",220.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W300 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05004015P","OBUDOWA UNIWERSALNA OU H500 X W400 X D150, PUSTA, DRZWI PEŁNE, IP41",226.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W400 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05004023P","OBUDOWA UNIWERSALNA OU H500 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",233.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05004025P","OBUDOWA UNIWERSALNA OU H500 X W400 X D250, PUSTA, DRZWI PEŁNE, IP41",235.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W400 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05004030P","OBUDOWA UNIWERSALNA OU H500 X W400 X D300, PUSTA, DRZWI PEŁNE, IP41",245.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W400 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05004035P","OBUDOWA UNIWERSALNA OU H500 X W400 X D350, PUSTA, DRZWI PEŁNE, IP41",265,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W400 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05005023P","OBUDOWA UNIWERSALNA OU H500 X W500 X D230, PUSTA, DRZWI PEŁNE, IP41",249.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W500 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05005030P","OBUDOWA UNIWERSALNA OU H500 X W500 X D300, PUSTA, DRZWI PEŁNE, IP41",280.39999999999998,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W500 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05005035P","OBUDOWA UNIWERSALNA OU H500 X W500 X D350, PUSTA, DRZWI PEŁNE, IP41",301.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W500 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05009040P","OBUDOWA UNIWERSALNA OU H500 X W900 X D400, PUSTA, DRZWI PEŁNE, IP41",517.6,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H500 X W900 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05504015P","OBUDOWA UNIWERSALNA OU H550 X W400 X D150, PUSTA, DRZWI PEŁNE, IP41",211.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W400 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05506014P","OBUDOWA UNIWERSALNA OU H550 X W600 X D140, PUSTA, DRZWI PEŁNE, IP41",255.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W600 X D140, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05506018P","OBUDOWA UNIWERSALNA OU H550 X W600 X D180, PUSTA, DRZWI PEŁNE, IP41",274.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W600 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05506023P","OBUDOWA UNIWERSALNA OU H550 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",298.39999999999998,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05506025P","OBUDOWA UNIWERSALNA OU H550 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",309.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05508023P","OBUDOWA UNIWERSALNA OU H550 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",365,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU05508030P","OBUDOWA UNIWERSALNA OU H550 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",410.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H550 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06003018P","OBUDOWA UNIWERSALNA OU H600 X W300 X D180, PUSTA, DRZWI PEŁNE, IP41",226.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W300 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06003030P","OBUDOWA UNIWERSALNA OU H600 X W300 X D300, PUSTA, DRZWI PEŁNE, IP41",237.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W300 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004015P","OBUDOWA UNIWERSALNA OU H600 X W400 X D150, PUSTA, DRZWI PEŁNE, IP41",220.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004020P","OBUDOWA UNIWERSALNA OU H600 X W400 X D200, PUSTA, DRZWI PEŁNE, IP41",235.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004023P","OBUDOWA UNIWERSALNA OU H600 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",245.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004030P","OBUDOWA UNIWERSALNA OU H600 X W400 X D300, PUSTA, DRZWI PEŁNE, IP41",276.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004035P","OBUDOWA UNIWERSALNA OU H600 X W400 X D350, PUSTA, DRZWI PEŁNE, IP41",297,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004040P","OBUDOWA UNIWERSALNA OU H600 X W400 X D400, PUSTA, DRZWI PEŁNE, IP41",317.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06004040T","OBUDOWA UNIWERSALNA OU H600 X W400 X D400, PUSTA, DRZWI PRZEZROCZYSTE, IP41",624.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W400 X D400, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU06006020P","OBUDOWA UNIWERSALNA OU H600 X W600 X D200, PUSTA, DRZWI PEŁNE, IP41",301.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W600 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06006023P","OBUDOWA UNIWERSALNA OU H600 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",316.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06006025P","OBUDOWA UNIWERSALNA OU H600 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",326.60000000000002,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06006030P","OBUDOWA UNIWERSALNA OU H600 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",352.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06006035P","OBUDOWA UNIWERSALNA OU H600 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",381.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06006040P","OBUDOWA UNIWERSALNA OU H600 X W600 X D400, PUSTA, DRZWI PEŁNE, IP41",417.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W600 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06008023P","OBUDOWA UNIWERSALNA OU H600 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",395.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06008030P","OBUDOWA UNIWERSALNA OU H600 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",452.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06008035P","OBUDOWA UNIWERSALNA OU H600 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",494,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06008040P","OBUDOWA UNIWERSALNA OU H600 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",535.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H600 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06506020P","OBUDOWA UNIWERSALNA OU H650 X W600 X D200, PUSTA, DRZWI PEŁNE, IP41",319.10000000000002,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H650 X W600 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06506023P","OBUDOWA UNIWERSALNA OU H650 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",334.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H650 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06506030P","OBUDOWA UNIWERSALNA OU H650 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",373.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H650 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06506035P","OBUDOWA UNIWERSALNA OU H650 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",409.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H650 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06507012P","OBUDOWA UNIWERSALNA OU H650 X W700 X D120, PUSTA, DRZWI PEŁNE, IP41",318.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H650 X W700 X D120, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU06902933P","OBUDOWA UNIWERSALNA OU H690 X W290 X D330, PUSTA, DRZWI PEŁNE, IP41",269.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS LAKÁS OU H690 X W290 X D330, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07001330P","OBUDOWA UNIWERSALNA OU H700 X W1300 X D300, PUSTA, DRZWI PEŁNE, IP41",813.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W1300 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07003020P","OBUDOWA UNIWERSALNA OU H700 X W300 X D200, PUSTA, DRZWI PEŁNE, IP41",233.1,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W300 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07004018P","OBUDOWA UNIWERSALNA OU H700 X W400 X D180, PUSTA, DRZWI PEŁNE, IP41",249.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W400 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07004023P","OBUDOWA UNIWERSALNA OU H700 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",248.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07005018P","OBUDOWA UNIWERSALNA OU H700 X W500 X D180, PUSTA, DRZWI PEŁNE, IP41",287.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W500 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07005023P","OBUDOWA UNIWERSALNA OU H700 X W500 X D230, PUSTA, DRZWI PEŁNE, IP41",312.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W500 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07005025P","OBUDOWA UNIWERSALNA OU H700 X W500 X D250, PUSTA, DRZWI PEŁNE, IP41",312.60000000000002,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W500 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07005030P","OBUDOWA UNIWERSALNA OU H700 X W500 X D300, PUSTA, DRZWI PEŁNE, IP41",348.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W500 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07005035P","OBUDOWA UNIWERSALNA OU H700 X W500 X D350, PUSTA, DRZWI PEŁNE, IP41",376.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W500 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07005040P","OBUDOWA UNIWERSALNA OU H700 X W500 X D400, PUSTA, DRZWI PEŁNE, IP41",412.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W500 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006014P","OBUDOWA UNIWERSALNA OU H700 X W600 X D140, PUSTA, DRZWI PEŁNE, IP41",302,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D140, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006015P","OBUDOWA UNIWERSALNA OU H700 X W600 X D150, PUSTA, DRZWI PEŁNE, IP41",308,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006018P","OBUDOWA UNIWERSALNA OU H700 X W600 X D180, PUSTA, DRZWI PEŁNE, IP41",315.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006023P","OBUDOWA UNIWERSALNA OU H700 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",351.2,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006025P","OBUDOWA UNIWERSALNA OU H700 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",399.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006030P","OBUDOWA UNIWERSALNA OU H700 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",424.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006035P","OBUDOWA UNIWERSALNA OU H700 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",438.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07006040P","OBUDOWA UNIWERSALNA OU H700 X W600 X D400, PUSTA, DRZWI PEŁNE, IP41",476,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W600 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07008023P","OBUDOWA UNIWERSALNA OU H700 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",455.2,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07008030P","OBUDOWA UNIWERSALNA OU H700 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",517.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07008035P","OBUDOWA UNIWERSALNA OU H700 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",562,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU07008040P","OBUDOWA UNIWERSALNA OU H700 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",606.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H700 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001023P","OBUDOWA UNIWERSALNA OU H800 X W1000 X D230, PUSTA, DRZWI PEŁNE, IP41",638.20000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1000 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001025P","OBUDOWA UNIWERSALNA OU H800 X W1000 X D250, PUSTA, DRZWI PEŁNE, IP41",678.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1000 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001030P","OBUDOWA UNIWERSALNA OU H800 X W1000 X D300, PUSTA, DRZWI PEŁNE, IP41",713.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1000 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001035P","OBUDOWA UNIWERSALNA OU H800 X W1000 X D350, PUSTA, DRZWI PEŁNE, IP41",766,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1000 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001040P","OBUDOWA UNIWERSALNA OU H800 X W1000 X D400, PUSTA, DRZWI PEŁNE, IP41",818.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1000 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001440P","OBUDOWA UNIWERSALNA OU H800 X W1450 X D400, PUSTA, DRZWI PEŁNE, IP41",1137.9000000000001,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1450 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08001540P","OBUDOWA UNIWERSALNA OU H800 X W1500 X D400, PUSTA, DRZWI PEŁNE, IP41",1172.5999999999999,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W1500 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08003023P","OBUDOWA UNIWERSALNA OU H800 X W300 X D230, PUSTA, DRZWI PEŁNE, IP41",256.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W300 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08003525P","OBUDOWA UNIWERSALNA OU H800 X W350 X D250, PUSTA, DRZWI PEŁNE, IP41",287.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W350 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08004025P","OBUDOWA UNIWERSALNA OU H800 X W400 X D250, PUSTA, DRZWI PEŁNE, IP41",309.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W400 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08004030P","OBUDOWA UNIWERSALNA OU H800 X W400 X D300, PUSTA, DRZWI PEŁNE, IP41",334.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W400 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08004035P","OBUDOWA UNIWERSALNA OU H800 X W400 X D350, PUSTA, DRZWI PEŁNE, IP41",360.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W400 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08005030T","OBUDOWA UNIWERSALNA OU H800 X W500 X D300, PUSTA, DRZWI PRZEZROCZYSTE, IP41",755.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W500 X D300, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU08005535P","OBUDOWA UNIWERSALNA OU H800 X W550 X D350, PUSTA, DRZWI PEŁNE, IP41",460.7,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W550 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006015P","OBUDOWA UNIWERSALNA OU H800 X W600 X D150, PUSTA, DRZWI PEŁNE, IP41",338.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006020P","OBUDOWA UNIWERSALNA OU H800 X W600 X D200, PUSTA, DRZWI PEŁNE, IP41",370.5,"1-ZE-02",null,null,null,null,"KPL","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006023P","OBUDOWA UNIWERSALNA OU H800 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",395.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006025P","OBUDOWA UNIWERSALNA OU H800 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",412.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006030P","OBUDOWA UNIWERSALNA OU H800 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",452.4,"1-ZE-02",null,null,null,null,"KPL","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006030T","OBUDOWA UNIWERSALNA OU H800 X W600 X D300, PUSTA, DRZWI PRZEZROCZYSTE, IP41",815.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D300, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU08006035P","OBUDOWA UNIWERSALNA OU H800 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",494,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006040P","OBUDOWA UNIWERSALNA OU H800 X W600 X D400, PUSTA, DRZWI PEŁNE, IP41",535.6,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08006060P","OBUDOWA UNIWERSALNA OU H800 X W600 X D600, PUSTA, DRZWI PEŁNE, IP41",821.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W600 X D600, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08007015P","OBUDOWA UNIWERSALNA OU H800 X W700 X D150, PUSTA, DRZWI PEŁNE, IP41",385.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W700 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08007030P","OBUDOWA UNIWERSALNA OU H800 X W700 X D300, PUSTA, DRZWI PEŁNE, IP41",517.6,"1-ZE-02",null,null,null,null,"KPL",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W700 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08008015P","OBUDOWA UNIWERSALNA OU H800 X W800 X D150, PUSTA, DRZWI PEŁNE, IP41",439.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W800 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08008023P","OBUDOWA UNIWERSALNA OU H800 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",516.20000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08008025P","OBUDOWA UNIWERSALNA OU H800 X W800 X D250, PUSTA, DRZWI PEŁNE, IP41",535.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W800 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08008030P","OBUDOWA UNIWERSALNA OU H800 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",582.79999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08008035P","OBUDOWA UNIWERSALNA OU H800 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",629.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08008040P","OBUDOWA UNIWERSALNA OU H800 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",677.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08009030P","OBUDOWA UNIWERSALNA OU H800 X W900 X D300, PUSTA, DRZWI PEŁNE, IP41",648.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W900 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08009530P","OBUDOWA UNIWERSALNA OU H800 X W950 X D300, PUSTA, DRZWI PEŁNE, IP41",680,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H800 X W950 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08504018P","OBUDOWA UNIWERSALNA OU H850 X W400 X D180, PUSTA, DRZWI PEŁNE, IP41",277.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W400 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08506014P","OBUDOWA UNIWERSALNA OU H850 X W600 X D140, PUSTA, DRZWI PEŁNE, IP41",349,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W600 X D140, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08506018P","OBUDOWA UNIWERSALNA OU H850 X W600 X D180, PUSTA, DRZWI PEŁNE, IP41",377.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W600 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08506023P","OBUDOWA UNIWERSALNA OU H850 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",419.1,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08506030P","OBUDOWA UNIWERSALNA OU H850 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",478.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08506035P","OBUDOWA UNIWERSALNA OU H850 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",521.79999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08508023P","OBUDOWA UNIWERSALNA OU H850 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",546.70000000000005,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08508025P","OBUDOWA UNIWERSALNA OU H850 X W800 X D250, PUSTA, DRZWI PEŁNE, IP41",566.20000000000005,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W800 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU08508030P","OBUDOWA UNIWERSALNA OU H850 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",614.79999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H850 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09003020P","OBUDOWA UNIWERSALNA OU H900 X W300 X D200, PUSTA, DRZWI PEŁNE, IP41",263.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W300 X D200, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09005030P","OBUDOWA UNIWERSALNA OU H900 X W500 X D300, PUSTA, DRZWI PEŁNE, IP41",435.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W500 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09006015P","OBUDOWA UNIWERSALNA OU H900 X W600 X D150, PUSTA, DRZWI PEŁNE, IP41",373.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W600 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09006023P","OBUDOWA UNIWERSALNA OU H900 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",444.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09006025P","OBUDOWA UNIWERSALNA OU H900 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",462.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09006030P","OBUDOWA UNIWERSALNA OU H900 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",506.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09006035P","OBUDOWA UNIWERSALNA OU H900 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",549.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09006040P","OBUDOWA UNIWERSALNA OU H900 X W600 X D400, PUSTA, DRZWI PEŁNE, IP41",594,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W600 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09008023P","OBUDOWA UNIWERSALNA OU H900 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",577.20000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W800 XD230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09008030P","OBUDOWA UNIWERSALNA OU H900 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",648.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09008035P","OBUDOWA UNIWERSALNA OU H900 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",698.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU09008040P","OBUDOWA UNIWERSALNA OU H900 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",748,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H900 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10004023P","OBUDOWA UNIWERSALNA OU H1000 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",291.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006014P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D140, PUSTA, DRZWI PEŁNE, IP41",408,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D140, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006018P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D180, PUSTA, DRZWI PEŁNE, IP41",433.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006023P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",492.7,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006026P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D260, PUSTA, DRZWI PEŁNE, IP41",521.79999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D260, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006030P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",559.29999999999995,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006030T","OBUDOWA UNIWERSALNA OU H1000 X W600 X D300, PUSTA, DRZWI PRZEZROCZYSTE, IP41",819.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D300, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU10006035P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",606.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10006040P","OBUDOWA UNIWERSALNA OU H1000 X W600 X D400, PUSTA, DRZWI PEŁNE, IP41",653.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W600 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10008018P","OBUDOWA UNIWERSALNA OU H1000 X W800 X D180, PUSTA, DRZWI PEŁNE, IP41",584.29999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W800 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10008023P","OBUDOWA UNIWERSALNA OU H1000 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",638.20000000000005,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10008025P","OBUDOWA UNIWERSALNA OU H1000 X W800 X D250, PUSTA, DRZWI PEŁNE, IP41",659.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W800 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10008030P","OBUDOWA UNIWERSALNA OU H1000 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",712,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10008035P","OBUDOWA UNIWERSALNA OU H1000 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",766,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10008040P","OBUDOWA UNIWERSALNA OU H1000 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",818.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10009035P","OBUDOWA UNIWERSALNA OU H1000 X W900 X D350, PUSTA, DRZWI PEŁNE, IP41",845.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W900 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10010030P","OBUDOWA UNIWERSALNA OU H1000 X W1000 X D300, PUSTA, DRZWI PEŁNE, IP41",867.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W1000 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10012030T","OBUDOWA UNIWERSALNA OU H1000 X W1200 X D300, PUSTA, DRZWI PRZEZROCZYSTE, IP41",0,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W1200 X D300, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU10012040P","OBUDOWA UNIWERSALNA OU H1000 X W1200 X D400, PUSTA, DRZWI PEŁNE, IP41",1115.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W1200 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10013025P","OBUDOWA UNIWERSALNA OU H1000 X W1300 X D250, PUSTA, DRZWI PEŁNE, IP41",908.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1000 X W1300 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10503018P","OBUDOWA UNIWERSALNA OU H1050 X W300 X D180, PUSTA, DRZWI PEŁNE, IP41",282.89999999999998,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1050 X W300 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU10504518P","OBUDOWA UNIWERSALNA OU H1050 X W450 X D180, PUSTA, DRZWI PEŁNE, IP41",362.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1050 X W450 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11505523P","OBUDOWA UNIWERSALNA OU H1150 X W550 X D300, PUSTA, DRZWI PEŁNE, IP41",595.29999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W550 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11506023P","OBUDOWA UNIWERSALNA OU H1150 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",566.20000000000005,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11506030P","OBUDOWA UNIWERSALNA OU H1150 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",639.70000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11506035P","OBUDOWA UNIWERSALNA OU H1150 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",689.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11508023P","OBUDOWA UNIWERSALNA OU H1150 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",728.6,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11508030P","OBUDOWA UNIWERSALNA OU H1150 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",809,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU11508035P","OBUDOWA UNIWERSALNA OU H1150 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",867.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1150 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12006023P","OBUDOWA UNIWERSALNA OU H1200 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",589.79999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12006030P","OBUDOWA UNIWERSALNA OU H1200 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",666,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12006035P","OBUDOWA UNIWERSALNA OU H1200 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",718.7,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12008025P","OBUDOWA UNIWERSALNA OU H1200 X W800 X D250, PUSTA, DRZWI PEŁNE, IP41",725,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W800 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12008030P","OBUDOWA UNIWERSALNA OU H1200 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",844.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12008035P","OBUDOWA UNIWERSALNA OU H1200 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",900.6,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12008040P","OBUDOWA UNIWERSALNA OU H1200 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",960.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12008535P","OBUDOWA UNIWERSALNA OU H1200 X W850 X D350, PUSTA, DRZWI PEŁNE, IP41",946.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W850 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12010023P","OBUDOWA UNIWERSALNA OU H1200 X W1000 X D230, PUSTA, DRZWI PEŁNE, IP41",929,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W1000 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12010030P","OBUDOWA UNIWERSALNA OU H1200 X W1000 X D300, PUSTA, DRZWI PEŁNE, IP41",1019.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W1000 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU12010040P","OBUDOWA UNIWERSALNA OU H1200 X W1000 X D400, PUSTA, DRZWI PEŁNE, IP41",1149,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W1000 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU1201213P","OBUDOWA UNIWERSALNA OU H1200 X W1200 X D130, PUSTA, DRZWI PEŁNE, IP41",954.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1200 X W1200 X D130, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13003023P","OBUDOWA UNIWERSALNA OU H1300 X W300 X D230, PUSTA, DRZWI PEŁNE, IP41",369,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W300 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13004030P","OBUDOWA UNIWERSALNA OU H1300 X W400 X D300, PUSTA, DRZWI PEŁNE, IP41",514.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W400 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13006018P","OBUDOWA UNIWERSALNA OU H1300 X W600 X D180, PUSTA, DRZWI PEŁNE, IP41",567.29999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W600 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13006023P","OBUDOWA UNIWERSALNA OU H1300 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",639.70000000000005,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13006025P","OBUDOWA UNIWERSALNA OU H1300 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",662,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13006030P","OBUDOWA UNIWERSALNA OU H1300 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",718.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13008023P","OBUDOWA UNIWERSALNA OU H1300 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",820.1,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13008030P","OBUDOWA UNIWERSALNA OU H1300 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",907.4,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU13008040P","OBUDOWA UNIWERSALNA OU H1300 X W800 X D400, PUSTA, DRZWI PEŁNE, IP41",981.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1300 X W800 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14001013P","OBUDOWA UNIWERSALNA OU H1400 X W1000 X D130, PUSTA, DRZWI PEŁNE, IP41",933.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1400 X W1000 X D130, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14001015P","OBUDOWA UNIWERSALNA OU H1400 X W1000 X D150, PUSTA, DRZWI PEŁNE, IP41",959.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1400 X W1000 X D150, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14004040P","OBUDOWA UNIWERSALNA OU H1400 X W400 X D400, PUSTA, DRZWI PEŁNE, IP41",646.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1400 X W400 X D400, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14503023P","OBUDOWA UNIWERSALNA OU H1450 X W300 X D230, PUSTA, DRZWI PEŁNE, IP41",416.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W300 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14504023P","OBUDOWA UNIWERSALNA OU H1450 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",516.20000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14506018P","OBUDOWA UNIWERSALNA OU H1450 X W600 X D180, PUSTA, DRZWI PEŁNE, IP41",634.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W600 X D180, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14506023P","OBUDOWA UNIWERSALNA OU H1450 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",713.3,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14506025P","OBUDOWA UNIWERSALNA OU H1450 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",736.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14506030P","OBUDOWA UNIWERSALNA OU H1450 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",798,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14506035P","OBUDOWA UNIWERSALNA OU H1450 X W600 X D350, PUSTA, DRZWI PEŁNE, IP41",857.5,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W600 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14508023P","OBUDOWA UNIWERSALNA OU H1450 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",911.8,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14508030P","OBUDOWA UNIWERSALNA OU H1450 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",1004.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU14508035P","OBUDOWA UNIWERSALNA OU H1450 X W800 X D350, PUSTA, DRZWI PEŁNE, IP41",1069.9000000000001,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1450 X W800 X D350, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU15006025P","OBUDOWA UNIWERSALNA OU H1500 X W600 X D250, PUSTA, DRZWI PEŁNE, IP41",761.9,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1500 X W600 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU15009025P","OBUDOWA UNIWERSALNA OU H1500 X W900 X D250, PUSTA, DRZWI PEŁNE, IP41",1040.7,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1500 X W900 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16003023P","OBUDOWA UNIWERSALNA OU H1600 X W300 X D230, PUSTA, DRZWI PEŁNE, IP41",463.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W300 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16003523P","OBUDOWA UNIWERSALNA OU H1600 X W350 X D230, PUSTA, DRZWI PEŁNE, IP41",516.20000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W350 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16003523T","OBUDOWA UNIWERSALNA OU H1600 X W350 X D230, PUSTA, DRZWI PRZEZROCZYSTE, IP41",654.9,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W350 X D230, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU16003525P","OBUDOWA UNIWERSALNA OU H1600 X W350 X D250, PUSTA, DRZWI PEŁNE, IP41",539.79999999999995,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W350 XD250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16004023P","OBUDOWA UNIWERSALNA OU H1600 X W400 X D230, PUSTA, DRZWI PEŁNE, IP41",571.70000000000005,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W400 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16004023T","OBUDOWA UNIWERSALNA OU H1600 X W400 X D230, PUSTA, DRZWI PRZEZROCZYSTE, IP41",709.1,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W400 X D230, ÜRES, ÁTLÁTSZÓ AJTÓ, IP41"]
["OU16006023P","OBUDOWA UNIWERSALNA OU H1600 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",786.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16006030P","OBUDOWA UNIWERSALNA OU H1600 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",877,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16008023P","OBUDOWA UNIWERSALNA OU H1600 X W800 X D230, PUSTA, DRZWI PEŁNE, IP41",1003.3,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W800 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16008025P","OBUDOWA UNIWERSALNA OU H1600 X W800 X D250, PUSTA, DRZWI PEŁNE, IP41",1031.0999999999999,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W800 X D250, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU16008030P","OBUDOWA UNIWERSALNA OU H1600 X W800 X D300, PUSTA, DRZWI PEŁNE, IP41",1101.8,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1600 X W800 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU18003023P","OBUDOWA UNIWERSALNA OU H1800 X W300 X D230, PUSTA, DRZWI PEŁNE, IP41",525.9,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1800 X W300 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU18006023P","OBUDOWA UNIWERSALNA OU H1800 X W600 X D230, PUSTA, DRZWI PEŁNE, IP41",884,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1800 X W600 X D230, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU18006030P","OBUDOWA UNIWERSALNA OU H1800 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",954.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1800 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OU19006030P","OBUDOWA UNIWERSALNA OU H1900 X W600 X D300, PUSTA, DRZWI PEŁNE, IP41",1036.5999999999999,"1-ZE-02",null,null,null,null,"SZT","85321000","27.90.51.0",null,null,null,null,null,"UNIVERZÁLIS HÁZ OU H1900 X W600 X D300, ÜRES, TÖMÖR AJTÓ, IP41"]
["OUD10040","DASZEK OBUDOWY OU W1000 X D400",404.2,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"OU W1000 X D400 HÁZ TETŐJE"]
["OUD8030","DASZEK OBUDOWY OU W800 X D300",343.6,"1-ZE-02",null,null,null,null,"SZT",null,null,null,null,null,null,null,"HÁZTETŐ OU W800 X D300"]
["OUS100M21","OUS 21M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1150, W1000, 7X46, BEZ SZYN I MASKOWNIC.",145.5,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 21M - ÉPÜLETTARTÓ SZERKEZETE, H1150, W1000, 7X46, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS30M06","OUS 6M - KONSTRUKCJA WSPORCZA ZABUDOWY, H400 X W300, 2X7, BEZ SZYN I MASKOWNIC.",51.2,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 6M - ÉPÜLET TARTÓSZERKEZETE, H400 X W300, 2X7, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS30M24","OUS 24M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1300 X W300, 8X7, BEZ SZYN I MASKOWNIC.",137.5,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 24M - ÉPÜLET TARTÓSZERKEZETE, H1300 X W300, 8X7, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS30M30","OUS 30M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1600 X W300, 10X7, BEZ SZYN I MASKOWNIC.",161.69999999999999,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 30M - ÉPÜLET TARTÓSZERKEZETE, H1600 X W300, 10X7, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M06","OUS 6M - KONSTRUKCJA WSPORCZA ZABUDOWY, H400 X W350, 2X10, BEZ SZYN I MASKOWNIC.",55.6,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 6M - ÉPÜLET TARTÓSZERKEZETE, H400 X W350, 2X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M09","OUS 9M - KONSTRUKCJA WSPORCZA ZABUDOWY, H550 X W350, 3X10, BEZ SZYN I MASKOWNIC.",70.8,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 9M - ÉPÜLET TARTÓSZERKEZETE, H550 X W350, 3X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M12","OUS 12M - KONSTRUKCJA WSPORCZA ZABUDOWY, H700 X W350, 4X10, BEZ SZYN I MASKOWNIC.",84.7,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 12M - ÉPÜLET TARTÓSZERKEZETE, H700 X W350, 4X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M15","OUS 15M - KONSTRUKCJA WSPORCZA ZABUDOWY, H850 X W350, 5X10, BEZ SZYN I MASKOWNIC.",99.8,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 15M - ÉPÜLET TARTÓSZERKEZETE, H850 X W350, 5X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M18","OUS 18M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1000 X W350, 6X10, BEZ SZYN I MASKOWNIC.",113.8,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 18M - ÉPÜLET TARTÓSZERKEZETE, H1000 X W350, 6X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M21","OUS 21M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1150 X W350, 7X10, BEZ SZYN I MASKOWNIC.",129.1,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 21M - ÉPÜLET TARTÓSZERKEZETE, H1150 X W350, 7X10, SÍNEK ÉS BURKOLATOK NÉLKÜL."]
["OUS35M24","OUS 24M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1300 X W350, 8X10, BEZ SZYN I MASKOWNIC.",145.80000000000001,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 24M - ÉPÜLET TARTÓSZERKEZETE, H1300 X W350, 8X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M27","OUS 27M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1450 X W350, 9X10, BEZ SZYN I MASKOWNIC.",158.19999999999999,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 27M - ÉPÜLET TARTÓSZERKEZETE, H1450 X W350, 9X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M30","OUS 30M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1600 X W350, 10X10, BEZ SZYN I MASKOWNIC.",165.7,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"OUS 30M - ÉPÜLET TARTÓSZERKEZETE, H1600 X W350, 10X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS35M33","OUS 33M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1750 X W350, 11X10, BEZ SZYN I MASKOWNIC.",174.5,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 33M - ÉPÜLET TARTÓSZERKEZETE, H1750 X W350, 11X10, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS40M06","OUS 6M - KONSTRUKCJA WSPORCZA ZABUDOWY, H400 X W400, 2X13, BEZ SZYN I MASKOWNIC.",56.5,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"OUS 6M - ÉPÜLET TARTÓSZERKEZETE, H400 X W400, 2X13, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS40M12","OUS 12M - KONSTRUKCJA WSPORCZA ZABUDOWY, H700 X W400, 4X13, BEZ SZYN I MASKOWNIC.",83.5,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 12M - ÉPÜLET TARTÓSZERKEZETE, H700 X W400, 4X13, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS40M14","OUS 14M - KONSTRUKCJA WSPORCZA ZABUDOWY, H800 X W400, 5X13, BEZ SZYN I MASKOWNIC.",91.6,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 14M - ÉPÜLET TARTÓSZERKEZETE, H800 X W400, 5X13, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS40M15","OUS 15M - KONSTRUKCJA WSPORCZA ZABUDOWY, H850 X W400, 5X13, BEZ SZYN I MASKOWNIC.",99.7,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 15M - ÉPÜLET TARTÓSZERKEZETE, H850 X W400, 5X13, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS40M27","OUS 27M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1450 X W400, 9X13, BEZ SZYN I MASKOWNIC.",161.69999999999999,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 27M - ÉPÜLET TARTÓSZERKEZETE, H1450 X W400, 9X13, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS40M30","OUS 30M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1600 X W400, 10X13, BEZ SZYN I MASKOWNIC.",169.8,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"OUS 30M - ÉPÜLET TARTÓSZERKEZETE, H1600 X W400, 10X13, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS42230","OUS SYSTEM - 4 PIONOWE SZYNY SYMETRYCZNE TS-35, W600, 6M",65.3,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS RENDSZER – 4 FÜGGŐLEGES SZIMMETRIKUS SÍN TS-35, W600, 6M"]
["OUS60M06","OUS 6M - KONSTRUKCJA WSPORCZA ZABUDOWY, H400 X W600, 2X24, BEZ SZYN I MASKOWNIC.",58.2,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 6M - ÉPÜLET TARTÓSZERKEZETE, H400 X W600, 2X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M09","OUS 9M - KONSTRUKCJA WSPORCZA ZABUDOWY, H550 X W600, 3X24, BEZ SZYN I MASKOWNIC.",74.8,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 9M - ÉPÜLET TARTÓSZERKEZETE, H550 X W600, 3X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M11","OUS 11M - KONSTRUKCJA WSPORCZA ZABUDOWY, H650 X W600, 3X24(3M)+24(2M), BEZ SZYN I MASKOWNIC.",83.2,"1-ZE-04",null,null,null,null,"SZT",null,null,"140124LK",null,null,null,null,"OUS 11M - ÉPÜLET TARTÓSZERKEZETE, H650 X W600, 3X24(3M)+24(2M), SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M12","OUS 12M - KONSTRUKCJA WSPORCZA ZABUDOWY, H700 X W600, 4X24, BEZ SZYN I MASKOWNIC.",88.9,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 12M - ÉPÜLETTARTÓ SZERKEZET, H700 X W600, 4X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M14","OUS 14M - KONSTRUKCJA WSPORCZA ZABUDOWY, H800 X W600, 4X24(3M)+24(2M), BEZ SZYN I MASKOWNIC.",94.3,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 14M - ÉPÜLET TARTÓSZERKEZETE, H800 X W600, 4X24(3M)+24(2M), SÍNEK ÉS BURKOLATOK NÉLKÜL."]
["OUS60M15","OUS 15M - KONSTRUKCJA WSPORCZA ZABUDOWY, H850 X W600, 5X24, BEZ SZYN I MASKOWNIC.",105.5,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 15M - ÉPÜLETTARTÓ SZERKEZETE, H850 X W600, 5X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M18","OUS 18M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1000 X W600, 6X24, BEZ SZYN I MASKOWNIC.",119.3,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 18M - ÉPÜLET TARTÓSZERKEZETE, H1000 X W600, 6X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M21","OUS 21M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1150 X W600, 7X24, BEZ SZYN I MASKOWNIC.",135.9,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 21M - ÉPÜLET TARTÓSZERKEZETE, H1150 X W600, 7X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M24","OUS 24M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1300 X W600, 8X24, BEZ SZYN I MASKOWNIC.",154.1,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 24M - ÉPÜLET TARTÓSZERKEZETE, H1300 X W600, 8X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M27","OUS 27M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1450 X W600, 9X24, BEZ SZYN I MASKOWNIC.",166.9,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 27M - ÉPÜLET TARTÓSZERKEZETE, H1450 X W600, 9X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M30","OUS 30M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1600 X W600, 10X24, BEZ SZYN I MASKOWNIC.",241.2,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"OUS 30M - ÉPÜLET TARTÓSZERKEZETE, H1600 X W600, 10X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS60M33","OUS 33M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1750 X W600, 11X24, BEZ SZYN I MASKOWNIC.",183.2,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 33M - ÉPÜLET TARTÓSZERKEZETE, H1750 X W600, 11X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M06","OUS 6M - KONSTRUKCJA WSPORCZA ZABUDOWY, H400 X W800, 2X35, BEZ SZYN I MASKOWNIC.",61.1,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 6M - ÉPÜLET TARTÓSZERKEZETE, H400 X W800, 2X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M09","OUS 9M - KONSTRUKCJA WSPORCZA ZABUDOWY, H550, W800, 3X24, BEZ SZYN I MASKOWNIC.",79.099999999999994,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 9M - ÉPÜLETTÁMASZTÓ SZERKEZETE, H550, W800, 3X24, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M12","OUS 12M - KONSTRUKCJA WSPORCZA ZABUDOWY, H700, W800, 4X35, BEZ SZYN I MASKOWNIC.",93,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 12M - ÉPÜLET TARTÓSZERKEZETE, H700, W800, 4X35, SÍNEK ÉS MASZKOK NÉLKÜL."]
["OUS80M15","OUS 15M - KONSTRUKCJA WSPORCZA ZABUDOWY, H850, W800, 5X35, BEZ SZYN I MASKOWNIC.",111,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 15M - ÉPÜLET TARTÓSZERKEZETE, H850, W800, 5X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M18","OUS 18M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1000, W800, 6X35, BEZ SZYN I MASKOWNIC.",125,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 18M - ÉPÜLET TARTÓSZERKEZETE, H1000, W800, 6X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M21","OUS 21M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1150, W800, 7X35, BEZ SZYN I MASKOWNIC.",143,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 21M - ÉPÜLET TARTÓSZERKEZETE, H1150, W800, 7X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M24","OUS 24M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1300, W800, 8X35, BEZ SZYN I MASKOWNIC.",162.4,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 24M - ÉPÜLET TARTÓSZERKEZETE, H1300, W800, 8X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M27","OUS 27M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1450 X W800, 9X35, BEZ SZYN I MASKOWNIC.",174.9,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 27M - ÉPÜLET TARTÓSZERKEZETE, H1450 X W800, 9X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M30","OUS 30M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1600 X W800, 10X35, BEZ SZYN I MASKOWNIC.",254.7,"1-ZE-04",null,null,null,null,"SZT",null,null,"131024LK",null,null,null,null,"OUS 30M - ÉPÜLET TARTÓSZERKEZETE, H1600 X W800, 10X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUS80M33","OUS 33M - KONSTRUKCJA WSPORCZA ZABUDOWY, H1750 X W800, 11X35, BEZ SZYN I MASKOWNIC.",211,"1-ZE-04",null,null,null,null,"SZT","85321000","27.90.51.0","131024LK",null,null,null,null,"OUS 33M - ÉPÜLET TARTÓSZERKEZETE, H1750 X W800, 11X35, SÍNEK ÉS FEDŐK NÉLKÜL."]
["OUZ10060M168R6","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 1000X600; 168 MODUŁÓW; 6 RZĘDÓW",724.2,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 1000X600-AS HÁZHOZ; 168 MODUL; 6 SOR"]
["OUZ10080M234R6","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 1000X800; 234 MODUŁY; 6 RZĘDÓW",963,"1-ZE-04",null,null,null,null,"SZT","85381000","27.12.40.0",null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 1000X800 HÁZHOZ; 234 MODUL; 6 SOR"]
["OUZ12060M196R7","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 1200X600; 196 MODUŁÓW; 7 RZĘDÓW",798,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 1200X600 HÁZHOZ; 196 MODUL; 7 SOR"]
["OUZ12080M273R7","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 1200X800; 273 MODUŁÓW; 7 RZĘDÓW",1006.1,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 1200X800 HÁZHOZ; 273 MODUL; 7 SOR"]
["OUZ140100M450R9","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 1400X1000; 450 MODUŁÓW; 9 RZĘDÓW",1295.2,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 1400X1000 HÁZHOZ; 450 MODUL; 9 SOR"]
["OUZ4030M24R2","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 400X300; 24 MODUŁÓW; 2 RZĘDY",374.7,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 400X300 HÁZHOZ; 24 MODUL; 2 SOR"]
["OUZ4035M28R2","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 400X350; 28 MODUŁÓW; 2 RZĘDY",385.9,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 400X350-ES HÁZHOZ; 28 MODUL; 2 SOR"]
["OUZ4040M32R2","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 400X400; 32 MODUŁÓW; 2 RZĘDY",395.5,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULÁRÁS 400X400-AS HÁZHOZ; 32 MODUL; 2 SOR"]
["OUZ4060M56R2","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 400X600; 56 MODUŁÓW; 2 RZĘDY",438.4,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 400X600-AS HÁZHOZ; 56 MODUL; 2 SOR"]
["OUZ5030M36R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 500X300; 36 MODUŁÓW; 3 RZĘDY",402.5,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 500X300 HÁZHOZ; 36 MODUL; 3 SOR"]
["OUZ5040M48R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 500X400; 48 MODUŁÓW; 3 RZĘDY",419.1,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 500X400 HÁZHOZ; 48 MODUL; 3 SOR"]
["OUZ5050M66R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 500X500; 66 MODUŁÓW; 3 RZĘDY",457.9,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 500X500 HÁZHOZ; 66 MODUL; 3 SOR"]
["OUZ6040M48R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 600X400; 48 MODUŁÓW; 3 RZĘDY",452.4,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 600X400 HÁZHOZ; 48 MODUL; 3 SOR"]
["OUZ6050M48R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 600X500; 66 MODUŁÓW; 3 RZĘDY",474.5,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 600X500 HÁZHOZ; 66 MODUL; 3 SOR"]
["OUZ6060M84R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 600X600; 84 MODUŁÓW; 3 RZĘDY",499.4,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 600X600 HÁZHOZ; 84 MODUL; 3 SOR"]
["OUZ6080M117R3","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 600X800; 117 MODUŁÓW; 3 RZĘDY",557.9,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 600X800 HÁZHOZ; 117 MODUL; 3 SOR"]
["OUZ7050M88R4","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 700X500; 88 MODUŁÓW; 4 RZĘDY",643.9,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 700X500 HÁZHOZ; 88 MODUL; 4 SOR"]
["OUZ8040M80R5","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 800X400; 80 MODUŁÓW; 5 RZĘDÓW",605.20000000000005,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 800X400 HÁZHOZ; 80 MODUL; 5 SOR"]
["OUZ8060M140R5","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 800X600; 140 MODUŁÓW; 5 RZĘDÓW",624.4,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 800X600-AS HÁZHOZ; 140 MODUL; 5 SOR"]
["OUZ8080M195R5","ZENERGY OU - RAMA MODUŁOWA OUZ DLA OBUDOWY 800X800; 195 MODUŁÓW; 5 RZĘDÓW",766.5,"1-ZE-04",null,null,null,null,"SZT",null,null,null,null,null,null,null,"ZENERGY OU - OUZ MODULKERET 800X800 HÁZHOZ; 195 MODUL; 5 SOR"]
["PROMET-DIS8","AlCubar - Blok dystrybucyjny 630A 4P, rozstaw 50mm, L=475mm",703.1,null,null,null,null,null,null,"8538909900",null,null,"5901988299996"]
["PWPZX2024","Kontroler Przeciwpożarowego Wyłącznika Prądu PWP ZX2024 230V AC, 0-10k Ohm",3456,"230726PK",null,null,null,null,null,"85365005",null,null,"5901988019754"]
["SDMQ2H","SDMQ2 CZUJNIK DYMU HOLD - MANUAL RESET",179.3,"200915PK",null,null,null,null,null,"85365005",null,null,"5901988025229"]
["SDMQ2N","SDMQ2 CZUJNIK DYMU NORMAL -AUTO RESET",179.3,"240115PK",null,null,null,null,null,"85365005",null,null,"5901988471552"]

{"sheet":"Zenergy-OE","index":1,"n_rows":93,"n_cols":54,"rows_kept":93,"cut":false,"hidden":false,"merged":[[91,47,91,50],[92,47,92,48],[77,47,77,48],[79,47,79,49],[80,47,80,48],[82,47,82,49],[85,47,85,49],[83,47,83,48],[88,47,88,50],[89,47,89,48],[89,39,89,40],[85,39,85,41],[86,39,86,40],[88,39,88,42],[38,47,38,48],[56,47,56,48],[76,47,76,49],[43,47,43,49],[44,47,44,48],[50,47,50,48],[52,47,52,49],[53,47,53,48],[55,47,55,49],[58,39,58,41],[46,47,46,49],[47,47,47,48],[49,47,49,49],[58,47,58,49],[55,39,55,41],[56,39,56,40],[41,39,41,40],[43,39,43,41],[44,39,44,40],[46,39,46,41],[59,39,59,40],[59,47,59,48],[74,39,74,40],[74,47,74,48],[67,47,67,49],[86,47,86,48],[77,39,77,40],[79,39,79,41],[76,39,76,41],[83,39,83,40],[82,39,82,41],[80,39,80,40],[68,39,68,40],[67,39,67,41],[70,47,70,49],[61,39,61,41],[61,47,61,49],[62,39,62,40],[62,47,62,48],[70,39,70,41],[64,39,64,41],[64,47,64,49],[73,47,73,49],[73,39,73,41],[23,50,24,53],[24,47,24,48],[40,47,40,49],[41,47,41,48],[27,47,27,48],[27,50,28,53],[28,47,28,48],[30,47,30,53],[31,47,31,48],[23,47,23,48],[37,47,37,53],[92,39,92,40],[10,47,10,53],[11,47,11,48],[13,47,13,53],[14,47,14,48],[16,47,16,53],[17,47,17,48],[19,47,19,53],[20,47,20,48],[22,48,22,53],[26,48,26,53],[50,39,50,40],[52,39,52,41],[37,39,37,45],[38,39,38,40],[40,39,40,41],[30,39,30,45],[31,39,31,40],[26,40,26,45],[27,39,27,40],[91,39,91,42],[32,47,32,48],[34,47,34,53],[35,47,35,48],[53,39,53,40],[27,42,28,45],[28,39,28,40],[47,39,47,40],[49,39,49,41],[32,39,32,40],[34,39,34,45],[35,39,35,40],[20,39,20,40],[22,40,22,45],[23,39,23,40],[23,42,24,45],[24,39,24,40],[23,31,23,32],[32,31,32,32],[30,31,30,37],[23,34,24,37],[80,31,80,32],[91,31,91,34],[88,31,88,34],[89,31,89,32],[82,31,82,33],[83,31,83,32],[27,31,27,32],[26,32,26,37],[27,34,28,37],[34,31,34,37],[37,31,37,37],[31,31,31,32],[28,31,28,32],[77,36,77,37],[35,31,35,32],[24,31,24,32],[43,31,43,33],[44,31,44,32],[46,31,46,33],[47,31,47,32],[85,31,85,33],[86,31,86,32],[52,31,52,33],[53,31,53,32],[76,31,76,33],[77,31,77,32],[56,31,56,32],[79,31,79,33],[65,31,65,32],[58,31,58,33],[59,31,59,32],[61,31,61,33],[64,31,64,33],[73,31,73,33],[62,31,62,32],[55,31,55,33],[50,31,50,32],[49,31,49,33],[38,31,38,32],[41,31,41,32],[40,31,40,33],[46,23,46,26],[49,23,49,26],[92,23,92,24],[86,23,86,24],[56,23,56,24],[52,23,52,26],[89,23,89,24],[79,23,79,26],[82,23,82,26],[85,23,85,26],[62,23,62,24],[88,23,88,26],[91,23,91,26],[59,23,59,24],[55,23,55,26],[58,23,58,26],[77,23,77,24],[83,23,83,24],[92,31,92,32],[80,23,80,24],[32,27,32,29],[32,23,32,26],[61,23,61,26],[76,23,76,26],[23,23,23,24],[50,23,50,24],[40,23,40,26],[43,23,43,26],[26,27,26,29],[41,23,41,24],[44,23,44,24],[38,23,38,24],[34,23,34,26],[71,23,71,24],[64,23,64,26],[24,23,24,24],[35,23,35,24],[47,23,47,24],[37,23,37,26],[53,23,53,24],[22,32,22,37],[8,23,8,25],[13,31,13,37],[19,31,19,37],[16,31,16,37],[11,31,11,32],[14,31,14,32],[17,31,17,32],[8,39,8,43],[10,23,11,27],[13,23,14,27],[16,23,17,27],[20,23,20,24],[8,26,8,29],[19,23,19,27],[22,23,22,29],[8,47,8,51],[20,31,20,32],[10,31,10,37],[10,39,10,45],[11,39,11,40],[13,39,13,45],[14,39,14,40],[16,39,16,45],[17,39,17,40],[8,31,8,35],[19,39,19,45],[71,39,71,40],[71,47,71,48],[65,39,65,40],[65,47,65,48],[68,47,68,48],[74,31,74,32],[71,31,71,32],[68,23,68,24],[68,31,68,32],[67,31,67,33],[65,23,65,24],[70,31,70,33],[67,23,67,26],[70,23,70,26],[73,23,73,26],[74,23,74,24]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,33]
[]
[]
[]
[]
[]
[]
["Nazwa projektu",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TODAY()","v":"2025-01-29"},null,null,"Wpisz nazwę",null,null,null,null,{"$f":"IF($Y$32=1,\"Obudowa 1\",\"Field 1\")","v":"Obudowa 1"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Obudowa 2\",\"Field 2\")","v":"Obudowa 2"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Obudowa 3\",\"Field 3\")","v":"Obudowa 3"},null,null,null,null,null,1]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Wysokość\",\"Height\")","v":"Wysokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Szerokość obudowy\",\"Field width\")","v":"Szerokość obudowy"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Szerokość obudowy\",\"Field width\")","v":"Szerokość obudowy"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Szerokość obudowy\",\"Field width\")","v":"Szerokość obudowy"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!C279:H300,Zbaza!C305:H326,Zbaza!C331:H352,Zbaza!C357:H378,Zbaza!C383:H404),Zbaza!BA13,Zbaza!BD4,Zbaza!BG4),\"\")","v":84065},null,{"$f":"IF(Zbaza!BA13>1,Zbaza!AB1-1,\"\")","v":2},null,33,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!C279:H294,Zbaza!C305:H320,Zbaza!C331:H346,Zbaza!C357:H372,Zbaza!C383:H398),Zbaza!BA12,Zbaza!BD4,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!BA12>1,Zbaza!AG1-1,\"\")","v":""},null,33,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!C279:H294,Zbaza!C305:H320,Zbaza!C331:H346,Zbaza!C357:H372,Zbaza!C383:H398),Zbaza!BA15,Zbaza!BD4,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!BA15>1,Zbaza!AL1-1,\"\")","v":""},null,33]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Głębokość\",\"Depth\")","v":"Głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Drzwi z przodu\",\"Front side\")","v":"Drzwi z przodu"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Drzwi z przodu\",\"Front side\")","v":"Drzwi z przodu"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Drzwi z przodu\",\"Front side\")","v":"Drzwi z przodu"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!C5:H26,Zbaza!C32:H53,Zbaza!C113:H134,Zbaza!S50:X71,Zbaza!S25:X46,Zbaza!C86:H107,Zbaza!C59:H80,Zbaza!S100:X121,Zbaza!S75:X96,Zbaza!K5:P26),Zbaza!BA13,Zbaza!BD4,Zbaza!AN67),\"\")","v":80365},null,{"$f":"IF(Zbaza!AB3=2,Zbaza!AB1-1,\"\")","v":2},null,33,null,null,null,{"$f":"IF(Zbaza!BA10>1,INDEX((Zbaza!C142:H163,Zbaza!C169:H190,Zbaza!C250:H271,Zbaza!S155:X176,Zbaza!S130:X151,Zbaza!C223:H244,Zbaza!C196:H217,Zbaza!S205:X226,Zbaza!S180:X201,Zbaza!K5:P26),Zbaza!BA10,Zbaza!BD4,Zbaza!AN68),\"\")","v":""},null,{"$f":"IF(Zbaza!AG3=2,Zbaza!AG1-1,IF(AN15<\"\",AH15,\"\"))","v":""},null,33,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!C5:H20,Zbaza!C32:H47,Zbaza!C113:H128,Zbaza!S50:X71,Zbaza!S25:X46,Zbaza!C86:H101,Zbaza!C59:H74,Zbaza!S100:X121,Zbaza!S75:X96,Zbaza!K5:P26),Zbaza!BA15,Zbaza!BD4,Zbaza!AN69),\"\")","v":""},null,{"$f":"IF(Zbaza!AL3=2,Zbaza!AL1-1,\"\")","v":""},null,33]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IP -",null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Plecy z tyłu\",\"Back side\")","v":"Plecy z tyłu"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Plecy z tyłu\",\"Back side\")","v":"Plecy z tyłu"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Plecy z tyłu\",\"Back side\")","v":"Plecy z tyłu"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!C5:H26,Zbaza!C32:H53,Zbaza!C113:H134,Zbaza!S50:X71,Zbaza!S25:X46,Zbaza!C86:H107,Zbaza!C59:H80,Zbaza!S100:X121,Zbaza!S75:X96,Zbaza!K5:P26),Zbaza!BA13,Zbaza!BD4,Zbaza!AN80),\"\")","v":81265},null,{"$f":"IF(Zbaza!AB2=2,Zbaza!AB1-1,\"\")","v":2},null,33,null,null,null,{"$f":"IF(Zbaza!BA10>1,INDEX((Zbaza!C142:H163,Zbaza!C169:H190,Zbaza!C250:H271,Zbaza!S155:X176,Zbaza!S130:X151,Zbaza!C223:H244,Zbaza!C196:H217,Zbaza!S205:X226,Zbaza!S180:X201,Zbaza!K5:P26),Zbaza!BA10,Zbaza!BD4,Zbaza!AN81),\"\")","v":""},null,{"$f":"IF(Zbaza!AG2=2,Zbaza!AG1-1,IF(AN18<\"\",AH18,\"\"))","v":""},null,33,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!C5:H20,Zbaza!C32:H47,Zbaza!C113:H128,Zbaza!S50:X71,Zbaza!S25:X46,Zbaza!C86:H101,Zbaza!C59:H74,Zbaza!S100:X121,Zbaza!S75:X96,Zbaza!K5:P26),Zbaza!BA15,Zbaza!BD4,Zbaza!AN82),\"\")","v":""},null,{"$f":"IF(Zbaza!AL2=2,Zbaza!AL1-1,\"\")","v":""},null,33]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Zestaw łączeniowy bokami\",\"Side-by-side connection\")","v":"Zestaw łączeniowy bokami"},null,null,null,null,null,{"$f":"IF($Y$32=1,\"Prąd\",\"\")","v":"Prąd"},null,{"$f":"IF($Y$32=1,\"Pokrywa górna\",\"Top cover\")","v":"Pokrywa górna"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Pokrywa górna\",\"Top cover\")","v":"Pokrywa górna"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Pokrywa górna\",\"Top cover\")","v":"Pokrywa górna"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!AG26>0,Zbaza!BT94,\"\")","v":""},null,{"$f":"IF(X21=\"\",\"\",Zbaza!AG26)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!K227:O248,Zbaza!K253:O274,Zbaza!K279:O300,Zbaza!K305:O326,Zbaza!K5:O26),Zbaza!BA13,Zbaza!BG4,Zbaza!AN5),\"\")","v":31465},null,{"$f":"IF(Zbaza!AB4>0,Zbaza!AB1-1,\"\")","v":2},null,33,null,null,null,{"$f":"IF(Zbaza!BA10>1,INDEX((Zbaza!S231:W252,Zbaza!S257:W278,Zbaza!S283:W304,Zbaza!S309:W330,Zbaza!K5:O26),Zbaza!BA10,Zbaza!BG4,Zbaza!AN6),\"\")","v":""},null,{"$f":"IF(Zbaza!AG4=2,Zbaza!AG1-1,IF(AN21<\"\",AH21,\"\"))","v":""},null,33,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!K227:O242,Zbaza!K253:O268,Zbaza!K279:O294,Zbaza!K305:O320,Zbaza!K5:O20),Zbaza!BA15,Zbaza!BG4,Zbaza!AN7),\"\")","v":""},null,{"$f":"IF(Zbaza!AL4>0,Zbaza!AL1-1,\"\")","v":""},null,33]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony\",\"Side\")","v":"Osłony"},null,null,null,null,null,null,null,{"$f":"IF(AF24=\"\",\"\",Zbaza!CT63)","v":""},{"$f":"IF($Y$32=1,\"Rama osłon z przodu\",\"Front plates support\")","v":"Rama osłon z przodu"},null,null,null,null,null,null,{"$f":"IF(AN24=\"\",\"\",Zbaza!CT79)","v":""},{"$f":"IF($Y$32=1,\"Rama osłon z przodu\",\"Front plates support\")","v":"Rama osłon z przodu"},null,null,null,null,null,null,{"$f":"IF(AV24=\"\",\"\",Zbaza!CT112)","v":""},{"$f":"IF($Y$32=1,\"Rama osłon z przodu\",\"Front plates support\")","v":"Rama osłon z przodu"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"boczne\",\"panels\")","v":"boczne"},null,{"$f":"IF(X24<100000,(Zbaza!AB4-1)+Zbaza!BS32,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AK20=2,INDEX((Zbaza!ES161:EX182,Zbaza!ES5:EX26,Zbaza!ES31:EX52,Zbaza!ES187:EX208,Zbaza!ES57:EX78,Zbaza!ES83:EX104,Zbaza!ES109:EX130,Zbaza!ES135:EX156),Zbaza!BA13,Zbaza!BD4,Zbaza!BV4),\"\")","v":""},null,{"$f":"IF(Zbaza!AB5=2,Zbaza!AB1-1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AJ23=2,INDEX((Zbaza!ES161:EX182,Zbaza!FA5:FF26,Zbaza!FA31:FF52,Zbaza!FA187:FF208,Zbaza!FA57:FF78,Zbaza!FA83:FF104,Zbaza!FA109:FF130,Zbaza!FA135:FF156),Zbaza!BA12+Zbaza!AL23,Zbaza!BD4,Zbaza!BV5),\"\")","v":""},null,{"$f":"IF(AN24=\"\",\"\",IF(Zbaza!BA13>10,Zbaza!AB1-1,Zbaza!AG1-1))","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AK26=2,INDEX((Zbaza!ES161:EX176,Zbaza!ES5:EX20,Zbaza!ES31:EX46,Zbaza!ES187:EX208,Zbaza!ES57:EX72,Zbaza!ES83:EX98,Zbaza!ES109:EX124,Zbaza!ES135:EX150),Zbaza!BA15,Zbaza!BD4,Zbaza!BV6),\"\")","v":""},null,{"$f":"IF(Zbaza!AL5=2,Zbaza!AL1-1,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!K171:P175,Zbaza!K155:P159,Zbaza!K163:P167,Zbaza!K179:P183,Zbaza!K187:P191,Zbaza!K195:P199,Zbaza!K203:P207,Zbaza!K211:P215),Zbaza!BG4,Zbaza!BD4,Zbaza!AN93),\"\")","v":89340},null,{"$f":"IF(X25<100000,(Zbaza!AB1-1)+Zbaza!BS29,\"\")","v":2},null,null,null,null,null,{"$f":"IF(Zbaza!AB12=3,36010,\"\")","v":""},null,{"$f":"IF(AF25=36010,2*AH24,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AG12=3,36010,\"\")","v":""},null,{"$f":"IF(AN25=36010,Zbaza!AG15*AP24,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AL12=3,36010,\"\")","v":""},null,{"$f":"IF(AV25=36010,Zbaza!AL15*AX24,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AF24=\"\",\"\",Zbaza!CM68)","v":""},{"$f":"IF($Y$32=1,\"Rama osłon z tyłu\",\"Back plates support\")","v":"Rama osłon z tyłu"},null,null,null,null,null,null,{"$f":"IF(AN24=\"\",\"\",Zbaza!CM84)","v":""},{"$f":"IF($Y$32=1,\"Rama osłon z tyłu\",\"Back plates support\")","v":"Rama osłon z tyłu"},null,null,null,null,null,null,{"$f":"IF(AV24=\"\",\"\",Zbaza!CM116)","v":""},{"$f":"IF($Y$32=1,\"Rama osłon z tyłu\",\"Back plates support\")","v":"Rama osłon z tyłu"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,{"$f":"IF(Zbaza!AK19=2,INDEX((Zbaza!ES161:EX182,Zbaza!ES5:EX26,Zbaza!ES31:EX52,Zbaza!ES187:EX208,Zbaza!ES57:EX78,Zbaza!ES83:EX104,Zbaza!ES109:EX130,Zbaza!ES135:EX156),Zbaza!BA13,Zbaza!BD4,Zbaza!BY4),\"\")","v":""},null,{"$f":"IF(Zbaza!AB6=2,Zbaza!AB1-1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AJ22=2,INDEX((Zbaza!ES161:EX182,Zbaza!FA5:FF26,Zbaza!FA31:FF52,Zbaza!FA187:FF208,Zbaza!FA57:FF78,Zbaza!FA83:FF104,Zbaza!FA109:FF130,Zbaza!FA135:FF156),Zbaza!BA12+Zbaza!AL23,Zbaza!BD4,Zbaza!BY5),\"\")","v":""},null,{"$f":"IF(AN28=\"\",\"\",IF(Zbaza!BA13>10,Zbaza!AB1-1,Zbaza!AG1-1))","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AK25=2,INDEX((Zbaza!ES161:EX176,Zbaza!ES5:EX20,Zbaza!ES31:EX46,Zbaza!ES187:EX208,Zbaza!ES57:EX72,Zbaza!ES83:EX98,Zbaza!ES109:EX124,Zbaza!ES135:EX150),Zbaza!BA15,Zbaza!BD4,Zbaza!BY6),\"\")","v":""},null,{"$f":"IF(Zbaza!AL6=2,Zbaza!AL1-1,\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!AB13=2,33010,\"\")","v":""},null,{"$f":"IF(AF29=33010,2*AH28,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AG13=2,33010,\"\")","v":""},null,{"$f":"IF(AN29=33010,Zbaza!AG16*AP28,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AL13=2,33010,\"\")","v":""},null,{"$f":"IF(AV29=33010,Zbaza!AL16*AX28,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Cokół\",\"Plinth\")","v":"Cokół"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Cokół\",\"Plinth\")","v":"Cokół"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Cokół\",\"Plinth\")","v":"Cokół"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Zbaza!BY14=1,1,2)","v":1},null,null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!K331:O352,Zbaza!K357:O378,Zbaza!K253:O274,Zbaza!K305:O326,Zbaza!K5:O26),Zbaza!BA13,Zbaza!BG4,Zbaza!AN18),\"\")","v":30065},null,{"$f":"IF(AF32=\"\",\"\",Zbaza!AB1-1)","v":2},null,33,null,null,null,{"$f":"IF(Zbaza!BA10>1,INDEX((Zbaza!K383:O404,Zbaza!K409:O430,Zbaza!S257:W278,Zbaza!S309:W330,Zbaza!K5:O26),Zbaza!BA10,Zbaza!BG4,Zbaza!AN18),\"\")","v":""},null,{"$f":"IF(Zbaza!AG3=2,Zbaza!AG1-1,IF(AN32<\"\",AH32,\"\"))","v":""},null,33,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!K331:O346,Zbaza!K357:O372,Zbaza!K253:O268,Zbaza!K305:O320,Zbaza!K5:O20),Zbaza!BA15,Zbaza!BG4,Zbaza!AN18),\"\")","v":""},null,{"$f":"IF(AV32=\"\",\"\",Zbaza!AL1-1)","v":""},null,33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Zdjęcie\",\"Picture\")","v":"Zdjęcie"},null,null,null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!K30:O33),Zbaza!BS13,Zbaza!BG4),\"\")","v":30043},null,{"$f":"IF(Zbaza!AB7=3,Zbaza!AB1-1,\"\")","v":2},null,null,null,null,null,{"$f":"IF(AN32=\"\",\"\",INDEX((Zbaza!K30:O33,Zbaza!K37:O40,Zbaza!K44:O47),Zbaza!BS13,Zbaza!BG4,Zbaza!AN25))","v":""},null,{"$f":"IF(Zbaza!AG3=2,Zbaza!AG1-1,IF(AN33<\"\",AH33,\"\"))","v":""},null,null,null,null,null,{"$f":"IF(AV32=\"\",\"\",INDEX((Zbaza!K30:O33,Zbaza!K37:O40,Zbaza!K44:O47),Zbaza!BS13,Zbaza!BG4,Zbaza!AN32))","v":""},null,{"$f":"IF(AV33=\"\",\"\",Zbaza!AL1-1)","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Przepust IP-55\",\"Gland plates IP-55\")","v":"Przepust IP-55"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Przepust IP-55\",\"Gland plates IP-55\")","v":"Przepust IP-55"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Przepust IP-55\",\"Gland plates IP-55\")","v":"Przepust IP-55"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV30,Zbaza!BG4)","v":""},null,{"$f":"IF(X36=\"\",\"\",Zbaza!BY19)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AB8>1,INDEX((Zbaza!S335:W356),Zbaza!BA13,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!AB8>1,1*Zbaza!AB1-1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AG8=2,INDEX((Zbaza!S374:W395),Zbaza!BA10,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!AG8>1,IF(AN12<\"\",1*Zbaza!AG1-1,AH36),\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AL8>1,INDEX((Zbaza!S335:W350),Zbaza!BA15,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!AL8>1,1*Zbaza!AL1-1,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Daszek\",\"External roof\")","v":"Daszek"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Daszek\",\"External roof\")","v":"Daszek"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Daszek\",\"External roof\")","v":"Daszek"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV31,Zbaza!BG4)","v":""},null,{"$f":"IF(X39=\"\",\"\",Zbaza!BY20)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AB9>1,INDEX((Zbaza!K130:O151),Zbaza!BA13,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(AF39=\"\",\"\",1*Zbaza!AB1-1)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AG9>1,INDEX((Zbaza!K130:O151),Zbaza!BA12,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!AG9>1,1*Zbaza!AG1-1,\"\")","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!AL9>1,INDEX((Zbaza!K130:O145),Zbaza!BA15,Zbaza!BG4),\"\")","v":""},null,{"$f":"IF(Zbaza!AL9>1,1*Zbaza!AL1-1,\"\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV32,Zbaza!BG4)","v":""},null,{"$f":"IF(X42=\"\",\"\",Zbaza!BY21)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB3,Zbaza!CE3,Zbaza!CQ35),\"\")","v":80965},null,{"$f":"IF(AF42=\"\",0,IF(Zbaza!AB38=2,Zbaza!AB1-1,((Zbaza!BJ17)*(Zbaza!AB1-1))))","v":2},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB2+Zbaza!CE7,Zbaza!CE2,Zbaza!CR35),\"\")","v":""},null,{"$f":"IF(AN42=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM17*(Zbaza!$AG$1-1),Zbaza!BM17*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB1,Zbaza!CE1,Zbaza!CS35),\"\")","v":""},null,{"$f":"IF(AV42=\"\",0,IF(Zbaza!AK38=2,Zbaza!AL1-1,((Zbaza!BP17)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV33,Zbaza!BG4)","v":""},null,{"$f":"IF(X45=\"\",\"\",Zbaza!BY22)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB20,Zbaza!CE20,Zbaza!CQ36),\"\")","v":""},null,{"$f":"IF(AF45=\"\",0,IF(Zbaza!AB39=2,Zbaza!AB1-1,((Zbaza!BJ18)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB19+Zbaza!CE24,Zbaza!CE19,Zbaza!CR36),\"\")","v":""},null,{"$f":"IF(AN45=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM18*(Zbaza!$AG$1-1),Zbaza!BM18*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB18,Zbaza!CE18,Zbaza!CS36),\"\")","v":""},null,{"$f":"IF(AV45=\"\",0,IF(Zbaza!AK39=2,Zbaza!AL1-1,((Zbaza!BP18)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV34,Zbaza!BG4)","v":""},null,{"$f":"IF(X48=\"\",\"\",Zbaza!BY23)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB37,Zbaza!CE37,Zbaza!CQ37),\"\")","v":""},null,{"$f":"IF(AF48=\"\",0,IF(Zbaza!AB40=2,Zbaza!AB1-1,((Zbaza!BJ19)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB36+Zbaza!CE41,Zbaza!CE36,Zbaza!CR37),\"\")","v":""},null,{"$f":"IF(AN48=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM19*(Zbaza!$AG$1-1),Zbaza!BM19*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB35,Zbaza!CE35,Zbaza!CS37),\"\")","v":""},null,{"$f":"IF(AV48=\"\",0,IF(Zbaza!AK40=2,Zbaza!AL1-1,((Zbaza!BP19)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV35,Zbaza!BG4)","v":""},null,{"$f":"IF(X51=\"\",\"\",Zbaza!BY24)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB54,Zbaza!CE54,Zbaza!CQ38),\"\")","v":""},null,{"$f":"IF(AF51=\"\",0,IF(Zbaza!AB41=2,Zbaza!AB1-1,((Zbaza!BJ20)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB53+Zbaza!CE58,Zbaza!CE53,Zbaza!CR38),\"\")","v":""},null,{"$f":"IF(AN51=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM20*(Zbaza!$AG$1-1),Zbaza!BM20*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB52,Zbaza!CE52,Zbaza!CS38),\"\")","v":""},null,{"$f":"IF(AV51=\"\",0,IF(Zbaza!AK41=2,Zbaza!AL1-1,((Zbaza!BP20)*(Zbaza!AL1-1))))","v":0},null,null,null,"y"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV36,Zbaza!BG4)","v":""},null,{"$f":"IF(X54=\"\",\"\",Zbaza!BY25)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB71,Zbaza!CE71,Zbaza!CQ39),\"\")","v":""},null,{"$f":"IF(AF54=\"\",0,IF(Zbaza!AB42=2,Zbaza!AB1-1,((Zbaza!BJ21)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB70+Zbaza!CE75,Zbaza!CE70,Zbaza!CR39),\"\")","v":""},null,{"$f":"IF(AN54=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM21*(Zbaza!$AG$1-1),Zbaza!BM21*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB69,Zbaza!CE69,Zbaza!CS39),\"\")","v":""},null,{"$f":"IF(AV54=\"\",0,IF(Zbaza!AK42=2,Zbaza!AL1-1,((Zbaza!BP21)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV37,Zbaza!BG4)","v":""},null,{"$f":"IF(X57=\"\",\"\",Zbaza!BY26)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB88,Zbaza!CE88,Zbaza!CQ40),\"\")","v":""},null,{"$f":"IF(AF57=\"\",0,IF(Zbaza!AB43=2,Zbaza!AB1-1,((Zbaza!BJ22)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB87+Zbaza!CE92,Zbaza!CE87,Zbaza!CR40),\"\")","v":""},null,{"$f":"IF(AN57=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM22*(Zbaza!$AG$1-1),Zbaza!BM22*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB86,Zbaza!CE86,Zbaza!CS40),\"\")","v":""},null,{"$f":"IF(AV57=\"\",0,IF(Zbaza!AK43=2,Zbaza!AL1-1,((Zbaza!BP22)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV38,Zbaza!BG4)","v":""},null,{"$f":"IF(X60=\"\",\"\",Zbaza!BY27)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB105,Zbaza!CE105,Zbaza!CQ41),\"\")","v":""},null,{"$f":"IF(AF60=\"\",0,IF(Zbaza!AB44=2,Zbaza!AB1-1,((Zbaza!BJ23)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB104+Zbaza!CE109,Zbaza!CE104,Zbaza!CR41),\"\")","v":""},null,{"$f":"IF(AN60=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM23*(Zbaza!$AG$1-1),Zbaza!BM23*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB103,Zbaza!CE103,Zbaza!CS41),\"\")","v":""},null,{"$f":"IF(AV60=\"\",0,IF(Zbaza!AK44=2,Zbaza!AL1-1,((Zbaza!BP23)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV39,Zbaza!BG4)","v":""},null,{"$f":"IF(X63=\"\",\"\",Zbaza!BY28)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB122,Zbaza!CE122,Zbaza!CQ42),\"\")","v":""},null,{"$f":"IF(AF63=\"\",0,IF(Zbaza!AB45=2,Zbaza!AB1-1,((Zbaza!BJ24)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB121+Zbaza!CE126,Zbaza!CE121,Zbaza!CR42),\"\")","v":""},null,{"$f":"IF(AN63=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM24*(Zbaza!$AG$1-1),Zbaza!BM24*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB120,Zbaza!CE120,Zbaza!CS42),\"\")","v":""},null,{"$f":"IF(AV63=\"\",0,IF(Zbaza!AK45=2,Zbaza!AL1-1,((Zbaza!BP24)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV40,Zbaza!BG4)","v":""},null,{"$f":"IF(X66=\"\",\"\",Zbaza!BY29)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB139,Zbaza!CE139,Zbaza!CQ43),\"\")","v":""},null,{"$f":"IF(AF66=\"\",0,IF(Zbaza!AB46=2,Zbaza!AB1-1,((Zbaza!BJ25)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB138+Zbaza!CE143,Zbaza!CE138,Zbaza!CR43),\"\")","v":""},null,{"$f":"IF(AN66=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM25*(Zbaza!$AG$1-1),Zbaza!BM25*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB137,Zbaza!CE137,Zbaza!CS43),\"\")","v":""},null,{"$f":"IF(AV66=\"\",0,IF(Zbaza!AK46=2,Zbaza!AL1-1,((Zbaza!BP25)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                     for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV41,Zbaza!BG4)","v":""},null,{"$f":"IF(X69=\"\",\"\",Zbaza!BY30)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB156,Zbaza!CE156,Zbaza!CQ44),\"\")","v":""},null,{"$f":"IF(AF69=\"\",0,IF(Zbaza!AB47=2,Zbaza!AB1-1,((Zbaza!BJ26)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB155+Zbaza!CE160,Zbaza!CE155,Zbaza!CR44),\"\")","v":""},null,{"$f":"IF(AN69=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM26*(Zbaza!$AG$1-1),Zbaza!BM26*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB154,Zbaza!CE154,Zbaza!CS44),\"\")","v":""},null,{"$f":"IF(AV69=\"\",0,IF(Zbaza!AK47=2,Zbaza!AL1-1,((Zbaza!BP26)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV42,Zbaza!BG4)","v":""},null,{"$f":"IF(X72=\"\",\"\",Zbaza!BY31)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB173,Zbaza!CE173,Zbaza!CQ45),\"\")","v":""},null,{"$f":"IF(AF72=\"\",0,IF(Zbaza!AB48=2,Zbaza!AB1-1,((Zbaza!BJ27)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB172+Zbaza!CE177,Zbaza!CE172,Zbaza!CR45),\"\")","v":""},null,{"$f":"IF(AN72=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM27*(Zbaza!$AG$1-1),Zbaza!BM27*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB171,Zbaza!CE171,Zbaza!CS45),\"\")","v":""},null,{"$f":"IF(AV72=\"\",0,IF(Zbaza!AK48=2,Zbaza!AL1-1,((Zbaza!BP27)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Osłony płyty\",\"Equipment for Width\")","v":"Osłony płyty"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV43,Zbaza!BG4)","v":""},null,{"$f":"IF(X75=\"\",\"\",Zbaza!BY32)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!K1:P1,Zbaza!K1:P1,Zbaza!K51:P73),Zbaza!CB190,Zbaza!CE190,Zbaza!CQ46),\"\")","v":""},null,{"$f":"IF(AF75=\"\",0,IF(Zbaza!AB49=2,Zbaza!AB1-1,((Zbaza!BJ28)*(Zbaza!AB1-1))))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!AG30>0,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K77:P126),Zbaza!CB189+Zbaza!CE194,Zbaza!CE189,Zbaza!CR46),\"\")","v":""},null,{"$f":"IF(AN75=\"\",0,IF(Zbaza!$X$1=1,Zbaza!BM28*(Zbaza!$AG$1-1),Zbaza!BM28*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!CW4:DH18,Zbaza!CW22:DH36,Zbaza!CW40:DH54,Zbaza!CW58:DH72,Zbaza!CW76:DH90,Zbaza!CW94:DH108,Zbaza!CW112:DH126,Zbaza!CW130:DH144,Zbaza!CW148:DH162,Zbaza!CW166:DH180,Zbaza!CW184:DH198,Zbaza!CW76:DH90,Zbaza!CW112:DH126,Zbaza!K51:P73),Zbaza!CB188,Zbaza!CE188,Zbaza!CS46),\"\")","v":""},null,{"$f":"IF(AV75=\"\",0,IF(Zbaza!AK49=2,Zbaza!AL1-1,((Zbaza!BP28)*(Zbaza!AL1-1))))","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH78","v":0},null,{"$f":"AP78","v":0},null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV44,Zbaza!BG4)","v":""},null,{"$f":"IF(X78=\"\",\"\",Zbaza!BY33)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA13,Zbaza!CH4),\"\")","v":""},null,{"$f":"IF(AF78=\"\",0,((Zbaza!BJ29)*(Zbaza!AB1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!$AG$30>0,INDEX((Zbaza!$DK$84:$EF$107,Zbaza!$DK$123:$EF$146),Zbaza!$BA$12+Zbaza!$CH$27,Zbaza!$CH21,Zbaza!$CH$20),\"\")","v":""},null,{"$f":"IF(AN78=\"\",0,IF(Zbaza!$AG$43=2,Zbaza!BM29*(Zbaza!$AG$1-1),Zbaza!$BM$29*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA15,Zbaza!CH38),\"\")","v":""},null,{"$f":"IF(AV78=\"\",0,((Zbaza!BP29)*(Zbaza!AL1-1)))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH79","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH81","v":0},null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV45,Zbaza!BG4)","v":""},null,{"$f":"IF(X81=\"\",\"\",Zbaza!BY34)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA13,Zbaza!CH5),\"\")","v":""},null,{"$f":"IF(AF81=\"\",0,((Zbaza!BJ30)*(Zbaza!AB1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!$AG$30>0,INDEX((Zbaza!$DK$84:$EF$107,Zbaza!$DK$123:$EF$146),Zbaza!$BA$12+Zbaza!$CH$27,Zbaza!$CH22,Zbaza!$CH$20),\"\")","v":""},null,{"$f":"IF(AN81=\"\",0,IF(Zbaza!$AG$43=2,Zbaza!BM30*(Zbaza!$AG$1-1),Zbaza!$BM$30*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA15,Zbaza!CH39),\"\")","v":""},null,{"$f":"IF(AV81=\"\",0,((Zbaza!BP30)*(Zbaza!AL1-1)))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH84","v":0},null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV46,Zbaza!BG4)","v":""},null,{"$f":"IF(X84=\"\",\"\",Zbaza!BY35)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA13,Zbaza!CH6),\"\")","v":""},null,{"$f":"IF(AF84=\"\",0,((Zbaza!BJ31)*(Zbaza!AB1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!$AG$30>0,INDEX((Zbaza!$DK$84:$EF$107,Zbaza!$DK$123:$EF$146),Zbaza!$BA$12+Zbaza!$CH$27,Zbaza!$CH23,Zbaza!$CH$20),\"\")","v":""},null,{"$f":"IF(AN84=\"\",0,IF(Zbaza!$AG$43=2,Zbaza!BM31*(Zbaza!$AG$1-1),Zbaza!$BM$31*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA15,Zbaza!CH40),\"\")","v":""},null,{"$f":"IF(AV84=\"\",0,((Zbaza!BP31)*(Zbaza!AL1-1)))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH87","v":0},null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV47,Zbaza!BG4)","v":""},null,{"$f":"IF(X87=\"\",\"\",Zbaza!BY36)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA13,Zbaza!CH7),\"\")","v":""},null,{"$f":"IF(AF87=\"\",0,((Zbaza!BJ32)*(Zbaza!AB1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!$AG$30>0,INDEX((Zbaza!$DK$84:$EF$107,Zbaza!$DK$123:$EF$146),Zbaza!$BA$12+Zbaza!$CH$27,Zbaza!$CH24,Zbaza!$CH$20),\"\")","v":""},null,{"$f":"IF(AN87=\"\",0,IF(Zbaza!$AG$43=2,Zbaza!BM32*(Zbaza!$AG$1-1),Zbaza!$BM$32*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA15,Zbaza!CH41),\"\")","v":""},null,{"$f":"IF(AV87=\"\",0,((Zbaza!BP32)*(Zbaza!AL1-1)))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH90","v":0},null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV48,Zbaza!BG4)","v":""},null,{"$f":"IF(X90=\"\",\"\",Zbaza!BY37)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA13,Zbaza!CH8),\"\")","v":""},null,{"$f":"IF(AF90=\"\",0,((Zbaza!BJ33)*(Zbaza!AB1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!$AG$30>0,INDEX((Zbaza!$DK$84:$EF$107,Zbaza!$DK$123:$EF$146),Zbaza!$BA$12+Zbaza!$CH$27,Zbaza!$CH25,Zbaza!$CH$20),\"\")","v":""},null,{"$f":"IF(AN90=\"\",0,IF(Zbaza!$AG$43=2,Zbaza!BM33*(Zbaza!$AG$1-1),Zbaza!$BM$33*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA15,Zbaza!CH42),\"\")","v":""},null,{"$f":"IF(AV90=\"\",0,((Zbaza!BP33)*(Zbaza!AL1-1)))","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria                         głębokość\",\"Accessories                         for Depth\")","v":"Akcesoria                         głębokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"},null,null,null,null,null,null,null,{"$f":"IF($Y$32=1,\"Akcesoria szerokość\",\"Accessories for Width\")","v":"Akcesoria szerokość"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AH93","v":0},null,null,null,null,{"$f":"INDEX((Zbaza!DK7:DP80),Zbaza!BV49,Zbaza!BG4)","v":""},null,{"$f":"IF(X93=\"\",\"\",Zbaza!BY38)","v":""},null,null,null,null,null,{"$f":"IF(Zbaza!BA13>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA13,Zbaza!CH9),\"\")","v":""},null,{"$f":"IF(AF93=\"\",0,((Zbaza!BJ34)*(Zbaza!AB1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!$AG$30>0,INDEX((Zbaza!$DK$84:$EF$107,Zbaza!$DK$123:$EF$146),Zbaza!$BA$12+Zbaza!$CH$27,Zbaza!$CH26,Zbaza!$CH$20),\"\")","v":""},null,{"$f":"IF(AN93=\"\",0,IF(Zbaza!$AG$43=2,Zbaza!BM34*(Zbaza!$AG$1-1),Zbaza!$BM$34*(Zbaza!$AB$1-1)))","v":0},null,null,null,null,null,{"$f":"IF(Zbaza!BA15>1,INDEX((Zbaza!DK84:EF107),Zbaza!BA15,Zbaza!CH43),\"\")","v":""},null,{"$f":"IF(AV93=\"\",0,((Zbaza!BP34)*(Zbaza!AL1-1)))","v":0}]

{"sheet":"Oferta","index":2,"n_rows":305,"n_cols":20,"rows_kept":305,"cut":false,"hidden":false,"merged":[[9,13,10,13],[8,9,8,10]]}
[null,null,null,null,{"$f":"IF(F2<>\"\",\"Udzielono dodatkowego upustu:\",\"\")","v":""},null,null,1500,null,"Data:",{"$f":"TODAY()","v":"2025-01-29"}]
[]
[]
[]
[]
[]
[null,null,null,null,{"$f":"Cennik!$B$2","v":"Cennik 03-2025"}]
[]
[null,null,null,null,null,null,null,null,"Wartość",{"$f":"SUM(K12:K305)","v":8639.8000000000011}]
["L.p","Numer","Szt.","Pak.","Opis","Rodzina","Cena za szt.","Upust","Grupa","Cena za szt.","Wartość",null,"Grupa","Rabat"]
[null,"katalogowy",null,"po",null,null,"katalogowa",null,"upustu","po upuście","netto",null,"rabatowa"]
[{"$f":"IF(B12<>\"\",A11+1,\"\")","v":1},89340,2,{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":11},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D400"},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_COVERS"},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":675},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(I12),TEXT(I12,\"0\"),I12),$M$12:$N$44,2,FALSE),\"\")","v":0},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},{"$f":"IF(B12<>\"\",G12*(1-H12),\"\")","v":675},{"$f":"IF(B12<>\"\",C12*(1-H12)*G12,\"\")","v":1350},null,"1-ZE-01",null,null,{"$f":"IF(B12<>\"\",$K$2,\"\")","v":0},null,{"$f":"IF(B12>1,B12,\"\")","v":89340},{"$f":"IF(R12=\"\",\"\",C12)","v":2},{"$f":"IF(B12=\"\",\"\",E12)","v":"ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D400"}]
[2,84065,2,{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":12},{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - RAMA, H2000 X D400 X W650"},{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_FRAME_2000"},{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":874.8},0,{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},874.8,1749.6,null,"1-ZE-02",null,null,{"$f":"IF(B13<>\"\",$K$2,\"\")","v":0},null,{"$f":"IF(B13>1,B13,\"\")","v":84065},2,{"$f":"IF(B13=\"\",\"\",E13)","v":"ZENERGY - RAMA, H2000 X D400 X W650"}]
[3,81265,2,{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":8},{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W650"},{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_COVERS"},{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":541.1},0,{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},541.1,1082.2,null,"1-ZE-03",null,null,0,null,81265,2,"ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W650"]
[4,80965,2,{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":2},{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W650 + WSPORNIKI,  ( 1850 X 550 )"},{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_PLAIN_PLATES"},{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":745.2},0,{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},745.2,1490.4,null,"1-ZE-04",null,null,0,null,80965,2,"ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W650 + WSPORNIKI,  ( 1850 X 550 )"]
[5,80365,2,{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":8},{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - DRZWI PEŁNE IP30, H2000 X W650"},{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_DOORS_2000"},{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":953.6},0,{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},953.6,1907.2,null,"1-ZE-06",null,null,0,null,80365,2,"ZENERGY - DRZWI PEŁNE IP30, H2000 X W650"]
[6,31465,2,{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":6},{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - POKRYWA GÓRNA IP30, W650, D400"},{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_COVERS"},{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":203},0,{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},203,406,null,"1-ZE-08",null,null,0,null,31465,2,"ZENERGY - POKRYWA GÓRNA IP30, W650, D400"]
[7,30065,2,{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":4},{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650"},{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_PLINTHS"},{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":177.1},0,{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},177.1,354.2,null,"1-ZE-09",null,null,0,null,30065,2,"ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650"]
[8,30043,2,{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":6},{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":"ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D400"},{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":"OE_PLINTHS"},{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":150.1},0,{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":"1-ZE-01"},150.1,300.2,null,"1-ZE-10",null,null,0,null,30043,2,"ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D400"]
["",null,null,{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,"1-ZE-18",null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,"1-ZE-19",null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",{"$f":"IF(R44=\"\",\"\",C44)","v":""},""]
["",null,null,{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
[{"$f":"IF(B76<>\"\",A75+1,\"\")","v":""},null,null,{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(I76),TEXT(I76,\"0\"),I76),$M$12:$N$44,2,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",G76*(1-H76),\"\")","v":""},{"$f":"IF(B76<>\"\",C76*(1-H76)*G76,\"\")","v":""},null,null,null,null,"",null,"",{"$f":"IF(R76=\"\",\"\",C76)","v":""},""]
["",null,null,{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B77<>\"\",$K$2,\"\")","v":""},null,{"$f":"IF(B77>1,B77,\"\")","v":""},"",{"$f":"IF(B77=\"\",\"\",E77)","v":""}]
["",null,null,{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
[{"$f":"IF(B140<>\"\",A139+1,\"\")","v":""},null,null,{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(I140),TEXT(I140,\"0\"),I140),$M$12:$N$44,2,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",G140*(1-H140),\"\")","v":""},{"$f":"IF(B140<>\"\",C140*(1-H140)*G140,\"\")","v":""},null,null,null,null,"",null,"",{"$f":"IF(R140=\"\",\"\",C140)","v":""},""]
["",null,null,{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B141<>\"\",$K$2,\"\")","v":""},null,{"$f":"IF(B141>1,B141,\"\")","v":""},"",{"$f":"IF(B141=\"\",\"\",E141)","v":""}]
["",null,null,{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
[{"$f":"IF(B204<>\"\",A203+1,\"\")","v":""},null,null,{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(I204),TEXT(I204,\"0\"),I204),$M$12:$N$44,2,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",G204*(1-H204),\"\")","v":""},{"$f":"IF(B204<>\"\",C204*(1-H204)*G204,\"\")","v":""},null,null,null,null,"",null,"",{"$f":"IF(R204=\"\",\"\",C204)","v":""},""]
["",null,null,{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B205<>\"\",$K$2,\"\")","v":""},null,{"$f":"IF(B205>1,B205,\"\")","v":""},"",{"$f":"IF(B205=\"\",\"\",E205)","v":""}]
["",null,null,{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
[{"$f":"IF(B268<>\"\",A267+1,\"\")","v":""},null,null,{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(I268),TEXT(I268,\"0\"),I268),$M$12:$N$44,2,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",G268*(1-H268),\"\")","v":""},{"$f":"IF(B268<>\"\",C268*(1-H268)*G268,\"\")","v":""},null,null,null,null,"",null,"",{"$f":"IF(R268=\"\",\"\",C268)","v":""},""]
["",null,null,{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B269<>\"\",$K$2,\"\")","v":""},null,{"$f":"IF(B269>1,B269,\"\")","v":""},"",{"$f":"IF(B269=\"\",\"\",E269)","v":""}]
["",null,null,{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
["",null,null,{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"","",""]
[{"$f":"IF(B301<>\"\",A300+1,\"\")","v":""},null,null,{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",G301*(1-H301),\"\")","v":""},{"$f":"IF(B301<>\"\",C301*(1-H301)*G301,\"\")","v":""},null,null,null,null,"",null,"","",""]
[{"$f":"IF(B302<>\"\",A301+1,\"\")","v":""},null,null,{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",G302*(1-H302),\"\")","v":""},{"$f":"IF(B302<>\"\",C302*(1-H302)*G302,\"\")","v":""},null,null,null,null,"",null,"","",""]
[null,null,null,{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",G303*(1-H303),\"\")","v":""},{"$f":"IF(B303<>\"\",C303*(1-H303)*G303,\"\")","v":""},null,null,null,null,"",null,"","",""]
[null,null,null,{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",G304*(1-H304),\"\")","v":""},{"$f":"IF(B304<>\"\",C304*(1-H304)*G304,\"\")","v":""},null,null,null,null,"",null,"","",""]
[null,null,null,{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$K$52318,7,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",G305*(1-H305),\"\")","v":""},{"$f":"IF(B305<>\"\",C305*(1-H305)*G305,\"\")","v":""},null,null,null,null,"",null,"","",""]

{"sheet":"Zgrupuj","index":3,"n_rows":307,"n_cols":57,"rows_kept":307,"cut":false,"hidden":false,"merged":[[8,9,8,10],[10,46,10,49],[1,41,1,44]]}
[null,null,null,null,{"$f":"IF(F2<>\"\",\"Udzielono dodatkowego upustu:\",\"\")","v":""},null,null,1500,null,"Data:",{"$f":"TODAY()","v":"2025-01-29"}]
[null,null,null,null,null,null,null,null,null,"Dla:","ZZ01",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"PROJEKT",{"$f":"CONCATENATE(AN16,AM14,AO16,AM14,AU11)","v":"__Wpisz nazwę zestawienia"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 1\",\"Project 1\")","v":"PROJEKT 1"},null,{"$f":"IF($R$2=1,\"1\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 2\",\"Project 2\")","v":"PROJEKT 2"},null,{"$f":"IF($R$2=2,\"2\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 3\",\"Project 3\")","v":"PROJEKT 3"},null,{"$f":"IF($R$2=3,\"3\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 4\",\"Project 4\")","v":"PROJEKT 4"},null,{"$f":"IF($R$2=4,\"4\",\"\")","v":""}]
[null,null,null,null,{"$f":"Cennik!$B$2","v":"Cennik 03-2025"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 5\",\"Project 5\")","v":"PROJEKT 5"},null,{"$f":"IF($R$2=5,\"5\",\"\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 6\",\"Project 6\")","v":"PROJEKT 6"},null,{"$f":"IF($R$2=6,\"6\",\"\")","v":""}]
[null,null,null,null,"Wpisz nazwę zestawienia",null,null,null,"Wartość",{"$f":"SUM(K12:K305)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 7\",\"Project 7\")","v":"PROJEKT 7"},null,{"$f":"IF($R$2=7,\"7\",\"\")","v":""}]
["L.p","Numer","Szt.","Pak.","Opis","Dostęp","Cena za szt.","Upust","Grupa","Cena za szt.","Wartość",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 8\",\"Project 8\")","v":"PROJEKT 8"},null,{"$f":"IF($R$2=8,\"8\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"Grupa","Rabat"]
[null,"katalogowy",null,"po",null,"ność","katalogowa",null,"upustu","po upuście","netto",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 9\",\"Project 9\")","v":"PROJEKT 9"},null,{"$f":"IF($R$2=9,\"9\",\"\")","v":""},null,null,null,null,{"$f":"IF(E9=\"\",\"\",E9)","v":"Wpisz nazwę zestawienia"},null,null,null,"WARTOŚĆ",null,null,null,null,"rabatowa"]
[{"$f":"IF(B12<>\"\",A11+1,\"\")","v":""},null,{"$f":"IF(A12<>\"\",1,\"\")","v":""},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(I12),TEXT(I12,\"0\"),I12),$BD$12:$BE$44,2,FALSE),\"\")","v":""},{"$f":"IF(B12<>\"\",VLOOKUP(IF(ISNUMBER(B12),TEXT(B12,\"0\"),B12),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B12<>\"\",G12*(1-H12),\"\")","v":""},{"$f":"IF(B12<>\"\",C12*(1-H12)*G12,\"\")","v":""},null,null,null,null,{"$f":"IF(B12<>\"\",$K$2,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 10\",\"Project 10\")","v":"PROJEKT 10"},null,{"$f":"IF($R$2=10,\"10\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-01",0.3]
["",null,"",{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B13<>\"\",VLOOKUP(IF(ISNUMBER(B13),TEXT(B13,\"0\"),B13),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TODAY()","v":"2025-01-29"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-02",0.02]
["",null,"",{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B14<>\"\",VLOOKUP(IF(ISNUMBER(B14),TEXT(B14,\"0\"),B14),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B14<>\"\",$K$2,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"_","2015-04-06",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-03",0.3]
["",null,"",{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B15<>\"\",VLOOKUP(IF(ISNUMBER(B15),TEXT(B15,\"0\"),B15),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"/",6,"/",201,5,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-04",0.02]
["",null,"",{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B16<>\"\",VLOOKUP(IF(ISNUMBER(B16),TEXT(B16,\"0\"),B16),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AL15,AM15,AN15,AO15,AP15,AQ15,AR15)","v":"4/6/2015"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-06",0.15]
["",null,"",{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B17<>\"\",VLOOKUP(IF(ISNUMBER(B17),TEXT(B17,\"0\"),B17),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-08",0.3]
["",null,"",{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B18<>\"\",VLOOKUP(IF(ISNUMBER(B18),TEXT(B18,\"0\"),B18),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B18<>\"\",$K$2,\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-09",0.1]
["",null,"",{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B19<>\"\",VLOOKUP(IF(ISNUMBER(B19),TEXT(B19,\"0\"),B19),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-10",0.3]
["",null,"",{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B20<>\"\",VLOOKUP(IF(ISNUMBER(B20),TEXT(B20,\"0\"),B20),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-18",0.02]
["",null,"",{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B21<>\"\",VLOOKUP(IF(ISNUMBER(B21),TEXT(B21,\"0\"),B21),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-ZE-19",0.2]
["",null,"",{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B22<>\"\",VLOOKUP(IF(ISNUMBER(B22),TEXT(B22,\"0\"),B22),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B23<>\"\",VLOOKUP(IF(ISNUMBER(B23),TEXT(B23,\"0\"),B23),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B24<>\"\",VLOOKUP(IF(ISNUMBER(B24),TEXT(B24,\"0\"),B24),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B25<>\"\",VLOOKUP(IF(ISNUMBER(B25),TEXT(B25,\"0\"),B25),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,{"$f":"IF(B25<>\"\",$K$2,\"\")","v":""}]
["",null,"",{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B26<>\"\",VLOOKUP(IF(ISNUMBER(B26),TEXT(B26,\"0\"),B26),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B27<>\"\",VLOOKUP(IF(ISNUMBER(B27),TEXT(B27,\"0\"),B27),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B28<>\"\",VLOOKUP(IF(ISNUMBER(B28),TEXT(B28,\"0\"),B28),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B29<>\"\",VLOOKUP(IF(ISNUMBER(B29),TEXT(B29,\"0\"),B29),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B30<>\"\",VLOOKUP(IF(ISNUMBER(B30),TEXT(B30,\"0\"),B30),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B31<>\"\",VLOOKUP(IF(ISNUMBER(B31),TEXT(B31,\"0\"),B31),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B32<>\"\",VLOOKUP(IF(ISNUMBER(B32),TEXT(B32,\"0\"),B32),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B33<>\"\",VLOOKUP(IF(ISNUMBER(B33),TEXT(B33,\"0\"),B33),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,""]
["",null,"",{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B34<>\"\",VLOOKUP(IF(ISNUMBER(B34),TEXT(B34,\"0\"),B34),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,{"$f":"IF(B34>1,B34,\"\")","v":""},{"$f":"IF(R34=\"\",\"\",C34)","v":""}]
["",null,"",{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B35<>\"\",VLOOKUP(IF(ISNUMBER(B35),TEXT(B35,\"0\"),B35),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,{"$f":"IF(B35>1,B35,\"\")","v":""},{"$f":"IF(R35=\"\",\"\",C35)","v":""}]
["",null,"",{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B36<>\"\",VLOOKUP(IF(ISNUMBER(B36),TEXT(B36,\"0\"),B36),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,{"$f":"IF(B36>1,B36,\"\")","v":""},{"$f":"IF(R36=\"\",\"\",C36)","v":""}]
["",null,"",{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B37<>\"\",VLOOKUP(IF(ISNUMBER(B37),TEXT(B37,\"0\"),B37),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,{"$f":"IF(B37>1,B37,\"\")","v":""},{"$f":"IF(R37=\"\",\"\",C37)","v":""}]
["",null,"",{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B38<>\"\",VLOOKUP(IF(ISNUMBER(B38),TEXT(B38,\"0\"),B38),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B39<>\"\",VLOOKUP(IF(ISNUMBER(B39),TEXT(B39,\"0\"),B39),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B40<>\"\",VLOOKUP(IF(ISNUMBER(B40),TEXT(B40,\"0\"),B40),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B41<>\"\",VLOOKUP(IF(ISNUMBER(B41),TEXT(B41,\"0\"),B41),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B42<>\"\",VLOOKUP(IF(ISNUMBER(B42),TEXT(B42,\"0\"),B42),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B43<>\"\",VLOOKUP(IF(ISNUMBER(B43),TEXT(B43,\"0\"),B43),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B44<>\"\",VLOOKUP(IF(ISNUMBER(B44),TEXT(B44,\"0\"),B44),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B45<>\"\",VLOOKUP(IF(ISNUMBER(B45),TEXT(B45,\"0\"),B45),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
["",null,"",{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B46<>\"\",VLOOKUP(IF(ISNUMBER(B46),TEXT(B46,\"0\"),B46),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B47<>\"\",VLOOKUP(IF(ISNUMBER(B47),TEXT(B47,\"0\"),B47),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B48<>\"\",VLOOKUP(IF(ISNUMBER(B48),TEXT(B48,\"0\"),B48),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B49<>\"\",VLOOKUP(IF(ISNUMBER(B49),TEXT(B49,\"0\"),B49),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B50<>\"\",VLOOKUP(IF(ISNUMBER(B50),TEXT(B50,\"0\"),B50),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B51<>\"\",VLOOKUP(IF(ISNUMBER(B51),TEXT(B51,\"0\"),B51),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B52<>\"\",VLOOKUP(IF(ISNUMBER(B52),TEXT(B52,\"0\"),B52),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B53<>\"\",VLOOKUP(IF(ISNUMBER(B53),TEXT(B53,\"0\"),B53),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B54<>\"\",VLOOKUP(IF(ISNUMBER(B54),TEXT(B54,\"0\"),B54),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B55<>\"\",VLOOKUP(IF(ISNUMBER(B55),TEXT(B55,\"0\"),B55),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B56<>\"\",VLOOKUP(IF(ISNUMBER(B56),TEXT(B56,\"0\"),B56),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B57<>\"\",VLOOKUP(IF(ISNUMBER(B57),TEXT(B57,\"0\"),B57),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B58<>\"\",VLOOKUP(IF(ISNUMBER(B58),TEXT(B58,\"0\"),B58),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B59<>\"\",VLOOKUP(IF(ISNUMBER(B59),TEXT(B59,\"0\"),B59),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B60<>\"\",VLOOKUP(IF(ISNUMBER(B60),TEXT(B60,\"0\"),B60),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B61<>\"\",VLOOKUP(IF(ISNUMBER(B61),TEXT(B61,\"0\"),B61),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B62<>\"\",VLOOKUP(IF(ISNUMBER(B62),TEXT(B62,\"0\"),B62),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B63<>\"\",VLOOKUP(IF(ISNUMBER(B63),TEXT(B63,\"0\"),B63),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B64<>\"\",VLOOKUP(IF(ISNUMBER(B64),TEXT(B64,\"0\"),B64),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B65<>\"\",VLOOKUP(IF(ISNUMBER(B65),TEXT(B65,\"0\"),B65),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B66<>\"\",VLOOKUP(IF(ISNUMBER(B66),TEXT(B66,\"0\"),B66),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B67<>\"\",VLOOKUP(IF(ISNUMBER(B67),TEXT(B67,\"0\"),B67),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B68<>\"\",VLOOKUP(IF(ISNUMBER(B68),TEXT(B68,\"0\"),B68),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B69<>\"\",VLOOKUP(IF(ISNUMBER(B69),TEXT(B69,\"0\"),B69),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B70<>\"\",VLOOKUP(IF(ISNUMBER(B70),TEXT(B70,\"0\"),B70),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B71<>\"\",VLOOKUP(IF(ISNUMBER(B71),TEXT(B71,\"0\"),B71),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B72<>\"\",VLOOKUP(IF(ISNUMBER(B72),TEXT(B72,\"0\"),B72),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B73<>\"\",VLOOKUP(IF(ISNUMBER(B73),TEXT(B73,\"0\"),B73),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B74<>\"\",VLOOKUP(IF(ISNUMBER(B74),TEXT(B74,\"0\"),B74),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B75<>\"\",VLOOKUP(IF(ISNUMBER(B75),TEXT(B75,\"0\"),B75),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
[{"$f":"IF(B76<>\"\",A75+1,\"\")","v":""},null,{"$f":"IF(A76<>\"\",1,\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(I76),TEXT(I76,\"0\"),I76),$BD$12:$BE$44,2,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",VLOOKUP(IF(ISNUMBER(B76),TEXT(B76,\"0\"),B76),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B76<>\"\",G76*(1-H76),\"\")","v":""},{"$f":"IF(B76<>\"\",C76*(1-H76)*G76,\"\")","v":""},null,null,null,null,{"$f":"IF(B76<>\"\",$K$2,\"\")","v":""},"","",{"$f":"IF(R76=\"\",\"\",C76)","v":""}]
["",null,"",{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B77<>\"\",VLOOKUP(IF(ISNUMBER(B77),TEXT(B77,\"0\"),B77),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","",{"$f":"IF(B77>1,B77,\"\")","v":""},""]
["",null,"",{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B78<>\"\",VLOOKUP(IF(ISNUMBER(B78),TEXT(B78,\"0\"),B78),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B79<>\"\",VLOOKUP(IF(ISNUMBER(B79),TEXT(B79,\"0\"),B79),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B80<>\"\",VLOOKUP(IF(ISNUMBER(B80),TEXT(B80,\"0\"),B80),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B81<>\"\",VLOOKUP(IF(ISNUMBER(B81),TEXT(B81,\"0\"),B81),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B82<>\"\",VLOOKUP(IF(ISNUMBER(B82),TEXT(B82,\"0\"),B82),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B83<>\"\",VLOOKUP(IF(ISNUMBER(B83),TEXT(B83,\"0\"),B83),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B84<>\"\",VLOOKUP(IF(ISNUMBER(B84),TEXT(B84,\"0\"),B84),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B85<>\"\",VLOOKUP(IF(ISNUMBER(B85),TEXT(B85,\"0\"),B85),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B86<>\"\",VLOOKUP(IF(ISNUMBER(B86),TEXT(B86,\"0\"),B86),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B87<>\"\",VLOOKUP(IF(ISNUMBER(B87),TEXT(B87,\"0\"),B87),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B88<>\"\",VLOOKUP(IF(ISNUMBER(B88),TEXT(B88,\"0\"),B88),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B89<>\"\",VLOOKUP(IF(ISNUMBER(B89),TEXT(B89,\"0\"),B89),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B90<>\"\",VLOOKUP(IF(ISNUMBER(B90),TEXT(B90,\"0\"),B90),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B91<>\"\",VLOOKUP(IF(ISNUMBER(B91),TEXT(B91,\"0\"),B91),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B92<>\"\",VLOOKUP(IF(ISNUMBER(B92),TEXT(B92,\"0\"),B92),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B93<>\"\",VLOOKUP(IF(ISNUMBER(B93),TEXT(B93,\"0\"),B93),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B94<>\"\",VLOOKUP(IF(ISNUMBER(B94),TEXT(B94,\"0\"),B94),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B95<>\"\",VLOOKUP(IF(ISNUMBER(B95),TEXT(B95,\"0\"),B95),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B96<>\"\",VLOOKUP(IF(ISNUMBER(B96),TEXT(B96,\"0\"),B96),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B97<>\"\",VLOOKUP(IF(ISNUMBER(B97),TEXT(B97,\"0\"),B97),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B98<>\"\",VLOOKUP(IF(ISNUMBER(B98),TEXT(B98,\"0\"),B98),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B99<>\"\",VLOOKUP(IF(ISNUMBER(B99),TEXT(B99,\"0\"),B99),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B100<>\"\",VLOOKUP(IF(ISNUMBER(B100),TEXT(B100,\"0\"),B100),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B101<>\"\",VLOOKUP(IF(ISNUMBER(B101),TEXT(B101,\"0\"),B101),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B102<>\"\",VLOOKUP(IF(ISNUMBER(B102),TEXT(B102,\"0\"),B102),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B103<>\"\",VLOOKUP(IF(ISNUMBER(B103),TEXT(B103,\"0\"),B103),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B104<>\"\",VLOOKUP(IF(ISNUMBER(B104),TEXT(B104,\"0\"),B104),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B105<>\"\",VLOOKUP(IF(ISNUMBER(B105),TEXT(B105,\"0\"),B105),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B106<>\"\",VLOOKUP(IF(ISNUMBER(B106),TEXT(B106,\"0\"),B106),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B107<>\"\",VLOOKUP(IF(ISNUMBER(B107),TEXT(B107,\"0\"),B107),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B108<>\"\",VLOOKUP(IF(ISNUMBER(B108),TEXT(B108,\"0\"),B108),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B109<>\"\",VLOOKUP(IF(ISNUMBER(B109),TEXT(B109,\"0\"),B109),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B110<>\"\",VLOOKUP(IF(ISNUMBER(B110),TEXT(B110,\"0\"),B110),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B111<>\"\",VLOOKUP(IF(ISNUMBER(B111),TEXT(B111,\"0\"),B111),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B112<>\"\",VLOOKUP(IF(ISNUMBER(B112),TEXT(B112,\"0\"),B112),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B113<>\"\",VLOOKUP(IF(ISNUMBER(B113),TEXT(B113,\"0\"),B113),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B114<>\"\",VLOOKUP(IF(ISNUMBER(B114),TEXT(B114,\"0\"),B114),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B115<>\"\",VLOOKUP(IF(ISNUMBER(B115),TEXT(B115,\"0\"),B115),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B116<>\"\",VLOOKUP(IF(ISNUMBER(B116),TEXT(B116,\"0\"),B116),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B117<>\"\",VLOOKUP(IF(ISNUMBER(B117),TEXT(B117,\"0\"),B117),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B118<>\"\",VLOOKUP(IF(ISNUMBER(B118),TEXT(B118,\"0\"),B118),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B119<>\"\",VLOOKUP(IF(ISNUMBER(B119),TEXT(B119,\"0\"),B119),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B120<>\"\",VLOOKUP(IF(ISNUMBER(B120),TEXT(B120,\"0\"),B120),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B121<>\"\",VLOOKUP(IF(ISNUMBER(B121),TEXT(B121,\"0\"),B121),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B122<>\"\",VLOOKUP(IF(ISNUMBER(B122),TEXT(B122,\"0\"),B122),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B123<>\"\",VLOOKUP(IF(ISNUMBER(B123),TEXT(B123,\"0\"),B123),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B124<>\"\",VLOOKUP(IF(ISNUMBER(B124),TEXT(B124,\"0\"),B124),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B125<>\"\",VLOOKUP(IF(ISNUMBER(B125),TEXT(B125,\"0\"),B125),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B126<>\"\",VLOOKUP(IF(ISNUMBER(B126),TEXT(B126,\"0\"),B126),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B127<>\"\",VLOOKUP(IF(ISNUMBER(B127),TEXT(B127,\"0\"),B127),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B128<>\"\",VLOOKUP(IF(ISNUMBER(B128),TEXT(B128,\"0\"),B128),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B129<>\"\",VLOOKUP(IF(ISNUMBER(B129),TEXT(B129,\"0\"),B129),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B130<>\"\",VLOOKUP(IF(ISNUMBER(B130),TEXT(B130,\"0\"),B130),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B131<>\"\",VLOOKUP(IF(ISNUMBER(B131),TEXT(B131,\"0\"),B131),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B132<>\"\",VLOOKUP(IF(ISNUMBER(B132),TEXT(B132,\"0\"),B132),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B133<>\"\",VLOOKUP(IF(ISNUMBER(B133),TEXT(B133,\"0\"),B133),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B134<>\"\",VLOOKUP(IF(ISNUMBER(B134),TEXT(B134,\"0\"),B134),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B135<>\"\",VLOOKUP(IF(ISNUMBER(B135),TEXT(B135,\"0\"),B135),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B136<>\"\",VLOOKUP(IF(ISNUMBER(B136),TEXT(B136,\"0\"),B136),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B137<>\"\",VLOOKUP(IF(ISNUMBER(B137),TEXT(B137,\"0\"),B137),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B138<>\"\",VLOOKUP(IF(ISNUMBER(B138),TEXT(B138,\"0\"),B138),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B139<>\"\",VLOOKUP(IF(ISNUMBER(B139),TEXT(B139,\"0\"),B139),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
[{"$f":"IF(B140<>\"\",A139+1,\"\")","v":""},null,{"$f":"IF(A140<>\"\",1,\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(I140),TEXT(I140,\"0\"),I140),$BD$12:$BE$44,2,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",VLOOKUP(IF(ISNUMBER(B140),TEXT(B140,\"0\"),B140),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B140<>\"\",G140*(1-H140),\"\")","v":""},{"$f":"IF(B140<>\"\",C140*(1-H140)*G140,\"\")","v":""},null,null,null,null,{"$f":"IF(B140<>\"\",$K$2,\"\")","v":""},"","",{"$f":"IF(R140=\"\",\"\",C140)","v":""}]
["",null,"",{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B141<>\"\",VLOOKUP(IF(ISNUMBER(B141),TEXT(B141,\"0\"),B141),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","",{"$f":"IF(B141>1,B141,\"\")","v":""},""]
["",null,"",{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B142<>\"\",VLOOKUP(IF(ISNUMBER(B142),TEXT(B142,\"0\"),B142),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B143<>\"\",VLOOKUP(IF(ISNUMBER(B143),TEXT(B143,\"0\"),B143),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B144<>\"\",VLOOKUP(IF(ISNUMBER(B144),TEXT(B144,\"0\"),B144),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B145<>\"\",VLOOKUP(IF(ISNUMBER(B145),TEXT(B145,\"0\"),B145),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B146<>\"\",VLOOKUP(IF(ISNUMBER(B146),TEXT(B146,\"0\"),B146),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B147<>\"\",VLOOKUP(IF(ISNUMBER(B147),TEXT(B147,\"0\"),B147),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B148<>\"\",VLOOKUP(IF(ISNUMBER(B148),TEXT(B148,\"0\"),B148),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B149<>\"\",VLOOKUP(IF(ISNUMBER(B149),TEXT(B149,\"0\"),B149),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B150<>\"\",VLOOKUP(IF(ISNUMBER(B150),TEXT(B150,\"0\"),B150),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B151<>\"\",VLOOKUP(IF(ISNUMBER(B151),TEXT(B151,\"0\"),B151),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B152<>\"\",VLOOKUP(IF(ISNUMBER(B152),TEXT(B152,\"0\"),B152),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B153<>\"\",VLOOKUP(IF(ISNUMBER(B153),TEXT(B153,\"0\"),B153),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B154<>\"\",VLOOKUP(IF(ISNUMBER(B154),TEXT(B154,\"0\"),B154),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B155<>\"\",VLOOKUP(IF(ISNUMBER(B155),TEXT(B155,\"0\"),B155),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B156<>\"\",VLOOKUP(IF(ISNUMBER(B156),TEXT(B156,\"0\"),B156),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B157<>\"\",VLOOKUP(IF(ISNUMBER(B157),TEXT(B157,\"0\"),B157),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B158<>\"\",VLOOKUP(IF(ISNUMBER(B158),TEXT(B158,\"0\"),B158),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B159<>\"\",VLOOKUP(IF(ISNUMBER(B159),TEXT(B159,\"0\"),B159),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B160<>\"\",VLOOKUP(IF(ISNUMBER(B160),TEXT(B160,\"0\"),B160),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B161<>\"\",VLOOKUP(IF(ISNUMBER(B161),TEXT(B161,\"0\"),B161),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B162<>\"\",VLOOKUP(IF(ISNUMBER(B162),TEXT(B162,\"0\"),B162),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B163<>\"\",VLOOKUP(IF(ISNUMBER(B163),TEXT(B163,\"0\"),B163),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B164<>\"\",VLOOKUP(IF(ISNUMBER(B164),TEXT(B164,\"0\"),B164),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B165<>\"\",VLOOKUP(IF(ISNUMBER(B165),TEXT(B165,\"0\"),B165),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B166<>\"\",VLOOKUP(IF(ISNUMBER(B166),TEXT(B166,\"0\"),B166),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B167<>\"\",VLOOKUP(IF(ISNUMBER(B167),TEXT(B167,\"0\"),B167),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B168<>\"\",VLOOKUP(IF(ISNUMBER(B168),TEXT(B168,\"0\"),B168),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B169<>\"\",VLOOKUP(IF(ISNUMBER(B169),TEXT(B169,\"0\"),B169),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B170<>\"\",VLOOKUP(IF(ISNUMBER(B170),TEXT(B170,\"0\"),B170),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B171<>\"\",VLOOKUP(IF(ISNUMBER(B171),TEXT(B171,\"0\"),B171),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B172<>\"\",VLOOKUP(IF(ISNUMBER(B172),TEXT(B172,\"0\"),B172),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B173<>\"\",VLOOKUP(IF(ISNUMBER(B173),TEXT(B173,\"0\"),B173),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B174<>\"\",VLOOKUP(IF(ISNUMBER(B174),TEXT(B174,\"0\"),B174),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B175<>\"\",VLOOKUP(IF(ISNUMBER(B175),TEXT(B175,\"0\"),B175),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B176<>\"\",VLOOKUP(IF(ISNUMBER(B176),TEXT(B176,\"0\"),B176),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B177<>\"\",VLOOKUP(IF(ISNUMBER(B177),TEXT(B177,\"0\"),B177),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B178<>\"\",VLOOKUP(IF(ISNUMBER(B178),TEXT(B178,\"0\"),B178),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B179<>\"\",VLOOKUP(IF(ISNUMBER(B179),TEXT(B179,\"0\"),B179),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B180<>\"\",VLOOKUP(IF(ISNUMBER(B180),TEXT(B180,\"0\"),B180),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B181<>\"\",VLOOKUP(IF(ISNUMBER(B181),TEXT(B181,\"0\"),B181),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B182<>\"\",VLOOKUP(IF(ISNUMBER(B182),TEXT(B182,\"0\"),B182),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B183<>\"\",VLOOKUP(IF(ISNUMBER(B183),TEXT(B183,\"0\"),B183),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B184<>\"\",VLOOKUP(IF(ISNUMBER(B184),TEXT(B184,\"0\"),B184),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B185<>\"\",VLOOKUP(IF(ISNUMBER(B185),TEXT(B185,\"0\"),B185),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B186<>\"\",VLOOKUP(IF(ISNUMBER(B186),TEXT(B186,\"0\"),B186),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B187<>\"\",VLOOKUP(IF(ISNUMBER(B187),TEXT(B187,\"0\"),B187),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B188<>\"\",VLOOKUP(IF(ISNUMBER(B188),TEXT(B188,\"0\"),B188),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B189<>\"\",VLOOKUP(IF(ISNUMBER(B189),TEXT(B189,\"0\"),B189),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B190<>\"\",VLOOKUP(IF(ISNUMBER(B190),TEXT(B190,\"0\"),B190),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B191<>\"\",VLOOKUP(IF(ISNUMBER(B191),TEXT(B191,\"0\"),B191),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B192<>\"\",VLOOKUP(IF(ISNUMBER(B192),TEXT(B192,\"0\"),B192),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B193<>\"\",VLOOKUP(IF(ISNUMBER(B193),TEXT(B193,\"0\"),B193),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B194<>\"\",VLOOKUP(IF(ISNUMBER(B194),TEXT(B194,\"0\"),B194),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B195<>\"\",VLOOKUP(IF(ISNUMBER(B195),TEXT(B195,\"0\"),B195),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B196<>\"\",VLOOKUP(IF(ISNUMBER(B196),TEXT(B196,\"0\"),B196),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B197<>\"\",VLOOKUP(IF(ISNUMBER(B197),TEXT(B197,\"0\"),B197),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B198<>\"\",VLOOKUP(IF(ISNUMBER(B198),TEXT(B198,\"0\"),B198),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B199<>\"\",VLOOKUP(IF(ISNUMBER(B199),TEXT(B199,\"0\"),B199),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B200<>\"\",VLOOKUP(IF(ISNUMBER(B200),TEXT(B200,\"0\"),B200),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B201<>\"\",VLOOKUP(IF(ISNUMBER(B201),TEXT(B201,\"0\"),B201),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B202<>\"\",VLOOKUP(IF(ISNUMBER(B202),TEXT(B202,\"0\"),B202),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B203<>\"\",VLOOKUP(IF(ISNUMBER(B203),TEXT(B203,\"0\"),B203),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
[{"$f":"IF(B204<>\"\",A203+1,\"\")","v":""},null,{"$f":"IF(A204<>\"\",1,\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(I204),TEXT(I204,\"0\"),I204),$BD$12:$BE$44,2,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",VLOOKUP(IF(ISNUMBER(B204),TEXT(B204,\"0\"),B204),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B204<>\"\",G204*(1-H204),\"\")","v":""},{"$f":"IF(B204<>\"\",C204*(1-H204)*G204,\"\")","v":""},null,null,null,null,{"$f":"IF(B204<>\"\",$K$2,\"\")","v":""},"","",{"$f":"IF(R204=\"\",\"\",C204)","v":""}]
["",null,"",{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B205<>\"\",VLOOKUP(IF(ISNUMBER(B205),TEXT(B205,\"0\"),B205),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","",{"$f":"IF(B205>1,B205,\"\")","v":""},""]
["",null,"",{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B206<>\"\",VLOOKUP(IF(ISNUMBER(B206),TEXT(B206,\"0\"),B206),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B207<>\"\",VLOOKUP(IF(ISNUMBER(B207),TEXT(B207,\"0\"),B207),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B208<>\"\",VLOOKUP(IF(ISNUMBER(B208),TEXT(B208,\"0\"),B208),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B209<>\"\",VLOOKUP(IF(ISNUMBER(B209),TEXT(B209,\"0\"),B209),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B210<>\"\",VLOOKUP(IF(ISNUMBER(B210),TEXT(B210,\"0\"),B210),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B211<>\"\",VLOOKUP(IF(ISNUMBER(B211),TEXT(B211,\"0\"),B211),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B212<>\"\",VLOOKUP(IF(ISNUMBER(B212),TEXT(B212,\"0\"),B212),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B213<>\"\",VLOOKUP(IF(ISNUMBER(B213),TEXT(B213,\"0\"),B213),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B214<>\"\",VLOOKUP(IF(ISNUMBER(B214),TEXT(B214,\"0\"),B214),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B215<>\"\",VLOOKUP(IF(ISNUMBER(B215),TEXT(B215,\"0\"),B215),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B216<>\"\",VLOOKUP(IF(ISNUMBER(B216),TEXT(B216,\"0\"),B216),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B217<>\"\",VLOOKUP(IF(ISNUMBER(B217),TEXT(B217,\"0\"),B217),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B218<>\"\",VLOOKUP(IF(ISNUMBER(B218),TEXT(B218,\"0\"),B218),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B219<>\"\",VLOOKUP(IF(ISNUMBER(B219),TEXT(B219,\"0\"),B219),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B220<>\"\",VLOOKUP(IF(ISNUMBER(B220),TEXT(B220,\"0\"),B220),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B221<>\"\",VLOOKUP(IF(ISNUMBER(B221),TEXT(B221,\"0\"),B221),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B222<>\"\",VLOOKUP(IF(ISNUMBER(B222),TEXT(B222,\"0\"),B222),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B223<>\"\",VLOOKUP(IF(ISNUMBER(B223),TEXT(B223,\"0\"),B223),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B224<>\"\",VLOOKUP(IF(ISNUMBER(B224),TEXT(B224,\"0\"),B224),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B225<>\"\",VLOOKUP(IF(ISNUMBER(B225),TEXT(B225,\"0\"),B225),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B226<>\"\",VLOOKUP(IF(ISNUMBER(B226),TEXT(B226,\"0\"),B226),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B227<>\"\",VLOOKUP(IF(ISNUMBER(B227),TEXT(B227,\"0\"),B227),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B228<>\"\",VLOOKUP(IF(ISNUMBER(B228),TEXT(B228,\"0\"),B228),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B229<>\"\",VLOOKUP(IF(ISNUMBER(B229),TEXT(B229,\"0\"),B229),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B230<>\"\",VLOOKUP(IF(ISNUMBER(B230),TEXT(B230,\"0\"),B230),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B231<>\"\",VLOOKUP(IF(ISNUMBER(B231),TEXT(B231,\"0\"),B231),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B232<>\"\",VLOOKUP(IF(ISNUMBER(B232),TEXT(B232,\"0\"),B232),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B233<>\"\",VLOOKUP(IF(ISNUMBER(B233),TEXT(B233,\"0\"),B233),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B234<>\"\",VLOOKUP(IF(ISNUMBER(B234),TEXT(B234,\"0\"),B234),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B235<>\"\",VLOOKUP(IF(ISNUMBER(B235),TEXT(B235,\"0\"),B235),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B236<>\"\",VLOOKUP(IF(ISNUMBER(B236),TEXT(B236,\"0\"),B236),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B237<>\"\",VLOOKUP(IF(ISNUMBER(B237),TEXT(B237,\"0\"),B237),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B238<>\"\",VLOOKUP(IF(ISNUMBER(B238),TEXT(B238,\"0\"),B238),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B239<>\"\",VLOOKUP(IF(ISNUMBER(B239),TEXT(B239,\"0\"),B239),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B240<>\"\",VLOOKUP(IF(ISNUMBER(B240),TEXT(B240,\"0\"),B240),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B241<>\"\",VLOOKUP(IF(ISNUMBER(B241),TEXT(B241,\"0\"),B241),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B242<>\"\",VLOOKUP(IF(ISNUMBER(B242),TEXT(B242,\"0\"),B242),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B243<>\"\",VLOOKUP(IF(ISNUMBER(B243),TEXT(B243,\"0\"),B243),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B244<>\"\",VLOOKUP(IF(ISNUMBER(B244),TEXT(B244,\"0\"),B244),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B245<>\"\",VLOOKUP(IF(ISNUMBER(B245),TEXT(B245,\"0\"),B245),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B246<>\"\",VLOOKUP(IF(ISNUMBER(B246),TEXT(B246,\"0\"),B246),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B247<>\"\",VLOOKUP(IF(ISNUMBER(B247),TEXT(B247,\"0\"),B247),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B248<>\"\",VLOOKUP(IF(ISNUMBER(B248),TEXT(B248,\"0\"),B248),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B249<>\"\",VLOOKUP(IF(ISNUMBER(B249),TEXT(B249,\"0\"),B249),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B250<>\"\",VLOOKUP(IF(ISNUMBER(B250),TEXT(B250,\"0\"),B250),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B251<>\"\",VLOOKUP(IF(ISNUMBER(B251),TEXT(B251,\"0\"),B251),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B252<>\"\",VLOOKUP(IF(ISNUMBER(B252),TEXT(B252,\"0\"),B252),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B253<>\"\",VLOOKUP(IF(ISNUMBER(B253),TEXT(B253,\"0\"),B253),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B254<>\"\",VLOOKUP(IF(ISNUMBER(B254),TEXT(B254,\"0\"),B254),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B255<>\"\",VLOOKUP(IF(ISNUMBER(B255),TEXT(B255,\"0\"),B255),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B256<>\"\",VLOOKUP(IF(ISNUMBER(B256),TEXT(B256,\"0\"),B256),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B257<>\"\",VLOOKUP(IF(ISNUMBER(B257),TEXT(B257,\"0\"),B257),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B258<>\"\",VLOOKUP(IF(ISNUMBER(B258),TEXT(B258,\"0\"),B258),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B259<>\"\",VLOOKUP(IF(ISNUMBER(B259),TEXT(B259,\"0\"),B259),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B260<>\"\",VLOOKUP(IF(ISNUMBER(B260),TEXT(B260,\"0\"),B260),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B261<>\"\",VLOOKUP(IF(ISNUMBER(B261),TEXT(B261,\"0\"),B261),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B262<>\"\",VLOOKUP(IF(ISNUMBER(B262),TEXT(B262,\"0\"),B262),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B263<>\"\",VLOOKUP(IF(ISNUMBER(B263),TEXT(B263,\"0\"),B263),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B264<>\"\",VLOOKUP(IF(ISNUMBER(B264),TEXT(B264,\"0\"),B264),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B265<>\"\",VLOOKUP(IF(ISNUMBER(B265),TEXT(B265,\"0\"),B265),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B266<>\"\",VLOOKUP(IF(ISNUMBER(B266),TEXT(B266,\"0\"),B266),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B267<>\"\",VLOOKUP(IF(ISNUMBER(B267),TEXT(B267,\"0\"),B267),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
[{"$f":"IF(B268<>\"\",A267+1,\"\")","v":""},null,{"$f":"IF(A268<>\"\",1,\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(I268),TEXT(I268,\"0\"),I268),$BD$12:$BE$44,2,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",VLOOKUP(IF(ISNUMBER(B268),TEXT(B268,\"0\"),B268),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B268<>\"\",G268*(1-H268),\"\")","v":""},{"$f":"IF(B268<>\"\",C268*(1-H268)*G268,\"\")","v":""},null,null,null,null,{"$f":"IF(B268<>\"\",$K$2,\"\")","v":""},"","",{"$f":"IF(R268=\"\",\"\",C268)","v":""}]
["",null,"",{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B269<>\"\",VLOOKUP(IF(ISNUMBER(B269),TEXT(B269,\"0\"),B269),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","",{"$f":"IF(B269>1,B269,\"\")","v":""},""]
["",null,"",{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B270<>\"\",VLOOKUP(IF(ISNUMBER(B270),TEXT(B270,\"0\"),B270),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B271<>\"\",VLOOKUP(IF(ISNUMBER(B271),TEXT(B271,\"0\"),B271),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B272<>\"\",VLOOKUP(IF(ISNUMBER(B272),TEXT(B272,\"0\"),B272),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B273<>\"\",VLOOKUP(IF(ISNUMBER(B273),TEXT(B273,\"0\"),B273),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B274<>\"\",VLOOKUP(IF(ISNUMBER(B274),TEXT(B274,\"0\"),B274),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B275<>\"\",VLOOKUP(IF(ISNUMBER(B275),TEXT(B275,\"0\"),B275),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B276<>\"\",VLOOKUP(IF(ISNUMBER(B276),TEXT(B276,\"0\"),B276),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B277<>\"\",VLOOKUP(IF(ISNUMBER(B277),TEXT(B277,\"0\"),B277),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B278<>\"\",VLOOKUP(IF(ISNUMBER(B278),TEXT(B278,\"0\"),B278),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B279<>\"\",VLOOKUP(IF(ISNUMBER(B279),TEXT(B279,\"0\"),B279),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B280<>\"\",VLOOKUP(IF(ISNUMBER(B280),TEXT(B280,\"0\"),B280),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B281<>\"\",VLOOKUP(IF(ISNUMBER(B281),TEXT(B281,\"0\"),B281),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B282<>\"\",VLOOKUP(IF(ISNUMBER(B282),TEXT(B282,\"0\"),B282),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B283<>\"\",VLOOKUP(IF(ISNUMBER(B283),TEXT(B283,\"0\"),B283),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B284<>\"\",VLOOKUP(IF(ISNUMBER(B284),TEXT(B284,\"0\"),B284),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B285<>\"\",VLOOKUP(IF(ISNUMBER(B285),TEXT(B285,\"0\"),B285),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B286<>\"\",VLOOKUP(IF(ISNUMBER(B286),TEXT(B286,\"0\"),B286),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B287<>\"\",VLOOKUP(IF(ISNUMBER(B287),TEXT(B287,\"0\"),B287),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B288<>\"\",VLOOKUP(IF(ISNUMBER(B288),TEXT(B288,\"0\"),B288),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B289<>\"\",VLOOKUP(IF(ISNUMBER(B289),TEXT(B289,\"0\"),B289),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B290<>\"\",VLOOKUP(IF(ISNUMBER(B290),TEXT(B290,\"0\"),B290),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B291<>\"\",VLOOKUP(IF(ISNUMBER(B291),TEXT(B291,\"0\"),B291),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B292<>\"\",VLOOKUP(IF(ISNUMBER(B292),TEXT(B292,\"0\"),B292),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B293<>\"\",VLOOKUP(IF(ISNUMBER(B293),TEXT(B293,\"0\"),B293),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B294<>\"\",VLOOKUP(IF(ISNUMBER(B294),TEXT(B294,\"0\"),B294),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B295<>\"\",VLOOKUP(IF(ISNUMBER(B295),TEXT(B295,\"0\"),B295),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B296<>\"\",VLOOKUP(IF(ISNUMBER(B296),TEXT(B296,\"0\"),B296),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B297<>\"\",VLOOKUP(IF(ISNUMBER(B297),TEXT(B297,\"0\"),B297),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B298<>\"\",VLOOKUP(IF(ISNUMBER(B298),TEXT(B298,\"0\"),B298),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B299<>\"\",VLOOKUP(IF(ISNUMBER(B299),TEXT(B299,\"0\"),B299),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
["",null,"",{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B300<>\"\",VLOOKUP(IF(ISNUMBER(B300),TEXT(B300,\"0\"),B300),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"","","",""]
[{"$f":"IF(B301<>\"\",A300+1,\"\")","v":""},null,{"$f":"IF(A301<>\"\",1,\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(I301),TEXT(I301,\"0\"),I301),$BD$12:$BE$44,2,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",VLOOKUP(IF(ISNUMBER(B301),TEXT(B301,\"0\"),B301),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},{"$f":"IF(B301<>\"\",G301*(1-H301),\"\")","v":""},{"$f":"IF(B301<>\"\",C301*(1-H301)*G301,\"\")","v":""},null,null,null,null,"",null,"",""]
[{"$f":"IF(B302<>\"\",A301+1,\"\")","v":""},"",{"$f":"IF(A302<>\"\",1,\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B302<>\"\",VLOOKUP(IF(ISNUMBER(B302),TEXT(B302,\"0\"),B302),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
[{"$f":"IF(B303<>\"\",A302+1,\"\")","v":""},"",{"$f":"IF(A303<>\"\",1,\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B303<>\"\",VLOOKUP(IF(ISNUMBER(B303),TEXT(B303,\"0\"),B303),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
[{"$f":"IF(B304<>\"\",A303+1,\"\")","v":""},"",{"$f":"IF(A304<>\"\",1,\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B304<>\"\",VLOOKUP(IF(ISNUMBER(B304),TEXT(B304,\"0\"),B304),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
[{"$f":"IF(B305<>\"\",A304+1,\"\")","v":""},"",{"$f":"IF(A305<>\"\",1,\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$4:$I$52318,6,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B305<>\"\",VLOOKUP(IF(ISNUMBER(B305),TEXT(B305,\"0\"),B305),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"","",null,null,null,null,"",null,"",""]
[null,null,null,null,{"$f":"IF(B306<>\"\",VLOOKUP(IF(ISNUMBER(B306),TEXT(B306,\"0\"),B306),Cennik!$A$3:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(B306<>\"\",VLOOKUP(IF(ISNUMBER(B306),TEXT(B306,\"0\"),B306),Cennik!$A$4:$K$52318,5,FALSE),\"\")","v":""},{"$f":"IF(B306<>\"\",VLOOKUP(IF(ISNUMBER(B306),TEXT(B306,\"0\"),B306),Cennik!$A$3:$K$52318,3,FALSE),\"\")","v":""},"",{"$f":"IF(B306<>\"\",VLOOKUP(IF(ISNUMBER(B306),TEXT(B306,\"0\"),B306),Cennik!$A$3:$F$52318,4,FALSE),\"\")","v":""},"",""]
[null,null,null,null,null,null,null,""]

{"sheet":"Zestawienie","index":4,"n_rows":305,"n_cols":19,"rows_kept":305,"cut":false,"hidden":false,"merged":[[8,9,8,10]]}
[null,null,null,null,"",null,null,1500,null,"Data:","2023-12-05"]
[null,null,null,null,null,null,null,null,null,"Dla:","ZZ01"]
[]
[]
[]
[]
[null,null,null,null,"Cennik 03-2023","Warunki płatności: "]
[null,null,"Dostawa: ",null,{"$error":"#N/A"}]
[null,null,null,null,"Wpisz nazwę zestawienia",null,null,null,"Wartość",{"$error":"#N/A"}]
["L.p","Numer","Szt.","Pak.","Opis","Data","Cena za szt.","Upust","Grupa","Cena za szt.","Wartość"]
[null,"katalogowy",null,"po",null,"ceny","katalogowa",null,"upustu","po upuście","netto",null,null,null,"12_5_Wpisz nazwę",null,null,"Wartość",{"$error":"#N/A"}]
[1,30043,2,0.1,"ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D400","1900-01-01T09:21:36",139,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,30043,2,"ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D400"]
[2,30065,2,0.05,"ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650","05:45:36",164,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,30065,2,"ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650"]
[3,31465,2,0.14000000000000001,"ZENERGY - POKRYWA GÓRNA IP30, W650, D400","23:31:12",188,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,31465,2,"ZENERGY - POKRYWA GÓRNA IP30, W650, D400"]
[4,80365,2,0.19,"ZENERGY - DRZWI PEŁNE IP30, H2000 X W650","1900-01-01T06:57:36",883,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,80365,2,"ZENERGY - DRZWI PEŁNE IP30, H2000 X W650"]
[5,80965,2,0.05,"ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W650 + WSPORNIKI,  ( 1850 X 550 )","01:26:24",690,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,80965,2,"ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W650 + WSPORNIKI,  ( 1850 X 550 )"]
[6,81265,2,0.17,"ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W650","1900-01-01T02:09:36",501,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,81265,2,"ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W650"]
[7,84065,2,0.45,"ZENERGY - RAMA, H2000 X D400 X W650","09:07:12",810,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,84065,2,"ZENERGY - RAMA, H2000 X D400 X W650"]
[8,89340,2,0.23,"ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D400","1900-01-01T06:00:00",625,{"$error":"#N/A"},"ZENE/01",{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ZZ01",null,89340,2,"ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D400"]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","","",null,null,"",null,"","",""]
["","","","","","","","","","",""]
["","","","","","","","","","",""]
[null,"","","","","","","","","",""]
[null,"","","","","","","","","",""]
[null,"","","","","","","","","",""]

{"sheet":"Zbaza","index":5,"n_rows":430,"n_cols":162,"rows_kept":430,"cut":false,"hidden":false,"merged":[[117,116,121,116],[117,117,121,117],[117,118,121,118],[117,119,121,119],[117,128,121,128],[78,118,82,118],[78,119,82,119],[78,120,82,120],[78,121,82,121],[78,122,82,122],[78,127,82,127],[78,128,82,128],[117,126,121,126],[117,127,121,127],[117,120,121,120],[117,121,121,121],[117,122,121,122],[117,123,121,123],[117,124,121,124],[117,125,121,125],[132,155,133,155],[106,155,107,155],[132,148,132,151],[328,9,329,9],[158,147,159,147],[220,1,221,1],[193,1,194,1],[328,2,328,7],[328,1,329,1],[254,17,255,17],[257,82,257,83],[177,17,178,17],[202,17,203,17],[200,9,201,9],[168,9,169,9],[152,9,153,9],[280,18,280,21],[118,113,121,113],[117,129,121,129],[117,130,121,130],[184,147,185,147],[184,155,185,155],[117,114,121,114],[117,115,121,115],[354,2,354,7],[380,1,381,1],[380,2,380,7],[371,17,372,17],[371,18,371,22],[354,1,355,1],[354,10,354,13],[332,18,332,22],[106,147,107,147],[184,9,185,9],[276,1,277,1],[276,2,276,7],[224,10,224,13],[192,10,192,14],[224,9,225,9],[139,1,140,1],[166,1,167,1],[168,10,168,14],[176,10,176,14],[200,10,200,14],[208,9,209,9],[208,10,208,14],[247,1,248,1],[152,17,153,17],[132,156,132,159],[54,155,55,155],[132,147,133,147],[71,40,71,45],[79,40,79,45],[69,40,69,45],[106,156,106,159],[2,155,3,155],[80,155,81,155],[2,148,2,151],[28,148,28,151],[106,148,106,151],[80,156,80,159],[80,148,80,151],[2,156,2,159],[28,155,29,155],[28,156,28,159],[85,40,85,45],[4,113,5,113],[31,40,31,43],[54,147,55,147],[81,40,81,45],[72,40,72,45],[5,40,5,43],[80,147,81,147],[4,114,4,119],[107,93,107,97],[99,40,99,43],[4,67,4,68],[106,93,106,97],[73,93,73,97],[74,93,74,97],[57,93,57,97],[58,93,58,97],[4,52,4,53],[4,40,4,43],[78,115,82,115],[78,114,82,114],[79,113,82,113],[78,129,82,129],[78,123,82,123],[78,124,82,124],[78,125,82,125],[78,126,82,126],[80,40,80,45],[78,130,82,130],[78,116,82,116],[78,117,82,117],[2,9,3,9],[72,17,73,17],[4,55,4,56],[4,58,4,59],[13,53,13,54],[17,40,17,43],[70,40,70,45],[34,9,35,9],[27,9,28,9],[67,40,67,45],[6,40,6,43],[2,140,2,141],[4,130,5,130],[4,131,4,136],[28,147,29,147],[2,147,3,147],[302,1,303,1],[2,1,3,1],[160,10,160,14],[276,10,276,13],[302,10,302,13],[276,9,277,9],[302,2,302,7],[257,79,257,80],[302,9,303,9],[127,9,128,9],[83,40,83,45],[228,18,228,21],[254,18,254,21],[176,9,177,9],[152,10,152,14],[250,9,251,9],[228,17,229,17],[250,10,250,13],[184,10,184,14],[29,1,30,1],[56,1,57,1],[74,9,75,9],[74,10,74,15],[48,9,49,9],[7,40,7,43],[8,40,8,43],[9,40,9,43],[59,40,59,43],[52,40,52,43],[38,40,38,43],[45,40,45,43],[10,40,10,43],[24,40,24,43],[66,40,66,45],[22,17,23,17],[83,1,84,1],[68,40,68,45],[48,10,48,15],[47,17,48,17],[41,9,42,9],[84,40,84,45],[82,40,82,45],[92,40,92,44],[127,17,128,17],[127,10,127,14],[110,1,111,1],[97,17,98,17],[380,9,381,9],[380,10,380,13],[354,9,355,9],[406,9,407,9],[406,10,406,13],[328,10,328,13],[306,18,306,21],[280,17,281,17],[306,17,307,17],[332,17,333,17]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Zenergy-OE'!AA9","v":"Wpisz nazwę"},{"$f":"CONCATENATE(T2,R14,S16,R14,T16,R14,U3,U4,U5,U6,U7,U8,U9,U10,U11,U12)","v":"PROJEKT___1"},null,{"$f":"IF(BA13>10,2,1)","v":1},"Pole 1",null,null,3,{"$f":"IF(AB1=1,AB1,AB1-1)","v":2},"Pole 2",null,null,1,{"$f":"IF(AG1=1,AG1,AG1-1)","v":1},"Pole 3",null,null,1,{"$f":"IF(AL1=1,AL1,AL1-1)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zest. szyn TS35",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE6=14,23,IF(CP35=1,$BA$15,CB6))","v":1},null,null,{"$f":"IF(CP35=1,BD4,CE6)","v":1},null,null,null,null,null,null,null,"+5",null,null,null,{"$f":"SUM(CQ2:CQ23)","v":5},{"$f":"IF(CR25>0,CR25,CR24)","v":11},{"$f":"SUM(CS2:CS17)","v":11},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"PROJEKT",{"$f":"CONCATENATE(S16,R14,T16,R14,U1)","v":"__Wpisz nazwę"},null,null,null,{"$f":"IF('Zenergy-OE'!AF18=\"\",1,0)","v":0},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BM4<6,1,0)","v":1},{"$f":"Z2+AA2-Y2","v":2},null,{"$f":"IF('Zenergy-OE'!AN18=\"\",1,0)","v":1},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BM5<6,1,0)","v":0},{"$f":"AE2+AF2-AD2","v":-1},null,{"$f":"IF('Zenergy-OE'!AV18=\"\",1,0)","v":1},{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BM6<6,1,0)","v":0},{"$f":"AJ2+AK2-AI2","v":-1},null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE5=14,25,IF(CO35=1,$BA$12,CB5))","v":1},null,null,{"$f":"IF(CO35=1,BD4,CE5)","v":1},null,null,null,null,null,null,null,"+4","Brak",1,null,{"$f":"IF(BA13=1,11,0)","v":0},{"$f":"IF(BA12=1,11,0)","v":11},{"$f":"IF(BA15=1,11,0)","v":11},1]
[null,"Szerokość obudowy","Drzwi pełne IP30   Wysokość",null,null,1,null,"Pole 1,3",null,"Szerokość obudowy","Pusty arkusz - formuły !!!!   Wysokość",null,null,10,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 1\",\"Project 1\")","v":"PROJEKT 1"},null,{"$f":"IF($R$2=1,\"1\",\"\")","v":"1"},null,null,null,{"$f":"IF('Zenergy-OE'!AF15=\"\",1,0)","v":0},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BJ4>1,1,0)","v":1},{"$f":"Z3+AA3-Y3","v":2},null,{"$f":"IF('Zenergy-OE'!AN15=\"\",1,0)","v":1},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BJ5>1,1,0)","v":0},{"$f":"AE3+AF3-AD3","v":-1},null,{"$f":"IF('Zenergy-OE'!AV15=\"\",1,0)","v":1},{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BJ6>1,1,0)","v":0},{"$f":"AJ3+AK3-AI3","v":-1},null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE4=14,23,IF(CN35=1,$BA$13,CB4))","v":6},null,null,{"$f":"IF(CN35=1,BD4,CE4)","v":5},null,null,null,null,null,null,null,"+3",300,2,null,{"$f":"IF(BA13=2,1,0)","v":0},{"$f":"IF(BA12=2,1,0)","v":0},{"$f":"IF(BA15=2,1,0)","v":0},2,null,"W 300 - 1","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLa",null,null,null,null,null,null,"Szerokość obudowy","Rama osłon czołowych na zawiasach  Wysokość, Pole 1,3",null,null,null,2,null,null,"Szerokość obudowy","Rama osłon czołowych na zawiasach  Wysokość, Pole 2",null,null,null,2]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 2\",\"Project 2\")","v":"PROJEKT 2"},null,{"$f":"IF($R$2=2,\"2\",\"\")","v":""},null,null,null,{"$f":"IF('Zenergy-OE'!AF21=\"\",1,0)","v":0},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BS4>1,1,0)","v":1},{"$f":"Z4+AA4-Y4","v":2},null,{"$f":"IF('Zenergy-OE'!AN21=\"\",1,0)","v":1},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BS5>1,1,0)","v":0},{"$f":"AE4+AF4-AD4","v":-1},null,{"$f":"IF('Zenergy-OE'!AV21=\"\",1,0)","v":1},{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BS6>1,1,0)","v":0},{"$f":"AJ4+AK4-AI4","v":-1},null,null,null,null,null,null,null,null,null,null,null,null,null,3,1,7,null,5,8,null,3,9,null,2,10,null,2,11,null,1,12,null,2,13,null,1,14,null,1,15,null,1,1,null,13,1,null,1,1,null,null,null,"+2",400,3,null,{"$f":"IF(BA13=3,2,0)","v":0},{"$f":"IF(BA12=3,2,0)","v":0},{"$f":"IF(BA15=3,2,0)","v":0},3,null,"Brak",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ref","Ilość",null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
["Brak","Brak",{"$f":"IF(C4=0,\"\",\"\")","v":""},"","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 3\",\"Project 3\")","v":"PROJEKT 3"},null,{"$f":"IF($R$2=3,\"3\",\"\")","v":""},null,null,null,{"$f":"IF('Zenergy-OE'!AF24=\"\",1,0)","v":1},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BV4>1,1,0)","v":0},{"$f":"Z5+AA5-Y5","v":0},null,{"$f":"IF('Zenergy-OE'!AN24=\"\",1,0)","v":1},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BW5>1,1,0)","v":1},{"$f":"IF(AK23=2,2,AE5+AF5-AD5)","v":0},null,{"$f":"IF('Zenergy-OE'!AV24=\"\",1,0)","v":1},{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BV6>1,1,0)","v":0},{"$f":"AJ5+AK5-AI5","v":-1},null,{"$f":"INDEX(($AO$13:$AR$15),$BA$4,$BS4)","v":2},"Pokrywa górna pole 1",null,null,null,null,null,null,null,null,null,null,4,"Stopień IP",null,null,"Wysokość",null,null,"Głębokość",null,null,1,"Drzwi",null,6,"Drzwi / plecy",null,"Cokół",null,null,1,"Pokrywa górna",null,1,"R. osłon front",null,1,"R. osłon tył",null,1,"Osłony",null,1,"Ilość mod.",null,1,"Akc.szerokość",null,null,null,"+1",450,4,null,{"$f":"IF(BA13=4,3,0)","v":0},{"$f":"IF(BA12=4,3,0)","v":0},{"$f":"IF(BA15=4,3,0)","v":0},4,null,"Osłona pełna",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Akcesoria","Głębokość obudowy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Akcesoria","Głębokość obudowy",null,null,null,null,null,null,null,"Pole 1",{"$f":"IF('Zenergy-OE'!AF12=\"\",0,IF('Zenergy-OE'!AF12>0,'Zenergy-OE'!AF12,0))","v":84065},{"$f":"IF('Zenergy-OE'!AH12=\"\",0,'Zenergy-OE'!AH12)","v":2},{"$f":"IF(EK5>1,VLOOKUP(IF(ISNUMBER(EK5),TEXT(EK5,\"0\"),EK5),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - RAMA, H2000 X D400 X W650"},{"$f":"IF(EK5>1,VLOOKUP(IF(ISNUMBER(EK5),TEXT(EK5,\"0\"),EK5),Cennik!$A$4:$F$52318,3,FALSE),0)","v":874.8},{"$f":"EL5*EN5","v":1749.6},null,"Brak","Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[400,300,40330,50330,60330,70330,80330,90330,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 4\",\"Project 4\")","v":"PROJEKT 4"},null,{"$f":"IF($R$2=4,\"4\",\"\")","v":""},null,null,null,{"$f":"IF('Zenergy-OE'!AF28=\"\",1,0)","v":1},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BY4>1,1,0)","v":0},{"$f":"Z6+AA6-Y6","v":0},null,{"$f":"IF('Zenergy-OE'!AN28=\"\",1,0)","v":1},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BZ5>1,1,0)","v":1},{"$f":"IF(AK23=2,2,AE6+AF6-AD6)","v":0},null,{"$f":"IF('Zenergy-OE'!AV28=\"\",1,0)","v":1},{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BY6>1,1,0)","v":0},{"$f":"AJ6+AK6-AI6","v":-1},null,{"$f":"INDEX(($AO$13:$AR$15),$BA$4,$BS5)","v":5},"Pokrywa górna pole 2",null,null,null,null,null,null,null,null,null,null,5,1,30,null,1,1200,null,1,230,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,6,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Plecy z wentylacją\",\"Vented back cover\")","v":"Plecy z wentylacją"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak - przedział kablowy\",\"None - cables\")","v":"Brak - przedział kablowy"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak - przedział kablowy\",\"None - cables\")","v":"Brak - przedział kablowy"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,null,null,0,600,5,null,{"$f":"IF(BA13=5,4,0)","v":0},{"$f":"IF(BA12=5,4,0)","v":0},{"$f":"IF(BA15=5,4,0)","v":0},5,null,"Osł. modułowa",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,230,300,400,600,800,null,null,null,null,null,null,null,null,null,null,null,null,"P 200",230,300,400,600,800,null,null,null,{"$f":"IF('Zenergy-OE'!AF15=\"\",0,IF('Zenergy-OE'!AF15>0,'Zenergy-OE'!AF15,0))","v":80365},{"$f":"IF('Zenergy-OE'!AH15=\"\",0,'Zenergy-OE'!AH15)","v":2},{"$f":"IF(EK6>1,VLOOKUP(IF(ISNUMBER(EK6),TEXT(EK6,\"0\"),EK6),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - DRZWI PEŁNE IP30, H2000 X W650"},{"$f":"IF(EK6>1,VLOOKUP(IF(ISNUMBER(EK6),TEXT(EK6,\"0\"),EK6),Cennik!$A$4:$F$52318,3,FALSE),0)","v":953.6},{"$f":"EL6*EN6","v":1907.2},null,300,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[450,400,40340,50340,60340,70340,80340,90340,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 5\",\"Project 5\")","v":"PROJEKT 5"},null,{"$f":"IF($R$2=5,\"5\",\"\")","v":""},null,null,null,{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BS13<4,1,0)","v":1},{"$f":"IF(BS13>1,1,0)","v":1},{"$f":"SUM(Y7:AA7)","v":3},null,null,{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BS20>1,1,0)","v":0},{"$f":"SUM(AE7:AF7)","v":0},null,null,{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BS21>1,1,0)","v":0},{"$f":"SUM(AJ7:AK7)","v":1},null,{"$f":"INDEX(($AO$13:$AR$15),$BA$4,$BS6)","v":5},"Pokrywa górna pole 3",null,null,null,null,null,null,null,null,null,null,6,2,43,null,2,1400,null,2,300,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi pełne\",\"Plain door\")","v":"Drzwi pełne"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Plecy pełne\",\"Plain back cover\")","v":"Plecy pełne"},null,2,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Cokół pełny 100mm\",\"100mm\")","v":"Cokół pełny 100mm"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Pokrywa pełna\",\"Plain\")","v":"Pokrywa pełna"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama osłon modułowych\",\"Modular\")","v":"Rama osłon modułowych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama osłon modułowych\",\"Modular\")","v":"Rama osłon modułowych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE5<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P, most pionowy na plecach\",\"Rear 3P vertical busbar support\")","v":"Izolator 3P, most pionowy na plecach"},null,null,null,-1,650,6,null,{"$f":"IF(BA13=6,5,0)","v":5},{"$f":"IF(BA12=6,5,0)","v":0},{"$f":"IF(BA15=6,5,0)","v":0},6,null,"Osł. przeszklona",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Brak",{"$f":"IF(DK6=0,\"\",\"\")","v":""},"","","","","",null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"IF(EB6=0,\"\",\"\")","v":""},"","","","","",null,null,null,{"$f":"IF('Zenergy-OE'!AF18=\"\",0,IF('Zenergy-OE'!AF18>0,'Zenergy-OE'!AF18,0))","v":81265},{"$f":"IF('Zenergy-OE'!AH18=\"\",0,'Zenergy-OE'!AH18)","v":2},{"$f":"IF(EK7>1,VLOOKUP(IF(ISNUMBER(EK7),TEXT(EK7,\"0\"),EK7),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - OSŁONA TYLNA PEŁNA IP30, H2000 X W650"},{"$f":"IF(EK7>1,VLOOKUP(IF(ISNUMBER(EK7),TEXT(EK7,\"0\"),EK7),Cennik!$A$4:$F$52318,3,FALSE),0)","v":541.1},1082.2,null,400,400,40140,50140,60140,70140,80140,90140,null,400,40140,50140,60140,70140,80140,90140]
[600,450,40345,50345,60345,70345,80345,90345,null,450,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 6\",\"Project 6\")","v":"PROJEKT 6"},null,{"$f":"IF($R$2=6,\"6\",\"\")","v":""},null,null,false,{"$f":"IF(X8=TRUE,1,0)","v":0},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BA4=3,1,0)","v":0},{"$f":"SUM(Y8:Z8)","v":1},false,{"$f":"IF(AC8=TRUE,1,0)","v":0},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BA10>13,1,0)","v":0},{"$f":"SUM(AD8:AF8)","v":0},false,{"$f":"IF(AH8=TRUE,1,0)","v":0},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BA4=3,1,0)","v":0},{"$f":"SUM(AI8:AJ8)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,7,3,55,null,3,1600,null,3,400,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi z wentylacją\",\"Vented door\")","v":"Drzwi z wentylacją"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi pełne\",\"Plain door\")","v":"Drzwi pełne"},null,3,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Cokół pełny 200mm\",\"200mm\")","v":"Cokół pełny 200mm"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Pokrywa wentylowana\",\"Vented\")","v":"Pokrywa wentylowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama osłon modułowych, plomba\",\"Modular sealed\")","v":"Rama osłon modułowych, plomba"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama osłon modułowych, plomba\",\"Modular sealed\")","v":"Rama osłon modułowych, plomba"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 4P, most pionowy na plecach\",\"Rear 4P vertical busbar support\")","v":"Izolator 4P, most pionowy na plecach"},null,null,null,-2,800,7,null,{"$f":"IF(BA13=7,6,0)","v":0},{"$f":"IF(BA12=7,6,0)","v":0},{"$f":"IF(BA15=7,6,0)","v":0},7,null,"Szyna stała TS35",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Wspornik płyt montażowych, boczny 200/230",31023,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31023,{"$f":"\"\"","v":""},{"$f":"IF(DP7=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF21=\"\",0,IF('Zenergy-OE'!AF21>0,'Zenergy-OE'!AF21,0))","v":31465},{"$f":"IF('Zenergy-OE'!AH21=\"\",0,'Zenergy-OE'!AH21)","v":2},{"$f":"IF(EK8>1,VLOOKUP(IF(ISNUMBER(EK8),TEXT(EK8,\"0\"),EK8),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - POKRYWA GÓRNA IP30, W650, D400"},{"$f":"IF(EK8>1,VLOOKUP(IF(ISNUMBER(EK8),TEXT(EK8,\"0\"),EK8),Cennik!$A$4:$F$52318,3,FALSE),0)","v":203},406,null,450,450,40145,50145,60145,70145,80145,90145,null,450,40145,50145,60145,70145,80145,90145]
[650,600,40360,50360,60360,70360,80360,90360,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 7\",\"Project 7\")","v":"PROJEKT 7"},null,{"$f":"IF($R$2=7,\"7\",\"\")","v":""},null,null,false,{"$f":"IF(X9=TRUE,1,0)","v":0},{"$f":"IF(BA13>1,1,0)","v":1},null,{"$f":"SUM(Y9:AA9)","v":1},null,{"$f":"IF(X9=TRUE,1,0)","v":0},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BA13>13,1,0)","v":0},{"$f":"SUM(AD9+AE9-AF9)","v":0},null,{"$f":"IF(X9=TRUE,1,0)","v":0},{"$f":"IF(BA15>1,1,0)","v":0},null,{"$f":"SUM(AI9:AK9)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,4,1800,null,4,600,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi transparentne\",\"Transparent door\")","v":"Drzwi transparentne"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi transparentne\",\"Transparent door\")","v":"Drzwi transparentne"},null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi wewnętrzne\",\"Internal door\")","v":"Drzwi wewnętrzne"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi wewnętrzne\",\"Internal door\")","v":"Drzwi wewnętrzne"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P, most pion. na plecach reg.\",\"Rear 3P vertical busbar support regulated\")","v":"Izolator 3P, most pion. na plecach reg."},null,null,null,-3,"650+150",8,null,{"$f":"IF(BA13=8,5,0)","v":0},{"$f":"IF(BA12=8,5,0)","v":0},{"$f":"IF(BA15=8,5,0)","v":0},8,null,"Szyna reg.TS35",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Wspornik płyt montażowych, boczny 400",{"$f":"IF(DK8=0,\"\",\"\")","v":""},31030,31040,31040,31040,{"$f":"IF(DP8=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,"Izol.1P bok PN",31712,{"$f":"IF(EC8=0,\"\",\"\")","v":""},{"$f":"IF(ED8=0,\"\",\"\")","v":""},{"$f":"IF(EE8=0,\"\",\"\")","v":""},{"$f":"IF(EF8=0,\"\",\"\")","v":""},{"$f":"IF(EG8=0,\"\",\"\")","v":""},null,null,null,{"$f":"IF('Zenergy-OE'!AF24=\"\",0,IF('Zenergy-OE'!AF24>0,'Zenergy-OE'!AF24,0))","v":0},{"$f":"IF('Zenergy-OE'!AH24=\"\",0,'Zenergy-OE'!AH24)","v":0},{"$f":"IF(EK9>1,VLOOKUP(IF(ISNUMBER(EK9),TEXT(EK9,\"0\"),EK9),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK9>1,VLOOKUP(IF(ISNUMBER(EK9),TEXT(EK9,\"0\"),EK9),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,600,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
["650+150",650,40365,50365,60365,70365,80365,90365,null,650,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 8\",\"Project 8\")","v":"PROJEKT 8"},null,{"$f":"IF($R$2=8,\"8\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"IF(BA13>13,BA13,BA14)","v":1},null,null,5,2000,null,5,800,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Plecy pełne\",\"Plain back cover\")","v":"Plecy pełne"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drzwi z wentylacją\",\"Vented door\")","v":"Drzwi z wentylacją"},null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozłączników listwowych\",\"Vertical Fuse Switch\")","v":"Rama rozłączników listwowych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozłączników listwowych\",\"Vertical Fuse Switch\")","v":"Rama rozłączników listwowych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 4P, most pion. na plecach reg.\",\"Rear 4P vertical busbar support regulated\")","v":"Izolator 4P, most pion. na plecach reg."},null,null,null,-4,850,9,null,{"$f":"IF(BA13=9,7,0)","v":0},{"$f":"IF(BA12=9,7,0)","v":0},{"$f":"IF(BA15=9,7,0)","v":0},9,null,"Płyta ocynk pełna",{"$f":"IF(CW3=0,\"\",\"\")","v":""},33032,33033,33034,33035,33036,{"$f":"IF(DC3=0,\"\",\"\")","v":""},33037,{"$f":"IF(DE3=0,\"\",\"\")","v":""},33038,{"$f":"IF(DG3=0,\"\",\"\")","v":""},33039,null,"Uchwyt płyt montażowych",31010,31010,31010,31010,31010,{"$f":"IF(DP9=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,"Izol.3P bok",{"$f":"IF(EB9=0,\"\",\"\")","v":""},{"$f":"IF(EC9=0,\"\",\"\")","v":""},{"$f":"IF(ED9=0,\"\",\"\")","v":""},31710,31710,31710,null,null,null,{"$f":"IF('Zenergy-OE'!AF25=\"\",0,IF('Zenergy-OE'!AF25>0,'Zenergy-OE'!AF25,0))","v":0},{"$f":"IF('Zenergy-OE'!AH25=\"\",0,'Zenergy-OE'!AH25)","v":0},{"$f":"IF(EK10>1,VLOOKUP(IF(ISNUMBER(EK10),TEXT(EK10,\"0\"),EK10),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK10>1,VLOOKUP(IF(ISNUMBER(EK10),TEXT(EK10,\"0\"),EK10),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,650,650,40165,50165,60165,70165,80165,90165,null,650,40165,50165,60165,70165,80165,90165]
[800,800,40380,50380,60380,70380,80380,90380,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 9\",\"Project 9\")","v":"PROJEKT 9"},null,{"$f":"IF($R$2=9,\"9\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"IF(BA13>13,2,BA14)","v":1},null,null,6,2200,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Plecy z wentylacją\",\"Vented back cover\")","v":"Plecy z wentylacją"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozłączników listwowych, plomba\",\"Vertical Fuse Switch sealed\")","v":"Rama rozłączników listwowych, plomba"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozłączników listwowych, plomba\",\"Vertical Fuse Switch sealed\")","v":"Rama rozłączników listwowych, plomba"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. 3P, podpora mostu na plecach, reg.\",\"Rear 3P vert. busbar bottom support regulated\")","v":"Izol. 3P, podpora mostu na plecach, reg."},null,null,null,-5,"650+200",10,null,{"$f":"IF(BA13=10,5,0)","v":0},{"$f":"IF(BA12=10,5,0)","v":0},{"$f":"IF(BA15=10,5,0)","v":0},10,null,"Płyta malow.otw.",{"$f":"IF(CW3=0,\"\",\"\")","v":""},33532,33533,33534,33535,33536,{"$f":"IF(DC3=0,\"\",\"\")","v":""},33537,{"$f":"IF(DE3=0,\"\",\"\")","v":""},33538,{"$f":"IF(DG3=0,\"\",\"\")","v":""},33539,null,"Izol. AlCubar / Cu 1P, most poziomy, 200/230",20110,{"$f":"IF(DL21=0,\"\",\"\")","v":""},{"$f":"IF(DM21=0,\"\",\"\")","v":""},20110,{"$f":"IF(DO21=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,"Izol.4P bok","","","",31711,31711,31711,null,null,null,{"$f":"IF('Zenergy-OE'!X25=\"\",0,IF('Zenergy-OE'!X25>0,'Zenergy-OE'!X25,0))","v":89340},{"$f":"IF('Zenergy-OE'!Z25=\"\",0,'Zenergy-OE'!Z25)","v":2},{"$f":"IF(EK11>1,VLOOKUP(IF(ISNUMBER(EK11),TEXT(EK11,\"0\"),EK11),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - OSŁONY BOCZNE PEŁNE IP30, H2000 X D400"},{"$f":"IF(EK11>1,VLOOKUP(IF(ISNUMBER(EK11),TEXT(EK11,\"0\"),EK11),Cennik!$A$4:$F$52318,3,FALSE),0)","v":675},1350,null,800,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[850,"650+150",40380,50380,60380,70380,80380,90380,null,"650+150",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"PROJEKT 10\",\"Project 10\")","v":"PROJEKT 10"},null,{"$f":"IF($R$2=10,\"10\",\"\")","v":""},null,null,null,{"$f":"IF('Zenergy-OE'!AF24=\"\",0,1)","v":0},{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BV4>4,1,0)","v":0},{"$f":"SUM(Y12:AA12)","v":1},{"$f":"IF(AL23>0,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AN24=\"\",0,1)","v":0},{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BV5>4,1,0)","v":0},{"$f":"SUM(AC12:AF12)","v":0},null,{"$f":"IF('Zenergy-OE'!AV24=\"\",0,1)","v":0},{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BV6>4,1,0)","v":0},{"$f":"SUM(AI12:AK12)","v":0},null,"IP","Brak","Pełna","Went.",null,null,null,null,null,null,null,null,null,{"$f":"IF(BA13>13,1,BA14)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozł. listwowych, analizator\",\"Vertical Fuse Switch Power Meter\")","v":"Rama rozł. listwowych, analizator"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozł. listwowych, analizator\",\"Vertical Fuse Switch Power Meter\")","v":"Rama rozł. listwowych, analizator"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. 4P, podpora mostu na plecach, reg.\",\"Rear 4P vert. busbar bottom support regulated\")","v":"Izol. 4P, podpora mostu na plecach, reg."},null,null,null,null,1000,11,null,{"$f":"IF(BA13=11,8,0)","v":0},{"$f":"IF(BA12=11,8,0)","v":0},{"$f":"IF(BA15=11,8,0)","v":0},11,null,"Płyta oc. pozioma",{"$f":"IF(CW2=0,\"\",\"\")","v":""},"","","","","","","","",{"$f":"IF(DF360=0,\"\",\"\")","v":""},{"$f":"IF(DG360=0,\"\",\"\")","v":""},{"$f":"IF(DH360=0,\"\",\"\")","v":""},null,"Izol. AlCubar / Cu 3P, most poziomy, 400",{"$f":"IF(DK11=0,\"\",\"\")","v":""},{"$f":"IF(DL11=0,\"\",\"\")","v":""},20113,20113,20113,null,null,null,null,null,null,null,null,null,null,null,"Iz.3P doizol.","","","",31714,31714,31714,null,null,null,{"$f":"IF('Zenergy-OE'!AF28=\"\",0,IF('Zenergy-OE'!AF28>0,'Zenergy-OE'!AF28,0))","v":0},{"$f":"IF('Zenergy-OE'!AH28=\"\",0,'Zenergy-OE'!AH28)","v":0},{"$f":"IF(EK12>1,VLOOKUP(IF(ISNUMBER(EK12),TEXT(EK12,\"0\"),EK12),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK12>1,VLOOKUP(IF(ISNUMBER(EK12),TEXT(EK12,\"0\"),EK12),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,"650+150","650+150",40165,50165,60165,70165,80165,90165,null,"650+150",40165,50165,60165,70165,80165,90165]
[1000,850,40385,50385,60385,70385,80385,90385,null,850,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,{"$f":"TODAY()","v":"2025-01-29"},null,null,null,null,{"$f":"IF('Zenergy-OE'!AF28=\"\",2,0)","v":2},{"$f":"IF(BY4=4,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AF28>80700,1,0)","v":1},{"$f":"IF('Zenergy-OE'!AF28=\"\",0,1)","v":0},{"$f":"SUM(X13:AA13)","v":3},{"$f":"IF('Zenergy-OE'!AN28=\"\",2,0)","v":2},{"$f":"IF(BY5=4,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AN28>80700,1,0)","v":1},{"$f":"IF('Zenergy-OE'!AN28=\"\",0,1)","v":0},{"$f":"SUM(AC13:AF13)","v":3},{"$f":"IF('Zenergy-OE'!AV28=\"\",2,0)","v":2},{"$f":"IF(BY6=4,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AV28>80700,1,0)","v":1},{"$f":"IF('Zenergy-OE'!AV28=\"\",0,1)","v":0},{"$f":"SUM(AH13:AK13)","v":3},null,30,5,2,1,null,null,null,null,null,null,null,null,null,6,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,13,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozł. listw, analizator, plomba\",\"Vertical Fuse Switch Power Meter sealed\")","v":"Rama rozł. listw, analizator, plomba"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama rozł. listw, analizator, plomba\",\"Vertical Fuse Switch Power Meter sealed\")","v":"Rama rozł. listw, analizator, plomba"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630A 3P pionowo na plecach\",\"Rear 3P AlCubar 630A vertical busbar support\")","v":"Izol. AlCubar 630A 3P pionowo na plecach"},null,null,null,null,1200,12,null,{"$f":"IF(BA13=12,9,0)","v":0},{"$f":"IF(BA12=12,9,0)","v":0},{"$f":"IF(BA15=12,9,0)","v":0},12,null,"Płyta licznikowa",{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar / Cu 4P, most poziomy, 400",{"$f":"IF(DK12=0,\"\",\"\")","v":""},{"$f":"IF(DL12=0,\"\",\"\")","v":""},20114,20114,20114,null,null,null,null,null,null,null,null,null,null,null,"Iz.4P doizol.","","","",31715,31715,31715,null,null,null,{"$f":"IF('Zenergy-OE'!AF29=\"\",0,IF('Zenergy-OE'!AF29>0,'Zenergy-OE'!AF29,0))","v":0},{"$f":"IF('Zenergy-OE'!AH29=\"\",0,'Zenergy-OE'!AH29)","v":0},{"$f":"IF(EK13>1,VLOOKUP(IF(ISNUMBER(EK13),TEXT(EK13,\"0\"),EK13),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK13>1,VLOOKUP(IF(ISNUMBER(EK13),TEXT(EK13,\"0\"),EK13),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,850,850,40185,50185,60185,70185,80185,90185,null,850,40185,50185,60185,70185,80185,90185]
[1200,"650+200",40385,50385,60385,70385,80385,90385,null,"650+200",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"_","2023-12-05",null,null,null,null,null,{"$f":"IF(BA13>1,1,0)","v":1},{"$f":"IF(BA4=3,1,0)","v":0},{"$f":"IF(BV19>1,1,0)","v":1},{"$f":"SUM(Y14:AA14)","v":2},null,{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BA4=3,1,0)","v":0},{"$f":"IF(BV20>1,1,0)","v":1},{"$f":"SUM(AD14:AF14)","v":1},null,{"$f":"IF(BA15>1,1,0)","v":0},{"$f":"IF(BA4=3,1,0)","v":0},{"$f":"IF(BV21>1,1,0)","v":0},{"$f":"SUM(AI14:AK14)","v":0},null,43,5,4,3,null,null,null,null,null,null,null,null,null,1,"Szerokość",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cokół",null,null,null,null,1,"Wersja",null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630A 4P pionowo na plecach\",\"Rear 4P AlCubar 630A vertical busbar support\")","v":"Izol. AlCubar 630A 4P pionowo na plecach"},null,null,null,null,1300,13,null,{"$f":"IF(BA13=13,10,0)","v":0},{"$f":"IF(BA12=13,10,0)","v":0},{"$f":"IF(BA15=13,10,0)","v":0},13,null,null,{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izolator AlCubar 1P, łącznik, poziom, 200/230",20120,{"$f":"IF(DL13=0,\"\",\"\")","v":""},{"$f":"IF(DM13=0,\"\",\"\")","v":""},20120,{"$f":"IF(DO13=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,"Iz.3P poz.podpora","","","",31723,31723,31723,null,null,null,{"$f":"IF('Zenergy-OE'!AF32=\"\",0,IF('Zenergy-OE'!AF32>0,'Zenergy-OE'!AF32,0))","v":30065},{"$f":"IF('Zenergy-OE'!AH32=\"\",0,'Zenergy-OE'!AH32)","v":2},{"$f":"IF(EK14>1,VLOOKUP(IF(ISNUMBER(EK14),TEXT(EK14,\"0\"),EK14),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - COKÓŁ H100, WENTYLOWANE OSŁONY PRZÓD,TYŁ, W650"},{"$f":"IF(EK14>1,VLOOKUP(IF(ISNUMBER(EK14),TEXT(EK14,\"0\"),EK14),Cennik!$A$4:$F$52318,3,FALSE),0)","v":177.1},354.2,null,"650+200","650+200",40165,50165,60165,70165,80165,90165,null,"650+200",40165,50165,60165,70165,80165,90165]
[1300,1000,40310,50310,60310,70310,80310,90310,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},1,2,"/",5,"/202",3,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF25=36010,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AN25=\"\",0,1)","v":0},{"$f":"SUM(AD15:AE15)","v":0},{"$f":"IF(AF15=2,1,2)","v":2},null,{"$f":"IF('Zenergy-OE'!AN25=36010,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AV25=\"\",0,1)","v":0},{"$f":"SUM(AI15:AJ15)","v":0},{"$f":"IF(AK15=2,1,2)","v":2},null,55,5,4,5,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak wyboru\",\"None\")","v":"Brak wyboru"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,null,null,null,null,"Polish version",null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa na plecach\",\"Cable tray\")","v":"Drabinka kablowa na plecach"},null,null,null,{"$f":"IF(AV13=14,12,0)","v":0},"650+650",14,null,{"$f":"IF(BA13=14,5,0)","v":0},{"$f":"IF(BA13=14,5,0)","v":0},null,14,null,null,{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 3P, łącznik, poziom, 400\",\"Horizontal200 1P insul.\")","v":"Izolator AlCubar 3P, łącznik, poziom, 400"},{"$f":"IF(DK14=0,\"\",\"\")","v":""},"",20123,20123,20123,null,null,null,null,null,null,null,null,null,null,null,"Iz.4P poz.podpora","","","",31724,31724,31724,null,null,null,{"$f":"IF('Zenergy-OE'!AF33=\"\",0,IF('Zenergy-OE'!AF33>0,'Zenergy-OE'!AF33,0))","v":30043},{"$f":"IF('Zenergy-OE'!AH33=\"\",0,'Zenergy-OE'!AH33)","v":2},{"$f":"IF(EK15>1,VLOOKUP(IF(ISNUMBER(EK15),TEXT(EK15,\"0\"),EK15),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - COKÓŁ H100, PEŁNE OSŁONY BOCZNE, D400"},{"$f":"IF(EK15>1,VLOOKUP(IF(ISNUMBER(EK15),TEXT(EK15,\"0\"),EK15),Cennik!$A$4:$F$52318,3,FALSE),0)","v":150.1},300.2,null,1000,1000,40110,50110,60110,70110,80110,90110,null,1000,40110,50110,60110,70110,80110,90110]
["650+612",1200,40312,50312,60312,70312,80312,90312,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"CONCATENATE(Q15,R15,S15,T15,U15,V15,W15)","v":"12/5/2023"},"12/5/2023",null,null,null,null,null,null,null,{"$f":"IF(AG1>1,1,0)","v":0},{"$f":"IF(AL1>1,1,0)","v":0},{"$f":"SUM(Z16:AA16)","v":0},null,{"$f":"IF('Zenergy-OE'!AF29=36010,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AN29=\"\",0,1)","v":0},{"$f":"SUM(AD16:AE16)","v":0},{"$f":"IF(AF16=2,1,2)","v":2},null,{"$f":"IF('Zenergy-OE'!AN29=36010,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AV29=\"\",0,1)","v":0},{"$f":"SUM(AI16:AJ16)","v":0},{"$f":"IF(AK16=2,1,2)","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 300\",\"Frame 300\")","v":"Rama 300"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Cokół pełny 100mm\",\"100mm\")","v":"Cokół pełny 100mm"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 moduł\",\"\")","v":"1 moduł"},null,null,"English version",null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa na drzwiach\",\"Door cable tray\")","v":"Drabinka kablowa na drzwiach"},null,null,null,{"$f":"IF(AV13=15,13,0)","v":0},"650+850",15,null,{"$f":"IF(BA13=15,5,0)","v":0},{"$f":"IF(BA13=15,7,0)","v":0},null,15,null,null,{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 4P, łącznik, poziom, 400\",\"Horizontal200 1P insul.\")","v":"Izolator AlCubar 4P, łącznik, poziom, 400"},"","",20124,20124,20124,null,null,null,null,null,null,null,null,null,null,null,"Iz.4P Linergy bok","","","",31774,31774,31774,null,null,null,{"$f":"IF('Zenergy-OE'!AF36=\"\",0,IF('Zenergy-OE'!AF36>0,'Zenergy-OE'!AF36,0))","v":0},{"$f":"IF('Zenergy-OE'!AH36=\"\",0,'Zenergy-OE'!AH36)","v":0},{"$f":"IF(EK16>1,VLOOKUP(IF(ISNUMBER(EK16),TEXT(EK16,\"0\"),EK16),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK16>1,VLOOKUP(IF(ISNUMBER(EK16),TEXT(EK16,\"0\"),EK16),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,1200,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
["650+812",1300,40313,50313,60313,70313,80313,90313,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 400A\",\"Frame 400A\")","v":"Rama 400A"},null,null,null,null,null,null,null,1,{"$f":"BJ17-1","v":0},null,1,null,null,1,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Cokół pełny 200mm\",\"200mm\")","v":"Cokół pełny 200mm"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa pod osłonę\",\"Front plate cable tray\")","v":"Drabinka kablowa pod osłonę"},null,null,null,{"$f":"IF(AV13=16,13,0)","v":0},"850+850",16,null,{"$f":"IF(BA13=16,7,0)","v":0},{"$f":"IF(BA13=16,7,0)","v":0},null,16,null,null,{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar / Cu 3P, doizolowanie poz. 400","","",20118,20118,20118,null,null,null,null,null,null,null,null,null,null,null,null,"","","",{"$f":"IF(EE16=0,\"\",\"\")","v":""},{"$f":"IF(EF16=0,\"\",\"\")","v":""},{"$f":"IF(EG16=0,\"\",\"\")","v":""},null,null,null,{"$f":"IF('Zenergy-OE'!AF39=\"\",0,IF('Zenergy-OE'!AF39>0,'Zenergy-OE'!AF39,0))","v":0},{"$f":"IF('Zenergy-OE'!AH39=\"\",0,'Zenergy-OE'!AH39)","v":0},{"$f":"IF(EK17>1,VLOOKUP(IF(ISNUMBER(EK17),TEXT(EK17,\"0\"),EK17),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK17>1,VLOOKUP(IF(ISNUMBER(EK17),TEXT(EK17,\"0\"),EK17),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,1300,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
["850+812","650+612",40365,50365,60365,70365,80365,90365,null,"650+612",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$20:$AR$22),$BA$4,$BS$13)","v":1},"Cokół / pokrywa pole 1 - 3",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 450A\",\"Frame 450A\")","v":"Rama 450A"},null,null,null,null,null,null,null,1,{"$f":"BJ18-1","v":0},null,1,null,null,1,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Dolna pełna pokrywa\",\"Plain cover\")","v":"Dolna pełna pokrywa"},null,null,null,null,null,null,null,{"$f":"IF(CE23=14,14,IF(CP36=1,$BA$15,CB23))","v":1},null,null,{"$f":"IF(CP36=1,BD4,CE23)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Metalowa kieszeń na dokumentację\",\"Drawing holder\")","v":"Metalowa kieszeń na dokumentację"},null,null,null,null,"650+300",17,null,{"$f":"IF(BA13=17,5,0)","v":0},{"$f":"IF(BA13=17,1,0)","v":0},null,17,null,null,{"$f":"IF(CW3=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar / Cu 4P, doizolowanie poz. 400","","",20119,20119,20119,null,null,null,null,null,null,null,null,null,null,null,"Przył.tr.3P 250A","","","",32700,32700,32700,null,null,null,{"$f":"IF('Zenergy-OE'!AF42=\"\",0,IF('Zenergy-OE'!AF42>0,'Zenergy-OE'!AF42,0))","v":80965},{"$f":"'Zenergy-OE'!AH42","v":2},{"$f":"IF(EK18>1,VLOOKUP(IF(ISNUMBER(EK18),TEXT(EK18,\"0\"),EK18),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":"ZENERGY - PŁYTA MONTAŻOWA PEŁNA H2000 X W650 + WSPORNIKI,  ( 1850 X 550 )"},{"$f":"IF(EK18>1,VLOOKUP(IF(ISNUMBER(EK18),TEXT(EK18,\"0\"),EK18),Cennik!$A$4:$F$52318,3,FALSE),0)","v":745.2},1490.4,null,"650+612","650+650",40165,50165,60165,70165,80165,90165,null,"650+650",40165,50165,60165,70165,80165,90165]
[null,"650+812",40365,50365,60365,70365,80365,90365,null,"650+812",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BM4<3,0,1)","v":0},{"$f":"IF(BJ4>4,0,1)","v":1},{"$f":"SUM(AI19:AI20)","v":1},null,null,"IP","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 600\",\"Frame 600\")","v":"Rama 600"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,null,null,2,11,null,1,null,null,{"$f":"IF(CE22=14,25,IF(CO36=1,$BA$12,CB22))","v":1},null,null,{"$f":"IF(CO36=1,BD4,CE22)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Pionowy zestaw szyn TS35, 6M\",\"6-Modules Vertical DIN-rail for terminals\")","v":"Pionowy zestaw szyn TS35, 6M"},null,null,null,null,"650+400",18,null,{"$f":"IF(BA13=18,5,0)","v":0},{"$f":"IF(BA13=18,2,0)","v":0},null,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Izol. AlCubar / Cu 1P, most poziomy z tyłu",20146,20146,20146,20146,20146,null,null,null,null,null,null,null,null,null,null,null,"Przył.tr.4P 250A","","","",32701,32701,32701,null,null,null,{"$f":"IF('Zenergy-OE'!AF45=\"\",0,IF('Zenergy-OE'!AF45>0,'Zenergy-OE'!AF45,0))","v":0},{"$f":"'Zenergy-OE'!AH45","v":0},{"$f":"IF(EK19>1,VLOOKUP(IF(ISNUMBER(EK19),TEXT(EK19,\"0\"),EK19),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK19>1,VLOOKUP(IF(ISNUMBER(EK19),TEXT(EK19,\"0\"),EK19),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,"650+812","650+850",40165,50165,60165,70165,80165,90165,null,"650+850",40185,50185,60185,70185,80185,90185]
[null,"850+812",40385,50385,60385,70385,80385,90385,null,"850+812",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BA13>1,1,0)","v":1},null,{"$f":"SUM(AI20+AJ19)","v":2},null,null,30,5,1,2,3,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A\",\"Frame 650A\")","v":"Rama 650A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,1,13,null,6,"Boki",null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  1\",\"Quantity 1\")","v":"Ilość  1"},null,{"$f":"IF(CE21=14,23,IF(CN36=1,$BA$13,CB21))","v":1},null,null,{"$f":"IF(CN36=1,BD4,CE21)","v":1},null,null,{"$f":"IF(BA13>10,2,1)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Poziomy zestaw dwóch szyn TS35\",\"Horizontal double DIN-rail for terminals\")","v":"Poziomy zestaw dwóch szyn TS35"},null,null,null,null,"850+300",19,null,{"$f":"IF(BA13=19,7,0)","v":0},{"$f":"IF(BA13=19,1,0)","v":0},null,19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Izol. AlCubar / Cu 3P, most poziomy z tyłu",20148,20148,20148,20148,20148,null,null,null,null,null,null,null,null,null,null,null,"Przył.tr.3P 630A","","","",32702,32702,32702,null,null,null,{"$f":"IF('Zenergy-OE'!AF48=\"\",0,IF('Zenergy-OE'!AF48>0,'Zenergy-OE'!AF48,0))","v":0},{"$f":"'Zenergy-OE'!AH48","v":0},{"$f":"IF(EK20>1,VLOOKUP(IF(ISNUMBER(EK20),TEXT(EK20,\"0\"),EK20),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK20>1,VLOOKUP(IF(ISNUMBER(EK20),TEXT(EK20,\"0\"),EK20),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,"850+812","850+850",40185,50185,60185,70185,80185,90185,null,"850+850",40185,50185,60185,70185,80185,90185]
[null,"650+300",40365,50365,60365,70365,80365,90365,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,5,1,2,4,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 800\",\"Frame 800\")","v":"Rama 800"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,1,"Cokół",null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  2\",\"Quantity 2\")","v":"Ilość  2"},null,1,2,null,1,2,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Osłona mostu poziomego\",\"Horizontal busbar cover\")","v":"Osłona mostu poziomego"},null,null,null,null,"850+400",20,null,{"$f":"IF(BA13=20,7,0)","v":0},{"$f":"IF(BA13=20,2,0)","v":0},null,20,null,"W 400 - 2","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,"Izol. AlCubar / Cu 4P, most poziomy z tyłu",20149,20149,20149,20149,20149,null,null,null,null,null,null,null,null,null,null,null,"Przył.tr.4P 630A","","","",32703,32703,32703,null,null,null,{"$f":"IF('Zenergy-OE'!AF51=\"\",0,IF('Zenergy-OE'!AF51>0,'Zenergy-OE'!AF51,0))","v":0},{"$f":"'Zenergy-OE'!AH51","v":0},{"$f":"IF(EK21>1,VLOOKUP(IF(ISNUMBER(EK21),TEXT(EK21,\"0\"),EK21),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK21>1,VLOOKUP(IF(ISNUMBER(EK21),TEXT(EK21,\"0\"),EK21),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+300",40165,50165,60165,70165,80165,90165,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+400",40365,50365,60365,70365,80365,90365,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BM5<3,0,1)","v":1},{"$f":"IF(BJ5>4,0,1)","v":1},{"$f":"SUM(AI23+AH22+AH23)","v":1},{"$f":"IF(BA12=1,1,0)","v":1},{"$f":"IF(AG5=2,AG1-1,IF(AG5=2,Zbaza!AG1-1,\"\"))","v":""},null,55,5,1,2,4,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A+150\",\"Frame 650A+150\")","v":"Rama 650A+150"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Cokół osłony boczne\",\"Plain sides\")","v":"Cokół osłony boczne"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Boki pełne, przykręcane\",\"\")","v":"Boki pełne, przykręcane"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  3\",\"Quantity 3\")","v":"Ilość  3"},null,1,"Osłony",null,1,"Ilość mod.",null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zestaw mocowania do ściany\",\"Zenergy cabinet wall sling rail\")","v":"Zestaw mocowania do ściany"},null,null,null,null,"150+650+300",21,null,{"$f":"IF(BA13=21,5,0)","v":0},{"$f":"IF(BA13=21,1,0)","v":0},null,21,null,"Brak",{"$f":"IF(CW21=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar / Cu 1P, most pionowy, bok 200/230",{"$f":"IF(DK10=0,\"\",\"\")","v":""},{"$f":"IF(DL10=0,\"\",\"\")","v":""},{"$f":"IF(DM10=0,\"\",\"\")","v":""},20100,{"$f":"IF(DO10=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF54=\"\",0,IF('Zenergy-OE'!AF54>0,'Zenergy-OE'!AF54,0))","v":0},{"$f":"'Zenergy-OE'!AH54","v":0},{"$f":"IF(EK22>1,VLOOKUP(IF(ISNUMBER(EK22),TEXT(EK22,\"0\"),EK22),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK22>1,VLOOKUP(IF(ISNUMBER(EK22),TEXT(EK22,\"0\"),EK22),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+400",40165,50165,60165,70165,80165,90165,null,"650+400",40140,50140,60140,70140,80140,90140]
[null,"850+300",40385,50385,60385,70385,80385,90385,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Szerokość obudowy","Osłona tylna went. IP30   Wysokość",null,null,5,null,"Pole 1,3",null,null,null,null,null,null,null,null,null,{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BA13>13,1,0)","v":0},{"$f":"SUM(AH23+AI22+AI23)","v":1},{"$f":"AI23+AK22","v":1},{"$f":"IF(AK23=2,BA13-1,0)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 850A\",\"Frame 850A\")","v":"Rama 850A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Cokół osłony boczne z przepustem\",\"Passage\")","v":"Cokół osłony boczne z przepustem"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Boki wentylowane, przykręcane\",\"\")","v":"Boki wentylowane, przykręcane"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  4\",\"Quantity 4\")","v":"Ilość  4"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,1,null,null,null,null,null,"150+650+400",22,null,{"$f":"IF(BA13=22,5,0)","v":0},{"$f":"IF(BA13=22,2,0)","v":0},null,22,null,"Osłona pełna",32010,32020,32030,32040,32050,32060,32070,32080,32090,32091,32092,32093,null,"Izol. AlCubar / Cu 3P, most pionowy z boku",{"$f":"IF(DK22=0,\"\",\"\")","v":""},"",20103,20103,20103,null,null,null,null,null,null,null,null,null,null,null,"Wsp.bok 1 rząd",31221,31222,31223,31224,31224,31224,null,null,null,{"$f":"IF('Zenergy-OE'!AF57=\"\",0,IF('Zenergy-OE'!AF57>0,'Zenergy-OE'!AF57,0))","v":0},{"$f":"'Zenergy-OE'!AH57","v":0},{"$f":"IF(EK23>1,VLOOKUP(IF(ISNUMBER(EK23),TEXT(EK23,\"0\"),EK23),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK23>1,VLOOKUP(IF(ISNUMBER(EK23),TEXT(EK23,\"0\"),EK23),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+300",40185,50185,60185,70185,80185,90185,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+400",40385,50385,60385,70385,80385,90385,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A+200\",\"Frame 650A+200\")","v":"Rama 650A+200"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Boki pełne wraz z ramą\",\"\")","v":"Boki pełne wraz z ramą"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  5\",\"Quantity 5\")","v":"Ilość  5"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE22<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,1,null,null,null,null,null,null,null,null,null,{"$f":"SUM(CR2:CR14)","v":11},null,23,null,"Osł. modułowa",{"$f":"IF(CW21=0,\"\",\"\")","v":""},32025,32035,32045,32055,{"$f":"IF(DB23=0,\"\",\"\")","v":""},"","","","","","",null,"Izol. AlCubar / Cu 4P, most pionowy z boku","","",20104,20104,20104,null,null,null,null,null,null,null,null,null,null,null,"Wsp.bok 2 rzędy",31231,31232,31233,31234,31234,31234,null,null,null,{"$f":"IF('Zenergy-OE'!AF60=\"\",0,IF('Zenergy-OE'!AF60>0,'Zenergy-OE'!AF60,0))","v":0},{"$f":"'Zenergy-OE'!AH60","v":0},{"$f":"IF(EK24>1,VLOOKUP(IF(ISNUMBER(EK24),TEXT(EK24,\"0\"),EK24),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK24>1,VLOOKUP(IF(ISNUMBER(EK24),TEXT(EK24,\"0\"),EK24),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL24*EN24","v":0},null,null,"850+400",40185,50185,60185,70185,80185,90185,null,"850+400",40140,50140,60140,70140,80140,90140]
[null,"150+650+300",40380,50380,60380,70380,80380,90380,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,{"$f":"IF(AB1<AG1,AG1-AB1,0)","v":0},{"$f":"IF(AG1<AL1,AL1-AG1,0)","v":0},{"$f":"SUM(AD25:AE25)","v":0},{"$f":"IF(BA13>13,1,0)","v":0},null,{"$f":"IF(BM6<3,0,1)","v":1},{"$f":"IF(BJ6>4,0,1)","v":1},{"$f":"SUM(AI25:AI26)","v":1},null,null,{"$f":"INDEX(($AO$27:$AR$29),$BS$20,$BS$13)","v":1},"Cokół boki / pokrywa pole 2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 1000A\",\"Frame 1000A\")","v":"Rama 1000A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Boki wentylowane wraz z ramą\",\"\")","v":"Boki wentylowane wraz z ramą"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  6\",\"Quantity 6\")","v":"Ilość  6"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,1,null,null,null,null,null,null,null,null,null,{"$f":"SUM(CR15:CR23)","v":0},null,24,null,"Osł. przeszklona",{"$f":"IF(CW21=0,\"\",\"\")","v":""},{"$f":"IF(CX21=0,\"\",\"\")","v":""},32039,32049,{"$f":"IF(DA21=0,\"\",\"\")","v":""},32069,{"$f":"IF(DC21=0,\"\",\"\")","v":""},32079,{"$f":"IF(DE21=0,\"\",\"\")","v":""},32089,{"$f":"IF(DG21=0,\"\",\"\")","v":""},32099,null,"Izol. AlCubar / Cu 3P, doizolowanie pion, bok 400","","",20108,20108,20108,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(EB24=0,\"\",\"\")","v":""},"","","","","",null,null,null,{"$f":"IF('Zenergy-OE'!AF63=\"\",0,IF('Zenergy-OE'!AF63>0,'Zenergy-OE'!AF63,0))","v":0},{"$f":"'Zenergy-OE'!AH63","v":0},{"$f":"IF(EK25>1,VLOOKUP(IF(ISNUMBER(EK25),TEXT(EK25,\"0\"),EK25),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK25>1,VLOOKUP(IF(ISNUMBER(EK25),TEXT(EK25,\"0\"),EK25),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+300",40165,50165,60165,70165,80165,90165,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+400",40380,50380,60380,70380,80380,90380,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,41330,51330,61330,71330,81330,91330,null,null,null,null,null,{"$f":"AG1-1","v":0},{"$f":"AL1-1","v":0},{"$f":"SUM(AD26:AE26)","v":0},{"$f":"AF26-AF25-AG25","v":0},null,{"$f":"IF(BA15>1,1,0)","v":0},null,{"$f":"SUM(AI26+AJ25)","v":1},null,null,"Cokół","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 1200\",\"Frame 1200\")","v":"Rama 1200"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  7\",\"Quantity 7\")","v":"Ilość  7"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,1,null,null,null,null,null,null,null,null,null,null,null,25,null,"Szyna stała TS35",32000,32000,32000,32000,32000,32000,32000,32000,32000,32000,32000,32000,null,"Izol. AlCubar / Cu 4P, doizolowanie pion, bok 400","","",20109,20109,20109,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF66=\"\",0,IF('Zenergy-OE'!AF66>0,'Zenergy-OE'!AF66,0))","v":0},{"$f":"'Zenergy-OE'!AH66","v":0},{"$f":"IF(EK26>1,VLOOKUP(IF(ISNUMBER(EK26),TEXT(EK26,\"0\"),EK26),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK26>1,VLOOKUP(IF(ISNUMBER(EK26),TEXT(EK26,\"0\"),EK26),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+400",40165,50165,60165,70165,80165,90165,null,"150+650+400",40140,50140,60140,70140,80140,90140]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,41340,51340,61340,71340,81340,91340,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P.boki",3,1,1,3,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 1300\",\"Frame 1300\")","v":"Rama 1300"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  8\",\"Quantity 8\")","v":"Ilość  8"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,{"$f":"IF($BA$12>1,0,IF($BA$13>10,$BA$13-1,CH21))","v":1},null,null,null,null,null,null,null,null,null,null,null,26,null,"Szyna reg.TS35",32005,32005,32005,32005,32005,32005,32005,32005,32005,32005,32005,32005,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Podpora szyny AlCubar\",\"Free 3P insulator\")","v":"Podpora szyny AlCubar"},20070,20070,20070,20070,20070,{"$f":"IF(DP3=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,"Izol.3P tył poz.","Izol.4P tył poz.",null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF69=\"\",0,IF('Zenergy-OE'!AF69>0,'Zenergy-OE'!AF69,0))","v":0},{"$f":"'Zenergy-OE'!AH69","v":0},{"$f":"IF(EK27>1,VLOOKUP(IF(ISNUMBER(EK27),TEXT(EK27,\"0\"),EK27),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK27>1,VLOOKUP(IF(ISNUMBER(EK27),TEXT(EK27,\"0\"),EK27),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,null,null,null,null,null,null,null,null,"Wysokość","Cokół bok głębokość pełny",null,null,null,null,null,null,450,41345,51345,61345,71345,81345,91345,null,null,null,null,null,{"$f":"IF(BA13>23,1,0)","v":0},{"$f":"IF(AG1+AL1>2,1,0)","v":0},{"$f":"IF(BT94=0,0,1)","v":1},{"$f":"AE28+AF28-AD28","v":1},null,{"$f":"IF('Zenergy-OE'!AN32=31105,0,1)","v":1},{"$f":"IF('Zenergy-OE'!AN32=31205,0,1)","v":1},{"$f":"SUM(AI28:AJ28)","v":2},null,null,"Przepust",3,2,2,3,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A+650A\",\"Frame 650A+650A\")","v":"Rama 650A+650A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  9\",\"Quantity 9\")","v":"Ilość  9"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,"Płyta ocynk pełna",{"$f":"IF(CW21=0,\"\",\"\")","v":""},33042,33043,33044,33045,33046,{"$f":"IF(DC21=0,\"\",\"\")","v":""},33047,{"$f":"IF(DE21=0,\"\",\"\")","v":""},33048,{"$f":"IF(DG21=0,\"\",\"\")","v":""},33049,null,"Izol. AlCubar 630 1P, most poziomy, 200/230",20160,{"$f":"IF(DL27=0,\"\",\"\")","v":""},{"$f":"IF(DM27=0,\"\",\"\")","v":""},20160,{"$f":"IF(DO27=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(EB27=0,\"\",\"\")","v":""},{"$f":"IF(EC27=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF72=\"\",0,IF('Zenergy-OE'!AF72>0,'Zenergy-OE'!AF72,0))","v":0},{"$f":"'Zenergy-OE'!AH72","v":0},{"$f":"IF(EK28>1,VLOOKUP(IF(ISNUMBER(EK28),TEXT(EK28,\"0\"),EK28),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK28>1,VLOOKUP(IF(ISNUMBER(EK28),TEXT(EK28,\"0\"),EK28),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,null,null,null,null,null,null,null,null,null,230,300,400,600,800,null,null,600,41360,51360,61360,71360,81360,91360,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV32=31105,0,1)","v":1},{"$f":"IF('Zenergy-OE'!AV32=31205,0,1)","v":1},{"$f":"SUM(AI29:AJ29)","v":2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A+850A\",\"Frame 650A+850A\")","v":"Rama 650A+850A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,{"$f":"SUM(BS30:BS40)","v":0},null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  10\",\"Quantity 10\")","v":"Ilość  10"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,28,null,"Płyta malow.otw.",{"$f":"IF(CW21=0,\"\",\"\")","v":""},33542,33543,33544,33545,33546,{"$f":"IF(DC21=0,\"\",\"\")","v":""},33547,{"$f":"IF(DE21=0,\"\",\"\")","v":""},33548,{"$f":"IF(DG21=0,\"\",\"\")","v":""},33549,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 3P, most poziomy, 400\",\"Horizontal200 1P insul.\")","v":"Izol. AlCubar 630 3P, most poziomy, 400"},{"$f":"IF(DK28=0,\"\",\"\")","v":""},"",20163,20163,20163,null,null,null,null,null,null,null,null,null,null,null,null,31703,31704,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF75=\"\",0,IF('Zenergy-OE'!AF75>0,'Zenergy-OE'!AF75,0))","v":0},{"$f":"'Zenergy-OE'!AH75","v":0},{"$f":"IF(EK29>1,VLOOKUP(IF(ISNUMBER(EK29),TEXT(EK29,\"0\"),EK29),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK29>1,VLOOKUP(IF(ISNUMBER(EK29),TEXT(EK29,\"0\"),EK29),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Szerokość obudowy","Rama osłon na zawiasach do plomb.  Wysokość, Pole 1,3",null,null,null,3,null,null,"Szerokość obudowy","Rama osłon na zawiasach do plomb.  Wysokość, Pole 2",null,null,null,3]
[null,"Szerokość obudowy","Drzwi wentylowane IP30 Wysokość",null,null,2,null,"Pole 1,3",null,"Brak",{"$f":"IF(K29=0,\"\",\"\")","v":""},{"$f":"IF(L29=0,\"\",\"\")","v":""},{"$f":"IF(M29=0,\"\",\"\")","v":""},{"$f":"IF(N29=0,\"\",\"\")","v":""},{"$f":"IF(O29=0,\"\",\"\")","v":""},null,null,650,41365,51365,61365,71365,81365,91365,null,null,null,null,null,null,{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF(BA13>10,2,0)","v":0},{"$f":"SUM(AE30:AF30)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 850A+850A\",\"Frame 850A+850A\")","v":"Rama 850A+850A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,{"$f":"IF(BV20=1,5,0)","v":0},1,null,1,1,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  11\",\"Quantity 11\")","v":"Ilość  11"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,"Akc.szerokość",null,null,null,null,null,null,null,null,null,null,29,null,"Płyta oc. pozioma",33741,33742,33743,33744,33745,33746,33747,33748,null,33749,{"$f":"IF(DG20=0,\"\",\"\")","v":""},{"$f":"IF(DH20=0,\"\",\"\")","v":""},null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 4P, most poziomy, 400\",\"Horizontal200 1P insul.\")","v":"Izol. AlCubar 630 4P, most poziomy, 400"},"","",20164,20164,20164,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF78=\"\",0,IF('Zenergy-OE'!AF78>0,'Zenergy-OE'!AF78,0))","v":0},{"$f":"'Zenergy-OE'!AH78","v":0},{"$f":"IF(EK30>1,VLOOKUP(IF(ISNUMBER(EK30),TEXT(EK30,\"0\"),EK30),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK30>1,VLOOKUP(IF(ISNUMBER(EK30),TEXT(EK30,\"0\"),EK30),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL30*EN30","v":0},null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,100,30023,30033,30043,30063,30083,null,null,800,41380,51380,61380,71380,81380,91380,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BA12>1,1,0)","v":0},{"$f":"IF('Zenergy-OE'!AF32<31200,1,0)","v":1},{"$f":"SUM(AI31:AJ31)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A+300\",\"Frame 650A+300\")","v":"Rama 650A+300"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,{"$f":"IF(BV20=2,4,0)","v":0},2,null,1,"Akcesoria głęb.",null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  12\",\"Quantity 12\")","v":"Ilość  12"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,null,null,null,null,null,null,null,null,null,30,null,"Płyta licznikowa",33204,33204,33204,33204,33204,33204,33204,33204,33204,33204,33204,33204,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 3P, doizolowanie poz.400\",\"Free 3P insulator\")","v":"Izol. AlCubar 630 3P, doizolowanie poz.400"},"","",20168,20168,20168,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF81=\"\",0,IF('Zenergy-OE'!AF81>0,'Zenergy-OE'!AF81,0))","v":0},{"$f":"'Zenergy-OE'!AH81","v":0},{"$f":"IF(EK31>1,VLOOKUP(IF(ISNUMBER(EK31),TEXT(EK31,\"0\"),EK31),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK31>1,VLOOKUP(IF(ISNUMBER(EK31),TEXT(EK31,\"0\"),EK31),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C31=0,\"\",\"\")","v":""},"","","","","",null,200,30123,30133,30143,30163,30183,null,null,"650+150",41380,51380,61380,71380,81380,91380,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO34:$AR36),$BS$21,$BS$13)","v":1},"Cokół boki / pokrywa pole 3",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 650A+400A\",\"Frame 650A+400A\")","v":"Rama 650A+400A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,{"$f":"IF(BV20=3,3,0)","v":0},3,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  13\",\"Quantity 13\")","v":"Ilość  13"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P, most pionowy na plecach\",\"Rear 3P vertical busbar support\")","v":"Izolator 3P, most pionowy na plecach"},null,null,null,null,null,null,null,null,null,null,31,null,null,{"$f":"IF(CW21=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 4P, doizolowanie poz.400\",\"Free 3P insulator\")","v":"Izol. AlCubar 630 4P, doizolowanie poz.400"},"","",20169,20169,20169,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF84=\"\",0,IF('Zenergy-OE'!AF84>0,'Zenergy-OE'!AF84,0))","v":0},{"$f":"'Zenergy-OE'!AH84","v":0},{"$f":"IF(EK32>1,VLOOKUP(IF(ISNUMBER(EK32),TEXT(EK32,\"0\"),EK32),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK32>1,VLOOKUP(IF(ISNUMBER(EK32),TEXT(EK32,\"0\"),EK32),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,40230,50230,60230,70230,80230,90230,null,"Pokr. Pełna",{"$f":"IF(K32=0,\"\",\"\")","v":""},{"$f":"IF(L32=0,\"\",\"\")","v":""},{"$f":"IF(M32=0,\"\",\"\")","v":""},{"$f":"IF(N32=0,\"\",\"\")","v":""},{"$f":"IF(O32=0,\"\",\"\")","v":""},null,null,850,41385,51385,61385,71385,81385,91385,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cokół","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 850A+300\",\"Frame 850A+300\")","v":"Rama 850A+300"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,{"$f":"IF(BV20=4,2,0)","v":0},4,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Wspornik płyt montażowych, boczny 200/230\",\"Side support for mounting plates D200/230\")","v":"Wspornik płyt montażowych, boczny 200/230"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  14\",\"Quantity 14\")","v":"Ilość  14"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 4P, most pionowy na plecach\",\"Rear 4P vertical busbar support\")","v":"Izolator 4P, most pionowy na plecach"},null,null,null,null,null,null,null,null,null,null,32,null,null,{"$f":"IF(CW21=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar 630 1P, most pionowy, 200/230","","",{"$f":"IF(DM32=0,\"\",\"\")","v":""},20151,{"$f":"IF(DO32=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF87=\"\",0,IF('Zenergy-OE'!AF87>0,'Zenergy-OE'!AF87,0))","v":0},{"$f":"'Zenergy-OE'!AH87","v":0},{"$f":"IF(EK33>1,VLOOKUP(IF(ISNUMBER(EK33),TEXT(EK33,\"0\"),EK33),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK33>1,VLOOKUP(IF(ISNUMBER(EK33),TEXT(EK33,\"0\"),EK33),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,400,40141,50141,60141,70141,80141,90141,null,400,40141,50141,60141,70141,80141,90141]
[null,400,40240,50240,60240,70240,80240,90240,null,null,null,null,null,null,null,null,null,"650+200",41385,51385,61385,71385,81385,91385,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF32=\"\",0,1)","v":1},{"$f":"IF('Zenergy-OE'!AN12=\"\",0,1)","v":0},{"$f":"SUM(AI34:AJ34)","v":1},null,null,"P.boki",3,1,1,3,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 850A+400A\",\"Frame 850A+400A\")","v":"Rama 850A+400A"},null,null,null,null,null,null,null,1,0,null,1,null,null,1,null,null,{"$f":"IF(BV20=5,1,0)","v":0},5,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Wspornik płyt montażowych, boczny 400\",\"Side support for mounting plates D400\")","v":"Wspornik płyt montażowych, boczny 400"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  15\",\"Quantity 15\")","v":"Ilość  15"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P, most pion. na plecach reg.\",\"Rear 3P vertical busbar support regulated\")","v":"Izolator 3P, most pion. na plecach reg."},null,null,null,null,null,null,null,null,null,null,33,null,null,{"$f":"IF(CW21=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar 630 3P, most pionowy z boku","","",20153,20153,20153,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF90=\"\",0,IF('Zenergy-OE'!AF90>0,'Zenergy-OE'!AF90,0))","v":0},{"$f":"'Zenergy-OE'!AH90","v":0},{"$f":"IF(EK34>1,VLOOKUP(IF(ISNUMBER(EK34),TEXT(EK34,\"0\"),EK34),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK34>1,VLOOKUP(IF(ISNUMBER(EK34),TEXT(EK34,\"0\"),EK34),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,450,40146,50146,60146,70146,80146,90146,null,450,40146,50146,60146,70146,80146,90146]
[null,450,40245,50245,60245,70245,80245,90245,null,"Wysokość","Cokół bok głębokość przepust",null,null,null,null,null,null,1000,41310,51310,61310,71310,81310,91310,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF32=\"\",0,1)","v":1},{"$f":"IF('Zenergy-OE'!AV12=\"\",0,1)","v":0},{"$f":"SUM(AI35:AJ35)","v":1},null,null,"Przepust",3,2,2,3,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 150+650A+300\",\"Frame 150+650A+300\")","v":"Rama 150+650A+300"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV20=6,0,0)","v":0},6,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Uchwyt płyt montażowych\",\"Plates grip for side support\")","v":"Uchwyt płyt montażowych"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  16\",\"Quantity 16\")","v":"Ilość  16"},null,{"$f":"IF(CE40=14,14,IF(CP37=1,$BA$15,CB40))","v":1},null,null,{"$f":"IF(CP37=1,BD4,CE40)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 4P, most pion. na plecach reg.\",\"Rear 4P vertical busbar support regulated\")","v":"Izolator 4P, most pion. na plecach reg."},null,null,null,null,{"$f":"IF(CE4>12,1,0)","v":1},{"$f":"IF(CE5>12,1,0)","v":0},{"$f":"IF(CE6>12,1,0)","v":0},{"$f":"IF($CE$4=13,14,IF($CE$4=14,14,$CQ$1))","v":14},{"$f":"IF($CE$5=13,14,IF($CE$5=14,14,$CR$1))","v":11},{"$f":"IF($CE$6=13,14,IF($CE$6=14,14,$CS$1))","v":11},34,null,null,{"$f":"IF(CW21=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Izol. AlCubar 630 4P, most pionowy z boku","","",20154,20154,20154,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF93=\"\",0,IF('Zenergy-OE'!AF93>0,'Zenergy-OE'!AF93,0))","v":0},{"$f":"'Zenergy-OE'!AH93","v":0},{"$f":"IF(EK35>1,VLOOKUP(IF(ISNUMBER(EK35),TEXT(EK35,\"0\"),EK35),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK35>1,VLOOKUP(IF(ISNUMBER(EK35),TEXT(EK35,\"0\"),EK35),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,600,40260,50260,60260,70260,80260,90260,null,null,230,300,400,600,800,null,null,1200,41312,51312,61312,71312,81312,91312,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Rama 150+650A+400A\",\"Frame 150+650A+400A\")","v":"Rama 150+650A+400A"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV20=7,-1,0)","v":0},7,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar / Cu 1P most poziomy 200/230\",\"Horizontal AlCubar / Cu 1P busbar support D200/230\")","v":"Izolator AlCubar / Cu 1P most poziomy 200/230"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  17\",\"Quantity 17\")","v":"Ilość  17"},null,{"$f":"IF(CE39=14,25,IF(CO37=1,$BA$12,CB39))","v":1},null,null,{"$f":"IF(CO37=1,BD4,CE39)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. 3P, podpora mostu na plecach, reg.\",\"Rear 3P vert. busbar bottom support regulated\")","v":"Izol. 3P, podpora mostu na plecach, reg."},null,null,null,null,{"$f":"IF(CE21>12,1,0)","v":0},{"$f":"IF(CE22>12,1,0)","v":0},{"$f":"IF(CE23>12,1,0)","v":0},{"$f":"IF($CE$21=13,14,IF($CE$21=14,14,$CQ$1))","v":5},{"$f":"IF($CE$22=13,14,IF($CE$22=14,14,$CR$1))","v":11},11,35,null,null,{"$f":"IF(CW21=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P,rozstaw 60 mm z plytą montażową\",\"\")","v":"Izolator 3P,rozstaw 60 mm z plytą montażową"},36020,36020,36020,36020,36020,{"$f":"IF(DP29=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pole 2",{"$f":"IF('Zenergy-OE'!AN12=\"\",0,IF('Zenergy-OE'!AN12>0,'Zenergy-OE'!AN12,0))","v":0},{"$f":"IF('Zenergy-OE'!AP12=\"\",0,'Zenergy-OE'!AP12)","v":0},{"$f":"IF(EK36>1,VLOOKUP(IF(ISNUMBER(EK36),TEXT(EK36,\"0\"),EK36),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK36>1,VLOOKUP(IF(ISNUMBER(EK36),TEXT(EK36,\"0\"),EK36),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,650,40166,50166,60166,70166,80166,90166,null,650,40166,50166,60166,70166,80166,90166]
[null,650,40265,50265,60265,70265,80265,90265,null,"Brak",{"$f":"IF(K36=0,\"\",\"\")","v":""},{"$f":"IF(L36=0,\"\",\"\")","v":""},{"$f":"IF(M36=0,\"\",\"\")","v":""},{"$f":"IF(N36=0,\"\",\"\")","v":""},{"$f":"IF(O36=0,\"\",\"\")","v":""},null,null,1300,41313,51313,61313,71313,81313,91313,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV20=8,-2,0)","v":0},8,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar / Cu 3P most poziomy 400\",\"Horizontal AlCubar / Cu 3P busbar support D400\")","v":"Izolator AlCubar / Cu 3P most poziomy 400"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  18\",\"Quantity 18\")","v":"Ilość  18"},null,{"$f":"IF(CE38=14,23,IF(CN37=1,$BA$13,CB38))","v":1},null,null,{"$f":"IF(CN37=1,BD4,CE38)","v":1},null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. 4P, podpora mostu na plecach, reg.\",\"Rear 4P vert. busbar bottom support regulated\")","v":"Izol. 4P, podpora mostu na plecach, reg."},null,null,null,null,{"$f":"IF(CE38>12,1,0)","v":0},{"$f":"IF(CE39>12,1,0)","v":0},{"$f":"IF(CE40>12,1,0)","v":0},{"$f":"IF($CE$38=13,14,IF($CE$38=14,14,$CQ$1))","v":5},{"$f":"IF($CE$39=13,14,IF($CE$39=14,14,$CR$1))","v":11},11,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P,rozstaw 100 mm z plytą montażową\",\"\")","v":"Izolator 3P,rozstaw 100 mm z plytą montażową"},36030,36030,36030,36030,36030,{"$f":"IF(DP36=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN15=\"\",0,IF('Zenergy-OE'!AN15>0,'Zenergy-OE'!AN15,0))","v":0},{"$f":"IF('Zenergy-OE'!AP15=\"\",0,'Zenergy-OE'!AP15)","v":0},{"$f":"IF(EK37>1,VLOOKUP(IF(ISNUMBER(EK37),TEXT(EK37,\"0\"),EK37),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK37>1,VLOOKUP(IF(ISNUMBER(EK37),TEXT(EK37,\"0\"),EK37),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,800,40280,50280,60280,70280,80280,90280,null,100,30100,30100,30100,30100,30100,null,null,"650+650",41365,51365,61365,71365,81365,91365,null,{"$f":"IF('Zenergy-OE'!AF42=\"\",0,1)","v":1},{"$f":"IF('Zenergy-OE'!AF42>40000,1,0)","v":1},{"$f":"SUM(Z38:AA38)","v":2},null,null,{"$f":"IF('Zenergy-OE'!AN42=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN42>40000,1,0)","v":1},{"$f":"SUM(AE38:AF38)","v":1},null,{"$f":"IF('Zenergy-OE'!AV42=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV42>40000,1,0)","v":1},{"$f":"SUM(AI38:AJ38)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV20=9,-3,0)","v":0},9,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar / Cu 4P most poziomy 400\",\"Horizontal AlCubar / Cu 4P busbar support D400\")","v":"Izolator AlCubar / Cu 4P most poziomy 400"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  19\",\"Quantity 19\")","v":"Ilość  19"},null,1,3,null,1,3,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630A 3P pionowo na plecach\",\"Rear 3P AlCubar 630A vertical busbar support\")","v":"Izol. AlCubar 630A 3P pionowo na plecach"},null,null,null,null,{"$f":"IF(CE55>12,1,0)","v":0},{"$f":"IF(CE56>12,1,0)","v":0},{"$f":"IF(CE57>12,1,0)","v":0},{"$f":"IF($CE$55=13,14,IF($CE$55=14,14,$CQ$1))","v":5},{"$f":"IF($CE$56=13,14,IF($CE$56=14,14,$CR$1))","v":11},11,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P,rozstaw 185 mm z plytą montażową\",\"\")","v":"Izolator 3P,rozstaw 185 mm z plytą montażową"},36010,36010,36010,36010,36010,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN18=\"\",0,IF('Zenergy-OE'!AN18>0,'Zenergy-OE'!AN18,0))","v":0},{"$f":"IF('Zenergy-OE'!AP18=\"\",0,'Zenergy-OE'!AP18)","v":0},{"$f":"IF(EK38>1,VLOOKUP(IF(ISNUMBER(EK38),TEXT(EK38,\"0\"),EK38),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK38>1,VLOOKUP(IF(ISNUMBER(EK38),TEXT(EK38,\"0\"),EK38),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+150",40166,50166,60166,70166,80166,90166,null,"650+150",40166,50166,60166,70166,80166,90166]
[null,"650+150",40280,50280,60280,70280,80280,90280,null,200,30000,30000,30000,30000,30000,null,null,"650+850",41365,51365,61365,71365,81365,91365,null,{"$f":"IF('Zenergy-OE'!AF45=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF45>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN45=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN45>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV45=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV45>40000,1,0)","v":1},1,null,null,{"$f":"INDEX(($AO41:$AR43),$BS$21,$BS$13)","v":1},"Cokół boki / pokrywa pole 4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV20=10,-4,0)","v":0},10,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 1P, łącznik, poziom, 200/230\",\"Horizontal AlCubar 1P busbar support D200/230 for Cu link\")","v":"Izolator AlCubar 1P, łącznik, poziom, 200/230"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  20\",\"Quantity 20\")","v":"Ilość  20"},null,1,"Osłony",null,1,"Ilość mod.",null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630A 4P pionowo na plecach\",\"Rear 4P AlCubar 630A vertical busbar support\")","v":"Izol. AlCubar 630A 4P pionowo na plecach"},null,null,null,null,{"$f":"IF(CE72>12,1,0)","v":0},{"$f":"IF(CE73>12,1,0)","v":0},{"$f":"IF(CE74>12,1,0)","v":0},{"$f":"IF($CE$72=13,14,IF($CE$72=14,14,$CQ$1))","v":5},{"$f":"IF($CE$73=13,14,IF($CE$73=14,14,$CR$1))","v":11},11,38,null,"W 450 - 3","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Wspornik szyny PE\",\"PE Support\")","v":"Wspornik szyny PE"},31930,31930,31930,31930,31930,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN21=\"\",0,IF('Zenergy-OE'!AN21>0,'Zenergy-OE'!AN21,0))","v":0},{"$f":"IF('Zenergy-OE'!AP21=\"\",0,'Zenergy-OE'!AP21)","v":0},{"$f":"IF(EK39>1,VLOOKUP(IF(ISNUMBER(EK39),TEXT(EK39,\"0\"),EK39),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK39>1,VLOOKUP(IF(ISNUMBER(EK39),TEXT(EK39,\"0\"),EK39),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,850,40186,50186,60186,70186,80186,90186,null,850,40186,50186,60186,70186,80186,90186]
[null,850,40285,50285,60285,70285,80285,90285,null,"Pokr. Pełna",{"$f":"IF(K39=0,\"\",\"\")","v":""},{"$f":"IF(L39=0,\"\",\"\")","v":""},{"$f":"IF(M39=0,\"\",\"\")","v":""},{"$f":"IF(N39=0,\"\",\"\")","v":""},{"$f":"IF(O39=0,\"\",\"\")","v":""},null,null,"850+850",41385,51385,61385,71385,81385,91385,null,{"$f":"IF('Zenergy-OE'!AF48=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF48>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN48=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN48>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV48=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV48>40000,1,0)","v":1},1,null,null,"Cokół","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV20=11,-5,0)","v":0},11,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 3P, łącznik, poziom, 400\",\"Horizontal AlCubar 3P busbar support D400 for Cu link\")","v":"Izolator AlCubar 3P, łącznik, poziom, 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  21\",\"Quantity 21\")","v":"Ilość  21"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa na plecach\",\"Cable tray\")","v":"Drabinka kablowa na plecach"},null,null,null,null,{"$f":"IF(CE89>12,1,0)","v":0},{"$f":"IF(CE90>12,1,0)","v":0},{"$f":"IF(CE91>12,1,0)","v":0},{"$f":"IF($CE$89=13,14,IF($CE$89=14,14,$CQ$1))","v":5},{"$f":"IF($CE$90=13,14,IF($CE$90=14,14,$CR$1))","v":11},11,39,null,"Brak",{"$f":"IF(CW39=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Drabinka kablowa 200/230",33171,{"$f":"IF(DL39=0,\"\",\"\")","v":""},{"$f":"IF(DM39=0,\"\",\"\")","v":""},33171,33171,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN24=\"\",0,IF('Zenergy-OE'!AN24>0,'Zenergy-OE'!AN24,0))","v":0},{"$f":"IF('Zenergy-OE'!AP24=\"\",0,'Zenergy-OE'!AP24)","v":0},{"$f":"IF(EK40>1,VLOOKUP(IF(ISNUMBER(EK40),TEXT(EK40,\"0\"),EK40),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK40>1,VLOOKUP(IF(ISNUMBER(EK40),TEXT(EK40,\"0\"),EK40),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+200",40166,50166,60166,70166,80166,90166,null,"650+200",40166,50166,60166,70166,80166,90166]
[null,"650+200",40285,50285,60285,70285,80285,90285,null,null,null,null,null,null,null,null,null,"650+300",41395,51395,61395,71395,81395,91395,null,{"$f":"IF('Zenergy-OE'!AF51=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF51>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN51=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN51>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV51=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV51>40000,1,0)","v":1},1,null,null,"P.boki",3,1,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 4P, łącznik, poziom, 400\",\"Horizontal AlCubar 4P busbar support D400 for Cu link\")","v":"Izolator AlCubar 4P, łącznik, poziom, 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  22\",\"Quantity 22\")","v":"Ilość  22"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE39<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa na drzwiach\",\"Door cable tray\")","v":"Drabinka kablowa na drzwiach"},null,null,null,null,{"$f":"IF(CE106>12,1,0)","v":0},{"$f":"IF(CE107>12,1,0)","v":0},{"$f":"IF(CE108>12,1,0)","v":0},{"$f":"IF($CE$106=13,14,IF($CE$106=14,14,$CQ$1))","v":5},{"$f":"IF($CE$107=13,14,IF($CE$107=14,14,$CR$1))","v":11},11,40,null,"Osłona pełna",32510,32520,32530,32540,32550,32560,32570,32580,32590,32591,32592,32593,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa 400\",\"Cable tray 400\")","v":"Drabinka kablowa 400"},33172,33173,33174,33174,33174,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN25=\"\",0,IF('Zenergy-OE'!AN25>0,'Zenergy-OE'!AN25,0))","v":0},{"$f":"IF('Zenergy-OE'!AP25=\"\",0,'Zenergy-OE'!AP25)","v":0},{"$f":"IF(EK41>1,VLOOKUP(IF(ISNUMBER(EK41),TEXT(EK41,\"0\"),EK41),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK41>1,VLOOKUP(IF(ISNUMBER(EK41),TEXT(EK41,\"0\"),EK41),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1000,40111,50111,60111,70111,80111,90111,null,1000,40111,50111,60111,70111,80111,90111]
[null,1000,40210,50210,60210,70210,80210,90210,null,"Wysokość","Cokół bok głębokość",null,null,null,null,null,null,"650+400",41311,51311,61311,71311,81311,91311,null,{"$f":"IF('Zenergy-OE'!AF54=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF54>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN54=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN54>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV54=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV54>40000,1,0)","v":1},1,null,null,"Przepust",3,2,2,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar / Cu 3P, doizolowanie poz. 400\",\"AlCubar / Cu 3P free busbar support D400\")","v":"Izol. AlCubar / Cu 3P, doizolowanie poz. 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  23\",\"Quantity 23\")","v":"Ilość  23"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa pod osłonę\",\"Front plate cable tray\")","v":"Drabinka kablowa pod osłonę"},null,null,null,null,{"$f":"IF(CE123>12,1,0)","v":0},{"$f":"IF(CE124>12,1,0)","v":0},{"$f":"IF(CE125>12,1,0)","v":0},{"$f":"IF($CE$123=13,14,IF($CE$123=14,14,$CQ$1))","v":5},{"$f":"IF($CE$124=13,14,IF($CE$124=14,14,$CR$1))","v":11},11,null,null,"Osł. modułowa",{"$f":"IF(CW39=0,\"\",\"\")","v":""},32525,32535,32545,32555,{"$f":"IF(DB41=0,\"\",\"\")","v":""},"","","","","","",null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Przepust membranowy IP55\",\"\")","v":"Przepust membranowy IP55"},31935,31935,31935,31935,31935,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN28=\"\",0,IF('Zenergy-OE'!AN28>0,'Zenergy-OE'!AN28,0))","v":0},{"$f":"IF('Zenergy-OE'!AP28=\"\",0,'Zenergy-OE'!AP28)","v":0},{"$f":"IF(EK42>1,VLOOKUP(IF(ISNUMBER(EK42),TEXT(EK42,\"0\"),EK42),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK42>1,VLOOKUP(IF(ISNUMBER(EK42),TEXT(EK42,\"0\"),EK42),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1200,40212,50212,60212,70212,80212,90212,null,null,230,300,400,600,800,null,null,"850+300",41385,51385,61385,71385,81385,91385,null,{"$f":"IF('Zenergy-OE'!AF57=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF57>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN57=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN57>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV57=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV57>40000,1,0)","v":1},1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar / Cu 4P, doizolowanie poz. 400\",\"AlCubar / Cu 4P free busbar support D400\")","v":"Izol. AlCubar / Cu 4P, doizolowanie poz. 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  24\",\"Quantity 24\")","v":"Ilość  24"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Metalowa kieszeń na dokumentację\",\"Drawing holder\")","v":"Metalowa kieszeń na dokumentację"},null,null,null,null,{"$f":"IF(CE140>12,1,0)","v":0},{"$f":"IF(CE141>12,1,0)","v":0},{"$f":"IF(CE142>12,1,0)","v":0},{"$f":"IF($CE$4100=13,14,IF($CE$140=14,14,$CQ$1))","v":5},{"$f":"IF($CE$141=13,14,IF($CE$141=14,14,$CR$1))","v":11},11,null,null,"Osł. przeszklona",{"$f":"IF(CW39=0,\"\",\"\")","v":""},{"$f":"IF(CX39=0,\"\",\"\")","v":""},32539,32549,{"$f":"IF(DA39=0,\"\",\"\")","v":""},32569,{"$f":"IF(DC39=0,\"\",\"\")","v":""},32579,{"$f":"IF(DE39=0,\"\",\"\")","v":""},32589,{"$f":"IF(DG39=0,\"\",\"\")","v":""},32599,null,"Kratka wentylacyjna 160x160",31940,31940,31940,31940,31940,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN29=\"\",0,IF('Zenergy-OE'!AN29>0,'Zenergy-OE'!AN29,0))","v":0},{"$f":"IF('Zenergy-OE'!AP29=\"\",0,'Zenergy-OE'!AP29)","v":0},{"$f":"IF(EK43>1,VLOOKUP(IF(ISNUMBER(EK43),TEXT(EK43,\"0\"),EK43),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK43>1,VLOOKUP(IF(ISNUMBER(EK43),TEXT(EK43,\"0\"),EK43),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1300,40213,50213,60213,70213,80213,90213,null,"Brak",{"$f":"IF(K43=0,\"\",\"\")","v":""},"","","","",null,null,"850+400",41385,51385,61385,71385,81385,91385,null,{"$f":"IF('Zenergy-OE'!AF60=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF60>40000,1,0)","v":1},{"$f":"SUM(Z44:AA44)","v":1},null,null,{"$f":"IF('Zenergy-OE'!AN60=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN60>40000,1,0)","v":1},{"$f":"SUM(AE44:AF44)","v":1},null,{"$f":"IF('Zenergy-OE'!AV60=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV60>40000,1,0)","v":1},{"$f":"SUM(AI44:AJ44)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator Cu 1P, most poziomy na plecach\",\"Rear Horizontal Cu 1P busbar support\")","v":"Izolator Cu 1P, most poziomy na plecach"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  25\",\"Quantity 25\")","v":"Ilość  25"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Pionowy zestaw szyn TS35, 6M\",\"6-Modules Vertical DIN-rail for terminals\")","v":"Pionowy zestaw szyn TS35, 6M"},null,null,null,null,{"$f":"IF(CE157>12,1,0)","v":0},{"$f":"IF(CE158>12,1,0)","v":0},{"$f":"IF(CE159>12,1,0)","v":0},{"$f":"IF($CE$157=13,14,IF($CE$157=14,14,$CQ$1))","v":5},{"$f":"IF($CE$158=13,14,IF($CE$158=14,14,$CR$1))","v":11},11,null,null,"Szyna stała TS35",32500,32500,32500,32500,32500,32500,32500,32500,32500,32500,32500,32500,null,"Kratka wentylacyjna 230x230",31941,31941,31941,31941,31941,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN32=\"\",0,IF('Zenergy-OE'!AN32>0,'Zenergy-OE'!AN32,0))","v":0},{"$f":"IF('Zenergy-OE'!AP32=\"\",0,'Zenergy-OE'!AP32)","v":0},{"$f":"IF(EK44>1,VLOOKUP(IF(ISNUMBER(EK44),TEXT(EK44,\"0\"),EK44),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK44>1,VLOOKUP(IF(ISNUMBER(EK44),TEXT(EK44,\"0\"),EK44),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+650",40166,50166,60166,70166,80166,90166,null,"650+650",40166,50166,60166,70166,80166,90166]
[null,"650+612",40265,50265,60265,70265,80265,90265,null,100,"","","","","",null,null,"650+150+300",41380,51380,61380,71380,81380,91380,null,{"$f":"IF('Zenergy-OE'!AF63=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF63>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN63=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN63>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV63=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV63>40000,1,0)","v":1},1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator Cu 3P, most poziomy na plecach\",\"Rear Horizontal Cu 3P busbar support\")","v":"Izolator Cu 3P, most poziomy na plecach"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  26\",\"Quantity 26\")","v":"Ilość  26"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Poziomy zestaw dwóch szyn TS35\",\"Horizontal double DIN-rail for terminals\")","v":"Poziomy zestaw dwóch szyn TS35"},null,null,null,null,{"$f":"IF(CE174>12,1,0)","v":0},{"$f":"IF(CE175>12,1,0)","v":0},{"$f":"IF(CE176>12,1,0)","v":0},{"$f":"IF($CE$4134=13,14,IF($CE$174=14,14,$CQ$1))","v":5},{"$f":"IF($CE$175=13,14,IF($CE$175=14,14,$CR$1))","v":11},11,null,null,"Szyna reg.TS35",32505,32505,32505,32505,32505,32505,32505,32505,32505,32505,32505,32505,null,"Przyłącza kablowe w przedziale 3P 250A",{"$f":"IF(DK26=0,\"\",\"\")","v":""},{"$f":"IF(DL26=0,\"\",\"\")","v":""},33100,33100,33100,{"$f":"IF(DP26=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN33=\"\",0,IF('Zenergy-OE'!AN33>0,'Zenergy-OE'!AN33,0))","v":0},{"$f":"IF('Zenergy-OE'!AP33=\"\",0,'Zenergy-OE'!AP33)","v":0},{"$f":"IF(EK45>1,VLOOKUP(IF(ISNUMBER(EK45),TEXT(EK45,\"0\"),EK45),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK45>1,VLOOKUP(IF(ISNUMBER(EK45),TEXT(EK45,\"0\"),EK45),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+850",40166,50166,60166,70166,80166,90166,null,"650+850",40186,50186,60186,70186,80186,90186]
[null,"650+812",40265,50265,60265,70265,80265,90265,null,200,"","","","","",null,null,"650+150+400",41380,51380,61380,71380,81380,91380,null,{"$f":"IF('Zenergy-OE'!AF66=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF66>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN66=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN66>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV66=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV66>40000,1,0)","v":1},1,null,null,{"$f":"INDEX(($AO48:$AR50),$BS$21,$BS$13)","v":1},"Cokół boki / pokrywa pole 5",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator Cu 4P, most poziomy na plecach\",\"Rear Horizontal Cu 4P busbar support\")","v":"Izolator Cu 4P, most poziomy na plecach"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  27\",\"Quantity 27\")","v":"Ilość  27"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Osłona mostu poziomego\",\"Horizontal busbar cover\")","v":"Osłona mostu poziomego"},null,null,null,null,{"$f":"IF(CE191>12,1,0)","v":0},{"$f":"IF(CE192>12,1,0)","v":0},{"$f":"IF(CE193>12,1,0)","v":0},{"$f":"IF($CE$4151=13,14,IF($CE$191=14,14,$CQ$1))","v":5},{"$f":"IF($CE$192=13,14,IF($CE$192=14,14,$CR$1))","v":11},11,null,null,"Płyta ocynk pełna",{"$f":"IF(CW39=0,\"\",\"\")","v":""},33052,33053,33054,33055,33056,{"$f":"IF(DC39=0,\"\",\"\")","v":""},33057,{"$f":"IF(DE39=0,\"\",\"\")","v":""},33058,{"$f":"IF(DG39=0,\"\",\"\")","v":""},33059,null,"Przyłącza kablowe w przedziale 4P 250A",{"$f":"IF(DK45=0,\"\",\"\")","v":""},"",33101,33101,33101,{"$f":"IF(DP45=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN36=\"\",0,IF('Zenergy-OE'!AN36>0,'Zenergy-OE'!AN36,0))","v":0},{"$f":"IF('Zenergy-OE'!AP36=\"\",0,'Zenergy-OE'!AP36)","v":0},{"$f":"IF(EK46>1,VLOOKUP(IF(ISNUMBER(EK46),TEXT(EK46,\"0\"),EK46),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK46>1,VLOOKUP(IF(ISNUMBER(EK46),TEXT(EK46,\"0\"),EK46),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+850",40186,50186,60186,70186,80186,90186,null,"850+850",40186,50186,60186,70186,80186,90186]
[null,"850+812",40285,50285,60285,70285,80285,90285,null,"Pokr. Pełna","","","","","",null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AF69=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF69>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN69=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN69>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV69=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV69>40000,1,0)","v":1},1,null,null,"Cokół","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 1P most pion z boku 200/230\",\"Vertical AlCubar / Cu 1P busbar support D200/230\")","v":"Izolator AlCubar 1P most pion z boku 200/230"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  28\",\"Quantity 28\")","v":"Ilość  28"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zestaw mocowania do ściany\",\"Zenergy cabinet wall sling rail\")","v":"Zestaw mocowania do ściany"},null,null,null,null,null,null,null,null,null,null,null,null,"Płyta malow.otw.",{"$f":"IF(CW39=0,\"\",\"\")","v":""},33552,33553,33554,33555,33556,{"$f":"IF(DC39=0,\"\",\"\")","v":""},33557,{"$f":"IF(DE39=0,\"\",\"\")","v":""},33558,{"$f":"IF(DG39=0,\"\",\"\")","v":""},33559,null,"Przyłącza kablowe w przedziale 3P 630A","","",33102,33102,33102,{"$f":"IF(DP46=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN39=\"\",0,IF('Zenergy-OE'!AN39>0,'Zenergy-OE'!AN39,0))","v":0},{"$f":"IF('Zenergy-OE'!AP39=\"\",0,'Zenergy-OE'!AP39)","v":0},{"$f":"IF(EK47>1,VLOOKUP(IF(ISNUMBER(EK47),TEXT(EK47,\"0\"),EK47),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK47>1,VLOOKUP(IF(ISNUMBER(EK47),TEXT(EK47,\"0\"),EK47),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+300",40166,50166,60166,70166,80166,90166,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+300",40265,50265,60265,70265,80265,90265,null,null,null,null,null,null,null,null,null,"Szerokość obudowy","Osłona tylna pełna IP30   Wysokość",null,null,4,null,"Pole 1,3",null,{"$f":"IF('Zenergy-OE'!AF72=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF72>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN72=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN72>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV72=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV72>40000,1,0)","v":1},1,null,null,"P.boki",3,1,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 3P most pionowy z boku 400\",\"Vertical AlCubar / Cu 3P busbar support D400\")","v":"Izolator AlCubar 3P most pionowy z boku 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  29\",\"Quantity 29\")","v":"Ilość  29"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta oc. pozioma",33751,33752,33753,33754,33755,33756,33757,33758,null,33759,{"$f":"IF(DG257=0,\"\",\"\")","v":""},{"$f":"IF(DH257=0,\"\",\"\")","v":""},null,"Przyłącza kablowe w przedziale 4P 630A","","",33103,33103,33103,{"$f":"IF(DP47=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN42=\"\",0,IF('Zenergy-OE'!AN42>0,'Zenergy-OE'!AN42,0))","v":0},{"$f":"'Zenergy-OE'!AP42","v":0},{"$f":"IF(EK48>1,VLOOKUP(IF(ISNUMBER(EK48),TEXT(EK48,\"0\"),EK48),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK48>1,VLOOKUP(IF(ISNUMBER(EK48),TEXT(EK48,\"0\"),EK48),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+400",40166,50166,60166,70166,80166,90166,null,"650+400",40141,50141,60141,70141,80141,90141]
[null,"650+400",40265,50265,60265,70265,80265,90265,null,"Szerokość obudowy W","Pełna płyta montażowa,  Wysokość obudowy H, POLE 1, 3",null,null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,{"$f":"IF('Zenergy-OE'!AF75=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AF75>40000,1,0)","v":1},1,null,null,{"$f":"IF('Zenergy-OE'!AN75=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AN75>40000,1,0)","v":1},1,null,{"$f":"IF('Zenergy-OE'!AV75=\"\",0,1)","v":0},{"$f":"IF('Zenergy-OE'!AV75>40000,1,0)","v":1},1,null,null,"Przepust",3,2,2,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 4P most pionowy z boku 400\",\"Vertical AlCubar / Cu 4P busbar support D400\")","v":"Izolator AlCubar 4P most pionowy z boku 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  30\",\"Quantity 30\")","v":"Ilość  30"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa",33205,33205,33205,33205,33205,33205,33205,33205,33205,33205,33205,33205,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN45=\"\",0,IF('Zenergy-OE'!AN45>0,'Zenergy-OE'!AN45,0))","v":0},{"$f":"'Zenergy-OE'!AP45","v":0},{"$f":"IF(EK49>1,VLOOKUP(IF(ISNUMBER(EK49),TEXT(EK49,\"0\"),EK49),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK49>1,VLOOKUP(IF(ISNUMBER(EK49),TEXT(EK49,\"0\"),EK49),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+300",40186,50186,60186,70186,80186,90186,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+300",40285,50285,60285,70285,80285,90285,null,null,1200,1400,1600,1800,2000,2200,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 3P doizolowanie pion, bok 400\",\"Vertical AlCubar / Cu 3P free busbar support D400\")","v":"Izolator AlCubar 3P doizolowanie pion, bok 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  31\",\"Quantity 31\")","v":"Ilość  31"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW39=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN48=\"\",0,IF('Zenergy-OE'!AN48>0,'Zenergy-OE'!AN48,0))","v":0},{"$f":"'Zenergy-OE'!AP48","v":0},{"$f":"IF(EK50>1,VLOOKUP(IF(ISNUMBER(EK50),TEXT(EK50,\"0\"),EK50),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK50>1,VLOOKUP(IF(ISNUMBER(EK50),TEXT(EK50,\"0\"),EK50),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+400",40186,50186,60186,70186,80186,90186,null,"850+400",40141,50141,60141,70141,80141,90141]
[null,"850+400",40285,50285,60285,70285,80285,90285,1,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,41230,51230,61230,71230,81230,91230,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator AlCubar 4P doizolowanie pion, bok 400\",\"Vertical AlCubar / Cu 4P free busbar support D400\")","v":"Izolator AlCubar 4P doizolowanie pion, bok 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  32\",\"Quantity 32\")","v":"Ilość  32"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW39=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN51=\"\",0,IF('Zenergy-OE'!AN51>0,'Zenergy-OE'!AN51,0))","v":0},{"$f":"'Zenergy-OE'!AP51","v":0},{"$f":"IF(EK51>1,VLOOKUP(IF(ISNUMBER(EK51),TEXT(EK51,\"0\"),EK51),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK51>1,VLOOKUP(IF(ISNUMBER(EK51),TEXT(EK51,\"0\"),EK51),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+300",40166,50166,60166,70166,80166,90166,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+300",40280,50280,60280,70280,80280,90280,2,300,40930,50930,60930,70930,80930,90930,null,400,41240,51240,61240,71240,81240,91240,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Podpora pionowej szyny AlCubar\",\"Vertical AlCubar holder\")","v":"Podpora pionowej szyny AlCubar"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  33\",\"Quantity 33\")","v":"Ilość  33"},null,{"$f":"IF(CE57=14,14,IF(CP38=1,$BA$15,CB57))","v":1},null,null,{"$f":"IF(CP38=1,BD4,CE57)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW39=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN54=\"\",0,IF('Zenergy-OE'!AN54>0,'Zenergy-OE'!AN54,0))","v":0},{"$f":"'Zenergy-OE'!AP54","v":0},{"$f":"IF(EK52>1,VLOOKUP(IF(ISNUMBER(EK52),TEXT(EK52,\"0\"),EK52),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK52>1,VLOOKUP(IF(ISNUMBER(EK52),TEXT(EK52,\"0\"),EK52),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+400",40166,50166,60166,70166,80166,90166,null,"150+650+400",40141,50141,60141,70141,80141,90141]
[null,"150+650+400",40280,50280,60280,70280,80280,90280,3,400,40940,50940,60940,70940,80940,90940,null,450,41245,51245,61245,71245,81245,91245,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO55:$AR57),$BS$21,$BS$13)","v":1},"Cokół boki / pokrywa pole 6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 1P most poziomy 200/230\",\"Horizontal AlCubar 1P 630A busbar support D200/230\")","v":"Izol. AlCubar 630 1P most poziomy 200/230"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  34\",\"Quantity 34\")","v":"Ilość  34"},null,{"$f":"IF(CE56=14,25,IF(CO38=1,$BA$12,CB56))","v":1},null,null,{"$f":"IF(CO38=1,BD4,CE56)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW39=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN57=\"\",0,IF('Zenergy-OE'!AN57>0,'Zenergy-OE'!AN57,0))","v":0},{"$f":"'Zenergy-OE'!AP57","v":0},{"$f":"IF(EK53>1,VLOOKUP(IF(ISNUMBER(EK53),TEXT(EK53,\"0\"),EK53),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK53>1,VLOOKUP(IF(ISNUMBER(EK53),TEXT(EK53,\"0\"),EK53),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,null,null,null,null,null,null,null,4,450,40945,50945,60945,70945,80945,90945,null,600,41260,51260,61260,71260,81260,91260,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cokół","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 3P most poziomy 400\",\"Horizontal AlCubar 3P 630A busbar support D400\")","v":"Izol. AlCubar 630 3P most poziomy 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  35\",\"Quantity 35\")","v":"Ilość  35"},null,{"$f":"IF(CE55=14,23,IF(CN38=1,$BA$13,CB55))","v":1},null,null,{"$f":"IF(CN38=1,BD4,CE55)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW39=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN60=\"\",0,IF('Zenergy-OE'!AN60>0,'Zenergy-OE'!AN60,0))","v":0},{"$f":"'Zenergy-OE'!AP60","v":0},{"$f":"IF(EK54>1,VLOOKUP(IF(ISNUMBER(EK54),TEXT(EK54,\"0\"),EK54),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK54>1,VLOOKUP(IF(ISNUMBER(EK54),TEXT(EK54,\"0\"),EK54),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL54*EN54","v":0}]
[null,null,null,null,null,null,null,null,5,600,40960,50960,60960,70960,80960,90960,null,650,41265,51265,61265,71265,81265,91265,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P.boki",3,1,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 4P most poziomy 400\",\"Horizontal AlCubar 4P 630A busbar support D400\")","v":"Izol. AlCubar 630 4P most poziomy 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  36\",\"Quantity 36\")","v":"Ilość  36"},null,1,4,null,1,4,null,null,"Akc.szerokość",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN63=\"\",0,IF('Zenergy-OE'!AN63>0,'Zenergy-OE'!AN63,0))","v":0},{"$f":"'Zenergy-OE'!AP63","v":0},{"$f":"IF(EK55>1,VLOOKUP(IF(ISNUMBER(EK55),TEXT(EK55,\"0\"),EK55),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK55>1,VLOOKUP(IF(ISNUMBER(EK55),TEXT(EK55,\"0\"),EK55),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Szerokość obudowy","Rama rozł. Listw. na zawiasach  Wysokość, Pole 1,3",null,null,null,5,null,null,"Szerokość obudowy","Rama rozł. Listw. na zawiasach  Wysokość, Pole 2",null,null,null,5]
[null,null,null,null,null,null,null,null,6,650,40965,50965,60965,70965,80965,90965,null,800,41280,51280,61280,71280,81280,91280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Przepust",3,2,2,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 3P doizolowanie poz.400\",\"AlCubar 3P 630A free busbar support D400\")","v":"Izol. AlCubar 630 3P doizolowanie poz.400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  37\",\"Quantity 37\")","v":"Ilość  37"},null,1,"Osłony",null,1,"Ilość mod.",null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN66=\"\",0,IF('Zenergy-OE'!AN66>0,'Zenergy-OE'!AN66,0))","v":0},{"$f":"'Zenergy-OE'!AP66","v":0},{"$f":"IF(EK56>1,VLOOKUP(IF(ISNUMBER(EK56),TEXT(EK56,\"0\"),EK56),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK56>1,VLOOKUP(IF(ISNUMBER(EK56),TEXT(EK56,\"0\"),EK56),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,"Szerokość obudowy","Drzwi wentyl. IP43   Wysokość",null,null,7,null,"Pole 1,3",7,800,40980,50980,60980,70980,80980,90980,null,"650+150",41280,51280,61280,71280,81280,91280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 4P doizolowanie poz.400\",\"AlCubar 4P 630A free busbar support D400\")","v":"Izol. AlCubar 630 4P doizolowanie poz.400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  38\",\"Quantity 38\")","v":"Ilość  38"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P, most pionowy na plecach\",\"Rear 3P vertical busbar support\")","v":"Izolator 3P, most pionowy na plecach"},null,null,null,null,null,null,null,null,null,null,null,null,"W 600 - 4","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN69=\"\",0,IF('Zenergy-OE'!AN69>0,'Zenergy-OE'!AN69,0))","v":0},{"$f":"'Zenergy-OE'!AP69","v":0},{"$f":"IF(EK57>1,VLOOKUP(IF(ISNUMBER(EK57),TEXT(EK57,\"0\"),EK57),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK57>1,VLOOKUP(IF(ISNUMBER(EK57),TEXT(EK57,\"0\"),EK57),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",8,"650+150",40980,50980,60980,70980,80980,90980,null,850,41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 1P most pion z boku 200/230\",\"Vertical 1P AlCubar 630A busbar support D200/230\")","v":"Izol. AlCubar 630 1P most pion z boku 200/230"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  39\",\"Quantity 39\")","v":"Ilość  39"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE56<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 4P, most pionowy na plecach\",\"Rear 4P vertical busbar support\")","v":"Izolator 4P, most pionowy na plecach"},null,null,null,null,null,null,"Pole 1",null,null,null,null,null,"Brak",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","","Brak",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN72=\"\",0,IF('Zenergy-OE'!AN72>0,'Zenergy-OE'!AN72,0))","v":0},{"$f":"'Zenergy-OE'!AP72","v":0},{"$f":"IF(EK58>1,VLOOKUP(IF(ISNUMBER(EK58),TEXT(EK58,\"0\"),EK58),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK58>1,VLOOKUP(IF(ISNUMBER(EK58),TEXT(EK58,\"0\"),EK58),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C58=0,\"\",\"\")","v":""},"","","","","",9,850,40985,50985,60985,70985,80985,90985,null,"650+200",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 3P most pionowy z boku 400\",\"Vertical 3P AlCubar 630A busbar support D400\")","v":"Izol. AlCubar 630 3P most pionowy z boku 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  40\",\"Quantity 40\")","v":"Ilość  40"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P, most pion. na plecach reg.\",\"Rear 3P vertical busbar support regulated\")","v":"Izolator 3P, most pion. na plecach reg."},null,null,null,null,null,null,"Ilość mod.przód",null,null,null,null,null,"Osłona pełna",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN75=\"\",0,IF('Zenergy-OE'!AN75>0,'Zenergy-OE'!AN75,0))","v":0},{"$f":"'Zenergy-OE'!AP75","v":0},{"$f":"IF(EK59>1,VLOOKUP(IF(ISNUMBER(EK59),TEXT(EK59,\"0\"),EK59),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK59>1,VLOOKUP(IF(ISNUMBER(EK59),TEXT(EK59,\"0\"),EK59),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,40430,50430,60430,70430,80430,90430,10,"650+200",40985,50985,60985,70985,80985,90985,null,1000,41210,51210,61210,71210,81210,91210,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO62:$AR64),$BS$21,$BS$13)","v":1},"Cokół boki / pokrywa pole 7",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630 4P most pionowy z boku 400\",\"Vertical 3P AlCubar 630A busbar support D400\")","v":"Izol. AlCubar 630 4P most pionowy z boku 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  41\",\"Quantity 41\")","v":"Ilość  41"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 4P, most pion. na plecach reg.\",\"Rear 4P vertical busbar support regulated\")","v":"Izolator 4P, most pion. na plecach reg."},null,null,null,{"$f":"IF(BV4>3,1,0)","v":0},{"$f":"IF(CM60=1,SUM(CN61:CN66),0)","v":0},null,1,{"$f":"IF(BA13>1,'Zenergy-OE'!AH42/(Zbaza!AC1),0)","v":1},{"$f":"IF(CB4>4,0,IF(CE4<13,CE4,0))","v":0},{"$f":"CQ60*CR60","v":0},{"$f":"SUM(CS60:CS71)","v":0},null,"Osł. modułowa",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",400,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN78=\"\",0,IF('Zenergy-OE'!AN78>0,'Zenergy-OE'!AN78,0))","v":0},{"$f":"'Zenergy-OE'!AP78","v":0},{"$f":"IF(EK60>1,VLOOKUP(IF(ISNUMBER(EK60),TEXT(EK60,\"0\"),EK60),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK60>1,VLOOKUP(IF(ISNUMBER(EK60),TEXT(EK60,\"0\"),EK60),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL60*EN60","v":0},null,null,450,40845,50845,60845,70845,80845,90845,null,450,40845,50845,60845,70845,80845,90845]
[null,400,40440,50440,60440,70440,80440,90440,11,1000,40910,50910,60910,70910,80910,90910,null,1200,41212,51212,61212,71212,81212,91212,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cokół","Brak",100,200,"Pokrywa",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P,rozstaw 60 mm\",\"Cu 3P Busbar support 60mm spacing\")","v":"Izolator 3P,rozstaw 60 mm"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  42\",\"Quantity 42\")","v":"Ilość  42"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. 3P, podpora mostu na plecach, reg.\",\"Rear 3P vert. busbar bottom support regulated\")","v":"Izol. 3P, podpora mostu na plecach, reg."},null,null,null,{"$f":"IF(BD4=1,20,0)","v":0},{"$f":"IF(BD4=1,0,0)","v":0},null,2,{"$f":"IF(BA13>1,'Zenergy-OE'!AH45/(Zbaza!AC1),0)","v":0},{"$f":"IF(CB21>4,0,IF(CE21<13,CE21,0))","v":1},0,{"$f":"IF(CT60<=CM67,CT60,CM67)","v":0},null,"Osł. przeszklona",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",450,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN81=\"\",0,IF('Zenergy-OE'!AN81>0,'Zenergy-OE'!AN81,0))","v":0},{"$f":"'Zenergy-OE'!AP81","v":0},{"$f":"IF(EK61>1,VLOOKUP(IF(ISNUMBER(EK61),TEXT(EK61,\"0\"),EK61),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK61>1,VLOOKUP(IF(ISNUMBER(EK61),TEXT(EK61,\"0\"),EK61),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,450,40445,50445,60445,70445,80445,90445,12,1200,40912,50912,60912,70912,80912,90912,null,1300,41213,51213,61213,71213,81213,91213,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P.boki",3,1,1,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P,rozstaw 100 mm\",\"Cu 3P Busbar support 100mm spacing\")","v":"Izolator 3P,rozstaw 100 mm"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  43\",\"Quantity 43\")","v":"Ilość  43"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. 4P, podpora mostu na plecach, reg.\",\"Rear 4P vert. busbar bottom support regulated\")","v":"Izol. 4P, podpora mostu na plecach, reg."},null,null,null,{"$f":"IF(BD4=2,24,0)","v":0},{"$f":"IF(BD4=2,0,0)","v":0},null,3,{"$f":"IF(BA13>1,'Zenergy-OE'!AH48/(Zbaza!AC1),0)","v":0},{"$f":"IF(CB38>4,0,IF(CE38<13,CE38,0))","v":1},0,{"$f":"IF(CT61=CM67,CT60-CT61,\"\")","v":""},null,"Szyna stała TS35",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",600,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN84=\"\",0,IF('Zenergy-OE'!AN84>0,'Zenergy-OE'!AN84,0))","v":0},{"$f":"'Zenergy-OE'!AP84","v":0},{"$f":"IF(EK62>1,VLOOKUP(IF(ISNUMBER(EK62),TEXT(EK62,\"0\"),EK62),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK62>1,VLOOKUP(IF(ISNUMBER(EK62),TEXT(EK62,\"0\"),EK62),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,650,40865,50865,60865,70865,80865,90865,null,650,40865,50865,60865,70865,80865,90865]
[null,600,40460,50460,60460,70460,80460,90460,13,1300,40913,50913,60913,70913,80913,90913,null,"650+650",41265,51265,61265,71265,81265,91265,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Przepust",3,2,2,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izolator 3P,rozstaw 185 mm\",\"Cu 3P Busbar support 185mm spacing\")","v":"Izolator 3P,rozstaw 185 mm"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  44\",\"Quantity 44\")","v":"Ilość  44"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630A 3P pionowo na plecach\",\"Rear 3P AlCubar 630A vertical busbar support\")","v":"Izol. AlCubar 630A 3P pionowo na plecach"},null,null,null,{"$f":"IF(BD4=3,28,0)","v":0},{"$f":"IF(BD4=3,5,0)","v":0},null,4,{"$f":"IF(BA13>1,'Zenergy-OE'!AH51/(Zbaza!AC1),0)","v":0},{"$f":"IF(CB55>4,0,IF(CE55<13,CE55,0))","v":1},0,{"$f":"IF(BV4=4,\"\",CT61)","v":0},null,"Szyna reg.TS35",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",650,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN87=\"\",0,IF('Zenergy-OE'!AN87>0,'Zenergy-OE'!AN87,0))","v":0},{"$f":"'Zenergy-OE'!AP87","v":0},{"$f":"IF(EK63>1,VLOOKUP(IF(ISNUMBER(EK63),TEXT(EK63,\"0\"),EK63),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK63>1,VLOOKUP(IF(ISNUMBER(EK63),TEXT(EK63,\"0\"),EK63),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,40465,50465,60465,70465,80465,90465,14,"650+612",40965,50965,60965,70965,80965,90965,null,"650+850",41265,51265,61265,71265,81265,91265,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Wspornik szyny PE\",\"PE busbar Support\")","v":"Wspornik szyny PE"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  45\",\"Quantity 45\")","v":"Ilość  45"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Izol. AlCubar 630A 4P pionowo na plecach\",\"Rear 4P AlCubar 630A vertical busbar support\")","v":"Izol. AlCubar 630A 4P pionowo na plecach"},null,null,null,{"$f":"IF(BD4=4,32,0)","v":0},{"$f":"IF(BD4=4,9,0)","v":0},null,5,{"$f":"IF(BA13>1,'Zenergy-OE'!AH54/(Zbaza!AC1),0)","v":0},{"$f":"IF(CB72>4,0,IF(CE72<13,CE72,0))","v":1},0,null,null,"Płyta ocynk pełna",{"$f":"IF(CW57=0,\"\",\"\")","v":""},33062,33063,33064,33065,33066,{"$f":"IF(DC57=0,\"\",\"\")","v":""},33067,{"$f":"IF(DE57=0,\"\",\"\")","v":""},33068,{"$f":"IF(DG57=0,\"\",\"\")","v":""},33069,800,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN90=\"\",0,IF('Zenergy-OE'!AN90>0,'Zenergy-OE'!AN90,0))","v":0},{"$f":"'Zenergy-OE'!AP90","v":0},{"$f":"IF(EK64>1,VLOOKUP(IF(ISNUMBER(EK64),TEXT(EK64,\"0\"),EK64),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK64>1,VLOOKUP(IF(ISNUMBER(EK64),TEXT(EK64,\"0\"),EK64),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+150",40865,50865,60865,70865,80865,90865,null,"650+150",40165,50165,60165,70165,80165,90165]
[null,800,40480,50480,60480,70480,80480,90480,15,"650+812",40965,50965,60965,70965,80965,90965,null,"850+850",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa 200/230\",\"Cable tray D200/230\")","v":"Drabinka kablowa 200/230"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  46\",\"Quantity 46\")","v":"Ilość  46"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa na plecach\",\"Cable tray\")","v":"Drabinka kablowa na plecach"},null,null,null,{"$f":"IF(BD4=5,36,0)","v":36},{"$f":"IF(BD4=5,13,0)","v":13},null,6,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH57/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB89>4,0,IF(CE89<13,CE89,0))","v":1},0,null,null,"Płyta malow.otw.",{"$f":"IF(CW57=0,\"\",\"\")","v":""},33562,33563,33564,33565,33566,{"$f":"IF(DC57=0,\"\",\"\")","v":""},33567,{"$f":"IF(DE57=0,\"\",\"\")","v":""},33568,{"$f":"IF(DG57=0,\"\",\"\")","v":""},33569,"650+150",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AN93=\"\",0,IF('Zenergy-OE'!AN93>0,'Zenergy-OE'!AN93,0))","v":0},{"$f":"'Zenergy-OE'!AP93","v":0},{"$f":"IF(EK65>1,VLOOKUP(IF(ISNUMBER(EK65),TEXT(EK65,\"0\"),EK65),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK65>1,VLOOKUP(IF(ISNUMBER(EK65),TEXT(EK65,\"0\"),EK65),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,850,40885,50885,60885,70885,80885,90885,null,850,40885,50885,60885,70885,80885,90885]
[null,"650+150",40480,50480,60480,70480,80480,90480,16,"850+812",40985,50985,60985,70985,80985,90985,null,"650+300",41295,51295,61295,71295,81295,91295,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa 400\",\"Cable tray D400\")","v":"Drabinka kablowa 400"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  47\",\"Quantity 47\")","v":"Ilość  47"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa na drzwiach\",\"Door cable tray\")","v":"Drabinka kablowa na drzwiach"},null,null,null,{"$f":"IF(BD4=6,40,0)","v":0},{"$f":"IF(BD4=6,17,0)","v":0},null,7,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH60/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB106>4,0,IF(CE106<13,CE106,0))","v":1},0,null,null,"Płyta oc. pozioma",{"$f":"IF(CW56=0,\"\",\"\")","v":""},"","","","","","","","",{"$f":"IF(DF149=0,\"\",\"\")","v":""},{"$f":"IF(DG149=0,\"\",\"\")","v":""},{"$f":"IF(DH149=0,\"\",\"\")","v":""},850,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pole 3",{"$f":"IF('Zenergy-OE'!AV12=\"\",0,IF('Zenergy-OE'!AX12>0,'Zenergy-OE'!AV12,0))","v":0},{"$f":"IF('Zenergy-OE'!AX12=\"\",0,'Zenergy-OE'!AX12)","v":0},{"$f":"IF(EK66>1,VLOOKUP(IF(ISNUMBER(EK66),TEXT(EK66,\"0\"),EK66),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK66>1,VLOOKUP(IF(ISNUMBER(EK66),TEXT(EK66,\"0\"),EK66),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+200",40865,50865,60865,70865,80865,90865,null,"650+200",40165,50165,60165,70165,80165,90165]
[null,850,40485,50485,60485,70485,80485,90485,17,"650+300",40965,50965,60965,70965,80965,90965,null,"650+400",41211,51211,61211,71211,81211,91211,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$75:$AT$77),$BA$4,$BJ4)","v":1},"Drzwi przód, pole 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Przepust membranowy IP55\",\"Diaphragm cable passage IP55\")","v":"Przepust membranowy IP55"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  48\",\"Quantity 48\")","v":"Ilość  48"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Drabinka kablowa pod osłonę\",\"Front plate cable tray\")","v":"Drabinka kablowa pod osłonę"},null,null,null,{"$f":"IF(CN60=0,SUM(CM61:CM66),CN60)","v":36},{"$f":"CT60-CM67","v":-36},null,8,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH63/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB123>4,0,IF(CE123<13,CE123,0))","v":1},0,null,null,"Płyta licznikowa",{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","","650+200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV15=\"\",0,IF('Zenergy-OE'!AX15>0,'Zenergy-OE'!AV15,0))","v":0},{"$f":"IF('Zenergy-OE'!AX15=\"\",0,'Zenergy-OE'!AX15)","v":0},{"$f":"IF(EK67>1,VLOOKUP(IF(ISNUMBER(EK67),TEXT(EK67,\"0\"),EK67),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK67>1,VLOOKUP(IF(ISNUMBER(EK67),TEXT(EK67,\"0\"),EK67),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+200",40485,50485,60485,70485,80485,90485,18,"650+400",40965,50965,60965,70965,80965,90965,null,"850+300",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$75:$AT$77),$BA$4,$BJ5)","v":10},"Drzwi przód, pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Kratka wentylacyjna 160x160\",\"IP54 filter 160x160\")","v":"Kratka wentylacyjna 160x160"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  49\",\"Quantity 49\")","v":"Ilość  49"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Metalowa kieszeń na dokumentację\",\"Drawing holder\")","v":"Metalowa kieszeń na dokumentację"},null,null,null,{"$f":"IF(BV4=4,\"\",CN67)","v":-36},null,null,9,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH66/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB140>4,0,IF(CE140<13,CE140,0))","v":1},0,null,null,null,{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",1000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV18=\"\",0,IF('Zenergy-OE'!AX18>0,'Zenergy-OE'!AV18,0))","v":0},{"$f":"IF('Zenergy-OE'!AX18=\"\",0,'Zenergy-OE'!AX18)","v":0},{"$f":"IF(EK68>1,VLOOKUP(IF(ISNUMBER(EK68),TEXT(EK68,\"0\"),EK68),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK68>1,VLOOKUP(IF(ISNUMBER(EK68),TEXT(EK68,\"0\"),EK68),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1000,40410,50410,60410,70410,80410,90410,19,"850+300",40985,50985,60985,70985,80985,90985,null,"850+400",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$75:$AT$77),$BA$4,$BJ6)","v":10},"Drzwi przód, pole 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Kratka wentylacyjna 230x230\",\"IP54 filter 230x230\")","v":"Kratka wentylacyjna 230x230"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Ilość  50\",\"Quantity 50\")","v":"Ilość  50"},null,{"$f":"IF(CE74=14,14,IF(CP39=1,$BA$15,CB74))","v":1},null,null,{"$f":"IF(CP39=1,BD4,CE74)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Pionowy zestaw szyn TS35, 6M\",\"6-Modules Vertical DIN-rail for terminals\")","v":"Pionowy zestaw szyn TS35, 6M"},null,null,null,null,null,null,10,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH69/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB157>4,0,IF(CE157<13,CE157,0))","v":1},0,null,null,null,{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",1200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV21=\"\",0,IF('Zenergy-OE'!AX21>0,'Zenergy-OE'!AV21,0))","v":0},{"$f":"IF('Zenergy-OE'!AX21=\"\",0,'Zenergy-OE'!AX21)","v":0},{"$f":"IF(EK69>1,VLOOKUP(IF(ISNUMBER(EK69),TEXT(EK69,\"0\"),EK69),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK69>1,VLOOKUP(IF(ISNUMBER(EK69),TEXT(EK69,\"0\"),EK69),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1200,40412,50412,60412,70412,80412,90412,20,"850+400",40985,50985,60985,70985,80985,90985,null,"650+150+300",41280,51280,61280,71280,81280,91280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Przyłącza kablowe w przedziale 3P 250A\",\"Cable Terminal Transfer 3P 250A\")","v":"Przyłącza kablowe w przedziale 3P 250A"},null,null,null,null,{"$f":"IF(CE73=14,25,IF(CO39=1,$BA$12,CB73))","v":1},null,null,{"$f":"IF(CO39=1,BD4,CE73)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Poziomy zestaw dwóch szyn TS35\",\"Horizontal double DIN-rail for terminals\")","v":"Poziomy zestaw dwóch szyn TS35"},null,null,null,null,null,null,11,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH72/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB174>4,0,IF(CE174<13,CE174,0))","v":1},0,null,null,null,{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","",1300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV24=\"\",0,IF('Zenergy-OE'!AX24>0,'Zenergy-OE'!AV24,0))","v":0},{"$f":"IF('Zenergy-OE'!AX24=\"\",0,'Zenergy-OE'!AX24)","v":0},{"$f":"IF(EK70>1,VLOOKUP(IF(ISNUMBER(EK70),TEXT(EK70,\"0\"),EK70),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK70>1,VLOOKUP(IF(ISNUMBER(EK70),TEXT(EK70,\"0\"),EK70),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+650",40865,50865,60865,70865,80865,90865,null,"650+650",40865,50865,60865,70865,80865,90865]
[null,1300,40413,50413,60413,70413,80413,90413,21,"150+650+300",40965,50965,60965,70965,80965,90965,null,"650+150+400",41280,51280,61280,71280,81280,91280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Przyłącza kablowe w przedziale 4P 250A\",\"Cable Terminal Transfer 4P 250A\")","v":"Przyłącza kablowe w przedziale 4P 250A"},null,null,null,null,{"$f":"IF(CE72=14,23,IF(CN39=1,$BA$13,CB72))","v":1},null,null,{"$f":"IF(CN39=1,BD4,CE72)","v":1},null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Osłona mostu poziomego\",\"Horizontal busbar cover\")","v":"Osłona mostu poziomego"},null,null,null,null,null,null,12,{"$f":"IF($BA$13>1,'Zenergy-OE'!AH75/(Zbaza!$AC$1),0)","v":0},{"$f":"IF(CB191>4,0,IF(CE191<13,CE191,0))","v":1},0,null,null,null,{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","","650+612",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV25=\"\",0,IF('Zenergy-OE'!AX25>0,'Zenergy-OE'!AV25,0))","v":0},{"$f":"IF('Zenergy-OE'!AX25=\"\",0,'Zenergy-OE'!AX25)","v":0},{"$f":"IF(EK71>1,VLOOKUP(IF(ISNUMBER(EK71),TEXT(EK71,\"0\"),EK71),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK71>1,VLOOKUP(IF(ISNUMBER(EK71),TEXT(EK71,\"0\"),EK71),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+850",40865,50865,60865,70865,80865,90865,null,"650+850",40885,50885,60885,70885,80885,90885]
[null,"650+612",40465,50465,60465,70465,80465,90465,22,"150+650+400",40965,50965,60965,70965,80965,90965,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Przyłącza kablowe w przedziale 3P 630A\",\"Cable Terminal Transfer 3P 630A\")","v":"Przyłącza kablowe w przedziale 3P 630A"},null,null,null,null,1,5,null,1,5,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zestaw mocowania do ściany\",\"Zenergy cabinet wall sling rail\")","v":"Zestaw mocowania do ściany"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW57=0,\"\",\"\")","v":""},"","","","","","","","","","","","650+812",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV28=\"\",0,IF('Zenergy-OE'!AX28>0,'Zenergy-OE'!AV28,0))","v":0},{"$f":"IF('Zenergy-OE'!AX28=\"\",0,'Zenergy-OE'!AX28)","v":0},{"$f":"IF(EK72>1,VLOOKUP(IF(ISNUMBER(EK72),TEXT(EK72,\"0\"),EK72),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK72>1,VLOOKUP(IF(ISNUMBER(EK72),TEXT(EK72,\"0\"),EK72),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+850",40885,50885,60885,70885,80885,90885,null,"850+850",40885,50885,60885,70885,80885,90885]
[null,"650+812",40465,50465,60465,70465,80465,90465,23,98,40995,50995,60995,70995,80995,90995,null,"Szerokość obudowy","Osłona tylna went. IP43   Wysokość",null,null,9,null,"Pole 1,3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Przyłącza kablowe w przedziale 4P 630A\",\"Cable Terminal Transfer 4P 630A\")","v":"Przyłącza kablowe w przedziale 4P 630A"},null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+812",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV29=\"\",0,IF('Zenergy-OE'!AX29>0,'Zenergy-OE'!AV29,0))","v":0},{"$f":"IF('Zenergy-OE'!AX29=\"\",0,'Zenergy-OE'!AX29)","v":0},{"$f":"IF(EK73>1,VLOOKUP(IF(ISNUMBER(EK73),TEXT(EK73,\"0\"),EK73),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK73>1,VLOOKUP(IF(ISNUMBER(EK73),TEXT(EK73,\"0\"),EK73),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+300",40865,50865,60865,70865,80865,90865,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+812",40485,50485,60485,70485,80485,90485,null,null,null,null,null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IP","Brak","D.pełne","D.went.","D.szkl.","P.pełne","P,went.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,"Pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV32=\"\",0,IF('Zenergy-OE'!AX32>0,'Zenergy-OE'!AV32,0))","v":0},{"$f":"IF('Zenergy-OE'!AX32=\"\",0,'Zenergy-OE'!AX32)","v":0},{"$f":"IF(EK74>1,VLOOKUP(IF(ISNUMBER(EK74),TEXT(EK74,\"0\"),EK74),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK74>1,VLOOKUP(IF(ISNUMBER(EK74),TEXT(EK74,\"0\"),EK74),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+400",40865,50865,60865,70865,80865,90865,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+300",40465,50465,60465,70465,80465,90465,null,"Szerokość obudowy W","Pełna płyta montażowa,  Wysokość obudowy H, POLE 2",null,null,null,null,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,10,1,2,3,4,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE73<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,"Ilość mod.przód",null,null,null,null,null,"W 650 - 5+12","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV33=\"\",0,IF('Zenergy-OE'!AX33>0,'Zenergy-OE'!AV33,0))","v":0},{"$f":"IF('Zenergy-OE'!AX33=\"\",0,'Zenergy-OE'!AX33)","v":0},{"$f":"IF(EK75>1,VLOOKUP(IF(ISNUMBER(EK75),TEXT(EK75,\"0\"),EK75),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK75>1,VLOOKUP(IF(ISNUMBER(EK75),TEXT(EK75,\"0\"),EK75),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+300",40885,50885,60885,70885,80885,90885,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+400",40465,50465,60465,70465,80465,90465,null,null,1200,1400,1600,1800,2000,2200,null,300,41430,51430,61430,71430,81430,91430,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,10,6,7,3,8,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,{"$f":"IF(BV5>3,1,0)","v":0},{"$f":"IF(CM76=1,SUM(CN77:CN82),0)","v":0},null,1,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP42/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH42/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB5>4,0,IF(CE5<13,CE5,0))","v":1},{"$f":"CQ76*CR76","v":0},{"$f":"SUM(CS76:CS87)","v":0},null,"Brak",{"$f":"IF(CW75=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV36=\"\",0,IF('Zenergy-OE'!AX36>0,'Zenergy-OE'!AV36,0))","v":0},{"$f":"IF('Zenergy-OE'!AX36=\"\",0,'Zenergy-OE'!AX36)","v":0},{"$f":"IF(EK76>1,VLOOKUP(IF(ISNUMBER(EK76),TEXT(EK76,\"0\"),EK76),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK76>1,VLOOKUP(IF(ISNUMBER(EK76),TEXT(EK76,\"0\"),EK76),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+400",40885,50885,60885,70885,80885,90885,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+300",40485,50485,60485,70485,80485,90485,1,"Brak",{"$f":"IF(CW208=0,\"\",\"\")","v":""},"","","","","",null,400,41440,51440,61440,71440,81440,91440,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,10,6,10,3,8,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=1,20,0)","v":0},{"$f":"IF(BD4=1,0,0)","v":0},null,2,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP45/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH43/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB22>4,0,IF(CE22<13,CE22,0))","v":1},0,{"$f":"IF(CT76<=CM83,CT76,CM83)","v":0},null,"Osłona pełna",32710,32720,32730,32740,32750,32760,32770,32780,32790,32791,32792,32793,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV39=\"\",0,IF('Zenergy-OE'!AX39>0,'Zenergy-OE'!AV39,0))","v":0},{"$f":"IF('Zenergy-OE'!AX39=\"\",0,'Zenergy-OE'!AX39)","v":0},{"$f":"IF(EK77>1,VLOOKUP(IF(ISNUMBER(EK77),TEXT(EK77,\"0\"),EK77),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK77>1,VLOOKUP(IF(ISNUMBER(EK77),TEXT(EK77,\"0\"),EK77),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+300",40865,50865,60865,70865,80865,90865,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+400",40485,50485,60485,70485,80485,90485,2,300,40930,50930,60930,70930,80930,90930,null,450,41445,51445,61445,71445,81445,91445,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=2,24,0)","v":0},{"$f":"IF(BD4=2,0,0)","v":0},null,3,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP48/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH44/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB39>4,0,IF(CE39<13,CE39,0))","v":1},0,{"$f":"IF(CT77=CM83,CT76-CT77,\"\")","v":""},null,"Osł. modułowa",{"$f":"IF(CW75=0,\"\",\"\")","v":""},32725,32735,32745,32755,{"$f":"IF(DB77=0,\"\",\"\")","v":""},"","","","","","","Brak",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV42=\"\",0,IF('Zenergy-OE'!AX42>0,'Zenergy-OE'!AV42,0))","v":0},{"$f":"'Zenergy-OE'!AX42","v":0},{"$f":"IF(EK78>1,VLOOKUP(IF(ISNUMBER(EK78),TEXT(EK78,\"0\"),EK78),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK78>1,VLOOKUP(IF(ISNUMBER(EK78),TEXT(EK78,\"0\"),EK78),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+400",40865,50865,60865,70865,80865,90865,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+300",40480,50480,60480,70480,80480,90480,3,400,40940,50940,60940,70940,80940,90940,null,600,41460,51460,61460,71460,81460,91460,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=3,28,0)","v":0},{"$f":"IF(BD4=3,5,0)","v":0},null,4,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP51/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH45/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB56>4,0,IF(CE56<13,CE56,0))","v":1},0,{"$f":"IF(BV5=4,\"\",CT77)","v":0},null,"Osł. przeszklona",{"$f":"IF(CW75=0,\"\",\"\")","v":""},{"$f":"IF(CX75=0,\"\",\"\")","v":""},32739,32749,{"$f":"IF(DA75=0,\"\",\"\")","v":""},32769,{"$f":"IF(DC75=0,\"\",\"\")","v":""},32779,{"$f":"IF(DE75=0,\"\",\"\")","v":""},32789,{"$f":"IF(DG75=0,\"\",\"\")","v":""},32799,300,"Akcesoria tył, Pole 1, 3","Brak","Izolator 3P, most pionowy na plecach","Izolator 4P, most pionowy na plecach","Izolator 3P, most pionowy na plecach regulowany","Izolator 4P, most pionowy na plecach regulowany","Izolator 3P, podpora mostu na plecach, regulowana","Izolator 4P, podpora mostu na plecach, regulowana","Izol. AlCubar 630A 3P pionowo na plecach","Izol. AlCubar 630A 4P pionowo na plecach","Drabinka kablowa na plecach","Drabinka kablowa na drzwi","Drabinka kablowa pod osłonę","Metalowa kieszeń na dokumentację","Pionowy zestaw szyn TS35, 6M","Poziomy zestaw dwóch szyn TS35","Osłona mostu poziomego","Zestaw mocowania do ściany",null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV45=\"\",0,IF('Zenergy-OE'!AX45>0,'Zenergy-OE'!AV45,0))","v":0},{"$f":"'Zenergy-OE'!AX45","v":0},{"$f":"IF(EK79>1,VLOOKUP(IF(ISNUMBER(EK79),TEXT(EK79,\"0\"),EK79),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK79>1,VLOOKUP(IF(ISNUMBER(EK79),TEXT(EK79,\"0\"),EK79),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,"150+650+400",40480,50480,60480,70480,80480,90480,4,450,40945,50945,60945,70945,80945,90945,null,650,41465,51465,61465,71465,81465,91465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$88:$AT$90),$BA$4,$BM4)","v":4},"Plecy tył, pole 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=4,32,0)","v":0},{"$f":"IF(BD4=4,9,0)","v":0},null,5,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP54/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH46/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB73>4,0,IF(CE73<13,CE73,0))","v":1},0,null,null,"Szyna stała TS35",32700,32700,32700,32700,32700,32700,32700,32700,32700,32700,32700,32700,400,"Szerokość obudowy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV48=\"\",0,IF('Zenergy-OE'!AX48>0,'Zenergy-OE'!AV48,0))","v":0},{"$f":"'Zenergy-OE'!AX48","v":0},{"$f":"IF(EK80>1,VLOOKUP(IF(ISNUMBER(EK80),TEXT(EK80,\"0\"),EK80),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK80>1,VLOOKUP(IF(ISNUMBER(EK80),TEXT(EK80,\"0\"),EK80),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,null,null,null,null,null,null,null,5,600,40960,50960,60960,70960,80960,90960,null,800,41480,51480,61480,71480,81480,91480,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$88:$AT$90),$BA$4,$BM5)","v":10},"Plecy tył, pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=5,36,0)","v":36},{"$f":"IF(BD4=5,13,0)","v":13},null,6,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP57/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH47/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB90>4,0,IF(CE90<13,CE90,0))","v":1},0,null,null,"Szyna reg.TS35",32705,32705,32705,32705,32705,32705,32705,32705,32705,32705,32705,32705,450,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV51=\"\",0,IF('Zenergy-OE'!AX51>0,'Zenergy-OE'!AV51,0))","v":0},{"$f":"'Zenergy-OE'!AX51","v":0},{"$f":"IF(EK81>1,VLOOKUP(IF(ISNUMBER(EK81),TEXT(EK81,\"0\"),EK81),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK81>1,VLOOKUP(IF(ISNUMBER(EK81),TEXT(EK81,\"0\"),EK81),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Szerokość obudowy","Rama rozł. Listw. do plombowania  Wysokość, Pole 1,3",null,null,null,6,null,null,"Szerokość obudowy","Rama rozł. Listw. do plombowania  Wysokość, Pole 2",null,null,null,6]
[null,null,null,null,null,null,null,null,6,650,40965,50965,60965,70965,80965,90965,null,"650+150",41480,51480,61480,71480,81480,91480,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$88:$AT$90),$BA$4,$BM6)","v":10},"Plecy tył, pole 3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=6,40,0)","v":0},{"$f":"IF(BD4=6,17,0)","v":0},null,7,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP60/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH48/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB107>4,0,IF(CE107<13,CE107,0))","v":1},{"$f":"CQ82*CR82","v":0},null,null,"Płyta ocynk pełna",{"$f":"IF(CW75=0,\"\",\"\")","v":""},33072,33073,33074,33075,33076,{"$f":"IF(DC75=0,\"\",\"\")","v":""},33077,{"$f":"IF(DE75=0,\"\",\"\")","v":""},33078,{"$f":"IF(DG75=0,\"\",\"\")","v":""},33079,600,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV54=\"\",0,IF('Zenergy-OE'!AX54>0,'Zenergy-OE'!AV54,0))","v":0},{"$f":"'Zenergy-OE'!AX54","v":0},{"$f":"IF(EK82>1,VLOOKUP(IF(ISNUMBER(EK82),TEXT(EK82,\"0\"),EK82),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK82>1,VLOOKUP(IF(ISNUMBER(EK82),TEXT(EK82,\"0\"),EK82),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,null,null,null,null,null,null,null,7,800,40980,50980,60980,70980,80980,90980,null,850,41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,{"$f":"IF(CN76=0,SUM(CM77:CM82),CN76)","v":36},{"$f":"CT76-CM83","v":-36},null,8,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP63/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH49/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB124>4,0,IF(CE124<13,CE124,0))","v":1},0,null,null,"Płyta malow.otw.",{"$f":"IF(CW75=0,\"\",\"\")","v":""},33572,33573,33574,33575,33576,{"$f":"IF(DC75=0,\"\",\"\")","v":""},33577,{"$f":"IF(DE75=0,\"\",\"\")","v":""},33578,{"$f":"IF(DG75=0,\"\",\"\")","v":""},33579,650,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!AV57=\"\",0,IF('Zenergy-OE'!AX57>0,'Zenergy-OE'!AV57,0))","v":0},{"$f":"'Zenergy-OE'!AX57","v":0},{"$f":"IF(EK83>1,VLOOKUP(IF(ISNUMBER(EK83),TEXT(EK83,\"0\"),EK83),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK83>1,VLOOKUP(IF(ISNUMBER(EK83),TEXT(EK83,\"0\"),EK83),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy","Drzwi pełne IP43/55   Wysokość",null,null,6,null,"Pole 1,3",8,"650+150",40980,50980,60980,70980,80980,90980,null,"650+200",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,{"$f":"IF(BV5=4,\"\",CN83)","v":-36},null,null,9,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP66/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH50/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB141>4,0,IF(CE141<13,CE141,0))","v":1},0,null,null,"Płyta oc. pozioma",33771,33772,33773,33774,33775,33776,33777,33778,null,33779,{"$f":"IF(DG256=0,\"\",\"\")","v":""},{"$f":"IF(DH256=0,\"\",\"\")","v":""},800,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV60=\"\",0,IF('Zenergy-OE'!AX60>0,'Zenergy-OE'!AV60,0))","v":0},{"$f":"'Zenergy-OE'!AX60","v":0},{"$f":"IF(EK84>1,VLOOKUP(IF(ISNUMBER(EK84),TEXT(EK84,\"0\"),EK84),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK84>1,VLOOKUP(IF(ISNUMBER(EK84),TEXT(EK84,\"0\"),EK84),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL84*EN84","v":0},null,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",9,850,40985,50985,60985,70985,80985,90985,null,1000,41410,51410,61410,71410,81410,91410,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,10,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP69/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH51/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB158>4,0,IF(CE158<13,CE158,0))","v":1},0,null,null,"Płyta licznikowa",33207,33207,33207,33207,33207,33207,33207,33207,33207,33207,33207,33207,"650+150",300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},33163,33183,{"$f":"\"\"","v":""},31953,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31083,31973,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV63=\"\",0,IF('Zenergy-OE'!AX63>0,'Zenergy-OE'!AV63,0))","v":0},{"$f":"'Zenergy-OE'!AX63","v":0},{"$f":"IF(EK85>1,VLOOKUP(IF(ISNUMBER(EK85),TEXT(EK85,\"0\"),EK85),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK85>1,VLOOKUP(IF(ISNUMBER(EK85),TEXT(EK85,\"0\"),EK85),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C85=0,\"\",\"\")","v":""},"","","","","",10,"650+200",40985,50985,60985,70985,80985,90985,null,1200,41412,51412,61412,71412,81412,91412,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE91=14,14,IF(CP40=1,$BA$15,CB91))","v":1},null,null,{"$f":"IF(CP40=1,BD4,CE91)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,11,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP72/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH52/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB175>4,0,IF(CE175<13,CE175,0))","v":1},0,null,null,null,{"$f":"IF(CW75=0,\"\",\"\")","v":""},"","","","","","","","","","","",850,400,{"$f":"\"\"","v":""},20204,20214,20224,20234,20244,20254,20174,20184,33164,33184,33194,31954,30944,30940,31084,31974,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV66=\"\",0,IF('Zenergy-OE'!AX66>0,'Zenergy-OE'!AV66,0))","v":0},{"$f":"'Zenergy-OE'!AX66","v":0},{"$f":"IF(EK86>1,VLOOKUP(IF(ISNUMBER(EK86),TEXT(EK86,\"0\"),EK86),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK86>1,VLOOKUP(IF(ISNUMBER(EK86),TEXT(EK86,\"0\"),EK86),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,450,40846,50846,60846,70846,80846,90846,null,450,40846,50846,60846,70846,80846,90846]
[null,300,40530,50530,60530,70530,80530,90530,11,1000,40910,50910,60910,70910,80910,90910,null,1300,41413,51413,61413,71413,81413,91413,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IP","P,went.","P.pełne","D.pełne","D.szkl.","D.went.","Brak",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE90=14,25,IF(CO40=1,$BA$12,CB90))","v":1},null,null,{"$f":"IF(CO40=1,BD4,CE90)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,12,{"$f":"IF($BA$11>1,'Zenergy-OE'!AP75/Zbaza!$AH$1,IF($AG$1>1,'Zenergy-OE'!AH53/Zbaza!$AC$1,0))","v":0},{"$f":"IF(CB192>4,0,IF(CE192<13,CE192,0))","v":1},0,null,null,null,{"$f":"IF(CW75=0,\"\",\"\")","v":""},"","","","","","","","","","","","650+200",450,{"$f":"\"\"","v":""},20205,20215,20225,20235,20245,20255,20175,20185,33165,33185,33195,31955,30954,30950,31085,31975,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV69=\"\",0,IF('Zenergy-OE'!AX69>0,'Zenergy-OE'!AV69,0))","v":0},{"$f":"'Zenergy-OE'!AX69","v":0},{"$f":"IF(EK87>1,VLOOKUP(IF(ISNUMBER(EK87),TEXT(EK87,\"0\"),EK87),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK87>1,VLOOKUP(IF(ISNUMBER(EK87),TEXT(EK87,\"0\"),EK87),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,400,40540,50540,60540,70540,80540,90540,12,1200,40912,50912,60912,70912,80912,90912,null,"650+650",41465,51465,61465,71465,81465,91465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,5,4,1,3,2,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE89=14,23,IF(CN40=1,$BA$13,CB89))","v":1},null,null,{"$f":"IF(CN40=1,BD4,CE89)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW75=0,\"\",\"\")","v":""},"","","","","","","","","","","",1000,600,{"$f":"\"\"","v":""},20206,20216,20226,20236,20246,20256,20176,20186,33166,33186,null,31956,30964,30960,31086,31976,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV72=\"\",0,IF('Zenergy-OE'!AX72>0,'Zenergy-OE'!AV72,0))","v":0},{"$f":"'Zenergy-OE'!AX72","v":0},{"$f":"IF(EK88>1,VLOOKUP(IF(ISNUMBER(EK88),TEXT(EK88,\"0\"),EK88),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK88>1,VLOOKUP(IF(ISNUMBER(EK88),TEXT(EK88,\"0\"),EK88),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,650,40866,50866,60866,70866,80866,90866,null,650,40866,50866,60866,70866,80866,90866]
[null,450,40545,50545,60545,70545,80545,90545,13,1300,40913,50913,60913,70913,80913,90913,null,"650+850",41465,51465,61465,71465,81465,91465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,9,8,6,3,7,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,6,null,1,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW75=0,\"\",\"\")","v":""},"","","","","","","","","","","",1200,650,{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31977,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV75=\"\",0,IF('Zenergy-OE'!AX75>0,'Zenergy-OE'!AV75,0))","v":0},{"$f":"'Zenergy-OE'!AX75","v":0},{"$f":"IF(EK89>1,VLOOKUP(IF(ISNUMBER(EK89),TEXT(EK89,\"0\"),EK89),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK89>1,VLOOKUP(IF(ISNUMBER(EK89),TEXT(EK89,\"0\"),EK89),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,600,40560,50560,60560,70560,80560,90560,14,"650+612",40965,50965,60965,70965,80965,90965,null,"850+850",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,10,8,6,3,10,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW75=0,\"\",\"\")","v":""},"","","","","","","","","","","",1300,800,{"$f":"\"\"","v":""},20208,20218,20228,20238,20248,20258,20178,20188,33168,33188,{"$f":"\"\"","v":""},31958,30985,30980,31088,31978,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV78=\"\",0,IF('Zenergy-OE'!AX78>0,'Zenergy-OE'!AV78,0))","v":0},{"$f":"'Zenergy-OE'!AX78","v":0},{"$f":"IF(EK90>1,VLOOKUP(IF(ISNUMBER(EK90),TEXT(EK90,\"0\"),EK90),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK90>1,VLOOKUP(IF(ISNUMBER(EK90),TEXT(EK90,\"0\"),EK90),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL90*EN90","v":0},null,null,"650+150",40866,50866,60866,70866,80866,90866,null,"650+150",40165,50165,60165,70165,80165,90165]
[null,650,40565,50565,60565,70565,80565,90565,15,"650+812",40985,50985,60985,70985,80985,90985,null,"650+300",41495,51495,61495,71495,81495,91495,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV91=2,31931,0)","v":0},null,3,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+612","650+150",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31978,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV81=\"\",0,IF('Zenergy-OE'!AX81>0,'Zenergy-OE'!AV81,0))","v":0},{"$f":"'Zenergy-OE'!AX81","v":0},{"$f":"IF(EK91>1,VLOOKUP(IF(ISNUMBER(EK91),TEXT(EK91,\"0\"),EK91),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK91>1,VLOOKUP(IF(ISNUMBER(EK91),TEXT(EK91,\"0\"),EK91),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,850,40886,50886,60886,70886,80886,90886,null,850,40886,50886,60886,70886,80886,90886]
[null,800,40580,50580,60580,70580,80580,90580,16,"850+812",40985,50985,60985,70985,80985,90985,null,"650+400",41411,51411,61411,71411,81411,91411,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BV91=3,31932,0)","v":31932},null,null,"Zestaw połączeniowy",null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE90<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+812",850,{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,33199,31959,30995,30990,31089,31979,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV84=\"\",0,IF('Zenergy-OE'!AX84>0,'Zenergy-OE'!AV84,0))","v":0},{"$f":"'Zenergy-OE'!AX84","v":0},{"$f":"IF(EK92>1,VLOOKUP(IF(ISNUMBER(EK92),TEXT(EK92,\"0\"),EK92),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK92>1,VLOOKUP(IF(ISNUMBER(EK92),TEXT(EK92,\"0\"),EK92),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+200",40866,50866,60866,70866,80866,90866,null,"650+200",40165,50165,60165,70165,80165,90165]
[null,"650+150",40580,50580,60580,70580,80580,90580,17,"650+300",40930,50930,60930,70930,80930,90930,null,"850+300",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$95:$AS$97),$BA$4,$BV$19)","v":1},"Boki obudowy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(BT91:BT92)","v":31932},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W 800 - 6","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.","850+812","650+200",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31086,31979,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV87=\"\",0,IF('Zenergy-OE'!AX87>0,'Zenergy-OE'!AV87,0))","v":0},{"$f":"'Zenergy-OE'!AX87","v":0},{"$f":"IF(EK93>1,VLOOKUP(IF(ISNUMBER(EK93),TEXT(EK93,\"0\"),EK93),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK93>1,VLOOKUP(IF(ISNUMBER(EK93),TEXT(EK93,\"0\"),EK93),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,850,40585,50585,60585,70585,80585,90585,18,"650+400",40940,50940,60940,70940,80940,90940,null,"850+400",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IP","Brak","B.pełny","B.went.","Pełny st.","Went.st.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BT93>1,BT93,0)","v":31932},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zestaw tulejkowy\",\"Tubular\")","v":"Zestaw tulejkowy"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,1000,{"$f":"\"\"","v":""},20200,20210,20220,20230,20240,20250,20170,20180,33160,33180,{"$f":"\"\"","v":""},31950,30916,30910,31080,31970,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV90=\"\",0,IF('Zenergy-OE'!AX90>0,'Zenergy-OE'!AV90,0))","v":0},{"$f":"'Zenergy-OE'!AX90","v":0},{"$f":"IF(EK94>1,VLOOKUP(IF(ISNUMBER(EK94),TEXT(EK94,\"0\"),EK94),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK94>1,VLOOKUP(IF(ISNUMBER(EK94),TEXT(EK94,\"0\"),EK94),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+200",40585,50585,60585,70585,80585,90585,19,"850+300",40930,50930,60930,70930,80930,90930,null,"650+150+300",41480,51480,61480,71480,81480,91480,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,8,1,2,5,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zestaw płytkowy\",\"Flat plate\")","v":"Zestaw płytkowy"},null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osłona pełna",{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,1200,{"$f":"\"\"","v":""},20201,20211,20221,20231,20241,20251,20171,20181,33161,33181,{"$f":"\"\"","v":""},31951,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31081,31971,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!AV93=\"\",0,IF('Zenergy-OE'!AX93>0,'Zenergy-OE'!AV93,0))","v":0},{"$f":"'Zenergy-OE'!AX93","v":0},{"$f":"IF(EK95>1,VLOOKUP(IF(ISNUMBER(EK95),TEXT(EK95,\"0\"),EK95),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK95>1,VLOOKUP(IF(ISNUMBER(EK95),TEXT(EK95,\"0\"),EK95),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1000,40510,50510,60510,70510,80510,90510,20,"850+400",40940,50940,60940,70940,80940,90940,null,"650+150+400",41480,51480,61480,71480,81480,91480,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,8,4,3,5,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. modułowa",{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,1300,{"$f":"\"\"","v":""},20202,20212,20222,20232,20242,20252,20172,20182,33162,33182,{"$f":"\"\"","v":""},31952,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31082,31972,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,"Akcesoria",{"$f":"IF('Zenergy-OE'!X36=\"\",0,IF('Zenergy-OE'!X36>0,'Zenergy-OE'!X36,0))","v":0},{"$f":"IF('Zenergy-OE'!Z36=\"\",0,'Zenergy-OE'!Z36)","v":0},{"$f":"IF(EK96>1,VLOOKUP(IF(ISNUMBER(EK96),TEXT(EK96,\"0\"),EK96),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK96>1,VLOOKUP(IF(ISNUMBER(EK96),TEXT(EK96,\"0\"),EK96),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+650",40866,50866,60866,70866,80866,90866,null,"650+650",40866,50866,60866,70866,80866,90866]
[null,1200,40512,50512,60512,70512,80512,90512,21,"150+650+300",40930,50930,60930,70930,80930,90930,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,8,4,8,5,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. przeszklona",{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"650+650",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31972,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X39=\"\",0,IF('Zenergy-OE'!Z39>0,'Zenergy-OE'!X39,0))","v":0},{"$f":"IF('Zenergy-OE'!Z39=\"\",0,'Zenergy-OE'!Z39)","v":0},{"$f":"IF(EK97>1,VLOOKUP(IF(ISNUMBER(EK97),TEXT(EK97,\"0\"),EK97),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK97>1,VLOOKUP(IF(ISNUMBER(EK97),TEXT(EK97,\"0\"),EK97),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+850",40866,50866,60866,70866,80866,90866,null,"650+850",40886,50886,60886,70886,80886,90886]
[null,1300,40513,50513,60513,70513,80513,90513,22,"150+650+400",40940,50940,60940,70940,80940,90940,null,"Szerokość obudowy","Osłona tylna pełna IP55   Wysokość",null,null,8,null,"Pole 1,3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna stała TS35",{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"650+850",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31966,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X42=\"\",0,IF('Zenergy-OE'!Z42>0,'Zenergy-OE'!X42,0))","v":0},{"$f":"IF('Zenergy-OE'!Z42=\"\",0,'Zenergy-OE'!Z42)","v":0},{"$f":"IF(EK98>1,VLOOKUP(IF(ISNUMBER(EK98),TEXT(EK98,\"0\"),EK98),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK98>1,VLOOKUP(IF(ISNUMBER(EK98),TEXT(EK98,\"0\"),EK98),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+850",40886,50886,60886,70886,80886,90886,null,"850+850",40886,50886,60886,70886,80886,90886]
[null,"650+612",40565,50565,60565,70565,80565,90565,23,null,null,null,null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna reg.TS35",{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"850+850",{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,33199,31957,30995,30990,31089,31967,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X45=\"\",0,IF('Zenergy-OE'!Z45>0,'Zenergy-OE'!X45,0))","v":0},{"$f":"IF('Zenergy-OE'!Z45=\"\",0,'Zenergy-OE'!Z45)","v":0},{"$f":"IF(EK99>1,VLOOKUP(IF(ISNUMBER(EK99),TEXT(EK99,\"0\"),EK99),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK99>1,VLOOKUP(IF(ISNUMBER(EK99),TEXT(EK99,\"0\"),EK99),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+300",40866,50866,60866,70866,80866,90866,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+812",40565,50565,60565,70565,80565,90565,24,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX(($AO$102:$AO$117),$BA$10,$AN$101)","v":0},"Obudowy łączone drzwi",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,11,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta ocynk pełna",{"$f":"IF(CW93=0,\"\",\"\")","v":""},33082,33083,33084,33085,33086,{"$f":"IF(DC93=0,\"\",\"\")","v":""},33087,{"$f":"IF(DE93=0,\"\",\"\")","v":""},33088,{"$f":"IF(DG93=0,\"\",\"\")","v":""},33089,null,"650+300",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31969,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X48=\"\",0,IF('Zenergy-OE'!Z48>0,'Zenergy-OE'!X48,0))","v":0},{"$f":"IF('Zenergy-OE'!Z48=\"\",0,'Zenergy-OE'!Z48)","v":0},{"$f":"IF(EK100>1,VLOOKUP(IF(ISNUMBER(EK100),TEXT(EK100,\"0\"),EK100),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK100>1,VLOOKUP(IF(ISNUMBER(EK100),TEXT(EK100,\"0\"),EK100),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+400",40866,50866,60866,70866,80866,90866,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+812",40585,50585,60585,70585,80585,90585,25,98,40995,50995,60995,70995,80995,90995,null,300,41530,51530,61530,71530,81530,91530,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Brak",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Prąd",null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta malow.otw.",{"$f":"IF(CW93=0,\"\",\"\")","v":""},33582,33583,33584,33585,33586,{"$f":"IF(DC93=0,\"\",\"\")","v":""},33587,{"$f":"IF(DE93=0,\"\",\"\")","v":""},33588,{"$f":"IF(DG93=0,\"\",\"\")","v":""},33589,null,"650+400",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31960,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X51=\"\",0,IF('Zenergy-OE'!Z51>0,'Zenergy-OE'!X51,0))","v":0},{"$f":"IF('Zenergy-OE'!Z51=\"\",0,'Zenergy-OE'!Z51)","v":0},{"$f":"IF(EK101>1,VLOOKUP(IF(ISNUMBER(EK101),TEXT(EK101,\"0\"),EK101),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK101>1,VLOOKUP(IF(ISNUMBER(EK101),TEXT(EK101,\"0\"),EK101),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+300",40886,50886,60886,70886,80886,90886,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+300",40565,50565,60565,70565,80565,90565,26,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,400,41540,51540,61540,71540,81540,91540,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"630 A",null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta oc. pozioma",{"$f":"IF(CW92=0,\"\",\"\")","v":""},"","","","","","","","",{"$f":"IF(DF377=0,\"\",\"\")","v":""},{"$f":"IF(DG377=0,\"\",\"\")","v":""},{"$f":"IF(DH377=0,\"\",\"\")","v":""},null,"850+300",{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,33199,31957,30995,30990,31089,31961,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X54=\"\",0,IF('Zenergy-OE'!Z54>0,'Zenergy-OE'!X54,0))","v":0},{"$f":"IF('Zenergy-OE'!Z54=\"\",0,'Zenergy-OE'!Z54)","v":0},{"$f":"IF(EK102>1,VLOOKUP(IF(ISNUMBER(EK102),TEXT(EK102,\"0\"),EK102),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK102>1,VLOOKUP(IF(ISNUMBER(EK102),TEXT(EK102,\"0\"),EK102),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"850+400",40886,50886,60886,70886,80886,90886,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+400",40565,50565,60565,70565,80565,90565,27,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,450,41545,51545,61545,71545,81545,91545,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1000 A",null,null,null,null,{"$f":"IF(CE108=14,14,IF(CP41=1,$BA$15,CB108))","v":1},null,null,{"$f":"IF(CP41=1,BD4,CE108)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa","","","","","","","","","","","","",null,"850+400",{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,33199,31957,30995,30990,31089,31963,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X57=\"\",0,IF('Zenergy-OE'!Z57>0,'Zenergy-OE'!X57,0))","v":0},{"$f":"IF('Zenergy-OE'!Z57=\"\",0,'Zenergy-OE'!Z57)","v":0},{"$f":"IF(EK103>1,VLOOKUP(IF(ISNUMBER(EK103),TEXT(EK103,\"0\"),EK103),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK103>1,VLOOKUP(IF(ISNUMBER(EK103),TEXT(EK103,\"0\"),EK103),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"150+650+300",40866,50866,60866,70866,80866,90866,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+300",40585,50585,60585,70585,80585,90585,28,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,41560,51560,61560,71560,81560,91560,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1600 A",null,null,null,null,{"$f":"IF(CE107=14,25,IF(CO41=1,$BA$12,CB107))","v":1},null,null,{"$f":"IF(CO41=1,BD4,CE107)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"150+650+300",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31962,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X60=\"\",0,IF('Zenergy-OE'!Z60>0,'Zenergy-OE'!X60,0))","v":0},{"$f":"IF('Zenergy-OE'!Z60=\"\",0,'Zenergy-OE'!Z60)","v":0},{"$f":"IF(EK104>1,VLOOKUP(IF(ISNUMBER(EK104),TEXT(EK104,\"0\"),EK104),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK104>1,VLOOKUP(IF(ISNUMBER(EK104),TEXT(EK104,\"0\"),EK104),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL104*EN104","v":0},null,null,"150+650+400",40866,50866,60866,70866,80866,90866,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+400",40585,50585,60585,70585,80585,90585,29,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,{"$f":"\"\"","v":""},null,650,41565,51565,61565,71565,81565,91565,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2500 A",null,null,null,null,{"$f":"IF(CE106=14,23,IF(CN41=1,$BA$13,CB106))","v":1},null,null,{"$f":"IF(CN41=1,BD4,CE106)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"150+650+400",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31971,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X63=\"\",0,IF('Zenergy-OE'!Z63>0,'Zenergy-OE'!X63,0))","v":0},{"$f":"IF('Zenergy-OE'!Z63=\"\",0,'Zenergy-OE'!Z63)","v":0},{"$f":"IF(EK105>1,VLOOKUP(IF(ISNUMBER(EK105),TEXT(EK105,\"0\"),EK105),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK105>1,VLOOKUP(IF(ISNUMBER(EK105),TEXT(EK105,\"0\"),EK105),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,"150+650+300",40580,50580,60580,70580,80580,90580,30,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,41580,51580,61580,71580,81580,91580,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,7,null,1,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,{"$f":"\"\"","v":""},{"$f":"IF(DL105=0,\"\",\"\")","v":""},"","","",{"$f":"IF(DP105=0,\"\",\"\")","v":""},{"$f":"IF(DQ105=0,\"\",\"\")","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"IF(DT105=0,\"\",\"\")","v":""},"","","",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"IF(DY105=0,\"\",\"\")","v":""},{"$f":"IF(EA105=0,\"\",\"\")","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X66=\"\",0,IF('Zenergy-OE'!Z66>0,'Zenergy-OE'!X66,0))","v":0},{"$f":"IF('Zenergy-OE'!Z66=\"\",0,'Zenergy-OE'!Z66)","v":0},{"$f":"IF(EK106>1,VLOOKUP(IF(ISNUMBER(EK106),TEXT(EK106,\"0\"),EK106),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK106>1,VLOOKUP(IF(ISNUMBER(EK106),TEXT(EK106,\"0\"),EK106),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0]
[null,"150+650+400",40580,50580,60580,70580,80580,90580,31,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+150",41580,51580,61580,71580,81580,91580,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,"Pole 3",null,null,null,null,null,null,{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,{"$f":"\"\"","v":""},"","","","",{"$f":"IF(DP106=0,\"\",\"\")","v":""},{"$f":"IF(DQ106=0,\"\",\"\")","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},"","","","",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"IF(DZ106=0,\"\",\"\")","v":""},{"$f":"IF(EA106=0,\"\",\"\")","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,{"$f":"IF('Zenergy-OE'!X69=\"\",0,IF('Zenergy-OE'!Z69>0,'Zenergy-OE'!X69,0))","v":0},{"$f":"IF('Zenergy-OE'!Z69=\"\",0,'Zenergy-OE'!Z69)","v":0},{"$f":"IF(EK107>1,VLOOKUP(IF(ISNUMBER(EK107),TEXT(EK107,\"0\"),EK107),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK107>1,VLOOKUP(IF(ISNUMBER(EK107),TEXT(EK107,\"0\"),EK107),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Szerokość obudowy","Rama rozł. iistw. z analizatorami  Wysokość, Pole 1,3",null,null,null,7,null,null,"Szerokość obudowy","Rama rozł. iistw. z analizatorami  Wysokość, Pole 2",null,null,null,7]
[null,null,null,null,null,null,null,null,32,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,850,41585,51585,61585,71585,81585,91585,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,{"$f":"IF(BV6>3,1,0)","v":0},{"$f":"IF(CM108=1,SUM(CN109:CN114),0)","v":0},null,"Ilość mod.przód",null,null,null,null,null,null,{"$f":"IF(CW93=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X72=\"\",0,IF('Zenergy-OE'!Z72>0,'Zenergy-OE'!X72,0))","v":0},{"$f":"IF('Zenergy-OE'!Z72=\"\",0,'Zenergy-OE'!Z72)","v":0},{"$f":"IF(EK108>1,VLOOKUP(IF(ISNUMBER(EK108),TEXT(EK108,\"0\"),EK108),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK108>1,VLOOKUP(IF(ISNUMBER(EK108),TEXT(EK108,\"0\"),EK108),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,null,null,null,null,null,null,null,33,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+200",41585,51585,61585,71585,81585,91585,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+150",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE107<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=1,20,0)","v":0},{"$f":"IF(BD4=1,0,0)","v":0},null,1,{"$f":"IF(BA15>1,'Zenergy-OE'!AX42/(Zbaza!AM1),0)","v":0},{"$f":"IF(CB6>4,0,IF(CE6<13,CE6,0))","v":1},{"$f":"CQ109*CR109","v":0},{"$f":"SUM(CS109:CS120)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X75=\"\",0,IF('Zenergy-OE'!Z75>0,'Zenergy-OE'!X75,0))","v":0},{"$f":"IF('Zenergy-OE'!Z75=\"\",0,'Zenergy-OE'!Z75)","v":0},{"$f":"IF(EK109>1,VLOOKUP(IF(ISNUMBER(EK109),TEXT(EK109,\"0\"),EK109),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK109>1,VLOOKUP(IF(ISNUMBER(EK109),TEXT(EK109,\"0\"),EK109),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,34,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,41510,51510,61510,71510,81510,91510,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=2,24,0)","v":0},{"$f":"IF(BD4=2,0,0)","v":0},null,2,{"$f":"IF(BA15>1,'Zenergy-OE'!AX45/(Zbaza!AM1),0)","v":0},{"$f":"IF(CB23>4,0,IF(CE23<13,CE23,0))","v":1},0,{"$f":"IF(CT109<=CM115,CT109,CM115)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X78=\"\",0,IF('Zenergy-OE'!Z78>0,'Zenergy-OE'!X78,0))","v":0},{"$f":"IF('Zenergy-OE'!Z78=\"\",0,'Zenergy-OE'!Z78)","v":0},{"$f":"IF(EK110>1,VLOOKUP(IF(ISNUMBER(EK110),TEXT(EK110,\"0\"),EK110),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK110>1,VLOOKUP(IF(ISNUMBER(EK110),TEXT(EK110,\"0\"),EK110),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},{"$f":"EL110*EN110","v":0},null,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy","Drzwi przeszklone IP55   Wysokość",null,null,3,null,"Pole 1,3",35,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,41512,51512,61512,71512,81512,91512,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+200",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=3,28,0)","v":0},{"$f":"IF(BD4=3,5,0)","v":0},null,3,{"$f":"IF(BA15>1,'Zenergy-OE'!AX48/(Zbaza!AM1),0)","v":0},{"$f":"IF(CB40>4,0,IF(CE40<13,CE40,0))","v":1},0,{"$f":"IF(CT110=CM115,CT109-CT110,\"\")","v":""},null,"W 850 - 7+13","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X81=\"\",0,IF('Zenergy-OE'!Z81>0,'Zenergy-OE'!X81,0))","v":0},{"$f":"IF('Zenergy-OE'!Z81=\"\",0,'Zenergy-OE'!Z81)","v":0},{"$f":"IF(EK111>1,VLOOKUP(IF(ISNUMBER(EK111),TEXT(EK111,\"0\"),EK111),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK111>1,VLOOKUP(IF(ISNUMBER(EK111),TEXT(EK111,\"0\"),EK111),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",36,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,41513,51513,61513,71513,81513,91513,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=4,32,0)","v":0},{"$f":"IF(BD4=4,9,0)","v":0},null,4,{"$f":"IF(BA15>1,'Zenergy-OE'!AX51/(Zbaza!AM1),0)","v":0},{"$f":"IF(CB57>4,0,IF(CE57<13,CE57,0))","v":1},0,{"$f":"IF(BV6=4,\"\",CT110)","v":0},null,"Brak",{"$f":"IF(CW111=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X84=\"\",0,IF('Zenergy-OE'!Z84>0,'Zenergy-OE'!X84,0))","v":0},{"$f":"IF('Zenergy-OE'!Z84=\"\",0,'Zenergy-OE'!Z84)","v":0},{"$f":"IF(EK112>1,VLOOKUP(IF(ISNUMBER(EK112),TEXT(EK112,\"0\"),EK112),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK112>1,VLOOKUP(IF(ISNUMBER(EK112),TEXT(EK112,\"0\"),EK112),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,450,40745,50745,60745,70745,80745,90745,null,450,40745,50745,60745,70745,80745,90745]
[null,"Brak",{"$f":"IF(C112=0,\"\",\"\")","v":""},"","","","","",37,98,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+650",41565,51565,61565,71565,81565,91565,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=5,36,0)","v":36},{"$f":"IF(BD4=5,13,0)","v":13},null,5,{"$f":"IF(BA15>1,'Zenergy-OE'!AX54/(Zbaza!AM1),0)","v":0},{"$f":"IF(CB74>4,0,IF(CE74<13,CE74,0))","v":1},0,null,null,"Osłona pełna",32910,32920,32930,32940,32950,32960,32970,32980,32990,32991,32992,32993,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X87=\"\",0,IF('Zenergy-OE'!Z87>0,'Zenergy-OE'!X87,0))","v":0},{"$f":"IF('Zenergy-OE'!Z87=\"\",0,'Zenergy-OE'!Z87)","v":0},{"$f":"IF(EK113>1,VLOOKUP(IF(ISNUMBER(EK113),TEXT(EK113,\"0\"),EK113),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK113>1,VLOOKUP(IF(ISNUMBER(EK113),TEXT(EK113,\"0\"),EK113),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,"","","","","","",38,"650+612",40995,50995,60995,70995,80995,90995,null,"650+850",41565,51565,61565,71565,81565,91565,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,{"$f":"IF(BD4=6,40,0)","v":0},{"$f":"IF(BD4=6,17,0)","v":0},null,6,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX57/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB91>4,0,IF(CE91<13,CE91,0))","v":1},0,null,null,"Osł. modułowa",{"$f":"IF(CW111=0,\"\",\"\")","v":""},32925,32935,32945,32955,{"$f":"IF(DB113=0,\"\",\"\")","v":""},"","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X90=\"\",0,IF('Zenergy-OE'!Z90>0,'Zenergy-OE'!X90,0))","v":0},{"$f":"IF('Zenergy-OE'!Z90=\"\",0,'Zenergy-OE'!Z90)","v":0},{"$f":"IF(EK114>1,VLOOKUP(IF(ISNUMBER(EK114),TEXT(EK114,\"0\"),EK114),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK114>1,VLOOKUP(IF(ISNUMBER(EK114),TEXT(EK114,\"0\"),EK114),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,650,40765,50765,60765,70765,80765,90765,null,650,40765,50765,60765,70765,80765,90765]
[null,400,40640,50640,60640,70640,80640,90640,39,"650+812",40995,50995,60995,70995,80995,90995,null,"850+850",41585,51585,61585,71585,81585,91585,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+650",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,{"$f":"IF(CN108=0,SUM(CM109:CM114),CN108)","v":36},{"$f":"CT108-CM115","v":-36},null,7,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX60/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB108>4,0,IF(CE108<13,CE108,0))","v":1},0,null,null,"Osł. przeszklona",{"$f":"IF(CW111=0,\"\",\"\")","v":""},{"$f":"IF(CX111=0,\"\",\"\")","v":""},32939,32949,{"$f":"IF(DA111=0,\"\",\"\")","v":""},32969,{"$f":"IF(DC111=0,\"\",\"\")","v":""},32979,{"$f":"IF(DE111=0,\"\",\"\")","v":""},32989,{"$f":"IF(DG111=0,\"\",\"\")","v":""},32999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X93=\"\",0,IF('Zenergy-OE'!Z93>0,'Zenergy-OE'!X93,0))","v":0},{"$f":"IF('Zenergy-OE'!Z93=\"\",0,'Zenergy-OE'!Z93)","v":0},{"$f":"IF(EK115>1,VLOOKUP(IF(ISNUMBER(EK115),TEXT(EK115,\"0\"),EK115),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK115>1,VLOOKUP(IF(ISNUMBER(EK115),TEXT(EK115,\"0\"),EK115),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,450,40645,50645,60645,70645,80645,90645,40,"850+812",40995,50995,60995,70995,80995,90995,null,"650+300",41595,51595,61595,71595,81595,91595,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+850",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,{"$f":"IF(BV6=4,\"\",CN115)","v":-36},null,null,8,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX63/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB125>4,0,IF(CE125<13,CE125,0))","v":1},0,null,null,"Szyna stała TS35",32900,32900,32900,32900,32900,32900,32900,32900,32900,32900,32900,32900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!X21=\"\",0,IF('Zenergy-OE'!Z21>0,'Zenergy-OE'!X21,0))","v":0},{"$f":"IF('Zenergy-OE'!Z21=\"\",0,'Zenergy-OE'!Z21)","v":0},{"$f":"IF(EK116>1,VLOOKUP(IF(ISNUMBER(EK116),TEXT(EK116,\"0\"),EK116),Cennik!$A$4:$F$52318,2,FALSE),\"\")","v":""},{"$f":"IF(EK116>1,VLOOKUP(IF(ISNUMBER(EK116),TEXT(EK116,\"0\"),EK116),Cennik!$A$4:$F$52318,3,FALSE),0)","v":0},0,null,null,"650+150",40765,50765,60765,70765,80765,90765,null,"650+150",40165,50165,60165,70165,80165,90165]
[null,600,40660,50660,60660,70660,80660,90660,41,"650+300",40995,50995,60995,70995,80995,90995,null,"650+400",41511,51511,61511,71511,81511,91511,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+850",1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,9,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX66/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB142>4,0,IF(CE142<13,CE142,0))","v":1},0,null,null,"Szyna reg.TS35",32905,32905,32905,32905,32905,32905,32905,32905,32905,32905,32905,32905,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,40785,50785,60785,70785,80785,90785,null,850,40785,50785,60785,70785,80785,90785]
[null,650,40665,50665,60665,70665,80665,90665,42,"650+400",40995,50995,60995,70995,80995,90995,null,"850+300",41585,51585,61585,71585,81585,91585,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,10,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX69/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB159>4,0,IF(CE159<13,CE159,0))","v":1},0,null,null,"Płyta ocynk pełna",{"$f":"IF(CW111=0,\"\",\"\")","v":""},33092,33093,33094,33095,33096,{"$f":"IF(DC111=0,\"\",\"\")","v":""},33097,{"$f":"IF(DE111=0,\"\",\"\")","v":""},33098,{"$f":"IF(DG111=0,\"\",\"\")","v":""},33099,null,"Akcesoria tył, Pole 2","Brak","Izolator 3P, most pionowy na plecach","Izolator 4P, most pionowy na plecach","Izolator 3P, most pionowy na plecach regulowany","Izolator 4P, most pionowy na plecach regulowany","Izolator 3P, podpora mostu na plecach, regulowana","Izolator 4P, podpora mostu na plecach, regulowana","Izol. AlCubar 630A 3P pionowo na plecach","Izol. AlCubar 630A 4P pionowo na plecach","Drabinka kablowa na plecach","Drabinka kablowa na drzwi","Drabinka kablowa pod osłonę","Metalowa kieszeń na dokumentację","Pionowy zestaw szyn TS35, 6M","Poziomy zestaw dwóch szyn TS35","Osłona mostu poziomego","Zestaw mocowania do ściany",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+200",40765,50765,60765,70765,80765,90765,null,"650+200",40165,50165,60165,70165,80165,90165]
[null,800,40680,50680,60680,70680,80680,90680,43,"850+300",40995,50995,60995,70995,80995,90995,null,"850+400",41585,51585,61585,71585,81585,91585,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,11,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX72/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB176>4,0,IF(CE176<13,CE176,0))","v":1},0,null,null,"Płyta malow.otw.",{"$f":"IF(CW111=0,\"\",\"\")","v":""},33592,33593,33594,33595,33596,{"$f":"IF(DC111=0,\"\",\"\")","v":""},33597,{"$f":"IF(DE111=0,\"\",\"\")","v":""},33598,{"$f":"IF(DG111=0,\"\",\"\")","v":""},33599,null,"Szerokość obudowy",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+150",40680,50680,60680,70680,80680,90680,44,"850+400",40995,50995,60995,70995,80995,90995,null,"650+150+300",41580,51580,61580,71580,81580,91580,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE125=14,14,IF(CP42=1,$BA$15,CB125))","v":1},null,null,{"$f":"IF(CP42=1,BD4,CE125)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,12,{"$f":"IF($BA$15>1,'Zenergy-OE'!AX75/(Zbaza!$AM$1),0)","v":0},{"$f":"IF(CB193>4,0,IF(CE193<13,CE193,0))","v":1},0,null,null,"Płyta oc. pozioma",33791,33792,33793,33794,33795,33796,33797,33798,null,33799,{"$f":"IF(DG292=0,\"\",\"\")","v":""},{"$f":"IF(DH292=0,\"\",\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,850,40685,50685,60685,70685,80685,90685,45,"150+650+300",40995,50995,60995,70995,80995,90995,null,"650+150+400",41580,51580,61580,71580,81580,91580,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE124=14,25,IF(CO42=1,$BA$12,CB124))","v":1},null,null,{"$f":"IF(CO42=1,BD4,CE124)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa",33209,33209,33209,33209,33209,33209,33209,33209,33209,33209,33209,33209,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+200",40685,50685,60685,70685,80685,90685,46,"150+650+400",40995,50995,60995,70995,80995,90995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE123=14,23,IF(CN42=1,$BA$13,CB123))","v":1},null,null,{"$f":"IF(CN42=1,BD4,CE123)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW111=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(EO5:EO116)","v":8639.7999999999993},null,null,"650+650",40765,50765,60765,70765,80765,90765,null,"650+650",40765,50765,60765,70765,80765,90765]
[null,1000,40610,50610,60610,70610,80610,90610,47,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,8,null,1,8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW111=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,"Rabat",0.2,{"$f":"EO122*(1-EN123)","v":6911.84},null,null,"650+850",40765,50765,60765,70765,80765,90765,null,"650+850",40785,50785,60785,70785,80785,90785]
[null,1200,40612,50612,60612,70612,80612,90612,48,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW111=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},33163,33183,{"$f":"\"\"","v":""},31953,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31083,31973,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"850+850",40785,50785,60785,70785,80785,90785,null,"850+850",40785,50785,60785,70785,80785,90785]
[null,1300,40613,50613,60613,70613,80613,90613,49,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW111=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,400,{"$f":"\"\"","v":""},20204,20214,20224,20234,20244,20254,20174,20184,33164,33184,33194,31954,30944,30940,31084,31974,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"650+300",40765,50765,60765,70765,80765,90765,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+612",40665,50665,60665,70665,80665,90665,50,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE124<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW111=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,450,{"$f":"\"\"","v":""},20205,20215,20225,20235,20245,20255,20175,20185,33165,33185,33195,31955,30954,30950,31085,31975,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"650+400",40765,50765,60765,70765,80765,90765,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+812",40665,50665,60665,70665,80665,90665,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,{"$f":"\"\"","v":""},20206,20216,20226,20236,20246,20256,20176,20186,33166,33186,{"$f":"\"\"","v":""},31956,30964,30960,31086,31976,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"850+300",40785,50785,60785,70785,80785,90785,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+812",40685,50685,60685,70685,80685,90685,null,"Szerokość obudowy","Daszek obudowy",null,null,null,null,null,null,"Szerokość obudowy","Osłona tylna went. IP30   Wysokość",null,null,5,null,"Pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650,{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,33197,31957,30974,30970,31087,31977,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"850+400",40785,50785,60785,70785,80785,90785,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+300",40665,50665,60665,70665,80665,90665,null,null,230,300,400,600,800,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W 1000 - 8","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,800,{"$f":"\"\"","v":""},20208,20218,20228,20238,20248,20258,20178,20188,33168,33188,{"$f":"\"\"","v":""},31958,30985,30980,31088,31978,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"150+650+300",40765,50765,60765,70765,80765,90765,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+400",40665,50665,60665,70665,80665,90665,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"IF(CW129=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,"650+150",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,{"$f":"\"\"","v":""},31957,30974,30970,31087,31978,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"150+650+400",40765,50765,60765,70765,80765,90765,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+300",40685,50685,60685,70685,80685,90685,null,300,30723,30733,30743,30763,30783,null,null,300,41330,51330,61330,71330,81330,91330,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osłona pełna",32110,32120,32130,32140,32150,32160,32170,32180,32190,32191,32192,32193,null,850,{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,33199,31959,30995,30990,31089,31979,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+400",40685,50685,60685,70685,80685,90685,null,400,30724,30734,30744,30764,30784,null,null,400,41340,51340,61340,71340,81340,91340,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. modułowa",{"$f":"IF(CW129=0,\"\",\"\")","v":""},32125,32135,32145,32155,{"$f":"IF(DB131=0,\"\",\"\")","v":""},"","","","","","",null,"650+200",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,{"$f":"\"\"","v":""},31957,30974,30970,31086,31979,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+300",40680,50680,60680,70680,80680,90680,null,450,30725,30735,30745,30765,30785,null,null,450,41345,51345,61345,71345,81345,91345,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. przeszklona",{"$f":"IF(CW129=0,\"\",\"\")","v":""},{"$f":"IF(CX129=0,\"\",\"\")","v":""},32139,32149,{"$f":"IF(DA129=0,\"\",\"\")","v":""},32169,{"$f":"IF(DC129=0,\"\",\"\")","v":""},32179,{"$f":"IF(DE129=0,\"\",\"\")","v":""},32189,{"$f":"IF(DG129=0,\"\",\"\")","v":""},32199,null,1000,{"$f":"\"\"","v":""},20200,20210,20220,20230,20240,20250,20170,20180,33160,33180,{"$f":"\"\"","v":""},31950,30916,30910,31080,31970,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"Szerokość obudowy","Rama rozł. listw. z analiz. do plomb. Wysokość, Pole 1,3",null,null,null,8,null,null,"Szerokość obudowy","Rama rozł. listw. z analiz. do plomb. Wysokość, Pole 2",null,null,null,8]
[null,"150+650+400",40680,50680,60680,70680,80680,90680,null,600,30726,30736,30746,30766,30786,null,null,600,41360,51360,61360,71360,81360,91360,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna stała TS35",32100,32100,32100,32100,32100,32100,32100,32100,32100,32100,32100,32100,null,1200,{"$f":"\"\"","v":""},20201,20211,20221,20231,20241,20251,20171,20181,33161,33181,{"$f":"\"\"","v":""},31951,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31081,31971,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,null,null,null,null,null,null,null,null,650,30727,30737,30747,30767,30787,null,null,650,41365,51365,61365,71365,81365,91365,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna reg.TS35",32105,32105,32105,32105,32105,32105,32105,32105,32105,32105,32105,32105,null,1300,{"$f":"\"\"","v":""},20202,20212,20222,20232,20242,20252,20172,20182,33162,33182,{"$f":"\"\"","v":""},31952,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31082,31972,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,800,30728,30738,30748,30768,30788,null,null,800,41380,51380,61380,71380,81380,91380,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta ocynk pełna",{"$f":"IF(CW132=0,\"\",\"\")","v":""},33012,33013,33014,33015,33016,{"$f":"IF(DC132=0,\"\",\"\")","v":""},33017,{"$f":"IF(DE132=0,\"\",\"\")","v":""},33018,{"$f":"IF(DG132=0,\"\",\"\")","v":""},33019,null,"650+650",{"$f":"\"\"","v":""},20207,20217,20227,20237,20247,20257,20177,20187,33167,33187,{"$f":"\"\"","v":""},{"$f":"IF(DW135=0,\"\",\"\")","v":""},30974,30970,31087,31972,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"650+150",30728,30738,30748,30768,30788,null,null,"650+150",41380,51380,61380,71380,81380,91380,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE142=14,14,IF(CP43=1,$BA$15,CB142))","v":1},null,null,{"$f":"IF(CP43=1,BD4,CE142)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta malow.otw.",{"$f":"IF(CW136=0,\"\",\"\")","v":""},33512,33513,33514,33515,33516,{"$f":"IF(DC133=0,\"\",\"\")","v":""},33517,{"$f":"IF(DE133=0,\"\",\"\")","v":""},33518,{"$f":"IF(DG133=0,\"\",\"\")","v":""},33519,null,"650+850",{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,{"$f":"\"\"","v":""},{"$f":"IF(DW136=0,\"\",\"\")","v":""},30995,30990,31089,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,850,30729,30739,30749,30769,30789,null,null,850,41385,51385,61385,71385,81385,91385,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE141=14,25,IF(CO43=1,$BA$12,CB141))","v":1},null,null,{"$f":"IF(CO43=1,BD4,CE141)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta oc. pozioma",33711,33712,33713,33714,33715,33716,33717,33718,"",33719,"","",null,"850+850",{"$f":"\"\"","v":""},20209,20219,20229,20239,20249,20259,20179,20189,33169,33189,{"$f":"\"\"","v":""},{"$f":"IF(DW137=0,\"\",\"\")","v":""},30995,30990,31089,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,450,40746,50746,60746,70746,80746,90746,null,450,40746,50746,60746,70746,80746,90746]
[null,null,null,null,null,null,null,null,null,"650+200",30729,30739,30749,30769,30789,null,null,"650+200",41385,51385,61385,71385,81385,91385,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE140=14,23,IF(CN43=1,$BA$13,CB140))","v":1},null,null,{"$f":"IF(CN43=1,BD4,CE140)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa",33201,33201,33201,33201,33201,33201,33201,33201,33201,33201,33201,33201,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},33163,33183,{"$f":"\"\"","v":""},31953,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31083,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy","Drzwi pełne IP30   Wysokość",null,null,1,null,"Pole 2",null,1000,30720,30730,30740,30760,30780,null,null,1000,41310,51310,61310,71310,81310,91310,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,9,null,1,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","","","","","","","","","","","",null,"650+400",{"$f":"\"\"","v":""},20204,20214,20224,20234,20244,20254,20174,20184,33164,33184,33194,31954,30944,30940,31084,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,650,40766,50766,60766,70766,80766,90766,null,650,40766,50766,60766,70766,80766,90766]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,1200,30721,30731,30741,30761,30781,null,null,1200,41312,51312,61312,71312,81312,91312,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","","","","","","","","","","","",null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},33163,33183,{"$f":"\"\"","v":""},31953,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31083,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C141=0,\"\",\"\")","v":""},"","","","","",null,1300,30722,30732,30742,30762,30782,null,null,1300,41313,51313,61313,71313,81313,91313,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","","","","","","","","","","","",null,"850+400",{"$f":"\"\"","v":""},20204,20214,20224,20234,20244,20254,20174,20184,33164,33184,33194,31954,30944,30940,31084,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"650+150",40766,50766,60766,70766,80766,90766,null,"650+150",40165,50165,60165,70165,80165,90165]
[null,300,40330,50330,60330,70330,80330,90330,null,"650+650",30722,30732,30742,30762,30782,null,null,"650+650",41365,51365,61365,71365,81365,91365,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE141<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","","","","","","","","","","","",null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},33163,33183,{"$f":"\"\"","v":""},31953,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},31083,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,850,40786,50786,60786,70786,80786,90786,null,850,40786,50786,60786,70786,80786,90786]
[null,400,40340,50340,60340,70340,80340,90340,null,"650+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"650+850",41385,51385,61385,71385,81385,91385,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","","","","","","","","","","","",null,"150+650+400",{"$f":"\"\"","v":""},20204,20214,20224,20234,20244,20254,20174,20184,33164,33184,33194,31954,30944,30940,31084,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,"650+200",40766,50766,60766,70766,80766,90766,null,"650+200",40165,50165,60165,70165,80165,90165]
[null,450,40345,50345,60345,70345,80345,90345,null,"850+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"850+850",41385,51385,61385,71385,81385,91385,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,600,40360,50360,60360,70360,80360,90360,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,40365,50365,60365,70365,80365,90365,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W 1200 - 9","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,800,40380,50380,60380,70380,80380,90380,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"850+300",41330,51330,61330,71330,81330,91330,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+650",40766,50766,60766,70766,80766,90766,null,"650+650",40766,50766,60766,70766,80766,90766]
[null,"650+150",40380,50380,60380,70380,80380,90380,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"850+400",41340,51340,61340,71340,81340,91340,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osłona pełna",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+850",40766,50766,60766,70766,80766,90766,null,"650+850",40786,50786,60786,70786,80786,90786]
[null,850,40385,50385,60385,70385,80385,90385,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"650+150+300",41330,51330,61330,71330,81330,91330,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. modułowa",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+850",40786,50786,60786,70786,80786,90786,null,"850+850",40786,50786,60786,70786,80786,90786]
[null,"650+200",40385,50385,60385,70385,80385,90385,null,"150+650+400",30721,30731,30741,30761,30781,null,null,"650+150+400",41340,51340,61340,71340,81340,91340,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. przeszklona",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+300",40766,50766,60766,70766,80766,90766,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1000,40310,50310,60310,70310,80310,90310,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna stała TS35",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+400",40766,50766,60766,70766,80766,90766,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1200,40312,50312,60312,70312,80312,90312,null,"Głębokość obudowy D","Boki wentylowane IP-30,  Wysokość obudowy H",null,null,null,null,2,null,"Szerokość obudowy","Osłona tylna pełna IP30   Wysokość",null,null,4,null,"Pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna reg.TS35",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",40786,50786,60786,70786,80786,90786,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1300,40313,50313,60313,70313,80313,90313,null,null,1200,1400,1600,1800,2000,2200,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE159=14,14,IF(CP44=1,$BA$15,CB159))","v":1},null,null,{"$f":"IF(CP44=1,BD4,CE159)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta ocynk pełna",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",40786,50786,60786,70786,80786,90786,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+612",40365,50365,60365,70365,80365,90365,null,230,49223,59223,69223,79223,89223,99223,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE158=14,25,IF(CO44=1,$BA$12,CB158))","v":1},null,null,{"$f":"IF(CO44=1,BD4,CE158)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta malow.otw.",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"150+650+300",40766,50766,60766,70766,80766,90766,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+812",40385,50385,60385,70385,80385,90385,null,300,49230,59230,69230,79230,89230,99230,null,300,41230,51230,61230,71230,81230,91230,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE157=14,23,IF(CN44=1,$BA$13,CB157))","v":1},null,null,{"$f":"IF(CN44=1,BD4,CE157)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta oc. pozioma",{"$f":"IF(CW411=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"150+650+400",40766,50766,60766,70766,80766,90766,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+812",40385,50385,60385,70385,80385,90385,null,400,49240,59240,69240,79240,89240,99240,null,400,41240,51240,61240,71240,81240,91240,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,10,null,1,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa",{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","",""]
[null,"650+300",40330,50330,60330,70330,80330,90330,null,600,49260,59260,69260,79260,89260,99260,null,450,41245,51245,61245,71245,81245,91245,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","",""]
[null,"650+400",40340,50340,60340,70340,80340,90340,null,800,49280,59280,69280,79280,89280,99280,null,600,41260,51260,61260,71260,81260,91260,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szerokość obudowy","Pusty arkusz - formuły !!!!   Wysokość, Pole 1,2,3",null,null,null,1]
[null,"850+300",40330,50330,60330,70330,80330,90330,null,null,null,null,null,null,null,null,null,650,41265,51265,61265,71265,81265,91265,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE158<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,"850+400",40340,50340,60340,70340,80340,90340,null,"Głębokość obudowy D","Boki wentylowane IP-43/54,  Wysokość obudowy H",null,null,null,null,3,null,800,41280,51280,61280,71280,81280,91280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+300",40330,50330,60330,70330,80330,90330,null,null,1200,1400,1600,1800,2000,2200,null,"650+150",41280,51280,61280,71280,81280,91280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW147=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+400",40340,50340,60340,70340,80340,90340,null,230,49423,59423,69423,79423,89423,99423,null,850,41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,300,49430,59430,69430,79430,89430,99430,null,"650+200",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,400,49440,59440,69440,79440,89440,99440,null,1000,41210,51210,61210,71210,81210,91210,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W 1300 - 10","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,600,49460,59460,69460,79460,89460,99460,null,1200,41212,51212,61212,71212,81212,91212,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy","Drzwi wentylowane IP30 Wysokość",null,null,2,null,"Pole 2",null,800,49480,59480,69480,79480,89480,99480,null,1300,41213,51213,61213,71213,81213,91213,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osłona pełna",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,"650+612",41265,51265,61265,71265,81265,91265,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. modułowa",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+150",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C168=0,\"\",\"\")","v":""},"","","","","",null,"Głębokość obudowy D","Boki pełne IP-30,  Wysokość obudowy H",null,null,null,null,1,null,"650+812",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. przeszklona",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,40230,50230,60230,70230,80230,90230,null,null,1200,1400,1600,1800,2000,2200,null,"850+812",41285,51285,61285,71285,81285,91285,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna stała TS35",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+200",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,400,40240,50240,60240,70240,80240,90240,null,230,49323,59323,69323,79323,89323,99323,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE176=14,14,IF(CP45=1,$BA$15,CB176))","v":1},null,null,{"$f":"IF(CP45=1,BD4,CE176)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna reg.TS35",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,450,40245,50245,60245,70245,80245,90245,null,300,49330,59330,69330,79330,89330,99330,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE175=14,25,IF(CO45=1,$BA$12,CB175))","v":1},null,null,{"$f":"IF(CO45=1,BD4,CE175)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta ocynk pełna",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,600,40260,50260,60260,70260,80260,90260,null,400,49340,59340,69340,79340,89340,99340,null,"850+300",41230,51230,61230,71230,81230,91230,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE174=14,23,IF(CN45=1,$BA$13,CB174))","v":1},null,null,{"$f":"IF(CN45=1,BD4,CE174)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta malow.otw.",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,40265,50265,60265,70265,80265,90265,null,600,49360,59360,69360,79360,89360,99360,null,"850+400",41240,51240,61240,71240,81240,91240,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,11,null,1,11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta oc. pozioma",{"$f":"IF(CW162=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+650",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,800,40280,50280,60280,70280,80280,90280,null,800,49380,59380,69380,79380,89380,99380,null,"650+150+300",41230,51230,61230,71230,81230,91230,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa",{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+150",40280,50280,60280,70280,80280,90280,null,null,null,null,null,null,null,null,null,"650+150+400",41240,51240,61240,71240,81240,91240,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,850,40285,50285,60285,70285,80285,90285,null,"Głębokość obudowy D","Boki pełne IP-43/55,  Wysokość obudowy H",null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE175<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+200",40285,50285,60285,70285,80285,90285,null,null,1200,1400,1600,1800,2000,2200,null,"Szerokość obudowy","Osłona tylna went. IP43   Wysokość",null,null,9,null,"Pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1000,40210,50210,60210,70210,80210,90210,null,230,49523,59523,69523,79523,89523,99523,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1200,40212,50212,60212,70212,80212,90212,null,300,49530,59530,69530,79530,89530,99530,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW165=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,1300,40213,50213,60213,70213,80213,90213,null,400,49540,59540,69540,79540,89540,99540,null,300,41430,51430,61430,71430,81430,91430,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+612",40265,50265,60265,70265,80265,90265,null,600,49560,59560,69560,79560,89560,99560,null,400,41440,51440,61440,71440,81440,91440,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+812",40285,50285,60285,70285,80285,90285,null,800,49580,59580,69580,79580,89580,99580,null,450,41445,51445,61445,71445,81445,91445,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pusty - 11","1 mod.","2 mod.","3 mod.","4 mod.","5 mod.","6 mod.","7 mod.","8 mod.","9 mod.","10 mod.","11 mod.","12 mod."]
[null,"850+812",40285,50285,60285,70285,80285,90285,null,null,null,null,null,null,null,null,null,600,41460,51460,61460,71460,81460,91460,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","",""]
[null,"650+300",40230,50230,60230,70230,80230,90230,null,"Głębokość obudowy D","Boki stałe pełne,  Wysokość obudowy H",null,null,null,null,5,null,650,41465,51465,61465,71465,81465,91465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osłona pełna",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szerokość obudowy","Drzwi wewnętrzne   Wysokość, Pole 1,3",null,null,null,4,null,null,"Szerokość obudowy","Drzwi wewnetrzne   Wysokość, Pole 2",null,null,null,4]
[null,"650+400",40240,50240,60240,70240,80240,90240,null,null,1200,1400,1600,1800,2000,2200,null,800,41480,51480,61480,71480,81480,91480,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. modułowa",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200"]
[null,"850+300",40230,50230,60230,70230,80230,90230,null,230,49324,59324,69324,79324,89324,99324,null,"650+150",41480,51480,61480,71480,81480,91480,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Osł. przeszklona",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+400",40240,50240,60240,70240,80240,90240,null,300,49331,59331,69331,79331,89331,99331,null,850,41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE193=14,14,IF(CP46=1,$BA$15,CB193))","v":1},null,null,{"$f":"IF(CP46=1,BD4,CE193)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna stała TS35",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,45330,55330,65330,75330,85330,95330,null,300,45330,55330,65330,75330,85330,95330]
[null,"150+650+300",40230,50230,60230,70230,80230,90230,null,400,49341,59341,69341,79341,89341,99341,null,"650+200",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE192=14,25,IF(CO46=1,$BA$12,CB192))","v":1},null,null,{"$f":"IF(CO46=1,BD4,CE192)","v":1},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Szyna reg.TS35",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,45340,55340,65340,75340,85340,95340,null,400,45340,55340,65340,75340,85340,95340]
[null,"150+650+400",40240,50240,60240,70240,80240,90240,null,600,49361,59361,69361,79361,89361,99361,null,1000,41410,51410,61410,71410,81410,91410,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CE191=14,23,IF(CN46=1,$BA$13,CB191))","v":1},null,null,{"$f":"IF(CN46=1,BD4,CE191)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta ocynk pełna",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,450,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,800,49381,59381,69381,79381,89381,99381,null,1200,41412,51412,61412,71412,81412,91412,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,12,null,1,12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta malow.otw.",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,41413,51413,61413,71413,81413,91413,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Osłony",null,1,"Ilość mod.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta oc. pozioma",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,650,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"Głębokość obudowy D","Boki stałe wentylowane IP-30,  Wysokość obudowy H",null,null,null,null,6,null,"650+612",41465,51465,61465,71465,81465,91465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Brak\",\"None\")","v":"Brak"},null,1,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"1 modułowa\",\"1 module\")","v":"1 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Płyta licznikowa",{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy","Drzwi wentyl. IP43   Wysokość",null,null,7,null,"Pole 2",null,null,1200,1400,1600,1800,2000,2200,null,"650+812",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy pełny\",\"Plain front plate\")","v":"Panel osłonowy pełny"},null,{"$f":"IF($BA$12>1,0,IF(CE192<13,0,IF($BA$13>13,$BA$13-1,0)))","v":0},{"$f":"IF('Zenergy-OE'!$Y$32=1,\"2 modułowa\",\"2 modules\")","v":"2 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+150",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+150",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,230,49224,59224,69224,79224,89224,99224,null,"850+812",41485,51485,61485,71485,81485,91485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy modułowy\",\"Modular front plate\")","v":"Panel osłonowy modułowy"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"3 modułowa\",\"3 modules\")","v":"3 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,850,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,850,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C195=0,\"\",\"\")","v":""},"","","","","",null,300,49231,59231,69231,79231,89231,99231,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Panel osłonowy przeszklony\",\"Transparent front plate\")","v":"Panel osłonowy przeszklony"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"4 modułowa\",\"4 modules\")","v":"4 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+200",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+200",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,40430,50430,60430,70430,80430,90430,null,400,49241,59241,69241,79241,89241,99241,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D stała\",\"Fixed TS35D rail\")","v":"Szyna montażowa TS35D stała"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"5 modułowa\",\"5 modules\")","v":"5 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,400,40440,50440,60440,70440,80440,90440,null,600,49261,59261,69261,79261,89261,99261,null,"850+300",41430,51430,61430,71430,81430,91430,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Szyna montażowa TS35D regulowana\",\"Adjustable TS35D rail\")","v":"Szyna montażowa TS35D regulowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"6 modułowa\",\"6 modules\")","v":"6 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CW183=0,\"\",\"\")","v":""},"","","","","","","","","","","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1200,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,450,40445,50445,60445,70445,80445,90445,null,800,49281,59281,69281,79281,89281,99281,null,"850+400",41440,51440,61440,71440,81440,91440,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta montażowa pełna ocynkowana"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"7 modułowa\",\"7 modules\")","v":"7 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,600,40460,50460,60460,70460,80460,90460,null,null,null,null,null,null,null,null,null,"650+150+300",41430,51430,61430,71430,81430,91430,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa otworowana ocynk\",\"Painted mounting plate\")","v":"Płyta montażowa otworowana ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"8 modułowa\",\"8 modules\")","v":"8 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+650",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+650",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,40465,50465,60465,70465,80465,90465,null,"Głębokość obudowy D","Boki stałe wentylowane IP-43/54,  Wysokość obudowy H",null,null,null,null,7,null,"650+150+400",41440,51440,61440,71440,81440,91440,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta montażowa pozioma ocynk\",\"Horizontal plain mounting plate\")","v":"Płyta montażowa pozioma ocynk"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"9 modułowa\",\"9 modules\")","v":"9 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,800,40480,50480,60480,70480,80480,90480,null,null,1200,1400,1600,1800,2000,2200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Zabudowa licznikowa\",\"kWh mounting plate\")","v":"Zabudowa licznikowa"},null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"10 modułowa\",\"10 modules\")","v":"10 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"850+850",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+150",40480,50480,60480,70480,80480,90480,null,230,49424,59424,69424,79424,89424,99424,null,"Szerokość obudowy","Osłona tylna pełna IP55   Wysokość",null,null,8,null,"Pole 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"11 modułowa\",\"11 modules\")","v":"11 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+300",45330,55330,65330,75330,85330,95330]
[null,850,40485,50485,60485,70485,80485,90485,null,300,49431,59431,69431,79431,89431,99431,null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"12 modułowa\",\"12 modules\")","v":"12 modułowa"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+400",45340,55340,65340,75340,85340,95340]
[null,"650+200",40485,50485,60485,70485,80485,90485,null,400,49441,59441,69441,79441,89441,99441,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Płyta pełna ocynkowana\",\"Plain mounting plate\")","v":"Płyta pełna ocynkowana"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"850+300",45330,55330,65330,75330,85330,95330]
[null,1000,40410,50410,60410,70410,80410,90410,null,600,49461,59461,69461,79461,89461,99461,null,300,41530,51530,61530,71530,81530,91530,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Zenergy-OE'!$Y$32=1,\"Łącznik płyt pełnych\",\"Plates connector\")","v":"Łącznik płyt pełnych"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"850+400",45340,55340,65340,75340,85340,95340]
[null,1200,40412,50412,60412,70412,80412,90412,null,800,49481,59481,69481,79481,89481,99481,null,400,41540,51540,61540,71540,81540,91540,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"150+650+300",45330,55330,65330,75330,85330,95330]
[null,1300,40413,50413,60413,70413,80413,90413,null,null,null,null,null,null,null,null,null,450,41545,51545,61545,71545,81545,91545,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"150+650+400",45340,55340,65340,75340,85340,95340]
[null,"650+612",40465,50465,60465,70465,80465,90465,null,"Głębokość obudowy D","Boki pusty,  Wysokość obudowy H",null,null,null,null,8,null,600,41560,51560,61560,71560,81560,91560]
[null,"650+812",40485,50485,60485,70485,80485,90485,null,null,1200,1400,1600,1800,2000,2200,null,650,41565,51565,61565,71565,81565,91565]
[null,"850+812",40485,50485,60485,70485,80485,90485,null,230,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,800,41580,51580,61580,71580,81580,91580]
[null,"650+300",40430,50430,60430,70430,80430,90430,null,300,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+150",41580,51580,61580,71580,81580,91580]
[null,"650+400",40440,50440,60440,70440,80440,90440,null,400,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,850,41585,51585,61585,71585,81585,91585]
[null,"850+300",40430,50430,60430,70430,80430,90430,null,600,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+200",41585,51585,61585,71585,81585,91585]
[null,"850+400",40440,50440,60440,70440,80440,90440,null,800,{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,1000,41510,51510,61510,71510,81510,91510]
[null,"150+650+300",40430,50430,60430,70430,80430,90430,null,null,null,null,null,null,null,null,null,1200,41512,51512,61512,71512,81512,91512]
[null,"150+650+400",40440,50440,60440,70440,80440,90440,null,null,null,null,null,null,null,null,null,1300,41513,51513,61513,71513,81513,91513]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+612",41565,51565,61565,71565,81565,91565]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"650+812",41585,51585,61585,71585,81585,91585]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+812",41585,51585,61585,71585,81585,91585]
[null,"Szerokość obudowy","Drzwi pełne IP43/55   Wysokość",null,null,6,null,"Pole 2",null,null,null,null,null,null,null,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C222=0,\"\",\"\")","v":""},"","","","","",null,null,null,null,null,null,null,null,null,"850+300",41530,51530,61530,71530,81530,91530]
[null,300,40530,50530,60530,70530,80530,90530,null,null,null,null,null,null,null,null,null,"850+400",41540,51540,61540,71540,81540,91540]
[null,400,40540,50540,60540,70540,80540,90540,null,"Szerokość obudowy","Pokrywa górna IP30 wentylacja",null,null,null,"Pole 1,3",null,null,"650+150+300",41530,51530,61530,71530,81530,91530]
[null,450,40545,50545,60545,70545,80545,90545,null,null,230,300,400,600,800,null,null,"650+150+400",41540,51540,61540,71540,81540,91540]
[null,600,40560,50560,60560,70560,80560,90560,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,40565,50565,60565,70565,80565,90565,null,300,30230,30330,30430,30630,30830]
[null,800,40580,50580,60580,70580,80580,90580,null,400,30240,30340,30440,30640,30840,null,null,"Szerokość obudowy","Pokrywa górna IP30 wentylacja",null,null,null,"Pole 2"]
[null,"650+150",40580,50580,60580,70580,80580,90580,null,450,30245,30345,30445,30645,30845,null,null,null,230,300,400,600,800]
[null,850,40585,50585,60585,70585,80585,90585,null,600,30260,30360,30460,30660,30860,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+200",40585,50585,60585,70585,80585,90585,null,650,30265,30365,30465,30665,30865,null,null,300,30230,30330,30430,30630,30830]
[null,1000,40510,50510,60510,70510,80510,90510,null,800,30280,30380,30480,30680,30880,null,null,400,30240,30340,30440,30640,30840]
[null,1200,40512,50512,60512,70512,80512,90512,null,"650+150",30280,30380,30480,30680,30880,null,null,450,30245,30345,30445,30645,30845]
[null,1300,40513,50513,60513,70513,80513,90513,null,850,30285,30385,30485,30685,30885,null,null,600,30260,30360,30460,30660,30860]
[null,"650+612",40565,50565,60565,70565,80565,90565,null,"650+200",30285,30385,30485,30685,30885,null,null,650,30265,30365,30465,30665,30865]
[null,"650+812",40585,50585,60585,70585,80585,90585,null,1000,30210,30310,30410,30610,30810,null,null,800,30280,30380,30480,30680,30880]
[null,"850+812",40585,50585,60585,70585,80585,90585,null,1200,30212,30312,30412,30612,30812,null,null,"650+150",30280,30380,30480,30680,30880]
[null,"650+300",40530,50530,60530,70530,80530,90530,null,1300,30213,30313,30413,30613,30813,null,null,850,30285,30385,30485,30685,30885]
[null,"650+400",40540,50540,60540,70540,80540,90540,null,"650+612",30265,30365,30465,30665,30865,null,null,"650+200",30285,30385,30485,30685,30885]
[null,"850+300",40530,50530,60530,70530,80530,90530,null,"650+812",30265,30365,30465,30665,30865,null,null,1000,30210,30310,30410,30610,30810]
[null,"850+400",40540,50540,60540,70540,80540,90540,null,"850+812",30285,30385,30485,30685,30885,null,null,1200,30212,30312,30412,30612,30812]
[null,"150+650+300",40530,50530,60530,70530,80530,90530,null,"650+300",30295,30395,30495,30695,30895,null,null,1300,30213,30313,30413,30613,30813]
[null,"150+650+400",40540,50540,60540,70540,80540,90540,null,"650+400",30211,30311,30411,30611,30811,null,null,"650+612",30265,30365,30465,30665,30865]
[null,null,null,null,null,null,null,null,null,"850+300",30218,30318,30418,30618,30818,null,null,"650+812",30285,30385,30485,30685,30885]
[null,null,null,null,null,null,null,null,null,"850+400",30219,30319,30419,30619,30819,null,null,"850+812",30285,30385,30485,30685,30885]
[null,null,null,null,null,null,null,null,null,"150+650+300",30222,30322,30422,30622,30822,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy","Drzwi przeszklone IP55   Wysokość",null,null,3,null,"Pole 2",null,"150+650+400",30223,30323,30423,30623,30823,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,"H 1200","H 1400","H 1600","H 1800","H 2000","H 2200",null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C249=0,\"\",\"\")","v":""},"","","","","",null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,"","","","","","",null,"Szerokość obudowy","Pokrywa górna IP30",null,null,null,"Pole 1,3",null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,400,40640,50640,60640,70640,80640,90640,"`",null,230,300,400,600,800,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,450,40645,50645,60645,70645,80645,90645,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,600,40660,50660,60660,70660,80660,90660,null,300,31230,31330,31430,31630,31830]
[null,650,40665,50665,60665,70665,80665,90665,null,400,31240,31340,31440,31640,31840,null,null,"Szerokość obudowy","Pokrywa górna IP30",null,null,null,"Pole 2"]
[null,800,40680,50680,60680,70680,80680,90680,null,450,31245,31345,31445,31645,31845,null,null,null,230,300,400,600,800]
[null,"650+150",40680,50680,60680,70680,80680,90680,null,600,31260,31360,31460,31660,31860,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,850,40685,50685,60685,70685,80685,90685,null,650,31265,31365,31465,31665,31865,null,null,300,31230,31330,31430,31630,31830]
[null,"650+200",40685,50685,60685,70685,80685,90685,null,800,31280,31380,31480,31680,31880,null,null,400,31240,31340,31440,31640,31840]
[null,1000,40610,50610,60610,70610,80610,90610,null,"650+150",31280,31380,31480,31680,31880,null,null,450,31245,31345,31445,31645,31845]
[null,1200,40612,50612,60612,70612,80612,90612,null,850,31285,31385,31485,31685,31885,null,null,600,31260,31360,31460,31660,31860]
[null,1300,40613,50613,60613,70613,80613,90613,null,"650+200",31285,31385,31485,31685,31885,null,null,650,31265,31365,31465,31665,31865]
[null,"650+612",40665,50665,60665,70665,80665,90665,null,1000,31210,31310,31410,31610,31810,null,null,800,31280,31380,31480,31680,31880]
[null,"650+812",40685,50685,60685,70685,80685,90685,null,1200,31212,31312,31412,31612,31812,null,null,"650+150",31280,31380,31480,31680,31880]
[null,"850+812",40685,50685,60685,70685,80685,90685,null,1300,31213,31313,31413,31613,31813,null,null,850,31285,31385,31485,31685,31885]
[null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+612",31265,31365,31465,31665,31865,null,null,"650+200",31285,31385,31485,31685,31885]
[null,"650+400",40640,50640,60640,70640,80640,90640,null,"650+812",31265,31365,31465,31665,31865,null,null,1000,31210,31310,31410,31610,31810]
[null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"850+812",31285,31385,31485,31685,31885,null,null,1200,31212,31312,31412,31612,31812]
[null,"850+400",40640,50640,60640,70640,80640,90640,null,"650+300",31295,31395,31495,31695,31895,null,null,1300,31213,31313,31413,31613,31813]
[null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,"650+400",31211,31311,31411,31611,31811,null,null,"650+612",31265,31365,31465,31665,31865]
[null,"150+650+400",40640,50640,60640,70640,80640,90640,null,"850+300",31218,31318,31418,31618,31818,null,null,"650+812",31285,31385,31485,31685,31885]
[null,null,null,null,null,null,null,null,null,"850+400",31219,31319,31419,31619,31819,null,null,"850+812",31285,31385,31485,31685,31885]
[null,null,null,null,null,null,null,null,null,"150+650+300",31222,31322,31422,31622,31822,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"150+650+400",31223,31323,31423,31623,31823,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy W","Rama o głębokości D 230 mm,  Wysokość obudowy H",null,null,null,null,null,null,"Szerokość obudowy","Pokrywa górna IP54/43 went.",null,null,null,"Pole 1,3",null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,1200,1400,1600,1800,2000,2200,null,null,230,300,400,600,800,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C278=0,\"\",\"\")","v":""},"","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,42030,52030,62030,72030,82030,92030,null,300,32230,32330,32430,32630,32830]
[null,400,42040,52040,62040,72040,82040,92040,null,400,32240,32340,32440,32640,32840,null,null,"Szerokość obudowy","Pokrywa górna IP54/43 went.",null,null,null,"Pole 2"]
[null,450,42045,52045,62045,72045,82045,92045,null,450,32245,32345,32445,32645,32845,null,null,null,230,300,400,600,800]
[null,600,42060,52060,62060,72060,82060,92060,null,600,32260,32360,32460,32660,32860,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,42065,52065,62065,72065,82065,92065,null,650,32265,32365,32465,32665,32865,null,null,300,32230,32330,32430,32630,32830]
[null,800,42080,52080,62080,72080,82080,92080,null,800,32280,32380,32480,32680,32880,null,null,400,32240,32340,32440,32640,32840]
[null,"650+150",42081,52081,62081,72081,82081,92081,null,"650+150",32280,32380,32480,32680,32880,null,null,450,32245,32345,32445,32645,32845]
[null,850,42085,52085,62085,72085,82085,92085,null,850,32285,32385,32485,32685,32885,null,null,600,32260,32360,32460,32660,32860]
[null,"650+200",42086,52086,62086,72086,82086,92086,null,"650+200",32285,32385,32485,32685,32885,null,null,650,32265,32365,32465,32665,32865]
[null,1000,42100,52100,62100,72100,82100,92100,null,1000,32210,32310,32410,32610,32810,null,null,800,32280,32380,32480,32680,32880]
[null,1200,42120,52120,62120,72120,82120,92120,null,1200,32212,32312,32412,32612,32812,null,null,"650+150",32280,32380,32480,32680,32880]
[null,1300,42130,52130,62130,72130,82130,92130,null,1300,32213,32313,32413,32613,32813,null,null,850,32285,32385,32485,32685,32885]
[null,"650+612",42131,52131,62131,72131,82131,92131,null,"650+612",32265,32365,32465,32665,32865,null,null,"650+200",32285,32385,32485,32685,32885]
[null,"650+812",42150,52150,62150,72150,82150,92150,null,"650+812",32265,32365,32465,32665,32865,null,null,1000,32210,32310,32410,32610,32810]
[null,"850+812",42170,52170,62170,72170,82170,92170,null,"850+812",32285,32385,32485,32685,32885,null,null,1200,32212,32312,32412,32612,32812]
[null,"650+300",42095,52095,62095,72095,82095,92095,null,"650+300",32295,32395,32495,32695,32895,null,null,1300,32213,32313,32413,32613,32813]
[null,"650+400",42105,52105,62105,72105,82105,92105,null,"650+400",32211,32311,32411,32611,32811,null,null,"650+612",32265,32365,32465,32665,32865]
[null,"850+300",42115,52115,62115,72115,82115,92115,null,"850+300",32218,32318,32418,32618,32818,null,null,"650+812",32285,32385,32485,32685,32885]
[null,"850+400",42125,52125,62125,72125,82125,92125,null,"850+400",32219,32319,32419,32619,32819,null,null,"850+812",32285,32385,32485,32685,32885]
[null,"150+650+300",42110,52110,62110,72110,82110,92110,null,"150+650+300",32222,32322,32422,32622,32822,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+400",42121,52121,62121,72121,82121,92121,null,"150+650+400",32223,32323,32423,32623,32823,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy W","Rama o głębokości D 300 mm,  Wysokość obudowy H",null,null,null,null,null,null,"Szerokość obudowy","Pokrywa górna IP55",null,null,null,"Pole 1,3",null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,1200,1400,1600,1800,2000,2200,null,null,230,300,400,600,800,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C304=0,\"\",\"\")","v":""},"","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,43030,53030,63030,73030,83030,93030,null,300,33230,33330,33430,33630,33830]
[null,400,43040,53040,63040,73040,83040,93040,null,400,33240,33340,33440,33640,33840,null,null,"Szerokość obudowy","Pokrywa górna IP55",null,null,null,"Pole 2"]
[null,450,43045,53045,63045,73045,83045,93045,null,450,33245,33345,33445,33645,33845,null,null,null,230,300,400,600,800]
[null,600,43060,53060,63060,73060,83060,93060,null,600,33260,33360,33460,33660,33860,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,43065,53065,63065,73065,83065,93065,null,650,33265,33365,33465,33665,33865,null,null,300,33230,33330,33430,33630,33830]
[null,800,43080,53080,63080,73080,83080,93080,null,800,33280,33380,33480,33680,33880,null,null,400,33240,33340,33440,33640,33840]
[null,"650+150",43081,53081,63081,73081,83081,93081,null,"650+150",33280,33380,33480,33680,33880,null,null,450,33245,33345,33445,33645,33845]
[null,850,43085,53085,63085,73085,83085,93085,null,850,33285,33385,33485,33685,33885,null,null,600,33260,33360,33460,33660,33860]
[null,"650+200",43086,53086,63086,73086,83086,93086,null,"650+200",33285,33385,33485,33685,33885,null,null,650,33265,33365,33465,33665,33865]
[null,1000,43100,53100,63100,73100,83100,93100,null,1000,33210,33310,33410,33610,33810,null,null,800,33280,33380,33480,33680,33880]
[null,1200,43120,53120,63120,73120,83120,93120,null,1200,33212,33312,33412,33612,33812,null,null,"650+150",33280,33380,33480,33680,33880]
[null,1300,43130,53130,63130,73130,83130,93130,null,1300,33213,33313,33413,33613,33813,null,null,850,33285,33385,33485,33685,33885]
[null,"650+612",43131,53131,63131,73131,83131,93131,null,"650+612",33265,33365,33465,33665,33865,null,null,"650+200",33285,33385,33485,33685,33885]
[null,"650+812",43150,53150,63150,73150,83150,93150,null,"650+812",33265,33365,33465,33665,33865,null,null,1000,33210,33310,33410,33610,33810]
[null,"850+812",43170,53170,63170,73170,83170,93170,null,"850+812",33285,33385,33485,33685,33885,null,null,1200,33212,33312,33412,33612,33812]
[null,"650+300",43095,53095,63095,73095,83095,93095,null,"650+300",33295,33395,33495,33695,33895,null,null,1300,33213,33313,33413,33613,33813]
[null,"650+400",43105,53105,63105,73105,83105,93105,null,"650+400",33211,33311,33411,33611,33811,null,null,"650+612",33265,33365,33465,33665,33865]
[null,"850+300",43115,53115,63115,73115,83115,93115,null,"850+300",33218,33318,33418,33618,33818,null,null,"650+812",33285,33385,33485,33685,33885]
[null,"850+400",43125,53125,63125,73125,83125,93125,null,"850+400",33219,33319,33419,33619,33819,null,null,"850+812",33285,33385,33485,33685,33885]
[null,"150+650+300",43110,53110,63110,73110,83110,93110,null,"150+650+300",33222,33322,33422,33622,33822,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+400",43121,53121,63121,73121,83121,93121,null,"150+650+400",33223,33323,33423,33623,33823,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Szerokość obudowy W","Rama o głębokości D 400 mm,  Wysokość obudowy H",null,null,null,null,null,null,"Szerokość obudowy","Cokół przód 100mm",null,null,null,"Pole 1,3",null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,1200,1400,1600,1800,2000,2200,null,null,230,300,400,600,800,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"Brak",{"$f":"IF(C330=0,\"\",\"\")","v":""},"","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,44030,54030,64030,74030,84030,94030,null,300,30030,30030,30030,30030,30030]
[null,400,44040,54040,64040,74040,84040,94040,null,400,30040,30040,30040,30040,30040,null,null,"Szerokość obudowy","Płyta dławicowa IP-55, Pole 1, 3"]
[null,450,44045,54045,64045,74045,84045,94045,null,450,30045,30045,30045,30045,30045,null,null,null,230,300,400,600,800]
[null,600,44060,54060,64060,74060,84060,94060,null,600,30060,30060,30060,30060,30060,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,650,44065,54065,64065,74065,84065,94065,null,650,30065,30065,30065,30065,30065,null,null,300,31523,31533,31543,31563,31583]
[null,800,44080,54080,64080,74080,84080,94080,null,800,30080,30080,30080,30080,30080,null,null,400,31524,31534,31544,31564,31584]
[null,"650+150",44081,54081,64081,74081,84081,94081,null,"650+150",30080,30080,30080,30080,30080,null,null,450,31525,31535,31545,31565,31585]
[null,850,44085,54085,64085,74085,84085,94085,null,850,30085,30085,30085,30085,30085,null,null,600,31526,31536,31546,31566,31586]
[null,"650+200",44086,54086,64086,74086,84086,94086,null,"650+200",30085,30085,30085,30085,30085,null,null,650,31527,31537,31547,31567,31587]
[null,1000,44100,54100,64100,74100,84100,94100,null,1000,30010,30010,30010,30010,30010,null,null,800,31528,31538,31548,31568,31588]
[null,1200,44120,54120,64120,74120,84120,94120,null,1200,30012,30012,30012,30012,30012,null,null,"650+150",31550,31552,31554,31556,31558]
[null,1300,44130,54130,64130,74130,84130,94130,null,1300,30013,30013,30013,30013,30013,null,null,850,31529,31539,31549,31569,31589]
[null,"650+612",44131,54131,64131,74131,84131,94131,null,"650+612",30065,30065,30065,30065,30065,null,null,"650+200",31551,31553,31555,31557,31559]
[null,"650+812",44150,54150,64150,74150,84150,94150,null,"650+812",30065,30065,30065,30065,30065,null,null,1000,31520,31530,31540,31560,31580]
[null,"850+812",44170,54170,64170,74170,84170,94170,null,"850+812",30085,30085,30085,30085,30085,null,null,1200,31521,31531,31541,31561,31581]
[null,"650+300",44095,54095,64095,74095,84095,94095,null,"650+300",30096,30096,30096,30096,30096,null,null,1300,31522,31532,31542,31562,31582]
[null,"650+400",44105,54105,64105,74105,84105,94105,null,"650+400",30006,30006,30006,30006,30006,null,null,"650+612",31527,31537,31547,31567,31587]
[null,"850+300",44115,54115,64115,74115,84115,94115,null,"850+300",30016,30016,30016,30016,30016,null,null,"650+812",31527,31537,31547,31567,31587]
[null,"850+400",44125,54125,64125,74125,84125,94125,null,"850+400",30026,30026,30026,30026,30026,null,null,"850+812",31529,31539,31549,31569,31589]
[null,"150+650+300",44110,54110,64110,74110,84110,94110,null,"150+650+300",30011,30011,30011,30011,30011,null,null,"650+300",31527,31537,31547,31567,31587]
[null,"150+650+400",44121,54121,64121,74121,84121,94121,null,"150+650+400",30021,30021,30021,30021,30021,null,null,"650+400",31527,31537,31547,31567,31587]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+300",31529,31539,31549,31569,31589]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"850+400",31529,31539,31549,31569,31589]
[null,"Szerokość obudowy W","Rama o głębokości D 600 mm,  Wysokość obudowy H",null,null,null,null,null,null,"Szerokość obudowy","Cokół przód 200mm",null,null,null,"Pole 1,3",null,null,"150+650+300",31550,31552,31554,31556,31558]
[null,null,1200,1400,1600,1800,2000,2200,null,null,230,300,400,600,800,null,null,"150+650+400",31550,31552,31554,31556,31558]
[null,"Brak",{"$f":"IF(C356=0,\"\",\"\")","v":""},"","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,300,46030,56030,66030,76030,86030,96030,null,300,30130,30130,30130,30130,30130]
[null,400,46040,56040,66040,76040,86040,96040,null,400,30140,30140,30140,30140,30140]
[null,450,46045,56045,66045,76045,86045,96045,null,450,30145,30145,30145,30145,30145]
[null,600,46060,56060,66060,76060,86060,96060,null,600,30160,30160,30160,30160,30160]
[null,650,46065,56065,66065,76065,86065,96065,null,650,30165,30165,30165,30165,30165]
[null,800,46080,56080,66080,76080,86080,96080,null,800,30180,30180,30180,30180,30180]
[null,"650+150",46081,56081,66081,76081,86081,96081,null,"650+150",30180,30180,30180,30180,30180]
[null,850,46085,56085,66085,76085,86085,96085,null,850,30185,30185,30185,30185,30185]
[null,"650+200",46086,56086,66086,76086,86086,96086,null,"650+200",30185,30185,30185,30185,30185]
[null,1000,46100,56100,66100,76100,86100,96100,null,1000,30110,30110,30110,30110,30110]
[null,1200,46120,56120,66120,76120,86120,96120,null,1200,30112,30112,30112,30112,30112]
[null,1300,46130,56130,66130,76130,86130,96130,null,1300,30113,30113,30113,30113,30113]
[null,"650+650",46131,56131,66131,76131,86131,96131,null,"650+612",30165,30165,30165,30165,30165]
[null,"650+850",46150,56150,66150,76150,86150,96150,null,"650+812",30165,30165,30165,30165,30165]
[null,"850+850",46170,56170,66170,76170,86170,96170,null,"850+812",30185,30185,30185,30185,30185,null,null,"Szerokość obudowy","Płyta dławicowa IP-55, Pole 2"]
[null,"650+300",46095,56095,66095,76095,86095,96095,null,"650+300",30196,30196,30196,30196,30196,null,null,null,230,300,400,600,800]
[null,"650+400",46105,56105,66105,76105,86105,96105,null,"650+400",30106,30106,30106,30106,30106,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+300",46115,56115,66115,76115,86115,96115,null,"850+300",30116,30116,30116,30116,30116,null,null,300,31523,31533,31543,31563,31583]
[null,"850+400",46125,56125,66125,76125,86125,96125,null,"850+400",30126,30126,30126,30126,30126,null,null,400,31524,31534,31544,31564,31584]
[null,"150+650+300",46110,56110,66110,76110,86110,96110,null,"150+650+300",30111,30111,30111,30111,30111,null,null,450,31525,31535,31545,31565,31585]
[null,"150+650+400",46121,56121,66121,76121,86121,96121,null,"150+650+400",30121,30121,30121,30121,30121,null,null,600,31526,31536,31546,31566,31586]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,650,31527,31537,31547,31567,31587]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,31528,31538,31548,31568,31588]
[null,"Szerokość obudowy W","Rama o głębokości D 800 mm,  Wysokość obudowy H",null,null,null,null,null,null,"Szerokość obudowy","Cokół przód 100mm",null,null,null,"Pole 2",null,null,"650+150",31550,31552,31554,31556,31558]
[null,null,1200,1400,1600,1800,2000,2200,null,null,230,300,400,600,800,null,null,850,31529,31539,31549,31569,31589]
[null,"Brak",{"$f":"IF(C382=0,\"\",\"\")","v":""},"","","","","",null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},null,null,"650+200",31551,31553,31555,31557,31559]
[null,300,48030,58030,68030,78030,88030,98030,null,300,30030,30030,30030,30030,30030,null,null,1000,31520,31530,31540,31560,31580]
[null,400,48040,58040,68040,78040,88040,98040,null,400,30040,30040,30040,30040,30040,null,null,1200,31521,31531,31541,31561,31581]
[null,450,48045,58045,68045,78045,88045,98045,null,450,30045,30045,30045,30045,30045,null,null,1300,31522,31532,31542,31562,31582]
[null,600,48060,58060,68060,78060,88060,98060,null,600,30060,30060,30060,30060,30060,null,null,"650+612",31527,31537,31547,31567,31587]
[null,650,48065,58065,68065,78065,88065,98065,null,650,30065,30065,30065,30065,30065,null,null,"650+812",31529,31539,31549,31569,31589]
[null,800,48080,58080,68080,78080,88080,98080,null,800,30080,30080,30080,30080,30080,null,null,"850+812",31529,31539,31549,31569,31589]
[null,"650+150",48081,58081,68081,78081,88081,98081,null,"650+150",30080,30080,30080,30080,30080,null,null,"650+300",31523,31533,31543,31563,31583]
[null,850,48085,58085,68085,78085,88085,98085,null,850,30085,30085,30085,30085,30085,null,null,"650+400",31524,31534,31544,31564,31584]
[null,"650+200",48086,58086,68086,78086,88086,98086,null,"650+200",30085,30085,30085,30085,30085,null,null,"850+300",31523,31533,31543,31563,31583]
[null,1000,48100,58100,68100,78100,88100,98100,null,1000,30010,30010,30010,30010,30010,null,null,"850+400",31524,31534,31544,31564,31584]
[null,1200,48120,58120,68120,78120,88120,98120,null,1200,30012,30012,30012,30012,30012,null,null,"150+650+300",31523,31533,31543,31563,31583]
[null,1300,48130,58130,68130,78130,88130,98130,null,1300,30013,30013,30013,30013,30013,null,null,"150+650+400",31524,31534,31544,31564,31584]
[null,"650+612",48131,58131,68131,78131,88131,98131,null,"650+612",30065,30065,30065,30065,30065]
[null,"650+812",48150,58150,68150,78150,88150,98150,null,"650+812",30085,30085,30085,30085,30085]
[null,"850+812",48170,58170,68170,78170,88170,98170,null,"850+812",30085,30085,30085,30085,30085]
[null,"650+300",48095,58095,68095,78095,88095,98095,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"650+400",48105,58105,68105,78105,88105,98105,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+300",48115,58115,68115,78115,88115,98115,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"850+400",48125,58125,68125,78125,88125,98125,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+300",48110,58110,68110,78110,88110,98110,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,"150+650+400",48121,58121,68121,78121,88121,98121,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[]
[]
[null,null,null,null,null,null,null,null,null,"Szerokość obudowy","Cokół przód 200mm",null,null,null,"Pole 2"]
[null,null,null,null,null,null,null,null,null,null,230,300,400,600,800]
[null,null,null,null,null,null,null,null,null,"Brak",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,300,30130,30130,30130,30130,30130]
[null,null,null,null,null,null,null,null,null,400,30140,30140,30140,30140,30140]
[null,null,null,null,null,null,null,null,null,450,30145,30145,30145,30145,30145]
[null,null,null,null,null,null,null,null,null,600,30160,30160,30160,30160,30160]
[null,null,null,null,null,null,null,null,null,650,30165,30165,30165,30165,30165]
[null,null,null,null,null,null,null,null,null,800,30180,30180,30180,30180,30180]
[null,null,null,null,null,null,null,null,null,"650+150",30180,30180,30180,30180,30180]
[null,null,null,null,null,null,null,null,null,850,30185,30185,30185,30185,30185]
[null,null,null,null,null,null,null,null,null,"650+200",30185,30185,30185,30185,30185]
[null,null,null,null,null,null,null,null,null,1000,30110,30110,30110,30110,30110]
[null,null,null,null,null,null,null,null,null,1200,30112,30112,30112,30112,30112]
[null,null,null,null,null,null,null,null,null,1300,30113,30113,30113,30113,30113]
[null,null,null,null,null,null,null,null,null,"650+612",30165,30165,30165,30165,30165]
[null,null,null,null,null,null,null,null,null,"650+812",30185,30185,30185,30185,30185]
[null,null,null,null,null,null,null,null,null,"850+812",30185,30185,30185,30185,30185]
[null,null,null,null,null,null,null,null,null,"650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"850+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"850+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"150+650+300",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]
[null,null,null,null,null,null,null,null,null,"150+650+400",{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""},{"$f":"\"\"","v":""}]